> ACS Host Pool Configuration Mode Commands
> The ACS Host Pool Configuration Mode is used to define a pool of host addresses within the ACS Configuration Mode. The host pool facilitates to create rules to handle the packets coming from or going to a group of hosts within an access policy.
> Important: The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> ip
> This command allows you to add/remove an individual or a range of host IPv4/IPv6 address(es) from the current host pool.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] ip { ip_address | ip_address/maskbit | range start_ip to end_ip }
> no
> If added previously, removes the specified IPv4/IPv6 address(es) from the current host pool.
> ip_address
> Specifies an IPv4/IPv6 address to add to the current host pool.
> ip_address must be an IPv4/IPv6 address.
> ip_address/maskbit
> Specifies an IPv4/IPv6 address/mask bits combination to add to the current host pool.
> ip_address must be an IPv4/IPv6 address.
> maskbit must be the number of bits in the subnet mask, and must be a numeric value.
> range start_ip to end_ip
> Specifies a range of IPv4/IPv6 addresses to add to the current host pool.
> start_ip specifies the starting IPv4/IPv6 address of the range, and must be less than end_ip.
> end_ip specifies the ending IPv4/IPv6 address of the range, and must be greater than start_ip.
> Usage
> Use this command to add an individual or a range of IPv4/IPv6 addresses to a host pool. Up to 10 sets of IPv4/IPv6 addresses can be configured in each host pool.
> Example
> The following command adds all IPv4 addresses from 10.2.3.4 through 10.4.5.6 to the current host pool:
> ip range 10.2.3.4 to 10.4.5.6

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883