> PCC-QoS-Profile Configuration Mode Commands
> The PCC-QoS-Profile Configuration Mode is used to define the QoS logic used by the operator for managing the QoS policy requirements and objectives for the network specific to a group of subscribers in the network. A QoS Profile represents a resource requirement identified by means of the corresponding QoS attributes like QCI, MBR, GBR, ARP etc.
> Important: This configuration mode is supported from StarOS Release 12.1 onward.
> arp-priority
> This command is used to define the Allocation and Retention Priority (ARP) values of the QoS profile in PCC-QoS-Profile which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] arp-priority arp_priority pre-emption {capable | not-capable} {not-vulnerable | vulnerable}
> no
> Removes the configured ARP priority set for PCC-QoS-Profile for PCC-Service instance on IPCF node.
> arp_priority
> Specifies the priority value for ARP in a PCC-QoS-Profile which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> arp_priority must be an integer from 1 through 15.
> pre-emption {capable | not-capable}
> Sets the Pre-emption capability related parameters with ARP priority in PCC-QoS-Profile name which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Pre-emption capability determines whether a bearer with a lower ARP priority level should be dropped to free up the required resources.
> capable: This keyword indicates that the service data flow is allowed to get resources that were already assigned to another service data flow with a lower priority level.
> non-capable: This keyword indicates that the service data flow is not allowed to get resources that were already assigned to another service data flow with a lower priority level.
> {not-vulnerable | vulnerable}
> Sets the Pre-emption vulnerability related parameters with ARP priority in PCC-QoS-Profile name which is to use in Subscriber profile in PCC-Service instance on IPCF node.
> Pre-emption vulnerability determines whether a bearer is applicable for dropping by a pre-emption capable bearer with a higher ARP priority value.
> not-vulnerable: This keyword indicates that the resources assigned to the service data flow shall not be pre-empted and allocated to a service data flow with a higher priority level.
> vulnerable: This keyword indicates that the resources assigned to the service data flow can be pre-empted and allocated to a service data flow with a higher priority level.
> Usage
> Use this command to define the ARP priority and pre-empt parameters in PCC-QoS-Profile which is to be used in Subscriber profile in PCC-Service instance on IPCF node.
> ARP controls how the IPCF reacts when there are insufficient resources to establish the new RAB. Typically it manages it by; 1) Deny the RAB request and 2) Preempt an existing RAB and accept the new RAB request.
> Example
> Following command sets the ARP Priority 2 with preemption capability and vulnerability in PCC-QoS-Profile instance on IPCF node.
> arp-priority 2 pre-emption capable vulnerable
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> guaranteed-bitrate
> This command defines the Guaranteed Bit Rate (GBR) value in bits per second for downlink and uplink traffic in PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] guaranteed-bitrate downlink downlink_gbr uplink uplink_gbr
> no
> Removes the configured GBR value set for PCC-QoS-Profile for PCC-Service instance on IPCF node.
> downlink downlink_gbr
> Sets the Guaranteed Bit Rate allowed in downlink direction (from PCEF to UE) in bits per second for a PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> downlink_gbr must be an integer from 0 through 104857600. A ‘zero’ value disables the downlink in specified PCC-QoS-Profile.
> uplink uplink_gbr
> Sets the Guaranteed Bit Rate allowed in uplink direction (from PCEF to PDN) in bits per second for a PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> uplink_gbr must be an integer from 0 through 104857600. A ‘zero’ value disables the uplink in specified PCC-QoS-Profile.
> Usage
> Use this command to define the Guaranteed Bit Rate value in bits per second for downlink and uplink traffic in PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> Example
> Following command sets the 1024 bits per seconds as uplink GBR and 2048 bits per second as downlink GBR in PCC-QoS-Profile instance on IPCF node.
> guaranteed-bitrate downlink 2048 uplink 1024
> max-bitrate
> This command defines the Maximum Bit Rate (MBR) value in bits per second for downlink and uplink traffic in PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] max-bitrate downlink downlink_mbr uplink uplink_mbr
> no
> Removes the configured Maximum Bit Rate value set for PCC-QoS-Profile for PCC-Service instance on IPCF node.
> downlink downlink_mbr
> Sets the Maximum Bit Rate allowed in downlink direction (from PCEF to UE) in bits per second for a PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> downlink_mbr must be an integer from 0 through 104857600. A ‘zero’ value disables the downlink in specified PCC-QoS-Profile.
> uplink uplink_mbr
> Sets the Maximum Bit Rate allowed in uplink direction (from PCEF to PDN) in bits per second for a PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> uplink_mbr must be an integer from 0 through 104857600. A ‘zero’ value disables the uplink in specified PCC-QoS-Profile.
> Usage
> Use this command to define the Maximum Bit Rate value in bits per second for downlink and uplink traffic in PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> Example
> Following command sets the 1024 bits per seconds as uplink MBR and 2048 bits per second as downlink MBR in PCC-QoS-Profile instance on IPCF node.
> max-bitrate downlink 2048 uplink 1024
> qci
> This command sets the QoS Class Identifier (QCI) for PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [no] qci qci_id
> no
> Removes the configured QCI value set for PCC-QoS-Profile for PCC-Service instance on IPCF node.
> qci qci_id
> Sets the QoS Class Identifier for a PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> qci_id must be an integer from 1 through 255.
> Usage
> Use this command to set the QoS Class Identifier for PCC-QoS-Profile which is to use for Subscriber profile in PCC-Service instance on IPCF node.
> Example
> Following command sets the QCI 101 for PCC-QoS-Profile instance on IPCF node.
> qci 101

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883