> Replacing Application Cards
> This chapter provides information on replacing a failed application card.
> This chapter includes the following sections:

> • | Determining Whether an Application Card has Failed

> • | Removing the Application Card

> • | Installing the Application Card

> • | Removing and Replacing the CompactFlash Memory Card on SMCs

> • | What to do with the Failed Application Card

> ESD Caution: During installation, maintenance, and/or removal, wear a grounding wrist strap to avoid ESD damage to the components. Failure to do so could result in damage to sensitive electronic components and potentially void your warranty.
> Determining Whether an Application Card has Failed
> The system has several ways to indicate an application card failure. The first indicator is that the Status LED on the System Management Card (SMC) turns red to indicate the failure of a chassis component. Another indicator is the Run/Fail LED on an application card is red or turns off if that card has a problem.
> If you see either of these indicators, you can determine the nature of the problem via the CLI or by checking the Simple Network Management Protocol (SNMP) traps.
> Using the CLI
> Monitor application cards in the chassis by executing the following CLI commands in Exec mode:
> show card diag slot_#
> slot_# is the chassis slot number in which the particular card that you wish to monitor is installed. For application cards, slot_# is any integer between 1 and 16. The following is a sample output for this command to monitor the card in chassis slot 8:
> Card 8:
> Card Usable : Yes
> Card Tests : Pass
> Boot Mode : Normal
> show card info slot_#
> The following is a sample output for this command issued to monitor the card in chassis slot 8:
> Card 8:
> Slot Type : SMC
> Card Type : System Management Card
> Card Revision : 1
> Operational State : Active
> Last State Change : Thursday January 27 16:00:32 EST 2008
> Administrative State : Enabled
> Card Lock : Locked
> Reboot Pending : No
> Card Usable : Yes
> Single Point of Failure : No
> Attachment : 24 (System Management I/O Card)
> Temperature : 20 C (limit 70 C)
> Voltage: 1.3 V : 1.3 V (min 1.2 V, max 1.4 V)
> Voltage: 1.5 V : 1.5 V (min 1.4 V, max 1.6 V)
> Voltage: 1.8 V : 1.8 V (min 1.7 V, max 1.9 V)
> Voltage: 2.5 V : 2.5 V (min 2.4 V, max 2.6 V)
> Voltage: 3.3 V : 3.3 V (min 3.1 V, max 3.5 V)
> Voltage: 5.0 V : 5.0 V (min 4.8 V, max 5.2 V)
> Card LEDs : Run/Fail: Green | Active: Green | Standby: Off
> System LEDs : Status: Green | Service: Off
> Compact Flash : Present
> Type : 128M disk
> Model : SanDiskSDCFB-128
> Serial Number : 10000008
> PCMCIA 1 : Not Present
> PCMCIA 2 : Not Present
> CPU 0 : Kernel Running, Tasks Running
> If any of this information appears to be erroneous, such as the operational state or an LED state, check for any of the SNMP alarms listed in the Using SNMP Traps section that follows.
> Using SNMP Traps
> The system supports SNMP traps that are triggered when conditions indicate the need to replace an application card. The system provides the following traps:

> SNMP Trap | Description
> starCardVoltageFailure | A voltage regulation failure has been detected in a card.
> starCardBootFailed | A card has failed to start up properly. The card is not operational.
> starCardFailed | The card has failed and is no longer operational.
> starCardSWFailed | An unrecoverable software error has occurred on the card.
> starCardPSCMigrateStart | A packet processing card migration operation has begun. The first varbind identifies the packet processing card whose tasks are being migrated from; the second varbind identifies the packet processing card where the tasks are being migrated to. If a migration is taking place, it is likely that there is a problem with the original packet processing card.
> starCardPSCMigrateComplete | A packet processing card migration operation has successfully completed. The first varbind identifies the packet processing card whose tasks are being migrated from; the second varbind identifies the packet processing card where the tasks are being migrated to.
> starCardPSCMigrateFailed | A packet processing card migration operation has failed. The first varbind identifies the packet processing card whose tasks are being migrated from; the second varbind identifies the packet processing card where the tasks are being migrated to.
> starCardSMCSwitchoverStart | An SMC switchover operation has begun. The first varbind identifies the SMC whose tasks are being switched from; the second varbind identifies the SMC where the tasks are being switched to. If a migration is taking place, it is likely that there is a problem with the original SMC.
> starCardSMCSwitchoverComplete | An SMC Switchover has completed successfully. The starSlotNum varbind identifies the new primary SMC.
> starCardSMCSwitchoverFailed | An SMC switchover operation has failed. The first varbind identifies the SMC whose tasks are being switched from; the second varbind identifies the SMC where the tasks are being switched to.

> ‌
> If any of the above traps have been generated, it is likely that an application card needs to be replaced.
> Removing the Application Card
> This section describes how to remove an application card.
> Important: Before you remove and replace an application card on an active system, refer to the System Administration and Configuration Reference for instructions on how to migrate or switch processes and services to a redundant (standby) card.

> Step 1 | Use a Phillips #2 screwdriver to loosen the screws at the top and bottom of the failed application card’s front panel.

> Step 2 | Lower the interlock switch on the front panel of the application card.

> Caution: To minimize the risk of data loss, ensure that all LEDs on the packet processing card are completely off and that SMCs have stopped blinking prior to removing the card from the chassis.

> Step 3 | Pull the ejector levers outward, firmly and straight, until the card is unseated from the chassis.

> Step 4 | Holding the card by its ejector levers, gently slide the card out of the chassis by pulling the card toward you.

> Caution: Do not leave chassis slots uncovered for extended periods of time. This reduces airflow through the chassis and could cause it to overheat. Make sure a card or a blanking panel is installed in every chassis slot at all times.

> Step 5 | Proceed to the Installing the Replacement Application Card section that follows for instructions on installing a new application card.

> Important: If the card just removed from the chassis was an SMC, proceed to the Removing and Replacing the CompactFlash Memory Card section later in this chapter.
> Installing the Application Card
> This section describes how to install an application card.

> Step 1 | Slide the interlock switch on the card fully downward. Flip the ejector levers outward and away from the card’s faceplate.

> Step 2 | Holding the card by its ejector levers, align the card with the upper and lower card guides of the appropriate chassis slot and gently slide the card into the slot until the levers touch the chassis frame.

> Caution: Take extra caution when installing packet processing cards. These cards contain heat sinks that could become loose or damaged if they come into contact with an adjacent card while the packet processing card is being inserted in the chassis slot.
> Important: If you are replacing a PSC with a PSCA in a chassis that contains PSCs, refer to the Chassis Hybrid Mode Operation appendix for additional configuration information.

> Step 3 | Push the ejector levers inward firmly and straight until the card is firmly seated in the chassis midplane and the ejector levers can be pushed in no further. Press firmly on the card’s faceplate to ensure that it is fully seated. The card’s front panel should be flush against the chassis’ upper and lower card mounts for the slot.

> Step 4 | Raise the interlock switch on the front panel of the application card to lock the ejector tab in place. The flange on the left-side of the interlock switch prevents movement of the ejector tab when raised completely.

> Important: The interlock switch must be fully raised in order to properly secure the application card’s top screw to the chassis.

> Step 5 | Use a Phillips #2 screwdriver to tighten the screws at the top and bottom of the application card’s front panel to secure the card.

> Removing and Replacing the CompactFlash Memory Card on SMCs
> SMC cards ship with a CompactFlash memory card that stores configuration files, software images, and session capacity/feature licensing keys for the system. The following figure displays the location of the CompactFlash memory card on the SMC.
> Location of CompactFlash Card
> In the event of an SMC hardware failure, you must remove the CompactFlash from the failed card and install it on the replacement SMC. This ensures that the proper software image, configuration files, and license keys are loaded as the system boots.
> Caution: To reduce the risk of damage, handle the CompactFlash memory card only when necessary as part of the maintenance process.
> Removing and Replacing the CompactFlash on an SMC
> This section provides instructions for the removal of the CompactFlash card from the failed SMC and its safe insertion in the replacement SMC.

> Step 1 | On the failed SMC, remove the card retainer clip that secures the CompactFlash module in the socket by pulling the ends of the card retainer clips out and away from the socket.

> Step 2 | Gently pull the module out of the socket.

> Step 3 | Repeat step 1 and step 2 to remove the module on the replacement SMC.

> Step 4 | Gently insert the module removed in step 1 into the socket on the replacement SMC.

> Step 5 | Replace the card retainer clip to secure the CompactFlash module in place.

> Step 6 | Proceed to the Installing the Replacement Application Card section of this chapter for instructions on installing the replacement SMC.

> What to do with the Failed Application Card
> If the failed application card is still under warranty, return it to the vendor for repair.
> If the failed application card is out of warranty, contact Cisco to determine if it can be sent in for repair at an additional cost.
> Important: Disposal of this product should be performed in accordance with all national laws and regulations.
> Refer to the support area of http://www.cisco.com for up-to-date product documentation pertaining to installation, configuration, and maintenance. A valid username and password is required to use this site. Please contact your local sales or service representative for additional information.
> Important: For addtional information on the RMA process, see the RMA Shipping Procedures appendix.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883