> MAP Schema Statistics
> The MAP (Mobile Application Part [SS7]) schema provides operational statistics that can be used for monitoring and troubleshooting the following products: SCM (E-CSCF)
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the MAP Schema

> Variables | Description | Data Type
> vpnname | Indicates the name of VPN context in which the MAP service is configured. This is a stat key variable. | String
> vpnid | Indicates the identifier of the VPN context in which the MAP service is configured. This is a stat key variable. | Int32
> servname | Indicates the name of the MAP service for which these statistics are collected. This is a stat key variable. | String
> map-open-req-tx | Total number of mobile application part (MAP) open requests sent. | Int32
> map-open-req-rx | Total number of mobile application part (MAP) open requests received. | Int32
> map-open-rsp-tx | Total number of MAP open response sent. | Int32
> map-open-rsp-rx | Total number of MAP open response received. | Int32
> map-close-tx | Total number of MAP close response sent. | Int32
> map-close-rx | Total number of MAP close response received. | Int32
> map-abort-tx | Total number of MAP abort request sent. | Int32
> map-abort-rx | Total number of MAP abort request received. | Int32
> map-auth-req-tx | Description: Total number of Send Authentication Request messages transmitted to HLR. Triggers: Counter increments when a MAP Send Authentication Request is initiated from SGSN. Availability: per MAP service | Int32
> map-auth-succes | Total number of MAP authentication successful. | Int32
> map-auth-fail | Description: Total number of User Error / Provider Error received in response to SAI request. Triggers: Counter increments when User Error / Provider Error is received from HLR. Availability: per MAP service | Int32
> map-auth-timeouts-rcvd | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when there is no response from the HLR for map-auth-fail-rep-req-tx message initiated from SGSN. Availability: per MAP service | Int32
> map-imei-req-tx | Description: Total number of MAP Check IMEI requests initiated towards EIR. Triggers: Counter increments when MAP CHECK IMEI Request is sent. Availability: per MAP service | Int32
> map-imei-succes | Description: Total number of successful responses for MAP Check IMEI requests. Triggers: Counter increments when MAP CHECK IMEI Request is sent. Availability: per MAP service | Int32
> map-imei-fail | Description: Total number of failure responses for MAP Check IMEI requests received from EIR. Triggers: Counter increments when MAP Return Error / Provider Error is received in response. Availability: per MAP service | Int32
> map-imei-timeout | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when there is no response from HLR. Availability: per MAP service | Int32
> map-gprs-update-loc-req-tx | Description: Total number of UGL (GPRS Update Location) request initiated towards HLR. Triggers: Counter increments when UGL request is sent to HLR. Availability: per MAP service | Int32
> map-gprs-update-loc-rsp-tx | Description: Total number of UGL (GPRS Update Location) request initiated towards HLR. Triggers: Counter increments when UGL request is sent to HLR. Availability: per MAP service | Int32
> map-gprs-update-loc-err-tx | Description: Total number of Failure response (User Error/Provider Error) messages received in response to UGL request. Triggers: Counter increments when MAP Return Error / Provider Error is received to UGL request. Availability: per MAP service | Int32
> map-gprs-update-loc- timeouts-rx | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments if there is no response from HLR. Availability: per MAP service | Int32
> map-sub-loc-rpt-req-tx | Description: Total Number of SLR (Subscriber Location Report) request initiated towards GMLC. Triggers: Counter increments when SLR request is sent to GMLC. Availability: per MAP service | Int32
> map-sub-loc-rpt-rsp-tx | Description: Total Number of successful response messages sent in response to SLR request. Triggers: Counter increments when successful response is received from GMLC. Availability: per MAP service | Int32
> map-sub-loc-rpt-err-tx | Description: Total Number of Failure response (User Error/Provider Error) messages received in response to SLR request. Triggers: Counter increments when MAP Return Error/Provider Error is received to SLR request. Availability: per MAP service | Int32
> map-sub-loc-rpt-timeouts-rx | Description: Total Number of timeouts that occurred while waiting for response to SLR request from GMLC. Triggers: Counter increments if there is no response to SLR request from GMLC. Availability: per MAP service | Int32
> map-prov-sub-loc-req-rx | Description: Total Number of PSL (Provide Subscriber Location) request received from GMLC. Triggers: Counter increments when MAP PSL request is received from GMLC. Availability: per MAP service | Int32
> map-prov-sub-loc-rsp-tx | Description: Total Number of successful PSL response messages sent to GMLC. Triggers: Counter increments when successful response is sent to GMLC. Availability: per MAP service | Int32
> map-prov-sub-loc-err-tx | Description: Total Number of error response messages sent to GMLC. Triggers: Counter increments when MAP Return Error is sent to GMLC. Availability: per MAP service | Int32
> map-cancel-loc-req-rx | Description: Total number of Cancel Location Request received from HLR. Triggers: Counter increments when MAP Cancel Location Request is received. Availability: per MAP service | Int32
> map-cancel-loc-rsp-tx | Description: Total number of successful Cancel Location Response messages sent to HLR. Triggers: Counter increments when successful response is sent to HLR. Availability: per MAP service | Int32
> map-cancel-loc-err-tx | Description: Total number of Error response messages sent to HLR. Triggers: Counter increments when MAP Return Error is sent to HLR. Availability: per MAP service | Int32
> map-del-subs-req-rx | Description: Total number of Delete Subscription Data Request received from HLR. Triggers: Counter increments when MAP Delete Subscription Data (DSD) message is received. Availability: per MAP service | Int32
> map-del-subs-rsp-tx | Description: Total number of successful responses for Delete Subscription Data request sent to HLR. Triggers: Counter increments when MAP Delete Subscription Data (DSD) message is received. Availability: per MAP service | Int32
> map-del-subs-ret-tx | Description: Total number of Error responses sent for Delete Subscription Data (DSD) request received. Triggers: Counter increments when failure response is sent to HLR. Availability: per MAP service | Int32
> map-insert-subs-rcvd | Total number of insert subscriber data requests received by MAP. | Int32
> map-standalone-isd-rcvd | Total number of standalone insert subscriber data requests received by MAP. | Int32
> map-isd-rsp-tx | Total number of insert subscriber data requests sent by MAP. | Int32
> map-isd-err-tx | Total number of insert subscriber data failure response sent by MAP. | Int32
> map-auth-fail-rept-req-tx | Description: Total number of Authentication Failure Report Request messages transmitted by MAP. Triggers: Counter increments when a message is initiated to inform HLR that certain vectors had problem in authenticating with the MS. Availability: per MAP service | Int32
> map-auth-fail-rept-rsp-rx | Description: Total number of Authentication Failure Report Request messages received by MAP. Triggers: Counter increments when successful response is received in response to map-auth-fail-rep-req-tx. Availability: per MAP service | Int32
> map-auth-fail-rept-err-rx | Description: Total number of User Error and Provider Error received for the Authentication Failure Report Request sent to HLR. Triggers: Counter increments when MAP Return Error/Provider Error is received in response to map-auth-fail-rep-req-tx message. There will be no effect on the call due to this. Availability: per MAP service | Int32
> map-auth-fail-rept-timeouts-rcvd | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when MAP Return Error / Provider Error is received in response to map-auth-fail-rep-req-tx. There will be no effect on the call due to this. Availability: per MAP service | Int32
> map-purge-req-tx | Description: Total number of MAP Purge Request messages initiated towards HLR. Triggers: Counter increments when MAP Purge Request is transmitted. Availability: per MAP service | Int32
> map-purge-success | Description: Total number of successful MAP Purge Request messages sent to HLR. Triggers: Counter increments when successful response is received from HLR. Availability: per MAP service | Int32
> map-purge-fail | Description: Total number of Failure response received from HLR. Triggers: Counter increments when MAP Return Error / Provider Error is received in response. Availability: per MAP service | Int32
> map-purge-timeouts-rcvd | Description: Total number of timeouts that occurred while waiting for response from HLR. Triggers: Counter increments when there is no response from HLR. Availability: per MAP service | Int32
> map-hlr-reset-rcvd | Total number of HLR reset indicator received by MAP. | Int32
> map-mo-fwd-req-sent | Total number of mobile originated forward request messages sent to MAP. | Int32
> map-mo-fwd-rsp-rcvd | Total number of mobile originated forward response messages received from MAP. | Int32
> map-mo-fwd-rsp-failed | Total number of mobile originated forward response messages failed at MAP. | Int32
> map-mo-fwd-rsp-time-out | Total number of mobile originated forward response messages timed-out at MAP. | Int32
> map-mt-fwd-req-sent | Total number of mobile terminated forward request messages sent to MAP. | Int32
> map-mt-fwd-rsp-rcvd | Total number of mobile terminated forward request messages received from MAP. | Int32
> map-mt-fwd-rsp-failed | Total number of mobile terminated forward response messages failed at MAP. | Int32
> map-ready-for-sm-req | Total number of MAP ready for session management request received. | Int32
> map-ready-for-sm-rsp | Total number of MAP ready for session management request response received. | Int32
> map-ready-for-sm-rsp-failed | Total number of MAP ready for session management requests failed. | Int32
> map-ready-for-sm-rsp-time-out | Total number of MAP ready for session management requests timed-out. | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883