> MSEG Peer Profile Configuration Mode Commands
> This configuration mode enables you to configure non-local Mobile Service Edge Gateway (MSEG) instances in the network. Though this mode is intended to contain peer-MSEG information, there is no restriction on configuring local MSEG instances. Local MSEG service instances will look up this list and the list of local MSEG services whenever necessary.
> Important: This configuration mode is not supported in this release. For more information please contact your Cisco account representative.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> mseg-gtpc
> This command allows you to add/remove MSEG service control addresses in an MSEG peer profile.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> mseg-gtpc ipv4/ipv6_address [ udp-port port_number ]
> no mseg-gtpc
> no
> Deletes the previously configured MSEG GTP-C address from the current MSEG peer profile.
> ipv4/ipv6_address
> Specifies the MSEG GTP-C IP address in IPv4 dotted-decimal or IPv6 colon-separated notation.
> udp-port port_number
> Specifies the UDP port number as an integer from 1 through 65535.
> Usage
> Use this command to add/remove MSEG service control addresses in an MSEG peer profile.
> Example
> The following command configures the MSEG GTP-C address 1.1.1.1 and the UDP port 111 in the current MSEG peer profile:
> mseg-gtpc 1.1.1.1 udp-port 111
> mseg-gtpu
> This command allows you to add/remove MSEG service data addresses in an MSEG peer profile.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] mseg-gtpu ipv4/ipv6_address
> no
> Deletes the specified MSEG GTP-U address from the current MSEG peer profile.
> ipv4/ipv6_address
> Specifies the MSEG GTP-U IP address in IPv4 dotted-decimal or IPv6 colon-separated notation.
> Usage
> Use this command to add/remove MSEG service data addresses in an MSEG peer profile. Multiple GTP-U addresses can be associated with an MSEG instance.
> Example
> The following command configures the MSEG GTP-U address 1.1.1.1 for the current MSEG peer profile:
> mseg-gtpu 1.1.1.1
> mseg-id
> This command allows you to configure the MSEG instance ID in an MSEG peer profile. Note that the MSEG profile is not activated until this ID is configured.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] mseg-id mseg_id
> no
> Deactivates the specified MSEG peer profile.
> mseg_id
> Specifies the MSEG instance ID as n integer from 1 through 65535.
> Usage
> Use this command to configure the MSEG instance ID in an MSEG peer profile.
> This ID must be unique across all MSEG installations in an operator’s domain. The MSEG profile is not activated until this ID is configured.
> Example
> The following command configures the MSEG instance ID in the current MSEG peer profile to 111:
> mseg-id 111

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883