> MSEG Ruleset Configuration Mode Commands
> The MSEG Ruleset Configuration Mode enables you to configure rules to be applied when evaluating whether a session should be offloaded or not.
> Important: This configuration mode is not supported in this release. For more information please contact your Cisco account representative.
> apn
> This command allows you to associate specified APN profile(s) with the rule.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] apn { if-match-profile apn_profile_name | if-no-match-profile apn_profile_name }
> no
> Removes the specified APN rule from the ruleset.
> if-match-profile apn_profile_name
> Specifies name of the APN profile to be applied on match as an alphanumeric string of 1 through 63 characters.
> if-no-match-profile apn_profile_name
> Specifies name of the APN profile to be applied on no match as an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to associate APN profile(s) to the rule, and specify which APN profile must be applied if the APN matches/does not match.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> imei
> This command allows you to associate specified International Mobile Equipment Identity (IMEI) profile(s) with the rule.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] imei { if-match-profile imei_profile_name | if-no-match-profile imei_profile_name }
> no
> Removes the specified IMEI rule from the ruleset.
> if-match-profile imei_profile_name
> Specifies name of the IMEI profile to be applied on match as an alphanumeric string of 1 through 63 characters.
> if-no-match-profile imei_profile_name
> Specifies name of the IMEI profile to be applied on no match as an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to associate IMEI profile(s) to the rule, and specify which IMEI profile must be applied if the subscriber IMEI matches/does not match.
> imsi
> This command allows you to associate specified IMSI profile(s) with the rule.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] imsi { if-match-profile imsi_profile_name | if-no-match-profile imsi_profile_name }
> no
> Removes the specified IMSI rule from the ruleset.
> if-match-profile imsi_profile_name
> Specifies name of the IMSI profile to be applied on match as an alphanumeric string of 1 through 63 characters.
> if-no-match-profile imsi_profile_name
> Specifies name of the IMSI profile to be applied on no match as an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to associate IMSI profile(s) to the rule, and specify which IMSI profile must be applied if the subscriber IMSI matches/does not match.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883