> show pgw
> This chapter describes the output of the show pgw command.
> show pgw-service all
> Displays configuration information for all P-GW services configured on the system.
> show pgw-service all Command Output Descriptions

> Field | Description
> Service name | The name of the P-GW service configured and running on the system.
> Service-ID | The system-generated identification number associated with the P-GW service name.
> Context | The context name where the P-GW service is configured.
> Accounting Context | The context name where the accounting configuration and/or interface(s) are configured.
> Accounting gtpp group | Displays all the configured GTPP server groups associated with this service for accounting.
> Status | Indicates whether the P-GW service is started or not.
> Restart Counter | Specifies the restart counter.
> EGTP Service | The eGTP service name configured for use by this service.
> LMA Service | The LMA service name configured for use by this service.
> GGSN Service | The GGSN service name associated with this service.
> Session-Delete-Delay Timer | Indicates whether there is a delay in terminating a session.
> Session-Delete-Delay Timeout | Specifies the time (msecs) to retain a session before terminating it.
> PLMN ID List | The Public Land Mobile Network identifier list associated with this P-GW service. A PLMN contains a Mobile Country Code (MCC) and Mobile Network Code (MNC). Up to five PLMN IDs can be configured for each P-GW service.
> Newcall Policy | The newcall policy configured for this P-GW service. Specifies whether the P-GW will accept or reject requests for a static IP address if the address is already in use by another session
> dns-client Context Name | The context where the DNS client is configured and used by this service.
> gx-li context | Refer to the Lawful Intercept Configuration Guide.
> gx-li transport | Refer to the Lawful Intercept Configuration Guide.
> QCI-QOS Mapping Table Name | The QoS Class Index to QoS mapping table configured for use with this service.
> Authorize | Enables/disables subscriber session authorization with HSS over S6b Diameter interface.
> Duplicate Subscriber Addr Request | Specifies whether the P-GW will accept or reject requests for a static IP address if the address is already in use by another session.
> Fqdn-name | The name of Fully Qualified Domain Name (FQDN) which is used for authorization over S6b interface between P-GW and 3GPP AAA/HSS.

> ‌
> show pgw-service statistics all
> show pgw-service statistics all Command Output Descriptions

> Field | Description
> PGW Node Level Statistics
> VPN Name | The name of the context in which the P-GW service is configured.
> Total bearers active
> Default bearers | The total number of active default bearers using the P-GW node.
> Non-Emergency | The total number of active default non-emergency bearers using the P-GW node.
> Emergency | The total number of active default emergency bearers using the P-GW node.
> Dedicated bearers | The total number of active dedicated bearers using the P-GW node.
> UE-initiated | The total number of active UE-initiated dedicated bearers using the P-GW node.
> Network-initiated | The total number of active network-initiated dedicated bearers using the P-GW node.
> Non-Emergency | The total number of active non-emergency dedicated bearers using the P-GW node.
> Emergency | The total number of active emergency dedicated bearers using the P-GW node.
> Total bearers setup
> Default bearers | The total number of default bearers set up using the P-GW node.
> Non-Emergency | The total number of default non-emergency bearers set up using the P-GW node.
> Emergency | The total number of default emergency bearers set up using the P-GW node.
> Dedicated bearers | The total number of dedicated bearers set up using the P-GW node.
> UE-initiated | The total number of UE-initiated dedicated bearers set up using the P-GW node.
> Network-initiated | The total number of network-initiated dedicated bearers set up using the P-GW node.
> Non-Emergency | The total number of non-emergency dedicated bearers set up using the P-GW node.
> Emergency | The total number of emergency dedicated bearers set up using the P-GW node.
> Total bearers released
> Default bearers | The total number of default bearers released using the P-GW node.
> Network init release | The total number of default bearers released due to an network-initiated release using the P-GW node.
> MME init release | The total number of default bearers released due to an MME-initiated release using the P-GW node.
> Dedicated bearers | The total number of dedicated bearers released using the P-GW node.
> Network init release | The total number of dedicated bearers released due to an network-initiated release using the P-GW node.
> MME Initiated release | The total number of dedicated bearers released due to an MME-initiated release using the P-GW node.
> Default bearer release | The total number of dedicated bearers released due to a default bearer release using the P-GW node.
> Total bearers release failure
> Default bearers | The total number of default bearer release failures using the P-GW node.
> Dedicated bearers | The total number of dedicated bearer release failures using the P-GW node.
> Total bearers rejected
> Default bearers | The total number of default bearers rejected using the P-GW node.
> Dedicated bearers | The total number of dedicated bearers rejected using the P-GW node.
> UE-req reject | The total number of UE-requested bearers rejected using the P-GW node.
> Network-req reject | The total number of network-requested bearers rejected using the P-GW node.
> Total Emergency default bearer rejected | The total number of emergency default bearer rejected using the P-GW node.
> Total Emergency dedicated bearers rejected | The total number of emergency dedicated bearer rejected using the P-GW node.
> Total bearers modified
> UE-initiated mod | The total number of UE-initiated bearers modified using the P-GW node.
> Network-initiated mod | The total number of network-initiated bearers modified using the P-GW node.
> Total bearers modification failure
> UE-initiated mod fail | The total number of UE-initiated bearer modification failures using the P-GW node.
> Network-initiated mod fail | The total number of network-initiated bearer modification failures using the P-GW node.
> Subscriber session statistics
> Total bearers active
> Default bearers | The total number of active default bearers using the P-GW service(s) on this system.
> Dedicated bearers | The total number of active dedicated bearers using the P-GW service(s) on this system. This counter increments for both network and UE-initiated dedicated bearers.
> Total bearers setup
> Default bearers | The total number of default bearers setup using the P-GW service(s) on this system.
> Dedicated bearers | The total number of dedicated bearers setup using the P-GW service(s) on this system. This counter increments for both network and UE-initiated dedicated bearer setup.
> Total bearers released
> Default bearers | The total number of default bearers released using the P-GW service(s) on this system.
> Network initiated release
> Admin disconnect | The total number of default bearers released due to an administrative disconnect using the P-GW service(s) on this system.
> GTP-U error ind | The total number of default bearers released due to a GTP-U error indication using the P-GW service(s) on this system.
> SGW Path failure | The total number of default bearers released due to an S-GW path failure using the P-GW service(s) on this system.
> MME Initiated release | The total number of default bearers released due to an MME initiated release using the P-GW service(s) on this system.
> Dedicated bearers | The total number of dedicated bearers released using the P-GW service(s) on this system.
> Network initiated release
> Admin disconnect | The total number of dedicated bearers released due to an administrative disconnect using the P-GW service(s) on this system.
> GTP-U error ind | The total number of dedicated bearers released due to a GTP-U error indication using the P-GW service(s) on this system.
> MME initiated release | The total number of dedicated bearers released due to an MME initiated release using the P-GW service(s) on this system.
> Default bearer release | The total number of dedicated bearers released due to a default bearer release using the P-GW service(s) on this system.
> Total bearers release failure
> Default bearers | The total number of default bearer release failures using the P-GW service(s) on this system.
> Dedicated bearers | The total number of dedicated bearer release failures using the P-GW service(s) on this system.
> Total bearers rejected:
> Default bearers | The total number of default bearers rejected using the P-GW service(s) on this system.
> No Resource | The total number of default bearers rejected due to a no resource condition using the P-GW service(s) on this system.
> Missing or unknown APN | The total number of default bearers rejected due to a missing or unknown APN using the P-GW service(s) on this system.
> APN selection-Mode mismatch | The total number of default bearers rejected due to an APN selection mode mismatch using the P-GW service(s) on this system.
> Pref PDN-Type not supported | The total number of default bearers rejected due to a preferred PDN type not supported condition using the P-GW service(s) on this system.
> APN restr violation | The total number of default bearers rejected due to an APN restriction violation using the P-GW service(s) on this system.
> Subs auth failed | The total number of default bearers rejected due to a subscriber authentication failure using the P-GW service(s) on this system.
> Subs static addr not allowed | The total number of default bearers rejected due to a disallowed subscriber static IP address using the P-GW service(s) on this system.
> Subs static addr not alloc | The total number of default bearers rejected due to an unallocated subscriber static IP address using the P-GW service(s) on this system.
> Dynamic addr not alloc | The total number of default bearers rejected due to an unallocated dynamic IP address using the P-GW service(s) on this system.
> Subs static addr not present | The total number of default bearers rejected due to a missing subscriber static IP address using the P-GW service(s) on this system.
> Dedicated bearers | The total number of dedicated bearers rejected using the P-GW service(s) on this system.
> UE-req reject | The total number of UE-requested dedicated bearers rejected using the P-GW service(s) on this system.
> Network-req reject | The total number of network-requested dedicated bearers rejected using the P-GW service(s) on this system.
> Total bearers modified
> UE-initiated modification | The total number of UE-initiated bearers modified using the P-GW service(s) on this system.
> QOS modification | The total number of UE-initiated bearers with a QoS modification using the P-GW service(s) on this system.
> TFT modification | The total number of UE-initiated bearers with a TFT modification using the P-GW service(s) on this system.
> Network-initiated modification | The total number of network-initiated bearers modified using the P-GW service(s) on this system.
> QOS modification | The total number of network-initiated bearers with a QoS modification using the P-GW service(s) on this system.
> TFT modification | The total number of network-initiated bearers with a TFT modification using the P-GW service(s) on this system.
> Total bearers modification failure
> UE-initiated mod failed | The total number of UE-initiated bearer modification failures using the P-GW service(s) on this system.
> QOS mod fail | The total number of UE-initiated bearer modification failures due to QoS modification failures using the P-GW service(s) on this system.
> Semantic err in TFT oper | The total number of UE-initiated bearer modification failures due to semantic errors in a TFT operation using the P-GW service(s) on this system.
> Syntact err in TFT oper | The total number of UE-initiated bearer modification failures due to syntactic errors in a TFT operation using the P-GW service(s) on this system.
> Semantic err in pkt filter | The total number of UE-initiated bearer modification failures due to semantic errors in a packet filter using the P-GW service(s) on this system.
> Syntact err in pkt filter | The total number of UE-initiated bearer modification failures due to syntactic errors in a packet filter using the P-GW service(s) on this system.
> Network-initiated mod failed | The total number of network-initiated bearer modification failures using the P-GW service(s) on this system.
> QOS mod fail | The total number of network-initiated bearer modification failures due to QoS modification failures using the P-GW service(s) on this system.
> Semantic err in TFT oper | The total number of network-initiated bearer modification failures due to semantic errors in a TFT operation using the P-GW service(s) on this system.
> Syntact err in TFT oper | The total number of network-initiated bearer modification failures due to syntactic errors in a TFT operation using the P-GW service(s) on this system.
> Semantic err in pkt filter | The total number of network-initiated bearer modification failures due to semantic errors in a packet filter using the P-GW service(s) on this system.
> Syntact err in pkt filter | The total number of network-initiated bearer modification failures due to syntactic errors in a packet filter using the P-GW service(s) on this system.
> Total PDN-Type stats
> PDN-Type IPv4 sessions | The total number of PDN-type IPv4 sessions using the P-GW service(s) on this system.
> Active | The total number of active PDN-type IPv4 sessions using the P-GW service(s) on this system.
> Setup | The total number of setup PDN-type IPv4 sessions using the P-GW service(s) on this system.
> Released | The total number of released PDN-type IPv4 sessions using the P-GW service(s) on this system.
> PDN-Type IPv6 sessions | The total number of PDN-type IPv6 sessions using the P-GW service(s) on this system.
> Active | The total number of active PDN-type IPv6 sessions using the P-GW service(s) on this system.
> Setup | The total number of setup PDN-type IPv6 sessions using the P-GW service(s) on this system.
> Released | The total number of released PDN-type IPv6 sessions using the P-GW service(s) on this system.
> PDN-Type IPv4v6 sessions | The total number of PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
> Active | The total number of active PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
> Setup | The total number of setup PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
> Released | The total number of released PDN-type IPv4v6 sessions using the P-GW service(s) on this system.
> IP address allocation statistics
> Total IPv4 addrs allocated | The total number of IPv4 addresses allocated using the P-GW service(s) on this system.
> Local pool add assign | The total number of local IP pool IPv4 addresses allocated using the P-GW service(s) on this system.
> Static addr assign | The total number of static IPv4 addresses allocated using the P-GW service(s) on this system.
> Radius provided addr assign | The total number of RADIUS-provided IPv4 addresses allocated using the P-GW service(s) on this system.
> Total IPv6 addrs allocated | The total number of IPv6 addresses allocated using the P-GW service(s) on this system.
> Stateless auto config | The total number of stateless address auto configuration IPv6 addresses allocated using the P-GW service(s) on this system.
> SGi tunneling statistics
> Total IPv4 tunnel sessions | The total number of IPv4 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> IP-in-IP tun sessn active | The total number of active IP-in-IP tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> IP-in-IP tun sessions setup | The total number of setup IP-in-IP tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> IP-in-IP tun sessions released | The total number of released IP-in-IP tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> GRE-tun sessions active | The total number of active GRE tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> GRE-tun sessions setup | The total number of setup GRE tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> GRE-tun session release | The total number of released GRE tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> Total IPv6 tunneled sessions | The total number of IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> 6to4 tun sessions active | The total number of active IPv4-in-IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> 6to4 tun session setup | The total number of setup IPv4-in-IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> 6to4 tun sessions released | The total number of released IPv4-in-IPv6 tunnel sessions using the P-GW service(s) SGi interface(s) on this system.
> Subscriber PLMN Statistics
> Home subscribers sessions | The total number of home subscriber sessions using the P-GW service(s) on this system.
> Sessions active | The total number of active home subscriber sessions using the P-GW service(s) on this system.
> Sessions setup | The total number of setup home subscriber sessions using the P-GW service(s) on this system.
> Sessions released | The total number of released home subscriber sessions using the P-GW service(s) on this system.
> Roaming subscribers sessions | The total number of roaming subscriber sessions using the P-GW service(s) on this system.
> Sessions active | The total number of active roaming subscriber sessions using the P-GW service(s) on this system.
> Sessions setup | The total number of setup roaming subscriber sessions using the P-GW service(s) on this system.
> Sessions released | The total number of released roaming subscriber sessions using the P-GW service(s) on this system.
> Visiting subscribers sessions | The total number of visiting subscriber sessions using the P-GW service(s) on this system.
> Sessions active | The total number of active visiting subscriber sessions using the P-GW service(s) on this system.
> Sessions setup | The total number of setup visiting subscriber sessions using the P-GW service(s) on this system.
> Sessions released | The total number of released visiting subscriber sessions using the P-GW service(s) on this system.
> Subscriber QoS Statistics
> Total bearers active
> QCI 1 - 9 | The total number of active bearers with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of active bearers with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of active bearers with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total bearers setup
> QCI 1 - 9 | The total number of setup bearers with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of setup bearers with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of setup bearers with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total bearers released
> QCI 1 - 9 | The total number of released bearers with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of released bearers with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of released bearers with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Subscriber Data Statistics
> Total Uplink packets forwarded
> QCI 1 - 9 | The total number of uplink packets forwarded with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of uplink packets forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of uplink packets forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total Uplink bytes forwarded
> QCI 1 - 9 | The total number of uplink bytes forwarded with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of uplink bytes forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of uplink bytes forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total Downlink packets forwarded
> QCI 1 - 9 | The total number of downlink packets forwarded with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of downlink packets forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of downlink packets forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total Downlink bytes forwarded
> QCI 1 - 9 | The total number of downlink bytes forwarded with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of downlink bytes forwarded with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of downlink bytes forwarded with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total Uplink packets dropped
> QCI 1 - 9 | The total number of uplink packets dropped with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of uplink packets dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of uplink packets dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total Uplink bytes dropped
> QCI 1 - 9 | The total number of uplink bytes dropped with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of uplink bytes dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of uplink bytes dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total Downlink packets dropped
> QCI 1 - 9 | The total number of downlink packets dropped with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of downlink packets dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of downlink packets dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.
> Total Downlink bytes dropped
> QCI 1 - 9 | The total number of downlink bytes dropped with a QoS Class Index using the P-GW service(s) on this system.
> Non-Std QCI (Non-GBR) | The total number of downlink bytes dropped with a non-standard QCI (non-GBR) using the P-GW service(s) on this system.
> Non-Std QCI (GBR) | The total number of downlink bytes dropped with a non-standard QCI (GBR) using the P-GW service(s) on this system.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883