> show pcc-policy
> This chapter describes the output of the show pcc-policy command.
> show pcc-policy service all
> show pcc-policy service all Command Output Description

> Field | Description
> Service name | Indicates the name of the PCC-Policy service instancefor which counters are displayed.
> Context name | Indicates the name of the context in which the PCC-Policy service instance is configured and running.
> Service State | Displays the state of PCC-Policy service instance on an IPCF node. Possible states are:
> • | Initial
> • | Connected
> • | Disconnected
> Diameter | This group displays information of Diameter configuration parameters configured in this PCC-Policy service instance.
> Origin | Indicates the name of the Diameter origin host configured in this PCC-Policy service instance.
> Dictionary | Indicates the Diameter dictionary configured and used for Diameter session (Gx) in this PCC-Policy service instance.
> Associate PCC-Service | Indicates the name of the PCC service which is associated with this PCC-Policy service instance.
> Max Policy Sessions | Indicates the maximum limit of policy (Gx) sessions allowed in this PCC-Policy service instance.
> Newcall Policy | Indicates the action configured when new calls arrived after reaching a threshold limit in this PCC-Policy service instance to manage the congestion control. If configured possible actions are:
> • | drop
> • | reject
> GPRS-Access-BCM | Indicates the Bearer Control Mode configured in PCC-Policy service instance to access the PCEF in GPRS network. If configured possible modes are:
> • | as-requested: the PCC-Policy service is configured to accept the BCM request from Application Server (AS) for PCEF access over Gx interface on IPCF node. This is the default mode.
> • | ue-nw: the PCC-Policy service is configured to accept the BCM request from UE and/or network element for PCEF access over Gx interface on IPCF node.
> • | ue-only: the PCC-Policy service is configured to accept the BCM request from UE only for PCEF access over Gx interface on IPCF node.
> eHRPD-Access-BCM | Indicates the Bearer Control Mode configured in PCC-Policy service instance to access the PCEF in eHRPD network. If configured possible modes are:
> • | as-requested: the PCC-Policy service is configured to accept the BCM request from Application Server (AS) for PCEF access over Gxa interface on IPCF node. This is the default mode.
> • | ue-nw: the PCC-Policy service is configured to accept the BCM request from UE and/or network element for PCEF access over Gxa interface on IPCF node.
> • | ue-only: the PCC-Policy service is configured to accept the BCM request from UE only for PCEF access over Gxa interface on IPCF node.
> Subscriber Binding ID | Indicatges the subscriber binding identifier used by bindmux for binding subscriber session to PCC-Policy service instance.If configured possible binding identifiers are:
> • | IMSI
> • | MSISDN
> • | NAI
> • | SIP-URI
> Subscription-ID Absence Action | Indicatges the action configured for PCC Policy when CCR-I message is received by IPCF/PCRF without a valid Subscription id (IMSI, NAT, E164 etc.). Possible actions are:
> • | Continue
> • | Reject

> ‌
> show pcc-policy service statistics
> show pcc-policy service statistics Command Output Description

> Field | Description
> Total Services | Indicates the total number of PCC-Policy services for which counters are displayed.
> Messages Statistics | This group displays the summary statistics of messages in a PCC Policy service instance.
> Total Messages Recv | Indicates total number of inbound messages received (CCR + RAA).
> Total Messages sent | Indicates total number of outbound messages sent (CCA + RAR).
> Total CCR | Indicates total number of known (I/U/T) and unknown CCR received.
> CCR-Initial | Indicates total number of CCR-I messages received.
> CCR-Updates | Indicates total number of CCR-U messages received.
> CCR-Terminate | Indicates total number of CCR-T messages received..
> Unknown CCR | Indicates total number of CCR messages received with type not determined.
> Total CCA | Indicates total number of known (I/U/T) and unknown CCA sent..
> CCA-Initial | Indicates total number of CCA-I messages sent.
> CCA-Updates | Indicates total number of CCA-U messages sent.
> CCA-Terminate | Indicates total number of CCA-T messages sent.
> Unknown CCA | Indicates total number of CCA messages sent as response to CCR with type not determined..
> CCA with Success | Indicates total number of CCA messages sent with Result-Code as DIAMETER_SUCCESS(2001).
> CCA-I with Success | Indicates total number of CCA-I messages sent with Result-Code as DIAMETER_SUCCESS(2001).
> CCA-U with Success | Indicates total number of CCA-U messages sent with Result-Code as DIAMETER_SUCCESS(2001).
> CCA-T with Success | Indicates total number of CCA-T messages sent with Result-Code as DIAMETER_SUCCESS(2001).
> CCA with Failures | Indicates total number of CCA messages rejected.
> CCA-I with Failures | Indicates total number of CCA-I messages rejected.
> CCA-U with Failures | Indicates total number of CCA-U messages rejected.
> CCA-T with Failures | Indicates total number of CCA-T messages rejected.
> Total RAA | Indicates total RAA messages received.
> Total RAR | Indicates total RAR messages sent.
> RAA with Sucesss | Indicates total RAA messages with Result-Code or Experimental-Result-Code as SUCCESS..
> RAA with Failure | Indicates total RAA messages with Result-Code or Experimental-Result-Code depicting FAILURE..
> RAA without Result | Indicates total RAA messages with both Result-Code or Experimental-Result-Code absent..
> Unexpected RAA | Indicates total RAA messages for the non-existing sessions.
> RAA parse Sucesss | Indicates total RAA messages with parsing SUCCESS..
> RAA parse Failure | Indicates total RAA messages with parsing FAILURE.
> Reauth probes | Indicates total RAA messages with reauthorization triggers for subscriber session due to expiry idle timeout timer.
> RAR for Sess Release | Indicates total RAR message with Session Release-Cause.
> Unspecified | Indicates total RAR message with Session Release-Cause AVP as UNSPECIFIED (0).
> UE-subscription-Reason | Indicates total RAR message with Session Release-Cause AVP as UE_SUBSCRIPTION_CHANGED (1).
> Insuff Server Resources | Indicates total RAR message with Session Release-Cause AVP as INSUFFICIENT_SERVER_RESOURCES (2).
> Total RAR Timeouts | Indicates total RAR messages for which no RAA response was received from PCEF.
> Update RAR Timeouts | Indicates total Timed-out RAR messages which were sent by PCRF for session updates (e.g. RAR with new / modified PCC rules / QoS).
> Release RAR Timeouts | Indicates total Timed-out RAR messages which were sent by PCRF for session termination (RAR with Session-Release-Cause AVP).
> Session-Level Statistics | This group displays the session level statistics of messages in a PCC Policy service instance.
> Current Sessions | Indicates the session counter which keeps track of existing sessions under this PCC-Policy service.
> Total Session Created | Indicates cumulative number of sessions created at the PCC-Policy service.
> Total Session Updates | Indicates cumulative number of sessions updates at the PCC-Policy service. This will include both PCRF-initiated and PCEF initiated updates.
> PCEF-Initiated | Indicates cumulative number of PCEF-initiated sessions updates at the PCC-Policy service. This will include session updates through CCR-U message.
> PCRF-Initiated | Indicates cumulative number of PCRF-initiated sessions updates at the PCC-Policy service. This will include session updates through RAR.
> Total Session Deleted | Indicates cumulative number of session deletion at the PCC-Policy service.
> PCEF-Initiated | Indicates cumulative number of PCEF-initiated session terminations at the PCC-Policy service initiated through CCR-T message.
> PCRF-Initiated | Indicates cumulative number of PCRF-initiated session termination at the PCC-Policy service initiated through RAR messages with Session-Release-Cause AVP.
> Peer Down Initiated | Indicates cumulative number of sessions terminations due to peer disconnect at the PCC-Policy service..
> Initial Reject | Indicates cumulative number of sessions terminations at the PCC-Policy service initiated through CCR-I rejection.
> Idle Timeout | Indicates the idle session timeout duration set for a subscriber session timer. Possible range of duration is 1 to 4294967295 in seconds. Special value of 0 indicates that timer is disabled and it is the default behavior.
> Setup Timeout | Indicates IPCF setup timeout duration set on a system for setup timer. Possible range of duration is 1 to 120 in seconds. By default Setup timeout value is 60 seconds. Special value of 0 indicates that timer is disabled.
> Long-duration Timeout | Indicates the long duration idle session timeout set for a subscriber session timer. Possible range of duration is 1 to 4294967295 in seconds. Special value of 0 indicates that timer is disabled and it is the default behavior.
> Failure Statistics | This group displays the statistics of various failure reasons in a PCC Policy service instance.
> Missng CCR-Type | Indicates total number of CCR messages with mandatory CC-Request-Type AVP missing.
> Unexpected CCR-I | Indicates total number of CCR-I message for existing session.
> Unexpected CCR-U | Indicates total number of CCR-U message for non-existing session.
> Unexpected CCR-T | Indicates total number of CCR-T message for non-existing session.
> Missng CCR-Num | Indicates total number of CCR messages with mandatory CC-Request-Number missing.
> Out-of-Order CCR | Indicates total number of CCR messages with out-of-order CC-Request-Number.
> PCC-Sess Create Fail | Indicates total number of PCC Session Creation Failure after receiving CCR-I due to miscellaneous reasons.
> Policy-Sess Create Fail | Indicates total number of PCC Policy Session Creation Failure after receiving CCR-I due to miscellaneous reasons.
> PCC-Sess Lookup Fail | Indicates total number of PCC Session Creation Failure after receiving CCR-U/T due to miscellaneous reasons.
> Policy-Sess Lookup Fail | Indicates total number of PCC Policy Session Creation Failure after receiving CCR-U/T due to miscellaneous reasons.
> Missing Origin-Host | Indicates total number of CCR messages with mandatory Origin-Host AVP missing.
> Invalid Origin-Host | Indicates total number of CCR messages with mandatory Origin-Host AVP invalid.
> Missing Origin-Realm | Indicates total number of CCR messages with mandatory Origin-Realm AVP missing.
> Invalid Origin-Realm | Indicates total number of CCR messages with mandatory Origin-Realm AVP invalid.
> Missing Dest-Realm | Indicates total number of CCR messages with mandatory Destination-Realm AVP missing.
> Invalid Dest-Realm | Indicates total number of CCR messages with mandatory Destination-Realm AVP invalid.
> Unsubscribed Triggers | Indicates total number of Event-Trigger received from PCEF for which PCRF has not subscribed (E.g. RAT_CHANGE received from PCEF even though it is not supplied previously by PCRF).
> Unknwown Triggers | Indicates total number of Event-Trigger received from PCEF which is undefined for the policy version. (E.g. Defaul-EPS-Bearer-QoS-Change received for R7-Gx).
> Non-Applicable Triggers | Indicates total number of Event-Trigger received from PCEF which is not applicable for the access-type. (E.g. Defaul-EPS-Bearer-QoS-Change received for R8 GGSN with 3GPP-GPRS access).
> Missing Trigger-Param | Indicates total number of Event-Trigger received from PCEF without the related parameter (E.g. PCEF sending RAT_CHANGE without the RAT-Type value).
> Invalid Trigger-Param | Indicates total number of Event-Trigger received from PCEF with invalid related parameter (E.g. PCEF sending RAT_CHANGE by RAT-Type reported is same as previous one).
> Event-Trigger in CCR-I | Indicates total number of Event-Trigger received from PCEF in CCR-I message.
> Event-Trigger in CCR-T | Indicates total number of Event-Trigger received from PCEF in CCR-T message.
> Invalid BCM Request | Indicates total number of failure cases where PCEF requests bearer control mode (BCM) as UE-ONLY by sending Network-Request-Not-Supported in CCR-I. However, operator configured BCM is UE-NW. Thus, BCM is not provisioned and PCRF rejects this CCR.
> QoS-Auth Fail | Indicates total number of failure when PCRF rejects the CCR in case of QoS-authorization failure in CCR-I message.
> Invalid Initial Param | Indicates total number of failure when PCRF rejects the CCR with Experimental Result-Code DIAMETER_ERROR_INITIAL_PARAMETERS due to incorrect information in the request.
> Invalid AVP Value | Indicates total number of failure when PCRF rejects the CCR with Result-Code DIAMETER_INVALID_AVP_VALUE due to incorrect AVP value in the request.
> Unsupported AVP | Indicates total number of failure when PCRF rejects the CCR with Result-Code DIAMETER_AVP_UNSUPPORTED due to incorrect AVP value in the request.
> Missing AVP | Indicates total number of failure when PCRF rejects the CCR with Result-Code DIAMETER_MISSING_AVP due to incorrect AVP value in the request.
> Session-Linking Failurre | Indicates total number of failure when PCRF rejects the CCR-I with Result-Code DIAMETER_AUTHORIZATION_REJECTED due to Session Linking failure.
> Unavail Srv Credits | Indicates total number of session failure due to unavailability of enough service credits for PCC-Policy Session creation.
> Multiple Policy Sess Reject | Indicates total number of session rejection due to no-support for multiple PCC session per subscriber available but attempted by PCEF.
> Diameter Statistics | This group displays the statistics of various Diameter interface messages in a PCC Policy service instance.
> App Register Success | Indicates total number of successful diabase registrations at this PCC-Policy service due to service addition.
> App Register Fail | Indicates total number of failed diabase registrations performed at this PCC-Policy service due to service addition.
> App Unregister Success | Indicates total number of successful diabase deregistration at this PCC-Policy service due to service removal.
> App Unregister Fail | Indicates total number of failed diabase deregistration performed at this PCC-Policy service due to service removal.
> App Reregister Success | Indicates total number of successful diabase re-registrations at this PCC-Policy service due to service modification.
> App Reregister Fail | Indicates total number of failed diabase registrations performed at this PCC-Policy service due to service modification.
> Total Msg Create Fail | Indicates total number of failure to create diabase messages for CCA and RAR.
> CCA Create Fail | Indicates total number of failure to create diabase messages for CCA.
> RAR Create Fail | Indicates total number of failure to create diabase messages for RAR.
> Total Msg Encode Fail | Indicates total number of failure to encode diabase message AVP for CCA and RAR.
> CCA Encode Fail | Indicates total number of failure to encode diabase message AVP for CCA.
> RAR Encode Fail | Indicates total number of failure to encode diabase message AVP for RAR.
> Total Msg Send Fail | Indicates total number of failure to send diabase messages for CCA and RAR.
> CCA Send Fail | Indicates total number of failure to send diabase messages for CCA.
> RAR Send Fail | Indicates total number of failure to send diabase messages for RAR.
> Termination Cause Statistics | This group displays the statistics of various causes for session termination in a PCC Policy service instance.
> Diameter Logout | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_LOGOUT (1).
> Serv | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_SERVICE_NOT_PROVIDED (2).
> Bad Answer | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_BAD_ANSWER (3).
> Administrative | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_ADMINISTRATIVE (4).
> Link Broken | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_LINK_BROKEN (5).
> Auth Expired | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_AUTH_EXPIRED (6).
> User Moved | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_USER_MOVED (7).
> Session Timeout | Indicates total number of session termination happened due to CCR-T with Termination-Cause AVP set to value DIAMETER_SESSION_TIMEOUT (8).
> Rule Report Statistics | This group displays the statistics of various Rule Reports in a PCC Policy service instance.
> Total Rules Reports | Indicates total number of rule-reports received for various PCC/QoS rules.
> Total Install Failures | Indicates total number of rule-reports received for various PCC/QoS rule installation failures.
> Total Install Success | Indicates total number of rule-reports received for various successful PCC rule installation.
> Total Credit Exhaustion | Indicates total number of rule-reports received for various PCC rule out-of-credit.
> Total Credit Reallocs | Indicates total number of rule-reports received for various PCC rule credit reallocation.
> Unknown Rule-Names | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as UNKNOWN_RULE_NAME (1).
> Rating Group Errors | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as RATING_GROUP_ERROR (2).
> Service-ID Errors | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as SERVICE_IDENTIFIER_ERROR (3).
> GW-PCEF Malfunctions | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as GW/PCEF_MALFUNCTION (4).
> Resource Limitations | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as RESOURCES_LIMITATIONS (5).
> Max-NR-Bearers Reached | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as MAX_NR_BEARERS_REACHED (6).
> Unknown Bearer ID | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as UNKNOWN_BEARER_ID (7).
> Missing BearerID | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as MISSING_BEARER_ID (8).
> Missing Flow-Desc | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as MISSING_FLOW_DESCRIPTION (9).
> Resource Alloc Fail | Indicates total number of rule-reports received for valrious PCC rule installation failures with Rule-Failure-Code as RESOURCE_ALLOCATION_FAILURE (10).
> QoS Validation Fail | Indicates total number of rule-reports received for various PCC rule installation failures with Rule-Failure-Code as UNSUCCESSFUL_QOS_VALIDATION (11).
> Usage Statistics | This group displays the usage statistics in a PCC Policy service instance.
> Total Usage Thresholds | Indicates total number of usage thresholds supplied to PCEF for various monitoring instances.
> Rule-Level Thresholds | Indicates total number of PCC-Rule-Level usage thresholds supplied to PCEF for various monitoring instances.
> Sess-Level Thresholds | Indicates total number of Session-Level usage thresholds supplied to PCEF for various monitoring instances.
> Rule-Level Report Req | Indicates total number of PCRF initiated PCC-Rule-Level usage report requests supplied to PCEF for various monitoring instances.
> Sess-Level Report Req | Indicates total number of PCRF initiated session-level usage report requests supplied to PCEF for various monitoring instances.
> Rule-Level Disable Requests | Indicates total number of PCRF initiated PCC-Rule-level usage report disable requests supplied to PCEF for various monitoring instances.
> Sess-Level Disable Req | Indicates total number of PCRF initiated session-level usage report disable requests supplied to PCEF for various monitoring instances.
> SPR Statistics | This group displays the statistics related to SSC/SPR instances and procedures associated with a PCC Policy service instance.
> Profile Register | Indicates total messages sent to SPR for Subscriber Profile Registration.
> Profile Deregister | Indicates total messages sent to SPR for Subscriber Profile Deregistration.
> Usage Register | Indicates total messages sent to SPR for Subscriber Usage Registration.
> Usage Deregister | Indicates total messages sent to SPR for Subscriber Usage Deregistration.
> Usage Updates | Indicates total messages sent to SPR for Subscriber Usage Update.

> ‌
> show pcc-policy session full all
> show pcc-policy session full all Command Output Description

> Field | Description
> Callid | Indicates the identity number of the IP-CAN call registered on the PCC-Policy service instancefor which counters are displayed.
> Session ID | Indicates the identity number of the IP-CAN session active on the PCC-Policy service instancefor which counters are displayed.
> Peer ID | Indicates the identity number (IP address) of the PCEF node used in IP-CAN session within the PCC-Policy service instancefor which counters are displayed.
> Service Name | Indicates the name of the PCC-Policy service instancefor which counters are displayed.
> Service Type | Indicates the type of IP-CAN session on the PCC-Policy service instancefor which counters are displayed.
> IMSI | Indicatges the IMSI number of subscriber used by bindmux for binding subscriber session to PCC-Policy service instance.
> MSISDN | Indicatges the MSISDN number of subscriber used by bindmux for binding subscriber session to PCC-Policy service instance.
> APN Name | Indicates the name of the APN used by IP-CAN session to serve subscriber in the PCC-Policy service instance.
> IMEI | Indicates the IMEI number of UE used by bindmux for binding subscriber session to PCC-Policy service instance.
> Session State | Indicates the state of the IP-CAN session on PCC-Policy service instance. Possible states are:
> • | Initial
> • | Connected
> • | Disconnected
> Framed-IPv4 | Indicates the IPv4 address, if used, for frame route relay prefix in IP-CAN session on PCC-Policy service instance.
> Framed-IPv6 | Indicates the IPv6 address, if used, for frame route relay prefix in IP-CAN session on PCC-Policy service instance.
> RAT-Type | Indicates the Radio Access Type used for this IP-CAN session. Possible RAT types are:
> • | UTRAN
> • | E-UTRAN
> • | GPRS
> SGSN_MCC | Indicates the Mobile Country Code used in IP-CAN session on PCC-Policy service instance.
> SGSN_MNC | Indicates the Mobile Network Code used in IP-CAN session on PCC-Policy service instance.
> IP-CAN-Type | Indicates the type of IP-CAN session active on PCC-Policy service instance.
> BCM | Indicates the Bearer Control Mode configured in PCC-Policy service instance to access the PCEF in GPRS/eHRPD network. If configured possible modes are:
> • | as-requested: the PCC-Policy service is configured to accept the BCM request from Application Server (AS) for PCEF access over Gx interface on IPCF node. This is the default mode.
> • | ue-nw: the PCC-Policy service is configured to accept the BCM request from UE and/or network element for PCEF access over Gx interface on IPCF node.
> • | ue-only: the PCC-Policy service is configured to accept the BCM request from UE only for PCEF access over Gx interface on IPCF node.
> ANC-Address | Indicates the IP address of the Access Network Controller node of the IP-CAN session on the PCC-Policy service instancefor which counters are displayed.
> ANC-Identifier | Indicates the identity number of the Access Network Controller node used in IP-CAN session within the PCC-Policy service instancefor which counters are displayed.
> Event-Trigger | Indicates the event triggers configured/activated for IP-CAN session within the PCC-Policy service instancefor which counters are displayed.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883