> BCMCS Schema Statistics
> The BCMCS schema provides operational statistics that can be used for monitoring and troubleshooting the following products: PDSN
> This schema provides the following types of statistics:

> • | Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached.

> • | All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed.

> • | The limit depends upon the data type.

> • | Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.

> • | Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

> The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

> • | Int32/Int64: An integer, either 32-bit or 64-bit:

> • | For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295.

> • | For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.

> • | Float: A numeric value that can be represented fractionally; for example, 1.345.

> • | String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

> Important: Unless otherwise indicated, all statistics are counters and all statistics are standards-based.
> Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
> Bulk Statistic Variables in the BCMCS Schema

> Variables | Description | Data Type
> vpnname | Description: The name of the context configured on the system that is currently facilitating the BCMCS configuration. This is a key variable. | String
> vpnid | Description: The identification number of the context configured on the system that is currently facilitating the BCMCS configuration. This is an internal reference number. This is a key variable. | Int32
> servname | Description: The name of the BCMCS service for which the statistics are displayed. This is a key variable. | String
> srsp-recv-total | Description: This proprietary counter indicates the total number of A11-BC service requests received by PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Service Request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-accept-total | Description: This proprietary counter indicates the total number of A11-BC service requests accepted by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Service Request is accepted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-denied-total | Description: This proprietary counter indicates the total number of A11-BC service requests denied by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Service Request is denied by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-reply-total | Description: This proprietary counter indicates the total number of A11-BC service responses sent by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Service Request is sent by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-discard-total | This proprietary counter indicates the total number of A11-BC service requests discarded by the PDSN service acting as the BSN.Triggers: Triggers: - Incremented when an A11-BC Service Request is discarded by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-accept-initial | Description: This proprietary counter indicates the total number of initial A11-BC service requests received and accepted by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Service Request is received and accepted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-recv-initial | Description: This proprietary counter indicates the total number of initial A11-BC service requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Service Request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-denied-initial | Description: This proprietary counter indicates the total number of initial A11-BC service requests received and rejected by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Service Request is received and rejected by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-discard-initial | Description: This proprietary counter indicates the total number of initial A11-BC service requests discarded by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Service Request is discarded by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-accept-renew | Description: This proprietary counter indicates the total number of renewal A11-BC service requests received and accepted by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Service Request is received and accepted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-denied-renew | Description: This proprietary counter indicates the total number of renewal A11-BC service requests received and denied by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Service Request is received and denied by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-recv-renew | Description: This proprietary counter indicates the total number of renewal A11-BC service requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Service Request is received by the PDSN service.Availability: per PDSN service, per PCF, per session Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-discard-renew | Description: This proprietary counter indicates the total number of renewal A11-BC service requests received and discarded by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Service Request is received and discarded by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-send-error | Description: This proprietary counter indicates the total number of A11-BC service responses for which errors were experienced during transmission. Triggers: - Incremented when PDSN service experienced errors while trying to send A11-BC service response. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-decode-error | Description: This proprietary counter indicates the total number of A11-BC service requests that had decode errors. Triggers: - Incremented when PDSN service experienced decode error while trying to process A11-BC service request. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-unhandled | Description: This proprietary counter indicates the total number of A11-BC service requests that had unhandled errors. Triggers: - Incremented when PDSN service experienced unhandled error while trying to process A11-BC service request. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-unspec | Description: This proprietary counter indicates the total number of A11-BC service requests that were denied for an unspecified reason. Triggers: - Incremented when PDSN service denied A11-BC service request with unspecified reason. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-auth | Description: This proprietary counter indicates the total number of A11-BC service requests that were denied due to mobile node failing authentication. Triggers: - Incremented when PDSN service denied A11-BC service request due to mobile node failing authentication. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-idmismatch | Description: This proprietary counter indicates the total number of A11-BC service requests that were denied due to identification mismatch. Triggers: - Incremented when PDSN service denied A11-BC service request due to identification mismatch. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-unknownbsn | Description: This proprietary counter indicates the total number of A11-BC service requests that were denied due to unknown BSN address. Triggers: - Incremented when PDSN service denied A11-BC service request due to unknown BSN address. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-noresource-nosessmgr | Description: This proprietary counter indicates the total number of A11-BC service requests that were denied with insufficient resource due to no session manager. Triggers: - Incremented when PDSN service denied A11-BC service request with insufficient resource due to no session manager. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-noresource-nomem | Description: This proprietary counter indicates the total number of A11-BC service requests that were denied with insufficient resource due to no memory.. Triggers: - Incremented when PDSN service denied A11-BC service request with insufficient resource due to no memory. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-noresource-sessmgrretried | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to insufficient resource, session managers retried reported per service. Triggers: - Incremented when PDSN service denied A11-BC service request due to Insufficient resource, session managers retried. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-noresource-inputq | Description: The total number of service requests denied due to insufficient resource, input queue exceeded reported per service. Triggers: - Incremented when PDSN service denied A11-BC service request due to Insufficient resource, input queue exceeded. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-badrequest-alrdorm | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to poorly formed request, session already dormant. Triggers: - Incremented when PDSN service denied A11-BC service request due to poorly formed request, session already dormant.. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-badrequest-alractive | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to poorly formed request, already active. Triggers: - Incremented when PDSN service denied A11-BC service request due to poorly formed request, already active. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-badrequest-other | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to poorly formed request, other reason. Triggers: - Incremented when PDSN service denied A11-BC service request due to poorly formed request, other reason. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-cong-adminprohib | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to administrative prohibition due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. Triggers: - Incremented when PDSN service denied A11-BC service request due to administrative prohibition due to congestion. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> srsp-deny-cong-unknownbsn | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. Triggers: - Incremented when PDSN service denied A11-BC service request due to congestion. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> num-sessions | Description: This proprietary gauge indicates the total number of current BCMCS Sessions. Triggers: - Incremented when a BCMCS session is established successfully. - Decremented when a BCMCS session is disconnected. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> recv-total | Description: This proprietary counter indicates the total number of A11-BC registration requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Registration Request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> accept-total | Description: This proprietary counter indicates the total number of A11-BC registration requests accepted by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Registration request is accepted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> denied-total | Description: This proprietary counter indicates the total number of A11-BC registration requests denied by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Registration request is denied by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> reply-total | Description: This proprietary counter indicates the total number of A11-BC service responses sent by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Registration request is sent by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> discard-total | Description: This proprietary counter indicates the total number of A11-BC registration requests discarded by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Registration request is discarded by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> accept-initial | Description: This proprietary counter indicates the total number of initial A11-BC registration requests received and accepted by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Registration request is received and accepted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> recv-initial | Description: This proprietary counter indicates the total number of initial A11-BC registration requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Registration request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> denied-initial | Description: This proprietary counter indicates the total number of initial A11-BC registration requests received and rejected by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Registration request is received and rejected by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> discard-initial | Description: This proprietary counter indicates the total number of initial A11-BC registration requests discarded by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC Registration request is discarded by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> accept-renew | Description: This proprietary counter indicates the total number of renewal A11-BC service requests received and accepted by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Service Request is received and accepted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> denied-renew | Description: This proprietary counter indicates the total number of renewal A11-BC registration requests received and denied by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Registration request is received and denied by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> discard-renew | Description: This proprietary counter indicates the total number of renewal A11-BC registration requests received and discarded by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Registration request is received and discarded by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> recv-renew | Description: This proprietary counter indicates the total number of renewal A11-BC registration requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC Registration request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> active-start-renew | Description: This proprietary counter indicates the total number of renewal A11-BC active start registration requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC active start Registration request is received by the PDSN service Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> active-stop-renew | Description: This proprietary counter indicates the total number of renewal A11-BC active stop registration requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an renewal A11-BC active stop Registration request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> accept-dereg | Description: This proprietary counter indicates the total number of deregistration A11-BC service requests received and accepted by the PDSN service acting as the BSN.. Triggers: - Incremented when an deregistration A11-BC Service Request is received and accepted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> denied-dereg | Description: This proprietary counter indicates the total number of A11-BC deregistration requests received and denied by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC deregistration Request is received and denied by the PDSN service Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> discard-dereg | Description: This proprietary counter indicates the total number of A11-BC deregistration requests received and discarded by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC deregistration request is received and discarded by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> recv-dereg | Description: This proprietary counter indicates the total number of A11-BC deregistration requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an initial A11-BC deregistration request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> active-stop-dereg | Description: This proprietary counter indicates the total number of ACTIVE STOP A11-BC deregistration requests received by the PDSN service acting as the BSN. Triggers: - Incremented when an initial ACTIVE STOP A11-BC deregistration request is received by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> send-error | Description: This proprietary counter indicates the total number of A11-BC deregistration replies for which errors were experienced during transmission. Triggers: - Incremented when A11-BC deregistration reply experiences error during transmission. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> hash-error | Description: This proprietary counter indicates the total number of A11-BC deregistration requests that had internal hash lookup errors. Triggers: - Incremented when an A11-BC deregistration request processing had internal hash lookup error. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> decode-error | Description: This proprietary counter indicates the total number of A11-BC registration requests that had decode errors. Triggers: - Incremented when PDSN service experienced decode error while trying to process A11-BC registration request. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> unhandled | Description: This proprietary counter indicates the total number of A11-BC registration requests that had unhandled errors. Triggers: - Incremented when PDSN service experienced unhandled error while trying to process A11-BC registration request. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> seqerror | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied due to unacceptable sequence number. Triggers: - Incremented when PDSN service denied A11-BC service request due to unacceptable sequence number. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-unspec | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 80H (Registration Denied - reason unspecified). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 80H (Registration Denied - reason unspecified). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-adminprohib | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 81H (Registration Denied - administratively prohibited). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 81H (Registration Denied - administratively prohibited). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-noresource | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 82H (Registration Denied - insufficient resources). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 82H (Registration Denied - insufficient resources). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-auth | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 83H (Registration Denied - mobile node failed authentication). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 83H (Registration Denied - mobile node failed authentication). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-idmismatch | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 85H (Registration Denied - identification mismatch). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 85H (Registration Denied - identification mismatch). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-badrequest | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 86H (Registration Denied - poorly formed request). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 86H (Registration Denied - poorly formed request). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-unknownbsn | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied unknown BSN address. Triggers: - Incremented when PDSN service denied A11-BC registration request due to unknown BSN address. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-revtununavail | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 89H (Registration Denied - requested reverse tunnel unavailable). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 89H (Registration Denied - requested reverse tunnel unavailable). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-revtunreq | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 8AH (Registration Denied - reverse tunnel is mandatory and “T”-bit not set). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 8AH (Registration Denied - reverse tunnel is mandatory and “T”-bit not set). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-unrecogvend | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 8DH (Registration Denied - unsupported vendor ID or unable to interpret data in the CVSE). Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 8DH (Registration Denied - unsupported vendor ID or unable to interpret data in the CVSE). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-sessclosed | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied using reply code of 0x8E for absent RP sessions. Triggers: - Incremented when PDSN service denied A11-BC registration request using reply code of 0x8E for absent RP sessions. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-bsninfo | Description: This proprietary counter indicates the total number of A11-BC registration requests that were denied because BSN information was unavailable. Triggers: - Incremented when PDSN service denied A11-BC registration due to non availability of BSN Information. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-noresource-nosessmgr | Description: This proprietary counter indicates the total number of A11-BC registration requests denied due to Insufficient resource, no session manager. Triggers: - Incremented when PDSN service denied A11-BC registration due to Insufficient resource, no session manager. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-noresource-nomem | Description: This proprietary counter indicates the total number of A11-BC registration requests denied due to Insufficient resource, no memory. Triggers: - Incremented when PDSN service denied A11-BC registration due to Insufficient resource, no memory. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-noresource-sessmgrretried | Description: This proprietary counter indicates the total number of A11-BC registration requests denied due to Insufficient resource, session managers retried. Triggers: - Incremented when PDSN service denied A11-BC registration due to Insufficient resource, session managers retried. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-noresource-inputq | Description: This proprietary counter indicates the total number of A11-BC registration requests denied due to Insufficient resource, session managers retried. Triggers: - Incremented when PDSN service denied A11-BC registration due to Insufficient resource, input queue exceeded. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-badrequest-alrdorm | Description: This proprietary counter indicates the total number of A11-BC registration requests denied due to to poorly formed request, session already dormant. Triggers: - Incremented when PDSN service denied A11-BC registration due to to poorly formed request, session already dormant. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-badrequest-alractive | Description: This proprietary counter indicates the total number of A11-BC registration requests denied due to poorly formed request, already active. Triggers: - Incremented when PDSN service denied A11-BC registration request due to poorly formed request, already active. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-badrequest-other | Description: This proprietary counter indicates the total number of A11-BC registration requests denied due to poorly formed request, other reason. Triggers: - Incremented when PDSN service denied A11-BC registration request due to poorly formed request, other reason. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-cong-drop | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. Triggers: - Incremented when PDSN service denied A11-BC service request due to congestion. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-cong-adminprohib | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to administrative prohibition due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. Triggers: - Incremented when PDSN service denied A11-BC service request due to administrative prohibition due to congestion. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> deny-cong-unknownbsn | Description: This proprietary counter indicates the total number of A11-BC service requests denied due to congestion. Refer to the Configuring Congestion Control chapter of this guide for additional information. Triggers: - Incremented when PDSN service denied A11-BC service request due to congestion. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-total | Description: This proprietary counter indicates the total number of A11-BC registration updates that were transmitted by the PDSN service acting as the BSN. Triggers: - Incremented when an A11-BC Registration update is transmitted by the PDSN service Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-accept | Description: This proprietary counter indicates the total number of A11-BC registration updates that were that were accepted by the PCF. Triggers: - Incremented when an A11-BC Registration update Ack is received from PCF. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-denied | Description: This proprietary counter indicates the total number of A11-BC registration updates that were denied by PCF. Triggers: - Incremented when an A11-BC Registration update NAK is received from PCF. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-unack | Description: This proprietary counter indicates the total number of A11-BC registration updates for which no acknowledgement was received from PCF. Triggers: - Incremented when an A11-BC Registration Ack is not received before the configured timeout. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-trans | Description: This proprietary counter indicates the total number of initial A11-BC registration updates for which no acknowledgement was received from PCF. Triggers: - Incremented when an initial A11-BC Registration request is transmitted by the PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-ttlnoretrans | Description: This proprietary counter indicates the total number of A11-BC registration updates that were not re-transmitted due to TTL expiration. Triggers: - This counter is derived as total A11-BC Registration updates transmitted less total A11-BC Registration requests retransmitted. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-retrans | Description: This proprietary counter indicates the total number of A11-BC registration updates that were re-transmitted. Triggers: - This counter is incremented when PDSN service retransmits A11-BC Registration update. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-received | Description: This proprietary counter indicates the total number of A11-BC registration update Acks that were received. Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Ack from PCF. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-ack-received | Description: This proprietary counter indicates the total number of A11-BC registration update Acks that were received. Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Ack from PCF. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-discard | Description: This proprietary counter indicates the total number A11-BC registration update Acks that were received and discarded by the PDSN service acting as the BSN. Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Ack from PCF is discarded in PDSN service. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-senderror | Description: This proprietary counter indicates the total number of A11-BC registration update for which errors were experienced during transmission. Triggers: - This counter is incremented when BSN experiences error during transmission of A11-BC Registration update. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-lifetime | Description: This proprietary counter indicates the total number of A11-BC registration updates sent due to Lifetimer Expiry. Triggers: - This counter is incremented when BSN sends A11-BC Registration update due to lifetimer expiry. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-uplyrinit | Description: This proprietary counter indicates the total number of A11-BC registration updates initiated by upper processing layers. Triggers: - This counter is incremented when BSN sends A11-BC Registration update due to a trigger from upper layer. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-other | Description: This proprietary counter indicates the total number of A11-BC registration updates due to reasons other than those listed here. Triggers: - This counter is incremented when BSN sends A11-BC Registration update due to reasons other than those listed here. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upd-smgrexit | Description: This proprietary counter indicates the total number of A11-BC registration updates due to sessmgr exit. Triggers: - This counter is incremented when BSN sends A11-BC Registration update due to session manager exit. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upddeny-unspec | Description: This proprietary counter indicates the total number of A11-BC registration Acknowledge received from PCF with reply code of 80H (Registration Denied - reason unspecified). Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Acknowledge with reply code of 80H (Registration Denied - reason unspecified). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upddeny-adminprohib | Description: This proprietary counter indicates the total number of A11-BC registration Acknowledge received from PCF with reply code of 81H (Registration Denied - administratively prohibited). Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Acknowledge with reply code of 81H (Registration Denied - administratively prohibited). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upddeny-auth | Description: This proprietary counter indicates the total number of A11-BC registration Acknowledge received from PCF with reply code of 83H (Registration Denied - mobile node failed authentication). Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Acknowledge with reply code of 83H (Registration Denied - mobile node failed authentication). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upddeny-idmismatch | Description: This proprietary counter indicates the total number of A11-BC registration Acknowledge received from PCF with reply code of 85H (Registration Denied - identification mismatch). Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Acknowledge with reply code of 85H (Registration Denied - identification mismatch). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> upddeny-badrequest | Description: This proprietary counter indicates the total number of A11-BC registration Acknowledge received from PCF with reply code of 86H (Registration Denied - poorly formed request). Triggers: - This counter is incremented when PDSN service receives A11-BC Registration Acknowledge with reply code of 86H (Registration Denied - poorly formed request). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> sec-violations | Description: This proprietary counter indicates the total number of security violations happened in A11 signaling. Triggers: - This counter is incremented when security violation occurs in BC A11 signaling due to bad authenticator, bad spi etc … Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> sec-badauth | Description: This proprietary counter indicates the total number of security violations happened in A11 signaling due to a mis-computed authenticator field. Triggers: - This counter is incremented when security violation occurs in BC A11 signaling due to bad authenticator field. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> sec-badid | Description: This proprietary counter indicates the total number of security violations happened in A11 signaling due to bad identification field Triggers: - This counter is incremented when security violation occurs in BC A11 signaling due to bad identification field. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> sec-badspi | Description: This proprietary counter indicates the total number of security violations happened in A11 signaling due to bad to the receipt of a Security Parameter Index (SPI) that was in the reserved range (0 through 255). Triggers: - This counter is incremented when security violation occurs in BC A11 signaling due to the receipt of a Security Parameter Index (SPI) that was in the reserved range (0 through 255). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> sec-mnhaauth | Description: This proprietary counter indicates the total number of security violations happened in A11 signaling due to missing mobile node-home agent authentication extensions. Triggers: - This counter is incremented when security violation occurs in BC A11 signaling due to missing mobile node-home agent authentication extensions. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> sec-regupdate | Description: This proprietary counter indicates the total number of security violations happened in A11 signaling due to missing registration update authentication extensions. Triggers: - This counter is incremented when security violation occurs in BC A11 signaling due to missing registration update authentication extensions. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-absent | Description: This proprietary counter indicates the total number of A11-BC registration acknowledgements that were received and discarded due to the session having been already ended because the acknowledgement was late. Triggers: - This counter is incremented when A11-BC registration acknowledgement is received and discarded due to session being already disconnected. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-nomem | Description: This proprietary counter indicates the total number of A11-BC registration acknowledgements that were received and discarded due to insufficient memory. Triggers: - This counter is incremented when A11-BC registration acknowledgement is received discarded due to insufficient memory. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-malform | Description: This proprietary counter indicates the total number of A11-BC registration acknowledgements that were received and discarded due to being poorly formed. Triggers: - This counter is incremented when A11-BC registration acknowledgement is received discarded due to being poorly formed. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-authfail | Description: This proprietary counter indicates the total number of A11-BC registration acknowledgements that were received and discarded due to the mobile node failing authentication. Triggers: - This counter is incremented when A11-BC registration acknowledgement is received discarded due to the mobile node failing authentication. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-bounce | Description: This proprietary counter indicates the total number A11-BC registration acknowledgements that were received and discarded due to internal communication messages between an A11 Manager task and a Session Manager bouncing (not successfully sent). Triggers: - This counter is incremented when message bounces occures between A11 Manager and Session Manager while trying to process an A11 BC Registration Acknowledge Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-inputq | Description: This proprietary counter indicates the total number A11-BC registration acknowledges that were received and discarded due to the queue in which incoming calls are kept prior to being processed exceeded its capacity. Triggers: - This counter is incremented when A11 BC registration acknowledge is discarded due to the queue in which incoming calls are kept prior to being processed exceeded its capacity. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-mismatchid | Description: This proprietary counter indicates the total number A11-BC registration acknowledges that were received and discarded due to due to reply code 85H (Registration Denied - identification mismatch). Triggers: - This counter is incremented when A11 BC registration acknowledge is discarded due to reply code 85H (Registration Denied - identification mismatch). Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-invpktlen | Description: This proprietary counter indicates the total number A11-BC registration acknowledges that were received and discarded due to due to to having an invalid packet length. Triggers: - This counter is incremented when A11 BC registration acknowledge is discarded due to to it having an invalid packet length. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> disc-misc | Description: This proprietary counter indicates the total number A11-BC registration acknowledges that were received and discarded due any other reasons. Triggers: - This counter is incremented when A11 BC registration acknowledge is discarded due to to any other reasons. Availability: per PDSN service, per PCF, per session Type: Counter | Int32
> Important: See Bulk Statistics Overview for statistics that are common to all schema.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883