> show call-control-profile
> This chapter describes the output of the show call-control-profile command.
> show call-control-profile full name
> This command displays the detailed configuration for a specifically named call control profile.
> show call-control-profile full name Command Output Descriptions

> Field | Description
> Call Control Profile Name | The name of the call control profile you chose to view.
> Accounting Context Name | The name of the accounting context associated with this call control profile.
> Accounting GTPP Group Name | The name of the GTTP accounting group associated withis call control profile.
> Acconting Mode (SGW) | The method selected for SGW accouting (GTTP [default], none or RADIUS/Diameter).
> GPRS Attach All | Indicates whether the call control profile allows or restricts attaches of all subscribers using the GPRS access type.
> GPRS Attach All Failure Code | The configured GMM failure code to be sent in reject messages to GPRS mobile subscribers attempting to attach.
> UMTS Attach All | Indicates whether the call control profile allows or restricts attaches of all subscribers using the UMTS access type.
> UMTS Attach All Failure Code | The configured GMM failure code to be sent in reject messages to UMTS mobile subscribers attempting to attach.
> GPRS RAU Intra All | Indicates whether the call control profile is configure to allow or restrict mobile subscribers with GPRS access-type extensions from the intra-SGSN RAU procedure.
> GPRS RAU Intra All Failure Code | The configured GMM failure cause code that identifies the reason an intra-SGSN RAU does not occur. This GMM cause code will be sent in the reject message to the GPRS mobile subscriber.
> UMTS RAU Intra All | Indicates whether the call control profile is configure to allow or restrict mobile subscribers with UMTS access-type extensions from the intra-RAU procedure.
> UMTS RAU Intra All Failure Code | The configured GMM failure cause code that identifies the reason an intra-SGSN RAU does not occur. This GMM cause code will be sent in the reject message to the UMTS mobile subscriber.
> GPRS RAU Inter-PLMN All | Indicates whether the call control profile is configure to allow or restrict mobile subscribers with GPRS access-type extensions from triggering RAUs between different PLMNs.
> GPRS RAU Inter-PLMN All Failure Code | The configured GMM failure cause code that identifies the reason an RAU does not occur between different PLMNs. This GMM cause code will be sent in the reject message to the GPRS mobile subscriber.
> UMTS RAU Inter-PLMN All | Indicates whether the call control profile is configure to allow or restrict mobile subscribers with UMTS access-type extensions from triggering RAUs between different PLMNs.
> UMTS RAU Inter-PLMN All Failure Code | The configured GMM failure cause code that identifies the reason an RAU does not occur between different PLMNs. This GMM cause code will be sent in the reject message to the UMTS mobile subscriber.
> GPRS RAU Inter All | Indicates whether the call control profile is configure to allow or restrict mobile subscribers with GPRS access-type extensions from the inter-SGSN RAU procedure.
> GPRS RAU Inter All Failure Code | The configured GMM failure cause code that identifies the reason an inter-SGSN RAU does not occur. This GMM cause code will be sent in the reject message to the GPRS mobile subscriber.
> UMTS RAU Inter All | Indicates whether the call control profile is configure to allow or restrict mobile subscribers with UMTS access-type extensions from the inter-RAU procedure.
> UMTS RAU Inter All Failure Code | The configured GMM failure cause code that identifies the reason an inter-SGSN RAU does not occur. This GMM cause code will be sent in the reject message to the UMTS mobile subscriber.
> Failure Code For Peer Sgsn Address Resolution Failure | The configured GMM failure cause code that indicates that the SGSN cannot resolve the IP address for a peer SGSN. This GMM cause code will be sent in the reject message to the mobile subscriber.
> GPRS SMS MO All | Indicates whether the call control profile allows or restricts mobile-originated SMS messages from subscribers using the GPRS access type.
> GPRS SMS MO All Failure Code | The configured GMM failure cause code that indicates that mobile-originated SMS messages from GPRS subscribers are not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> UMTS SMS MO All | Indicates whether the call control profile allows or restricts mobile-originated SMS messages from subscribers using the UMTS access type.
> UMTS SMS MO All Failure Code | The configured GMM failure cause code that indicates that mobile-originated SMS messages from UMTS subscribers are not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> GPRS SMS MT All | Indicates whether the call control profile allows or restricts mobile-terminated SMS messages to subscribers using the GPRS access type.
> GPRS SMS MT All Failure Code | The configured GMM failure cause code that indicates that mobile-terminated SMS messages to GPRS subscribers are not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> UMTS SMS MT All | Indicates whether the call control profile allows or restricts mobile-terminated SMS messages to subscribers using the UMTS access type.
> UMTS SMS MT All Failure Code | The configured GMM failure cause code that indicates that mobile-terminated SMS messages to UMTS subscribers are not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> GPRS Primary PDP Context Activation All | Indicates whether primary PDP context activation is allowed for GPRS mobile subscribers.
> GPRS Secondary PDP Context Activation All | Indicates whether secondary PDP context activation is allowed for GPRS mobile subscribers.
> GPRS PDP Context Activation All Failure Code | The configured GMM failure cause code that indicates that PDP context activation by GPRS subscribers is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> UMTS Primary PDP Context Activation All | Indicates whether primary PDP context activation is allowed for UMTS mobile subscribers.
> UMTS Secondary PDP Context Activation All | Indicates whether secondary PDP context activation is allowed for UMTS mobile subscribers.
> UMTS PDP Context Activation All Failure Code | The configured GMM failure cause code that indicates that PDP context activation by UMTS subscribers is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> GPRS Nw Init Primary PDP Context Activation All | Indicates whether network-initiated primary PDP context activation is allowed for GPRS mobile subscribers.
> GPRS Nw Init Primary PDP Ctxt Activation All Failure Code | The configured GMM failure cause code that indicates that network-initiated primary PDP context activation by GPRS subscribers is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> GPRS Nw Init Secondary PDP Ctxt Activation All | Indicates whether network-initiated secondary PDP context activation is allowed for GPRS mobile subscribers.
> GPRS Nw Init Secondary PDP Ctxt Activation All Failure Code | The configured GMM failure cause code that indicates that network-initiated secondary PDP context activation by GPRS subscribers is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> UMTS Nw Init Primary PDP Context Activation All | Indicates whether network-initiated primary PDP context activation is allowed for UMTS mobile subscribers.
> UMTS Nw Init Primary PDP Ctxt Activation All Failure Code | The configured GMM failure cause code that indicates that network-initiated primary PDP context activation by UMTS subscribers is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> UMTS Nw Init Secondary PDP Ctxt Activation All | Indicates whether network-initiated secondary PDP context activation is allowed for UMTS mobile subscribers.
> UMTS Nw Init Secondary PDP Ctxt Activation All Failure Code | The configured GMM failure cause code that indicates that network-initiated secondary PDP context activation by UMTS subscribers is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> SRNS Intra All | Indicates whether intra-SRNS (Serving Radio Network Subsystem) relocation is allowed for mobile subscribers.
> SRNS Intra All Failure Code | The configured GMM failure cause code that indicates that intra-SRNS relocation is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> SRNS Inter All | Indicates whether inter-SRNS relocation is allowed for mobile subscribers.
> SRNS Inter All Failure Code | The configured GMM failure cause code that indicates that inter-SRNS relocation is not permitted. This GMM cause code will be sent in the reject message to the mobile subscriber.
> Sgtp-service Context | The name of the context that has the applicable SGTP service for this call control profile associated with it.
> Service | The name of the SGTP service associated with the context.
> Authentication All-Events | Indicates whether authentication for all events (attaches, activates, and so forth) has been enabled or disabled.
> Authentication Attach | Indicates whether authentication for an Attach with a local P-TMSI or Attaches with an IMSI has been enabled or disabled.
> Authentication Attach (Inter RAT) | Indicates whether Attach message authentication has been enabled or disabled for re-authorizing subscribers on a change in Radio Access Type (RAT) of the subscriber’s node.
> Authentication Attach (Gprs only) | Indicates whether Attach message authentication has been enabled or disabled for calls from GPRS mobile subscribers.
> Authentication Attach (Combined) | Indicates whether authentication for combined GPRS/IMSI Attaches has been enabled or disabled.
> Authentication Activate | Indicates whether authentication for activate requests has been enabled or disabled.
> Authentication Service Request | Indicates whether authentication for all service requests has been enabled or disabled.
> Authentication Service Request (Signaling) | Indicates whether authentication for signaling service requests has been enabled or disabled.
> Authentication Service Request (Data) | Indicates whether authentication for data service requests has been enabled or disabled.
> Authentication Service Request (Page Response) | Indicates whether authentication for page response service requests has been enabled or disabled.
> Authentication RAU | Indicates whether authentication for routing area updates has been enabled or disabled.
> Authentication RAU (Periodic) | Indicates whether authentication for periodic RAU Requests has been enabled or disabled.
> Authentication RAU (Ra update) | Indicates whether authentication for RA update RAU Requests has been enabled or disabled.
> Authentication RAU (Ra update with Local Ptmsi) | Indicates whether authentication for RA update using the local P-TMSI type of RAU Requests has been enabled or disabled.
> Authentication RAU (Ra update with Foreign Ptmsi) | Indicates whether authentication for RA update using foreign P-TMSI type of RAU Requests has been enabled or disabled.
> Authentication RAU (Imsi Combined Update) | Indicates whether authentication for RA update RAU Requests using the inter-RAT P-TMSI has been enabled or disabled.
> Authentication RAU (Combined Update) | Indicates whether authentication for RAU Requests using the local P-TMSI has been enabled or disabled.
> Authentication RAU (Combined Update IRAT PTMSI) | Indicates whether authentication for RAU Requests using inter-RAT and the local P-TMSI has been enabled or disabled.
> Authentication RAU (Imsi Combined Update) | Indicates whether authentication for RAU Requests using IMSI and local P-TMSI values has been enabled or disabled.
> Authentication RAU (Imsi Combined Update IRAT PTMSI) | Indicates whether authentication for RAU Requests using IMSI values, inter-RAT, and the local P-TMSI has been enabled or disabled.
> Authentication Detach | Indicates whether authentication for Detach Requests has been enabled or disabled.
> Authentication SMS | Indicates whether authentication for all SMS messages has been enabled or disabled.
> Authentication SMS (MO-SMS) | Indicates whether authentication for mobile-originated SMS messages has been enabled or disabled.
> Authentication SMS (MT-SMS) | Indicates whether authentication for mobile-terminated SMS messages has been enabled or disabled.
> Regional Subscription Restriction Failure Code Value | The configured GMM failure cause code that indicates that mobile subscriber lacks the required subscription to place calls to the region. This GMM cause code will be sent in the reject message to the mobile subscriber.
> ARD-Checking | Indicates whether access restriction data (ARD) checking in incoming subscriber data (ISD) messages has been enabled or disabled.
> ARD Failure Code | The configured GMM failure cause code that indicates the incoming subscriber data has failed ARD checking. This GMM cause code will be sent in the reject message to the mobile subscriber.
> Zone-Code Check | Indicates whether zone code checking has been enabled or disabled.
> Usage of Auth Vectors From Old Sgsn | Indicates whether the ability of an SGSN to receive authorization vectors from other SGSNs has been enabled or disabled.
> Order of Preference for Integrity Algorithm is | The integrity algorithm that receives first priority.
> Order of Preference for Encryption Algorithm is | The encryption algorithm that receives first priority.
> Order of Preference for Gprs Ciphering Algorithm is | The GPRS ciphering algorithm that receives first priority.
> PTMSI-signature allocation | Indicates whether P-TMSI signature allocation has been enabled or disabled.
> PTMSI-Signature-Realloc Interval value UMTS | The time interval (in minutes) for skipping the P-TMSI signature service/RAU/attach request message procedure for UMTS mobile subscribers.
> PTMSI-Signature-Realloc Interval value GPRS | The time interval (in minutes) for skipping the P-TMSI signature service/RAU/attach request message procedure for GPRS mobile subscribers.
> PTMSI-Signature-Realloc Frequency value UMTS | How many times P-TMSI signature reallocation for service requests can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc Frequency value GPRS | How many times P-TMSI signature reallocation for service requests can be skipped for GPRS mobile subscribers.
> PTMSI-Signature-Realloc Attach Frequency value UMTS | How many times P-TMSI signature reallocation for Attach requests can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc Attach Frequency value GPRS | How many times P-TMSI signature reallocation for Attach requests can be skipped for GPRS mobile subscribers.
> PTMSI-Signature-Realloc RAU (Generic) Frequency value UMTS | How many times P-TMSI signature reallocation for routing area updates can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc RAU (Generic) Frequency value GPRS | How many times P-TMSI signature reallocation for routing area updates can be skipped for GPRS mobile subscribers.
> PTMSI-Signature-Realloc RAU Periodic Frequency value UMTS | How many times P-TMSI signature reallocation for periodic routing area updates can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc RAU Periodic Frequency value GPRS | How many times P-TMSI signature reallocation for periodic routing area updates can be skipped for GPRS mobile subscribers.
> PTMSI-Signature-Realloc RAU RA Update Frequency value UMTS | How many times P-TMSI signature reallocation for routing area update RA updates can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc RAU RA Update Frequency value GPRS | How many times P-TMSI signature reallocation for routing area update RA updates can be skipped for GPRS mobile subscribers.
> PTMSI-Signature-Realloc RAU Combined Update Frequency value UMTS | How many times P-TMSI signature reallocation for combined requests can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc RAU Combined Update Frequency value GPRS | How many times P-TMSI signature reallocation for combined requests can be skipped for GPRS mobile subscribers.
> PTMSI-Signature-Realloc RAU Imsi Combined Update Frequency value UMTS | How many times P-TMSI signature reallocation for combined RAU updates with IMSI values can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc RAU Imsi Combined Update Frequency value GPRS | How many times P-TMSI signature reallocation for combined RAU updates with IMSI values can be skipped for GPRS mobile subscribers.
> PTMSI-Signature-Realloc Ptmsi-Reallocation-Cmd Update Frequency value UMTS | How many times P-TMSI signature reallocation during PTMSI reallocation can be skipped for UMTS mobile subscribers.
> PTMSI-Signature-Realloc Ptmsi-Reallocation-Cmd Update Frequency value GPRS | How many times P-TMSI signature reallocation during PTMSI reallocation can be skipped for GPRS mobile subscribers.
> PTMSI-Realloc Attach | Indicates whether P-TMSI reallocation has been enabled or disabled.
> PTMSI-Realloc Interval | The time interval (in minutes) for skipping the P-TMSI reallocation during the service/RAU/attach request message procedure.
> PTMSI-Realloc Frequency | How many times P-TMSI reallocation can be skipped during service/RAU/attach request message procedure.
> PTMSI-Realloc RAU | Indicates whether P-TMSI reallocation during routing area updates has been enabled or disabled.
> PTMSI-Realloc RAU (Periodic) | Indicates whether P-TMSI reallocation during periodic routing area updates has been enabled or disabled.
> PTMSI-Realloc RAU (Periodic) Frequency value | How many times P-TMSI reallocation can be skipped during the periodic RAU message procedure.
> PTMSI-Realloc RAU (Ra-Update) | Indicates whether P-TMSI reallocation during the RA update RAU request procedure has been enabled or disabled.
> PTMSI-Realloc RAU (Ra-Update) Frequency | How many times P-TMSI reallocation can be skipped during the RA update RAU message procedure.
> PTMSI-Realloc RAU (Combined-Update) | Indicates whether P-TMSI reallocation during the RAU combined update procedure has been enabled or disabled.
> PTMSI-Realloc RAU (Combined-Update) Frequency | How many times P-TMSI reallocation can be skipped during the RAU combined update message procedure.
> PTMSI-Realloc RAU (Combined-Update with IMSI attach) | Indicates whether P-TMSI reallocation during the RAU combined update with IMSI procedure has been enabled or disabled.
> PTMSI-Realloc RAU (Combined-Update with IMSI) Frequency | How many times P-TMSI reallocation can be skipped during the RAU combined update with IMSI message procedure.
> PTMSI-Realloc Service Request (Signalling) | Indicates whether P-TMSI reallocation during signaling service requests has been enabled or disabled.
> PTMSI-Realloc Service Request (Signalling) Freq | How many times P-TMSI reallocation can be skipped during the signaling service request message procedure.
> PTMSI-Realloc Service Request (Data) | Indicates whether P-TMSI reallocation during data service requests has been enabled or disabled.
> PTMSI-Realloc Service Request (Data) Freq | How many times P-TMSI reallocation can be skipped during the data service request message procedure.
> PTMSI-Realloc Service Request (Page Response) | Indicates whether P-TMSI reallocation during page response service requests has been enabled or disabled.
> PTMSI-Realloc Service Request (Page Response) Freq | How many times P-TMSI reallocation can be skipped during the page response service request message procedure.
> Inactivity detection for establishing pdp contexts | Indicates whether an SGSN will be periodic polled to verify that it can accept requests to establish a PDP context.
> Inactivity detection for establishing pdp contexts - Timer | The timeout value in milliseconds for determining that a SGSN is unresponsive.
> Inactivity detection for establishing pdp contexts - Action | The action to be taken if a SGSN is declared unresponsive.
> Monitor Re-attaches after Inactivity Detach | Indicates whether the SGSN will be monitored to determine if it has become responsive again after an inactivity timeout and detach.
> Charging Characteristics Prefer Local | When enabled, indicates whether the call-control profile prefers the charging characteristics settings from the call control profile instead of the charging characteristics received from the HLR.
> Charging Characteristics Behavior | The behavior bit in charging characteristics provided by the call control profile when the HLR does not provide a value.
> Charging Characteristics Profile-Index | The charging characteristics profile index specified by the call control profile, such as 4 for prepaid billing or 8 for normal billing.
> Charging Characteristics Behavior No Records | The behavior bit in charging characteristics that is used to determine that no accounting records will be generated.
> APN restriction | If this feature is enable, the SGSN sends the maximum APN restriction value in every CPC Request message sent to the GGSN
> UMTS Gmm-Information | When this feature is enabled, indicates that GPRS mobility management (GMM) parameters will be included in message to UMTS mobile subscribers.
> GPRS Gmm-Information | When this feature is enabled, indicates that GMM parameters will be included in message to GPRS mobile subscribers.
> User Equipment Identity Retrieval | Indicates whether International Mobile Equipment Identity (IMEI) or software version (SV) retrieval and validation has been enabled or disabled.
> MAP UGL Message. Include Access Type Private Extension | The specific access-type private extension included in GPRS Location Update (GLU) request MAP messages.
> MAP UGL Message. Include IMEISV | The specific International Mobile equipment Identity-Software Version (IMEI-SV) information included in GLU request MAP messages.
> Reuse of authentication triplets | Indicates whether the reuse of authentication triplets in the event of a failure has been enabled or disabled.
> Re-Authentication | Indicates whether the re-authentication feature, which instructs the SGSN to retry authentication with another RAND in situations where failure of the first authentication has occurred, has been enabled or disabled.
> Direct Tunnel | Indicates if the SGSN allows direct tunneling if the direct tunneling is supported by destination node.
> GTPU Fast Path | Indicates whether Fast Path support for network processing unit (NPU) processing of GTP-U packets of user sessions has been enabled or disabled.
> Super Charger | Indicates whether the SGSN’s ability to work with a super-charged network is enabled or disabled. By enabling the super charger functionality for 2G or 3G connections controlled by an operator policy, the SGSN changes the hand-off and location update procedures to reduce signaling traffic management.
> Sending Radio Access Technology (RAT) IE | When this feature is enabled, the SGSN sends RAT information elements (IEs) within GTP messages.
> Sending User Location Information (ULI) IE | When this feature is enabled, the SGSN sends ULI IEs within GTP messages.
> Sending IMEISV IE | When this feature is enabled, the SGSN includes the IMEISV values of the mobile subscriber when sending GTP messages of the type “Create PDP Context Request”.
> Derive IMEISV from IMEI | When this feature is enabled, the SGSN sends the IMEI to the GGSN as an IMEI-SV.
> Sending MS Time Zone IE | When this feature is enabled, the SGSN sends the mobile subscribers timezone IE in GTP messages of the type “Create PDP Request” and “Update PDPContext Request”.
> Treat as HPLMN | When this feature is enabled, the MME or SGSN treats an IMSI series as coming from the home PLMN.
> Location Reporting for UMTS | When this feature is enabled, the MME can query and receive UE location reports from an eNodeB.
> Location Reporting for GPRS | When this feature is enabled, the MME can query and receive UE location reports from an eNodeB.
> Network Feature Support
> IMS Voice Over PS | Indicates whether IMS Voice over Packet-Switched information element (IE) is supported as part of the MME (Network) Feature
> Qos | Indicates the transmission of quality of service (QoS) parameters has been enabled or disabled.
> AMBR | Indicates whether an aggregate maximum bit rate (AMBR) will be enforced for user equipment.
> Gn/Gp ARP | Indicates whether Gn-Gp pre-release 8 ARP and pre-emption parameters will be enforced or not.
> High Priority (H) (Default) | The high-priority (address retention protocol) ARP value used for QoS.
> Medium Priority (M) (Default) | The medium-priority ARP value used for QoS.
> Gn/Gp Pre-Emption Capabilities (Default) | The pre-emption capability criteria for PDP contexts imported from an SGSN on Gn/Gp interfaces.
> Gn/Gp Pre-Emption Vulnerabilities (Default) | The pre-emption vulnerability criteria for PDP contexts imported from an SGSN on Gn/Gp interfaces.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883