> Remote Address List Configuration Mode Commands
> The Remote Address List Configuration Mode is used to configure address lists for the Remote Address-based Accounting feature on a per-context basis.
> address
> Configures addresses within a Remote Address List.
> Product
> PDSN, HA
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] address ip_address netmask subnet
> no
> Removes a previously configured address.
> ip_address
> Specifies the IP address of the remote device.
> ip_address is entered using IPv4 dotted-decimal or IPv6 colon-separated notation.
> netmask subnet
> Specifies the subnet mask of the remote device.
> subnet is the netmask expressed in IPv4 dotted-decimal or IPv6 colon-separated notation.
> Usage
> Use this command to configure remote address lists for use with the Remote Address-based accounting feature. A maximum of 10 address can be configured per list.
> Example
> The following command adds an IP address of 192.168.100.1 with a subnet mask of 255.255.255.0 to the list:
> address 192.168.100.1 netmask 255.255.255.0
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883