> MSEG IMEI Profile Configuration Mode Commands
> The MSEG IMEI Profile Configuration Mode enables to configure International Mobile Equipment Identifier (IMEI) ranges in Mobile Service Edge Gateway (MSEG) IMEI profiles.
> Important: This configuration mode is not supported in this release. For more information please contact your Cisco account representative.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> imei-range
> This command allows you to add/remove IMEI ranges in an MSEG IMEI profile.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] imei-range start imei_prefix_range_start end imei_prefix_range_end [ sv imei_sw_version ]
> no
> Deletes the specified IMEI prefix range.
> start imei_prefix_range_start
> Specifies the start of the IMEI prefix range as an integer.
> end imei_prefix_range_end
> Specifies the end of the IMEI prefix range as an integer.
> sv imei_sw_version
> Specifies software version of IMEISV as a 2-digit integer.
> Usage
> Use this command to add/remove IMEI ranges in an MSEG IMEI profile.
> Multiple, non-overlapping, IMEI ranges can be specified in each IMEI profile. IMEI ranges are level-one filters.
> Example
> The following command adds an IMEI range starting with the IMEI prefix 123 and ending with the IMEI prefix 456:
> imei-range start 123 end 456

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883