> P-GW Service Configuration Mode Commands
> The P-GW (PDN Gateway) Service Configuration Mode is used to create and manage the relationship between specified services used for either GTP or PMIP network traffic.
> associate
> Associates the P-GW service with specific pre-configured services and/or policies configured in the same context.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> associate { egtp-service name [ lma-service name ] | ggsn-service name | lma-service name [ egtp-service name ] | qci-qos-mapping name }
> no associate { egtp-service | lma-service | qci-qos-mapping }
> no
> Removes the selected association from this service.
> { egtp-service name [ lma-service name ] | lma-service name [ egtp-service name ] }
> egtp-service name [ lma-service name ]: Specifies that the P-GW service is to be associated with an existing eGTP service within this context.
> name must be an alphanumeric string of 1 through 63 characters and be an existing eGTP service.
> Configure an associated LMA service name to support handoffs between PMIPv6 and GTP. name must be an alphanumeric string of 1 through 63 characters and be an existing LMA service.
> lma-service name [ egtp-service name ]: Specifies that the P-GW service is to be associated with an existing LMA service within this context.
> name must be an alphanumeric string of 1 through 63 characters and be an existing LMA service.
> Configure an associated eGTP service name to support handoffs between PMIPv6 and GTP. name must be an alphanumeric string of 1 through 63 characters and be an existing eGTP service.
> ggsn-service name
> Specifies that the P-GW service is to be associated with an existing GGSN service within this context.
> name must be an alphanumeric string of 1 through 63 characters and be an existing GGSN service.
> qci-qos-mapping name
> Specifies that the P-GW service is to be associated with an existing QCI-QoS mapping configuration within this context.
> name must be an alphanumeric string of 1 through 63 characters and be an existing QCI-QoS mapping configuration.
> QCI-Qos mapping is typically configured in a AAA context. Refer to the QCI-QoS Mapping Configuration Mode Commands chapter for more information.
> Usage
> Use this command to associate the P-GW service with other pre-configured services and/or policies configured in the same context.
> Example
> The following command associates this service with an eGTP service called egtp1:
> associate egtp-service egtp1
> authorize-with-hss
> This command enables or disables subscriber session authorization via a Home Subscriber Server (HSS) over an S6b Diameter interface. This feature is required to support the interworking of GGSN with P-GW and HA.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> authorize-with-hss [ report-ipv6-addr ]
> [ default | no ] authorize-with-hss
> [ default | no ]
> Disables the default authorization of subscriber over S6b interface. Resets the command to the default setting of “authorize locally” from an internal APN authorization configuration.
> report-ipv6-addr
> Enables the IPv6 address reporting through Authorization-Authentication-Request (AAR) towards the S6b interface.
> Usage
> Use this command to enable/disable the authorization support for subscriber over S6b interface, which is used between P-GW and the 3GPP AAA to exchange the information related to charging, GGSN discovery, etc.
> dns-client
> Specifies the DNS client context to use for sending DNS queries.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> dns-client context name
> [ default | no ] dns-client context
> default
> Returns the command to the default setting of targeting the DNS client in the context where the P-GW service resides.
> no
> Disables DNS queries.
> context name
> Specifies the name of the context where the DNS client is used for the resolution of PCSCF-FQDN received from S6b interface.
> name must be an existing context expressed as an alphanumeric string of 1 through 79 characters.
> Usage
> Use this command to specify the context where the DNS client resides to perform P-CSCF-FQDN resolution from the S6b interface.
> Example
> The following command identifies the egress1 context as the context where the DNS client resides:
> dns-client context egress1
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> fqdn
> Configures a Fully Qualified Domain Name for this P-GW service used in messages between the P-GW and a 3GPP AAA server over the S6b interface.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> fqdn host domain_name realm realm_name
> [ default | no ] fqdn
> default
> Returns the command to the default setting of “null”.
> no
> Removes the configured FQDN from this service configuration.
> host domain_name
> Specifies the domain name of the P-GW service.
> domain_name must be an alphanumeric string of 1 through 255 characters.
> realm realm_name
> Specifies the realm name of the P-GW service.
> realm_name must be an alphanumeric string of 1 through 255 characters.
> Usage
> Use this command to identify the P-GW service using an FQDN required when sending messages over the S6b interface to a 3GPP AAA server.
> Important: In order to properly interact with other nodes in the network, the FQDN should be less than or equal to 96 alphanumeric characters.
> Topology Matching (eHRPD only)
> You may specify which P-GW you wish an HSGW interface to connect with by enabling topology matching within the FQDNs for both the HSGW service and P-GW service. Topology matching selects geographically closer nodes and reduces backhaul traffic for a specified interface.
> The following optional keywords enable or disable topology matching when added to the beginning of an FQDN:

> • | topon.interface_name.

> Beginning an FQDN with topon initiates topology matching with available HSGWs in the network. Once this feature is enabled, the rest of the FQDN is processed from right to left until a matching regional designator is found on a corresponding HSGW FQDN.

> • | topoff.interface_name.

> By default, topology matching is disabled. If you enable topology matching for any interfaces within a node, however, all interfaces not using this feature should be designated with topoff.
> Example
> The following command configures the FQDN for this P-GW service as 123abc.all.com with a realm name of all.com:
> fqdn host 123abc.all.com realm all.com
> The following command configures this P-GW service with an FQDN that enables topology matching:
> fqdn host topon.interface_name.pgw01.bos.ma.node.epc .mnc<value>.mcc<value>.3gppnetwork.org realm node.epc.mnc.mcc.3gppnetwork.org
> Important: The associated HSGW service must have a corresponding FQDN similar to the following:
> topon.interface_name.hsgw01.bos.ma.node.epc.mncvalue.mccvalue.3gppnetwork.org
> gx-li
> Refer to the Lawful Intercept Configuration Guide for a description of this command.
> newcall
> Configures the P-GW to accept or reject requests for a static IP address if the address is already in use by another session.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> newcall duplicate-subscriber-requested-address { accept | reject }
> no newcall duplicate-subscriber-requested-address
> no
> Returns the command to the default setting of “reject”.
> duplicate-subscriber-requested-address { accept | reject }
> Default: reject
> accept: Specifies that the old session with the requested address will be ended to accept the new session with the same address.
> reject: Specifies that the new session requesting the same address will be rejected.
> Usage
> Use this command to configure the behavior of the P-GW service when receiving requests for static IP address already in use by other sessions.
> Important: This command is only applicable to sessions using services supporting duplicate address abort. These services include HA, GGSN, and P-GW.
> Example
> The following command allows for the acceptance of requests for static IP addresses already in use by other sessions:
> newcall duplicate-subscriber-requested-address accept
> plmn
> Configures Public Land Mobile Network identifiers used to determine if a mobile station is visiting, roaming, or belongs to this network.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> plmn id mcc number mnc number [ primary ]
> id mcc number mnc number
> mcc number: Specifies the mobile country code (MCC) portion of the PLMN identifier.
> number is the PLMN MCC identifier and must be an integer from 100 through 999.
> mnc number: Specifies the mobile network code (MNC) portion of the PLMN identifier.
> number is the PLMN MNC identifier and can be configured to a 2- or 3-digit integer from 00 through 999.
> primary
> When multiple PLMN IDs are configured, the primary keyword can be used to designate one of the PLMN IDs to be used for the AAA attribute.
> Usage
> The PLMN identifier is used to aid the P-GW service in the determination of whether or not a mobile station is visiting, roaming, or home. Multiple P-GW services can be configured with the same PLMN identifier. Up to five PLMN IDs can be configured for each P-GW Service.
> Example
> The following command configures the PLMN identifier with an MCC of 462 and MNC of 02:
> plmn id mcc 462 mnc 02
> session-delete-delay
> Configures a delay in terminating a session.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> session-delete-delay timeout [ msec ]
> [ default | no ] session-delete-delay timeout
> default
> Resets the command to the default setting of 10000 milliseconds.
> no
> Disables the feature.
> timeout msec
> Default: 10000
> Specifies the time to retain the session (in milliseconds) before terminating it.
> msec must be an integer from 1000 to 60000.
> Usage
> Use this command to set a delay to provide session continuity in break-before-make scenarios.
> Example
> The following command sets the session delete delay to the default setting of 10,000 milliseconds:
> session-delete-delay timeout

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883