> Cisco ANA Management Application Integration
> This chapter is for Administrators working with Cisco ANA integration. It provides some new information regarding options connected with Cisco Oid strings, and a list of supported ANA MIBS.
> New CLI Options
> The following are new CLI options:
> sysOId Options
> For ASR5000 and XT2 users, the default OId string is 1.3.6.1.4.1.8164. Users also have the option to use the new-style Cisco OId string: 1.3.6.1.4.1.9.
> Use the following new CLI:[local]asr5000(config)# system sysoid-style new|default
> Important: This command can be combined with sysdescas follows:system sysdesc-sysoid-style new|default. However, this combination affects BOTH sysDesc AND sysOId equally: that is, they can both be old-style or they can both be new-style. The System CLI offers an option to configure sysDesc independently, but SysOId is not a user-configurable parameter.
> sysDesc Options
> For ASR5000 and XT2 users, the default system description is:
> Linux asr5000 2.6.18-staros-v2-private-deb #1 SMP (date/time) i686
> The Cisco default description is:
> Cisco StarOS Software, ASR5000 Intelligent Mobile Gateway, Version 12.2. Copyright (c) 2011 by Cisco Systems, Inc.
> Users can opt for either description using the following CLI command: [local]asr5000(config)# system sysdesc-style new|default
> Important: This command can be combined with sysOIdas follows:system sysdesc-sysoid-style new|default. However, this combination affects BOTH sysDesc AND sysOId equally: that is, they can both be old-style or they can both be new-style. The System CLI offers an option to configure sysDesc independently, but SysOId is not a user-configurable parameter.
> Serial Number Configuration
> ASR 5000 and XT2 users can configure the chassis serial number with the following CLI:
> [local]asr5000(config)# system chassis-serial-number <string>
> Standards-Based MIBs
> The following are standards-based and read-only:
> Entity MIB
> The Entity MIB is implemented as described in RFC4133 and is Read-Only. The following are not supported for this release:

> • | entPhysicalAlias

> • | entPhysicalAssetID

> • | entPhysicalMfgDate

> • | entPhysicalUris

> • | entLogicalTable

> • | entLPMappingTable

> • | entPhysicalContainsTable

> IF MIB
> The IF MIB is implemented per RFC1213, RFC1573, and RFC2863 and is Read-Only. The following are not supported for this release:

> • | ifStackTable

> • | ifStackLastChange

> • | ifRcvAddressTable

> • | ifTestTable

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883