> show gtpu-service
> This chapter includes the show gtpu-service command output tables.
> show gtpu-service all
> show gtpu-service all Command Output Descriptions

> Field | Description
> Service name | The name of the service configured in the named context.
> Context | The name of the context where the service is configured.
> State | The status of the service, i.e., “Initiated”.
> Echo Interval | The duration between the sending of GTP-U echo messages.
> Sequence Number | Identifies if the sequence number is added to every GTP-U packet.
> Include UDP Port Ext.Hdr | Indicates if an extention header, in the GTP-U packet header, allowing for error indication messages will be added.
> Max-retransmissions | The number of user data packet request message retransmissions that can be sent before an error condition is established.
> Retransmission Timeout | The number of seconds between the re-sending of GTP-U echo messages
> IPSEC Tunnel Idle Timeout | The number of seconds an IPSec tunnel is idle before tunnel deletion is triggered.
> Allow Error-Indication | Indicate if the error indication will be allowed or suppressed upon the receipt of a user data packet for a non-existent session.
> Address List | Identifies the IP address used to transmit/receive GTP-U packets.
> Path Failure Detection on gtp echo msgs | Identifies if the path failure detection is enabled upon reaching the maximum number of echo retransmissions.

> ‌

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883