> PCC-Usage-Monitor Configuration Mode Commands
> The PCC-Usage-Monitor Configuration mode provides a mechanism to set the usage threshold limit in a PCC-Service-Profile to trigger a required condition and action set in PCC-Service instance.
> Important: This configuration mode is supported from StarOS Release 12.1 onward.
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> usage-limit volume
> Sets the usage limit by volume for a subscriber profile for a PCC-Service-Profile on an IPCF node.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> [default usage-limit volume [downlink dlink_volume | total total_volume | uplink uplink_volume]
> default
> Sets the usage limit volume to “0” for downlink, uplink and total bucket in a PCC-Service-Profile.
> downlink dlink_volume
> Specifies the usage volume (in kilobytes) in the downlink direction (from PCEF to UE) as an integer from 1 through 4294967296. A “0” (zero) value disables the downlink volume usage. Default: 0
> total total_volume
> Specifies the usage volume (in kilobytes) in the downlink and uplink directions (from PCEF to UE and PCEF to PDN) as an integer from 1 through 4294967296. A “0” (zero) value disables the downlink volume usage. Default: 0
> uplink uplink_volume
> Specifies the usage volume (in kilobytes) in the uplink direction (from PCEF to PDN) as an integer from 1 through 4294967296. A “0” (zero) value disables the downlink volume usage. Default: 0
> Usage
> Use this command to set the usage limit in volume for subscriber profile for a PCC-Service-Profile on IPCF node.
> Example
> The following command sets the usage limit volume to 20000 kilobytes in the upload direction within a PCC-Service-Profile.
> usage-limit volume uplink 20000
> The following command sets the usage limit volume to 400000 kilobytes in the download direction within a PCC-Service-Profile.
> usage-limit volume downlink 400000

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883