> Exec Mode Show Commands (H-L)
> This section includes the commands show ha-service through show lte-policy.
> The Exec Mode is the initial entry point into the command line interface system. Exec mode show commands are useful in troubleshooting and basic system monitoring.
> show ha-service
> Displays information on configured home agent services.
> Product
> HA
> Privilege
> Security Administrator Operator, Inspector
> Syntax
> show ha-service { all | name ha_name } [ | { grep grep_options | more } ]
> all | name ha_name
> all: Displays information on all Home Agent services is to be displayed.
> name ha_name: Displays information for an existing HA service specified as an alphanumeric string of 1 through 63 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Display home agent service configuration information.
> Example
> The following commands displays information on the HA service sampleService and all services, respectively.
> show ha-service name sampleService
> show ha-service all
> show hardware
> Displays information on the system hardware.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show hardware { card [ card_num ] | inventory | version [ board | diags | fans] } [ | { grep grep_options | more } ]
> card [ card_num ]
> Provide the hardware information for all cards or the card specified by card_num. card_num must be a value in the range 1 through 48 and must refer to an installed card.
> inventory
> Display the hardware information for all slots in tabular format.
> version [ board | diags | fans]
> Display the CPU information for all application cards and fan controller version for the upper and lower fan trays.
> board: Only include the CPLD and FPGA version information.
> diags: Only include the CFE diagnostics version information.
> fans: Show the fan controller versions for the upper and lower fan trays.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Show the hardware information to verify part lists and hardware component versions with reserve stock
> Example
> The following displays the hardware information for a card installed in slot 1.
> show hardware card 1
> The following command displays the hardware inventory for the entire chassis.
> show hardware inventory
> The following command results in the display of the CPU version for all application cards displaying only the CPLD and FPGA information.
> show hardware version board
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hd raid
> Shows the output of the Redundant Array of Independent Disks (RAID) established on the SMCs.
> Product
> All
> Privilege
> Security Administrator, Administrator, Administrator, Operator
> Syntax
> show hd raid [ verbose ]
> Example
> show hd raid verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hd-storage-policy
> Displays Array Configuration Replicator (ACR) counter and statistic information.
> Product
> HSGW, P-GW, S-GW
> Privilege
> Inspector
> Syntax
> show hd-storage-policy { all | counters [ all ] [ name name ] [ verbose ] | name name | statistics [ all ] [ name name ] [ verbose ] }
> all
> Displays ACR information for all HD storage policies configured on the system.
> counters [ all ] [ name name ] [ verbose ]
> all: Displays ACR counter information for all HD storage policies configured on the system.
> name name: Displays ACR counter information for an existing HD storage policy specified as an alphanumeric string of 0 through 63 characters.
> statistics [ all ] [ name name ] [ verbose ]
> all: Displays ACR statistical information for all HD storage policies configured on the system.
> name name: Displays ACR statistical information for an existing HD storage policy specified as an alphanumeric string of 0 through 63 characters.
> verbose
> Displays HD storage statistics based on instance.
> Usage
> Use this command to display ACR counter and statistic information.
> Example
> The following command displays ACR statistic information for an HD storage policy named pgwsgw:
> show hd-storage-policy statistics name pgwsgw
> show hnbgw access-control-db
> Displays the white list of IMSI records in the Access Control database residing on Home-NodeB Gateway (HNB-GW) service instances that control HNB and UE access to HNB-GW sessions.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw access-control-db { hnbgw-service hnbgw_svc_name | imsi imsi_value}
> hnbgw-service hnbgw_svc_name
> Displays Access Control database records for an existing HNB-GW service specified as an alphanumeric string of 1 through 63 characters.
> imsi imsi_value
> Specifies the International Mobile Subscriber Identification (IMSI) number which is found on the Access Control database for he HNB-GW service.
> imsi_value is an integer consisting of the 3-digit MCC (Mobile Country Code), the 2- or 3-digit MNC (Mobile Network Code) followed by the MSIN (Mobile Subscriber Identification Number). The total IMSI value must not exceed 15 digits.
> Usage
> This command displays the white list IMSI records in an Access Control database residing on Home-NodeB Gateway (HNB-GW) service instances. The white list controls HNB and UE access to HNB-GW sessions. Access Control database records can be filtered by HNB-GW service or IMSI value.
> Example
> The following command displays the information for registered IMSIs and their status in the HNB-GW database named hnbgw1:
> show hnbgw access-control-db hnbgw-service hnbgw1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hnbgw counters
> Displays the session counter information for Home-NodeB Gateway (HNB-GW) services connected on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw counters [ hnbgw-service hnbgw_svc_name | hnbid hnb_identifier ] [ | { grep grep_options | more } ]
> hnbgw-service hnbgw_svc_name
> Filters the counter display based on an existing HNB-GW service name specified as an alphanumeric string of 1 through 63 characters.
> hnbid hnb_identifier
> Filters the counter display based on a Home-NodeB identifier specified as an alphanumeric string of 1 through 255 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter.
> Usage
> Use this command to view the session counter information for HNB-GW services configured and HNBs connected on this system.
> Example
> The following command displays the counters for the HNB-GW service named hnbgw1:
> show hnbgw counter hnbgw-service hnbgw1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hnbgw sessions
> Displays the active/dormant session information about registered HNB(s) on Home-NodeB Gateway (HNB-GW) service instances configured and running on this system based on different filter criteria.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw sessions [full | summary] [all] [address hnb_ip_address | cell-id cell_id | hnb-access-mode [open | closed] | hnb-local-id hnb_id | hnbgw-service hnbgw_svc_name | hnbid hnb_glbl_id | mcc mcc | mnc mnc [lac lac | rac rac | rnc rnc]] [ | {grep grep_options | more }]
> full
> Displays the full information for a specific registered HNB session(s) on an HNB-GW service instance running on the system. The display can be filtered based on given filtering criteria.
> summary
> Displays summarized information for a specific registered HNB session(s) on an HNB-GW service instance running on the system. The display can be filtered based on given filtering criteria.
> all
> Displays summarized information for all registered HNB sessions on an HNB-GW service instance running on the system. The display can be filtered based on given filtering criteria.
> address hnb_ip_address
> Filters the display of full or summarized session statistics to show only HNB session(s) based on the registered HNB IP address expressed in IPv4 dotted-decimal notation.
> cell-id cell_id
> Filters the display of full or summarized session statistics to show only HNB session(s) based on the registered Femto cell ID where the user/subscriber is geographically located. and must be an integer from 0 through 268435455.cell_id is an integer from 0 through 268435455.
> hnb-access-mode [open | closed]
> Filters the display of full or summarized session statistics to show only HNB session(s) based on the HNB access mode in an HNB-GW service instance.

> • | open filters the session statistics for open HNBs connected with HNB-GW service instance in Open Access mode.

> • | closed filters the session statistics for closed HNBs connected with HNB-GW service instance in Closed Access mode.

> hnb-local-id hnb_id
> Filters the display of full or summarized session statistics to show only HNB session(s) based on the registered local ID of HNB specified as an integer from 1 through 25.
> hnbgw-service hnbgw_svc_name
> Filters the display of session statistics to show only registered HNB session(s) based on an existing HNB-GW service name specified as an alphanumeric string of 1 through 63 characters.
> hnbid hnb_glbl_id
> Displays summarized or full information of HNB session(s) based on the registered global ID of HNB specified as an integer between 1 through 255.
> mcc mcc
> Displays summary information of HNB session(s) based on the registered Mobile Country Code (MCC) identification number of the UE specified as an integer between 101 through 999.
> mnc mnc
> Displays summarized or full information of HNB session(s) based on the registered Mobile Network Code (MCC) identification number of the UE specified as a 2- or 3-digit integer between 00 through 999.
> lac lac
> Displays summarized or full information for HNB session(s) based on the registered Location Area Code (LAC) identification number of the UE specified as an integer between 1 through 65535.
> rac rac
> Displays summarized or full information for HNB session(s) based on the registered Radio Access Code (RAC) identification number of the UE specified as an integer between 1 through 255.
> rnc rnc
> Displays summarized or full information for HNB session(s) based on the registered Radio Network Code (RAC) identification number of the HNB specified as an integer between 1 through 65535.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter.
> Usage
> Use this command to view the session statistics of all or specific registered HNB session(s) or in selected part of user session for HNB-GW services configured and running on this system.
> Example
> The following command displays summarized session statistics for all registered HNBs on the HNB-GW service named hnbgw1:
> show hnbgw sessions summary hnbgw-service hnbgw1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hnbgw statistics hnbgw-service
> Displays the session statistics for Home-NodeB Gateway (HNB-GW) services configured and running on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw statistics hnbgw-service hnbgw_svc_name [ hnbap-only | ranap-only | rua-only | sccp-only | sctp-only ] [ verbose] [ | { grep grep_options | more } ]
> hnbgw-service hnbgw_svc_name
> Filters the display of session statistics for an existing HNB-GW service name specified as an alphanumeric string of 1 through 63 characters.
> hnbap-only
> Filters the display of session statistics to show only Home NodeB Application Part (HNBAP) traffic for the selected HNB-GW service which is configured and running on this system.
> ranap-only
> Flitters the display of session statistics t to show only Radio Access Network Application Protocol (RANAP) traffic for the selected HNB-GW service which is configured and running on this system.
> rua-only
> Filters the display of session statistics to show only RANAP User Adaptation (RUA) traffic for the selected HNB-GW service which is configured and running on this system.
> sccp-only
> Filters the display of session statistics to show only Signaling Connection Control Part (SCCP) traffic for the selected HNB-GW service which is configured and running on this system.
> sctp-only
> Filters the display of session statistics to show only Stream Control Transmission Protocol (SCTP) traffic for selected HNB-GW service which is configured and running on this system.
> verbose
> Displays detailed statistics for all sessions on HNB-GW services or for a selected filtered and named HNB-GW service which is configured and running on this system.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter.
> Usage
> Use this command to view the session statistics for overall session or in selected part of user session for HNB-GW services configured and running on this system.
> Example
> The following command displays session statistics for the HNBAP part of session details for the HNB-GW service named hnbgw1:
> show hnbgw statistics hnbgw-service hnbgw1 hnbap-only
> The following command displays session statistics for the RANAP part of session with maximum details for the HNB-GW service named hnbgw1:
> show hnbgw statistics hnbgw-service hnbgw1 ranap-only verbose
> show hnbgw statistics hnbid
> Displays the session statistics for Home-NodeB (HNB) connected to an HNB-GW service on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw statistics hnbid hnb_identifier [ hnbap-only | ranap-only | rua -only] [ verbose] [ | { grep grep_options | more } ]
> hnbid hnb_identifier
> Filters the display of session statistics based on an existing Home-NodeB identifier specified as an alphanumeric string of 1 through 255 characters.
> hnbap-only
> Filters the display of session statistics display to show only Home NodeB Application Part (HNBAP) traffic for the selected HNB which is connected to this system through HNB-GW service.
> ranap-only
> Filters the display of session statistics display to show only Radio Access Network Application Protocol (RANAP) traffic for the selected HNB which is connected to this system through HNB-GW service.
> rua-only
> Filters the display of session statistics display to show only RANAP User Adaptation (RUA) traffic for the selected HNB which is connected to this system through HNB-GW service.
> verbose
> Displays detailed statistics for all HNB sessions or for the selected filter and HNB which is connected to this system through HNB-GW service.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in Command Line Interface Overview chapter.
> Usage
> Use this command to view the session statistics for overall session or in selected part of user session for selected HNB which is connected to this system through HNB-GW service.
> Example
> The following command displays session statistics for the HNBAP part of session details for the HNB identified as hnb112234 on this system:
> show hnbgw statistics hnbid hnb112234 hnbap-only
> The following command displays detailed session statistics for the RANAP part of session details for the HNB identified as hnb112234 on this system:
> show hnbgw statistics hnbid hnb112234 ranap-only verbose
> show hnbgw-service
> Displays the configuration details for configured HNB-GW service(s) on this system.
> Product
> HNB-GW
> Privilege
> Inspector
> Syntax
> show hnbgw-service { all | hnbgw-service hnbgw_svc_name }
> all
> Displays configuration and other default parameters for all HNB-GW service configured on this system.
> hnbgw-service hnbgw_svc_name
> Displays configuration and default parameters for an existing HNB-GW service name specified as an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to view the configuration and service parameters set for all or any specific HNB-GW service(s) on this system.
> Example
> The following command displays configuration parameters for all HNB-GW services configured on this system:
> show hnbgw-service all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show hsgw-service
> Displays information for HRPD Serving Gateway (HSGW) services on this system.
> Product
> HSGW
> Privilege
> Inspector
> Syntax
> show hsgw-service { all | name service_name | statistics { all | name service _name } } [ pcf-status [ address IPv4_address | filter { all | icmp-monitored | no-calls | summary | up } ] [ | { grep grep_options | more } ]
> all
> Displays configuration information for all HSGW services configured on this system.
> name service_name
> Displays configuration information for an existing HSGW service specified as an alphanumeric string of 1 through 63 characters.
> statistics
> Displays node-level statistics for the HSGW.
> pcf-status
> Displays information about status of Packet Control Functions (PCFs) being monitored.
> address IPv4_address
> Displays status information for the specified PCF.
> IPv4_address must be specified using IPv4 dotted-decimal notation.
> filter { all | icmp-monitored | no-calls | summary | up }
> Filters the PCF status information. Must be followed by the filter to be applied.
> all: Shows all the PCFs.
> icmp-monitored: Shows only PCFs which are ICMP monitored.
> no-calls: Shows only PCFs which has no active sessions.
> summary: Shows only a summary of the status of the PCFs.
> up: Shows only PCFs which are alive.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of Chapter 1 of the Command Line Interface Reference Guide.
> Usage
> Use this command to view configuration information for HSGW services on this system.
> Example
> The following command displays service statistics for the HSGW service named hsgw1:
> show hsgw-service name hsgw1
> show hss-peer-service
> Displays service, session, and statistics information for Home Subscriber Server (HSS) peer services configured on this system.
> Product
> MME
> Privilege
> Inspector
> Syntax
> show hss-peer-service { service { all | name name } | session { all | callid id | full | mdn mdn | nai nai | summary } | statistics { all | service name | summary } } [ | { grep grep_options | more } ]
> service { all | name name }
> Displays HSS peer service statistics for HSS peer services configured on this system.
> all: Displays HSS peer service statistics for all configured HSS peer services on this system.
> name name: Displays HSS peer service statistics for an existing HSS peer service specified as an alphanumeric string of 1 through 63 characters.
> session { all | callid id | full | mdn mdn | nai nai | summary }
> Displays HSS peer service statistics for sessions on this system.
> all: Displays HSS peer service statistics for all sessions on this system.
> This keyword is also used to further filter the full and summary options.
> callid id: Displays summarized or detailed statistics of HSS peer service sessions running and filtered on the basis of the call identifier specified as an 8-digit hexadecimal number.
> This keyword is also used to further filter the full and summary options.
> mdn mdn: Displays summarized or detailed statistics of MME sessions running and filtered on the basis of an existing Mobile Directory Number (MDN) expressed as an alphanumeric string of 1 through 100 characters.
> This keyword is also used to further filter the full and summary options.
> nai nai: Displays summarized or detailed statistics of MME-HSS sessions running and filtered on the basis of an existing Network Access Identifier (NAI) expressed as an alphanumeric string of 1 through 128 characters.
> This keyword is also used to further filter the full and summary options.
> summary: Displays a summarized output of session information. This keyword can be further filtered by adding the following options:

> • | full

> • | callid id

> • | mdn mdn

> • | nai nai

> statistics { all | service name | summary }
> Displays statistics for HSS peer services configured on this system.
> all: Displays statistics for all HSS peer services configured on this system.
> service name: Displays statistics for a an existing HSS peer service expressed as an alphanumeric string of 1 through 63 characters.
> summary: Displays summarized statistics for all HSS peer services configured on this system.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter of the Command Line Interface Reference.
> Usage
> Use this command to display service, session, and statistics information for HSS peer services configured on this system.
> Example
> The following command displays HSS peer service information and statistics for a session with a call ID of 08f11fa4:
> show hss-peer-service sessions full callid 08f11fa4
> show imei-profile
> Displays information for configured International Mobile Equipment Identity (IMEI) profiles.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show imei-profile { all | full { all | name imei_name } | name imei_name } [ | { grep grep_options | more } ]
> all
> Lists all IMEI profiles configured on the system.
> full { all | name apn_name }
> full: Instructs the system to display all information in the IMEI profile(s).
> all: Displays a full set of information for all IMEI profiles configured on the system.
> name imei_name: Displays a full set of information for a specific IMEI profile.
> apn_name: Must be an existing IMEI profile expressed as an alphanumeric string of 1 through 64 characters.
> name imei_name
> Displays information for a specific IMEI profile expressed as an alphanumeric string of 1 through 64 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information for IMEI profiles configured on the system. APN profiles are configured through the global configuration mode and in the IMEI profile configuration mode. For more information regarding IMEI profile commands, refer to the IMEI Profile Configuration Mode Commands chapter.
> Example
> The following command displays all available information for an IMEI profile named imeiprof1:
> show imei-profile full name imeiprof1
> show ims-authorization policy-control
> Displays information and statistics specific to the policy control in IP Multimedia Subsystem (IMS) authorization service.
> Product
> SCM, GGSN, IMS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ims-authorization policy-control statistics [ service ims_auth_svc_name | server { ip-address ip_address [ port port_value ] | name server_name } ] [ | { grep grep_options | more } ]
> statistics
> Displays the total collected statistics of all policy control parameters of IMS authorization service sessions since the last system restart or clear command.
> service ims_auth_svc_name
> Displays the total collected statistics of all IMS authorization sessions processed by a specific IMS authorization service since the last system restart or clear command. ims_auth_svc_name must be an existing IMS authorization service name, expressed as an alphanumeric string of 1 through 64 characters.
> server { ip-address ip_address [ port port_value ] | name server_name }
> Displays the server-level message statistics and the server IP address.
> Specify the PCRF server name (1 through 64 alphanumeric characters), or server IP address in IPv4 dotted-decimal or IPv6 colon-separated notation.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information and statistics about policy control configuration in existing IMS authorization services.
> Example
> The following command displays the existing IMS authorization service name ims_auth_gx1 on the system:
> show ims-authorization policy-control statistics service ims_auth_gx1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization policy-gate
> Displays information of installed Policy Gates for specific subscriber in an IP Multimedia Subsystem (IMS) authorization (IMSA) service.
> Product
> SCM, GGSN, IMS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ims-authorization policy-gate { { status [ summary | full ] [ { imsi imsi_value [ nsapi nsapi_value ] } | callid call_id | { ims-auth-service ims_auth_svc } [ rulename rule_name ] } | { counters [ all | { imsi imsi_value [ nsapi nsapi_value ] } | { rulename rule_name} | { callid call_id } ] } [ | { grep grep_options | more } ] ]
> status [ summary | full ]
> Displays the status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based on the specified criteria.
> summary: Limits the display to a summary on the status of the installed policy gates and their flow definitions along with their run-time status in an IMS authorization service based on the specified criteria.
> full: Displays the full information on status of the installed policy gates and their flow definitions along with their run-time status in an IMS authorization service based on the specified criteria.
> counters all
> Displays the counters/statistics of the installed policy gates and their flow definitions along with their run-time status in an IMS authorization service based on the specified criteria.
> all displays all counters of the installed gates and their flow definitions along with their run-time status in an IMS authorization service based on the specified criteria.
> imsi imsi_value [ nsapi nsapi_value ]
> Displays all of the counters/status of the installed policy gates and their flow definitions along with the run-time status in an IMS authorization service based on the International Mobile Subscriber Identity (IMSI).
> nsapi nsapi_value specifies the Network Service Access Point Identifier (NSAPI) and limits the display to a single PDP context of the subscriber.
> callid call_id
> Displays all of the counters/status of the installed policy gates and their flow definitions along with their run-time status in an IMS authorization service based on the call identifier.
> ims-auth-service ims_auth_svc
> Displays the status of the installed policy gates and their flow definitions along with their run-time status in the named IMS authorization service.
> rulename rule_name
> Displays all of the counters/status of the installed policy gates and their flow definitions along with their run-time status in an IMS authorization service based on the named dynamic charging rule.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display information/statistics/counters about all of the installed policy gates and their flow definitions along with the run-time status with specified criteria and filters in existing IMS authorization services.
> Example
> The following command displays the full status of the installed policy gates in an existing IMS authorization service on the system:
> show ims-authorization policy-gate status full
> The following command displays the all counters of the installed policy gates in an existing IMS authorization service on the system:
> show ims-authorization policy-gate counters all
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization servers
> Displays information and statistics specific to the authorization servers used for IP Multimedia Subsystem (IMS) authorization (IMSA) service.
> Product
> SCM, GGSN, IMS
> Privilege
> Security Administrator, Administrator
> Syntax
> show ims-authorization servers [ ims-auth-service ims_auth_svc_name [ | { grep grep_options | more } ] ]
> server [ ims-auth-service ims_auth_svc_name ]
> Displays the information and statistics for all authorization servers configured within an IMS authorization service in a system.
> ims-auth-service ims_auth_svc_name: Displays the configured authorization servers for IMS authorization within the named IMS authorization service.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display information and statistics about IMS authorization servers configured on a system or IMS authorization service.
> Example
> The following command displays the information and statistics of the authorization servers in the IMS authorization service named in ims_auth_gx1:
> show ims-authorization servers ims-auth-service ims_auth_gx1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization service
> Displays information, configuration, and statistics of all/specific IP Multimedia Subsystem (IMS) authorization (IMSA) service.
> Product
> SCM, GGSN, IMS
> Privilege
> Security Administrator, Administrator
> Syntax
> show ims-authorization service { { all [ verbose ] | name ims_auth_svc_name | summary ] } | { statistics [ all | name ims_auth_svc_name ] [ verbose ] } [ | { grep grep_options | more } ]
> all [ verbose ]
> Displays information and configuration for all configured IMS authorization services with a single line of information for each IMS authorization service.
> verbose: Displays all information and configuration data for all IMS authorization services configured on system.
> name ims_auth_svc_name ]
> Displays the information, statistics, and configuration data for the named IMS authorization service.
> summary
> Displays summarized information and configuration data for all IMS authorization services configured in a system.
> statistics [ all | name ims_auth_svc_name ] [ verbose ]
> Displays the IMS Authorization service statistics including following information:

> • | Initial authorization procedures

> • | Re-authorization procedures initiated by us

> • | Re-authorization procedures initiated by servers

> • | Various failure statistics

> If no criteria are specified, only summarized statistics for all IMS Authorization services are displayed

> • | all: displays individual statistics for every IMS authorization service configured on system.

> • | name ims_auth_svc_name: Displays the statistics for the IMS authorization service named in ims_auth_svc_name

> • | verbose: displays detailed statistics for a configured IMS authorization service.

> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display the status, counters and configuration. for an IMS Authorization service. The status includes the state of a server table switchover. The Statistics option displays information about various processes.
> Example
> The following command displays the information and configuration data of the IMS authorization service named in ims_auth_gx1:
> show ims-authorization service name ims_auth_gx1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ims-authorization sessions
> Displays information, configuration, and statistics of sessions active in an IP Multimedia Subsystem (IMS) authorization (IMSA) service.
> Product
> SCM, GGSN, IMS
> Privilege
> Security Administrator, Administrator
> Syntax
> show ims-authorization session [ full | summary | ggsn-only ] | [ all | [ ims-auth-service ims_auth_svc_name | imsi imsi_value [ nsapi nsapi_value ] | apn apn_name | ip-address ip_address | callid call_id ] [ | { grep grep_options | more } ] ]
> full
> Displays complete information and configuration data for all sessions in IMS authorization services configured in a system.
> summary
> Displays summarized information and configuration data for all sessions in IMS authorization services configured in a system.
> ggsn-only
> Displays GGSN-specific information in addition to detailed information about the session.
> all
> Displays information and configuration for all sessions running in IMS authorization services with a single line of information for each IMS authorization session.
> ims-auth-service ims_auth_svc_name ]
> Displays the information, statistics, and configuration data for sessions in the named IMS authorization service.
> imsi imsi_value [ nsapi nsapi_value ]
> Displays all of the counters/status of the running services in an IMS authorization service based on the specified International Mobile Subscriber Identity (IMSI) and Network Service Access Point Identifier (NSAPI). The display is limited to a single PDP context of the subscriber.
> apn apn_name
> Displays all of the counters/status for the running services in an IMS authorization service based on the specified Access Point Name (APN).
> ip-address ip_address
> Displays all of the counters/status for the running services in IMS authorization service based on the specified host IP address.
> callid call_id
> Displays all of the counters/status for the running services in IMS authorization service based on the named call identifier.
> summary
> Displays summarized information and configuration data for all IMS authorization services configured in a system.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> Please refer to the Regulating a Command’s Output section of the Command Line Interface Reference for details on the usage of grep and more.
> Usage
> Use this command to display the sessions running under IMS Authorization service on a system with different filter criteria.
> Example
> The following command displays the information and statistical data for a session in an IMS authorization service:
> show ims-authorization sessions full
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ip
> Displays information for the IP-based interface access group and access control list (ACL) along with the address resolution protocol (ARP) information for the current context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip { access-group [ statistics] | access-list [ list_name ] | arp [ arp_ip_address ] | [ summary ] | statistics ] ] | localhosts [ host_name ] | prefix-list [ detail [ list_name ] | name list_name | summary [ list_name ] ] | rip | route [ route_ip_address [ route_gw_address ] ] | static-route sroute_ip_address [ sroute_gw_address ] | vrf vrf-name} [ | { grep grep_options | more } ]
> access-group [ statistics ]
> Displays all configured access groups in the current context along with their priority values.
> statistics: Displays all configured access groups along with packet and byte counters for each ACL rule hit for the current context. It also shows the priority values.
> access-list [ list_name ]
> Indicates the output is to display the information for all ACLs or the named ACL.
> arp [ arp_ip_address ]
> Displays the ARP table or the ARP information associated with the IP address specified using IPv4 dotted-decimal or IPv6 colon-separated notation.
> Important: When it restarts, the VPN Manager removes all interfaces from the kernel; the kernel then removes all ARP entries. When this happens, the NPU still holds all of the ARP entries so that there is no traffic disruption. From a user point of view, show ip arp is broken since this command gathers information from the kernel and not the NPU.
> localhosts [ host_name ]
> Displays all the local host information or only for the named host.
> prefix-list [ detail [ list_name ] | name list_name | summary [ list_name ] ]
> Displays information on configured IP prefix lists. With no keyword supplied, a list of all prefix lists and their entries is displayed.
> detail [ list_name ]: Lists detailed information for all prefix lists and their entries. If a list name is specified only the details for the specified prefix list are displayed. list_name is an alphanumeric string of 1 through 79 characters.
> name list_nam: Lists the entries for an existing prefix list specified as an alphanumeric string of 1 through 79 characters.
> summary [ list_name ]: Lists summary information for all prefix lists and their entries. If a list name is specified, only the summary for the specified prefix list are displayed. list_name is an alphanumeric string of 1 through 79 characters.
> rip
> Displays general Routing Information Protocol (RIP) routing process information. (RIP is not supported at this time.)
> route [ route_ip_address [ route_gw_address ] ]
> displays the route information to the specified IP address. The route gateway address may be specified as needed to identify the route. The IP addresses are specified using tIPv4 dotted-decimal or IPv6 colon-separated notation.
> static-route sroute_ip_address [ sroute_gw_address ]
> Displays the static route information for the specified IP address. The static route gateway address may also be specified to identify the route. the IP addresses are specified using IPv4 dotted-decimal or IPv6 colon-separated notation.
> vrf vrf_name
> Displays Virtual Routing and Forwarding (VRF) information for the named VRF.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Show the IP information to verify and/or troubleshooting communication difficulties between to a remote host/node.
> Example
> The following command displays the ACL for the list named sampleACL.
> show ip access-list sampleACL
> The following command will output the static route information to remote host 10.2.3.4.
> show ip static-route 10.2.3.4
> show ip as-path-access-list
> Displays the contents of a Border Gateway Protocol (BGP) router Autonomous System (AS) path access list in the current context.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip as-path-access-list list_name
> list_name
> Specifies the name of an existing AS path access list configured in the current context as an alphanumeric string of 1 through 79 characters.
> Usage
> Use this command to display the configured entries for the specified BGP router AS path access list in the current context.
> Example
> The following command displays the contents of an AS path access list named ASlist1:
> show ip as-path-access-list ASlist1
> show ip bgp
> Displays Border Gateway Protocol (BGP) information for the current context.
> Product
> HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip bgp [ ip_address/mask | debugging | filter-list list_name | neighbors [ ip_adrress ] | route-map map_name | vpnv4 { all [ network | neighbors | summary ] | vrf vrf-name [ network ] | route-distinguisher [ network | neighbors | summary ] } [ | { grep grep_options | more } ]
> ip_address/mask
> Specifies the IP address and netmask bits for the network for which information should be displayed. The IP address and mask is the number of subnet bits, representing a subnet mask in CIDR notation. These must be entered in the IPv4 dotted-decimal or IPv6 colon-separated CIDR notation.
> debugging
> Displays debug flags that are enabled.
> filter-list list_name
> Displays routes that match the specified filter list.
> neighbors [ip_address]
> Displays information for all neighbors or a neighbor specified as an IP address in IPv4 dotted-decimal or IPv6 colon-separated notation.
> route-map map_name
> Displays routes that match the specified route-map.
> vpnv4 { all [ network | neighbors | summary ] | vrf vrf-name [ network ] | route-distinguisher [ network | neighbors | summary ] }
> Displays all VPNv4 routing data, routing data for a VRF, or a route-distinguisher.

> • | all: Displays all VPN routing information. If this is specified, the information displayed is gathered from all the VRF's known to BGP and displayed. It could contain the list of neighbors, the list of networks, or a particular network

> • | network: Displays the network for which information in the BGP routing table.

> • | neighbors: Displays neighbor information for the all the VRFs including the default VRF or for the VRF with a matching RD value.

> • | summary: Displays summary information of neighbors for all the VRFs including the default VRF or for the VRF with a matching RD value.

> • | vrf vrf name: Displays information only gathered from the named VRF. If there is no such VRF, an error is reported.

> • | network: Displays the network for which information in the BGP routing table.

> • | route-distinguisher: If specified along with the RD value, the information displayed is gathered from the corresponding VRF whose RD value is the same as the specified value. If there is no VRF associated with such an RD, an error is reported.

> • | network: Displays the network for which information in the BGP routing table.

> • | neighbors: Displays neighbor information for the all the VRFs including the default vrf VRF for the VRF with a matching RD value.

> • | summary: shows summary information of neighbors for all the vrfs including the default vrf or for the VRF with a matching RD value.

> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command display to BGP information for the current context.
> Example
> The following command displays information for all BGP neighbors:
> show ip bgp neighbors
> show ip interface
> Displays statistical and configuration information for the IP-based interfaces, including a Virtual Routing and Forwarding (VRF) table for a specific context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip interface [ vrf vrf-name ] [ name intfc_name [ statistics ] [ tunnel [ gre-keepalive ] ] [ summary ] [ | { grep grep_options | more } ]
> vrf vrf_name
> Displays Virtual Routing and Forwarding (VRF) routing information for an existing VRF specified as an alphanumeric string of 1 through 63 characters.
> name intfc_name
> Displays information for an existing interface specified as an alphanumeric string of 1 through 79 characters. If no interface name is specified, the information for all IP interfaces is displayed.
> tunnel [ gre-keepalive ]
> Filters the IP interface information for GRE/IP-in-IP tunnel type interfaces.
> gre-keepalive: Displays the keepalive information for a generic routing encapsulation (GRE) tunnel configured with this IP interface.
> statistics
> Displays the session statistics of all ingress and egress packets processed through this IP interface.
> summary
> Displays summarized information about requested IP interfaces.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display the summarized of detailed configuration and statistical information for a configured IP interface. This information can be used to verify and/or troubleshoot communication difficulties between to a remote host/node.
> Example
> The following command displays the interface information, including statistics, for the IP interface sampleInterface.
> show ip interface sampleInterface statistics
> The following command displays the GRE keepalive information for an IP interface named in IP_gre1.
> show ip interface IP_gre1 unnel gre-keepalive
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ip ospf
> Displays Open Shortest Path First (OSPF) routing information.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip ospf [ border-routers | database [ verbose ] [ ls-id ip_addr ] [ adv-router ip_addr ] [ ls-type { router | network | summary | asbr-summary | external | nssa | integer } ] | debugging | interface | neighbor [ details ] | route | virtual-links ]
> border-routers
> Displays all known area border routers (ABRs) and autonomous system border routers (ASBRs) for OSPF.
> database [ verbose ] [ ls-id ip_addr ] [ adv-router ip_addr ] [ ls-type { router | network | summary | asbr-summary | external | nssa | integer } ]
> Displays a summary of the database information for OSPF.
> verbose: Displays detailed OSPF database information.
> ls-id ip_addr: Displays OSPF database information for the link state advertisements (LSAs) with the specified link state identifier (LSID). ip_addr is entered using IPv4 dotted-decimal notation.
> adv-router ip_addr: Displays OSPF database information for the advertising router with the specified LSID. ip_addr is entered using IPv4 dotted-decimal notation.
> ls-type { router | network | summary | asbr-summary | external | nssa | LSA_Numerical_Type } ]: Displays OSPF database information for the specified LSA type.
> debugging
> Lists which debugging parameters are enabled.
> interface
> Displays interface information for OSPF.
> neighbor [ details ]
> Displays summarized information about all known OSPF neighbors.
> details: Displays detailed information about all known OSPF neighbors.
> route [ summary ]
> Displays the OSPF routing table.
> summary: Displays the number of intra-area, inter-area, external-1 and external-2 routes.
> virtual-links
> Displays the OSPF virtual links.
> Usage
> Use this command to display OSPF information.
> Example
> To display general OSPF information, enter the following command;
> show ip ospf
> show ip policy-forward
> Displays information for IP packet redirecting policy for Home Agent (HA).
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip policy-forward
> Usage
> Use this command to see all the settings for IP packet redirection configuration from existing HA to new HA during upgrade.
> Important: This is a customer specific command.
> Example
> The following command displays forward policy configuration for an HA:
> show ip policy-forward
> show ip pool
> Displays statistics specific to IP pools.
> Product
> PDSN, GGSN, HA, ASN-GW, A-BG
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip pool [ address { pool-name pool_name | group-name group_name } { used | free | hold | release } [ limit limit ] | group-name group_name | groups | hold-timer { imsi imsi | msid msid | username username [ imsi imsi | msid msid ] } | overlap | pool-name pool_name | private | public | resource | static | summary | verbose | wide ]
> address { pool-name pool_name | group-name group_name } { used | free | hold | release} [ limit limit ]
> Displays IP pool addresses for the specified IP pool or pool group that are currently in the specified state.
> pool-name pool_name: Displays IP addresses from an existing IP pool name specified as an alphanumeric string of 1 through 31 characters.
> group-name group_name: Displays IP addresses from an existing IP pool group name specified as an alphanumeric string of 1 through 31 characters.
> used: Displays the IP addresses that are in a used state.
> free: Displays the IP addresses that are in a free state.
> hold: Displays the IP addresses that are in a hold state.
> release: Displays the IP addresses that are in a release state.
> limit limit: Specifies the maximum number of address to display as an integer from 1 through 524287.
> group-name group_name
> Displays information about an existing IP pool group name specified as an alphanumeric string of 1 through 31 characters.
> groups
> Lists information about all IP pool groups.
> hold-timer {imsi imsi | msid msid | username username [imsi imsi | msid msid]}
> Displays hold timer address information for the specified IMSI, MSID, or username.
> imsi imsi: Displays hold-timer information for a valid IMSI (International Mobile Subscriber Identity), specified as a 15-character field that identifies the subscriber’s home country and carrier.
> msid msid: Displays hold-timer information for the MSID specified as a number from 7 through 16 digits.
> username username: Displays hold-timer information for an existing username specified as an alphanumeric string of 1 through 127 characters.
> Important: Active users cannot be displayed. If an active ID or username is entered, the following error message appears: Failure: No address matching the specified information was found! Please confirm that the options used match the network architecture/deployment,i.e. IMSI/MSID only, Username only, or IMSI/MSID plus Username. Please note that this command does not apply for addresses in the used state.
> overlap
> Lists information on overlapping IP pools
> pool-name pool_name
> Displays information about an existing IP pool.
> private
> Displays information about IP pools marked Private.
> public
> Displays information about IP pools marked Public.
> resource
> Displays information about resource IP pools.
> static
> Displays information about static IP pools.
> summary
> Displays a summary of all IP pool information.
> verbose
> Displays detailed information about all IP pools.
> wide
> Displays detailed information formatted to more than 80 columns.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display statistics pertaining to IP Pools in the current context.
> Example
> The following command displays IP address information for an IP Pool named pool1:
> show ip pool address pool-name pool
> To display a summary list for all IP pools in the current context, enter the following command:
> show ip pool summary
> The following command displays IP pool information for all IP pools configured in the current context:
> show ip pool verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ip ipsp
> Displays the names of IP pools that are enabled for the IP pool sharing protocol (IPSP) and lists the disposition of addresses in the pools.
> Product
> PDSN, HA, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip ipsp [ summary ]
> summary
> Displays only the disposition of the addresses in the participating IP pools. Does not show the names of the participating IP pools.
> Usage
> Use this command to list the names of IP pools that are participating in the IPSP and list the disposition of IP addresses in those pools.
> Important: For information on configuring and using IPSP refer to the System Administration Guide.
> Example
> To list information on all IPSP participating pools and address disposition, enter the following command:
> show ip ipsp
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ip traffic sctp
> Displays statistics that track Stream Control Transmission Control (SCTP) packets. This command obtains kernel SCTP traffic information for the specified card and CPU in a particular context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ip traffic sctp card <slot_number> cpu <cpu_number>
> card <slot_number>
> Displays SCTP traffic for the card in slot number 1, 2, 8 or 9.
> cpu <cpu_number>
> Displays SCTP traffic for CPU number 0, 1, 2 or 3 on the specified card.
> Usage
> Use this command to debug the flow of SCTP traffic to a CPU kernel.
> Example
> To display SCTP traffic statistics for CPU 0 on the SMC in slot 8 enter the following command:
> show ip traffic sctp card 8 cpu 0
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ipms status
> Displays the status of Intelligent Packet Monitoring System (IPMS) client service with information related to system and call events. It also displays the status of configured IPMS servers.
> Product
> IPMS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipms status [ summary | all | server address ip_address ]
> summary
> Displays the summary of all configured IPMS client and IPMS servers.
> all
> Displays information for all configured IPMS client and IPMS servers.
> server address ip_address
> Displays status for the IPMS server specified as an IP address in IPv4 dotted-decimal or IPv6 colon-separated notation.
> Usage
> This command is used to show/verify the status or configuration of one or all IPMS server along with system and call event information.
> Example
> The following command displays status of an IPMS server with IP address 10.2.3.4:
> show ipms status server address 10.2.3.4
> show ipsg
> Displays information and statistics specific to the IP Services Gateway (IPSG) service.
> Product
> IPSG
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipsg { service { all [ counters ] | name name } | sessions { all | callid num | counters { criteria } | full { criteria } | ip-address address | msid num | peer-address address | summary { criteria } | username name } | statistics [ name name | peer-address address ] } [ | { grep grep_options | more } ]
> service { all [ counters ] | name name }
> Displays information about the configured IPSG service.
> all [ counters ]: Displays information about all of the configured IPSG services on the system.
> name name: Displays information about an existing IPSG service specified as an alphanumeric string of 1 through 63 characters.
> sessions { all | callid num | counters { criteria } | full { criteria } | imsi num | ip-address address | msid num | peer-address address | summary { criteria } | username name }
> all: Displays session information including call ID, NAI, and home address for all current IPSG sessions. This is the default behavior for the sessions keyword.
> callid num: Displays session information for a current IPSG session based on the call ID specified as an 8-digit hexadecimal number.
> counters { criteria }: Displays session counters for sessions matching the criteria. (See criteria below.)
> full { criteria }: Displays all available session information for sessions matching the criteria. (See criteria below.)
> ip-address address:
> msid num: Displays session information for a current IPSG session based on the MSID. num must be an existing IPSG service session MSID, expressed as an 8-digit hexadecimal number.
> peer-address address: Displays session information for a current IPSG session based on the IP address of the device sending the RADIUS accounting messages. address must be an existing IPSG service session IP address for the device sending the RADIUS accounting messages, entered using IPv4 dotted-decimal notation.
> summary { criteria }: Displays a summary of available session information for sessions matching the criteria. (See criteria below.)
> username name: Displays session information for a IPSG session based on the username of the subscriber specified as an alphanumeric string of 1 through 127 characters.
> criteria:
> all: Displays session information for all existing IPSG service sessions.
> callid num: Displays session information for a specific IPSG session based on the call ID specified as an 8-digit hexadecimal number.
> ip-address address: Displays session information for a specific IPSG session based on the IP address of the subscriber specified in IPv4 dotted-decimal notation.
> msid num: Displays session information for an IPSG session based on the MSID.
> peer-address address: Displays session information for a current IPSG session based on the IP address of the device sending the RADIUS accounting messages. address must be an existing IPSG service session IP address for the device sending the RADIUS accounting messages, entered using IPv4 dotted-decimal notation.
> username name: Displays session information for a specific IPSG session based on the username of the subscriber. name is an existing IPSG service session subscriber username, expressed as an alphanumeric string of 1 through 127 characters.
> statistics [ name name | peer-address address ]
> Displays the total collected statistics of all IPSG sessions since the last system restart or clear command.
> name name: Displays the total collected statistics of all IPSG sessions processed by a specific service since the last system restart or clear command. name must be an existing IPSG service name expressed as an alphanumeric string of 1 through 63 characters.
> peer-address address: Displays the total collected statistics of all IPSG sessions associated with a specific IP address of the device responsible for sending the RADIUS accounting messages. Displayed statistics are from the last system restart or clear command.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to display information and statistics about existing IPSG services.
> Example
> The following command displays the existing IPSG services on the system:
> show ipsg service all
> The following command displays all the existing IPSG service sessions on the system:
> show ipsg session all
> The following command displays the cumulative IPSG session statistics on the system:
> show ipsg statistics
> The following command displays the cumulative IPSG session statistics on the system for an IPSG service named ipsg1:
> show ipsg statistics name ipsg1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ipv6
> Displays information for each rule in an IPv6 access control group.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 { access-group [ statistics ] [ | { grep grep_options | more } ] | access-list [list_name ] [ | { grep grep_options | more } ] | interface [ name interface_name [ statistics ] | summary | vrf vrf_name | | { grep grep_options | more } ] | neighbors [ IPv6-ADDRESS ] [vrf vrf_name] | [ | { grep grep_options | more } ] }
> access-group
> Displays all configured access groups in the current context along with the priority values.
> statistics
> Displays statistics for each rule in an IPv6 access control group.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> access-list [ list_name ]
> Displays IPv6 access control list information an existing access list name specified as an alphanumeric string of 1 through 47 characters.
> interface
> Displays interface information for the current context.
> name interface_name
> Displays detailed information for an existing interface name specified as an alphameric string of 1 through 79 characters.
> statistics
> Displays the number of inbound and outbound IP packets registered by kernel.
> summary
> Displays summary information about all IP interfaces.
> vrf vrf_name
> Displays information related to an existing VRF specified as an alphanumeric string of 1 through 63 characters.
> neighbors [ ipv6_address ]
> the IP address specified in IPv6 colon-separated notation.
> Usage
> Show the IPv6 information to verify and/or troubleshoot communication between/to a remote host/node.
> Example
> The following command displays the ACL for the list named sampleACL.
> show ipv6 access-list sampleACL samplev6ACL
> The following command displays the interface information, including statistics, for the IPv6 interface samplev6interface.
> show ipv6 interface name samplev6interface statistics
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show ipv6 ospf
> Displays information regarding the configuration of the OSPFv3 Protocol on this system.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 ospf [ database | debugging | interface | nieghbor | route | virtual-links ] [ verbose [ verbose ] [ | { grep grep_options | more } ]
> show ipv6 ospf database [ adv-router ipv4-address ] [ ls-type { external | inter-prefix | inter-router | intra-prefix | link | network | router }
> show ipv6 ospf debugging
> show ipv6 ospf interface
> show ipv6 ospf neighbor [ details]
> show ipv6 ospf route [ summary ]
> show ipv6 ospf virtual-links
> show ipv6 ospf database
> Displays the OSPFv3 database including the following components.

> • | adv-router ipv4-address: Displays OSPF database information from the advertising router specified as an IP address in IPv4 dotted-decimal notation.

> • | ls-type: Displays the specified Link-State Advertisement (LSA) type, which can be one of the following:

> • | external: Display External LSA information

> • | inter-prefix: Displays Inter Area Prefix LSA information

> • | inter-router: Displays Inter Area Router LSA information

> • | intra-prefix: Displays Intra Area Prefix LSA information

> • | link: Displays Link LSA information

> • | network: Displays Network LSA information

> • | router: Displays Router LSA information

> show ipv6 ospf debugging
> Displays OSPFv3 Debugging Flags.
> show ipv6 ospf interface
> Displays OSPFv3 Interfaces.
> show ipv6 ospf neighbor [ details ]
> Displays OSPFv3 neighbors with the option for full details.
> show ipv6 ospf route [ summary ]
> Displays OSPFv3 route information with the option for summarized information.
> show ipv6 ospf virtual-links
> Displays OSPFv3 virtual links.
> verbose
> Displays detailed information.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to see all OSPFv3 information.
> Example
> The following command displays ipv6 ospf information:
> show ipv6 ospf
> show ipv6 pool
> Displays information related IPv6 Pool configuration/state.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 pool[ group-name group-name ] [ pool-name pool-name ] [ summary ] [ verbose ] [ | { grep grep_options | more } ]
> group-name group-name
> Displays IP address pool information for an existing group-name specified as an alphanumeric string of 1 through 31 characters.
> pool-name pool-name
> Displays IPv6 address pool information for an existing pool name specified as an alphanumeric string of 1 through 31 characters.
> summary
> Displays summary information about all IP address pools; this is the default.
> verbose
> Displays detailed information about all IP address pools.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to see all the ipv6 pool information.
> Example
> The following command displays ipv6 pool information:
> show ipv6 pool
> show ipv6 prefix-list
> Displays information related to an IPv6 prefix list.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 prefix-list[ detail prefix-list-name ] [ name prefix-list-name [ ip-address/mask [ longer ] [ match-first ] ] [ seq seq_value ] ] [ summary prefix-list-name] [ | { grep grep_options | more } ]
> detail prefix-list-name
> Displays detailed IP address information for an existing prefix-list specified as an alphanumeric string of 1 through 79 characters.
> name prefix-list-name
> Displays IP address information for an existing prefix-list specified as an alphanumeric string of 1 through 79 characters.
> ip-address/mask
> Specifies an IPv6 Network Address/Mask Bits combination in CIDR notation.
> longer
> Displays IP address prefix-list details in longer format.
> match-first
> Displays first matched IP address prefix-list details.
> seq seq_value
> Specifies the sequence number as an integer from 1 through 4294967295.
> seq_value is the integer value between 1 through 4294967295.
> summary prefix-list-name
> Displays prefix-list summary for an existing prefix-list specified as an alphanumeric string of 1 through 79 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to see all the ipv6 prefix-list information.
> Example
> The following command displays ipv6 prefix-list information:
> show ipv6 prefix-list
> show ipv6 route
> Displays information related to specific route for current context.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 route [ ip-address/mask ] [ vrf vrf-name ] [ | { grep grep_options | more } ]
> ip-address/mask
> Specifies an IP address entered using IPv6 colon-separated and CIDR notation.
> vrf vrf-name
> Displays Virtual Routing and Forwarding (VRF) routing information for an existing VRF specified as an alphanumeric string of 1 through 63 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to see all the ipv6 route information.
> Example
> The following command displays ipv6 route information:
> show ipv6 route 2001:0db8:85a3:0000:0000:8a2e:0370:7334/5
> show ipv6 route-access-list
> Displays the route access list.
> Product
> PDSN, GGSN, ASN-GW
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show ipv6 route-access-list [ route-access-list ] [ | { grep grep_options | more } ]
> route-access-list
> route-access-list is an alphanumeric string of 1 through 79 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to see all the IPv6 route access list information.
> Example
> The following command displays ipv6 route access list information:
> show ipv6 route-access-list
> show iups-service
> Displays information for Iu-PS services in the current context. The IuPS interface links the Radio Network Controller (RNC) with the Packet Switched Core Network.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show iups-service { all | name srvc_name} [ gtpu-table | rnc { all | id rnc_id } ] [ | { grep grep_options | more } ]
> all
> Shows information for all configured IuPS services.
> name srvc_name
> Specifies an existing IuPS service as an alphanumeric string of 1 through 63 characters.
> gtpu-table
> Displays the configured GTPU database.
> rnc all
> Displays information for all configured RNCs.
> rnc rnc_id
> Specifies the identification number of an existing RNC configuration instance as an integer from 0 through 4095.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Iu-PS services control the interface between the SGSN and the RNCs in the UMTS radio access network (UTRAN). Iu-PS services include the control plane and the data plane between these nodes.
> Use this command to display information for a specific Iu-PS service or for all Iu-PS services configured within the context. A filtering keyword can limit the display to only information for a specific RNC or for a GTPU table in the Iu-PS service configuration.
> Example
> The next command displays information for all Iu-PS services configured in the current context:
> show iups-service all
> This command displays information for a specific RNC for a specific Iu-PS services:
> show iups-service name iups-svc-1 rnc 123name
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show l2tp sessions
> Displays information for Layer 2 Tunneling Protocol (L2TP) tunnels.
> Product
> LNS, PDSN, GGSN, HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show l2tp sessions [ full | summary | counters ] [ all | callid id | username name | msid ms_id | lac-service service_name | lns-service service_name peer-address [ operator ] peer_address ]
> full
> Displays all available information for the specified sessions.
> summary
> Displays a summary of available information for the specified sessions.
> counters
> Displays counters for the specified L2TP sessions.
> all
> Displays all current sessions.
> callid id
> Displays session information for the call ID. specified an 8-byte hexadecimal number. The output of the command show l2tp tunnels contains a field labeled Callid Hint which lists the call ID information to use with this command.
> username name
> Displays session information for an existing subscriber specified as an alphanumeric string of 1 through 127 characters. Wildcard characters $ and * are allowed.
> msid ms_id
> Displays session information for the MSID specified as 7 to 16 digits for an IMSI, MIN, or RMI. Wildcard characters $ and * are allowed.
> lac-service service_name
> Displays all L2TP sessions in the specified LAC service.
> lns-service service_name
> Displays all L2TP sessions in the specified LNS service.
> peer-address [ operator ] peer_address
> Displays all L2TP sessions to the destination (peer LNS) specified as an IP address in IPv4 dotted-decimal notation.
> In conjunction with sessions keyword, indicates a range of peers is to be displayed.
> peer-address [ operator ] peer_address is specified using IPv4 dotted-decimal notation.
> operator implies how to logically specify a range of peer-address and it must be one of the following:

> • | <: IP address less than the specified peer_address

> • | >: IP address less than the specified peer_address

> • | greater-than: IP address less than the specified peer_address

> • | less-than: IP address less than the specified peer_address

> Usage
> Use this command to show information for sessions in the current context.
> Important: If this command is executed from within the local context, cumulative session information is displayed for all contexts.
> Example
> The following command displays cumulative statistics for all sessions processed within the current context:
> show l2tp sessions
> The following command displays all information pertaining to the L2TP session of a subscriber named isp1vpnuser1:
> show l2tp session full username isp1vpnuser1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show l2tp statistics
> Displays statistics for all Layer 2 Tunneling Protocol (L2TP) tunnels and sessions.
> Product
> LNS, PDSN, GGSN, HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show l2tp statistics [ lac-service service_name | lns-service service_name | peer-address peer_ip_address ]
> lac-service service_name
> Displays L2TP statistics for all tunnels and sessions in an existing L2TP Access Concentrator (LAC) service specified as an alphanumeric string of 1 through 63 characters.
> lns-service service_name
> Displays L2TP statistics for all tunnels and sessions in tan existing L2TP Network Server (LNS) service specified as an alphanumeric string of 1 through 63 characters.
> peer-address peer_address
> Displays L2TP statistics for all tunnels and sessions to the destination (peer LNS) at the IP address specified in IPv4 dotted-decimal notation.
> Usage
> Use this command to display statistics for L2TP services.
> Example
> The following command displays statistics for a specific LAC service named vpn1:
> show l2tp statistics lac-service vpn1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show l2tp tunnels
> Displays information for Layer 2 Tunneling Protocol (L2TP) tunnels.
> Product
> LNS, PDSN, GGSN, HA
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show l2tp tunnels [ full | summary | counters ] [ all | callid id | username name | msid ms_id | lac-service service_name | lns-service service_name | peer-address [ operator ] peer_address ]
> full
> Displays all available information for the specified tunnels.
> summary
> Displays a summary of available information for the specified tunnels.
> counters
> Displays counters for the specified L2TP tunnels.
> all
> Displays all current tunnels.
> callid id
> Displays tunnel information for the call id specified as an 8-digit hexadecimal number. The output of the command show l2tp tunnels contains a field labeled Callid Hint which lists the call id information to use with this command.
> username name
> Displays tunnel information for an existing subscriber specified as an alphanumeric string of 1 through 127 characters. Wildcard characters $ and * are allowed.
> msid ms_id
> Displays tunnel information for the MSID specified as 7 to 16 digits for an IMSI, MIN, or RMI. Wildcard characters $ and * are allowed.
> lac-service service_name
> Displays all L2TP tunnels in the specified LAC service.
> lns-service service_name
> Displays all L2TP tunnels in the specified LNS service.
> peer-address [ operator ] peer_address
> Displays all L2TP tunnels to the destination (peer LNS) at the IP address specified in IPv4 dotted-decimal notation.
> In conjunction with tunnels keyword, indicates a range of peers is to be displayed.
> peer-address [ operator ]: Specifies a peer address using IPv4 dotted-decimal notation.
> operator implies how to logically specify a range of peer-address and it must be one of the following:

> • | <: IP address less than the specified peer_address

> • | >: IP address less than the specified peer_address

> • | greater-than: IP address less than the specified peer_address

> • | less-than: IP address less than the specified peer_address

> Usage
> Use this command to show information for tunnels in the current context.
> Example
> The following command displays all of the tunnels currently being facilitated by LAC services within the current context:
> show l2tp tunnels all
> The following command displays information pertaining to the L2TP tunnel(s) established for a LAC-service named vpn1:
> show l2tp tunnels full lac-service vpn1
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show lawful-intercept
> Refer to the Lawful Intercept Configuration Guide for a full description of this command.
> show lawful-intercept ssdf statistics
> Refer to the Lawful Intercept Configuration Guide for a description of these statistics.
> show lac-service
> Displays the information for all L2TP Access Concentrator (LAC) services or for a particular LAC service.
> Product
> PDSN, HA, GGSN
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show lac-service { all | name service_name } [ | { grep grep_options | more } ]
> all
> Display information for all LAC services.
> name service_name
> Display information only for an existing LAC service specified as an alphanumeric string of 1 through 63 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to list information for LAC services configured on this system.
> Example
> The following commands display information for all LAC services and the LAC service named lac1, respectively.
> show lac-service allshow lac-service name lac1
> show leds
> Displays the current status of the light emitting diodes (LEDs) for a specific card or all cards.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show leds { all | card_num } [ | { grep grep_options | more } ]
> all | card_num
> all: Displays the LED status for all cards.
> card_num: Displays the LED status for the card specified by its slot number.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Display the status of the LEDs as a part of an automated periodic script which checks the LEDs of the chassis.
> Important: This command is not supported on all platforms.
> Example
> The following commands display the LED status for all cards and only card 8, respectively.
> show leds all
> show leds 8
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show license information
> Displays information about the licenses installed on this system, as well as the maximum number of sessions.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show license information { key_name | full } | { key } [ | { grep grep_options | more } ]
> key_name | full
> key_name: Displays the information for an existing license key specified as an alphanumeric string of 1 of 1 through 500 characters.
> full: Displays the full features and quantities without any hardware limits in place.
> key:
> Displays the installed keys in encrypted format.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Displays the license information to verify the proper keys have been installed. This command is also helpful in troubleshooting user system access due to the maximum number of sessions being reached.
> Example
> The following displays the encrypted installed key and the information for sampleKey respectively.
> show license information sampleKey
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show linecard
> Displays information on the interface cards installed in the rear of the system chassis.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show linecard { dlci-utilization card# | table } [ | { grep grep_options | more } ]
> dlci-utilization card#
> SGSN only
> In tabular format, displays current data link utilization (in 5 minute and 15 minute breakdowns) information for all Frame Relay ports on the specified CLC-type line card. Data links are referred to by data link connection identifiers (DLCI).
> card# - Identifies the chassis slot number where the line card resides. Enter an integer from 1 to 48.
> table
> Displays information on all line card slots in tabular format.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to show the line card information

> • | to verify hardware inventories and installed components.

> • | to review DLCI utilization for a specific Frame Relay channelized line card.

> Important: This command is not supported on all platforms.
> Example
> Use the following command to display a table with information identifying all line cards installed in the chassis:
> show linecard table
> Use the following command to display DLCI utilization information for all ports on CLC card in slot 27:
> show linecard dlci-utilization 27
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show linkmgr
> Displays statistics for the link manager (linkmgr).
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show linkmgr { all | instance instance } [ parser | | ]
> all
> Display statistics for all link managers.
> instance instance
> Display statistics for a single instance of a link manager specified as an integer from 1 to 4.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> This command displays statistical information for the SGSN’s link manager which handles the layer between the session manager and the SS7 functionality downwards from layer 3.
> Example
> Use the following command to display the statistics for link manager 4:
> show linkmgr 4
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show llc statistics
> Displays traffic statistics for the GPRS logical link-control (LLC) layer.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show llc statistics [ gprs-service srvc_name ] [ verbose ] [ | { grep grep_options | more } ]
> gprs-service srvc_name
> Displays the statistics for an existing GPRS service specified as an alphanumeric string of 1 through 63 characters.
> verbose
> Displays all possible statistics for specified command or keyword.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For more information on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Reference.
> Usage
> This command can display either a summarized or full (verbose) view of statistics collected for the traffic that has gone through the LLC layer for either all GPRS services or for a specified GPRS service.
> Example
> The following command displays the frame Tx/Rx LLC statistics for GPRS service gprs1:
> show llc statistics gprs-service gprs1
> show llc status
> Displays status information for the GPRS logical link-control (LLC) layer.
> Product
> SGSN
> Privilege
> Inspector
> Syntax
> show llc status gprs-service srvc_name sessmgr instance instance { dlci ms-id ms_id sapi sapid | lsap sapid sapid | ms ms_id | usap sapid sapid [ | { grep grep_options | more } ]
> gprs-service srvc_name
> Displays the LLC layer status for an existing GPRS service specified as an alphanumeric string of 1 through 63 characters.
> sessmgr instance instance
> Displays the LLC status for a session manager instance specified as an integer from 1 to 4294967295.
> dlci ms-id ms_id [ sapi sapid ]
> Displays the LLC status for a specific data link connection identifier (DLCI) between the LLC and the mobile station (MS). ms_id must be an integer from 0 to 65536 that identifies the DLCI interface connecting to a specific MS.
> sapi: Filters the display of the LLC status information to focus on a specific service access point interface (SAPI) within the specified DLCI specified as.an integer from 1 to 11
> lsap sapid
> Refines the display of the LLC status to focus on a specific lower service access point interface (LSAP) specified as an integer from 0 to 65536.
> ms-id ms_id
> Displays the LLC status for a connected MS specified as an integer from 0 to 65536.
> usap sapid
> Refines the display of the LLC statistics to focus on a specific upper service access point interface (USAP) specified as an integer from 0 to 65536.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For more information on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Reference.
> Usage
> This command can display either a summarized or full (verbose) view of statistics collected for the traffic that has gone through the LLC layer for either all GPRS services or for a specified GPRS service.
> Example
> The following command displays the frame Tx/Rx LLC statistics for GPRS service gprs1:
> show llc statistics gprs-service gprs1
> show lma-service
> Displays statistic and counter information for Local Mobility Anchor (LMA) services on this system.
> Product
> P-GW
> Privilege
> Inspector
> Syntax
> show lma-service all
> show lma-service name service_name
> show lma-service session [ all | callid id | counters | full | ipv6-address { < address | > address | address | greater-than address [ less-than address ] | less-than address [ greater-than address ] } | summary | username name ]
> show lma-service statistics [ lma-service name ] } [ | { grep grep_options | more } ]
> all
> Displays information about all configured LMA services on this system.
> name service_name
> Displays configuration information for an existing LMA service specified as an alphanumeric string of 1 through 63 characters.
> session [ all | callid id | counters | full | ipv6-address { < address | > address | address | greater-than address [ less-than address ] | less-than address [ greater-than address ] } | summary | username name ]
> Displays session information filtered by the following parameters:
> all: Displays all active LMA sessions using LMA services on the system.
> callid id: Displays available session information for the call identification number specified as an eight-byte hexadecimal number.
> counters: Displays session counters for active LMA sessions using LMA services on the system. This keyword can also be filtered by the following:

> • | all

> • | callid

> • | ipv6-address

> • | username

> Refer to the keyword descriptions in this command for information regarding these filters.
> full: Displays additional session information for active LMA sessions using LMA services on the system. This keyword includes the information in the output of the all keyword plus additional information. This keyword can also be filtered by the following:

> • | all

> • | callid

> • | ipv6-address

> • | username

> Refer to the keyword descriptions in this command for information regarding these filters.
> ipv6-address:

> • | < address and less-than address: Displays summarized information for a group of IPv6 addresses that are less than the specified IPv6 address using one of these keywords. A range can be specified by including an address with the greater-than option. address must be specified in IPv6 colon-separated notation.

> • | > address and greater-than address: Displays summarized information for a group of IPv6 addresses that are greater than the specified IPv6 address using one of these keywords. A range can be specified by including an address with the less-than option. address must be specified in IPv6 colon-separated notation.

> • | address: Displays summarized information for a specific IPv6 address using an LMA service on this system. address must be specified in IPv6 colon-separated notation.

> summary: Displays the number of LMA sessions currently active for LMA services configured on the system.
> username name: Displays available session information for an existing user specified as an alphanumeric string of 1 through 127 characters.
> statistics [ lma-service name ]
> lma-service name: Displays LMA service statistics for an existing LMA service specified as an alphanumeric string of 1 through 63 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section of Chapter 1 of the Command Line Interface Reference Guide.
> Usage
> Use this command to view configuration information for LMA services on this system.
> Example
> The following command displays service statistics for the LMA service named lma1:
> show lma-service name lma1
> show lns-service
> Displays the information for all L2TP Network Server (LNS) services or for a particular LNS service.
> Product
> PDSN, HA, GGSN, LNS
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show lns-service { all | name service_name } [ | { grep grep_options | more } ]
> all
> Display information for all LNS services.
> name service_name
> Displays information only for an existing LNS service specified as an alphanumeric string of 1 through 63 characters.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> Use this command to list information for LNS services configured on this system.
> Example
> The following commands display information for all LNS services and the LNS service named lns1, respectively.
> show lns-service all
> show lns-service name lns1
> show local-user
> Displays information pertaining to local-user accounts.
> Product
> All
> Privilege
> Security Administrator
> Syntax
> show local-user [ [ username name ] [ inactive filter ] [ verbose | wide ] | statistics [ verbose ] ]
> username name
> Displays information for an existing local-user administrative account specified as an alphanumeric string of 3 through 16 characters that is case sensitive.
> inactive filter
> Specifies a filter for displaying inactive local-user accounts:

> • | < days: Displays accounts that have been inactive less than the specified number of days.

> • | > days: Displays accounts that have been inactive more than the specified number of days.

> • | greater-than days: Displays accounts that have been inactive more than the specified number of days.

> • | less-than days: Displays accounts that have been inactive less than the specified number of days.

> days can be configured to an integer from 1 through 365.
> [ verbose | wide ]
> Specifies how the information is to be displayed as one of the following options:

> • | verbose: The data is displayed in list format. Additional information is provided beyond what is displayed when the wide option is used.

> • | wide: The data is displayed in tabular format. This is the default setting.

> statistics [ verbose ]
> Displays local-user statistics.
> Using the verbose keyword displays additional statistics.
> Usage
> Use this command to display information and statistics on local-user administrative accounts.
> Example
> The following command displays detailed information on local-user administrative accounts that have been inactive for more than 10 days:
> show local-user inactive greater-than 10 verbose
> The following command displays detailed information for a local-user account named Test:
> show local-user username Test verbose
> The following command displays detailed local-user account statistics:
> show local-user statistics verbose
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.
> show logging
> Displays the defined logging filters for the current context.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show logging [ active | verbose ] [ | { grep grep_options | more } ]
> active | verbose
> active: Displays only active CLI logging filter information in concise format.
> verbose: Displays as much information as possible.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> View log filters to troubleshoot disk utilization issues.
> Example
> show logging
> show logging active
> show logging verbose
> show logging active verbose
> show logs
> Displays active and inactive logs filtered by the options specified.
> Product
> All
> Privilege
> Security Administrator, Administrator, Operator, Inspector
> Syntax
> show logs [ active ] [ inactive ] [ callid call_id ] [ event-verbosity evt_verboseness ] [ facility facility ] [ level severity_level ] [ pdu-data pdu_format ] [ pdu-verbosity pdu_verboseness ] [ proclet facility ] [ since from_date_time [ until to_date_time ] ] [ | { grep grep_options | more } ]
> active
> Displays data from active logs.
> inactive
> Displays data from inactive logs.
> callid call_id
> Displays log information only for a call ID specified as a 4-digit hexadecimal number.
> event-verbosity evt_verboseness
> Specifies the level of verboseness to use in displaying of event data as one of:

> • | min - displays minimal information about the event. Information includes event name, facility, event ID, severity level, date, and time.

> • | concise - displays detailed information about the event, but does not provide the event source within the system.

> • | full - displays detailed information about event, including source information, identifying where within the system the event was generated.

> facility facility
> Specifies the facility to modify the filtering of logged information for as one of:

> • | a10: A10 interface facility

> • | a11: A11 interface facility

> • | a11mgr: A11 Manager facility

> • | aaa-client: AAA client facility

> • | aaamgr: AAA manager logging facility

> • | aaaproxy: AAA Proxy facility

> • | aal2: AAL2 protocol logging facility

> • | acl-log: Access Control List logging facility

> • | acsctrl: Active Charging Service (ACS) Controller facility

> • | acsmgr: Active Charging Service (ACS) Manager facility

> • | alarmctrl: Alarm Controller facility

> • | alcap: ALCAP protocol logging facility

> • | alcapmgr: ALCAPMgr logging facility

> • | all: All facilities

> • | asngwmgr: ASN Gateway Manager facility

> • | asnpcmgr: ASN Paging Controller Manager facility

> • | bfd: BFD protocol logging facility

> • | bgp: Border Gateway Protocol (BGP) facility

> • | bindmux: IPCF BindMux-De-mux Manager logging facility

> • | bssap+: Base Station Sub-system Application Part+ protocol facility for the login interface between the SGSN and the MSC/VLR (2.5G and 3G)

> • | bssgp: Base Station Sub-system GPRS Protocol logging facility handles exchange information between the SGSN and the BSS (2.5G only)

> • | callhome: Call home application logging facility

> • | cap: CAMEL Application Part (CAP) logging facility for protocol used in prepaid applications (2.5G and 3G)

> • | cli: CLI logging facility

> • | credit-control: Credit Control facility

> • | cscf: IMS/MMD CSCF

> • | cscfmgr: SIP CSCF Manager facility

> • | cscfttmgr: SIP CSCFTT Manager facility

> • | csp: Card Slot Port controller facility

> • | css: Content Service Selection (CSS) facility

> • | css-sig: Content Service Selection (CSS) RADIUS Signaling facility

> • | cx-diameter: Cx Diameter Messages facility

> • | dcardctrl: IPSEC Daughter Card Controller logging facility

> • | dcardmgr: IPSEC Daughter Card Manager logging facility

> • | demuxmgr: Demux Manager API facility

> • | dgmbmgr: Diameter Gmb Application Manager logging facility

> • | dhcp: Dynamic Host Configuration Protocol logging facility

> • | dhcpv6: DHCPv6

> • | dhost: Distributed Host logging facility

> • | diabase: Diabase messages facility

> • | diameter: Diameter endpoint logging facility

> • | diameter-acct: Diameter Accounting

> • | diameter-auth: Diameter Authentication

> • | diameter-dns: Diameter DNS subsystem

> • | diameter-ecs: ACS Diameter signaling facility

> • | diameter-hdd: Diameter HDD Interface facility

> • | diameter-svc: Diameter Service

> • | diamproxy: DiamProxy logging facility

> • | dpath: IPSEC Data Path facility

> • | drvctrl: Driver Controller facility

> • | eap-ipsec: EAP

> • | eap-sta-s6a-s13-s6b-diameter: EAP/STA/S6A/S13/S6B Diameter messages facility

> • | ecs-css: ACSMGR <-> Session Manager Signalling Interface facility

> • | egtpc: eGTP-C logging facility

> • | egtpmgr: eGTP manager logging facility

> • | egtpu: eGTP-U logging facility

> • | epdg: ePDG logging facility

> • | evlog: Event log facility

> • | famgr: Foreign Agent manager logging facility

> • | firewall: Firewall logging facility

> • | fng: FNG logging facility

> • | gmm:

> • | For 2.5G: Logs the GPRS Mobility Management (GMM) layer (above LLC layer)

> • | For 3G: Logs the access application layer (above the RANAP layer)

> • | gprs-app: GPRS Application logging facility

> • | gprs-ns: GPRS Network Service Protocol (layer between SGSN and the BSS) logging facility

> • | gq-rx-tx-diameter: Gq/Rx/Tx Diameter messages facility

> • | gss-gcdr: GTPP Storage Server GCDR facility

> • | gtpc: GTP-C protocol logging facility

> • | gtpcmgr: GTP-C protocol Manager logging facility

> • | gtpp: GTP-PRIME protocol logging facility

> • | gtpu: GTP-U protocol logging facility

> • | gtpumgr: GTPU Demux manager

> • | gx-ty-diameter: Gx/Ty Diameter messages facility

> • | gy-diameter: Gy Diameter messages facility

> • | hamgr: Home Agent manager logging facility

> • | hat: High Availability Task (HAT) process facility

> • | hdctrl: HD Controller logging facility

> • | hnb-gw: HNB-GW (3G Femto GW) logging facility

> • | hnbmgr: HNBMGR (3G Femto GW DemuxMgr) logging facility

> • | hss-peer-service: HSS Peer Service facility

> • | igmp: IGMP

> • | ikev2: IKEv2

> • | ims-authorizatn: IMS Authorization Service facility

> • | ims-sh: HSS SH Service facility

> • | imsimgr: SGSN IMSI Manager facility

> • | imsue: IMSUE

> • | ip-arp: IP Address Resolution Protocol facility

> • | ip-interface: IP interface facility

> • | ip-route: IP route facility

> • | ipms: IPMS logging facility

> • | ipsec: IP Security logging facility

> • | ipsg: IP Service Gateway interface logging facility

> • | ipsgmgr: IP Services Gateway facility

> • | ipsp: IP Pool Sharing Protocol logging facility

> • | kvstore: KV Store facility

> • | l2tp-control: L2TP control logging facility

> • | l2tp-data: L2TP data logging facility

> • | l2tpdemux: L2TP Demux Manager logging facility

> • | l2tpmgr: L2TP Manager logging facility

> • | lagmgr: LAGMGR logging facility

> • | ldap: Lightweight Directory Access Protocol (LDAP) messages logging facility

> • | li: Refer to the Lawful Intercept Interface Reference for a description of this command.

> • | linkmgr: SGSN/BSS SS7 Link Manager logging facility (2.5G only)

> • | llc: Logical Link Control (LLC) Protocol logging facility; for SGSN: logs the LLC layer between the GMM and the BSSGP layers for logical links between the MS and the SGSN

> • | local-policy: Local Policy Service facility

> • | m3ua: M3UA Protocol logging facility

> • | magmgr: Mobile Access Gateway manager logging facility

> • | map: MAP Protocol logging facility

> • | megadiammgr: Megadiameter Manager (SLF Service) logging facility

> • | mme-app: Mobility Management Entity Application logging facility

> • | mme-misc: MME miscellaneous logging facility

> • | mmedemux: Mobility Management Entity Demux Manager logging facility

> • | mmemgr: MME Manager facility

> • | mmgr: Master Manager logging facility

> • | mobile-ip: Mobile IP processes

> • | mobile-ip-data: Mobile IP data facility

> • | mobile-ipv6: Mobile IPv6 logging facility

> • | mpls: MPLS protocol logging facility

> • | mseg-app: MSEG application logging facility

> • | mseg-gtpc: MSEG GTPC application logging facility

> • | mseg-gtpu: MSEG GTPU application logging facility

> • | msegmgr: MSEGMgr (MSEG DemuxMgr) logging facility

> • | mtp2: MTP2 Service logging facility

> • | mtp3: MTP3 Protocol logging facility

> • | multicast-proxy: Multicast Proxy logging facility

> • | npuctrl: Network Processor Unit Control facility

> • | npumgr: Network Processor Unit Manager facility

> • | npumgr-acl: NPUMGR ACL logging facility

> • | npumgr-flow: NPUMGR FLOW logging facility

> • | npumgr-fwd: NPUMGR FWD logging facility

> • | npumgr-init: NPUMGR INIT logging facility

> • | npumgr-port: NPUMGR PORT logging facility

> • | npumgr-recovery: NPUMGR RECOVERY logging facility

> • | ntfy-intf: Notification Interface logging facility

> • | orbs: Object Request Broker System logging facility

> • | ospf: OSPF protocol logging facility

> • | ospfv3: OSPFv3 protocol logging facility

> • | p2p: Peer-to-Peer Detection logging facility

> • | pccmgr: IPCF PCC Manager library

> • | pdg: PDG logging facility

> • | pdgdmgr: PDG Demux Manager logging facility

> • | pdif: PDIF logging facility

> • | pgw: PDN Gateway logging facility

> • | phs: Payload Header Suppression

> • | phs-control: PHS X1/X5 and X2/X6 Interface logging facility

> • | phs-data: PHS Data logging facility

> • | phs-eapol: PHS EAPOL logging facility

> • | phsgwmgr: PHS Gateway Manager facility

> • | phspcmgr: PHS Paging Controller Manager facility

> • | pmm-app: PMM application logging facility

> • | ppp: PPP link and packet facilities

> • | pppoe: PPPOE logging facility

> • | push: VPNMGR CDR push logging facility

> • | radius-acct: RADIUS accounting logging facility

> • | radius-auth: RADIUS authentication logging facility

> • | radius-coa: RADIUS change of authorization and radius disconnect

> • | ranap: Radio Access Network Application Part (RANAP) Protocol facility logging info flow between SGSN and RNS (3G)

> • | rct: Recovery Control Task logging facility

> • | rdt: Redirect Task logging facility

> • | resmgr: Resource Manager logging facility

> • | rf-diameter: Rf Diameter messages facility

> • | rip: RIP logging facility (RIP is not supported at this time.)

> • | rohc: RObust Header Compression facility

> • | rsvp: Reservation Protocol logging facility

> • | rua: RUA (3G Femto GW - RUA messages) logging facility

> • | s1ap: S1AP Protocol logging facility

> • | sccp: SCCP Protocol logging connection-oriented messages between RANAP and TCAP layers.

> • | sct: Shared Configuration Task logging facility

> • | sctp: SCTP Protocol logging facility

> • | sessctrl: Session Controller logging facility

> • | sessmgr: Session Manager logging facility

> • | sesstrc: session trace logging facility

> • | sft: Switch Fabric Task logging facility

> • | sgs: SGs protocol logging facility

> • | sgsn-app: SGSN-APP logging various SGSN ‘glue’ interfaces, e.g., between PMM, MAP,. GPRS-FSM, SMS.

> • | sgsn-failures: SGSN call failures (attach/activate rejects) logging facility (2.5G)

> • | sgsn-gtpc: SGSN GTP-C Protocol logging control messages between the SGSN and the GGSN

> • | sgsn-gtpu: SGSN GTP-U Protocol logging user data messages between the SGSN and GGSN

> • | sgsn-mbms-bearer: SGSN MBMS Bearer app (SMGR) logging facility

> • | sgsn-misc: Used by stack manager to log binding and removing between layers

> • | sgsn-system: SGSNs System Components logging facility; used infrequently

> • | sgsn-test: SGSN Tests logging facility; used infrequently

> • | sgtpcmgr: SGSN GTPC Manager logging information exchange through SGTPC and the GGSN

> • | sgw: Serving Gateway facility

> • | sh-diameter: Sh Diameter messages facility

> • | sitmain: System Initialization Task main logging facility

> • | sm-app: SM Protocol logging facility

> • | sms: Short Message Service (SMS) logging messages between the MS and the SMSC

> • | sndcp: SNDCP Protocol logging facility

> • | snmp: SNMP logging facility

> • | sprmgr: IPCF SPR Manager logging facility

> • | srdb: Static Rating Database

> • | srp: Service Redundancy Protocol (SRP) logging facility

> • | sscfnni: SSCFNNI Protocol logging facility

> • | sscop: SSCOP Protocol logging facility

> • | ssh-ipsec: SSH IP Security logging facility

> • | ssl: SSL (Secure socket layer messages) logging facility

> • | stat: Statistics logging facility

> • | system: System logging facility

> • | tacacsplus: TACACS+ Protocol logging facility

> • | tcap: TCAP Protocol logging facility

> • | testctrl: Test Controller logging facility

> • | testmgr: Test Manager logging facility

> • | threshold: threshold logging facility

> • | ttg: TTG logging facility

> • | tucl: TUCL logging facility

> • | udr: User detail record facility (used with the Charging Service)

> • | user-data: User data logging facility

> • | user-l3tunnel: User layer-3 tunnel logging facility

> • | usertcp-stack: User TCP Stack

> • | vpn: Virtual Private Network logging facility

> • | wimax-data: WiMAX DATA

> • | wimax-r6: WiMAX R6

> level severity_level
> level severity_level: Specifies the level of information to be logged from the following list which is ordered from highest to lowest:

> • | critical - display critical events

> • | error - display error events and all events with a higher severity level

> • | warning - display warning events and all events with a higher severity level

> • | unusual - display unusual events and all events with a higher severity level

> • | info - display info events and all events with a higher severity level

> • | trace - display trace events and all events with a higher severity level

> • | debug - display all events

> pdu-data pdu_format
> Specifies output format for the display of packet data units as one of:

> • | none - output is in raw format (unformatted).

> • | hex - output being displayed in hexadecimal format.

> • | hex-ascii - output being displayed in hexadecimal and ASCII similar to a main-frame dump.

> pdu-verbosity pdu_verboseness
> Specifies the level of verboseness to use in displaying of packet data units as an integer from 1 through 5, where 5 is the most detailed.
> proclet facility
> Shows the logs from a specific proclet facility. The available facilities are the same as those listed earlier.
> since from_date_time [ until to_date_time ]
> Default: no limit.
> since from_date_time: indicates only the log information which has been collected more recently than from_date_time is to be displayed.
> until to_date_time: indicates no log information more recent than to_date_time is to be displayed. until defaults to current time when omitted.
> from_date_time and to_date_time must be formatted as YYYY:MM:DD:HH:mm or YYYY:MM:DD:HH:mm:ss. Where:

> • | YYYY = 4-digit year

> • | MM = 2-digit month in the range 01 through 12

> • | DD = 2-digit day in the range 01 through 31

> • | HH = 2-digit hour in the range 00 through 23

> • | mm = 2-digit minute in the range 00 through 59

> • | ss = 2-digit second in the range 00 through 59

> to_date_time must be a time which is more recent than from_date_time.
> The use of the until keyword allows for a time range of log information while only using the since keyword will display all information up to the current time.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of grep and more, refer to the Regulating a Command’s Output section of the Command Line Interface Overview chapter.
> Usage
> View log files for general maintenance or troubleshooting system issues.
> Example
> The following command displays log information for the a11mgr facility starting with July 1th, 2011 at midnight.
> show logs facility allmgr since 2011:07:11:00:00
> The following command displays the log information for call ID FE881D32 only in active logs.
> show logs active callid FE881D32
> show lte-policy
> Displays information for Long term Evolution (LTE) policy configurations on this system including handover restriction lists, subscriber maps, and tracking area identifiers (TAIs).
> Product
> MME
> Privilege
> Inspector
> Syntax
> show lte-policy { ho-restriction-list { name name | summary } | subscriber-map { name name | summary } | tai-mgmt-db { name name | summary } } [ | { grep grep_options | more } ]
> ho-restriction-list { name name | summary }
> Displays information about handover restriction lists configured on this system.
> name name: Displays information about a specific handover restriction list configured on this system. name must be an existing HO restriction list, expressed as an alphanumeric string of 1 to 64 characters.
> summary: Displays summarized information about all handover restriction lists configured on this system.
> subscriber-map { name name | summary }
> Displays information about subscriber maps configured on this system.
> name name: Displays information about an existing subscriber map specified as an alphanumeric string of 1 through 64 characters.
> summary: Displays summarized information about all subscriber maps configured on this system.
> tai-mgmt-db { name name | summary }
> Displays information about TAI management databases configured on this system.
> name name: Displays information about an existing TAI management database specified as an alphanumeric string of 1 through 64 characters.
> summary: Displays summarized information about all TAI management databases configured on this system.
> | { grep grep_options | more }
> Pipes (sends) the output of this command to the specified command. You must specify a command to which the output of this command will be sent.
> For details on the usage of the grep and more commands, refer to the Regulating a Command’s Output section in CLI Overview chapter.
> Usage
> Use this command to display information for LTE policy configurations on this system including handover restriction lists, subscriber maps, and tracking area identifiers (TAIs).
> Example
> The following command displays information about a subscriber map named map3:
> show lte-policy subscriber-map name map3
> Important: Output descriptions for commands are available in the Statistics and Counters Reference.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883