> Web Element Manager MIB
> The figure that follows illustrates the hierarchical structure of the management information base (MIB) for the Web Element Manager.
> MIB Textual Conventions
> starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000)
> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000). starEmsMIBObjects(1)
> starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000). starEmsMIBObjects(1).starEmsNotifMgmt(2)
> Object
> starEmsNotifInfo
> Object ID
> enterprises.8164.1.1000.1.2.5
> Description
> A textual description of EMS notification, which potentially contains additional information (more than just the type of alarm). If the text of the message exceeds 64 bytes, the message will be truncated to 63 bytes and a '*' character will be appended to indicate the message has been truncated.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsNotifRaisedTime
> Object ID
> enterprises.8164.1.1000.1.2.6
> Description
> This object indicates the time when this notification was generated.
> Syntax
> TimeStamp
> Access
> Read-only
> Object
> starEmsProcMonThreshold
> Object ID
> enterprises.8164.1.1000.1.2.7
> Description
> This object indicates the current threshold value of process monitoring.
> Syntax
> DisplayString (SIZE (1..10))
> Access
> Read-only
> Object
> starEmsInterfaceAddr
> Object ID
> enterprises.8164.1.1000.1.2.8
> Description
> The object indicates the Interface address of host machine where EMS server is running
> Syntax
> InetAddress
> Access
> Read-only
> Object
> starEmsInterfaceName
> Object ID
> enterprises.8164.1.1000.1.2.9
> Description
> This object indicates the interface name of host machine where EMS server is running.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsIMGAddr
> Object ID
> enterprises.8164.1.1000.1.2.10
> Description
> The object indicates the IP address of IMG.
> Syntax
> InetAddress
> Access
> Read-only
> Object
> starEmsFtpFileName
> Object ID
> enterprises.8164.1.1000.1.2.11
> Description
> This object indicates name of the file which FTP’d and then deleted from the IMG.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsIMGState
> Object ID
> enterprises.8164.1.1000.1.2.12
> Description
> IMG state. unreachable(0) IMG is ICMP unreachable active(1) IMG is CORBA reachable inactive(1) IMG is CORBA unreachable reachable(0) IMG is ICMP reachable
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unreachable(0)
> active(1)
> inactive(2)
> reachable(3)
> Object
> starEmsBulkStatFileXferTime
> Object ID
> enterprises.8164.1.1000.1.2.13
> Description
> The configured value of a Bulkstat file transfer in minutes.
> Syntax
> INTEGER(1..999999)
> Access
> Read-only
> Object
> starEmsXMLFtpFileName
> Important: This attribute is obsolete.
> Object ID
> enterprises.8164.1.1000.1.2.14
> Description
> This object indicates name of the BulkStat XML file which is to be FTPed on the NMS.
> Syntax
> DisplayString (SIZE (1..256))
> Access
> Read-only
> Object
> starEmsXMLFtpDestAddr
> Object ID
> enterprises.8164.1.1000.1.2.15
> Description
> This object indicates destination IP address (NMS) for BulkStat XML file FTP.
> Syntax
> InetAddress
> Access
> Read-only
> Object
> starEmsXMLFtpDestPath
> Object ID
> enterprises.8164.1.1000.1.2.16
> Description
> This object indicates destination path where BulkStat XML file is to be FTP’d.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> Read-only
> Object
> starEmsIMGPreviousState
> Object ID
> enterprises.8164.1.1000.1.2.17
> Description
> IMG state. unmanageable(0) IMG is not CORBA reachable manageable(1) IMG is CORBA reachable
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> unmanageable(0)
> manageable(1)
> Object
> starEmsIMGName
> Object ID
> enterprises.8164.1.1000.1.2.18
> Description
> The object indicates the name of IMG.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsPortMonThreshold
> Object ID
> enterprises.8164.1.1000.1.2.19
> Description
> This object indicates the configured threshold value of port monitoring.
> Syntax
> DisplayString (SIZE (1..20))
> Access
> Read-only
> Object
> starEmsPortMonCurrent
> Object ID
> enterprises.8164.1.1000.1.2.20
> Description
> This object indicates the current threshold value of port monitoring.
> Syntax
> DisplayString (SIZE (1..20))
> Access
> Read-only
> Object
> starEmsTotalPendingEvts
> Object ID
> enterprises.8164.1.1000.1.2.21
> Description
> This object indicates the number of pending events for monitor in server queue.
> Syntax
> INTEGER(1..100000)
> Access
> Read-only
> Object
> starEmsMaxLimit
> Object ID
> enterprises.8164.1.1000.1.2.22
> Description
> This object indicates the limit of the server queue to store pending events.
> Syntax
> InetAddress
> Access
> Read-only
> Object
> starEmsClientAddr
> Object ID
> enterprises.8164.1.1000.1.2.23
> Description
> The object indicates the IP address of EMS Client.
> Syntax
> DisplayString (SIZE (1..256))
> Access
> Read-only
> Object
> starEmsMonOldEvtTimeStamp
> Object ID
> enterprises.8164.1.1000.1.2.24
> Description
> This object indicates the timestamp for last Monitor Pending Event.
> Syntax
> DisplayString (SIZE (1..256))
> Access
> Read-only
> Object
> starEmsMonitorType
> Object ID
> enterprises.8164.1.1000.1.2.25
> Description
> This object indicates the monitor type.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> protocol(0)
> subscriber(1)
> Object
> starEmsMonitorUserName
> Object ID
> enterprises.8164.1.1000.1.2.26
> Description
> This object indicates the User name.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsDevicePath
> Object ID
> enterprises.8164.1.1000.1.2.27
> Description
> This object indicates the Device name.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> Read-only
> Object
> starEmsPrevHostName
> Object ID
> enterprises,8164.1.1000.1.2.28
> Description
> This object indicates the name of the previous host running EMS before failover.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsCurrHostName
> Object ID
> enterprises,8164.1.1000.1.2.29
> Description
> This object indicates the name of the current host running EMS.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsP2PProtocolType
> Object ID
> enterprises,8164.1.1000.1.2.30
> Description
> This object indicates the protocol type.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> ip(1)
> tcp(2)
> udp(3)
> http(4)
> htpps(5)
> ftp(6)
> ftpcontrol(7)
> ftpdata(8)
> wtp(9)
> wsp(10)
> dns(11)
> icmp(12)
> pop3(13)
> sip(14)
> sdp(15)
> smtp(16)
> mms(17)
> filetransfer(18)
> rtp(19)
> rtsp(20)
> imap(21)
> totalp2p(22)
> p2punknown(23)
> p2pskype(24)
> p2pbittorrent(25)
> p2pedonkey(26)
> p2pmsn(27)
> p2pyahoo(28)
> p2pporb(29)
> p2pfasttrack(30)
> p2pslingbox(31)
> p2pvcast(32)
> p2pgnutella(33)
> Object
> starEmsP2PProtocolVal
> Object ID
> enterprises,8164.1.1000.1.2.31
> Description
> This object indicates the protocol value.
> Syntax
> INTEGER
> Access
> Read-only
> Enumeration
> uplinkbytes(0)
> downlinkbytes(1)
> totalbytes(2)
> uplinkpkts(3)
> downlinkpkts(4)
> totalpkts(5)
> uplinkbytespercent(6)
> downlinkbytespercent(7)
> totalbytespercent(8)
> uplinkpktspercent(9)
> downlinkpktspercent(10)
> totalpktspercent(11)
> Object
> starEmsSyslogLoggedTime
> Object ID
> enterprises,8164.1.1000.1.2.32
> Description
> This object indicates the logged time for the syslog message.
> Syntax
> TimeStamp
> Access
> Read-only
> Object
> starEmsSyslogFacility
> Object ID
> enterprises,8164.1.1000.1.2.33
> Description
> This object indicates the facility of syslog message.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsSyslogPriority
> Object ID
> enterprises,8164.1.1000.1.2.34
> Description
> This object indicates the syslog message priority.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsSyslogHostName
> Object ID
> enterprises,8164.1.1000.1.2.35
> Description
> This object indicates the hostname.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsSyslogKeyword
> Object ID
> enterprises,8164.1.1000.1.2.36
> Description
> This object indicates the keywords detected in the syslog message.
> Syntax
> DisplayString (SIZE (1..64))
> Access
> Read-only
> Object
> starEmsSyslogMessage
> Object ID
> enterprises,8164.1.1000.1.2.37
> Description
> This object indicates the syslog message contents.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> Read-only
> Object
> starEmsSyslogFilePath
> Object ID
> enterprises,8164.1.1000.1.2.38
> Description
> This object indicates the syslog message file path.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> Read-only
> Object
> starEmsDBName
> Object ID
> enterprises,8164.1.1000.1.2.39
> Description
> This object indicates the database name.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> Read-only
> Object
> starEmsBulkstatCounter
> Object ID
> enterprises,8164.1.1000.1.2.40
> Description
> This object indicates the bulkstat counter name.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> Read-only
> Object
> starEmsBulkStatRecordDetails
> Object ID
> enterprises,8164.1.1000.1.2.41
> Description
> This object indicates the bulkstat record detail information.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> Read-only
> Object
> starEmsBulkStatRecordTime
> Object ID
> enterprises,8164.1.1000.1.2.42
> Description
> This object indicates the bulkstat record time
> Syntax
> TimeStamp
> Access
> Read-only
> Object
> starEmsBulkStatThreshold
> Important: This attribute is obsolete.
> Object ID
> enterprises,8164.1.1000.1.2.43
> Description
> This object indicates the configured threshold value of the bulkstat counter.
> Syntax
> INTEGER(0..100000)
> Access
> Read-only
> Object
> starEmsbulkStatCurrent
> Important: This attribute is obsolete.
> Object ID
> enterprises,8164.1.1000.1.2.44
> Description
> This object indicates the current threshold (delta) value of the bulkstat counter.
> Syntax
> INTEGER(0..100000)
> Access
> Read-only
> Object
> starEMSCFMcrdbsHostAddress
> Object ID
> enterprises,8164.1.1000.1.2.45
> Description
> MCRDBS IP address
> Syntax
> InetAddress
> Access
> Read-Only
> Object
> starEMSCFDbType
> Object ID
> enterprises,8164.1.1000.1.2.46
> Description
> Type sfmdb(1) Starent Format Master DataBase. sfmdbinc(2) Starent Format Master DataBase Incremental. optcmdb(6) Optmized Customer Master DataBase. optcmdbinc(7) Optmized Customer Master DataBase Incremental. optcmbldb(14) Optmized Customer Master Blacklist DataBase sfunkdb(5) Starent format unknown URL database
> Syntax
> INTEGER {
> sfmdb(1),
> sfmdbinc(2),
> optcmdb(6),
> optcmdbinc(7),
> optcmbldb(14)
> sfunkdb(5)
> Access
> Read-Only
> Object
> starEmsCFSourceDbFileName
> Object ID
> enterprises,8164.1.1000.1.2.47
> Description
> This object indicates name of the file whose SFTP/Conversion is failed.
> Syntax
> Displaystring (SIZE(1..64))
> Access
> Read-Only
> Object
> starEMSCFCdpHostAddress
> Object ID
> enterprises,8164.1.1000.1.2.48
> Description
> CDP IP Address
> Syntax
> InetAddress
> Access
> Read-Only
> Object
> starEMSCFFromDbType
> Object ID
> enterprises,8164.1.1000.1.2.49
> Description
> Type. sfmdb(1) Starent Format Master DataBase. sfmdbinc(2) Starent Format Master DataBase Incremental . blacklist(10) Blacklist DataBase. sfmbldb(11) Starent Format Master Blacklist DataBase.
> Syntax
> INTEGER
> sfmdb(1),
> sfmdbinc(2),
> blacklist(10),
> sfmbldb(11)
> Access
> Read-Only
> Object
> starEMSCFToDbType
> Object ID
> enterprises,8164.1.1000.1.2.50
> Description
> Databases Type optcmdb(6) Optmized Customer Master DataBase. optcmdbinc(7) Optmized Customer Master DataBase Incremental. sfmbldb(11) Starent Format Master Blacklist DataBase. optcmbldb(14) Optmized Customer Master Blacklist DataBase.
> Syntax
> INTEGER
> optcmdb(6),
> optcmdbinc(7),
> sfmbldb(11),
> optcmbldb(14)
> Access
> Read-Only
> Object
> starEMSCFDestDbName
> Object ID
> enterprises,8164.1.1000.1.2.51
> Description
> This object indicates the name of the destination file, used to specify the destination file created after conversion.
> Syntax
> DisplayString (SIZE(1..64)
> Access
> Read-Only
> Object
> starEMSCFFtpHostInfo
> Object ID
> enterprises,8164.1.1000.1.2.52
> Description
> FTP host IP address
> Syntax
> DisplayString (SIZE(1..64))
> Access
> Read-Only
> Object
> starEMSBulkstatCounterValue
> Object ID
> enterprises,8164.1.1000.1.2.53.
> Description
> Bulkstat counter current value
> Syntax
> Integer (0..100000)
> Access
> Read-Only
> Object
> starEmsBulkStatFilterDetails
> Object ID
> enterprises,8164.1.1000.1.2.54.
> Description
> This object indicates the bulkstat Threshold related filter combinations.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> read-only
> Object
> starEmsBulkStatCurrentDouble
> Object ID
> enterprises,8164.1.1000.1.2.55.
> Description
> This object indicates the current threshold (delta) value of bulkstat counter.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> read-only
> Object
> starEmsBulkStatThresholdDouble
> Object ID
> enterprises,8164.1.1000.1.2.56.
> Description
> This object indicates the configured threshold value of bulkstat counter.
> Syntax
> DisplayString (SIZE (1..1024))
> Access
> read-only
> Object
> starEmsConfigBackupFileName
> Object ID
> enterprises,8164.1.1000.1.2.57.
> Description
> This object indicates name of the IMG configuration-file created during the config-backup operation.
> Syntax
> DisplayString (SIZE (1..256))
> Access
> read-only
> starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000)
> starEmsTraps(2)
> Object
> starEmsFmEmailFailed
> Object ID
> enterprises.8164.1.1000.2.3
> Description
> This notification is generated when EMS fault management module email notification failure has occurred.
> Objects
> starEmsNotifRaisedTime
> starEmsNotifInfo
> Object
> starEmsFmScriptFailed
> Object ID
> enterprises.8164.1.1000.2.4
> Description
> This notification is generated when EMS fault management module script execution failure has occurred.
> Objects
> starEmsNotifRaisedTime
> starEmsNotifInfo
> Object
> starEmsFmSyslogFailed
> Object ID
> enterprises.8164.1.1000.2.5
> Description
> This notification is generated when EMS fault management module syslog message logging failure has occurred.
> Objects
> starEmsNotifRaisedTime
> starEmsNotifInfo
> Object
> starEmsWebServerProcStart
> Object ID
> enterprises.8164.1.1000.2.6
> Description
> This notification is generated by EMS Process Monitoring when EMS web server process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsWebServerProcStop
> Object ID
> enterprises.8164.1.1000.2.7
> Description
> This notification is generated by EMS Process Monitoring when EMS web server process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsWebServerProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.8
> Description
> This notification is generated by EMS Process Monitoring when EMS web server process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS web server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsWebServerProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.9
> Description
> This notification is generated by EMS Process Monitoring when EMS web server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS web server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsDataBaseProcStart
> Object ID
> enterprises.8164.1.1000.2.10
> Description
> This notification is generated by EMS Process Monitoring when EMS data base process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsDataBaseProcStop
> Object ID
> enterprises.8164.1.1000.2.11
> Description
> This notification is generated by EMS Process Monitoring when EMS data base process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsDataBaseProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.12
> Description
> This notification is generated by EMS Process Monitoring when EMS data base process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS data base process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsDataBaseProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.13
> Description
> This notification is generated by EMS Process Monitoring when EMS data base process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS data base process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsServerProcStart
> Object ID
> enterprises.8164.1.1000.2.14
> Description
> This notification is generated by EMS Process Monitoring when EMS server process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsServerProcStop
> Object ID
> enterprises.8164.1.1000.2.15
> Description
> This notification is generated by EMS Process Monitoring when EMS server process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsServerProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.16
> Description
> This notification is generated by EMS Process Monitoring when EMS server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsServerProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.17
> Description
> This notification is generated by EMS Process Monitoring when EMS server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsScriptServerProcStart
> Object ID
> enterprises.8164.1.1000.2.18
> Description
> This notification is generated by EMS Process Monitoring when EMS script server process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsScriptServerProcStop
> Object ID
> enterprises.8164.1.1000.2.19
> Description
> This notification is generated by EMS Process Monitoring when EMS script server process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsScriptServerProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.20
> Description
> This notification is generated by EMS Process Monitoring when EMS script server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS script server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsScriptServerProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.21
> Description
> This notification is generated by EMS Process Monitoring when EMS script server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS script server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsServerDirAccessible
> Object ID
> enterprises.8164.1.1000.2.22
> Description
> This notification is generated by EMS Process Monitoring when EMS server directory becomes accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsServerDirNonAccessible
> Object ID
> enterprises.8164.1.1000.2.23
> Description
> This notification is generated by EMS Process Monitoring when EMS server directory is not accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsServerDirUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.24
> Description
> This notification is generated by EMS Process Monitoring when EMS server directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS server directory size usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsServerDirUsageNormal
> Object ID
> enterprises.8164.1.1000.2.25
> Description
> This notification is generated by EMS Process Monitoring when EMS server directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS server directory size usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsDataBaseDirAccessible
> Object ID
> enterprises.8164.1.1000.2.26
> Description
> This notification is generated by EMS Process Monitoring when EMS data base directory becomes accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsDataBaseDirNonAccessible
> Object ID
> enterprises.8164.1.1000.2.27
> Description
> This notification is generated by EMS Process Monitoring when EMS data base directory is not accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsDataBaseDirUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.28
> Description
> This notification is generated by EMS Process Monitoring when EMS data base directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS data base directory size value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsDataBaseDirUsageNormal
> Object ID
> enterprises.8164.1.1000.2.29
> Description
> This notification is generated by EMS Process Monitoring when EMS data base directory size usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS data base directory size usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsFTPDirAccessible
> Object ID
> enterprises.8164.1.1000.2.30
> Description
> This notification is generated by EMS Process Monitoring when EMS FTP directory becomes accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsFTPDirNonAccessible
> Object ID
> enterprises.8164.1.1000.2.31
> Description
> This notification is generated by EMS Process Monitoring when EMS FTP directory is not accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsFTPDirUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.32
> Description
> This notification is generated by EMS Process Monitoring when EMS FTP directory usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS FTP directory usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsFTPDirUsageNormal
> Object ID
> enterprises.8164.1.1000.2.33
> Description
> This notification is generated by EMS Process Monitoring when EMS FTP directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS FTP directory size usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsBlkArchDirAccessible
> Object ID
> enterprises.8164.1.1000.2.34
> Description
> This notification is generated by EMS Process Monitoring when EMS bulk archive directory becomes accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBlkArchDirNonAccessible
> Object ID
> enterprises.8164.1.1000.2.35
> Description
> This notification is generated by EMS Process Monitoring when EMS bulk archive directory is not accessible.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBlkArchDirUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.36
> Description
> This notification is generated by EMS Process Monitoring when EMS bulk archive directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS bulk archive directory size value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsBlkArchDirUsageNormal
> Object ID
> enterprises.8164.1.1000.2.37
> Description
> This notification is generated by EMS Process Monitoring when EMS bulk archive directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS bulk archive directory size usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsInterfaceStateUp
> Object ID
> enterprises.8164.1.1000.2.38
> Description
> This notification is generated by EMS Process Monitoring when EMS interface state comes up. Varbinds indicate interface IP address and name.
> Objects
> starEmsNotifRaisedTime
> starEmsInterfaceAddr
> starEmsInterfaceName
> Object
> starEmsInterfaceStateDown
> Object ID
> enterprises.8164.1.1000.2.39
> Description
> This notification is generated by EMS Process Monitoring when EMS interface state goes down. Varbinds indicate interface address and name
> Objects
> starEmsNotifRaisedTime
> starEmsInterfaceAddr
> starEmsInterfaceName
> Object
> starEmsCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.40
> Description
> This notification is generated by EMS Process Monitoring when EMS CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS CPU usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.41
> Description
> This notification is generated by Process Monitoring when EMS CPU usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS CPU usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsSwapUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.42
> Description
> This notification is generated by Process Monitoring when EMS swap usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS swap usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsSwapUsageNormal
> Object ID
> enterprises.8164.1.1000.2.43
> Description
> This notification is generated by Process Monitoring when EMS swap usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS swap usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsPCFtpFailed
> Object ID
> enterprises.8164.1.1000.2.44
> Description
> This notification is generated by Periodic Configuration Saving module when FTP fails while fetching a config file from the IMG.
> Objects
> starEmsNotifRaisedTime
> starEmsImgAddr
> starEmsFtpFileName
> starEmsNotifInfo
> Object
> starEmsPCFileDeletionFailed
> Object ID
> enterprises.8164.1.1000.2.45
> Description
> This notification is generated by Periodic Configuration Saving module when deletion of file on the IMG fails.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGAddr
> starEmsFtpFileName
> starEmsNotifInfo
> Object
> starEmsBulkStatFtpFailed
> Object ID
> enterprises.8164.1.1000.2.46
> Description
> This notification is generated by Bulkstat module when bulkstat file transfer operation from IMG fails or gets delayed than the expected time
> Objects
> starEmsNotifRaisedTime
> starEmsBulkStatFileXferTime
> starEmsIMGState
> starEmsIMGAddr
> Object
> starEmsBulkStatFtpClear
> Object ID
> enterprises.8164.1.1000.2.47
> Description
> This notification is generated by BulkStat module when bulkstat file transfer operation from IMG succeeds and starEmsBulkStatFtpFailed trap is already raised for the IMG.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGAddr
> Object
> starEmsXMLFtpFailed
> Object ID
> enterprises.8164.1.1000.2.48
> Description
> This notification is generated by EMS when FTP of Bulkstat XML file on the NMS fails.
> Objects
> starEmsNotifRaisedTime
> starEmsXMLFtpDestAddr
> starEmsXMLFtpDestPath
> starEmsNotifInfo
> Object
> starEmsXMLFtpSuccess
> Object ID
> enterprises.8164.1.1000.2.49
> Description
> This notification is generated by EMS when FTP of Bulk stat XML file on the NMS succeed.
> Objects
> starEmsNotifRaisedTime
> starEmsXMLFtpDestAddr
> starEmsXMLFtpDestPath
> starEmsNotifInfo
> Object
> starEmsIMGUnmanageable
> Object ID
> enterprises.8164.1.1000.2.50
> Description
> This notification is generated by EMS when IMG becomes unmanageable.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsIMGAddr
> starEmsIMGPreviousState
> Object
> starEmsIMGManageable
> Object ID
> enterprises.8164.1.1000.2.51
> Description
> This notification is generated by EMS when IMG becomes manageable.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsIMGAddr
> starEmsIMGPreviousState
> Object
> starEmsPortMonThresholdBelowLimit
> Object ID
> enterprises.8164.1.1000.2.52
> Description
> This notification is generated by EMS Port Monitoring when delta value for a particular port has fallen below the configured threshold value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsIMGAddr
> starSlotNum
> starPortNum
> starEmsPortMonThreshold
> starEmsPortMonCurrent
> Object
> starEmsPortMonThresholdNormal
> Object ID
> enterprises.8164.1.1000.2.53
> Description
> This notification is generated by EMS Port Monitoring when delta value for a particular port threshold comes to normal value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsIMGAddr
> starSlotNum
> starPortNum
> starEmsPortMonThreshold
> starEmsPortMonCurrent
> Object
> starEmsPortMonError
> Object ID
> enterprises.8164.1.1000.2.54
> Description
> This notification is generated by EMS Port Monitoring when any error in fetching values from a particular IMG.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsIMGAddr
> starEmsNotifInfo
> Object
> starEmsWebServerProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.55
> Description
> This notification is generated by EMS Process Monitoring when EMS web server process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsDataBaseProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.56
> Description
> This notification is generated by EMS Process Monitoring when EMS Data Base process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsServerProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.57
> Description
> This notification is generated by EMS Process Monitoring when EMS server process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsScriptServerProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.58
> Description
> This notification is generated by EMS Process Monitoring when EMS Script server process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBulkStatServerProcStart
> Object ID
> enterprises.8164.1.1000.2.59
> Description
> This notification is generated by EMS Process Monitoring when Ems Bulkstat server process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBulkStatServerProcStop
> Object ID
> enterprises.8164.1.1000.2.60
> Description
> This notification is generated by EMS Process Monitoring when Ems Bulkstat server process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBulkStatServerProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.61
> Description
> This notification is generated by EMS Process Monitoring when Ems Bulkstat server process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBulkStatServerProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.62
> Description
> This notification is generated by EMS Process Monitoring when EMS Bulkstat server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS Bulkstat server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsBulkStatServerProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.63
> Description
> This notification is generated by EMS Process Monitoring when EMS Bulkstat server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS Bulkstat server process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsBulkStatParserProcStart
> Object ID
> enterprises.8164.1.1000.2.64
> Description
> his notification is generated by EMS Process Monitoring when Ems Bulkstat parser process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBulkStatParserProcStop
> Object ID
> enterprises.8164.1.1000.2.65
> Description
> This notification is generated by EMS Process Monitoring when Ems Bulkstat parser process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBulkStatParserProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.66
> Description
> This notification is generated by EMS Process Monitoring when Ems Bulkstat parser process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsBulkStatParserProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.67
> Description
> This notification is generated by EMS Process Monitoring when EMS Bulkstat parser process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS Bulkstat parser process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsBulkStatParserProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.68
> Description
> This notification is generated by EMS Process Monitoring when EMS Bulkstat parser process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS Bulkstat parser process cpu usage value in percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsIMGRateControlStart
> Object ID
> enterprises.8164.1.1000.2.69
> Description
> This notification is generated by EMS when IMG Rate-Control is stated. IMG's CORBA server resource utilization is over limit.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsIMGAddr
> Object
> starEmsIMGRateControlStop
> Object ID
> enterprises.8164.1.1000.2.70
> Description
> This notification is generated by EMS when IMG Rate-Control is stopped. IMG's CORBA server resource utilization is over limit.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsIMGAddr
> Object
> starEmsMonitorQueueFull
> Object ID
> enterprises.8164.1.1000.2.71
> Description
> This notification is generated by EMS when monitor event queue is full.
> Objects
> starEmsNotifRaisedTime
> starEmsTotalPendingEvts
> starEmsMaxLimit
> starEmsClientAddr
> starEmsMonOldEvtTimeStamp
> starEmsMonitorType
> starEmsMonitorUserName
> Object
> starEmsMonitorQueueInLimit
> Object ID
> enterprises.8164.1.1000.2.72
> Description
> This notification is generated by EMS when the monitor event queue is partially full.
> Objects
> starEmsNotifRaisedTime
> starEmsTotalPendingEvts
> starEmsMaxLimit
> starEmsClientAddr
> starEmsMonitorType
> starEmsMonitorUserName
> Object
> starClusterFailoverHappened
> Object ID
> enterprises.8164.1.1000.2.73
> Description
> This notification is generated by EMS when cluster failover happens.
> Objects
> starEmsNotifRaisedTime
> starEmsPrevHostName
> starEmsCurrHostName
> Object
> starEmsDBBackupNoDiscSpace
> Object ID
> enterprises.8164.1.1000.2.74
> Description
> This notification is generated by EMS when disc space gets full. No disc space is available.
> Objects
> starEmsNotifRaisedTime
> starEmsDevicePath
> Object
> starEMSP2PProtocolUsageHigh
> Object ID
> enterprises.8164.1.1000.2.75
> Description
> This notification is generated by EMS when protocol values are beyond the threshold value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsP2PProtocolType
> starEmsP2PProtocolVal
> Object
> starEmsP2PProtocolUsageLimit
> Object ID
> enterprises.8164.1.1000.2.76
> Description
> This notification is generated by EMS when protocol values are within limit.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsP2PProtocolType
> starEmsP2PProtocolVal
> Object
> starEmsKeywordDetectedInSyslog
> Object ID
> enterprises.8164.1.1000.2.77
> Description
> This notification is generated by EMS when a configured keyword is detected in the syslog message.
> Objects
> starEmsNotifRaisedTime
> starEmsSyslogLoggedTime
> starEmsSyslogFacility
> starEmsSyslogPriority
> starEmsSyslogHostname
> starEmsSyslogKeyword
> starEmsSyslogMessage
> starEmsSyslogFilePath
> Object
> starEmsDBMigration
> Object ID
> enterprises.8164.1.1000.2.78
> Description
> This notification is generated by EMS when the database migration is done for a particular database.
> Objects
> starEmsNotifRaisedTime
> starEmsDBName
> Object
> starEmsNBServerProcStart
> Object ID
> enterprises.8164.1.1000.2.79
> Description
> This notification is generated by EMS process monitoring when the EMS NB server process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsNBServerProcStop
> Object ID
> enterprises.8164.1.1000.2.80
> Description
> This notification is generated by EMS process monitoring when the EMS NB server process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsNBServerProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.81
> Description
> This notification is generated by EMS process monitoring when the EMS NB server process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsNBServerProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.82
> Description
> This notification is generated by EMS process monitoring when the NB server process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current NB server process CPU value as a percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsNBServerProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.83
> Description
> This notification is generated by EMS process monitoring when the NB server process CPU usage threshold comes to a normal value. The starEmsThreshold varbind indicates current NB server process cpu value as a percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsNotifyServiceProcStart
> Object ID
> enterprises.8164.1.1000.2.84
> Description
> This notification is generated by EMS process monitoring when the EMS notification service process comes up.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsNotifyServiceProcStop
> Object ID
> enterprises.8164.1.1000.2.85
> Description
> This notification is generated by EMS process monitoring when the EMS notification service process goes down.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsNotifyServiceProcDetectRestart
> Object ID
> enterprises.8164.1.1000.2.86
> Description
> This notification is generated by EMS process monitoring when the EMS notification service process restart is detected.
> Objects
> starEmsNotifRaisedTime
> Object
> starEmsNotifyServiceProcCPUUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.87
> Description
> This notification is generated by EMS process monitoring when the Ems Notification Service process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current Ems Notification Service process cpu usage value as a percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsNotifyServiceProcCPUUsageNormal
> Object ID
> enterprises.8164.1.1000.2.88
> Description
> This notification is generated by EMS process monitoring when the Ems Notification Service process CPU usage threshold comes to normal. The starEmsThreshold varbind indicates current Ems Notification Service process cpu usage value as a percentage.
> Objects
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> Object
> starEmsBulkStatCounterThresholdAboveLimit
> Important: This Trap is obsolete.
> Object ID
> enterprises.8164.1.1000.2.89
> Description
> This notification is generated by the EMS bulkstat parser when the delta value for a particular bulkstat counter has exceeded its configured threshold value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsBulkstatCounter
> starEmsBulkStatRecordDetails
> starEmsBulkStatRecordTime
> starEmsBulkStatThreshold
> starEmsBulkStatCurrent
> Object
> starEmsBulkStatCounterThresholdNormal
> Important: This Trap is obsolete.
> Object ID
> enterprises.8164.1.1000.2.90
> Description
> This notification is generated by the EMS bulkstat parser when the delta value for a particular bulkstat counter comes to the normal value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsBulkstatCounter
> starEmsBulkStatRecordDetails
> starEmsBulkStatRecordTime
> starEmsBulkStatThreshold
> starEmsBulkStatCurrent
> Object
> starEmsCFDBDirAccessible
> Object ID
> enterprises.8164.1.1000.2.91
> Description
> This notification is generated by EMS Process Monitoring when EMS content filtering directory is accessible.
> Objects
> starEMSNotifRaisedTime
> Object
> starEmsCFDBDirNonAccessible
> Object ID
> enterprises.8164.1.1000.2.92
> Description
> This notification is generated by EMS Process Monitoring when EMS content filtering directory is not accessible.
> Possible Cause: None given.
> Action Clear: A starEmsCFDBDirAccessible message is generated when the database comes back online.
> Objects
> starEMSNotifRaisedTime
> Object
> starEmsCFDBDirUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.93
> Description
> EMS content filtering directory usage threshold is exceeded.
> Possible Cause: This is a user-configurable parameter.
> Action Clear: A starEMSCFDBDirUsageNormal notification is issued when usage drops below the threshold.
> Objects
> starEMSNotifRaisedTime
> starEMSProcMonThreshold
> Object
> starEmsCFDBDirUsageNormal
> Object ID
> enterprises.8164.1.1000.2.94
> Description
> EMS content filtering directory usage has come to normal value.
> Objects
> starEMSNotifRaisedTime
> starEMSProcMonThreshold
> Object
> starEmsCFDbImportFailed
> Object ID
> enterprises.8164.1.1000.2.95
> Description
> This notification is generated by CFEMS when failed to Import database file.
> Possible Cause: None given
> Action Clear: A starEmsCFDbImportSucceeded message is generated when the database file is successfully imported.
> Objects
> starEmsNotifRaisedTime,
> starEmsCFMcrdbsHostAddress,
> starEmsCFDbType,
> starEmsCFSourceDbFileName
> Object
> starEmsCFDbImportSucceeded
> Object ID
> enterprises.8164.1.1000.2.96
> Description
> This notification is generated by CFEMS Database file is imported.
> Objects
> starEmsNotifRaisedTime,
> starEmsCFMcrdbsHostAddress,
> starEmsCFDbType,
> starEmsCFSourceDbFileName
> Object
> starEmsCFDbExportFailed
> Object ID
> enterprises.8164.1.1000.2.97
> Description
> This notification is generated by CFEMS when database has failed to export.
> Possible Cause: None given
> Action Clear: A starEmsCFDbExportSucceeded message is generated.
> Objects
> starEmsNotifRaisedTime,
> starEmsCFCdpHostAddress,
> starEmsCFDbType,
> starEmsCFSourceDbFileName
> Object
> starEmsCFDbExportSucceeded
> Object ID
> enterprises.8164.1.1000.2.98
> Description
> This notification is generated by CFEMS on successful export of a database file.
> Objects
> starEmsNotifRaisedTime,
> starEmsCFCdpHostAddress,
> starEmsCFDbType,
> starEmsCFSourceDbFileName
> Object
> starEmsCFDbConversionFailed
> Object ID
> enterprises.8164.1.1000.2.99
> Description
> CF database conversion/manipulation operation failed.
> Possible Cause: None given
> Action Clear: A starEmsCFDbConversionSucceeded message is generated.
> Objects
> starEmsNotifRaisedTime,
> starEmsCFFromDbType,
> starEmsCFToDbType,
> starEmsCFSourceDbFileName,
> starEmsCFDestDbFileName
> Object
> starEmsCFDbConversionSucceeded
> Object ID
> enterprises.8164.1.1000.2.100
> Description
> This notification is generated by CFEMS when Database conversion done successfully.
> Objects
> starEmsNotifRaisedTime,
> starEmsCFFromDbType,
> starEmsCFToDbType,
> starEmsCFSourceDbFileName,
> starEmsCFDestDbFileName
> Object
> starEmsCFFtpConnetionFailed
> Object ID
> enterprises.8164.1.1000.2.101
> Description
> SFTP Connection failed.
> Objects
> starEmsNotifRaisedTime,
> starEmsCFFtpHostInfo
> Object
> starEmsBulkStatCounterUsageOverLimit
> Important: This Trap is obsolete.
> Object ID
> enterprises.8164.1.1000.2.102
> Description
> This notification is generated by EMS bulkstat parser when counter value for a particular bulkstat counter has reached or exceeded the configured threshold value.
> Possible Cause:This is a user-configurable parameter.
> Action Clear:A starEmsBulkStatCounterUsageNormal message is generated when usage drops below the threshold.
> Objects
> starEmsNotifRaisedTime,
> starEmsIMGName,
> starEmsBulkStatCounter,
> starEmsBulkStatRecordDetails,
> starEmsBulkStatRecordTime,
> starEmsBulkStatThreshold,
> starEmsBulkStatCounterValue
> Object
> starEmsBulkStatCounterUsageNormal
> Important: This Trap is obsolete.
> Object ID
> enterprises.8164.1.1000.2.103
> Description
> This message is generated when usage drops below the threshold.
> Objects
> starEmsNotifRaisedTime,
> starEmsIMGName,
> starEmsBulkStatCounter,
> starEmsBulkStatRecordDetails,
> starEmsBulkStatRecordTime,
> starEmsBulkStatThreshold,
> starEmsBulkStatCounterValue
> Object
> starEmsConfigBackupFtpFailed
> Object ID
> enterprises.8164.1.1000.2.104
> Description
> This notification is generated by EMS when FTP of Config Backup file from STxx to EMS fails.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsNotifInfo
> Object
> starEmsConfigBackupFtpSuccess
> Object ID
> enterprises.8164.1.1000.2.105
> Description
> his notification is generated by EMS when FTP of Config Backup file from STxx to EMS succeed.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsNotifInfo
> Object
> starEmsBulkStatIncrementalCounterThresholdAboveLimit
> Object ID
> enterprises.8164.1.1000.2.106
> Description
> This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter has exceeded the configured threshold value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsBulkStatCounter
> starEmsBulkStatRecordDetails
> starEmsBulkStatRecordTime
> starEmsBulkStatThresholdDouble
> starEmsBulkStatCurrentDouble
> starEmsBulkStatFilterDetails
> Object
> starEmsBulkStatIncrementalCounterThresholdNormal
> Object ID
> enterprises.8164.1.1000.2.107
> Description
> This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter comes to normal value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsBulkStatCounter
> starEmsBulkStatRecordDetails
> starEmsBulkStatRecordTime
> starEmsBulkStatThresholdDouble
> starEmsBulkStatCurrentDouble
> starEmsBulkStatFilterDetails
> Object
> starEmsBulkStatGaugeCounterUsageOverLimit
> Object ID
> enterprises.8164.1.1000.2.108
> Description
> This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter has exceeded the configured threshold value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsBulkStatCounter
> starEmsBulkStatRecordDetails
> starEmsBulkStatRecordTime
> starEmsBulkStatThresholdDouble
> starEmsBulkStatCurrentDouble
> starEmsBulkStatFilterDetails
> Object
> starEmsBulkStatGaugeCounterUsageNormal
> Object ID
> enterprises.8164.1.1000.2.109
> Description
> This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter comes to normal value.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsBulkStatCounter
> starEmsBulkStatRecordDetails
> starEmsBulkStatRecordTime
> starEmsBulkStatThresholdDouble
> starEmsBulkStatCurrentDouble
> starEmsBulkStatFilterDetails
> Object
> starEmsConfigBackupFileDiff
> Object ID
> enterprises.8164.1.1000.2.110
> Description
> This notification is generated by WEM during periodic config-backup operation. It is generated to indicate that the recently downloaded configuration file is different from the configuration file downloaded in the last config-backup operation. The third varbind indicates the name of the latest downloaded config-file. The fourth varbind indicates the name of the config file that was downloaded during the last config-backup opeartions.
> Objects
> starEmsNotifRaisedTime
> starEmsIMGName
> starEmsConfigBackupFileName
> starEmsConfigBackupFileName
> starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000)
> starEmsMIBConformances(3)
> starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000)
> starEmsMIBConformances(3).starEmsMIBCompliances(1)
> Object
> starEmsMIBCompliance
> Object ID
> enterprises.8164.1.1000.3.1.1
> Description
> The compliance statements for entities which implement the STARENT EMS MIB.
> Required Groups
> starEmsNotifMgmtGroup
> starEmsNotifGroup
> starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000)
> starEmsMIBConformances(3).starEmsMIBGroups(2)
> Object Group
> starEmsNotifMgmtGroup
> Object ID
> enterprises.8164.1.1000.3.2.1
> Description
> This is a collection of objects related with notification management on EMS.
> Objects
> starEmsNotifInfo
> starEmsNotifRaisedTime
> starEmsProcMonThreshold
> starEmsInterfaceAddr
> starEmsInterfaceName
> starEmsIMGAddr
> starEmsFtpFileName
> starEmsIMGState
> starEmsBulkStatFileXferTime
> starEmsXMLFtpFileName
> starEmsXMLFtpDestAddr
> starEmsXMLFtpDestPath
> starEmsIMGPreviousState
> starEmsIMGName
> starEmsPortMonThreshold
> starEmsPortMonCurrent
> starEmsDevicePath
> starEmsPrevHostName
> starEmsCurrHostName
> starEmsP2PProtocolType
> starEmsP2PProtocolValue
> starEmsSyslogLoggedTime
> starEmsSyslogFacility
> starEmsSyslogPriority
> starEmsSyslogHostname
> starEmsSyslogKeyword
> starEmsSyslogMessage
> starEmsSyslogFilePath
> starEmsDBName
> starEmsBulkStatCounter
> starEmsBulkStatRecordDetails
> starEmsBulkStatRecordTime
> starEmsBulkStatThreshold
> starEmsBulkStatCurrent
> starEmsCFMcrdbsHostAddress,
> starEmsCFDbType,
> starEmsCFSourceDbFileName,
> starEmsCFCdpHostAddress,
> starEmsCFFromDbType,
> starEmsCFToDbType,
> starEmsCFDestDbFileName,
> starEmsBulkStatCounterValue
> starEmsBulkStatFilterDetails
> starEmsBulkStatCounterDouble
> starEmsBulkStatThresholdDouble
> starEmsConfigBackupFileName
> Object Group
> starEmsNotifGroup
> Object ID
> enterprises.8164.1.1000.3.2.2
> Description
> A collection of EMS notifications.
> Object Group
> starEmsFmEmailFailed
> starEmsFmScriptFailed
> starEmsFmSyslogFailed
> starEmsWebServerProcStart
> starEmsWebServerProcStop
> starEmsWebServerProcCPUUsageOverLimit
> starEmsWebServerProcCPUUsageNormal
> starEmsDataBaseProcStart
> starEmsDataBaseProcStop
> starEmsDataBaseProcCPUUsageOverLimit
> starEmsDataBaseProcCPUUsageNormal
> starEmsServerProcStart
> starEmsServerProcStop
> starEmsServerProcCPUUsageOverLimit
> starEmsServerProcCPUUsageNormal
> starEmsScriptServerProcStart
> starEmsScriptServerProcStop
> starEmsScriptServerProcCPUUsageOverLimit
> starEmsScriptServerProcCPUUsageNormal
> starEmsServerDirAccessible
> starEmsServerDirNonAccessible
> starEmsServerDirUsageOverLimit
> starEmsServerDirUsageNormal
> starEmsDataBaseDirAccessible
> starEmsDataBaseDirNonAccessible
> starEmsDataBaseDirUsageOverLimit
> starEmsDataBaseDirUsageNormal
> starEmsFTPDirAccessible
> starEmsFTPDirNonAccessible
> starEmsFTPDirUsageOverLimit
> starEmsFTPDirUsageNormal
> starEmsBlkArchDirAccessible
> starEmsBlkArchDirNonAccessible
> starEmsBlkArchDirUsageOverLimit
> starEmsBlkArchDirUsageNormal
> starEmsInterfaceStateUp
> starEmsInterfaceStateDown
> starEmsCPUUsageOverLimit
> starEmsCPUUsageNormal
> starEmsSwapUsageOverLimit
> starEmsSwapUsageNormal
> starEmsPCFtpFailed
> starEmsPCFileDeletionFailed
> starEmsBulkStatFtpFailed
> starEmsBulkStatFtpClear
> starEmsXMLFtpFailed
> starEmsXMLFtpSuccess
> starEmsIMGUnmanageable
> starEmsIMGManageable
> starEmsPortMonThresholdBelowLimit
> starEmsPortMonThresholdNormal
> starEmsPortMonError
> starEmsWebServerProcDetectRestart
> starEmsDataBaseProcDetectRestart
> starEmsServerProcDetectRestart
> starEmsScriptServerProcDetectRestart
> starEmsBulkStatServerProcStart
> starEmsBulkStatServerProcStop
> starEmsBulkStatServerProcDetectRestart
> starEmsBulkStatServerProcCPUUsageOverLimit
> starEmsBulkStatServerProcCPUUsageNormal
> starEmsBulkStatParserProcStart
> starEmsBulkStatParserProcStop
> starEmsBulkStatParserProcDetectRestart
> starEmsBulkStatParserProcCPUUsageOverLimit
> starEmsBulkStatParserProcCPUUsageNormal
> starEmsIMGRateControlStart
> starEmsIMGRateControlStop
> starEmsMonitorQueueFull
> starEmsMonitorQueueInLimit
> starEmsNotifRaisedTime
> starClusterFailoverHappened
> starEmsDBBackupNoDiscSpace
> starEmsP2PProtocolUsageHigh
> starEmsP2PProtocolUsageLimit
> starEmsNBServerProcStart
> starEmsNBServerProcStop
> starEmsNBServerProcDetectRestart
> starEmsNBServerProcCPUUsageOverLimit
> starEmsNBServerProcCPUUsageNormal
> starEmsNotifyServiceProcStart
> starEmsNotifyServiceProcStop
> starEmsNotifyServiceProcDetectRestart
> starEmsNotifyServiceProcCPUUsageOverLimit
> starEmsNotifyServiceProcCPUUsageNormal
> starEmsKeywordDetectedInSyslog
> starEmsDBMigration
> starEmsBulkStatCounterThresholdAboveLimit
> starEmsBulkStatCounterThresholdNormal
> starEmsCFDBDirAccessible
> starEmsCFDBDirNonAccessible,
> starEmsCFDBDirUsageOverLimit,
> starEmsCFDBDirUsageNormal,
> starEmsCFDbImportFailed,
> starEmsCFDbImportSucceeded,
> starEmsCFDbExportFailed,
> starEmsCFDbExportSucceeded,
> starEmsCFDbConversionFailed,
> starEmsCFDbConversionSucceeded,
> starEmsCFFtpConnetionFailed,
> starEmsBulkStatCounterUsageOverLimit,
> starEmsBulkStatCounterUsageNormal
> starEmsConfigBackupFtpFailed
> starEmsConfigBackupFtpSuccess
> starEmsBulkStatIncrementalCounterThresholdAboveLimit
> starEmsBulkStatIncrementalCounterThresholdNormal
> starEmsBulkStatGaugeCounterUsageOverLimit
> starEmsBulkStatGaugeCounterUsageNormal
> starEmsConfigBackupFileDiff

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883