> Accounting Management
> This section contains additions and changes made to the accounting-related parameters in Release 12.x.
> Topics covered in this chapter are:

> l | Bulk Statistic Enhancements

> l | CDR Enhancements

> l | Diameter Attributes

> l | RADIUS Attributes

> l | Web Element Manager Enhancements

> Bulk Statistic Enhancements
> This section lists bulk statistic additions and changes in Release 12.x.

> l | Bulk Statistic Enhancements in Release 12.0

> l | Bulk Statistic Enhancements in Release 12.1

> l | Bulk Statistic Enhancements in Release 12.2

> For detailed information on bulk statistics refer to the System Administration Guide and Statistics and Counters Reference.
> Bulk Statistic Enhancements in Release 12.0
> This section lists bulk statistic additions and changes in Release 12.0.

> l | New Bulk Statistics

> l | Modified Bulk Statistics

> l | Obsoleted Bulk Statistics

> New Bulk Statistics
> Support for the following bulk statistics were added in Release 12.0.
> Context Schema

> l | sfw-ipv6-discardpackets

> l | sfw-ipv6-malpackets

> l | sfw-icmpv6-discardpackets

> l | sfw-icmpv6-malpackets

> Diameter Authentication Schema

> l | asa-rsp-rej-sent

> l | req-sock-write-err

> l | rsp-sock-write-err

> l | any-sock-read-err

> l | rem-disconnect

> l | loc-disconnect

> DLCI-Util Schema

> l | card

> l | port

> l | dlci_util_path

> l | dlci_util_ds1e1

> l | dlci_util_timeslot

> l | dlci_util_dlci_no

> l | dlci_util_nsvc

> l | dlci_util_nse

> l | dlci_util_dlci_curr_rx

> l | dlci_util_dlci_curr_tx

> l | dlci_util_dlci_5min_rx

> l | dlci_util_dlci_5min_tx

> l | dlci_util_dlci_15min_rx

> l | dlci_util_dlci_15min_tx

> ECS Schema

> l | h323-calls

> l | h323-uplk-bytes

> l | h323-dwnlk-bytes

> l | h323-uplk-pkts

> l | h323-dwnlk-pkts

> l | h323-q931-messages

> l | h323-h245-messages

> l | h323-ras-messages

> l | pptp-flows

> l | pptp-gre-flows

> l | pptp-uplk-bytes

> l | pptp-dwnlk-bytes

> l | pptp-uplk-pkts

> l | pptp-dwnlk-pkts

> l | pptp-inv-pkts

> l | pptp-unknown-pkts

> l | pptp-gre-uplk-bytes

> l | pptp-gre-dwnlk-bytes

> l | pptp-gre-uplk-pkts

> l | pptp-gre-dwnlk-pkts

> l | tftp-flows

> l | tftp-uplk-bytes

> l | tftp-dwnlk-bytes

> l | tftp-uplk-pkts

> l | tftp-dwnlk-pkts

> l | tftp-total-read-sessions

> l | tftp-total-write-sessions

> l | tftp-unsupp-req-pkts

> l | tftp-invalid-ctrl-pkts

> l | tftp-invalid-data-pkts

> l | tftp-data-uplk-bytes

> l | tftp-data-dwnlk-bytes

> l | tftp-data-uplk-pkts

> l | tftp-data-dwnlk-pkts

> l | p2p-skype-unclassified-uplnk-bytes — This variable replaces p2p-skype-non-audio-uplnk-bytes.

> l | p2p-skype-unclassified-dwlnk-bytes — This variable replaces p2p-skype-non-audio-dwlnk-bytes.

> l | p2p-skype-unclassified-uplnk-pkts — This variable replacesp2p-skype-non-audio-uplnk-pkts.

> l | p2p-skype-unclassified-dwlnk-pkts — This variable replaces p2p-skype-non-audio-dwlnk-pkts.

> l | p2p-msn-unclassified-uplnk-bytes — This variable replaces p2p-msn-non-audio-or-video-uplnk-bytes.

> l | p2p-msn-unclassified-dwlnk-bytes — This variable replaces p2p-msn-non-audio-or-video-dwlnk-bytes.

> l | p2p-msn-unclassified-uplnk-pkts — This variable replaces p2p-msn-non-audio-or-video-uplnk-pkts.

> l | p2p-msn-unclassified-dwlnk-pkts — This variable replaces p2p-msn-non-audio-or-video-dwlnk-pkts.

> l | p2p-yahoo-unclassified-uplnk-bytes — This variable replaces p2p-yahoo-non-audio-uplnk-bytes.

> l | p2p-yahoo-unclassified-dwlnk-bytes — This variable replaces p2p-yahoo-non-audio-dwlnk-bytes.

> l | p2p-yahoo-unclassified-uplnk-pkts — This variable replaces p2p-yahoo-non-audio-uplnk-pkts.

> l | p2p-yahoo-unclassified-dwlnk-pkts — This variable replaces p2p-yahoo-non-audio-dwlnk-pkts.

> l | p2p-oscar-unclassified-uplnk-bytes — This variable replaces p2p-oscar-non-audio-uplnk-bytes.

> l | p2p-oscar-unclassified-dwlnk-bytes — This variable replaces p2p-oscar-non-audio-dwlnk-bytes.

> l | p2p-oscar-unclassified-uplnk-pkts — This variable replaces p2p-oscar-non-audio-uplnk-pkts.

> l | p2p-oscar-unclassified-dwlnk-pkts — This variable replaces p2p-oscar-non-audio-dwlnk-pkts.

> l | p2p-gtalk-unclassified-uplnk-bytes — This variable replaces p2p-gtalk-non-audio-uplnk-bytes.

> l | p2p-gtalk-unclassified-dwlnk-bytes — This variable replaces p2p-gtalk-non-audio-dwlnk-bytes.

> l | p2p-gtalk-unclassified-uplnk-pkts — This variable replaces p2p-gtalk-non-audio-uplnk-pkts.

> l | p2p-gtalk-unclassified-dwlnk-pkts — This variable replaces p2p-gtalk-non-audio-dwlnk-pkts.

> l | p2p-oscar-video-uplnk-bytes

> l | p2p-oscar-video-dwlnk-bytes

> l | p2p-oscar-video-uplnk-pkts

> l | p2p-oscar-video-dwlnk-pkts

> l | p2p-gtalk-video-uplnk-bytes

> l | p2p-gtalk-video-dwlnk-bytes

> l | p2p-gtalk-video-uplnk-pkts

> l | p2p-gtalk-video-dwlnk-pkts

> l | p2p-yahoo-video-uplnk-bytes

> l | p2p-yahoo-video-dwlnk-bytes

> l | p2p-yahoo-video-uplnk-pkts

> l | p2p-yahoo-video-dwlnk-pkts

> l | p2p-blackberry-uplnk-bytes

> l | p2p-blackberry-dwlnk-bytes

> l | p2p-blackberry-uplnk-pkts

> l | p2p-blackberry-dwlnk-pkts

> l | p2p-gmail-uplnk-bytes

> l | p2p-gmail-dwlnk-bytes

> l | p2p-gmail-uplnk-pkts

> l | p2p-gmail-dwlnk-pkts

> l | p2p-itunes-uplnk-bytes

> l | p2p-itunes-dwlnk-bytes

> l | p2p-itunes-uplnk-pkts

> l | p2p-itunes-dwlnk-pkts

> l | p2p-myspace-uplnk-bytes

> l | p2p-myspace-dwlnk-bytes

> l | p2p-myspace-uplnk-pkts

> l | p2p-myspace-dwlnk-pkts

> l | p2p-teamviewer-uplnk-bytes

> l | p2p-teamviewer-dwlnk-bytes

> l | p2p-teamviewer-uplnk-pkts

> l | p2p-teamviewer-dwlnk-pkts

> l | p2p-twitter-uplnk-bytes

> l | p2p-twitter-dwlnk-bytes

> l | p2p-twitter-uplnk-pkts

> l | p2p-twitter-dwlnk-pkts

> l | p2p-viber-uplnk-bytes

> l | p2p-viber-dwlnk-bytes

> l | p2p-viber-uplnk-pkts

> l | p2p-viber-dwlnk-pkts

> eGTP-C Service Schema

> l | csfb-sent-suspendnotf

> l | csfb-sent-retranssuspendnotf

> l | csfb-recv-suspendnotf

> l | csfb-recv-retranssuspendnotf

> l | csfb-sent-suspendack

> l | csfb-sent-suspendackaccept

> l | csfb-sent-suspendackdenied

> l | csfb-recv-suspendackp

> l | csfb-recv-suspendackaccept

> l | csfb-recv-suspenddenied

> l | csfb-sent-resumenotf

> l | csfb-sent-retransresumenotf

> l | csfb-recv-resumenotf

> l | csfb-recv-retransresumenotf

> l | csfb-sent-resumeack

> l | csfb-sent-resumeackaccept

> l | csfb-sent-resumeackdenied

> l | csfb-recv-resumeackp

> l | csfb-recv-resumeackaccept

> l | csfb-recv-resumedenied

> SGs Schema
> This is a new schema in 12.0.

> l | vpnname

> l | vpnid

> l | servname

> l | servid

> l | pag-req-tx

> l | pag-req-retx

> l | pag-req-rx

> l | pag-rej-tx

> l | pag-rej-retx

> l | pag-rej-rx

> l | service-req-tx

> l | service-req-retx

> l | service-req-rx

> l | dl-ud-tx

> l | dl-ud-retx

> l | dl-ud-rx

> l | ul-ud-tx

> l | ul-ud-retx

> l | ul-ud-rx

> l | localupd-req-tx

> l | localupd-req-retx

> l | localupd-req-rx

> l | localupd-accept-tx

> l | localupd-accept-retx

> l | localupd-accept-rx

> l | localupd-rej-tx

> l | localupd-rej-retx

> l | localupd-rej-rx

> l | tmsi-reloc-tx

> l | tmsi-reloc-retx

> l | tmsi-reloc-rx

> l | alert-req-tx

> l | alert-req-retx

> l | alert-req-rx

> l | alert-ack-tx

> l | alert-ack-retx

> l | alert-ack-rx

> l | alert-rej-tx

> l | alert-rej-retx

> l | alert-rej-rx

> l | ue-actind-tx

> l | ue-actind-retx

> l | ue-actind-rx

> l | eps-detind-tx

> l | eps-detind-retx

> l | eps-detind-rx

> l | eps-detack-tx

> l | eps-detack-retx

> l | eps-detack-rx

> l | imsi-detind-tx

> l | imsi-detind-retx

> l | imsi-detind-rx

> l | imsi-detack-tx

> l | imsi-detack-retx

> l | imsi-detack-rx

> l | reset-ind-tx

> l | reset-ind-retx

> l | reset-ind-rx

> l | reset-ack-tx

> l | reset-ack-retx

> l | reset-ack-rx

> l | mm-inforeq-tx

> l | mm-inforeq-retx

> l | mm-inforeq-rx

> l | rel-req-tx

> l | rel-req-retx

> l | rel-req-rx

> l | status-tx

> l | status-retx

> l | status-rx

> l | ue-unreach-tx

> l | ue-unreach-retx

> l | ue-unreach-rx

> l | unk-msg-tx

> l | unk-msg-retx

> l | unk-msg-rx

> SGSN Schema

> l | redir-attach-rej-gprs-pna

> l | redir-attach-rej-comb-pna

> l | redir-peroidic-rau-pna

> l | redir-rau-gprs-intra-sgsn-rej-pna

> l | redir-rau-comb-intra-sgsn-rej-pna

> l | redir-rau-gprs-inter-sgsn-rej-pna

> l | redir-rau-comb-inter-sgsn-rej-pna

> l | redir-rau-gprs-inter-rat-pna

> l | redir-rau-comb-inter-rat-pna

> l | redir-rau-gprs-inter-serv-pna

> l | redir-rau-comb-inter-serv-pna

> l | redir-attach-rej-gprs-lana

> l | redir-attach-rej-comb-lana

> l | redir-peroidic-rau-lana

> l | redir-rau-gprs-intra-sgsn-rej-lana

> l | redir-rau-comb-intra-sgsn-rej-lana

> l | redir-rau-gprs-inter-sgsn-rej-lana

> l | redir-rau-comb-inter-sgsn-rej-lana

> l | redir-rau-gprs-inter-rat-lana

> l | redir-rau-comb-inter-rat-lana

> l | redir-rau-gprs-inter-serv-lana

> l | redir-rau-comb-inter-serv-lana

> l | redir-attach-rej-gprs-rna

> l | redir-attach-rej-comb-rna

> l | redir-peroidic-rau-rna

> l | redir-rau-gprs-intra-sgsn-rej-rna

> l | redir-rau-comb-intra-sgsn-rej-rna

> l | redir-rau-gprs-inter-sgsn-rej-rna

> l | redir-rau-comb-inter-sgsn-rej-rna

> l | redir-rau-gprs-inter-rat-rna

> l | redir-rau-comb-inter-rat-rna

> l | redir-rau-gprs-inter-serv-rna

> l | redir-rau-comb-inter-serv-rna

> l | redir-attach-rej-gprs-ngs

> l | redir-attach-rej-comb-ngs

> l | redir-peroidic-rau-ngs

> l | redir-rau-gprs-intra-sgsn-rej-ngs

> l | redir-rau-comb-intra-sgsn-rej-ngs

> l | redir-rau-gprs-inter-sgsn-rej-ngs

> l | redir-rau-comb-inter-sgsn-rej-ngs

> l | redir-rau-gprs-inter-rat-ngs

> l | redir-rau-comb-inter-rat-ngs

> l | redir-rau-gprs-inter-serv-ngs

> l | redir-rau-comb-inter-serv-ngs

> l | redir-attach-rej-gprs-cpcr

> l | redir-attach-rej-comb-cpcr

> l | redir-peroidic-rau-cpcr

> l | redir-rau-gprs-intra-sgsn-rej-cpcr

> l | redir-rau-comb-intra-sgsn-rej-cpcr

> l | redir-rau-gprs-inter-sgsn-rej-cpcr

> l | redir-rau-comb-inter-sgsn-rej-cpcr

> l | redir-rau-gprs-inter-rat-cpcr

> l | redir-rau-comb-inter-rat-cpcr

> l | redir-rau-gprs-inter-serv-cpcr

> l | redir-rau-comb-inter-serv-cpcr

> l | redir-attach-rej-gprs-ur

> l | redir-attach-rej-comb-ur

> l | redir-peroidic-rau-ur

> l | redir-rau-gprs-intra-sgsn-rej-ur

> l | redir-rau-comb-intra-sgsn-rej-ur

> l | redir-rau-gprs-inter-sgsn-rej-ur

> l | redir-rau-comb-inter-sgsn-rej-ur

> l | redir-rau-gprs-inter-rat-ur

> l | redir-rau-comb-inter-rat-ur

> l | redir-rau-gprs-inter-serv-ur

> l | redir-rau-comb-inter-serv-ur

> System Schema

> l | asnpc-cursess

> l | asnpc-curactive

> l | asnpc-ttlsetup

> l | asnpc-retriesexhaust

> l | asnpc-tidfail

> l | asnpc-luattempted

> l | asnpc-ludenied

> l | asnpc-lucomp

> l | asnpc-pagattempted

> l | asnpc-pagsucceeded

> l | asnpc-annoucetriggered

> l | cc-upd-titsutime

> l | cf-cat-backup-pkts-hit

> l | cf-cat-backup-pkts-block

> l | cf-cat-cdn-pkts-hit

> l | cf-cat-cdn-pkts-block

> l | cf-cat-photo-pkts-hit

> l | cf-cat-photo-pkts-block

> l | cf-cat-plag-pkts-hit

> l | cf-casngw-simple-ip-reanchored

> l | disc-reason-454

> l | disc-reason-455

> l | disc-reason-456

> l | disc-reason-457

> l | disc-reason-458

> l | disc-reason-459

> l | disc-reason-460

> l | disc-reason-461

> l | disc-reason-462

> l | disc-reason-463

> l | disc-reason-464

> l | disc-reason-465

> l | disc-reason-466

> l | disc-reason-467

> l | disc-reason-468

> l | disc-reason-469

> l | disc-reason-470

> l | disc-reason-471

> l | disc-reason-472

> l | disc-reason-473

> l | disc-reason-474

> l | disc-reason-475

> l | disc-reason-476

> l | disc-reason-477

> l | disc-reason-478

> l | disc-reason-479

> l | disc-reason-480

> l | disc-reason-481

> l | disc-reason-482

> l | disc-reason-483

> l | disc-reason-484

> l | disc-reason-485

> l | disc-reason-486

> l | disc-reason-487

> l | disc-reason-488

> l | disc-reason-489

> l | phsgw-cursess

> l | phsgw-cur-active-call

> l | phsgw-total-sess-setup

> l | phsgw-retriesexhaust

> l | phsgw-uplink-sfs

> l | phsgw-downlink-sfs

> l | phsgw-tidfail

> l | phsgw-handoffattempt

> l | phsgw-handoffdenied

> l | phsgw-handoffcomp

> l | phsgw-authsucc

> l | phsgw-authfailures

> l | phsgw-3partyauthsucc

> l | phsgw-3partyauthfailures

> l | phspc-cursess

> l | phspc-total-sess-setup

> l | phspc-retriesexhaust

> l | phspc-tidfail

> l | phspc-locupdate-attempt

> l | phspc-locupdate-denied

> l | phspc-locupdate-comp

> l | phspc-paging-attemptat-plag-pkts-block

> l | ipsecctrl-lte-template-reqs

> l | ipsecctrl-lte-template-unreg-reqs

> l | ipsecctrl-lte-map-reqs

> l | ipsecctrl-lte-map-est

> l | ipsecctrl-lte-map-del-reqs

> l | ipsecctrl-lte-map-failed

> l | ipsecctrl-lte-map-state-notif

> l | ipsecctrl-lte-ipsecmgr-death-notif

> l | ipsecctrl-lte-qos-maps

> Modified Bulk Statistics
> The following bulk statistics were modified in Release 12.0.
> None for this release.
> Obsoleted Bulk Statistics
> The following bulk statistics were obsoleted in Release 12.0.
> ECS Schema

> l | p2p-skype-voice-uplnk-bytes

> l | p2p-skype-voice-dwlnk-bytes

> l | p2p-skype-voice-uplnk-pkts

> l | p2p-skype-voice-dwlnk-pkts

> l | p2p-skype-non-voice-uplnk-bytes

> l | p2p-skype-non-voice-dwlnk-bytes

> l | p2p-skype-non-voice-uplnk-pkts

> l | p2p-skype-non-voice-dwlnk-pkts

> l | p2p-msn-voice-uplnk-bytes

> l | p2p-msn-voice-dwlnk-bytes

> l | p2p-msn-voice-uplnk-pkts

> l | p2p-msn-voice-dwlnk-pkts

> l | p2p-msn-non-voice-uplnk-bytes

> l | p2p-msn-non-voice-dwlnk-bytes

> l | p2p-msn-non-voice-uplnk-pkts

> l | p2p-msn-non-voice-dwlnk-pkts

> l | p2p-yahoo-voice-uplnk-bytes

> l | p2p-yahoo-voice-dwlnk-bytes

> l | p2p-yahoo-voice-uplnk-pkts

> l | p2p-yahoo-voice-dwlnk-pkts

> l | p2p-yahoo-non-voice-uplnk-bytes

> l | p2p-yahoo-non-voice-dwlnk-bytes

> l | p2p-yahoo-non-voice-uplnk-pkts

> l | p2p-yahoo-non-voice-dwlnk-pkts

> l | p2p-oscar-voice-uplnk-bytes

> l | p2p-oscar-voice-dwlnk-bytes

> l | p2p-oscar-voice-uplnk-pkts

> l | p2p-oscar-voice-dwlnk-pkts

> l | p2p-oscar-non-voice-uplnk-bytes

> l | p2p-oscar-non-voice-dwlnk-bytes

> l | p2p-oscar-non-voice-uplnk-pkts

> l | p2p-oscar-non-voice-dwlnk-pkts

> l | p2p-gtalk-voice-uplnk-bytes

> l | p2p-gtalk-voice-dwlnk-bytes

> l | p2p-gtalk-voice-uplnk-pkts

> l | p2p-gtalk-voice-dwlnk-pkts

> l | p2p-gtalk-non-voice-uplnk-bytes

> l | p2p-gtalk-non-voice-dwlnk-bytes

> l | p2p-gtalk-non-voice-uplnk-pkts

> l | p2p-gtalk-non-voice-dwlnk-pkts

> MME Schema

> l | out-rau-ho-4gto3g-s3-attempted

> l | out-rau-ho-4gto3g-s3-success

> l | out-rau-ho-4gto3g-s3-failures

> l | in-tau-ho-2gto4g-gngp-attempted

> l | in-tau-ho-2gto4g-gngp-success

> l | in-tau-ho-2gto4g-gngp-failures

> l | out-rau-ho-4gto2g-gngp-attempted

> l | out-rau-ho-4gto2g-gngp-success

> l | out-rau-ho-4gto2g-gngp-failures

> System Schema

> l | cf-dyn-rateblock

> l | cf-cat-adv-pkts-hit

> l | cf-cat-adv-pkts-block

> l | cf-cat-auct-pkts-hit

> l | cf-cat-auct-pkts-block

> l | cf-cat-clean-pkts-hit

> l | cf-cat-clean-pkts-block

> l | cf-cat-cporn-pkts-hit

> l | cf-cat-cporn-pkts-block

> l | cf-cat-esrb-pkts-hit

> l | cf-cat-esrb-pkts-block

> l | cf-cat-p2p-pkts-hit

> l | cf-cat-p2p-pkts-block

> l | cf-cat-radio-pkts-hit

> l | cf-cat-radio-pkts-block

> l | cf-cat-sftwre-pkts-hit

> l | cf-cat-sftwre-pkts-block

> l | cf-cat-spywre-pkts-hit

> l | cf-cat-spywre-pkts-block

> l | cf-cat-susp-pkts-hit

> l | cf-cat-susp-pkts-block

> Bulk Statistic Enhancements in Release 12.1
> This section lists bulk statistic additions and changes in Release 12.1.

> l | New Bulk Statistics

> l | Modified Bulk Statistics

> l | Obsoleted Bulk Statistics

> New Bulk Statistics
> Following new commands added for IPCF support in release 12.1:
> Bulkstats Configuration Mode

> l | pcc-af schema

> l | pcc-policy schema

> l | pcc-sp-endpt schema

> l | pcc-service schema

> pcc-af Schema
> This is a new schema provided for PCC solution on IPCF node in Release 12.1.

> l | vpnname

> l | vpnid

> l | servname

> l | servid

> l | total-rx-inbound-msgs

> l | total-rx-outbound-msgs

> l | total-rx-aar-rcvd

> l | total-rx-aar-accept-sent

> l | total-rx-str-rcvd

> l | total-rx-srt-accept-sent

> l | total-rx-rar-sent

> l | total-rx-raa-rcvd

> l | total-rx-asr-sent

> l | total-rx-asa-rcvd

> pcc-policy Schema
> This is a new schema provided for PCC solution on IPCF node in Release 12.1.

> l | vpnname

> l | vpnid

> l | servname

> l | servid

> l | total-gx-inbound-msgs

> l | total-gx-outbound-msgs

> l | total-gx-ccr-rcvd

> l | total-gx-ccr-rej-sent

> l | total-gx-cca-accept-sent

> l | total-gx-ccri-rcvd

> l | total-gx-ccai-rej-sent

> l | total-gx-ccai-accept-sent

> l | total-gx-ccru-rcvd

> l | total-gx-ccru-rej-sent

> l | total-gx-ccru-accept-sent

> l | total-gx-ccrt-rcvd

> l | total-gx-ccrt-rej-sent

> l | total-gx-ccrt-accept-sent

> l | total-gx-unknown-ccr-rcvd

> l | total-gx-unknown-ccr-rej

> l | total-gx-rar-sent

> l | total-gx-raa-rcvd

> l | total-gx-rar-timeouts

> l | total-gx-raa-parse-success

> l | total-gx-raa-parse-fail

> l | total-gx-cca-sent

> l | total-gx-ccai-sent

> l | total-gx-ccau-sent

> l | total-gx-ccat-sent

> l | total-gx-rar-sess-release

> l | total-gx-raa-success-code

> l | total-gx-raa-failure-code

> pcc-service Schema
> This is a new schema provided for PCC solution on IPCF node in Release 12.1.

> l | vpnname

> l | vpnid

> l | servname

> l | servid

> l | total-gx-processed

> l | total-gy-processed

> l | total-spr-processed

> l | total-unknown-req

> l | total-pur-updates

> l | total-snr-requests

> l | total-pnr-requests

> l | total-profile-match-hits

> l | total-profile-match-miss

> l | total-quota-reports

> l | total-unknown-rt-req

> pcc-sp-endpt Schema
> This is a new schema provided for PCC solution on IPCF node in Release 12.1.

> l | vpnname

> l | vpnid

> l | endpt-name

> l | req-open

> l | req-close

> l | req-update-profile

> l | req-update-profile-answer

> l | req-user-data-req

> l | req-user-data-answer

> l | req-checkpoints

> l | req-recoveries

> l | req-user-data-query

> l | req-push-notif-req

> l | req-push-notif-answer

> l | req-subscr-notif-req

> l | req-subscr-notif-answer

> l | success-open

> l | success-close

> l | success-update-profile

> l | success-update-profile-answer

> l | success-user-data-req

> l | success-user-data-answer

> l | success-checkpoints

> l | success-recoveries

> l | success-user-data-query

> l | success-push-notif-req

> l | success-push-notif-answer

> l | success-subscr-notif-req

> l | success-subscr-notif-answer

> l | error-open

> l | error-close

> l | error-update-profile

> l | error-update-profile-answer

> l | error-user-data-req

> l | error-user-data-answer

> l | error-checkpoints

> l | error-recoveries

> l | error-user-data-query

> l | error-push-notif-req

> l | error-push-notif-answer

> l | error-subscr-notif-req

> l | error-subscr-notif-answer

> Modified Bulk Statistics
> The following bulk statistics were modified in Release 12.1.
> None for this release.
> Obsoleted Bulk Statistics
> The following bulk statistics were obsoleted in Release 12.1.
> None for this release.
> Bulk Statistic Enhancements in Release 12.2
> This section lists bulk statistic additions and changes in Release 12.2.

> l | New Bulk Statistics

> l | Modified Bulk Statistics

> l | Obsoleted Bulk Statistics

> New Bulk Statistics
> Support for the following bulk statistics were added in Release 12.2.
> Context Schema

> l | nat-total-flows

> l | nat44-total-flows

> l | nat64-total-flows

> l | bypass-nat-total-flows

> l | bypass-nat-ipv4-total-flows

> l | bypass-nat-ipv6-total-flows

> CSCF Schema

> l | srtp-sent

> l | srtp-recv

> l | srtcp-sent

> l | srtcp-recv

> ECS Schema

> l | ecs-dns-learnt-ipv4-entries

> l | ecs-dns-flushed-ipv4-entries

> l | ecs-dns-replaced-ipv4-entries

> l | ecs-dns-overflown-ipv4-entries

> l | ecs-dns-learnt-ipv6-entries

> l | ecs-dns-flushed-ipv6-entries

> l | ecs-dns-replaced-ipv6-entries

> l | ecs-dns-overflown-ipv6-entries

> l | ip-charge-uplk-bytes

> l | ip-charge-dwnlk-bytes

> l | ip-charge-uplk-pkts

> l | ip-charge-dwnlk-pkts

> l | video-opt-total-transrated

> l | video-opt-transrated-sh263

> l | video-opt-transrated-h264

> l | video-opt-failed-sh263

> l | video-opt-failed-h264

> l | video-opt-total-input-bytes

> l | video-opt-total-input-bytes-sh263

> l | video-opt-total-input-bytes-h264

> l | video-opt-total-output-bytes

> l | video-opt-total-output-bytes-sh263

> l | video-opt-total-output-bytes-h264

> l | video-opt-avg-input-bitrate

> l | video-opt-avg-input-bitrate-sh263

> l | video-opt-avg-input-bitrate-h264

> l | video-opt-avg-output-bitrate

> l | video-opt-avg-output-bitrate-sh263

> l | video-opt-avg-output-bitrate-h264

> l | video-opt-avg-rate-reduction

> l | video-opt-avg-rate-reduction-sh263

> l | video-opt-avg-rate-reduction-h264

> l | tcpprxy-usrtotsocksopn

> l | tcpprxy-inettotsocksopn

> l | tcpprxy-usrsockopnfail

> l | tcpprxy-inetsockopnfail

> l | tcpprxy-usrtotconnattmpt

> l | tcpprxy-inettotconnattmpt

> l | tcpprxy-usraccsucc

> l | tcpprxy-inetaccsucc

> l | tcpprxy-usraccfail

> l | tcpprxy-inetaccfail

> l | tcpprxy-usrcuropnsocks

> l | tcpprxy-inetcuropnsocks

> l | tcpprxy-usrcuralloctcpvect

> l | tcpprxy-inetcuralloctcpvect

> l | tcpprxy-usriptotpktsrcvd

> l | tcpprxy-inetiptotpktsrcvd

> l | tcpprxy-usriphdrerr

> l | tcpprxy-inetiphdrerr

> l | tcpprxy-usripunknownproto

> l | tcpprxy-inetipunknownproto

> l | tcpprxy-usripincomdiscpkts

> l | tcpprxy-inetipincomdiscpkts

> l | tcpprxy-usrtcpincomseg

> l | tcpprxy-inettcpincomseg

> l | tcpprxy-usrtcpincomerrseg

> l | tcpprxy-inettcpincomerrseg

> l | tcpprxy-usrtcpincomretransseg

> l | tcpprxy-inettcpincomretransseg

> l | tcpprxy-usrtcpoutgodataseg

> l | tcpprxy-inettcpoutgodataseg

> l | tcpprxy-usrtcpoutgorstseg

> l | tcpprxy-inettcpoutgorstseg

> l | tcpprxy-usrtcpoutgoretransseg

> l | tcpprxy-inettcpoutgoretransseg

> l | tcpprxy-usrtcpconnfail

> l | tcpprxy-inettcpconnfail

> l | tcpprxy-usrtcprstineststate

> l | tcpprxy-inettcprstineststate

> l | tcpprxy-usrtcpcurestconn

> l | tcpprxy-inettcpcurestconn

> l | tcpprxy-totprxyflows

> l | tcpprxy-currprxyflows

> l | tcpprxy-curactopnonusr

> l | tcpprxy-curactopnoninet

> l | tcpprxy-curpassopnonusr

> l | tcpprxy-curpassopnoninet

> l | tcpprxy-curestonboth

> l | tcpprxy-totpassopnsuccusr

> l | tcpprxy-totactopnsuccusr

> l | tcpprxy-totpassopnsuccinet

> l | tcpprxy-totactopnsuccinet

> l | tcpprxy-flowlimit

> l | tcpprxy-backloglimit

> l | tcpprxy-usrsocklimit

> l | tcpprxy-inetsocklimit

> l | tcpprxy-memthresholdlimit

> l | tcpprxy-incompactopn

> l | tcpprxy-incompassopn

> l | tcpprxy-usrsocknoerr

> l | tcpprxy-usrsocknopermissn

> l | tcpprxy-usrsocknomem

> l | tcpprxy-usrsocktoomanysocks

> l | tcpprxy-usrsockothers

> l | tcpprxy-inetsocknoerr

> l | tcpprxy-inetsocknopermissn

> l | tcpprxy-inetsocknomem

> l | tcpprxy-inetsocktoomanysock

> l | tcpprxy-inetsockothers

> l | tcpprxy-usrsockerropwouldblk

> l | tcpprxy-inetsockerropwouldblk

> l | tcpprxy-usrsockerropinprog

> l | tcpprxy-inetsockerropinprog

> l | tcpprxy-usrsockerrconnrstbypeer

> l | tcpprxy-inetsockerrconnrstbypeer

> l | tcpprxy-usrsockerrsendaftershtdwn

> l | tcpprxy-inetsockerrsendaftershtdwn

> l | tcpprxy-usrsockerroptmout

> l | tcpprxy-inetsockerroptmout

> l | tcpprxy-usrsockerrconnabort

> l | tcpprxy-inetsockerrconnabort

> l | tcpprxy-usrsockerrconnref

> l | tcpprxy-inetsockerrconnref

> l | tcpprxy-usrsockerrtoomanysocks

> l | tcpprxy-inetsockerrtoomanysocks

> l | tcpprxy-usrsockerrothers

> l | tcpprxy-inetsockerrothers

> l | tcpprxy-sockmigflowsinit

> l | tcpprxy-sockmigflowsmigattmpts

> l | tcpprxy-sockmigflowssucc

> l | tcpprxy-sockmigmemallocfail

> l | tcpprxy-sockmigpermissndenied

> l | tcpprxy-sockmigpossibtcpstatechng

> l | tcpprxy-sockmigpkttrimfail

> l | tcpprxy-sockmigothers

> l | tcpprxy-facacsmemlimit

> l | tcpprxy-facprxymemlimit

> l | tcpprxy-facflowspersublimit

> l | tcpprxy-factotprxyflowlimit

> l | video-readdress-get-req-redirected

> l | video-readdress-post-req-redirected

> l | video-readdress-other-req-redirected

> l | video-readdress-res-redirected

> l | video-readdress-req-with-xheader-inserted

> l | video-readdress-connect-failed-to-video-server

> l | video-readdress-upl-bytes-redirected

> l | video-readdress-upl-pkts-redirected

> l | video-readdress-dnl-bytes-redirected

> l | video-readdress-dnl-pkts-redirected

> l | p2p-meebo-voice-duration

> l | p2p-meebo-video-uplnk-bytes

> l | p2p-meebo-video-dwlnk-bytes

> l | p2p-meebo-video-uplnk-pkts

> l | p2p-meebo-video-dwlnk-pkts

> l | p2p-meebo-audio-uplnk-bytes

> l | p2p-meebo-audio-dwlnk-bytes

> l | p2p-meebo-audio-uplnk-pkts

> l | p2p-meebo-audio-dwlnk-pkts

> l | p2p-meebo-unclassified-uplnk-bytes

> l | p2p-meebo-unclassified-dwlnk-bytes

> l | p2p-meebo-unclassified-uplnk-pkts

> l | p2p-meebo-unclassified-dwlnk-pkts

> l | p2p-antsp2p-uplnk-bytes

> l | p2p-antsp2p-dwlnk-bytes

> l | p2p-antsp2p-uplnk-pkts

> l | p2p-antsp2p-dwlnk-pkts

> l | p2p-imo-uplnk-bytes

> l | p2p-imo-dwlnk-bytes

> l | p2p-imo-uplnk-pkts

> l | p2p-imo-dwlnk-pkts

> l | p2p-netmotion-uplnk-bytes

> l | p2p-netmotion-dwlnk-bytes

> l | p2p-netmotion-uplnk-pkts

> l | p2p-netmotion-dwlnk-pkts

> l | p2p-ogg-uplnk-bytes

> l | p2p-ogg-dwlnk-bytes

> l | p2p-ogg-uplnk-pkts

> l | p2p-ogg-dwlnk-pkts

> l | p2p-openvpn-uplnk-bytes

> l | p2p-openvpn-dwlnk-bytes

> l | p2p-openvpn-uplnk-pkts

> l | p2p-openvpn-dwlnk-pkts

> l | p2p-quicktime-uplnk-bytes

> l | p2p-quicktime-dwlnk-bytes

> l | p2p-quicktime-uplnk-pkts

> l | p2p-quicktime-dwlnk-pkts

> l | p2p-spotify-uplnk-bytes

> l | p2p-spotify-dwlnk-bytes

> l | p2p-spotify-uplnk-pkts

> l | p2p-spotify-dwlnk-pkts

> l | p2p-tango-uplnk-bytes

> l | p2p-tango-dwlnk-bytes

> l | p2p-tango-uplnk-pkts

> l | p2p-tango-dwlnk-pkts

> l | p2p-ultrabac-uplnk-bytes

> l | p2p-ultrabac-dwlnk-bytes

> l | p2p-ultrabac-uplnk-pkts

> l | p2p-ultrabac-dwlnk-pkts

> l | p2p-usenet-uplnk-bytes

> l | p2p-usenet-dwlnk-bytes

> l | p2p-usenet-uplnk-pkts

> l | p2p-usenet-dwlnk-pkts

> l | p2p-tunnelvoice-uplnk-bytes

> l | p2p-tunnelvoice-dwlnk-bytes

> l | p2p-tunnelvoice-uplnk-pkts

> l | p2p-tunnelvoice-dwlnk-pkts

> l | p2p-scydo-uplnk-bytes

> l | p2p-scydo-dwlnk-bytes

> l | p2p-scydo-uplnk-pkts

> l | p2p-scydo-dwlnk-pkts

> l | p2p-whatsapp-uplnk-bytes

> l | p2p-whatsapp-dwlnk-bytes

> l | p2p-whatsapp-uplnk-pkts

> l | p2p-whatsapp-dwlnk-pkts

> l | p2p-mypeople-uplnk-bytes

> l | p2p-mypeople-dwlnk-bytes

> l | p2p-mypeople-uplnk-pkts

> l | p2p-mypeople-dwlnk-pkts

> l | p2p-rdt-uplnk-bytes

> l | p2p-rdt-dwlnk-bytes

> l | p2p-rdt-uplnk-pkts

> l | p2p-rdt-dwlnk-pkts

> eGTP-C Schema

> l | tun-sent-changenotfreq

> l | tun-sent-retranschangenotfreq

> l | tun-recv-changenotfreq

> l | tun-recv-retranschangenotfreq

> l | tun-sent-changenotfresp

> l | tun-sent-changenotfrespaccept

> l | tun-sent-changenotfrespdenied

> l | tun-sent-retranschangenotfresp

> l | tun-recv-changenotfresp

> l | tun-recv-changenotfrespaccept

> l | tun-recv-changenotfrespdenied

> l | tun-recv-creinddatafwdngrspaccept

> l | mobility-sent-ranInforelay

> l | mobility-recv-ranInforelay

> l | mobility-sent-configxfertun

> l | mobility-recv-configxfertun

> l | gtpv1path-recv-echoresp

> HSGW Schema

> l | sessstat-totcur-pdn-ipv4

> l | sessstat-totcur-pdn-ipv6

> l | sessstat-totcur-pdn-ipv4v6

> l | ipv4-pdn-to-user-pkt

> l | ipv4-pdn-to-user-byte

> l | ipv4-pdn-from-user-pkt

> l | ipv4-pdn-from-user-byte

> l | ipv6-pdn-to-user-pkt

> l | ipv6-pdn-to-user-byte

> l | ipv6-pdn-from-user-pkt

> l | ipv6-pdn-from-user-byte

> l | ipv4v6-pdn-ipv4-to-user-pkt

> l | ipv4v6-pdn-ipv4-to-user-byte

> l | ipv4v6-pdn-ipv4-from-user-pkt

> l | ipv4v6-pdn-ipv4-from-user-byte

> l | ipv4v6-pdn-ipv6-to-user-pkt

> l | ipv4v6-pdn-ipv6-to-user-byte

> l | ipv4v6-pdn-ipv6-from-user-pkt

> l | ipv4v6-pdn-ipv6-from-user-byte

> MME Schema

> l | sess-ecm-connect

> l | ecmevent-s1rel-loadbalance

> l | s1ap-transdata-cfgupd

> l | s1ap-transdata-cfgtfr

> l | s1ap-recdata-cfgupdfail

> l | s1ap-recdata-cfgupdack

> l | s1ap-recdata-enbcfgtfr

> l | s1ap-enodeb-assoc

> l | s1ap-err-unknownmme-ues1apid

> l | s1ap-err-unknownenb-ues1apid

> l | s1ap-err-unknownpair-ues1apid

> l | s1ap-err-tfr-synerr

> l | s1ap-err-semanticerr

> l | s1ap-err-msgnotcompatible

> l | s1ap-err-aserej

> l | s1ap-err-aseignore-notify

> l | s1ap-err-asefalsely-constrmsg

> l | paging-tai-list-success

> l | epsattach-emergency-attempted

> l | epsattach-emergency-success

> l | epsattach-emergency-failures

> l | emm-msgtx-imei-not-accept

> l | emm-msgtx-roaming-restrict-ta

> l | emm-msgtx-plmn-not-allow

> l | emm-msgtx-no-suitable-cell-ta

> l | emm-msgtx-ta-not-allow

> l | emm-msgtx-tau-imei-not-accept

> l | emm-msgtx-tau-roaming-restrict-ta

> l | emm-msgtx-tau-plmn-not-allow

> l | emm-msgtx-tau-no-suitable-cell-ta

> l | emm-msgtx-tau-ta-not-allow

> l | emm-msgtx-tau-cs-service-notif

> l | emm-msgrx-identity-resp

> l | emm-msgrx-ext-service-req

> l | esm-msgtx-brralloc-rej-insuff-resource

> l | esm-msgtx-brrmod-rej-insuff-resource

> l | esm-msgrx-deactivate-brr-accept

> l | out-rau-ho-4gto3g2g-gngp-attempted

> l | out-rau-ho-4gto3g2g-gngp-success

> l | out-rau-ho-4gto3g2g-gngp-failures

> l | in-tau-ho-2g3gto4g-gngp-attempted

> l | in-tau-ho-2g3gto4g-gngp-success

> l | in-tau-ho-2g3gto4g-gngp-failures

> l | out-rau-ho-4gto3g2g-s3-attempted

> l | out-rau-ho-4gto3g2g-s3-success

> l | out-rau-ho-4gto3g2g-s3-failures

> l | out-s1-ho-4gto3g-s3-attempted

> l | out-s1-ho-4gto3g-s3-success

> l | out-s1-ho-4gto3g-s3-failures

> l | in-tau-ho-2g3gto4g-s3-attempted

> l | in-tau-ho-2g3gto4g-s3-success

> l | in-tau-ho-2g3gto4g-s3-failures

> l | in-s1-ho-3gto4g-s3-attempted

> l | in-s1-ho-3gto4g-s3-success

> l | in-s1-ho-3gto4g-s3-failures

> l | out-s1-ho-4gto2g-s3-attempted

> l | out-s1-ho-4gto2g-s3-success

> l | out-s1-ho-4gto2g-s3-failures

> l | in-s1-ho-2gto4g-s3-attempted

> l | in-s1-ho-2gto4g-s3-success

> l | in-s1-ho-2gto4g-s3-failures

> l | s1-ho-4gto3g-cs-nodtm-sv-attempted

> l | s1-ho-4gto3g-cs-nodtm-sv-success

> l | s1-ho-4gto3g-cs-nodtm-sv-failures

> l | s1-ho-4gto3g-cs-sv-attempted

> l | s1-ho-4gto3g-cs-sv-success

> l | s1-ho-4gto3g-cs-sv-failures

> l | s1-ho-4gto3g-csps-sv-attempted

> l | s1-ho-4gto3g-csps-sv-success

> l | s1-ho-4gto3g-csps-sv-failures

> l | pdn-all

> l | pdn-connected

> l | pdn-idle

> l | pdn-emergency-all

> l | pdn-emergency-connected

> l | pdn-emergency-idle

> l | brr-all

> l | brr-connected

> l | brr-idle

> l | sess-call-all

> l | sess-call-connected

> l | sess-call-idle

> l | sess-emergency-call-all

> l | sess-emergency-call-connected

> l | sess-emergency-call-idle

> l | sess-unauth-call-all

> l | sess-unauth-call-connected

> l | sess-unauth-call-idle

> NAT-Realm Schema

> l | nat-rlm-bytes-nat44-tx

> l | nat-rlm-bytes-nat64-tx

> l | nat-rlm-nat44-flows

> l | nat-rlm-nat64-flows

> l | nat-rlm-ip-denied-nat44

> l | nat-rlm-ip-denied-nat64

> l | nat-rlm-port-denied-nat44

> l | nat-rlm-port-denied-nat64

> PGW Schema

> l | sessstat-bearact-emergency-def

> l | sessstat-bearact-emergency-auth-imsi-def

> l | sessstat-bearact-emergency-unauth-imsi-def

> l | sessstat-bearact-emergency-only-imei-def

> l | sessstat-bearact-emergency-ded

> l | sessstat-bearact-emergency-auth-imsi-ded

> l | sessstat-bearact-emergency-unauth-imsi-ded

> l | sessstat-bearact-emergency-only-imei-ded

> l | sessstat-bearsetup-emergency-def

> l | sessstat-bearsetup-emergency-auth-imsi-def

> l | sessstat-bearsetup-emergency-unauth-imsi-def

> l | sessstat-bearsetup-emergency-only-imei-def

> l | sessstat-bearsetup-emergency-ded

> l | sessstat-bearsetup-emergency-auth-imsi-ded

> l | sessstat-bearsetup-emergency-unauth-imsi-ded

> l | sessstat-bearsetup-emergency-only-imei-ded

> l | sessstat-bearrej-emergency-def

> l | sessstat-bearrej-emergency-ded

> l | ipv4-pdn-to-user-pkt

> l | ipv4-pdn-to-user-byte

> l | ipv4-pdn-from-user-pkt

> l | ipv4-pdn-from-user-byte

> l | ipv6-pdn-to-user-pkt

> l | ipv6-pdn-to-user-byte

> l | ipv6-pdn-from-user-pkt

> l | ipv6-pdn-from-user-byte

> l | ipv4v6-pdn-ipv4-to-user-pkt

> l | ipv4v6-pdn-ipv4-to-user-byte

> l | ipv4v6-pdn-ipv4-from-user-pkt

> l | ipv4v6-pdn-ipv4-from-user-byte

> l | ipv4v6-pdn-ipv6-to-user-pkt

> l | ipv4v6-pdn-ipv6-to-user-byte

> l | ipv4v6-pdn-ipv6-from-user-pkt

> l | ipv4v6-pdn-ipv6-from-user-byte

> SGW Schema

> l | ipv4-pdn-to-user-pkt

> l | ipv4-pdn-to-user-byte

> l | ipv4-pdn-from-user-pkt

> l | ipv4-pdn-from-user-byte

> l | ipv6-pdn-to-user-pkt

> l | ipv6-pdn-to-user-byte

> l | ipv6-pdn-from-user-pkt

> l | ipv6-pdn-from-user-byte

> l | ipv4v6-pdn-ipv4-to-user-pkt

> l | ipv4v6-pdn-ipv4-to-user-byte

> l | ipv4v6-pdn-ipv4-from-user-pkt

> l | ipv4v6-pdn-ipv4-from-user-byte

> l | ipv4v6-pdn-ipv6-to-user-pkt

> l | ipv4v6-pdn-ipv6-to-user-byte

> l | ipv4v6-pdn-ipv6-from-user-pkt

> l | ipv4v6-pdn-ipv6-from-user-byte

> System Schema

> l | sess-txpackets-umts

> l | sess-txbytes-umts

> l | sess-rxpackets-umts

> l | sess-rxbytes-umts

> l | sess-txpackets-gprs

> l | sess-txbytes-gprs

> l | sess-rxpackets-gprs

> l | sess-rxbytes-gprs

> l | sess-txpackets-lte

> l | sess-txbytes-lte

> l | sess-rxpackets-lte

> l | sess-rxbytes-lte

> l | sess-txpackets-ehrpd

> l | sess-txbytes-ehrpd

> l | sess-rxpackets-ehrpd

> l | sess-rxbytes-ehrpd

> l | sess-total-sessions-1xrtt

> l | sess-num-calls-arrived-1xrtt

> l | sess-num-calls-disconnected-1xrtt

> l | sess-total-sessions-evdorev0

> l | sess-num-calls-arrived-evdorev0

> l | sess-num-calls-disconnected-evdorev0

> l | sess-total-sessions-evdoreva

> l | sess-num-calls-arrived-evdoreva

> l | sess-num-calls-disconnected-evdoreva

> l | sess-total-sessions-evdora

> l | sess-num-calls-arrived-evdora

> l | sess-num-calls-disconnected-evdora

> l | sess-total-sessions-umts

> l | sess-num-calls-arrived-umts

> l | sess-ttlconnected-umts

> l | sess-num-calls-disconnected-umts

> l | sess-total-sessions-gprs

> l | sess-num-calls-arrived-gprs

> l | sess-ttlconnected-gprs

> l | sess-num-calls-disconnected-gprs

> l | sess-total-sessions-ehrpd

> l | sess-num-calls-arrived-ehrpd

> l | sess-ttlconnected-ehrpd

> l | sess-num-calls-disconnected-ehrpd

> l | sess-total-sessions-lte

> l | sess-num-calls-arrived-lte

> l | sess-ttlconnected-lte

> l | sess-num-calls-disconnected-lte

> l | ikev2-csa-delmultspisnt

> l | ikev2-csa-delmultspircv

> l | cca-init-2001-rc

> l | cca-init-5003-rc

> l | cca-init-4011-rc

> l | cca-init-4012-rc

> l | cca-updt-2001-rc

> l | cca-updt-5003-rc

> l | cca-updt-4011-rc

> l | cca-updt-4012-rc

> l | fail-action-term

> l | fail-action-contd

> l | offline-active-sess

> l | disc-reason-490

> l | disc-reason-491

> l | disc-reason-492

> l | disc-reason-493

> l | disc-reason-494

> l | disc-reason-495

> l | disc-reason-496

> l | disc-reason-497

> l | disc-reason-498

> l | disc-reason-499

> l | disc-reason-500

> l | disc-reason-501

> l | disc-reason-502

> l | disc-reason-503

> l | disc-reason-504

> l | disc-reason-505

> l | disc-reason-506

> l | disc-reason-507

> l | disc-reason-508

> l | disc-reason-509

> l | disc-reason-510

> Modified Bulk Statistics
> The following bulk statistics were modified in Release 12.2.
> Card Schema

> l | All card statistics except CPU names now show “Type: Gauge”.

> GTPP Schema

> l | aaa-acct-arch (type = gauge)

> l | SGSN-change-limit

> The above statistic was changed to the following:

> l | Serving-Node-change-limit

> IMSA Schema

> l | dpca-cursess (type = gauge)

> PGW Schema

> l | essstat-bearmodfail-uesyntft

> The above statistic was changed to the following:

> l | sessstat-bearmodfail-uesyntft

> Port Schema

> l | util-rx-curr (type = gauge)

> l | util-tx-curr (type = gauge)

> l | util-rx-5min (type = gauge)

> l | util-tx-5min (type = gauge)

> l | util-rx-15min (type = gauge)

> l | util-tx-15min (type = gauge)

> SGW Schema

> l | sessstat-pdnsetuptype-ipv4

> l | sessstat-pdnsetuptype-ipv6

> l | sessstat-pdnsetuptype-ipv4v6

> The statistics above were changed to the following (in order):

> l | sessstat-totcur-pdn-ipv4

> l | sessstat-totcur-pdn-ipv6

> l | sessstat-totcur-pdn-ipv4v6

> System Schema

> l | sess-ttlconnected (type = gauge)

> l | sess-curttlcalls (type = gauge)

> l | sess-cursipconn (type = gauge)

> l | sess-curmipconn (type = gauge)

> l | sess-curpmipconn (type = gauge)

> l | sess-curhaipsecconn (type = gauge)

> l | sess-ipsg-cur-archive-call (type = gauge)

> l | ipsg-total-archive-serv (type = gauge)

> l | sess-curnonanchorconn (type = gauge)

> l | flow-curdynamic (type = gauge)

> l | ssl-cachetotalsess (type = gauge)

> l | ggsn-cursgsnact (type = gauge)

> l | cf-cursub (type = gauge)

> l | disc-reason-489

> l | disc-reason-490

> l | disc-reason-491

> l | disc-reason-499

> l | disc-reason-500

> Obsoleted Bulk Statistics
> The following bulk statistics were obsoleted in Release 12.2.
> eGTP-C Schema

> l | sess-cur

> l | tun-recv-upduplanereq

> l | tun-recv-retransupduplanereq

> l | tun-sent-upduplaneresp

> l | tun-sent-upduplanerespaccept

> l | tun-sent-upduplanerespdenied

> l | tun-sent-deactbear

> l | tun-recv-deactbear

> l | tun-sent-deactbearfail

> l | tun-recv-deactbearfail

> l | gtpv1tun-sent-gpdu

> l | gtpv1tun-recv-gpdu

> l | gtpv1tun-txoctet

> l | gtpv1tun-rxoctet

> l | gtpv1tun-sent-gtpuerror

> l | gtpv1tun-recv-gtpuerror

> l | gtpv1tun-sent-endmarker

> l | gtpv1path-sent-hdrnotif

> l | gtpv1path-recv-hdrnotif

> MME Schema

> l | emmevent-assoc-attempt

> l | emmevent-assoc-success

> l | emmevent-assoc-failure

> l | emmevent-associmsi-attempt

> l | emmevent-associmsi-success

> l | emmevent-associmsi-failure

> l | emmevent-assoclocguti-attempt

> l | emmevent-assoclocguti-success

> l | emmevent-assoclocguti-failure

> l | emmevent-assocnonlocguti-attempt

> l | emmevent-assocnonlocguti-success

> l | emmevent-assocnonlocguti-failure

> l | emmevent-tau-attempt

> l | emmevent-tau-success

> l | emmevent-tau-failure

> l | emmevent-detach-attempt

> l | emmevent-detach-success

> l | emmevent-detach-failure

> l | ecmevent-lastenb-success

> l | ecmevent-lasttai-success

> l | ecmevent-tailist-success

> l | ecmevent-paging-attempt

> l | ecmevent-paging-success

> l | ecmevent-paging-failure

> l | esmevent-pdndiscon-attempt

> l | esmevent-pdndiscon-success

> l | esmevent-pdndiscon-failure

> l | esmevent-dedbearact-attempt

> l | esmevent-dedbearact-success

> l | esmevent-dedbearact-failure

> l | esmevent-beardeact-attempt

> l | esmevent-beardeact-success

> l | esmevent-beardeact-failure

> l | esmctrlmsg-recv-cleartext

> l | esmctrlmsg-recv-integrity

> l | esmctrlmsg-recv-cipher

> l | esmctrlmsg-recv-accept

> l | esmctrlmsg-recv-discard

> l | esmctrlmsg-recv-denied

> l | esmctrlmsg-recv-deocdefail

> l | emmevent-tauattach-success

> l | emmevent-tauattach-failure

> l | emmevent-outrauho4g3g-success

> l | emmevent-outrauho4g3g-failure

> l | emmevent-outs1ho4g3g-success

> l | emmevent-outs1ho4g3g-failure

> l | emmevent-intauho3g4g-success

> l | emmevent-intauho3g4g-failure

> l | emmevent-ins1ho3g4g-success

> l | emmevent-ins1ho3g4g-failure

> l | emm-msgtx-imsi-detach

> l | emm-msgtx-tau-esm-failure

> l | esm-msgtx-brralloc-rej-pgw-rej

> l | esm-msgrx-discarded

> l | esm-msgrx-decode-failures

> l | out-rau-ho-4gto3g-gngp-attempted

> l | out-rau-ho-4gto3g-gngp-success

> l | out-rau-ho-4gto3g-gngp-failures

> l | in-tau-ho-2gto4g-gngp-attempted

> l | in-tau-ho-2gto4g-gngp-success

> l | in-tau-ho-2gto4g-gngp-failures

> l | in-tau-ho-3gto4g-gngp-attempted

> l | in-tau-ho-3gto4g-gngp-success

> l | in-tau-ho-3gto4g-gngp-failures

> l | out-rau-ho-4gto2g-gngp-attempted

> l | out-rau-ho-4gto2g-gngp-success

> l | out-rau-ho-4gto2g-gngp-failures

> l | out-rau-ho-4gto3g-s3-attempted

> l | out-rau-ho-4gto3g-s3-success

> l | out-rau-ho-4gto3g-s3-failures

> l | tot-pdn-current

> l | tot-pdn-max

> l | connected-pdn-current

> l | connected-pdn-max

> l | idle-pdn-current

> l | idle-pdn-max

> l | tot-brr-current

> l | tot-brr-max

> l | connected-brr-current

> l | connected-brr-max

> l | idle-brr-current

> l | idle-brr-max

> Web Element Manager Path
> Click Accounting | Bulk Statistics Configuration.
> CDR Enhancements
> This section lists changes to GTPP dictionaries in Release 12.x.
> CDR Changes in Release 12.0
> This section lists GTPP dictionary changes in Release 12.0.
> Length of charging rulebase-name in LOSDVs of eG-CDRs/P-GW-CDRs - Behavior Change
> This change applies to all eG-CDR/PGW-CDR dictionaries.
> The maximum character length of Charging Rulebase Name field in LOSDVs of eG-CDRs and P-GW-CDRs is now configurable. This change is now available in 12.0 and later releases.
> In earlier releases, in case of Custom5 or Custom40 dictionaries, the rulebase name used to get trimmed to 16 characters. In other dictionaries the complete rulebase name used to appear in the LOSDVs.
> A new CLI command now enables to configure maximum length of the rulebase name between 1 through 63 characters. If configured as 0 (zero), the rulebase name is not trimmed. This new CLI command is available at the context and GTPP group levels.
> For more information, refer to the “gtpp egcdr rulebase-max-length” command in the Context Configuration Mode Commands and GTPP Server Group Configuration Mode Commands chapters of the Command Line Interface Reference.
> qoSInformationNeg Field in all LOSDV - Behavior Change
> This behavior change applies to the following ASN-encoded eG-CDR dictionaries:

> l | custom5

> l | custom6

> l | custom7

> l | custom8

> l | custom9

> l | custom12

> l | custom14

> l | custom15

> l | custom17

> l | custom19

> l | custom20

> l | custom22

> l | custom30

> l | custom33

> l | custom36

> l | custom37

> In earlier releases, the “qosInformationNeg” field was included only once per rating group. This resulted in skipping this field for the next LOSDV that has the same rating group but different service ID.
> With this change, in cases where the same rating group but different service ID combination is used, it is included once per rating_group+service_id combination.
> network-initiated-pdp-context Field
> This change applies to the following dictionaries:

> l | custom6

> l | custom8

> l | custom13

> l | custom24

> Existing ‘network-initiated-pdp-context’ field has been implemented and will not populate if the PDP context is activated by the network side or if the customer is enabling a RAU from LTE to 3G.
> custom33 Dictionary
> Previously, the APN OI and NI were length encoded and now the APN OI and NI are dot encoded.
> custom24 Dictionary
> The custom24 GTPP dictionary for P-GW CDRs now supports the following values in Charging Characteristics Selection Mode:

> l | servingNodeSupplied (0)

> l | homeDefault (3)

> l | roamingDefault (4)

> l | visitingDefault (5)

> l | AAASupplied (6)

> l | GWOverride (7)

> Refer to the AAA and GTPP Interface Administration and Reference for details.
> custom40 Dictionary
> New custom40 GTPP dictionary for P-GW CDRs has been implemented.
> Refer to the AAA and GTPP Interface Administration and Reference for details.
> Command Enhancements
> This section identifies GTPP command changes available in release 12.0.
> gtpp egcdr rulebase-max-length
> This command is used to configure the maximum length of charging rulebase name in LOSDVs of eG-CDRs/P-GW-CDRs to between 1 through 63 characters. If configured to 0 (zero) the rulebase name is not trimmed. This CLI command is now available in 12.0 and later releases.
> Context Configuration Mode and GTPP Group Configuration Mode
> gtpp egcdr rulebase-max-length rulebase_name_max_length
> no gtpp egcdr rulebase-max-length
> show gtpp group
> This command displays information pertaining to all or the specified GTPP group. The output of this command now includes the following new field:
> Rulebase-max-length: Indicates the maximum length of charging rulebase name in LOSDVs of eG-CDRs/P-GW-CDRs, if configured to a non-zero value.
> Exec Mode
> show gtpp group [ name gtpp_group_name | all ] [ | { grep grep_options | more } ]
> CDR Changes in Release 12.2
> This section lists GTPP dictionary changes in Release 12.2.
> Diameter Attributes
> This section lists additions and changes to Diameter attributes in Release 12.x.

> l | Diameter Attributes in Release 12.0

> l | Diameter Attributes in Release 12.1

> l | Diameter Attributes in Release 12.2

> Refer to the AAA and GTPP Interface Administration and Reference for details.
> Diameter Attributes in Release 12.0
> This section lists additions and changes to Diameter attributes in Release 12.0.

> l | New Attributes

> l | Modified Attributes

> l | Removed Attributes

> New Attributes
> The following Diameter attributes are new in Release 12.0.

> l | CHAP-Auth

> l | CHAP-Challenge

> l | CHAP-Ident

> l | CHAP-Response

> l | IMSI-Unauthenticated-Flag

> l | SN-Charging-Id

> l | User-Password

> l | Wildcarded-Public-Identity

> Modified Attributes
> The following Diameter attributes were modified in Release 12.0.

> l | Experimental-Result-Code

> Removed Attributes
> The following Diameter attributes were removed in Release 12.0.

> l | EPS-Information

> l | HSGW-Address

> l | PGW-Address

> l | PGW-MCC-MNC

> l | SGW-Address

> Diameter Attributes in Release 12.1
> This section lists additions and changes to Diameter attributes in Release 12.1.

> l | New Attributes

> l | Modified Attributes

> l | Removed Attributes

> New Attributes
> The following Diameter attributes are new in Release 12.1.
> None for this release.
> Modified Attributes
> The following Diameter attributes were modified in Release 12.1.
> None for this release.
> Removed Attributes
> The following Diameter attributes were removed in Release 12.1.
> None for this release.
> Diameter Attributes in Release 12.2
> This section lists additions and changes to Diameter attributes in Release 12.2.

> l | New Attributes

> l | Modified Attributes

> l | Removed Attributes

> New Attributes
> The following Diameter attributes are new in Release 12.2.

> l | Active-APN

> l | Age-Of-Location-Information

> l | Cause

> l | Cell-Global-Identity

> l | Charging-Characteristics-Selection-Mode

> l | Current-Location-Retrieved

> l | EPS-Location-Information

> l | EPS-User-State

> l | EUTRAN-Cell-Global-Identity

> l | Error-Diagnostic

> l | Flow-Direction

> l | Geodetic-Information

> l | Geographical-Information

> l | ICS-Indicator

> l | IMS-Voice-Over-PS-Sessions-Supported

> l | Last-UE-Activity-Time

> l | Location-Area-Identity

> l | MME-Location-Information

> l | MME-User-State

> l | QoS-Rule-Base-Name

> l | Routing-Area-Identity

> l | SGSN-Location-Information

> l | SGSN-User-State

> l | Service-Area-Identity

> l | Tracking-Area-Identity

> l | User-State

> Modified Attributes
> The following Diameter attributes were modified in Release 12.2.

> l | Access-Network-Charging-Physical-Access-Id — The Vendor ID has been changed from 10415 to 8164.

> l | Access-Network-Charging-Physical-Access-Id-Realm — The Vendor ID has been changed from 10415 to 8164.

> l | Access-Network-Charging-Physical-Access-Id-Value — The Vendor ID has been changed from 10415 to 8164.

> l | AN-GW-Address — The M-flag has been changed from 1 to 0.

> l | APN-Aggregate-Max-Bitrate-DL — The M-flag has been changed from 1 to 0.

> l | APN-Aggregate-Max-Bitrate-UL — The M-flag has been changed from 1 to 0.

> l | CoA-IP-Address — The M-flag has been changed from 1 to 0.

> l | CoA-Information — The M-flag has been changed from 1 to 0.

> l | Default-EPS-Bearer-QoS — The M-flag has been changed from 1 to 0.

> l | Event-Report-Indication — The M-flag has been changed from 1 to 0.

> l | Flow-Information — The M-flag has been changed from 1 to 0 and the sub AVP “FLOW_DIRECTION” has been added.

> l | Flow-Label — The M-flag has been changed from 1 to 0.

> l | Packet-Filter-Content — The M-flag has been changed from 1 to 0.

> l | Packet-Filter-Identifier — The M-flag has been changed from 1 to 0.

> l | Packet-Filter-Information — The M-flag has been changed from 1 to 0.

> l | Packet-Filter-Operation — The M-flag has been changed from 1 to 0.

> l | QoS-Rule-Definition — Sub AVP “FLOW_INFORMATION” has been added.

> l | QoS-Rule-Install — The following sub AVPs QOS_RULE_NAME, QOS_RULE_BASE_NAME, RESOURCE_ALLOCATION_NOTIFICATION, RULE_ACTIVATION_TIME, RULE_DEACTIVATION_TIME have been added.

> l | QoS-Rule-Remove — Sub AVP “QOS_RULE_BASE_NAME” has been added.

> l | QoS-Rule-Report — Sub AVP “QOS_RULE_BASE_NAME” has been added.

> l | RAT-Type — The M-flag has been changed from 1 to 0.

> l | Resource-Allocation-Notification — The M-flag has been changed from 1 to 0.

> l | Security-Parameter-Index — The M-flag has been changed from 1 to 0.

> l | Specific-APN-Info — Sub AVP “VISITED_NETWORK_IDENTIFIER” has been added.

> l | Subscription-Data - Sub AVP “ICS_INDICATOR” has been added.

> l | Tunnel-Header-Filter — The M-flag has been changed from 1 to 0.

> l | Tunnel-Header-Length — The M-flag has been changed from 1 to 0.

> l | Tunnel-Information — The M-flag has been changed from 1 to 0.

> Removed Attributes
> The following Diameter attributes were removed in Release 12.2.

> l | HSGW-Address

> l | PGW-Address

> l | SGW-Address

> RADIUS Attributes
> This section lists additions and changes to RADIUS attributes in Release 12.x.

> l | RADIUS Attributes in Release 12.0

> l | RADIUS Attributes in Release 12.1

> l | RADIUS Attributes in Release 12.2

> Refer to the AAA and GTPP Interface Administration and Reference for details.
> RADIUS Attributes in Release 12.0
> This section lists additions and changes to RADIUS attributes in Release 12.0.

> l | New Attributes

> l | Modified Attributes

> l | Removed Attributes

> New Attributes
> The following RADIUS attributes are new in Release 12.0.

> l | Callback-Id

> l | SN-Handoff-Indicator

> l | SN-MIP-Send-Host-Config

> Modified Attributes
> The following RADIUS attributes were modified in Release 12.0.

> l | 3GPP2-IP-Services-Authorized

> l | 3GPP2-FEID

> l | 3GPP-Allocate-IPType

> l | Acct-Input-Packets

> l | Acct-Output-Packets

> l | Acct-Termination-Cause

> l | SN-Disconnect-Reason

> l | SN-Service-Type

> l | SN1-Disconnect-Reason

> l | WiMAX-PPAQ

> Removed Attributes
> The following RADIUS attributes were removed in Release 12.0.
> None for this release.
> RADIUS Attributes in Release 12.1
> This section lists additions and changes to RADIUS attributes in Release 12.1.

> l | New Attributes

> l | Modified Attributes

> l | Removed Attributes

> New Attributes
> The following RADIUS attributes are new in Release 12.1.
> None for this release.
> Modified Attributes
> The following RADIUS attributes were modified in Release 12.1.
> None for this release.
> Removed Attributes
> The following RADIUS attributes were removed in Release 12.1.
> None for this release.
> RADIUS Attributes in Release 12.2
> This section lists additions and changes to RADIUS attributes in Release 12.2.

> l | New Attributes

> l | Modified Attributes

> l | Removed Attributes

> New Attributes
> The following RADIUS attributes are new in Release 12.2.

> l | SN-LI-Dest-Address

> l | SN-User-Privilege

> l | SN1-LI-Dest-Address

> l | SN1-NAT-Port

> l | SN1-Roaming-Status

> Modified Attributes
> The following RADIUS attributes were modified in Release 12.2.

> l | 3GPP2-MEID — The description for this attribute has been changed.

> l | NAS-Port-Type — The following two Enum values “Wireless_XGP=36” and “Wireless_DHCP=41” have been added.

> l | SN-Disconnect-Reason — The following Enum values have been added:

> l | sgsn-ptmsi-crunch = 499

> l | 3Gto4G-context-replacement = 500

> l | 4Gto3G-context-replacement = 501

> l | mme-isr-sgsn-init-detach = 502

> l | sgsn-isr-addl-ptmsi-rai = 503

> l | sgsn-sgw-dbr-cause-isr-deact = 504

> l | sgsn-isr-mme-init-detach = 505

> l | mme-sgw-dbr-cause-isr-deact = 506

> l | ptmsi-signature-mismatch = 507

> l | camel-invalid-configuration = 508

> l | sgsn-actv-reject-on-dns-failure = 509

> l | mme-no-eps-bearers-activated=510

> l | SN-Service-Type

> l | SN1-Disconnect-Reason — The following Enum values have been added:

> l | sgsn-ptmsi-crunch = 499

> l | 3Gto4G-context-replacement = 500

> l | 4Gto3G-context-replacement = 501

> l | mme-isr-sgsn-init-detach = 502

> l | sgsn-isr-addl-ptmsi-rai = 503

> l | sgsn-sgw-dbr-cause-isr-deact = 504

> l | sgsn-isr-mme-init-detach = 505

> l | mme-sgw-dbr-cause-isr-deact = 506

> l | ptmsi-signature-mismatch = 507

> l | camel-invalid-configuration = 508

> l | sgsn-actv-reject-on-dns-failure = 509

> l | mme-no-eps-bearers-activated=510

> l | SN1-NAT-Info-Record — The following sub-attributes “Calling-Station-Id” and “3GPP-Charging-Id” have been added.

> l | SN1-Service-Type

> Removed Attributes
> The following RADIUS attributes were removed in Release 12.2.
> None for this release.
> Web Element Manager Enhancements
> This section describes the Accounting enhancements made in Web Element Manager releases 12.0 and 12.2
> Web Element Manager Accounting Enhancements in Release 12.0
> The following WEM Accounting enhancements were made for Release 12.0.
> Enhancements to View/Graph Bulk Statistics Feature
> Previously, the Bulk Statistics Graphing feature allowed the user to view only 20 data sample points per page. This required the user to click to a second page if the number of data points exceeded 20.
> The Bulk Statistics Graphing feature has been enhanced to allow the user to zoom in or out to view as few or as many graph data samplings on a single page. By providing a zoom a mechanism for viewing a large number of data samples on a single screen, users can more effective analyze the trend shown in the graph.
> The slider mechanism is just below the graph display. By moving the slider control to the left or right, the user can decrease or increase the number of data samples shown.
> Above the graph display, there are discrete zoom controls that allow the user to click to see one of the following graph views:

> l | 1hr: Display all data samples for a one-hour period.

> l | 3hr: Display all data samples for a three-hour period.

> l | 6hr: Display all data samples for a six-hour period.

> l | Max: Display all available data samples

> IMPORTANT: The existing X-scale, X-scroll and Y-scale functionality have been replaced by the zoom in/zoom out feature. In addition, the Page size label has been removed, as the new zoom feature eliminates the need to view a graph over multiple pages.
> Web Element Manager Path

> l | Accounting | View/Graph Bulk Statistics

> HNBGW RANAP Bulk Statistic Enhancements
> The following bulk statistics were added to the HNBGW RANAP schema in WEM Release 12.0

> HNBGW RANAP Bulk Statistic Schema Enhancements in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> HNBGW RANAP Statistics / RANAP / CS Domain / Relocation Request | Relocation Request Tx | cs-reloc-req-tx
> RAB Setup Tx | cs-reloc-req-tx-rab-setup-tx
> Relocation Request ACK Rx | cs-reloc-req-ack-rx
> RAB Setup Success Rx | cs-reloc-req-ack-rx-rab-setup-succ-rx
> RAB Setup Fail Rx | cs-reloc-req-ack-rx-rab-setup-fail-rx
> RAB Setup Dropped | cs-reloc-req-ack-rx-rab-setup-dropped
> Relocation Detect Rx | cs-reloc-detect-rx
> Relocation Complete Rx | cs-reloc-comp-rx
> Relocation Failure Rx | cs-reloc-fail-rx
> Relocation Required Rx | cs-reloc-reqd-rx
> HNBGW RANAP Statistics / RANAP / CS Domain / Relocation Request / UMTS AMR Codec | RAB Setup Tx | cs-reloc-req-amr-codec-rab-setup-tx
> RAB Setup Success Rx | cs-reloc-req-amr-codec-rab-setup-succ-rx
> RAB Setup Fail Rx | cs-reloc-req-amr-codec-rab-setup-fail-rx
> HNBGW RANAP Statistics / RANAP / CS Domain / Relocation Request / UMTS AMR2 Codec | RAB Setup Tx | cs-reloc-req-amr2-codec-rab-setup-tx
> RAB Setup Success Rx | cs-reloc-req-amr2-codec-rab-setup-succ-rx
> RAB Setup Fail Rx | cs-reloc-req-amr2-codec-rab-setup-fail-rx
> HNBGW RANAP Statistics / RANAP / CS Domain / Relocation Request / Other Codec | RAB Setup Tx | cs-reloc-req-other-codec-rab-setup-tx
> RAB Setup Success Rx | cs-reloc-req-no-codec-rab-setup-succ-rx
> RAB Setup Fail Rx | cs-reloc-req-no-codec-rab-setup-fail-rx
> HNBGW RANAP Statistics / RANAP / CS Domain / Relocation Request / Unknown Codec | RAB Setup Tx | cs-reloc-req-unknown-codec-rab-setup-tx
> RAB Setup Success Rx | cs-reloc-req-unknown-codec-rab-setup-succ-rx
> RAB Setup Fail Rx | cs-reloc-req-unknown-codec-rab-setup-fail-rx

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> CS NW RANAP Bulk Statistic Enhancements
> The following bulk statistics have been added to the CS NW RANAP schema in WEM Release 12.0.

> CS NW RANAP Bulk Statistic Enhancements in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> CS NW RANAP Statistics / RANAP / Relocation Request | Relocation Request Rx | reloc-req-rx
> RAB Setup Rx | reloc-req-rx-rab-setup-r
> Relocation Request ACK Tx | reloc-req-ack-tx
> RAB Setup Success Tx | reloc-req-ack-tx-rab-setup-succ-tx
> Total RAB Setup Fail Tx | reloc-req-ack-tx-tot-rab-setup-fail-tx
> RAB Setup Fail (Local) Tx | reloc-req-ack-tx-rab-setup-fail-local-tx
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / Radio Network Layer Cause | Invalid Rab Id | reloc-req-ack-local-fail-invalid-rab-id
> Interaction With Other Proc | reloc-req-ack-local-fail-interact-othr-proc
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / Transport Layer Cause | Sig Transport Resource Fail | reloc-req-ack-local-fail-sig-trans-res-fail
> Iu Transport Conn failed to Establish | reloc-req-ack-local-fail-iu-conn-fail-to-estab
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / Protocol Layer Cause | Transfer syntax error | reloc-req-ack-local-fail-trans-syn-err
> Abstract syntax error(Ignore) | reloc-req-ack-local-fail-abs-syn-err-ign
> Semantic error | reloc-req-ack-local-fail-semantic-err
> Abstract syntax error(Reject) | reloc-req-ack-local-fail-abs-syn-err-rej
> Msg not compatible with receiver state | reloc-req-ack-local-fail-msg-not-comp
> Abstract syntax error (Falsely constructed msg) | reloc-req-ack-local-fail-falsely-construct-msg
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / Miscellaneous Cause | No Resource Available | reloc-req-ack-local-fail-no-res-avalable
> Unspecified | reloc-req-ack-local-fail-unspecified
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / UMTS AMR Codec | RAB Setup Rx | reloc-req-amr-codec-rab-setup-rx
> RAB Setup Success Tx | reloc-req-amr-codec-rab-setup-succ-tx
> Total RAB Setup Fail Tx | reloc-req-amr-codec-tot-rab-setup-fail-tx
> RAB Setup Fail (Local) Tx | reloc-req-amr-codec-rab-setup-fail-local-tx
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / UMTS AMR2 Codec | RAB Setup Rx | reloc-req-amr2-codec-rab-setup-rx
> RAB Setup Success Tx | reloc-req-amr2-codec-rab-setup-succ-tx
> Total RAB Setup Fail Tx | reloc-req-amr2-codec-tot-rab-setup-fail-t
> RAB Setup Fail (Local) Tx | reloc-req-amr2-codec-rab-setup-fail-local-tx
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / Other Codec | RAB Setup Rx | reloc-req-other-codec-rab-setup-rx
> RAB Setup Success Tx | reloc-req-other-codec-rab-setup-succ-tx
> Total RAB Setup Fail Tx | reloc-req-other-codec-tot-rab-setup-fail-tx
> RAB Setup Fail(Local) Tx | reloc-req-other-codec-rab-setup-fail-local-tx
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / No Codec | RAB Setup Rx | reloc-req-no-codec-rab-setup-rx
> RAB Setup Success Tx | reloc-req-no-codec-rab-setup-succ-tx
> Total RAB Setup Fail Tx | reloc-req-no-codec-tot-rab-setup-fail-tx
> RAB Setup Fail(Local) Tx | reloc-req-no-codec-rab-setup-fail-local-tx
> CS NW RANAP Statistics / RANAP / Relocation Request / Local Failure Cause / Unknown Codec | RAB Setup Rx | reloc-req-unkwn-codec-rab-setup-succ-tx
> Total RAB Setup Fail Tx | reloc-req-unkwn-codec-tot-rab-setup-fail-tx
> RAB Setup Fail (Local) Tx | reloc-req-unkwn-codec-rab-setup-fail-local-tx
> CS NW RANAP Statistics / RANAP / Relocation Request / Relocation | Relocation Detect Tx | reloc-detect-tx
> Relocation Complete Tx | reloc-comp-tx
> Total Relocation Failure Tx | total-reloc-fail-tx
> Relocation Failure (Local) Tx | reloc-fail-local-tx
> Relocation Required Tx | reloc-reqd-tx
> CS NW RANAP Statistics / RANAP / Relocation Request / Relocation / Local Failure Cause / Radio Network Layer Cause | Invalid Rab Id | reloc-fail-tx-local-fail-invalid-rab-id
> Interaction With Other Proc | reloc-fail-tx-local-fail-interact-othr-proc
> CS NW RANAP Statistics / RANAP / Relocation Request / Relocation / Local Failure Cause / Transport Layer Cause | Sig Transport Resource Fail | reloc-fail-tx-local-fail-sig-trans-res-fail
> Iu Transport Conn failed to Establish | reloc-fail-tx-local-fail-iu-conn-fail-to-estab
> CS NW RANAP Statistics / RANAP / Relocation Request / Relocation / Local Failure Cause / Protocol Layer Cause | Transfer syntax error | reloc-fail-tx-local-fail-trans-syn-err
> Abstract syntax error (Ignore) | reloc-fail-tx-local-fail-abs-syn-err-ign
> Semantic error | reloc-fail-tx-local-fail-semantic-err
> Abstract syntax error(Reject) | reloc-fail-tx-local-fail-abs-syn-err-rej
> Msg not compatible with receiver state | reloc-fail-tx-local-fail-msg-not-comp
> Abstract syntax error (Falsely constructed msg) | reloc-fail-tx-local-fail-falsely-construct-msg
> CS NW RANAP Statistics / RANAP / Relocation Request / Relocation / Local Failure Cause / Miscellaneous Cause | No Resource Available | reloc-fail-tx-local-fail-no-res-avalable
> Unspecified | reloc-fail-tx-local-fail-unspecified

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> ASNGW Bulk Statistic Enhancements
> The following bulk statistics were added to the ASNGW schema in WEM Release 12.0.

> ASNGW Bulk Statistic Schema Enhancements in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> ASNGW Statistics / R6 Messages / R6 Path Modification Request Messages | Total Sent | r6pathmodreq-totsent
> Retransmissions Sent | r6pathmodreq-retranssent
> Total Send Failures | r6pathmodreq-totsendfail
> Total Received | r6pathmodreq-totrec
> Total Accepted | r6pathmodreq-totacc
> Total Relayed | r6pathmodreq-totrelay
> Total Denied | r6pathmodreq-totdenied
> Total Discarded | r6pathmodreq-totdiscard
> Badly Formed | r6pathmodreq-badform
> Decode Error | r6pathmodreq-decodeerr
> Unspecified Error | r6pathmodreq-unspecerr
> Missing Mandatory TLV | r6pathmodreq-missmandtlv
> TLV Value Invalid | r6pathmodreq-tlvvalinval
> Unknown TLV | r6pathmodreq-unknowntlv
> Duplicate TLV Found | r6pathmodreq-duptlvfound
> No Session Found | r6pathmodreq-nosessfound
> Admin Prohibited | r6pathmodreq-adminprohib
> No Resource Drops | r6pathmodreq-noresourcedrop
> Transaction Id. Error | r6pathmodreq-transiderr
> ASNGW Statistics / R6 Messages / R6 Path Modification Response Messages | Total Sent | r6pathmodrsp-totsent
> Retransmissions Sent | r6pathmodrsp-retranssent
> Total Send Failures | r6pathmodrsp-totsendfail
> Total Received | r6pathmodrsp-totrec
> Total Accepted | r6pathmodrsp-totacc
> Total Relayed | r6pathmodrsp-totrelay
> Total Denied | r6pathmodrsp-totdenied
> Total Discarded | r6pathmodrsp-totdiscard
> Badly Formed | r6pathmodrsp-badform
> Decode Error | r6pathmodrsp-decodeerr
> Unspecified Error | r6pathmodrsp-unspecerr
> Missing Mandatory TLV | r6pathmodrsp-missmandtlv
> TLV Value Invalid | r6pathmodrsp-tlvvalinval
> Unknown TLV | r6pathmodrsp-unknowntlv
> Duplicate TLV Found | r6pathmodrsp-duptlvfound
> No Session Found | r6pathmodrsp-nosessfound
> Admin Prohibited | r6pathmodrsp-adminprohib
> No Resource Drops | r6pathmodrsp-noresourcedrop
> Transaction Id. Error | r6pathmodrsp-transiderr
> ASNGW Statistics / R6 Messages / R6 Path Modification Ack Messages | Total Sent | r6pathmodack-totsent
> Retransmissions Sent | r6pathmodack-retranssent
> Total Send Failures | r6pathmodack-totsendfail
> Total Received | r6pathmodack-totrec
> Total Accepted | r6pathmodack-totacc
> Total Relayed | r6pathmodack-totrelay
> Total Denied | r6pathmodack-totdenied
> Total Discarded | r6pathmodack-totdiscard
> Badly Formed | r6pathmodack-badform
> Decode Error | r6pathmodack-decodeerr
> Unspecified Error | r6pathmodack-unspecerr
> Missing Mandatory TLV | r6pathmodack-missmandtlv
> TLV Value Invalid | r6pathmodack-tlvvalinval
> Unknown TLV | r6pathmodack-unknowntlv
> Duplicate TLV Found | r6pathmodack-duptlvfound
> No Session Found | r6pathmodack-nosessfound
> Admin Prohibited | r6pathmodack-adminprohib
> No Resource Drops | r6pathmodack-noresourcedrop
> Transaction Id. Error | r6pathmodack-transiderr
> ASNGW Statistics / R6 Messages / R4 Path Modification Request Messages | Total Sent | r4pathmodreq-totsent
> Retransmissions Sent | r4pathmodreq-retranssent
> Total Send Failures | r4pathmodreq-totsendfail
> Total Received | r4pathmodreq-totrec
> Total Accepted | r4pathmodreq-totacc
> Total Relayed | r4pathmodreq-totrelay
> Total Denied | r4pathmodreq-totdenied
> Total Discarded | r4pathmodreq-totdiscard
> Badly Formed | r4pathmodreq-badform
> Decode Error | r4pathmodreq-decodeerr
> Unspecified Error | r4pathmodreq-unspecerr
> Missing Mandatory TLV | r4pathmodreq-missmandtlv
> TLV Value Invalid | r4pathmodreq-tlvvalinval
> Unknown TLV | r4pathmodreq-unknowntlv
> Duplicate TLV Found | r4pathmodreq-duptlvfound
> No Session Found | r4pathmodreq-nosessfound
> Admin Prohibited | r4pathmodreq-adminprohib
> No Resource Drops | r4pathmodreq-noresourcedrop
> Transaction Id. Error | r4pathmodreq-transiderr
> ASNGW Statistics / R6 Messages / R4 Path Modification Response Messages | Total Sent | r4pathmodrsp-totsent
> Retransmissions Sent | r4pathmodrsp-retranssent
> Total Send Failures | r4pathmodrsp-totsendfail
> Total Received | r4pathmodrsp-totrec
> Total Accepted | r4pathmodrsp-totacc
> Total Relayed | r4pathmodrsp-totrelay
> Total Denied | r4pathmodrsp-totdenied
> Total Discarded | r4pathmodrsp-totdiscard
> Badly Formed | r4pathmodrsp-badform
> Decode Error | r4pathmodrsp-decodeerr
> Unspecified Error | r4pathmodrsp-unspecerr
> Missing Mandatory TLV | r4pathmodrsp-missmandtlv
> TLV Value Invalid | r4pathmodrsp-tlvvalinval
> Unknown TLV | r4pathmodrsp-unknowntlv
> Duplicate TLV Found | r4pathmodrsp-duptlvfound
> No Session Found | r4pathmodrsp-nosessfound
> Admin Prohibited | r4pathmodrsp-adminprohib
> No Resource Drops | r4pathmodrsp-noresourcedrop
> Transaction Id. Error | r4pathmodrsp-transiderr
> ASNGW Statistics / R6 Messages / R4 Path Modification Ack Messages | Total Sent | r4pathmodack-totsent
> Retransmissions Sent | r4pathmodack-retranssent
> Total Send Failures | r4pathmodack-totsendfail
> Total Received | r4pathmodack-totrec
> Total Accepted | r4pathmodack-totacc
> Total Relayed | r4pathmodack-totrelay
> Total Denied | r4pathmodack-totdenied
> Total Discarded | r4pathmodack-totdiscard
> Badly Formed | r4pathmodack-badform
> Decode Error | r4pathmodack-decodeerr
> Unspecified Error | r4pathmodack-unspecerr
> Missing Mandatory TLV | r4pathmodack-missmandtlv
> TLV Value Invalid | r4pathmodack-tlvvalinval
> Unknown TLV | r4pathmodack-unknowntlv
> Duplicate TLV Found | r4pathmodack-duptlvfound
> No Session Found | r4pathmodack-nosessfound
> Admin Prohibited | r4pathmodack-adminprohib
> No Resource Drops | r4pathmodack-noresourcedrop
> Transaction Id. Error | r4pathmodack-transiderr
> ASNGW Statistics / R6 Messages / R6 Capability Req Messages | Total Sent | r6capabilityreq-totsent
> Retransmissions Sent | r6capabilityreq-retranssent
> Total Send Failures | r6capabilityreq-totsendfail
> Total Received | r6capabilityreq-totrec
> Total Accepted | r6capabilityreq-totacc
> Total Relayed | r6capabilityreq-totrelay
> Total Denied | r6capabilityreq-totdenied
> Total Discarded | r6capabilityreq-totdiscard
> Badly Formed | r6capabilityreq-badform
> Decode Error | r6capabilityreq-decodeerr
> Unspecified Error | r6capabilityreq-unspecerr
> Missing Mandatory TLV | r6capabilityreq-missmandtlv
> TLV Value Invalid | r6capabilityreq-tlvvalinval
> Unknown TLV | r6capabilityreq-unknowntlv
> Duplicate TLV Found | r6capabilityreq-duptlvfound
> Admin Prohibited | r6capabilityreq-admprohibit
> No Resource Drops | r6capabilityreq-noresourcedrop
> Transaction Id. Error | r6capabilityreq-transiderr
> ASNGW Statistics / R6 Messages / R6 Capability Rsp Messages | Total Sent | r6capabilityrsp-totsent
> Retransmissions Sent | r6capabilityrsp-retranssent
> Total Send Failures | r6capabilityrsp-totsendfail
> Total Received | r6capabilityrsp-totrec
> Total Accepted | r6capabilityrsp-totacc
> Total Relayed | r6capabilityrsp-totrelay
> Total Denied | r6capabilityrsp-totdenied
> Total Discarded | r6capabilityrsp-totdiscard
> Badly Formed | r6capabilityrsp-badform
> Decode Error | r6capabilityrsp-decodeerr
> Unspecified Error | r6capabilityrsp-unspecerr
> Missing Mandatory TLV | r6capabilityrsp-missmandtlv
> TLV Value Invalid | r6capabilityrsp-tlvvalinval
> Unknown TLV | r6capabilityrsp-unknowntlv
> Duplicate TLV Found | r6capabilityrsp-duptlvfound
> No Session Found | r6capabilityrsp-nosessfound
> Admin Prohibited | r6capabilityrsp-admprohibit
> No Resource Drops | r6capabilityrsp-noresourcedrop
> Transaction Id. Error | r6capabilityrsp-transiderr
> ASNGW Statistics / R6 Messages / R6 Capability Ack Messages | Total Sent | r6capabilityack-totsent
> Retransmissions Sent | r6capabilityack-retranssent
> Total Send Failures | r6capabilityack-totsendfail
> Total Received | r6capabilityack-totrec
> Total Accepted | r6capabilityack-totacc
> Total Relayed | r6capabilityack-totrelay
> Total Denied | r6capabilityack-totdenied
> Total Discarded | r6capabilityack-totdiscard
> Badly Formed | r6capabilityack-badform
> Decode Error | r6capabilityack-decodeerr
> Unspecified Error | r6capabilityack-unspecerr
> Missing Mandatory TLV | r6capabilityack-missmandtlv
> TLV Value Invalid | r6capabilityack-tlvvalinval
> Unknown TLV | r6capabilityack-unknowntlv
> Duplicate TLV Found | r6capabilityack-duptlvfound
> No Session Found | r6capabilityack-nosessfound
> Admin Prohibited | r6capabilityack-admprohibit
> No Resource Drops | r6capabilityack-noresourcedrop
> Transaction Id. Error | r6capabilityack-transiderr
> ASNGW Statistics / R6 Messages / R4 Capability Req Messages | Total Sent | r4capabilityreq-totsent
> Retransmissions Sent | r4capabilityreq-retranssent
> Total Send Failures | r4capabilityreq-totsendfail
> Total Received | r4capabilityreq-totrec
> Total Accepted | r4capabilityreq-totacc
> Total Relayed | r4capabilityreq-totrelay
> Total Denied | r4capabilityreq-totdenied
> Total Discarded | r4capabilityreq-totdiscard
> Badly Formed | r4capabilityreq-badform
> Decode Error | r4capabilityreq-decodeerr
> Unspecified Error | r4capabilityreq-unspecerr
> Missing Mandatory TLV | r4capabilityreq-missmandtlv
> TLV Value Invalid | r4capabilityreq-tlvvalinval
> Unknown TLV | r4capabilityreq-unknowntlv
> Duplicate TLV Found | r4capabilityreq-duptlvfound
> No Session Found | r4capabilityreq-nosessfound
> Admin Prohibited | r4capabilityreq-admprohibit
> No Resource Drops | r4capabilityreq-noresourcedrop
> Transaction Id. Error | r4capabilityreq-transiderr
> ASNGW Statistics / R6 Messages / R4 Capability Rsp Messages | Total Sent | r4capabilityrsp-totsent
> Retransmissions Sent | r4capabilityrsp-retranssent
> Total Send Failures | r4capabilityrsp-totsendfail
> Total Received | r4capabilityrsp-totrec
> Total Accepted | r4capabilityrsp-totacc
> Total Relayed | r4capabilityrsp-totrelay
> Total Denied | r4capabilityrsp-totdenied
> Total Discarded | r4capabilityrsp-totdiscard
> Badly Formed | r4capabilityrsp-badform
> Decode Error | r4capabilityrsp-decodeerr
> Unspecified Error | r4capabilityrsp-unspecerr
> Missing Mandatory TLV | r4capabilityrsp-missmandtlv
> TLV Value Invalid | r4capabilityrsp-tlvvalinval
> Unknown TLV | r4capabilityrsp-unknowntlv
> Duplicate TLV Found | r4capabilityrsp-duptlvfound
> No Session Found | r4capabilityrsp-nosessfound
> Admin Prohibited | r4capabilityrsp-admprohibit
> No Resource Drops | r4capabilityrsp-noresourcedrop
> Transaction Id. Error | r4capabilityrsp-transiderr
> ASNGW Statistics / R6 Messages / R4 Capability Ack Messages | Total Sent | r4capabilityack-totsent
> Retransmissions Sent | r4capabilityack-retranssent
> Total Send Failures | r4capabilityack-totsendfail
> Total Received | r4capabilityack-totrec
> Total Accepted | r4capabilityack-totacc
> Total Relayed | r4capabilityack-totrelay
> Total Denied | r4capabilityack-totdenied
> Total Discarded | r4capabilityack-totdiscard
> Badly Formed | r4capabilityack-badform
> Decode Error | r4capabilityack-decodeerr
> Unspecified Error | r4capabilityack-unspecerr
> Missing Mandatory TLV | r4capabilityack-missmandtlv
> TLV Value Invalid | r4capabilityack-tlvvalinval
> Unknown TLV | r4capabilityack-unknowntlv
> Duplicate TLV Found | r4capabilityack-duptlvfound
> No Session Found | r4capabilityack-nosessfound
> Admin Prohibited | r4capabilityack-admprohibit
> No Resource Drops | r4capabilityack-noresourcedrop

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> MME Bulk Statistics Enhancements
> The following bulk statistic was added to the MME schema in WEM Release 12.0.

> MME Bulk Statistic Enhancement in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> MME Statistics / EMM Events / Outbound Relocations (using S1 HO procedures) | Failures | emmevent-outs1ho4g3g-failure

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> System Bulk Statistics Enhancements
> The following bulk statistics were added to the System schema in WEM Release 12.0.

> System Bulk Statistic Enhancements in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> System Statistics / Session Managers / Setup Time Statistics | 16..18 sec | sess-setuptime-over16sec
> System Statistics / CC Bad Answer Statistics | Auth-Application-Id | cc-badans-auth-appid
> Session-Id | cc-badans-sessid
> CC-Request-Number | cc-badans-cc-req-num
> CC-Request-Type | cc-badans-cc-req-type
> Origin-Host | cc-badans-origin-host
> Origin-Realm | cc-badans-origin-realm
> Parse-Message-Errors | cc-badans-parsemsg-err
> Parse-Mscc-Errors | cc-badans-parsemscc-err
> Misc | cc-badans-misc-err
> System Statistics / Session Disconnect Reasons | CT-PMIP-RRQ-NVSE-Value-Change | disc-reason-427
> tcp-read-failed | disc-reason-428
> tcp-write-failed | disc-reason-429
> ssl-handshake-failed | disc-reason-430
> ssl-renegotiate-failed | disc-reason-431
> ssl-bad-message | disc-reason-432
> ssl-alert-received | disc-reason-433
> ssl-disconnect | disc-reason-434
> ssl-migration | disc-reason-435
> sgsn-ard-failure | disc-reason-436
> sgsn-camel-release | disc-reason-437

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> SGW Bulk Statistic Enhancements in Release 12.0.
> The following table lists the SGW bulk statistics added in WEM Release 12.0.

> SGW Bulk Statistic Enhancements in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> SGW Statistics / Session Level Statistics / PDNs Released Reason | S4 Error Ind | sessstat-pdnrelrsn-s4err
> S12 Error Ind | sessstat-pdnrelrsn-s12err
> Path Failure S4 | sessstat-pdnrelrsn-pathfail-S4
> Path Failure S12 | sessstat-pdnrelrsn-pathfail-S12
> Path Failure S4-U | sessstat-pdnrelrsn-pathfail-S4-u
> SGW Statistics / Bearer Level Statistics / Dedicated Bearers Released Reason | S4 Error Ind | totepsbearrel-dedrsn-s4err
> S12 Error Ind | totepsbearrel-dedrsn-s12err
> SGW Statistics / Bearer Level Statistics / Dedicated Bearers Released Reason (con’t) | Path Failure S12 | totepsbearrel-dedrsn-pathfail-s12
> Path Failure S4-U | totepsbearrel-dedrsn-pathfail-s4-u
> SGW Statistics / Inter-SGW Handover Statistics / X2 Based | Success | intersgwhaovstat-pdnin-x2-success
> Fail | intersgwhaovstat-pdnin-x2-fail
> SGW Statistics / Inter-SGW Handover Statistics / Idle-mode TAU | Success | intersgwhaovstat-pdnin-idletau-success
> Fail | intersgwhaovstat-pdnin-idletau-fail
> SGW Statistics / Inter-SGW Handover Statistics / S1 Based | Success | intersgwhaovstat-pdnin-s1-success
> Fail | intersgwhaovstat-pdnin-s1-fail
> SGW Statistics / Inter-SGW Handover Statistics / Inter System | Fail | intersgwhaovstat-intersystem-fail
> Success | intersgwhaovstat-intersystem-success
> Fail | intersgwhaovstat-intersystem-fail
> SGW Statistics / Intra-SGW Handover Statistics / Intra-MME | Success | intersgwhaovstat-intra-intramme-success
> Fail | intersgwhaovstat-intra-intramme-fail
> SGW Statistics / Intra-SGW Handover Statistics / Inter-MME | Success | intersgwhaovstat-intra-intermme-success
> Fail | intersgwhaovstat-intra-intermme-fail
> SGW Statistics / S1U Total Data Statistics / Uplink | Pkts | s1u-uplnk-packets
> Bytes | s1u-uplnk-bytes
> Dropped Pkts | s1u-uplnk-dropped-packets
> Dropped Bytes | s1u-uplnk-dropped-bytes
> Bytes QCI 1 | s1u-uplnk-qci1totbyte
> Pkts QCI 1 | s1u-uplnk-qci1totpkt
> Bytes QCI 2 | s1u-uplnk-qci2totbyte
> Pkts QCI 2 | s1u-uplnk-qci2totpkt
> Bytes QCI 3 | s1u-uplnk-qci3totbyte
> Pkts QCI 3 | s1u-uplnk-qci3totpkt
> Bytes QCI 4 | s1u-uplnk-qci4totbyte
> Pkts QCI 4 | s1u-uplnk-qci4totpkt
> Bytes QCI 5 | s1u-uplnk-qci5totbyte
> Pkts QCI 5 | s1u-uplnk-qci5totpkt
> Bytes QCI 6 | s1u-uplnk-qci6totbyte
> Pkts QCI 6 | s1u-uplnk-qci6totpkt
> Bytes QCI 7 | s1u-uplnk-qci7totbyte
> Pkts QCI 7 | s1u-uplnk-qci7totpkt
> Bytes QCI 8 | s1u-uplnk-qci8totbyte
> Pkts QCI 8 | s1u-uplnk-qci8totpkt
> Bytes QCI 9 | s1u-uplnk-qci9totbyte
> Pkts QCI 9 | s1u-uplnk-qci9totpkt
> Bytes Non-Std QCI | s1u-uplnk-othertotbyte
> Pkts Non-Std QCI | s1u-uplnk-othertotpkt
> Dropped Bytes QCI 1 | s1u-uplnk-drop-qci1totbyte
> Dropped Pkts QCI 1 | s1u-uplnk-drop-qci1totpkt
> Dropped Bytes QCI 1 | s1u-uplnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s1u-uplnk-drop-qci2totbyte
> Dropped Pkts QCI 2 | s1u-uplnk-drop-qci2totpkt
> Dropped Bytes QCI 3 | s1u-uplnk-drop-qci3totbyte
> Dropped Pkts QCI 3 | s1u-uplnk-drop-qci3totpkt
> SGW Statistics / S1U Total Data Statistics / Uplink (con’t) | Dropped Bytes QCI 4 | s1u-uplnk-drop-qci4totbyte
> Dropped Pkts QCI 4 | s1u-uplnk-drop-qci4totpkt
> Dropped Bytes QCI 5 | s1u-uplnk-drop-qci5totbyte
> Dropped Pkts QCI 5 | s1u-uplnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s1u-uplnk-drop-qci6totpkt
> Dropped Bytes QCI 6 | s1u-uplnk-drop-qci6totbyte
> Dropped Pkts QCI 7 | s1u-uplnk-drop-qci7totpkt
> Dropped Bytes QCI 7 | s1u-uplnk-drop-qci7totbyte
> Dropped Pkts QCI 8 | s1u-uplnk-drop-qci8totpkt
> Dropped Bytes QCI 8 | s1u-uplnk-drop-qci8totbyte
> Dropped Pkts QCI 9 | s1u-uplnk-drop-qci9totpkt
> Dropped Bytes QCI 9 | s1u-uplnk-drop-qci9totbyte
> Dropped Pkts Non-Std QCI | s1u-uplnk-drop-otherpkt
> Dropped Bytes Non-Std QCI | s1u-uplnk-drop-othertotbyte
> SGW Statistics / S1U Total Data Statistics / Downlink | Pkts | s1u-downlnk-packets
> Bytes | s1u-downlnk-bytes
> Dropped Pkts | s1u-downlnk-dropped-packets
> Dropped Bytes | s1u-downlnk-dropped-bytes
> Bytes QCI 1 | s1u-downlnk-qci1totbyte
> Pkts QCI 1 | s1u-downlnk-qci1totpkt
> Bytes QCI 2 | s1u-downlnk-qci2totbyte
> Pkts QCI 2 | s1u-downlnk-qci2totpkt
> Bytes QCI 3 | s1u-downlnk-qci3totbyte
> Pkts QCI 3 | s1u-downlnk-qci3totpkt
> Bytes QCI 4 | s1u-downlnk-qci4totbyte
> Pkts QCI 4 | s1u-downlnk-qci4totpkt
> Bytes QCI 5 | s1u-downlnk-qci5totbyte
> Pkts QCI 5 | s1u-downlnk-qci5totpkt
> Bytes QCI 6 | s1u-downlnk-qci6totbyte
> Pkts QCI 6 | s1u-downlnk-qci6totpkt
> Bytes QCI 7 | s1u-downlnk-qci7totbyte
> Pkts QCI 7 | s1u-downlnk-qci7totpkt
> Bytes QCI 8 | s1u-downlnk-qci8totbyte
> Pkts QCI 8 | s1u-downlnk-qci8totpkt
> Bytes QCI 9 | s1u-downlnk-qci9totbyte
> Pkts QCI 9 | s1u-downlnk-qci9totpkt
> Bytes Non-Std QCI | s1u-downlnk-othertotbyte
> Pkts Non-Std QCI | s1u-downlnk-othertotpkt
> Dropped Bytes QCI 1 | s1u-downlnk-drop-qci1totbyte
> SGW Statistics / S1U Total Data Statistics / Downlink (con’t) | Dropped Pkts QCI 1 | s1u-downlnk-drop-qci1totpkt
> Dropped Bytes QCI 2 | s1u-downlnk-drop-qci2totbyte
> Dropped Pkts QCI 2 | s1u-downlnk-drop-qci2totpkt
> Dropped Bytes QCI 3 | s1u-downlnk-drop-qci3totbyte
> Dropped Pkts QCI 3 | s1u-downlnk-drop-qci3totpkt
> Dropped Bytes QCI 4 | s1u-downlnk-drop-qci4totbyte
> Dropped Pkts QCI 4 | s1u-downlnk-drop-qci4totpkt
> Dropped Bytes QCI 5 | s1u-downlnk-drop-qci5totbyte
> Dropped Pkts QCI 5 | s1u-downlnk-drop-qci5totpkt
> Dropped Bytes QCI 6 | s1u-downlnk-drop-qci6totbyte
> Dropped Pkts QCI 6 | s1u-downlnk-drop-qci6totpkt
> Dropped Bytes QCI 7 | s1u-downlnk-drop-qci7totbyte
> Dropped Pkts QCI 7 | s1u-downlnk-drop-qci7totpkt
> Dropped Bytes QCI 8 | s1u-downlnk-drop-qci8totbyte
> Dropped Pkts QCI 8 | s1u-downlnk-drop-qci8totpkt
> Dropped Bytes QCI 9 | s1u-downlnk-drop-qci9totbyte
> Dropped Pkts QCI 9 | s1u-downlnk-drop-qci9totpkt
> Dropped Bytes Non-Std QCI | s1u-downlnk-drop-othertotbyte
> Dropped Pkts Non-Std QCI | s1u-downlnk-drop-othertotpkt
> SGW Statistics / S4U Total Data Statistics / Uplink | Pkts | s4u-uplnk-packets
> Bytes | s4u-uplnk-bytes
> Dropped Pkts | s4u-uplnk-dropped-packets
> Dropped Bytes | s4u-uplnk-dropped-bytes
> Bytes QCI 1 | s4u-uplnk-qci1totbyte
> Pkts QCI 1 | s4u-uplnk-qci1totpkt
> Bytes QCI 2 | s4u-uplnk-qci2totbyte
> Pkts QCI 2 | s4u-uplnk-qci2totpkt
> Bytes QCI 3 | s4u-uplnk-qci3totbyte
> Pkts QCI 3 | s4u-uplnk-qci3totpkt
> Bytes QCI 4 | s4u-uplnk-qci4totbyte
> Pkts QCI 4 | s4u-uplnk-qci4totpkt
> Bytes QCI 5 | s4u-uplnk-qci5totbyte
> Pkts QCI 5 | s4u-uplnk-qci5totpkt
> Bytes QCI 6 | s4u-uplnk-qci6totbyte
> Pkts QCI 6 | s4u-uplnk-qci6totpkt
> Bytes QCI 7 | s4u-uplnk-qci7totbyte
> Pkts QCI 7 | s4u-uplnk-qci7totpkt
> Bytes QCI 8 | s4u-uplnk-qci8totbyte
> SGW Statistics / S4U Total Data Statistics / Uplink (con’t) |  |
> Pkts QCI 8 | s4u-uplnk-qci8totpkt
> Bytes QCI 9 | s4u-uplnk-qci9totbyte
> Pkts QCI 9 | s4u-uplnk-qci9totpkt
> Bytes Non-Std QCI | s4u-uplnk-othertotbyte
> Pkts Non-Std QCI | s4u-uplnk-othertotpkt
> Dropped Bytes QCI 1 | s4u-uplnk-drop-qci1totbyte
> Dropped Pkts QCI 1 | s4u-uplnk-drop-qci1totpkt
> Dropped Bytes QCI 2 | s4u-uplnk-drop-qci2totbyte
> Dropped Pkts QCI 2 | s4u-uplnk-drop-qci2totpkt
> Dropped Bytes QCI 3 | s4u-uplnk-drop-qci3totbyte
> Dropped Pkts QCI 3 | s4u-uplnk-drop-qci3totpkt
> Dropped Bytes QCI 4 | s4u-uplnk-drop-qci4totbyte
> Dropped Pkts QCI 4 | s4u-uplnk-drop-qci4totpkt
> Dropped Bytes QCI 5 | s4u-uplnk-drop-qci5totbyte
> Dropped Pkts QCI 5 | s4u-uplnk-drop-qci5totpkt
> Dropped Bytes QCI 6 | s4u-uplnk-drop-qci6totbyte
> Dropped Pkts QCI 6 | s4u-uplnk-drop-qci6totpkt
> Dropped Bytes QCI 7 | s4u-uplnk-drop-qci7totbyte
> Dropped Pkts QCI 7 | s4u-uplnk-drop-qci7totpkt
> Dropped Bytes QCI 8 | s4u-uplnk-drop-qci8totbyte
> Dropped Pkts QCI 8 | s4u-uplnk-drop-qci8totpkt
> Dropped Bytes QCI 9 | s4u-uplnk-drop-qci9totbyte
> Dropped Pkts QCI 9 | s4u-uplnk-drop-qci9totpkt
> Dropped Bytes Non-Std QCI | s4u-uplnk-drop-othertotbyte
> Dropped Pkts Non-Std QCI | s4u-uplnk-drop-otherpkt
> SGW Statistics / S4U Total Data Statistics / Downlink | Pkts | s4u-downlnk-packets
> Bytes | s4u-downlnk-bytes
> Dropped Pkts | s4u-downlnk-dropped-packets
> Dropped Bytes | s4u-downlnk-dropped-bytes
> Bytes QCI 1 | s4u-downlnk-qci1totbyte
> Pkts QCI 1 | s4u-downlnk-qci1totpkt
> Bytes QCI 2 | s4u-downlnk-qci2totbyte
> Pkts QCI 2 | s4u-downlnk-qci2totpkt
> Bytes QCI 3 | s4u-downlnk-qci3totbyte
> Pkts QCI 3 | s4u-downlnk-qci3totpkt
> Bytes QCI 4 | s4u-downlnk-qci4totbyte
> Pkts QCI 4 | s4u-downlnk-qci4totpkt
> Bytes QCI 5 | s4u-downlnk-qci5totbyte
> Pkts QCI 5 | s4u-downlnk-qci5totpkt
> SGW Statistics / S4U Total Data Statistics / Downlink (con’t) | Bytes QCI 6 | s4u-downlnk-qci6totbyte
> Pkts QCI 6 | s4u-downlnk-qci6totpkt
> Bytes QCI 7 | s4u-downlnk-qci7totbyte
> Pkts QCI 7 | s4u-downlnk-qci7totpkt
> Bytes QCI 8 | s4u-downlnk-qci8totbyte
> Pkts QCI 8 | s4u-downlnk-qci8totpkt
> Bytes QCI 9 | s4u-downlnk-qci9totbyte
> Pkts QCI 9 | s4u-downlnk-qci9totpkt
> Bytes Non-Std QCI | s4u-downlnk-othertotbyte
> Pkts Non-Std QCI | s4u-downlnk-othertotpkt
> Dropped Bytes QCI 1 | s4u-downlnk-drop-qci1totbyte
> Dropped Pkts QCI 1 | s4u-downlnk-drop-qci1totpkt
> Dropped Bytes QCI 2 | s4u-downlnk-drop-qci2totbyte
> Dropped Pkts QCI 2 | s4u-downlnk-drop-qci2totpkt
> Dropped Bytes QCI 3 | s4u-downlnk-drop-qci3totbyte
> Dropped Pkts QCI 3 | s4u-downlnk-drop-qci3totpkt
> Dropped Bytes QCI 4 | s4u-downlnk-drop-qci4totbyte
> Dropped Pkts QCI 4 | s4u-downlnk-drop-qci4totpkt
> Dropped Bytes QCI 5 | s4u-downlnk-drop-qci5totbyte
> Dropped Pkts QCI 5 | s4u-downlnk-drop-qci5totpkt
> Dropped Bytes QCI 6 | s4u-downlnk-drop-qci6totbyte
> Dropped Pkts QCI 6 | s4u-downlnk-drop-qci6totpkt
> Dropped Bytes QCI 7 | s4u-downlnk-drop-qci7totbyte
> Dropped Pkts QCI 7 | s4u-downlnk-drop-qci7totpkt
> Dropped Bytes QCI 8 | s4u-downlnk-drop-qci8totbyte
> Dropped Pkts QCI 8 | s4u-downlnk-drop-qci8totpkt
> Dropped Bytes QCI 9 | s4u-downlnk-drop-qci9totbyte
> SGW Statistics / S4U Total Data Statistics / Downlink (con’t) | Dropped Pkts QCI 9 | s4u-downlnk-drop-qci9totpkt
> Dropped Bytes Non-Std QCI | s4u-downlnk-drop-othertotbyte
> Dropped Pkts Non-Std QCI | s4u-downlnk-drop-othertotpkt
> SGW Statistics / S5 Total Data Statistics / Uplink | Pkts | s5-uplnk-packets
> Bytes | s5-uplnk-bytes
> Dropped Pkts | s5-uplnk-dropped-packets
> Dropped Bytes | s5-uplnk-dropped-bytes
> Pkts QCI 1 | s5-uplnk-qci1totpkt
> Pkts QCI 2 | s5-uplnk-qci2totpkt
> Pkts QCI 3 | s5-uplnk-qci3totpkt
> Pkts QCI 4 | s5-uplnk-qci4totpkt
> Pkts QCI 5 | s5-uplnk-qci5totpkt
> SGW Statistics / S5 Total Data Statistics / Uplink (con’t) | Pkts QCI 6 | s5-uplnk-qci6totpkt
> Pkts QCI 7 | s5-uplnk-qci7totpkt
> Pkts QCI 8 | s5-uplnk-qci8totpkt
> Pkts QCI 9 | s5-uplnk-qci9totpkt
> Pkts Non-Std QCI | s5-uplnk-othertotpkt
> Bytes QCI 1 | s5-uplnk-qci1totbyte
> Bytes QCI 2 | s5-uplnk-qci1totbyte
> Bytes QCI 3 | s5-uplnk-qci1totbyte
> Bytes QCI 4 | s5-uplnk-qci1totbyte
> Bytes QCI 5 | s5-uplnk-qci1totbyte
> Bytes QCI 6 | s5-uplnk-qci1totbyte
> Bytes QCI 7 | s5-uplnk-qci1totbyte
> Bytes QCI 8 | s5-uplnk-qci1totbyte
> Bytes QCI 9 | s5-uplnk-qci1totbyte
> Bytes Non-Std QCI | s5-uplnk-othertotbyte
> Dropped Pkts QCI 1 | s5-uplnk-drop-qci1totpkt
> Dropped Pkts QCI 2 | s5-uplnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s5-uplnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s5-uplnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s5-uplnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s5-uplnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s5-uplnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s5-uplnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s5-uplnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s5-uplnk-drop-otherpkt
> Dropped Bytes QCI 1 | s5-uplnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s5-uplnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s5-uplnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s5-uplnk-drop-qcir4totbyte
> Dropped Bytes QCI 5 | s5-uplnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s5-uplnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s5-uplnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s5-uplnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s5-uplnk-drop-qci9totbyte
> Dropped Bytes Non-Std QCI | s5-uplnk-drop-othertotbyte
> SGW Statistics / S5 Total Data Statistics / Downlink | Pkts | s5-downlnk-packets
> Bytes | s5-downlnk-bytes
> Dropped Pkts | s5-downlnk-dropped-packets
> Dropped Bytes | s5-downlnk-dropped-bytes
> SGW Statistics / S5 Total Data Statistics / Downlink (con't.) | Pkts QCI 1 | s5-downlnk-qci1totpkt
> Pkts QCI 2 | s5-downlnk-qci2totpkt
> Pkts QCI 3 | s5-downlnk-qci3totpkt
> Pkts QCI 4 | s5-downlnk-qci4totpkt
> Pkts QCI 5 | s5-downlnk-qci5otpkt
> Pkts QCI 6 | s5-downlnk-qci6totpkt
> Pkts QCI 7 | s5-downlnk-qci7totpkt
> Pkts QCI 8 | s5-downlnk-qci8totpkt
> Pkts QCI 9 | s5-downlnk-qci9totpkt
> Pkts Non-Std QCI | s5-downlnk-othertotpkt
> Bytes QCI 1 | s5-downlnk-qci1totbyte
> Bytes QCI 2 | s5-downlnk-qci2totbyte
> Bytes QCI 3 | s5-downlnk-qci3totbyte
> Bytes QCI 4 | s5-downlnk-qci4totbyte
> Bytes QCI 5 | s5-downlnk-qci5totbyte
> Bytes QCI 6 | s5-downlnk-qci6totbyte
> Bytes QCI 7 | s5-downlnk-qci7totbyte
> Bytes QCI 8 | s5-downlnk-qci8totbyte
> Bytes QCI 9 | s5-downlnk-qci9totbyte
> Bytes Non-Std QCI | s5-downlnk-othertotbyte
> Dropped Pkts QCI 1 | s5-downlnk-drop-qci1totpkt
> Dropped Pkts QCI 2 | s5-downlnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s5-downlnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s5-downlnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s5-downlnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s5-downlnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s5-downlnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s5-downlnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s5-downlnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s5-downlnk-drop-otherpkt
> Dropped Bytes QCI 1 | s5-downlnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s5-downlnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s5-downlnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s5-downlnk-drop-qci4totbyte
> Dropped Bytes QCI 5 | s5-downlnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s5-downlnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s5-downlnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s5-downlnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s5-downlnk-drop-qci9totbyte
> SGW Statistics / S5 Total Data Statistics / Downlink (con't.) | Dropped Bytes Non-Std QCI | s5-downlnk-drop-othertotbyte
> Dropped Pkts Non-Std QCI | s5-downlnk-drop-othertotpkt
> SGW Statistics / S8 Total Data Statistics / Uplink | Pkts | s8-uplnk-packets
> Bytes | s8-uplnk-bytes
> Dropped Pkts | s8-uplnk-dropped-packets
> Dropped Bytes | s8-uplnk-dropped-bytes
> Pkts QCI 1 | s8-uplnk-qci1totpkt
> Pkts QCI 2 | s8-uplnk-qci2totpkt
> Pkts QCI 3 | s8-uplnk-qci3totpkt
> Pkts QCI 4 | s8-uplnk-qci4totpkt
> Pkts QCI 5 | s8-uplnk-qci5totpkt
> Pkts QCI 6 | s8-uplnk-qci6totpkt
> Pkts QCI 7 | s8-uplnk-qci7totpkt
> Pkts QCI 8 | s8-uplnk-qci8totpkt
> Pkts QCI 9 | s8-uplnk-qci9totpkt
> Pkts Non-Std QCI | s8-uplnk-othertotpkt
> Bytes QCI 1 | s8-uplnk-qci1totbyte
> Bytes QCI 2 | s8-uplnk-qci1totbyte
> Bytes QCI 3 | s8-uplnk-qci1totbyte
> Bytes QCI 4 | s8-uplnk-qci1totbyte
> Bytes QCI 5 | s8-uplnk-qci1totbyte
> Bytes QCI 6 | s8-uplnk-qci1totbyte
> Bytes QCI 7 | s8-uplnk-qci1totbyte
> Bytes QCI 8 | s8-uplnk-qci1totbyte
> Bytes QCI 9 | s8-uplnk-qci1totbyte
> Bytes Non-Std QCI | s8-uplnk-othertotbyte
> Dropped Pkts QCI 1 | s8-uplnk-drop-qci1totpkt
> Dropped Pkts QCI 2 | s8-uplnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s8-uplnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s8-uplnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s8-uplnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s8-uplnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s8-uplnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s8-uplnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s8-uplnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s8-uplnk-drop-otherpkt
> Dropped Bytes QCI 1 | s8-uplnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s8-uplnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s8-uplnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s8-uplnk-drop-qcir4totbyte
> SGW Statistics / S8 Total Data Statistics / Uplink (con’t) | Dropped Bytes QCI 5 | s8-uplnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s8-uplnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s8-uplnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s8-uplnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s8-uplnk-drop-qci9totbyte
> Dropped Bytes Non-Std QCI | s8-uplnk-drop-othertotbyte
> SGW Statistics / S8 Total Data Statistics / Downlink | Pkts | s8-downlnk-packets
> Bytes | s8-downlnk-bytes
> Dropped Pkts | s8-downlnk-dropped-packets
> Dropped Bytes | s8-downlnk-dropped-bytes
> Pkts QCI 1 | s8-downlnk-qci1totpkt
> Pkts QCI 2 | s8-downlnk-qci2totpkt
> Pkts QCI 3 | s8-downlnk-qci3totpkt
> Pkts QCI 4 | s8-downlnk-qci4totpkt
> Pkts QCI 5 | s8-downlnk-qci5otpkt
> Pkts QCI 6 | s8-downlnk-qci6totpkt
> Pkts QCI 7 | s8-downlnk-qci7totpkt
> Pkts QCI 8 | s8-downlnk-qci8totpkt
> Pkts QCI 9 | s8-downlnk-qci9totpkt
> Pkts Non-Std QCI | s8-downlnk-othertotpkt
> Bytes QCI 1 | s8-downlnk-qci1totbyte
> Bytes QCI 2 | s8-downlnk-qci2totbyte
> Bytes QCI 3 | s8-downlnk-qci3totbyte
> Bytes QCI 4 | s8-downlnk-qci4totbyte
> Bytes QCI 5 | s8-downlnk-qci5totbyte
> Bytes QCI 6 | s8-downlnk-qci6totbyte
> Bytes QCI 7 | s8-downlnk-qci7totbyte
> Bytes QCI 8 | s8-downlnk-qci8totbyte
> Bytes QCI 9 | s8-downlnk-qci9totbyte
> Bytes Non-Std QCI | s8-downlnk-othertotbyte
> Dropped Pkts QCI 1 | s8-downlnk-drop-qci1totpkt
> Dropped Pkts QCI 2 | s8-downlnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s8-downlnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s8-downlnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s8-downlnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s8-downlnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s8-downlnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s8-downlnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s8-downlnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s8-downlnk-drop-otherpkt
> SGW Statistics / S8 Total Data Statistics / Downlink (count.) | Dropped Bytes QCI 1 | s8-downlnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s8-downlnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s8-downlnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s8-downlnk-drop-qci4totbyte
> Dropped Bytes QCI 5 | s8-downlnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s8-downlnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s8-downlnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s8-downlnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s8-downlnk-drop-qci9totbyte
> Dropped Bytes Non-Std QCI | s8-downlnk-drop-othertotbyte
> Dropped Pkts Non-Std QCI | s8-downlnk-drop-othertotpkt
> SGW Statistics / S5S8 Total Data Statistics / Uplink | Pkts | s5s8-uplnk-packets
> Bytes | s5s8-uplnk-bytes
> Dropped Pkts | s5s8-uplnk-dropped-packets
> Dropped Bytes | s5s8-uplnk-dropped-bytes
> Pkts QCI 1 | s5s8-uplnk-qci1totpkt
> Pkts QCI 2 | s5s8-uplnk-qci2totpkt
> Pkts QCI 3 | s5s8-uplnk-qci3totpkt
> Pkts QCI 4 | s5s8-uplnk-qci4totpkt
> Pkts QCI 5 | s5s8-uplnk-qci5totpkt
> Pkts QCI 6 | s5s8-uplnk-qci6totpkt
> Pkts QCI 7 | s5s8-uplnk-qci7totpkt
> Pkts QCI 8 | s5s8-uplnk-qci8totpkt
> Pkts QCI 9 | s5s8-uplnk-qci9totpkt
> Pkts Non-Std QCI | s5s8-uplnk-othertotpkt
> Bytes QCI 1 | s5s8-uplnk-qci1totbyte
> Bytes QCI 2 | s5s8-uplnk-qci1totbyte
> Bytes QCI 3 | s5s8-uplnk-qci1totbyte
> Bytes QCI 4 | s5s8-uplnk-qci1totbyte
> Bytes QCI 5 | s5s8-uplnk-qci1totbyte
> Bytes QCI 6 | s5s8-uplnk-qci1totbyte
> Bytes QCI 7 | s5s8-uplnk-qci1totbyte
> Bytes QCI 8 | s5s8-uplnk-qci1totbyte
> Bytes QCI 9 | s5s8-uplnk-qci1totbyte
> Bytes Non-Std QCI | s5s8-uplnk-othertotbyte
> Dropped Pkts QCI 1 | s5s8-uplnk-drop-qci1totpkt
> Dropped Pkts QCI 2 | s5s8-uplnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s5s8-uplnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s5s8-uplnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s5s8-uplnk-drop-qci5totpkt
> SGW Statistics / S5S8 Total Data Statistics / Uplink (con’t) | Dropped Pkts QCI 6 | s5s8-uplnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s5s8-uplnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s5s8-uplnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s5s8-uplnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s5s8-uplnk-drop-otherpkt
> Dropped Bytes QCI 1 | s5s8-uplnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s5s8-uplnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s5s8-uplnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s5s8-uplnk-drop-qcir4totbyte
> Dropped Bytes QCI 5 | s5s8-uplnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s5s8-uplnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s5s8-uplnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s5s8-uplnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s5s8-uplnk-drop-qci9totbyte
> Dropped Bytes Non-Std QCI | s5s8-uplnk-drop-othertotbyte
> SGW Statistics / S5S8 Total Data Statistics / Downlink | Pkts | s5s8-downlnk-packets
> Bytes | s5s8-downlnk-bytes
> Dropped Pkts | s5s8-downlnk-dropped-packets
> Dropped Bytes | s5s8-downlnk-dropped-bytes
> Pkts QCI 1 | s5s8-downlnk-qci1totpkt
> Pkts QCI 2 | s5s8-downlnk-qci2totpkt
> Pkts QCI 3 | s5s8-downlnk-qci3totpkt
> Pkts QCI 4 | s5s8-downlnk-qci4totpkt
> Pkts QCI 5 | s5s8-downlnk-qci5otpkt
> Pkts QCI 6 | s5s8-downlnk-qci6totpkt
> Pkts QCI 7 | s5s8-downlnk-qci7totpkt
> Pkts QCI 8 | s5s8-downlnk-qci8totpkt
> Pkts QCI 9 | s5s8-downlnk-qci9totpkt
> Pkts Non-Std QCI | s5s8-downlnk-othertotpkt
> Bytes QCI 1 | s5s8-downlnk-qci1totbyte
> Bytes QCI 2 | s5s8-downlnk-qci2totbyte
> Bytes QCI 3 | s5s8-downlnk-qci3totbyte
> Bytes QCI 4 | s5s8-downlnk-qci4totbyte
> Bytes QCI 5 | s5s8-downlnk-qci5totbyte
> Bytes QCI 6 | s5s8-downlnk-qci6totbyte
> Bytes QCI 7 | s5s8-downlnk-qci7totbyte
> Bytes QCI 8 | s5s8-downlnk-qci8totbyte
> Bytes QCI 9 | s5s8-downlnk-qci9totbyte
> Bytes Non-Std QCI | s5s8-downlnk-othertotbyte
> Dropped Pkts QCI 1 | s5s8-downlnk-drop-qci1totpkt
> SGW Statistics / S5S8 Total Data Statistics / Downlink (con’t) | Dropped Pkts QCI 2 | s5s8-downlnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s5s8-downlnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s5s8-downlnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s5s8-downlnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s5s8-downlnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s5s8-downlnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s5s8-downlnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s5s8-downlnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s5s8-downlnk-drop-otherpkt
> Dropped Bytes QCI 1 | s5s8-downlnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s5s8-downlnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s5s8-downlnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s5s8-downlnk-drop-qci4totbyte
> Dropped Bytes QCI 5 | s5s8-downlnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s5s8-downlnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s5s8-downlnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s5s8-downlnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s5s8-downlnk-drop-qci9totbyte
> Dropped Bytes Non-Std QCI | s5s8-downlnk-drop-othertotbyte
> Dropped Pkts Non-Std QCI | s5s8-downlnk-drop-othertotpkt
> SGW Statistics / S12 Total Data Statistics / Uplink | Pkts | s12-uplnk-packets
> Bytes | s12-uplnk-bytes
> Dropped Pkts | s12-uplnk-dropped-packets
> Dropped Bytes | s12-uplnk-dropped-bytes
> Pkts QCI 1 | s12-uplnk-qci1totpkt
> Pkts QCI 2 | s12-uplnk-qci2totpkt
> Pkts QCI 3 | s12-uplnk-qci3totpkt
> Pkts QCI 4 | s12-uplnk-qci4totpkt
> Pkts QCI 5 | s12-uplnk-qci5totpkt
> Pkts QCI 6 | s12-uplnk-qci6totpkt
> Pkts QCI 7 | s12-uplnk-qci7totpkt
> Pkts QCI 8 | s12-uplnk-qci8totpkt
> Pkts QCI 9 | s12-uplnk-qci9totpkt
> Pkts Non-Std QCI | s12-uplnk-othertotpkt
> Bytes QCI 1 | s12-uplnk-qci1totbyte
> Bytes QCI 2 | s12-uplnk-qci1totbyte
> Bytes QCI 3 | s12-uplnk-qci1totbyte
> Bytes QCI 4 | s12-uplnk-qci1totbyte
> Bytes QCI 5 | s12-uplnk-qci1totbyte
> SGW Statistics / S12 Total Data Statistics / Uplink (con’t) | Bytes QCI 6 | s12-uplnk-qci1totbyte
> Bytes QCI 7 | s12-uplnk-qci1totbyte
> Bytes QCI 8 | s12-uplnk-qci1totbyte
> Bytes QCI 9 | s12-uplnk-qci1totbyte
> Bytes Non-Std QCI | s12-uplnk-othertotbyte
> Dropped Pkts QCI 1 | s12-uplnk-drop-qci1totpkt
> Dropped Pkts QCI 2 | s12-uplnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s12-uplnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s12-uplnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s12-uplnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s12-uplnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s12-uplnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s12-uplnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s12-uplnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s12-uplnk-drop-otherpkt
> Dropped Bytes QCI 1 | s12-uplnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s12-uplnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s12-uplnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s12-uplnk-drop-qcir4totbyte
> Dropped Bytes QCI 5 | s12-uplnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s12-uplnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s12-uplnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s12-uplnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s12-uplnk-drop-qci9totbyte
> Dropped Bytes Non-Std QCI | s12-uplnk-drop-othertotbyte
> SGW Statistics / S12 Total Data Statistics / Downlink | Pkts | s12-downlnk-packets
> Bytes | s12-downlnk-bytes
> Dropped Pkts | s12-downlnk-dropped-packets
> Dropped Bytes | s12-downlnk-dropped-bytes
> Pkts QCI 1 | s12-downlnk-qci1totpkt
> Pkts QCI 2 | s12-downlnk-qci2totpkt
> Pkts QCI 3 | s12-downlnk-qci3totpkt
> Pkts QCI 4 | s12-downlnk-qci4totpkt
> Pkts QCI 5 | s12-downlnk-qci5otpkt
> Pkts QCI 6 | s12-downlnk-qci6totpkt
> Pkts QCI 7 | s12-downlnk-qci7totpkt
> Pkts QCI 8 | s12-downlnk-qci8totpkt
> Pkts QCI 9 | s12-downlnk-qci9totpkt
> Pkts Non-Std QCI | s12-downlnk-othertotpkt
> SGW Statistics / S12 Total Data Statistics / Downlink (con’t) | Bytes QCI 1 | s12-downlnk-qci1totbyte
> Bytes QCI 2 | s12-downlnk-qci2totbyte
> Bytes QCI 3 | s12-downlnk-qci3totbyte
> Bytes QCI 4 | s12-downlnk-qci4totbyte
> Bytes QCI 5 | s12-downlnk-qci5totbyte
> Bytes QCI 6 | s12-downlnk-qci6totbyte
> Bytes QCI 7 | s12-downlnk-qci7totbyte
> Bytes QCI 8 | s12-downlnk-qci8totbyte
> Bytes QCI 9 | s12-downlnk-qci9totbyte
> Bytes Non-Std QCI | s12-downlnk-othertotbyte
> Dropped Pkts QCI 1 | s12-downlnk-drop-qci1totpkt
> Dropped Pkts QCI 2 | s12-downlnk-drop-qci2totpkt
> Dropped Pkts QCI 3 | s12-downlnk-drop-qci3totpkt
> Dropped Pkts QCI 4 | s12-downlnk-drop-qci4totpkt
> Dropped Pkts QCI 5 | s12-downlnk-drop-qci5totpkt
> Dropped Pkts QCI 6 | s12-downlnk-drop-qci6totpkt
> Dropped Pkts QCI 7 | s12-downlnk-drop-qci7totpkt
> Dropped Pkts QCI 8 | s12-downlnk-drop-qci8totpkt
> Dropped Pkts QCI 9 | s12-downlnk-drop-qci9totpkt
> Dropped Pkts Non-Std QCI | s12-downlnk-drop-otherpkt
> Dropped Bytes QCI 1 | s12-downlnk-drop-qci1totbyte
> Dropped Bytes QCI 2 | s12-downlnk-drop-qci2totbyte
> Dropped Bytes QCI 3 | s12-downlnk-drop-qci3totbyte
> Dropped Bytes QCI 4 | s12-downlnk-drop-qci4totbyte
> Dropped Bytes QCI 5 | s12-downlnk-drop-qci5totbyte
> Dropped Bytes QCI 6 | s12-downlnk-drop-qci6totbyte
> Dropped Bytes QCI 7 | s12-downlnk-drop-qci7totbyte
> Dropped Bytes QCI 8 | s12-downlnk-drop-qci8totbyte
> Dropped Bytes QCI 9 | s12-downlnk-drop-qci9totbyte
> Dropped Bytes Non-Std QCI | s12-downlnk-drop-othertotbyte
> Dropped Pkts Non-Std QCI | s12-downlnk-drop-othertotpkt

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> ECS Bulk Statistic Enhancements
> The following bulk statistics were added to the ECS schema in WEM Release 12.0.
> .

> ECS Bulk Statistic Enhancements in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> ECS Statistics / TFTP | Total TFTP Flows | tftp-flows
> Total Uplink Bytes | tftp-uplk-bytes
> Total Uplink Packets | tftp-uplk-pkts
> Total Downlink Bytes | tftp-dwnlk-bytes
> Total Downlink Packets | tftp-dwnlk-pkts
> Total Read Sessions | tftp-total-read-sessions
> Total Write Sessions | tftp-total-write-sessions
> Total Packets with Unknown Request Type | tftp-unsupp-req-pkts
> Total Invalid Control Packets | tftp-invalid-ctrl-pkts
> Total Invalid Data Packets | tftp-invalid-data-pkts
> Uplink Data Bytes | tftp-data-uplk-bytes
> Downlink Data Bytes | tftp-data-dwnlk-bytes
> Uplink Data Pkts | tftp-data-uplk-pkts
> Downlink Data Pkts | tftp-data-dwnlk-pkts

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> Changes in Data Values to HNBGW SCTP Schema Bulk Statistics
> The following HNBGW SCTP bulk statistics data values have been changed from Int32 to Int64 to accommodate the potential value of the statistics.

> HNBGW SCTP Bulk Statistic Schema Data Values Changed to Int64 in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> HNBGW SCTP Statistics / SCTP | Total Bytes Sent To Lower Layer | total-bytes-sent-to-lower-layer
> Total Bytes Received From Lower Layer | total-bytes-rcvd-from-lower-layer
> Total Packets Sent To Lower Layer | total-packets-sent-to-lower-layer
> Total Packets Received From Lower Layer | total-packets-rcvd-from-lower-layer
> HNBGW SCTP Statistics / SCTP / Transmitted SCTP Data | Init Chunks | trans-sctp-data-init-chunks
> Init Ack Chunks | trans-sctp-data-init-ack-chunks
> Shutdown Chunks | trans-sctp-data-shutdown-chunks
> Shutdown Ack Chunks | trans-sctp-data-shutdown-ack-chunks
> Cookie Chunks | trans-sctp-data-cookie-chunks
> Cookie Ack Chunks | trans-sctp-data-cookie-ack-chunks
> Data Chunks | trans-sctp-data-data-chunks
> Data Ack Chunks | trans-sctp-data-data-ack-chunks
> Shutdown Complete Chunks | trans-sctp-data-shutdown-comp-chunks
> HNBGW SCTP Statistics / SCTP / Transmitted SCTP Data (con’t) | Heartbeat Chunks | trans-sctp-data-heartbeat-chunks
> HeartBeat Ack Chunks | trans-sctp-data-heartbeat-chunks
> Abort Chunks | trans-sctp-data-abort-chunks
> Error Chunks | trans-sctp-data-error-chunks
> HNBGW SCTP Statistics / Received SCTP Data | Init Chunks | rcvd-sctp-data-init-chunks
> Init Ack Chunks | rcvd-sctp-data-init-ack-chunks
> Shutdown Chunks | rcvd-sctp-data-shutdown-chunks
> Shutdown Ack Chunks | rcvd-sctp-data-shutdown-ack-chunks
> Cookie Chunks | rcvd-sctp-data-cookie-chunks
> Cookie Ack Chunks | rcvd-sctp-data-cookie-ack-chunks
> Data Chunks | rcvd-sctp-data-data-chunks
> Data Ack Chunks | rcvd-sctp-data-data-chunks
> Shutdown Complete Chunks | rcvd-sctp-data-shutdown-comp-chunks
> Heartbeat Chunks | rcvd-sctp-data-heartbeat-chunks
> HeartBeat Ack Chunks | rcvd-sctp-data-heartbeat-ack-chunks
> Abort Chunks | rcvd-sctp-data-abort-chunks
> Error Chunks | rcvd-sctp-data-error-chunks
> HNBGW SCTP Statistics / Retransmitted SCTP Data | Init Chunks | retrans-sctp-data-init-chunks
> Shutdown Chunks | retrans-sctp-data-shutdown-chunks
> Shutdown Ack Chunks | retrans-sctp-data-shutdown-ack-chunks
> Data Chunks | retrans-sctp-data-data-chunks
> Cookie Chunks | retrans-sctp-data-cookie-chunks

> Web Element Manager Path
> On the WEM server: <ems_dir>/server/bsschema/hnbgw_sctp_counter.xml
> Changes in Data Values to HNBGW RTP Schema Bulk Statistics
> The following HNBGW RTP bulk statistics data values have been changed from Int32 to Int64 to accommodate the potential value of the statistics.

> HNBGW RTP Bulk Statistic Schema Data Values Changed to Int64 in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> HNBGW RTP Statistics / RTP | RTP Uplink Packets Rx | rtp-uplink-pkts-rx
> RTP Uplink Bytes Rx | rtp-uplink-byts-rx
> RTP Uplink Packets dropped | rtp-uplink-pkts-dropped
> RTP Uplink Bytes dropped | rtp-uplink-byts-dropped
> RTP Downlink Packets Tx | rtp-downlink-pkts-tx
> RTP Downlink Bytes Tx | rtp-downlink-byts-tx
> HNBGW RTP Statistics / RTP / RTP Uplink Packets Drop Cause | RAB not in CONNECTED state | rtp-uplink-pkts-drop-rab_not-in_conn_state
> Miscellaneous | rtp-uplink-pkts-dropped-misc
> HNBGW RTP Statistics / RTP / RTP Uplink Bytes Drop Cause | RAB not in CONNECTED state | rtp-uplink-byts-drop-rab_not-in_conn_state
> Miscellaneous | rtp-uplink-byts-dropped-misc
> HNBGW RTP Statistics / RTP / RTCP | Sender Report Rx (From HNB) | rtcp-sender-report-rx
> RTCP Sender Report Tx (To HNB) | rtcp-sender-report-tx
> RTCP SDES Report Rx (From HNB) | rtcp-sdes-report-rx
> RTCP SDES Report Tx (To HNB) | rtcp-sdes-report-tx
> RTCP BYE Report Rx (From HNB) | rtcp-bye-report-rx
> RTCP APP Report Tx (From HNB) | rtcp-app-report-rx
> RTCP Uplink Packets Rx | rtcp-uplink-pkts-rx
> RTCP Uplink Bytes Rx | rtcp-uplink-byts-rx
> RTCP Uplink Packets dropped | rtcp-uplink-pkts-dropped
> RTCP Uplink Bytes dropped | rtcp-uplink-pkts-dropped
> RTCP Downlink Packets Tx | rtcp-downlink-pkts-tx
> RTCP Downlink Bytes Tx | rtcp-downlink-byts-tx
> HNBGW RTP Statistics / RTP / RTCP / Uplink Packets Drop Cause | RAB not in CONNECTED state | rtcp-uplink-pkts-drop-rab_not-in_conn_state
> Miscellaneous | rtcp-uplink-pkts-dropped-misc
> HNBGW RTP Statistics / RTP-MUX | RTP-MUX Uplink Packets Rx | rtp-mux-uplink-pkts-rx
> RTP-MUX Uplink Packets dropped | rtp-mux-uplink-pkts-dropped
> RTP-MUX Uplink Bytes Rx | rtp-mux-uplink-byts-rx
> RTP-MUX Uplink Bytes dropped | rtp-mux-uplink-byts-dropped
> RTP-MUX RTP Stream Received | rtp-mux-rtp-stream-rcvd
> RTP-MUX RTP Stream Dropped | rtp-mux-rtp-stream-dropped
> HNBGW RTP Statistics / RTP-MUX / RTP-MUX Uplink Packets Drop Cause | Miscellaneous | rtp-mux-uplink-pkts-dropped-misc
> HNBGW RTP Statistics / RTP-MUX / RTP-MUX Uplink Bytes Drop Cause | Miscellaneous | rtp-mux-uplink-byts-dropped-misc
> HNBGW RTP Statistics / RTP-MUX / RTP-MUX Stream Drop Cause | Miscellaneous | rtp-mux-rtp-stream-dropped-misc

> Web Element Manager Path
> On the WEM server: <ems_dir>/server/bsschema/hnbgw_rtp_counter.xml.
> Changes in Data Values to CS NW RTP Schema Bulk Statistics
> The following CS NW RTP bulk statistics data values have been changed from Int32 to Int64 to accommodate the potential value of the statistics.

> CS NW RTP Schema Bulk Statistics Data Values Changed to Int64 in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> CS NW RTP Statistics / RTP | RTP Uplink Packets Tx | rtp-uplink-pkts-tx
> RTP Uplink Bytes Tx | rtp-uplink-byts-tx
> RTP Downlink Packets Rx | rtp-downlink-pkts-rx
> RTP Downlink Bytes Rx | rtp-downlink-byts-rx
> RTP Downlink Packets dropped | rtp-downlink-pkts-dropped
> RTP Downlink Bytes dropped | rtp-downlink-byts-dropped
> CS NW RTP Statistics / RTP / Downlink Packets Drop Cause | RAB not in CONNECTED state | rtp-downlink-pkts-drop-rab_not-in_conn_state
> Miscellaneous | rtp-downlink-pkts-drop-misc
> CS NW RTP Statistics / RTP / Downlink Bytes Drop Cause | RAB not in CONNETED state | rtp-downlink-byts-drop-rab_not-in_conn_state
> Miscellaneous | rtp-downlink-byts-drop-misc
> CS NW RTP Statistics / RTPC | RTCP Uplink Packets Tx | rtcp-uplink-pkts-tx
> RTCP Uplink Bytes Tx | rtcp-uplink-byts-tx
> RTCP Downlink Packets Rx | rtcp-downlink-pkts-rx
> RTCP Downlink Bytes Rx | rtcp-downlink-byts-rx
> RTCP Downlink Packets dropped | rtcp-downlink-pkts-dropped
> RTCP Downlink Bytes dropped | rtcp-downlink-byts-dropped
> CS NW RTP Statistics / RTPC / RTPC Downlink Packets Drop Cause | RAB not in CONNECTED state | rtcp-downlink-pkts-drop-rab_not-in_conn_state
> Miscellaneous | rtcp-downlink-pkts-drop-misc
> CS NW RTP Statistics / RTPC / RTPC Downlink Bytes Drop Cause | RAB not in CONNECTED state | rtcp-downlink-byts-drop-rab_not-in_conn_state
> Miscellaneous | rtcp-downlink-byts-drop-misc

> Web Element Manager Path
> On the WEM server: <ems_dir>/server/bsschema/cs_nw_rtp_counter.xml
> Changes in Data Values to AAL2 Schema Bulk Statistics
> The following AAL2 bulk statistics data values have been changed from Int32 to Int64 to accommodate the potential value of the statistics.

> AAL2 Bulk Statistic Schema Values Changed to Data Value Int64 in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> AAL2 Statistics / AAL2 | AAL2 Uplink Packets Tx | uplink-pkts-tx
> AAL2 Uplink Bytes Tx | uplink-byts-tx
> AAL2 Downlink Packets Rx | downlink-pkts-rx
> AAL2 Downlink Bytes Rx | downlink-byts-rx
> AAL2 Downlink Packets dropped | downlink-pkts-dropped
> AAL2 Downlink Bytes dropped | downlink-byts-dropped
> AAL2 Statistics / AAL2 / AAL2 Downlink Packets Drop Cause | RAB not in CONNECTED state | downlink-pkts-drop-rab-not-in-conn-state
> Miscellaneous | downlink-pkts-drop-cause-misc
> AAL2 Statistics / AAL2 / AAL2 Downlink Bytes Drop Cause | RAB not in CONNECTED state | downlink-byts-drop-rab-not-in-conn-state
> Miscellaneous | downlink-byts-drop-cause-misc

> Web Element Manager Path
> On the WEM server: <ems_dir>/server/bsschema/aal2_counter.xml
> Changes in Data Values to MME Schema Bulk Statistics
> The following mme bulk statistics data values have been changed from Incremental to Gauge.

> MME Bulk Statistic Schema Values Changed to Gauge in WEM Release 12.0
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> MME Statistics | Attached Calls | emmcall-attach-currcall
> Maximum Calls | emmcall-attach-maxcall
> Current Calls | emmcall-connect-curcall
> Maximum Calls | emmcall-connect-maxcall
> Current Calls | emmcall-idle-curcall
> Maximum Calls | emmcall-idle-maxcall

> Web Element Manager Path
> On the WEM server: <ems_dir>/server/bsschema/mme_counter.xml
> New Bulkstatistic Schemas
> The following Schemas can be found in the XML files on the WEM server:

> l | ENAPP

> l | Misc_for_EMS

> l | PDG

> l | PROFAPP

> l | SHAPP

> Web Element Manager Path
> On the WEM server: <ems_dir>/server/bsschema/<schema name>
> For counter descriptions, refer to the latest edition of the Bulkstatistics and Counters guide.
> Web Element Manager Accounting Enhancements in Release 12.2
> The following WEM Accounting enhancements were made for Release 12.2.
> Enhancements to View/Graph Bulk Statistics Feature
> Previously, the Bulk Statistics Graphing feature allowed the user to view only 20 data sample points per page. This required the user to click to a second page if the number of data points exceeded 20.
> The Bulk Statistics Graphing feature has been enhanced to allow the user to zoom in or out to view as few or as many graph data samplings on a single page. By providing a zoom a mechanism for viewing a large number of data samples on a single screen, users can more effective analyze the trend shown in the graph.
> The slider mechanism is just below the graph display. By moving the slider control to the left or right, the user can decrease or increase the number of data samples shown.
> Above the graph display, there are discrete zoom controls that allow the user to click to see one of the following graph views:

> l | 1hr: Display all data samples for a one-hour period.

> l | 3hr: Display all data samples for a three-hour period.

> l | 6hr: Display all data samples for a six-hour period.

> l | Max: Display all available data samples

> IMPORTANT: The existing X-scale, X-scroll and Y-scale functionality have been replaced by the zoom in/zoom out feature. In addition, the Page size label has been removed, as the new zoom feature eliminates the need to view a graph over multiple pages.
> Web Element Manager Path

> l | Accounting | View/Graph Bulk Statistics

> GTPC Bulk Statistic Schema Support
> GTPC schema bulk statistics support is now available in WEM.
> Web Element Manager Path
> Accounting Menu | Bulk Statistics Configuration | Bulk Statistics Dialog Box | Bulk Statistics Configuration Dialog Box - Schema Tab
> System Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the System schema in WEM Release 12.2.

> System Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> System Schema / ASNGW Managers | Service Flow Information | asngw-sfs
> TID Failures | asngw-tidfail
> System Schema / Session Disconnect Reasons | sgsn-egtpc-connection-failed | disc-reason-438
> sgsn-egtpc-create-session-failed | disc-reason-439
> sgsn-hss-detach | disc-reason-440
> sgsn-hss-connection-failure | disc-reason-441
> sgsn-pgw-detach | disc-reason-442
> sgsn-s5-not-supported-for-apn | disc-reason-443
> sgsn-no-rab-for-gbr-bearer | disc-reason-444
> sgsn-sgw-selection-failure | disc-reason-445
> sgsn-pgw-selection-failure | disc-reason-446
> wimax-hotlining-status-change | disc-reason-447
> ggsn-no-rsp-from-sgsn | disc-reason-448
> diameter-protocol-error | disc-reason-449
> diameter-request-timeout | disc-reason-450
> operator-policy | disc-reason-451
> spr-connection-error | disc-reason-452
> mipha-dup-wimax-session | disc-reason-453
> invalid-version-attr | disc-reason-454
> sgsn-zone-code-failure | disc-reason-455/
> invalid-qci | disc-reason-456
> no_rules | disc-reason-457
> sgsn-rnc-no-dual-pdp-init-pdp-deact | disc-reason-458
> mme-init-ctxt-setup-failure | disc-reason-459
> System Schema / Session Disconnect Reasons (con’t) | mme-driver-initiated | disc-reason-460
> mme-s1ap-connection-down | disc-reason-461
> mme-s1ap-reset-recd | disc-reason-462
> mme-s6a-response-timeout | disc-reason-463
> mme-s13-response-timeout | disc-reason-464
> mme-Illegal-equipment | disc-reason-465
> mme-unexpected-attach | disc-reason-466
> mme-sgw-selection-failure | disc-reason-467
> mme-pgw-selection-failure | disc-reason-468
> mme-reselection-to-sgsn | disc-reason-469
> mme-relocation-to-sgsn | disc-reason-470
> mme-reselection-to-mm | disc-reason-471
> mme-relocation-to-mme | disc-reason-472
> mme-tau-attach-collision | disc-reason-473
> mme-old-sgsn-resolution-failure | disc-reason-474
> mme-old-mme-resolution-failure | disc-reason-475
> mme-reloc-ho-notify-timeout | disc-reason-476
> mme-reloc-ho-req-ack-timeout | disc-reason-477
> mme-create-session-timeout | disc-reason-478
> mme-create-session-failure | disc-reason-479
> mme-s11-path-failure | disc-reason-480
> mme-policy-no-ue-irat | disc-reason-481
> mme-x2-handover-failed | disc-reason-482
> mme-attach-restrict | disc-reason-483
> mme-regional-zone-code | disc-reason-484
> mme-no-response-from-ue | disc-reason-485
> mme-sgw-relocation-failed | disc-reason-486
> mme-implicit-detach | disc-reason-487
> sgsn-detach-notify | disc-reason-488
> emergency-inactivity-timeout | disc-reason-489
> policy-initiated-release | disc-reason-490
> gy-result-code-system-failure | disc-reason-491
> mme-zone-code-validation-failed | disc-reason-492
> System Statistics / CC Update Reporting Reason Statistics | TITSU Time | cc-upd-titsutime
> System Statistics / CCA Initial Message Stats | Result Code 2001 | cca-init-2001-rc
> Result Code 4011 | cca-init-4011-rc
> Result Code 4012 | cca-init-4012-rc
> Result Code 5003 | cca-init-5003-rc
> System Statistics / CCA Update Message Stats | Result Code 2001 | cca-updt-2001-rc
> Result Code 4011 | cca-updt-4011-rc
> Result Code 4012 | cca-updt-4012-rc
> Result Code 5003 | cca-updt-5003-rc
> System Statistics / Failure Handling Stats | Action-Continue | fail-action-contd
> Action-Terminated | fail-action-term
> System Statistics / Miscellaneous | NPU Flow - Usage | npu-capacity-usage
> NPU Flow - Effective | npu-capacity
> Session Information - Capacity Usage | session-capacity-usage
> System Capacity Usage | system-capacity-usage
> Session Information - Capacity | session-capacity
> System Statistics / Number of Active Sessions | PDSN | pdsn-activdata
> HSGW | hsgw-activdata
> ASNGW | asngw-activdata
> HA | ha-activedata
> MME | mme-activedata
> PGW | pgw-activedata
> SGW | sgw-activedata
> System Statistics / LTE Node Tunnels Statistics | Total IPsec Manager Death Notifications | ipsecctrl-lte-ipsecmgr-death-notif
> Total Crypto Maps Delete Requests | ipsecctrl-lte-map-del-reqs
> Total Crypto Maps Established | ipsecctrl-lte-map-est
> Total Crypto Maps Failed | ipsecctrl-lte-map-failed
> Total Crypto Map Requests | ipsecctrl-lte-map-reqs
> Total Crypto Maps State Change Notifications Sent | ipsecctrl-lte-map-state-notif
> Total Crypto Maps with QoS | ipsecctrl-lte-qos-maps
> Total Service Template Requests | ipsecctrl-lte-template-reqs
> Total Service Template Unregister Requests | ipsecctrl-lte-template-unreg-reqs

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> SGW Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the SGW schema in WEM Release 12.2.

> SGW Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> SGW Statistics / S1U Total Data Statistics / Downlink | Dropped Bytes Non-Std QCI | datastat-downlink-dropstat-othertotbyte
> Dropped Pkts Non-Std QCI | datastat-downlink-dropstat-othertotpkt
> Dropped Bytes QCI1 | datastat-downlink-dropstat-qci1totbyte
> Dropped Pkts QCI1 | datastat-downlink-dropstat-qci1totpkt
> Dropped Bytes QCI2 | datastat-downlink-dropstat-qci2totbyte
> Dropped Pkts QCI2 | datastat-downlink-dropstat-qci2totpkt
> Dropped Bytes QCI3 | datastat-downlink-dropstat-qci3totbyte
> Dropped Pkts QCI3 | datastat-downlink-dropstat-qci3totpkt
> Dropped Bytes QCI4 | datastat-downlink-dropstat-qci4totbyte
> Dropped Pkts QCI4 | datastat-downlink-dropstat-qci4totpkt
> Dropped Bytes QCI5 | datastat-downlink-dropstat-qci5totbyte
> Dropped Pkts QCI5 | datastat-downlink-dropstat-qci5totpkt
> Dropped Bytes QCI6 | datastat-downlink-dropstat-qci6totbyte
> Dropped Pkts QCI6 | datastat-downlink-dropstat-qci6totpkt
> Dropped Bytes QCI7 | datastat-downlink-dropstat-qci7totbyte
> Dropped Pkts QCI7 | datastat-downlink-dropstat-qci7totpkt
> Dropped Bytes QCI8 | datastat-downlink-dropstat-qci8totbyte
> Dropped Pkts QCI8 | datastat-downlink-dropstat-qci8totpkt
> Dropped Bytes QCI9 | datastat-downlink-dropstat-qci9totbyte
> Dropped Pkts QCI9 | datastat-downlink-dropstat-qci9totpkt
> Bytes Non-Std QCI | datastat-downlink-othertotbyte
> Pkts Non-Std QCI | datastat-downlink-othertotpkt
> Bytes QCI 1 | datastat-downlink-qci1totbyte
> Pkts QCI 1 | datastat-downlink-qci1totpkt
> Bytes QCI 2 | datastat-downlink-qci2totbyte
> Pkts QCI 2 | datastat-downlink-qci2totpkt
> Bytes QCI 3 | datastat-downlink-qci3totbyte
> Pkts QCI 3 | datastat-downlink-qci3totpkt
> Bytes QCI 4 | datastat-downlink-qci4totbyte
> Pkts QCI 4 | datastat-downlink-qci4totpkt
> Bytes QCI 5 | datastat-downlink-qci5totbyte
> Pkts QCI 5 | datastat-downlink-qci5totpkt
> Bytes QCI 6 | datastat-downlink-qci6totbyte
> Pkts QCI 6 | datastat-downlink-qci6totpkt
> Bytes QCI 7 | datastat-downlink-qci7totbyte
> Pkts QCI 7 | datastat-downlink-qci7totpkt
> Bytes QCI 8 | datastat-downlink-qci8totbyte
> Pkts QCI 8 | datastat-downlink-qci8totpkt
> SGW Statistics / S1U Total Data Statistics / Downlink (con’t) | Bytes QCI 9 | datastat-downlink-qci9totbyte
> Pkts QCI 9 | datastat-downlink-qci9totpkt
> Dropped Pkts Non-Std QCI | s1u-downlnk-drop-othertotpkt
> SGW Statistics / S1U Total Data Statistics / Uplink | Pkts Non-Std QCI | datastat-uplink-dropstat-othertotpkt
> Dropped Bytes QCI 1 | datastat-uplink-dropstat-qci1totbyte
> Dropped Pkts QCI 1 | datastat-uplink-dropstat-qci1totpkt
> Dropped Bytes QCI 2 | datastat-uplink-dropstat-qci2totbyte
> Dropped Pkts QCI 2 | datastat-uplink-dropstat-qci2totpkt
> Dropped Bytes QCI 3 | datastat-uplink-dropstat-qci3totbyte
> Dropped Pkts QCI 3 | datastat-uplink-dropstat-qci3totpkt
> Dropped Bytes QCI 4 | datastat-uplink-dropstat-qci4totbyte
> Dropped Pkts QCI 4 | datastat-uplink-dropstat-qci4totpkt
> Dropped Bytes QCI 5 | datastat-uplink-dropstat-qci5totbyte
> Dropped Pkts QCI 5 | datastat-uplink-dropstat-qci5totpkt
> Dropped Bytes QCI 6 | datastat-uplink-dropstat-qci6totbyte
> Dropped Pkts QCI 6 | datastat-uplink-dropstat-qci6totpkt
> Dropped Bytes QCI 7 | datastat-uplink-dropstat-qci7totbyte
> Dropped Pkts QCI 7 | datastat-uplink-dropstat-qci7totpkt
> Dropped Bytes QCI 8 | datastat-uplink-dropstat-qci8totbyte
> Dropped Pkts QCI 8 | datastat-uplink-dropstat-qci8totpkt
> Dropped Bytes QCI 9 | datastat-uplink-dropstat-qci9totbyte
> Dropped Pkts QCI 9 | datastat-uplink-dropstat-qci9totpkt
> Bytes Non-Std QCI | datastat-uplink-othertotbyte
> Pkts Non-Std QCI | datastat-uplink-othertotpkt
> Bytes QCI 1 | datastat-uplink-qci1totbyte
> Pkts QCI 1 | datastat-uplink-qci1totpkt
> Bytes QCI 2 | datastat-uplink-qci2totbyte
> Pkts QCI 2 | datastat-uplink-qci2totpkt
> Bytes QCI 3 | datastat-uplink-qci3totbyte
> Pkts QCI 3 | datastat-uplink-qci3totpkt
> Bytes QCI 4 | datastat-uplink-qci4totbyte
> Pkts QCI 4 | datastat-uplink-qci4totpkt
> Bytes QCI 5 | datastat-uplink-qci5totbyte
> Pkts QCI 5 | datastat-uplink-qci5totpkt
> Bytes QCI 6 | datastat-uplink-qci6totbyte
> Pkts QCI 6 | datastat-uplink-qci6totpkt
> Bytes QCI 7 | datastat-uplink-qci7totbyte
> SGW Statistics / S1U Total Data Statistics / Uplink (con’t) | Pkts QCI 7 | datastat-uplink-qci7totpkt
> Bytes QCI 8 | datastat-uplink-qci8totbyte
> Pkts QCI 8 | datastat-uplink-qci8totpkt
> Bytes QCI 9 | datastat-uplink-qci9totbyte
> Pkts QCI 9 | datastat-uplink-qci9totpkt
> SGW Statistics / S1U Total Data Statistics / Intra-SGW Handover Statistics | Intra-MME | intrasgwhaovstat-intramme
> Inter-MME | intrasgwhaovstat-intermme
> SGW Statistics / Inter-SGW Handover Statistics / Inter System | Inter System (directory) | intersgwhaovstat-intersystem
> Success | intersgwhaovstat-intersystem-success
> Fail | intersgwhaovstat-intersystem-fail
> SGW Statistics / Intra-SGW Handover Statistics | Inter-MME (directory) | intrasgwhaovstat-intermme
> Success | intrasgwhaovstat-intermme-success
> Fail | intrasgwhaovstat-intermme-fail
> Intra-MME (directory) | intrasgwhaovstat-intramme
> Success | intrasgwhaovstat-intramme-success
> Fail | intrasgwhaovstat-intramme-fail
> SGW Statistics / PDN PLM Statistics / Home PDNs | PDNs active | plmnstat-home-pdn-active
> PDNs released | plmnstat-home-pdn-released
> PDNs setup | plmnstat-home-pdn-setup
> SGW Statistics / PDN PLM Statistics / Roaming PDNs | PDNs active | plmnstat-roam-pdn-active
> PDNs setup | plmnstat-roam-pdn-setup
> PDNs released | plmnstat-roam-pdn-released
> SGW Statistics / PDN PLM Statistics / Visiting PDNs | PDNs active | plmnstat-vist-pdn-active
> PDNs setup | plmnstat-vist-pdn-setup
> PDNs released | plmnstat-vist-pdn-released
> SGW Statistics / S12 Total Data Statistics / Downlink | Dropped Pkts Non-Std QCI | s12-downlnk-drop-othertotpkt
> SGW Statistics / S4U Total Data Statistics / Downlink | Dropped Pkts Non-Std QCI | s4u-downlnk-drop-othertotpkt
> SGW Statistics / S5 Total Data Statistics / Downlink | Dropped Pkts Non-Std QCI | s5-downlnk-drop-othertotpkt
> SGW Statistics / S5S8 Total Data Statistics / Downlink | Dropped Pkts Non-Std QCI | s5s8-downlnk-drop-othertotpkt
> SGW Statistics / S8 Total Data Statistics / Downlink | Dropped Pkts Non-Std QCI | s8-downlnk-drop-othertotpkt
> SGW Statistics / Source Violation | Packets Dropped | srcviolatestat-packets-dropped
> Bytes Dropped | srcviolatestat-bytes-dropped

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> PGW Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the PGW schema in WEM Release 12.2.

> PGW Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> PGW Schema / Subscriber Session Statistics / Total Bearers Active / Default Bearers | Emergency | sessstat-bearact-emergency-def
> Authentic IMSI | sessstat-bearact-emergency-auth-imsi-def
> Un-Authentic IMSI | sessstat-bearact-emergency-unauth-imsi-def
> Only IMEI | sessstat-bearact-emergency-only-imei-def
> PGW Schema / Subscriber Session Statistics / Total Bearers Active / Dedicated Bearers | Emergency | sessstat-bearact-emergency-ded
> Authentic IMSI | sessstat-bearact-emergency-auth-imsi-ded
> Un-Authentic IMSI | sessstat-bearact-emergency-unauth-imsi-ded
> Only IMEI | sessstat-bearact-emergency-only-imei-ded
> PGW Schema / Subscriber Session Statistics / Total Bearers Setup / Default Bearers | Emergency | sessstat-bearsetup-emergency-def
> Authentic IMSI | sessstat-bearsetup-emergency-auth-imsi-def
> Only IMEI | sessstat-bearsetup-emergency-only-imei-def
> Un-Authentic IMSI | sessstat-bearsetup-emergency-unauth-imsi-def
> PGW Schema / Subscriber Session Statistics / Total Bearers Setup / Dedicated Bearers | UE-Initiated | sessstat-bearsetup-ue-init-ded
> Network-Initiated | sessstat-bearsetup-nw-init-ded
> Emergency | sessstat-bearsetup-emergency-ded
> Authentic IMSI | sessstat-bearsetup-emergency-auth-imsi-ded
> Only IMEI | sessstat-bearsetup-emergency-only-imei-ded
> Un-Authentic IMSI | sessstat-bearsetup-emergency-unauth-imsi-ded
> PGW Schema / Subscriber Session Statistics / Total Bearers Rejected / Default Bearers | Total Emergency Default Bearers Rejected | sessstat-bearrej-emergency-def
> PGW Schema / Subscriber Session Statistics / Total Bearers Rejected / Dedicated Bearers | Total Emergency Dedicated Bearers Rejected | sessstat-bearrej-emergency-ded

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> EGTPC Schema Bulk Statistics Enhancements
> The following bulk statistics were added to the EGTPC schema in WEM Release 12.2.

> EGTPC Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> EGTPC Statistics / General | Current Sessions | sess-cur
> EGTPC Statistics / Tunnel / Create Session Request | Sent | tun-sent-cresess
> Retransmitted Sent | tun-sent-retranscresess
> Received | tun-recv-cresess
> Retransmitted Received | tun-recv-retranscresess
> EGTPC Statistics / Tunnel / Create Session Response | Initial Sent | tun-sent-cresessresp
> Accept Sent | tun-sent-cresessrespaccept
> Denied Sent | tun-sent-cresessrespdenied
> Retransmitted Sent | tun-sent-retranscresessresp
> Initial Received | tun-recv-cresessresp
> Accept Received | tun-recv-cresessrespaccept
> Denied Received | tun-recv-cresesssrespdenied
> EGTPC Statistics / Tunnel / Modify Bearer Request | Initial Sent | tun-sent-modbearreq
> Retransmitted Sent | tun-sent-retransmodbearreq
> Initial received | tun-recv-modbearreq
> Retransmitted Received | tun-recv-retransmodbearreq
> EGTPC Statistics / Tunnel / Modify Bearer Response | Initial Sent | tun-sent-modbearresp
> Accept Sent | tun-sent-modbearrespaccept
> Denied Sent | tun-sent-modbearrespdenied
> Retransmitted Sent | tun-sent-retransmodbearresp
> Initial Received | tun-recv-modbearresp
> Accept Received | tun-recv-modbearrespaccept
> Denied Received | tun-recv-modbearrespdenied
> EGTPC Statistics / Tunnel / Delete Session Request | Initial Sent | tun-sent-delsessreq
> Retransmitted Sent | tun-sent-retransdelsessreq
> Initial Received | tun-recv-delsessreq
> Retransmitted Received | tun-recv-retransdelsessreq
> EGTPC Statistics / Tunnel / Delete Session Response | Initial Sent | tun-sent-delsessresp
> Accept Sent | tun-sent-delsessrespaccept
> denied Sent | tun-sent-delsessrespdenied
> Initial Received | tun-recv-delsessresp
> Accept received | tun-recv-delsessrespaccept
> Denied Received | tun-recv-delsessrespdenied
> EGTPC Statistics / Tunnel / Downlink Data Notification Request | Initial Sent | tun-sent-dlinknotif
> Retransmitted Sent | tun-sent-retransdlinknotif
> Initial Received | tun-recv-dlinknotif
> Retransmitted Received | tun-recv-retransdlinknotif
> EGTPC Statistics / Tunnel / Downlink Data Notification Acknowledgement | Received | tun-recv-dlinknotifack
> Accept | tun-recv-dlinknotifackaccept
> Denied | tun-recv-dlinknotifackdenied
> EGTPC Statistics / Tunnel / Downlink Data Failure Indication | Sent | tun-sent-dlinkdatafail
> Received | tun-recv-dlinkdatafail
> EGTPC Statistics / Tunnel / Release Access Bearers Request | Initial Sent | tun-sent-relaccbearreq
> Retransmitted Sent | tun-sent-retransrelaccbearreq
> Initial Receive | tun-recv-relaccbearreq
> Retransmitted Received | tun-recv-retransrelaccbearreq
> EGTPC Statistics / Tunnel / Release Access Bearers Response | Initial Sent | tun-sent-relaccbearresp
> Accept Sent | tun-sent-relaccbearrespaccept
> Denied Sent | tun-sent-relaccbearrespdenied
> Retransmitted Sent | tun-sent-retransrelaccbearresp
> Initial Received | tun-recv-relaccbearresp
> Accept Received | tun-recv-relaccbearrespaccept
> Denied Received | tun-recv-relaccbearrespdenied
> EGTPC Statistics / Tunnel / Create Bearer Request | Initial Sent | tun-sent-crebear
> Retransmitted Sent | tun-sent-retranscrebear
> Initial Received | tun-recv-crebear
> Retransmitted Received | tun-recv-retranscrebear
> EGTPC Statistics / Tunnel / Create Bearer Response | Initial Sent | tun-sent-crebearresp
> Accept Sent | tun-sent-crebearrespaccept
> Denied Sent | tun-sent-crebearrespdenied
> Retransmitted Sent | tun-sent-retranscrebearresp
> Initial Received | tun-recv-crebearresp
> Accept Received | tun-recv-crebearrespaccept
> Denied Received | tun-recv-crebearrespdenied
> EGTPC Statistics / Tunnel / Update Bearer Request | Initial Sent | tun-sent-updbearreq
> Retransmitted Sent | tun-sent-retransupdbearreq
> Initial Received | tun-recv-updbearreq
> Transmitted Received | tun-recv-retransupdbearreq
> EGTPC Statistics / Tunnel / Update Bearer Response | Initial Sent | tun-sent-updbearresp
> Accept Sent | tun-sent-updbearrespaccept
> Denied Sent | tun-sent-updbearrespdenied
> Initial Received | tun-recv-updbearresp
> Accept Received | tun-recv-updbearrespaccept
> Denied Received | tun-recv-updbearrespdenied
> EGTPC Statistics / Tunnel / Delete Bearer Request | Initial Sent | tun-sent-delbearreq
> Retransmitted Sent | tun-sent-retransdelbearreq
> Initial received | tun-recv-delbearreq
> Retransmitted Received | tun-recv-retransdelbearreq
> EGTPC Statistics / Tunnel / Delete Bearer Response | Initial Sent | tun-sent-delbearresp
> Accept Sent | tun-sent-delbearrespaccept
> Denied Sent | tun-sent-delbearrespdenied
> Initial Received | tun-recv-delbearresp
> Accept Received | tun-recv-delbearrespaccept
> Denied Received | tun-recv-delbearrespdenied
> EGTPC Statistics / Tunnel / Bearer Resource Command | Sent | tun-sent-bearrescmd
> Received | tun-recv-bearrescmd
> Failure Sent | tun-sent-bearrescmd-fail
> Failure Received | tun-recv-bearrescmd-fail
> Retrans TX | tun-sent-retransbearrescmd
> Retrans RX | tun-recv-retransbearrescmd
> EGTPC Statistics / Tunnel / Bearer Resource Failure Indication | Retrans TX | tun-sent-retransbearrescmd-fail
> Retrans RX | tun-recv-retransbearrescmd-fail
> EGTPC Statistics / Tunnel / Modify Bearer Failure Indication | Retrans TX | tun-sent-retransmodbearfail
> Retrans RX | tun-recv-retransmodbearfail
> EGTPC Statistics / Tunnel / Delete Bearer Command | Initial TX | tun-sent-delbearcmd
> Retrans TX | tun-sent-retransdelbearcmd
> Initial RX | tun-recv-delbearcmd
> Receive RX | tun-recv-retransdelbearcmd
> EGTPC Statistics / Tunnel / Delete Bearer Failure Indication | Initial TX | tun-sent-delbearfail
> Retrans TX | tun-sent-retransdelbearfail
> Initial RX | tun-recv-delbearfail
> Receive RX | tun-recv-retransdelbearfail
> EGTPC Statistics / Tunnel / Update User Plane Request | Received | tun-recv-upduplanereq
> Retransmitted | tun-recv-retransupduplanereq
> EGTPC Statistics / Tunnel / Update User Plane Response | Initial Sent | tun-sent-upduplaneresp
> Accept Sent | tun-sent-upduplanerespaccept
> Denied Sent | tun-sent-upduplanerespdenied
> EGTPC Statistics / Tunnel / Modify Bearer Command | Sent | tun-sent-modbearcmd
> Received | tun-recv-modbearcmd
> Failure Indication Sent | tun-sent-modbearfail
> Failure Indication Received | tun-recv-modbearfail
> Retrans TX | tun-sent-retransmodbearcmd
> Retrans RX | tun-recv-retransmodbearcmd
> EGTPC Statistics / Tunnel / Deactivate Bearer Command | Sent | tun-sent-deactbear
> Received | tun-recv-deactbear
> Failure Indication Sent | tun-sent-deactbearfail
> Failure Indication Received | tun-recv-deactbearfail
> EGTPC Statistics / Tunnel / Create Ind Data Forwarding Tunnel Request | Initial TX | tun-sent-creinddatafwdngreq
> Retrans TX | tun-sent-retranscreinddatafwdngreq
> Initial RX | tun-recv-creinddatafwdngreq
> Retrans RX | tun-recv-retranscreinddatafwdngreq
> EGTPC Statistics / Tunnel / Create Ind Data Forwarding Tunnel Response | Initial TX | tun-sent-creinddatafwdngrsp
> Accepted TX | tun-sent-creinddatafwdngrspaccept
> Denied TX | tun-sent-creinddatafwdngrspdenied
> Retrans TX | tun-sent-retranscreinddatafwdngrsp
> Initial RX | tun-recv-creinddatafwdngrsp
> Denied RX | tun-recv-creinddatafwdngrspdenied
> EGTPC Statistics / Tunnel / Delete Ind Data Forwarding Tunnel Request | Initial TX | tun-sent-delinddatafwdngreq
> Retrans TX | tun-sent-retransdelinddatafwdngreq
> Initial RX | tun-recv-delinddatafwdngreq
> Retrans RX | tun-recv-retransdelinddatafwdngreq
> EGTPC Statistics / Tunnel / Delete Ind Data Forwarding Tunnel Response | Initial TX | tun-sent-delinddatafwdngrsp
> Accepted TX | tun-sent-delinddatafwdngrspaccept
> Denied TX | tun-sent-delinddatafwdngrspdenied
> Initial RX | tun-recv-delinddatafwdngrsp
> Accepted RX | tun-recv-delinddatafwdngrspaccept
> Denied RX | tun-recv-delinddatafwdngrspdenied
> EGTPC Statistics / Path / Echo Request | Initial Sent | path-sent-echoreq
> Retransmitted Sent | path-sent-retransechoreq
> Initial Receive | path-recv-echoreq
> EGTPC Statistics / Path / Echo Response | Total Sent | path-sent-echoresp
> Total Received | path-recv-echoresp
> EGTPC Statistics / Path / Version Not Supported | Total Sent | path-sent-versnotsupp
> Total Received | path-recv-versnotsupp
> EGTPC Statistics / GTP-U Tunnel | G-PDU Sent | gtpv1tun-sent-gpdu
> G-PDU Received | gtpv1tun-recv-gpdu
> T-PDU Octets Sent | gtpv1tun-txoctet
> T-PDU Octets Received | gtpv1tun-rxoctet
> GTP-U Error Indication Sent | gtpv1tun-sent-gtpuerror
> GTP-U Error Indication Received | gtpv1tun-recv-gtpuerror
> GTP-U End Marker Message Sen | gtpv1tun-sent-endmarker
> EGTPC Statistics / GTP-U Path | Echo Request Sent | gtpv1path-sent-echoreq
> Echo Request Received | gtpv1path-recv-echoreq
> Echo Response Sent | gtpv1path-sent-echoresp
> Echo Response Received | gtpv1path-recv-echoresp
> Supported Extension Header Notification Sent | gtpv1path-sent-hdrnotif
> Supported Extension Header Notification Received | gtpv1path-recv-hdrnotif
> EGTPC Statistics / PGW S5S8 | Packets TX | OutSigPktS5S8PGW
> Packets RX | IncSigPktS5S8PGW
> Bytes TX | OutSigOctS5S8PGW
> Bytes RX | IncSigOctS5S8PGW
> EGTPC Statistics / SGW S5S8 | Packets TX | OutSigPktS5S8SGW
> Packets RX | IncSigPktS5S8SGW
> Bytes TX | OutSigOctS5S8SGW
> Bytes RX | IncSigOctS5S8SGW
> EGTPC Statistics / SGW S11S4 | Packets TX | OutSigPktS11S4SGW
> Packets RX | IncSigPktS11S4SGW
> Bytes TX | OutSigOctS11S4SGW
> Bytes RX | IncSigOctS11S4SGW
> EGTPC Statistics / MME S11S10 | Packets TX | OutSigPktS11S10MME
> Packets RX | IncSigPktS11S10MME
> Bytes TX | OutSigOctS11S10MME
> Bytes RX | IncSigOctS11S10MME
> EGTPC Statistics / SGSNS4 | Packets TX | OutSigPktS4SGSN
> Packets RX | IncSigPktS4SGSN
> Bytes TX | OutSigOctS4SGSN
> Bytes RX | IncSigOctS4SGSN
> EGTPC Statistics / Mobility Management Messages / Configuration Transfer Tunnel | Initial RX | mobility-recv-configxfertun
> Initial TX | mobility-sent-configxfertun
> EGTPC Statistics / Mobility Management Messages / RAN Information Relay | Initial RX | mobility-recv-ranInforelay
> Initial TX | mobility-sent-ranInforelay
> EGTPC Statistics / Mobility Management Messages / Context Request | Initial TX | mobility-sent-ctxreq
> Retrans TX | mobility-sent-retransctxreq
> Initial RX | mobility-recv-ctxreq
> Retrans RX | mobility-recv-retransctxreq
> EGTPC Statistics / Mobility Management Messages / Context Response | Initial TX | mobility-sent-ctxrsp
> Retrans TX | mobility-sent-retransctxrsp
> Initial RX | mobility-recv-ctxrsp
> Retrans RX | mobility-recv-retransctxrsp
> Accepted TX | mobility-sent-ctxrspaccept
> Denied TX | mobility-sent-ctxrspdenied
> Accepted RX | mobility-recv-ctxrspaccept
> Denied RX | mobility-recv-ctxrspdenied
> EGTPC Statistics / Mobility Management Messages / Context Acknowledge | Initial TX | mobility-sent-ctxack
> Retrans TX | mobility-sent-retransctxack
> Initial RX | mobility-recv-ctxack
> Retrans RX | mobility-recv-retransctxack
> Accepted TX | mobility-sent-ctxackaccept
> Denied TX | mobility-sent-ctxackdenied
> Accepted RX | mobility-recv-ctxackaccept
> Denied RX | mobility-recv-ctxackdenied
> EGTPC Statistics / Mobility Management Messages / Identification Request | Initial TX | mobility-sent-idtreq
> Retrans TX | mobility-sent-retransidtreq
> Initial RX | mobility-recv-idtreq
> Retrans RX | mobility-recv-retransidtreq
> EGTPC Statistics / Mobility Management Messages / Identification Response | Total TX | mobility-sent-idtrsp
> Retrans TX | mobility-sent-retransidtrsp
> Total RX | mobility-recv-idtrsp
> Retrans RX | mobility-recv-retransidtrsp
> Accepted TX | mobility-sent-idtrspaccept
> Denied TX | mobility-sent-idtrspdenied
> Accepted RX | mobility-recv-idtrspaccept
> Denied RX | mobility-recv-idtrspdenied
> EGTPC Statistics / Mobility Management Messages / Forward Relocation Request | Initial TX | mobility-sent-fwdrelreq
> Retrans TX | mobility-sent-retransfwdrelreq
> Initial RX | mobility-recv-fwdrelreq
> Retrans RX | mobility-recv-retransfwdrelreq
> EGTPC Statistics / Mobility Management Messages / Forward Relocation Response | Initial TX | mobility-sent-fwdrelrsp
> Retrans TX | mobility-recv-retransfwdrelrsp
> Initial RX | mobility-sent-fwdrelrspaccept
> Retrans RX | mobility-sent-retransfwdrelrsp
> Initial RX | mobility-recv-fwdrelrsp
> Accepted | mobility-recv-fwdrelrspaccept
> Denied | mobility-recv-fwdrelrspdenied
> Denied TX | mobility-sent-fwdrelrspdenied
> EGTPC Statistics / Mobility Management Messages / Forward Access Context Notification | Initial TX | mobility-sent-fwdaccnotif
> Retrans TX | mobility-sent-retransfwdaccnotf
> Initial RX | mobility-recv-fwdaccnotf
> Retrans RX | mobility-recv-retransfwdaccnotf
> EGTPC Statistics / Mobility Management Messages / Forward Access Context Acknowledge | Initial TX | mobility-sent-fwdaccack
> Retrans TX | mobility-sent-retransfwdaccack
> Initial RX | mobility-recv-fwdaccack
> Retrans RX | mobility-recv-retransfwdaccack
> Accepted TX | mobility-sent-fwdaccackaccept
> Denied TX | mobility-sent-fwdaccackdenied
> Accepted RX | mobility-recv-fwdaccackaccept
> Denied RX | mobility-recv-fwdaccackdenied
> EGTPC Statistics / Mobility Management Messages / Forward Relocation Complete Notification | Initial TX | mobility-sent-fwdrelcmpnotf
> Retrans TX | mobility-sent-retransfwdrelcmpnotf
> Initial RX | mobility-recv-fwdrelcmpnotf
> Retrans RX | mobility-recv-retransfwdrelcmpnotf
> EGTPC Statistics / Mobility Management Messages / Forward Relocation Complete Acknowledge | Initial TX | mobility-sent-fwdrelcmpack
> Retrans TX | mobility-sent-retransfwdrelcmpack
> Initial RX | mobility-recv-fwdrelcmpack
> Retrans RX | mobility-recv-retransfwdrelcmpack
> Accepted TX | mobility-sent-fwdrelcmpackaccept
> Denied TX | mobility-sent-fwdrelcmpackdenied
> Accepted RX | mobility-recv-fwdrelcmpackaccept
> Denied RX | mobility-recv-fwdrelcmpackdenied
> EGTPC Statistics / Mobility Management Messages / Relocation Cancel Request | Initial TX | mobility-sent-relcancelreq
> Retrans TX | mobility-sent-retransrelcancelreq
> Initial RX | mobility-recv-relcancelreq
> Retrans RX | mobility-recv-retransrelcancelreq
> EGTPC Statistics / Mobility Management Messages / Relocation Cancel Response | Initial TX | mobility-sent-relcancelrsp
> Retrans TX | mobility-sent-retransrelcancelrsp
> Initial RX | mobility-recv-relcancelrsp
> Retrans RX | mobility-recv-retransrelcancelrsp
> Accepted TX | mobility-sent-relcancelrspaccept
> Denied TX | mobility-sent-relcancelrspdenied
> Accepted RX | mobility-recv-relcancelrspaccept
> Denied RX | mobility-recv-relcancelrspdenied
> EGTPC Statistics / Trace Management Messages / Trace Session Activation | Initial Tx | trace-sent-activate
> Initial RX | trace-recv-activate
> EGTPC Statistics / Trace Management Messages / Trace Session Deactivation | Initial TX | trace-sent-deactivate
> Initial RX | trace-recv-deactivate
> EGTPC Statistics / CS Fallback Messages / Suspend Notification | Initial TX | csfb-sent-suspendnotf
> Retrans TX | csfb-sent-retranssuspendnotf
> Initial RX | csfb-recv-suspendnotf
> Retrans RX | csfb-recv-retranssuspendnotf
> EGTPC Statistics / CS Fallback Messages / Suspend Acknowledge | Initial TX | csfb-sent-suspendack
> Accept TX | csfb-sent-suspendackaccept
> Denied TX | csfb-sent-suspendackdenied
> Initial RX | csfb-recv-suspendack
> Accept RX | csfb-recv-suspendackaccept
> Denied RX | csfb-recv-suspenddenied
> EGTPC Statistics / CS Fallback Messages / Resume Notification | Initial TX | csfb-sent-resumenotf
> Retrans TX | csfb-sent-retransresumenotf
> Initial RX | csfb-recv-resumenotf
> Retrans RX | csfb-recv-retransresumenotf
> EGTPC Statistics / CS Fallback Messages / Resume Acknowledge | Initial TX | csfb-sent-resumeack
> Accept TX | csfb-sent-resumeackaccept
> Denied TX | csfb-sent-resumeackdenied
> Initial RX | csfb-recv-resumeack
> Accept RX | csfb-recv-resumeackaccept
> Denied RX | csfb-recv-resumedenied
> EGTPC Statistics / Tunnel Management Messages / Change Notification Request | Initial RX | tun-recv-changenotfreq
> Initial TX | tun-sent-changenotfreq
> Retrans RX | tun-recv-retranschangenotfreq
> Retrans RX | tun-sent-retranschangenotfreq
> EGTPC Statistics / Tunnel Management Messages / Change Notification Response | Initial RX | tun-recv-changenotfresp
> Accepted RX | tun-recv-changenotfrespaccept
> Denied RX | tun-recv-changenotfrespdenied
> Initial TX | tun-sent-changenotfresp
> Accepted TX | tun-sent-changenotfrespaccept
> Denied TX | tun-sent-changenotfrespdenied
> Retrans TX | tun-sent-retranschangenotfresp

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> MME Schema Bulk Statistic Enhancements
> The following bulk statistics were added to the MME schema in WEM Release 12.2

> MME Bulk Statistic Schema Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> MME Statistics / S1AP Statistics / Transmitted S1AP Data | MME Config Update | s1ap-transdata-cfgupd
> MME Config Transfer | s1ap-transdata-cfgtfr
> MME Statistics / S1AP Statistics / Received S1AP Data | MME Config Update Fail | s1ap-recdata-cfgupdfail
> MME Config Update Ack | s1ap-recdata-cfgupdack
> eNB Config Transfer | s1ap-recdata-enbcfgtfr
> MME Statistics / S1AP Statistics / Radio Network Error Statistics | Unknown MME UE S1AP Id | s1ap-err-unknownmme-ues1apid
> Unknown ENB UE S1AP Id | s1ap-err-unknownenb-ues1apid
> Unknown UE S1AP Id Pair | s1ap-err-unknownpair-ues1apid
> MME Statistics / S1AP Statistics / Protocol, Error Statistics | Transfer Syntax Error | s1ap-err-tfr-synerr
> Semantic Error | s1ap-err-semanticerr
> Message Not Compatible | s1ap-err-msgnotcompatible
> Abstract Syntax Error - Falsely Constr Msg | s1ap-err-asefalsely-constrmsg
> Abstract Syntax Error - Ignore And Notify | s1ap-err-aseignore-notify
> Abstract Syntax Error - Reject | s1ap-err-aserej
> MME Statistics / S1AP Statistics / eNodeB Statistics | Total eNodeB Associations | s1ap-enodeb-assoc
> MME Statistics / EMM Statistics / EPS Associations by Attach using IMSI | Attempted | epsattach-imsi-attempted
> Success | epsattach-imsi-success
> Failure | epsattach-imsi-failures
> MME Statistics / EMM Statistics / EPS Associations by Attach using Local GUTI | Attempted | epsattach-guti-local-attempted
> Success | epsattach-guti-local-success
> Failure | epsattach-guti-local-failures
> MME Statistics / EMM Statistics / EPS Associations by Attach using Foreign GUTI | Attempted | epsattach-guti-foreign-attempted
> Success | epsattach-guti-foreign-success
> Failures | epsattach-guti-foreign-failures
> MME Statistics / EMM Statistics / EPS Associations by P-TMSI | Attempted | epsattach-ptmsi-attempted
> Success | epsattach-ptmsi-success
> Failures | epsattach-ptmsi-failures
> MME Statistics / EMM Statistics / EPS Associations by TAU using Foreign GUTI | Attempted | epstauattach-guti-foreign-attempted
> Success | epstauattach-guti-foreign-success
> Failures | epstauattach-guti-foreign-failures
> MME Statistics / EMM Statistics / EPS Associations by TAU using PTMSI | Attempted | epstauattach-ptmsi-attempted
> Success | epstauattach-ptmsi-success
> Failures | epstauattach-ptmsi-failures
> MME Statistics / EMM Statistics / EPS Associations for Emergency Bearer Services | Attempted | epsattach-emergency-attempted
> Success | epsattach-emergency-success
> Failure | epsattach-emergency-failures
> MME Statistics / EMM Statistics / Associations by Combined Attach using IMSI | Attempted | combinedattach-imsi-attempted
> Success | combinedattach-imsi-success
> Success EPS Only | combinedattach-imsi-success-eps
> Failure | combinedattach-imsi-failure
> MME Statistics / EMM Statistics / Associations by Combined Attach using Local GUTI | Attempted | combinedattach-guti-local-attached
> Success | combinedattach-guti-local-success
> Success EPS Only | combinedattach-guti-local-success-eps
> Failure | combinedattach-guti-local-failure
> MME Statistics / EMM Statistics / Associations by Combined Attach using Foreign GUTI | Attempted | combinedattach-guti-foreign-attempted
> Success | combinedattach-guti-foreign-success
> Success EPS Only | combinedattach-guti-foreign-success-eps
> Failure | combinedattach-guti-foreign-failure
> MME Statistics / EMM Statistics / Associations by Combined Attach using P-TMSI | Attempted | combinedattach-ptmsi-attempted
> Success | combinedattach-ptmsi-success
> Success EPS Only | combinedattach-ptmsi-success-eps
> Failure | combinedattach-ptmsi-failure
> MME Statistics / EMM Statistics / Associations by Combined TAU using Foreign GUTI | Attempted | combined-tauattach-guti-foreign-attempted
> Success | combined-tauattach-guti-foreign-success
> Success EPS Only | combined-tauattach-guti-foreign-success-eps
> Failure | combined-tauattach-guti-foreign-failure
> MME Statistics / EMM Statistics / Associations by Combined TAU using P-TMSI | Attempted | combined-tauattach-ptmsi-attempted
> Success | combined-tauattach-ptmsi-success
> Success EPS Only | combined-tauattach-ptmsi-success-eps
> Failure | combined-tauattach-ptmsi-failure
> MME Statistics / EMM Statistics / Periodic TAU | Attempted | tau-periodic-attempted
> Success | tau-periodic-success
> Failures | tau-periodic-failures
> MME Statistics / EMM Statistics / Normal TAU without SGW Relocation | Attempted | tau-normal-attempted
> Success | tau-normal-success
> Failures | tau-normal-failures
> MME Statistics / EMM Statistics / TAU with Bearer Activation | Attempted | tau-active-attempted
> Success | tau-active-success
> Failures | tau-active-failures
> MME Statistics / EMM Statistics / TAU with SGW Relocation | Attempted | tau-sgw-change-attempted
> Success | tau-sgw-change-success
> Failures | tau-sgw-change-failures
> MME Statistics / ECM Statistics / Paging Initiation Events | Attempted | paging-init-events-attempted
> Success | paging-init-events-success
> Failures | paging-init-events-failures
> Success At Last eNB | paging-last-enb-success
> Success At Last TAI | paging-last-tai-success
> Success At TAI List | ecmevent-tailist-success
> S1 Release for Load Rebalancing | ecmevent-s1rel-loadbalance
> MME Statistics / Total EMM Control Messages / Sent | Attach Accept | emm-msgtx-attach-accept
> Retransmissions | emm-msgtx-attach-accept-retx
> Attach Reject | emm-msgtx-attach-reject
> IMSI Unknown in HSS | emm-msgtx-imsi-unknown-hss
> Illegal UE | emm-msgtx-illegal-ue
> Illegal ME | emm-msgtx-illegal-me
> EPS Not Allowed | emm-msgtx-eps-not-allowed
> Network Failure | emm-msgtx-network-failure
> ESM Failure | emm-msgtx-esm-failure
> Decode Failure | emm-msgtx-decode-failure
> Authentication Reject | emm-msgtx-auth-reject
> Authentication Request | emm-msgtx-auth-req
> Retransmissions | emm-msgtx-auth-req-retx
> Detach Request | emm-msgtx-detach-request
> MME Statistics / Total EMM Control Messages / Sent (con’t) | Retransmissions | emm-msgtx-detach-req-retx
> Reattach Required | emm-msgtx-reattach-req
> Reattach Not Required | emm-msgtx-rettach-not-req
> Detach Accept | emm-msgtx-detach-accept
> Downlink NAS Transport | emm-msgtx-downlink-transport
> EMM Information | emm-msgtx-emm-info
> EMM Status | emm-msgtx-emm-status
> GUTI Relocations | emm-msgtx-guti-reloc
> Retransmissions | emm-msgtx-guti-reloc-retx
> Identity Request | emm-msgtx-identity-req
> Retransmissions | emm-msgtx-identity-req-retx
> Security Mode Command | emm-msgtx-sm-cmd
> Retransmissions | emm-msgtx-sm-cmd-retx
> Service Reject | emm-msgtx-service-reject
> UE Identity Unknown | emm-msgtx-ue-identity-unk
> Implicitly Detached | emm-msgtx-impl-detached
> TAU Accept | emm-msgtx-tau-accept
> Retransmissions | emm-msgtx-tau-accept-retx
> TAU Reject | emm-msgtx-tau-reject
> IMSI Unknown in HSS | emm-msgtx-tau-imsi-unknown-hss
> TAU Illegal UE | emm-msgtx-tau-illegal-ue
> TAU Illegal ME | emm-msgtx-tau-illegal-me
> EPS Not Allowed | emm-msgtx-tau-eps-not-allowed
> TAU Network Fail | emm-msgtx-tau-network-fail
> Decode Failure | emm-msgtx-tau-decode-failure
> No Bearer Active | emm-msgtx-tau-no-bearer-active
> UE Identity Unknown | emm-msgtx-tau-ue-identity-unk
> Implicit Detached | emm-msgtx-tau-implicit-detached
> IMEI Not Accepted | emm-msgtx-imei-not-accept
> No suitable cells in TA | emm-msgtx-no-suitable-cell-ta
> PLMN Not Allowed | emm-msgtx-plmn-not-allow
> Roaming Restricted TA | emm-msgtx-roaming-restrict-ta
> TA Not Allowed | emm-msgtx-ta-not-allow
> TAU - CS Service Notification | emm-msgtx-tau-cs-service-notif
> TAU - IMEI not accepted | emm-msgtx-tau-imei-not-accept
> TAU - No suitable cells in TA | emm-msgtx-tau-no-suitable-cell-ta
> TAU - PLMN not allowed | emm-msgtx-tau-plmn-not-allow
> TAU - Roaming Restricted TA | emm-msgtx-tau-roaming-restrict-ta
> TAU - TA not allowed | emm-msgtx-tau-ta-not-allow
> MME Statistics / Total EMM Control Messages / Received | Clear Text Messages | emm-msgrx-plain-nas
> Integrity-check Enabled | emm-msgrx-integrity
> Ciphered Messages | emm-msgrx-ciphered
> Accepted | emm-msgrx-accepted
> Ignored Messages | emm-msgrx-discarded
> Decode Failures | emm-msgrx-decode-failure
> Attach Complete | emm-msgrx-attach-complete
> Denied | emm-msgrx-denied
> Attach Request | emm-msgrx-attach-req
> Retransmissions | emm-msgrx-attach-retx
> Authentication Failure | emm-msgrx-auth-failure
> Authentication Response | emm-msgrx-auth-resp
> Switch Off | emm-msgrx-detach-req-switchoff
> Not Switchoff | emm-msgrx-detach-req-not-switchoff
> Detach Request | emm-msgrx-detach-req
> IMSI Detach | emm-msgrx-imsi-detach
> EMM Status | emm-msgrx-emm-status
> GUTI Reloc Complete | emm-msgrx-guti-reloc-complete
> Security Mode Complete | emm-msgrx-sm-complete
> Security Mode Reject | emm-msgrx-sm-reject
> Service Request | emm-msgrx-service-req
> TAU Request | emm-msgrx-tau-req
> Retransmissions | emm-msgrx-tau-retx
> TAU Complete | emm-msgrx-tau-complete
> Extended Service Request | emm-msgrx-ext-service-req
> Identity Response | emm-msgrx-identity-resp
> MME Statistics / Total ESM Control Messages / Received | Clear-text messages | esm-msgrx-plain-nas
> Accepted | esm-msgrx-accepted
> Brr Rsrc Alloc Request | esm-msgrx-brr-rsrc-alloc-req
> Brr Rsrc Modify Request | esm-msgrx-brr-rsrc-modify-req
> Ciphered messages | esm-msgrx-ciphered
> Act Dedicated Brr Accept | esm-msgrx-ded-brr-accept
> Act Dedicated Brr Reject | esm-msgrx-ded-brr-reject
> Denied | esm-msgrx-denied
> Act Default Brr Accept | esm-msgrx-dflt-brr-accept
> Act Default Brr Reject | esm-msgrx-dflt-brr-reject
> ESM Status | esm-msgrx-em-status
> ESM Information Response | esm-msgrx-esm-info-resp
> MME Statistics / Total ESM Control Messages / Received (con’t) | Integrity-check enabled | esm-msgrx-integrity
> Modify Brr Ctxt Accept | esm-msgrx-mod-brr-accept
> Modify Brr Ctxt Reject | esm-msgrx-mod-brr-reject
> PDN Connectivity Request | esm-msgrx-pdn-con-req
> PDN Disconnect Request | esm-msgrx-pdn-discon-req
> Deactivate Brr Accept | esm-msgrx-deactivate-brr-accept
> MME Statistics / Total ESM Control Messages / Sent | Act Dedicated Bearer | esm-msgtx-act-ded-brr
> Retransmissions | esm-msgtx-act-ded-brr-retx
> Act Default Bearer | esm-msgtx-act-dflt-brr
> Retransmissions | esm-msgtx-act-dflt_bee-retx
> Bearer Alloc Reject | esm-msgtx-brralloc-rej
> Collision with NW Op | esm-msgtx-brralloc-rej-collision-nwop
> Invalid Bearer Id | esm-msgtx-brralloc-rej-invalid-brrid
> Invalid PTI | esm-msgtx-brralloc-rej-invalid-pti
> PTI Already in Use | esm-msgtx-brralloc-rej-pt1-inuse
> Semantic Error TFT | esm-msgtx-brralloc-rej-semantic-errtft
> Syntactic Error TFT | esm-msgtx-brralloc-rej-syntactic-errtft
> Bearer Modify Reject | esm-msgtx-brrmod-rej
> PTI Already in Use | esm-msgtx-brrmod-rej-pti-inuse
> Semantic Error TFT | esm-msgtx-brrmod-rej-semantic-errtft
> Syntactic Error TFT | esm-msgtx-brrmod-rej-syntactic-errtft
> Invalid Bearer ID | esm-msgtx-brrmod-rej-invalid-brrid
> Collision with NW Op | esm-msgtx-brrmod-rej-collision-nwop
> Rejected By PGW/SGW | esm-msgtx-brrmod-rej-pgw-rej
> Invalid PTI | esm-msgtx-brrmod-rej-invalid-pti
> Deactivate Bearer | esm-msgtx-deactbrr
> Retransmissions | esm-msgtx-deactbrr-retx
> ESM Information Req | esm-msgtx-deactbrr-esm-info-req
> Retransmissions | esm-msgtx-deactbrr-esm-info-req-retx
> Modify Bearer | esm-msgtx-deactbrr-modbrr
> Retransmissions | esm-msgtx-deactbrr-moderr-retx
> PDN Connectivity Reject | esm-msgtx-pdncon-rej
> PTI Already in Use | esm-msgtx-pdncon-rej-pti-inuse
> Unknown or Missing APN | esm-msgtx-pdncon-rej-apn-unk
> Unknown PDN Type | esm-msgtx-pdncon-rej-pdntype-unk
> Invalid Bearer ID | esm-msgtx-pdncon-rej-inv-brrid
> Invalid PTI | esm-msgtx-pdncon-rej-inv-pti
> Rejected By PGW/SGW | esm-msgtx-pdncon-rej-pgw-rej
> MME Statistics / Total ESM Control Messages / Sent (con’t) | PDN Disconnect Reject | esm-msgtx-pdndiscon-rej
> PTI Already in Use | esm-msgtx-pdndiscon-rej-pti-inuse
> Last PDN Disconnection | esm-msgtx-pdndiscon-rej-lastpdn
> Invalid PTI | esm-msgtx-pdndiscon-rej-inv-pti
> Invalid Bearer ID | esm-msgtx-pdndiscon-rej-inv-brrid
> Rejected By PGW/SGW | esm-msgtx-pdndiscon-rej-pgw-rej
> Bearer Alloc Reject - Insufficient Resources | esm-msgtx-brralloc-rej-insuff-resource
> Bearer Modify Reject - Insufficient Resources | esm-msgtx-brrmod-rej-insuff-resource
> MME Statistics / ESM Statistics / UE Initiated PDN Disconnections | Attempted | pdn-disconnect-ue-attempted
> Success | pdn-disconnect-ue-success
> Failure | pdn-disconnect-ue-failures
> MME Statistics / ESM Statistics / MME Initiated PDN Disconnections | Attempted | pdn-disconnect-mme-attempted
> Success | pdn-disconnect-mme-success
> Failure | pdn-disconnect-mme-failures
> MME Statistics / ESM Statistics / PGW/SGW Initiated PDN Disconnections | Attempted | pdn-disconnect-pgw-attempted
> Success | pdn-disconnect-pgw-success
> Failure | pdn-disconnect-pgw-failures
> MME Statistics / ESM Statistics / HSS Initiated PDN Disconnections | Attempted | pdn-disconnect-hss-attempted
> Success | pdn-disconnect-hss-success
> Failure | pdn-disconnect-hss-failures
> MME Statistics / ESM Statistics / UE Initiated Dedicated Bearer Activations | Attempted | dedi-brr-activation-ue-attempted
> Success | dedi-brr-activation-ue-success
> Failure | dedi-brr-activation-ue-failures
> MME Statistics / ESM Statistics / MME Initiated Bearer Deactivations | Attempted | brr-deactivation-mme-attempted
> Success | brr-deactivation-mme-success
> Failure | brr-deactivation-mme-failures
> MME Statistics / ESM Statistics / PGW / SGW Initiated Bearer Deactivations | Attempted | brr-deactivation-pgw-attempted
> Success | brr-deactivation-pgw-success
> Failure | brr-deactivation-pgw-failures
> MME Statistics / ESM Statistics / UE Initiated Bearer Deactivations | Attempted | brr-deactivation-ue-attempted
> Success | brr-deactivation-ue-success
> Failure | brr-deactivation-ue-failures
> MME Statistics / ESM Statistics / HSS Initiated Bearer Modifications | Attempted | brr-modification-hss-attempted
> Success | brr-modification-hss-success
> Failure | brr-modification-hss-failures
> MME Statistics / ESM Statistics / PGW/SGW Initiated Bearer Modifications | Attempted | brr-modification-pgw-attemted
> Success | brr-modification-pgw-success
> Failure | brr-modification-pgw-failures
> MME Statistics / ESM Statistics / UE Initiated Bearer Modifications | Attempted | brr-modification-ue-attempted
> Success | brr-modification-ue-success
> Failure | brr-modification-ue-failures
> MME Statistics / EUTRAN - EUTRAN using S10 Interface / Outbound relocation using TAU Procedure | Attempted | out-tau-ho-4gto4g-s10-attempted
> Success | out-tau-ho-4gto4g-s10-success
> Failures | out-tau-ho-4gto4g-s10-failures
> MME Statistics / EUTRAN - EUTRAN using S10 Interface / Outbound relocation using S1 HO Procedure | Attempted | out-s1-ho-4gto4g-s10-attempted
> Success | out-s1-ho-4gto4g-s10-success
> Failures | out-s1-ho-4gto4g-s10-failures
> MME Statistics / EUTRAN - EUTRAN using S10 Interface / Inbound relocation using TAU Procedure | Attempted | in-tau-ho-4gto4g-s10-attempted
> Success | in-tau-ho-4gto4g-s10-success
> Failures | in-tau-ho-4gto4g-s10-failures
> MME Statistics / EUTRAN - EUTRAN using S10 Interface / Inbound relocation using S1 HO Procedure | Attempted | in-s1-ho-4gto4g-s10-attempted
> Success | in-s1-ho-4gto4g-s10-success
> Failures | in-s1-ho-4gto4g-s10-failures
> MME Statistics / EUTRAN - UTRAN using GnGp Interface / Outbound Relocation using S1 HO Procedure | Attempted | out-s1-ho-4gto3g-gngp-attempted
> Success | out-s1-ho-4gto3g-gngp-success
> Failures | out-s1-ho-4gto3g-gngp-failures
> MME Statistics / EUTRAN - UTRAN using GnGp Interface / Inbound Relocation using S1 HO Procedure | Attempted | in-s1-ho-3gto4g-gngp-attempted
> Success | in-s1-ho-3gto4g-gngp-success
> Failures | in-s1-ho-3gto4g-gngp-failures
> MME Statistics / EUTRAN - GERAN using GnGp Interface / Outbound relocation using S1 HO Procedure | Attempted | out-s1-ho-4gto2g-gngp-attempted
> Success | out-s1-ho-4gto2g-gngp-success
> Failures | out-s1-ho-4gto2g-gngp-failures
> MME Statistics / EUTRAN - GERAN using GnGp Interface / Inbound relocation using S1 HO Procedure | Attempted | in-s1-ho-2gto4g-gngp-attempted
> Success | in-s1-ho-2gto4g-gngp-success
> Failures | in-s1-ho-2gto4g-gngp-failures
> MME Statistics / EUTRAN - GERAN A/Gb Mode Inter-RAT Handovers using S3 Interface / Inbound Relocation | Attempted | in-s1-ho-2gto4g-s3-attempted
> Success | in-s1-ho-2gto4g-s3-success
> Failures | in-s1-ho-2gto4g-s3-failures
> MME Statistics / EUTRAN - GERAN A/Gb Mode Inter-RAT Handovers using S3 Interface / Outbound Relocation | Attempted | out-s1-ho-4gto3g-s3-attempted
> Success | out-s1-ho-4gto3g-s3-success
> Failures | out-s1-ho-4gto3g-s3-failures
> MME Statistics / EUTRAN - UTRAN Iu mode Inter-RAT Handovers using S3 Interface / Inbound Relocation | Attempted | in-s1-ho-3gto4g-s3-attempted
> Success | in-s1-ho-3gto4g-s3-success
> Failures | in-s1-ho-3gto4g-s3-failures
> MME Statistics / EUTRAN - UTRAN Iu mode Inter-RAT Handovers using S3 Interface / Outbound Relocation | Attempted | out-s1-ho-4gto2g-s3-attempted
> Success | out-s1-ho-4gto2g-s3-success
> Failures | out-s1-ho-4gto2g-s3-failures
> MME Statistics / EUTRAN - UTRAN/GERAN Iu or A/Gb mode Cell Reselections using Gn/Gp Interface / Inbound Relocation using TAU Procedure | Attempted | out-rau-ho-4gto3g2g-gngp-attempted
> Success | out-rau-ho-4gto3g2g-gngp-success
> Failures | out-rau-ho-4gto3g2g-gngp-failures
> MME Statistics / EUTRAN - UTRAN/GERAN Iu or A/Gb mode Cell Reselections using Gn/Gp Interface / Outbound Relocation using RAU Procedure | Attempted | in-tau-ho-2g3gto4g-gngp-attempted
> Success | in-tau-ho-2g3gto4g-gngp-success
> Failures | in-tau-ho-2g3gto4g-gngp-failures
> MME Statistics / EUTRAN - UTRAN/GERAN Iu or A/Gb mode Cell Reselections using S3 Interface / Outbound Relocation using RAU Procedure | Attempted | in-tau-ho-2g3gto4g-s3-attempted
> Success | in-tau-ho-2g3gto4g-s3-success
> Failures | in-tau-ho-2g3gto4g-s3-failures
> MME Statistics / EUTRAN - UTRAN/GERAN Iu or A/Gb mode Cell Reselections using S3 Interface / Inbound Relocation using TAU Procedure | Attempted | out-rau-ho-4gto3g2g-s3-attempted
> Success | out-rau-ho-4gto3g2g-s3-success
> Failures | out-rau-ho-4gto3g2g-s3-failures
> MME Statistics / EUTRAN - UTRAN/GERAN using Sv Interface / CS only Handover with no DTM Support | Attempted | s1-ho-4gto3g-cs-nodtm-sv-attempted
> Success | s1-ho-4gto3g-cs-nodtm-sv-success
> Failures | s1-ho-4gto3g-cs-nodtm-sv-failures
> MME Statistics / EUTRAN - UTRAN/GERAN using Sv Interface / CS Only Handover | Attempted | s1-ho-4gto3g-cs-sv-attempted
> Success | s1-ho-4gto3g-cs-sv-success
> Failures | s1-ho-4gto3g-cs-sv-failures
> MME Statistics / EUTRAN - UTRAN/GERAN using Sv Interface / CS and PS Handover | Attempted | s1-ho-4gto3g-csps-sv-attempted
> Success | s1-ho-4gto3g-csps-sv-success
> Failures | s1-ho-4gto3g-csps-sv-failures
> MME Statistics / EUTRAN - UTRAN/GERAN using Sv Interface / PDN Statistics | All PDNs | pdn-all
> Connected PDNs | pdn-connected
> Idle PDNs | pdn-idle
> MME Statistics / EUTRAN - UTRAN/GERAN using Sv Interface / Emergency PDN Statistics | All PDNs | pdn-emergency-all
> Connected PDNs | pdn-emergency-connected
> Idle PDNs | pdn-emergency-idle
> MME Statistics / EUTRAN - UTRAN/GERAN using Sv Interface / Bearer Statistics | All Bearers | brr-all
> Connected Bearers | brr-connected
> Idle Bearers | brr-idle
> MME Statistics / EUTRAN - UTRAN/GERAN using Sv Interface / Session Statistics | Attached Calls | sess-call-all
> Connected Calls | sess-call-connected
> Idle Calls | sess-call-idle
> Emergency Session Statistics - Attached Calls | sess-emergency-call-all
> Emergency Session Statistics - Connected Calls | sess-emergency-call-connected
> Emergency Session Statistics - Connected Calls | sess-emergency-call-idle
> Emergency Session Statistics - Idle Calls | sess-emergency-call-idle
> Unauthenticated Session Statistics - Attached Calls | sess-unauth-call-all
> Unauthenticated Session Statistics - Connected Calls | sess-unauth-call-idle
> Total Connected Sessions | sess-ecm-connect

> MAP Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the MAP schema in WEM Release 12.2.

> MAP Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> MAP Schema / Map Statistics | Open Request TX | map-open-req-tx
> Open Request RX | map-open-req-rx
> Open Response TX | map-open-rsp-tx
> Open Response RX | map-open-rsp-rx
> Close Request TX | map-close-tx
> Close Request RX | map-close-rx
> Abort Request TX | map-abort-tx
> Abort Request RX | map-abort-rx
> HLR RESET RX | map-hlr-reset-rcvd
> MAP Schema / Map Statistics / Authentication | Request TX | map-auth-req-tx
> Successful | map-auth-succes
> Failed | map-auth-fail
> Timed Out | map-auth-timeouts-rcvd
> MAP Schema / Map Statistics / Check IMEI | Request TX | map-imei-req-tx
> Successful | map-imei-succes
> Failed | map-imei-fail
> Timed Out | map-imei-timeout
> MAP Schema / Map Statistics / GPRS Location Update | Request TX | map-gprs-update-loc-req-tx
> Successful | map-gprs-update-loc-rsp-tx
> Failed | map-gprs-update-loc-err-tx
> Timed Out | map-gprs-update-loc-timeouts-rx
> MAP Schema / Map Statistics / Subscriber Location | Request TX | map-sub-loc-rpt-req-tx
> Successful | map-sub-loc-rpt-rsp-tx
> Failed | map-sub-loc-rpt-err-tx
> Timed Out | map-sub-loc-rpt-timeouts-rx
> MAP Schema / Map Statistics / Provide Subscriber Location | Request RX | map-prov-sub-loc-req-rx
> Successful Response TX | map-prov-sub-loc-rsp-tx
> Failure Response TX | map-prov-sub-loc-err-tx
> MAP Schema / Map Statistics / Cancel Location | Request RX | map-cancel-loc-req-rx
> Successful Response TX | map-cancel-loc-rsp-tx
> Failure Response TX | map-cancel-loc-err-tx
> MAP Schema / Map Statistics / Delete Subscriber Data | Request RX | map-del-subs-req-rx
> Successful Response TX | map-del-subs-rsp-tx
> Failure Response TX | map-del-subs-ret-tx
> MAP Schema / Map Statistics / Insert Subscriber | Data(ISD)Requests RX | map-insert-subs-rcvd
> StandAlone ISD Request RX | map-standalone-isd-rcvd
> ISD Response TX | map-isd-rsp-tx
> ISD Failure Response TX | map-isd-err-tx
> MAP Schema / Map Statistics / Authentication Failure Report | Request TX | map-auth-fail-rept-req-tx
> Successful | map-auth-fail-rept-rsp-rx
> Failed | map-auth-fail-rept-err-rx
> Timed Out | map-auth-fail-rept-timeouts-rcvd
> MAP Schema / Map Statistics / Purge | Request TX | map-purge-req-tx
> Successful | map-purge-success
> Failed | map-purge-fail
> Timed Out | map-purge-timeouts-rcvd
> MAP Schema / Map Statistics / MO Forward | Request TX | map-mo-fwd-req-sent
> Successful | map-mo-fwd-rsp-rcvd
> Failed | map-mo-fwd-rsp-failed
> Timed Out | map-mo-fwd-rsp-time-out
> MAP Schema / Map Statistics / MT Forward | Request RX | map-mt-fwd-req-sent
> Successful Response Tx | map-mt-fwd-rsp-rcvd
> Failure Response Tx | map-mt-fwd-rsp-failed
> MAP Schema / Map Statistics / Ready for SM | Request TX | map-ready-for-sm-req
> Successful | map-ready-for-sm-rsp
> Failure | map-ready-for-sm-rsp-failed
> Timed Out | map-ready-for-sm-rsp-time-out

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> ASNGW Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the ASNGW schema in WEM Release 12.2.

> ASNGW Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> ASNGW / R6 Messages / R6 Keep Alive Request Message | Total Sent | r6keepalivereq-totsent
> Retransmissions Sent | r6keepalivereq-retranssent
> Total Send Failures | r6keepalivereq-totsendfail
> Total Received | r6keepalivereq-totrec
> Total Accepted | r6keepalivereq-totacc
> Total Relayed | r6keepalivereq-totrelay
> Total Denied | r6keepalivereq-totdenied
> Total Discarded | r6keepalivereq-totdiscard
> Badly Formed | r6keepalivereq-badform
> Decode Error | r6keepalivereq-decodeerr
> Unspecified Error | r6keepalivereq-unspecerr
> TLV Value Invalid | r6keepalivereq-tlvvalinval
> Missing Mandatory TLV | r6keepalivereq-missmandtlv
> Unknown TLV | r6keepalivereq-unknowntlv
> Duplicate TLV Found | r6keepalivereq-duptlvfound
> No Session Found | r6keepalivereq-nosessfound
> No Resource Drops | r6keepalivereq-noresourcedrop
> Admin Prohibited | r6keepalivereq-admprohibit
> Transaction ID Error | r6keepalivereq-transiderr
> ASNGW / R6 Messages / R6 Keep Alive Response Message | Total Sent | r6keepaliversp-totsent
> | Retransmissions Sent | r6keepaliversp-retranssent
> | Total Send Failures | r6keepaliversp-totsendfail
> | Total Received | r6keepaliversp-totrec
> | Total Accepted | r6keepaliversp-totacc
> | Total Relayed | r6keepaliversp-totrelay
> | Total Denied | r6keepaliversp-totdenied
> | Total Discarded | r6keepaliversp-totdiscard
> | Badly Formed | r6keepaliversp-badform
> | Decode Error | r6keepaliversp-decodeerr
> | Unspecified Error | r6keepaliversp-unspecerr
> | TLV Value Invalid | r6keepaliversp-tlvvalinval
> | Missing Mandatory TLV | r6keepaliversp-missmandtlv
> | Unknown TLV | r6keepaliversp-unknowntlv
> | Duplicate TLV Found | r6keepaliversp-duptlvfound
> | No Session Found | r6keepaliversp-nosessfound
> | No Resource Drops | r6keepaliversp-noresourcedrop
> | Admin Prohibited | r6keepaliversp-admprohibit
> | Transaction ID Error | r6keepaliversp-transiderr

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> RP Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the RP schema in WEM Release 12.2.

> RP Schema Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> RP / Session Update Send Reason | Always On Indication | sess-always-on-indication

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> ASNPC Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the ASNPC schema in WEM Release 12.2.

> ASNPC Schema Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> ASNPC Statistics / R6 Messages / R6 Idle Mode Entry MS State Change Request Msg | Total Sent | r6imentstachareq-totsent
> Retransmissions Sent | r6imentstachareq-retranssent
> Total Send Failures | r6imentstachareq-totsendfail
> Total Received | r6imentstachareq-totrec
> Total Accepted | r6imentstachareq-totacc
> Total Relayed | r6imentstachareq-totrelay
> Total Denied | r6imentstachareq-totdenied
> Total Discarded | r6imentstachareq-totdiscard
> Badly Formed | r6imentstachareq-badform
> Decode Error | r6imentstachareq-decodeerr
> Unspecified Error | r6imentstachareq-unspecerr
> Missing Mandatory TLV | r6imentstachareq-missmandtlv
> TLV Value Invalid | r6imentstachareq-tlvvalinval
> Unknown TLV | r6imentstachareq-unknowntlv
> Duplicate TLV Found | r6imentstachareq-duptlvfound
> No Session Found | r6imentstachareq-nosessfound
> Admin Prohibited | r6imentstachareq-admprohibit
> No Resource Drops | r6imentstachareq-noresourcedrop
> Trans ID Error | r6imentstachareq-transiderr
> ASNPC Statistics / R6 Messages / R6 Idle Mode Entry MS State Change Response Msg | Total Sent | r6imentstacharsp-totsent
> Retransmissions Sent | r6imentstacharsp-retranssent
> Total Send Failures | r6imentstacharsp-totsendfail
> Total Received | r6imentstacharsp-totrec
> Total Accepted | r6imentstacharsp-totacc
> Total Relayed | r6imentstacharsp-totrelay
> Total Denied | r6imentstacharsp-totdenied
> Total Discarded | r6imentstacharsp-totdiscard
> Badly Formed | r6imentstacharsp-badform
> Decode Error | r6imentstacharsp-decodeerr
> Unspecified Error | r6imentstacharsp-unspecerr
> Missing Mandatory TLV | r6imentstacharsp-missmandtlv
> TLV Value Invalid | r6imentstacharsp-tlvvalinval
> Unknown TLV | r6imentstacharsp-unknowntlv
> Duplicate TLV Found | r6imentstacharsp-duptlvfound
> No Session Found | r6imentstacharsp-nosessfound
> Admin Prohibited | r6imentstacharsp-admprohibit
> No Resource Drops | r6imentstacharsp-noresourcedrop
> Trans ID Error | r6imentstacharsp-transiderr
> ASNPC Statistics / R6 Messages / R6 Idle Mode Entry MS State Change Ack Msg | Total Sent | r6imentstachaack-totsent
> Retransmissions Sent | r6imentstachaack-retranssent
> Total Send Failures | r6imentstachaack-totsendfail
> Total Received | r6imentstachaack-totrec
> Total Accepted | r6imentstachaack-totacc
> Trans ID Error | r6imentstachaack-transiderr
> ASNPC Statistics / R6 Messages / R6 Idle Mode Exit MS State Change Request Msg | Total Sent | r6imexitstachareq-totsent
> | Retransmissions Sent | r6imexitstachareq-retranssent
> | Total Send Failures | r6imexitstachareq-totsendfail
> | Total Received | r6imexitstachareq-totrec
> | Total Accepted | r6imexitstachareq-totacc
> | Total Relayed | r6imexitstachareq-totrelay
> | Total Denied | r6imexitstachareq-totdenied
> | Total Discarded | r6imexitstachareq-totdiscard
> | Badly Formed | r6imexitstachareq-badform
> | Decode Error | r6imexitstachareq-decodeerr
> | Unspecified Error | r6imexitstachareq-unspecerr
> | Missing Mandatory TLV | r6imexitstachareq-missmandtlv
> | TLV Value Invalid | r6imexitstachareq-tlvvalinval
> | Unknown TLV | r6imexitstachareq-unknowntlv
> | Duplicate TLV Found | r6imexitstachareq-duptlvfound
> | No Session Found | r6imexitstachareq-nosessfound
> | Admin Prohibited | r6imexitstachareq-admprohibit
> | No Resource Drops | r6imexitstachareq-noresourcedrop
> | Trans ID Error | r6imexitstachareq-transiderr
> ASNPC Statistics / R6 Messages / R6 Idle Mode Exit MS State Change Response Msg | Total Sent | r6imexitstacharsp-totsent
> Retransmissions Sent | r6imexitstacharsp-retranssent
> Total Send Failures | r6imexitstacharsp-totsendfail
> Total Received | r6imexitstacharsp-totrec
> Total Accepted | r6imexitstacharsp-totacc
> Total Relayed | r6imexitstacharsp-totrelay
> Total Denied | r6imexitstacharsp-totdenied
> Total Discarded | r6imexitstacharsp-totdiscard
> Badly Formed | r6imexitstacharsp-badform
> Decode Error | r6imexitstacharsp-decodeerr
> Unspecified Error | r6imexitstacharsp-unspecerr
> Missing Mandatory TLV | r6imexitstacharsp-missmandtlv
> TLV Value Invalid | r6imexitstacharsp-tlvvalinval
> Unknown TLV | r6imexitstacharsp-unknowntlv
> Duplicate TLV Found | r6imexitstacharsp-duptlvfound
> No Session Found | r6imexitstacharsp-nosessfound
> Admin Prohibited | r6imexitstacharespadmprohibit
> No Resource Drops | r6imexitstacharsp-noresourcedrop
> Trans ID Error | r6imexitstacharsp-transiderr
> ASNPC Statistics / R6 Messages / R6 Location Update Request Msg | Total Sent | r6locupdreq-totsent
> Retransmissions Sent | r6locupdreq-retranssent
> Total Send Failures | r6locupdreq-totsendfail
> Total Received | r6locupdreq-totrec
> Total Accepted | r6locupdreq-totacc
> Total Relayed | r6locupdreq-totrelay
> Total Denied | r6locupdreq-totdenied
> Total Discarded | r6locupdreq-totdiscard
> Badly Formed | r6locupdreq-badform
> Decode Error | r6locupdreq-decodeerr
> Unspecified Error | r6locupdreq-unspecerr
> Missing Mandatory TLV | r6locupdreq-missmandtlv
> TLV Value Invalid | r6locupdreq-tlvvalinval
> Unknown TLV | r6locupdreq-unknowntlv
> Duplicate TLV Found | r6locupdreq-duptlvfound
> No Session Found | r6locupdreq-nosessfound
> Admin Prohibited | r6locupdreq-admprohibit
> No Resource Drops | r6locupdreq-noresourcedrop
> Trans ID Error | r6locupdreq-transiderr
> ASNPC Statistics / R6 Messages / R6 Location Update Response Msg | Total Sent | r6locupdrsp-totsent
> Retransmissions Sent | r6locupdrsp-retranssent
> Total Send Failures | r6locupdrsp-totsendfail
> Total Received | r6locupdrsp-totrec
> Total Accepted | r6locupdrsp-totacc
> Total Relayed | r6locupdrsp-totrelay
> Total Denied | r6locupdrsp-totdenied
> Total Discarded | r6locupdrsp-totdiscard
> Badly Formed | r6locupdrsp-badform
> Decode Error | r6locupdrsp-decodeerr
> Unspecified Error | r6locupdrsp-unspecerr
> Missing Mandatory TLV | r6locupdrsp-missmandtlv
> TLV Value Invalid | r6locupdrsp-tlvvalinval
> Unknown TLV | r6locupdrsp-unknowntlv
> Duplicate TLV Found | r6locupdrsp-duptlvfound
> No Session Found | r6locupdrsp-nosessfound
> Admin Prohibited | r6locupdreq-admprohibit
> No Resource Drops | r6locupdrsp-noresourcedrop
> Trans ID Error | r6locupdrsp-transiderr
> ASNPC Statistics / R6 Messages / R6 Location Update Confirm Msg | Total Sent | r6locupdcnf-totsent
> Retransmissions Sent | r6locupdcnf-retranssent
> Total Send Failures | r6locupdcnf-totsendfail
> Total Received | r6locupdcnf-totrec
> Total Accepted | r6locupdcnf-totacc
> Total Relayed | r6locupdcnf-totrelay
> Total Denied | r6locupdcnf-totdenied
> Total Discarded | r6locupdcnf-totdiscard
> Badly Formed | r6locupdcnf-badform
> Decode Error | r6locupdcnf-decodeerr
> Unspecified Error | r6locupdcnf-unspecerr
> Missing Mandatory TLV | r6locupdcnf-missmandtlv
> TLV Value Invalid | r6locupdcnf-tlvvalinval
> Unknown TLV | r6locupdcnf-unknowntlv
> Duplicate TLV Found | r6locupdcnf-duptlvfound
> No Session Found | r6locupdcnf-nosessfound
> Admin Prohibited | r6locupdcnf-admprohibit
> No Resource Drops | r6locupdcnf-noresourcedrop
> Trans ID Error | r6locupdcnf-transiderr
> ASNPC Statistics / R6 Messages / R6 Paging Announce Msg | Total Sent | r6pagannouce-totsent
> Retransmissions Sent | r6pagannouce-retranssent
> Total Send Failures | r6pagannouce-totsendfail
> Total Received | r6pagannouce-totrec
> Total Accepted | r6pagannouce-totacc
> Total Relayed | r6pagannouce-totrelay
> Total Denied | r6pagannouce-totdenied
> Total Discarded | r6pagannouce-totdiscard
> Badly Formed | r6pagannouce-badform
> Decode Error | r6pagannouce-decodeerr
> Unspecified Error | r6pagannouce-unspecerr
> Missing Mandatory TLV | r6pagannouce-missmandtlv
> TLV Value Invalid | r6pagannouce-tlvvalinval
> Unknown TLV | r6pagannouce-unknowntlv
> Duplicate TLV Found | r6pagannouce-duptlvfound
> No Session Found | r6pagannouce-nosessfound
> Admin Prohibited | r6pagannouce-admprohibit
> No Resource Drops | r6pagannouce-noresourcedrop
> Trans ID Error | r6pagannouce-transiderr
> ASNPC Statistics / R6 Messages / R6 Keep Alive Request Msg | Total Received | r6keepalivereq-totrec
> Total Accepted | r6keepalivereq-totacc
> Total Relayed | r6keepalivereq-totrelay
> Total Denied | r6keepalivereq-totdenied
> Total Discarded | r6keepalivereq-totdiscard
> Badly Formed | r6keepalivereq-badform
> Decode Error | r6keepalivereq-decodeerr
> Unspecified Error | r6keepalivereq-unspecerr
> Missing Mandatory TLV | r6keepalivereq-missmandtlv
> TLV Value Invalid | r6keepalivereq-tlvvalinval
> Unknown TLV | r6keepalivereq-unknowntlv
> Duplicate TLV Found | r6keepalivereq-duptlvfound
> No Session Found | r6keepalivereq-nosessfound
> Admin Prohibited | r6keepalivereq-admprohibit
> No Resource Drops | r6keepalivereq-noresourcedrop
> Trans ID Error | r6keepalivereq-transiderr
> ASNPC Statistics / R6 Messages / R6 Keep Alive Response Msg | Total Sent | r6keepaliversp-totsent
> Retransmissions Sent | r6keepaliversp-retranssent
> Total Send Failures | r6keepaliversp-totsendfail
> ASNPC Statistics / R6 Messages / R6 Unknown Messages | Total Received | r6unknown-totrec
> Total Accepted | r6unknown-totacc
> Total Relayed | r6unknown-totrelay
> Total Denied | r6unknown-totdenied
> Total Discarded | r6unknown-totdiscard
> Badly Formed | r6unknown-badform
> Decode Error | r6unknown-decodeerr
> Unspecified Error | r6unknown-unspecerr
> Missing Mandatory TLV | r6unknown-missmandtlv
> TLV Value Invalid | r6unknown-tlvvalinval
> Unknown TLV | r6unknown-unknowntlv
> Duplicate TLV Found | r6unknown-duptlvfound
> No Session Found | r6unknown-nosessfound
> Admin Prohibited | r6unknown-admprohibit
> No Resource Drops | r6unknown-noresourcedrop
> Trans ID Error | r6unknown-transiderr
> ASNPC Statistics / R4 Messages / R4 Idle Mode Entry MS State Change Request Msg | Total Sent | r4imentstachareq-totsent
> Retransmissions Sent | r4imentstachareq-retranssent
> Total Send Failures | r4imentstachareq-totseTrans ID Error: ndfail
> Total Received | r4imentstachareq-totrec
> Total Accepted | r4imentstachareq-totacc
> Total Relayed | r4imentstachareq-totrelay
> Total Denied | r4imentstachareq-totdenied
> Total Discarded | r4imentstachareq-totdiscard
> Badly Formed | r4imentstachareq-badform
> Decode Error | r4imentstachareq-decodeerr
> Unspecified Error | r4imentstachareq-unspecerr
> Missing Mandatory TLV | r4imentstachareq-missmandtlv
> TLV Value Invalid | r4imentstachareq-tlvvalinval
> Unknown TLV | r4imentstachareq-unknowntlv
> Duplicate TLV Found | r4imentstachareq-duptlvfound
> No Session Found | r4imentstachareq-nosessfound
> Admin Prohibited | r4imentstachareq-admprohibit
> No Resource Drops | r4imentstachareq-noresourcedrop
> Trans ID Error | r4imentstachareq-transiderr
> ASNPC Statistics / R4 Messages / R4 Idle Mode Entry MS State Change Response Msg | Total Sent | r4imentstacharsp-totsent
> Retransmissions Sent | r4imentstacharsp-retranssent
> Total Send Failures | r4imentstacharsp-totsendfail
> Total Received | r4imentstacharsp-totrec
> Total Accepted | r4imentstacharsp-totacc
> Total Relayed | r4imentstacharsp-totrelay
> Total Denied | r4imentstacharsp-totdenied
> Total Discarded | r4imentstacharsp-totdiscard
> Badly Formed | r4imentstacharsp-badform
> Decode Error | r4imentstacharsp-decodeerr
> Unspecified Error | r4imentstacharsp-unspecerr
> Missing Mandatory TLV | r4imentstacharsp-missmandtlv
> TLV Value Invalid | r4imentstacharsp-tlvvalinval
> Unknown TLV | r4imentstacharsp-unknowntlv
> Duplicate TLV Found | r4imentstacharsp-duptlvfound
> No Session Found | r4imentstacharsp-nosessfound
> Admin Prohibited | r4imentstacharsp-admprohibit
> No Resource Drops | r4imentstacharsp-noresourcedrop
> Trans ID Error | r4imentstacharsp-transiderr
> ASNPC Statistics / R4 Messages / R4 Idle Mode Entry MS State Change Ack Msg | Total Sent | r4imentstachaack-totsent
> Retransmissions Sent | r4imentstachaack-retranssent
> Total Send Failures | r4imentstachaack-totsendfail
> Total Received | r4imentstachaack-totrec
> Total Accepted | r4imentstachaack-totacc
> Total Relayed | r4imentstachaack-totrelay
> Total Denied | r4imentstachaack-totdenied
> Total Discarded | r4imentstachaack-totdiscard
> Badly Formed | r4imentstachaack-badform
> Decode Error | r4imentstachaack-decodeerr
> Unspecified Error | r4imentstachaack-unspecerr
> Missing Mandatory TLV | r4imentstachaack-missmandtlv
> TLV Value Invalid | r4imentstachaack-tlvvalinval
> Unknown TLV | r4imentstachaack-unknowntlv
> Duplicate TLV Found | r4imentstachaack-duptlvfound
> No Session Found | r4imentstachaack-nosessfound
> Admin Prohibited | r4imentstachaack-admprohibit
> No Resource Drops | r4imentstachaack-noresourcedrop
> Trans ID Error | r4imentstachaack-transiderr
> ASNPC Statistics / R4 Messages / R4 Idle Mode Exit MS State Change Request Msg | Total Sent | r4imexitstachareq-totsent
> Retransmissions Sent | r4imexitstachareq-retranssent
> Total Send Failures | r4imexitstachareq-totsendfail
> Total Received | r4imexitstachareq-totrec
> Total Accepted | r4imexitstachareq-totacc
> Total Relayed | r4imexitstachareq-totrelay
> Total Denied | r4imexitstachareq-totdenied
> Total Discarded | r4imexitstachareq-totdiscard
> Badly Formed | r4imexitstachareq-badform
> Decode Error | r4imexitstachareq-decodeerr
> Unspecified Error | r4imexitstachareq-unspecerr
> Missing Mandatory TLV | r4imexitstachareq-missmandtlv
> TLV Value Invalid | r4imexitstachareq-tlvvalinval
> Unknown TLV | r4imexitstachareq-unknowntlv
> Duplicate TLV Found | r4imexitstachareq-duptlvfound
> No Session Found | r4imexitstachareq-nosessfound
> Admin Prohibited | r4imexitstachareq-admprohibit
> No Resource Drops | r4imexitstachareq-noresourcedrop
> Trans ID Error | r4imexitstachareq-transiderr
> ASNPC Statistics / R4 Messages / R4 Idle Mode Exit MS State Change Response Msg | Total Sent | r4imexitstacharsp-totsent
> Retransmissions Sent | r4imexitstacharsp-retranssent
> Total Send Failures | r4imexitstacharsp-totsendfail
> Total Received | r4imexitstacharsp-totrec
> Total Accepted | r4imexitstacharsp-totacc
> Total Relayed | r4imexitstacharsp-totrelay
> Total Denied | r4imexitstacharsp-totdenied
> Total Discarded | r4imexitstacharsp-totdiscard
> Badly Formed | r4imexitstacharsp-badform
> Decode Error | r4imexitstacharsp-decodeerr
> Unspecified Error | r4imexitstacharsp-unspecerr
> Missing Mandatory TLV | r4imexitstacharsp-missmandtlv
> TLV Value Invalid | r4imexitstacharsp-tlvvalinval
> Unknown TLV | r4imexitstacharsp-unknowntlv
> Duplicate TLV Found | r4imexitstacharsp-duptlvfound
> No Session Found | r4imexitstacharsp-nosessfound
> Admin Prohibited | r4imexitstacharsp-admprohibit
> No Resource Drops | r4imexitstacharsp-noresourcedrop
> Trans ID Error | r4imexitstacharsp-transiderr
> ASNPC Statistics / R4 Messages / R4 Initiate Paging Request Msg | Total Sent | r4inipagreq-totsent
> Retransmissions Sent | r4inipagreq-retranssent
> Total Send Failures | r4inipagreq-totsendfail
> Total Received | r4inipagreq-totrec
> Total Accepted | r4inipagreq-totacc
> Total Relayed | r4inipagreq-totrelay
> Total Denied | r4inipagreq-totdenied
> Total Discarded | r4inipagreq-totdiscard
> Badly Formed | r4inipagreq-badform
> Decode Error | r4inipagreq-decodeerr
> Unspecified Error | r4inipagreq-unspecerr
> Missing Mandatory TLV | r4inipagreq-missmandtlv
> TLV Value Invalid | r4inipagreq-tlvvalinval
> Unknown TLV | r4inipagreq-unknowntlv
> Duplicate TLV Found | r4inipagreq-duptlvfound
> No Session Found | r4inipagreq-nosessfound
> Admin Prohibited | r4inipagreq-admprohibit
> No Resource Drops | r4inipagreq-noresourcedrop
> Trans ID Error | r4inipagreq-transiderr
> ASNPC Statistics / R4 Messages / R4 Initiate Paging Response Msg | Total Sent | r4inipagrsp-totsent
> | Retransmissions Sent | r4inipagrsp-retranssent
> | Total Send Failures | r4inipagrsp-totsendfail
> | Total Received | r4inipagrsp-totrec
> | Total Accepted | r4inipagrsp-totacc
> | Total Relayed | r4inipagrsp-totrelay
> | Total Denied | r4inipagrsp-totdenied
> | Total Discarded | r4inipagrsp-totdiscard
> | Badly Formed | r4inipagrsp-badform
> | Decode Error | r4inipagrsp-decodeerr
> | Unspecified Error | r4inipagrsp-unspecerr
> | Missing Mandatory TLV | r4inipagrsp-missmandtlv
> | TLV Value Invalid | r4inipagrsp-tlvvalinval
> | Unknown TLV | r4inipagrsp-unknowntlv
> | Duplicate TLV Found | r4inipagrsp-duptlvfound
> | No Session Found | r4inipagresp-nosessfound
> | Admin Prohibited | r4inipagrsp-admprohibit
> | No Resource Drops | r4inipagrsp-noresourcedrop
> | Trans ID Error | r4inipagrsp-transiderr
> ASNPC Statistics / R4 Messages / R4 Network Exit MS State Change Request Msg | Total Sent | r4nwexitmsstachareq-totsent
> | Retransmissions Sent | r4nwexitmsstachareq-retranssent
> | Total Send Failures | r4nwexitmsstachareq-totsendfail
> | Total Received | r4nwexitmsstachareq-totrec
> | Total Accepted | r4nwexitmsstachareq-totacc
> | Total Relayed | r4nwexitmsstachareq-totrelay
> | Total Denied | r4nwexitmsstachareq-totdenied
> | Total Discarded | r4nwexitmsstachareq-totdiscard
> | Badly Formed | r4nwexitmsstachareq-badform
> | Decode Error | r4nwexitmsstachareq-decodeerr
> | Unspecified Error | r4nwexitmsstachareq-unspecerr
> | Missing Mandatory TLV | r4nwexitmsstachareq-missmandtlv
> | TLV Value Invalid | r4nwexitmsstachareq-tlvvalinval
> | Unknown TLV | r4nwexitmsstachareq-unknowntlv
> | Duplicate TLV Found | r4nwexitmsstachareq-duptlvfound
> | No Session Found | r4nwexitmsstachareq-nosessfound
> | Admin Prohibited | r4nwexitmsstachareq-admprohibit
> | No Resource Drops | r4nwexitmsstachareq-noresourcedrop
> | Trans ID Error | r4nwexitmsstachareq-transiderr
> ASNPC Statistics / R4 Messages / R4 Net Work Exit MS State Change Request Msg | Total Sent | r4nwexitmsstacharsp-totsent
> Retransmissions Sent | r4nwexitmsstacharsp-retranssent
> Total Send Failures | r4nwexitmsstacharsp-totsendfail
> Total Received | r4nwexitmsstacharsp-totrec
> Total Accepted | r4nwexitmsstacharsp-totacc
> Total Relayed | r4nwexitmsstacharsp-totrelay
> Total Denied | r4nwexitmsstacharsp-totdenied
> Total Discarded | r4nwexitmsstacharsp-totdiscard
> Badly Formed | r4nwexitmsstacharsp-badform
> Decode Error | r4nwexitmsstacharsp--decodeerr
> Unspecified Error | r4nwexitmsstacharsp-unspecerr
> Missing Mandatory TLV | r4nwexitmsstacharsp-missmandtlv
> TLV Value Invalid | r4nwexitmsstacharsp-tlvvalinval
> Unknown TLV | r4nwexitmsstacharsp-unknowntlv
> Duplicate TLV Found | r4nwexitmsstacharsp-duptlvfound
> No Session Found | r4nwexitmsstacharsp-nosessfound
> Admin Prohibited | r4nwexitmsstacharsp-admprohibit
> No Resource Drops | r4nwexitmsstacharsp-noresourcedrop
> Trans ID Error | r4nwexitmsstacharsp-transiderr
> ASNPC Statistics / R4 Messages / R4 Delete MS Entry Request Msg | Total Sent | r4delmsentreq-totsent
> Retransmissions Sent | r4delmsentreq-retranssent
> Total Send Failures | r4delmsentreq-totsendfail
> Total Received | r4delmsentreq-totrec
> Total Accepted | r4delmsentreq-totacc
> Total Relayed | r4delmsentreq-totrelay
> Total Denied | r4delmsentreq-totdenied
> Total Discarded | r4delmsentreq-totdiscard
> Badly Formed | r4delmsentreq-badform
> Decode Errorr4delmsentreq-tlvvalinval | r4delmsentreq-decodeerr
> Unspecified Error | r4delmsentreq-unspecerr
> Missing Mandatory TLV | r4delmsentreq-missmandtlv
> TLV Value Invalid | r4delmsentreq-tlvvalinval
> Unknown TLV | r4delmsentreq-unknowntlv
> Duplicate TLV Found | r4delmsentreq-duptlvfound
> No Session Found | r4delmsentreq-nosessfound
> Admin Prohibited | r4delmsentreq-admprohibit
> No Resource Drops | r4delmsentreq-noresourcedrop
> Trans ID Error | r4delmsentreq-transiderr
> ASNPC Statistics / R4 Messages / R4 Delete MS Entry Response Msg | Total Sent | r4delmsentrsp-totsent
> Retransmissions Sent | r4delmsentrsp-retranssent
> Total Send Failures | r4delmsentrsp-totsendfail
> Total Received | r4delmsentrsp-totrec
> Total Accepted | r4delmsentrsp-totacc
> Total Relayed | r4delmsentrsp-totrelay
> Total Denied | r4delmsentrsp-totdenied
> Total Discarded | r4delmsentrsp-totdiscard
> Badly Formed | r4delmsentrsp-badform
> Decode Error | r4delmsentrsp-decodeerr
> Unspecified Error | r4delmsentrsp-unspecerr
> Missing Mandatory TLV | r4delmsentrsp-missmandtlv
> TLV Value Invalid | r4delmsentrsp-tlvvalinval
> Unknown TLV | r4delmsentrsp-unknowntlv
> Duplicate TLV Found | r4delmsentrsp-duptlvfound
> No Session Found | r4delmsentrsp-nosessfound
> Admin Prohibited | r4delmsentrsp-admprohibit
> No Resource Drops | r4delmsentrsp-noresourcedrop
> Trans ID Error | r4delmsentrsp-transiderr
> ASNPC Statistics / R4 Messages / R4 Anchor PC Ind Msg | Total Sent | r4anchorpcind-totsent
> Retransmissions Sent | r4anchorpcind-retranssent
> Total Send Failures | r4anchorpcind-totsendfail
> Total Received | r4anchorpcind-totrec
> Total Accepted | r4anchorpcind-totacc
> Total Relayed | r4anchorpcind-totrelay
> Total Denied | r4anchorpcind-totdenied
> Total Discarded | r4anchorpcind-totdiscard
> Badly Formed | r4anchorpcind-badform
> Decode Error | r4anchorpcind-decodeerr
> Unspecified Error | r4anchorpcind-unspecerr
> Missing Mandatory TLV | r4anchorpcind-missmandtlv
> TLV Value Invalid | r4anchorpcind-tlvvalinval
> Unknown TLV | r4anchorpcind-unknowntlv
> Duplicate TLV Found | r4anchorpcind-duptlvfound
> No Session Found | r4anchorpcind-nosessfound
> Admin Prohibited | r4anchorpcind-admprohibit
> No Resource Drops | r4anchorpcind-noresourcedrop
> Trans ID Error | r4anchorpcind-transiderr
> ASNPC Statistics / R4 Messages / R4 Anchor PC Ack Msg | Total Sent | r4anchorpcack-totsent
> | Retransmissions Sent | r4anchorpcack-retranssent
> | Total Send Failures | r4anchorpcack-totsendfail
> | Total Received | r4anchorpcack-totrec
> | Total Accepted | r4anchorpcack-totacc
> | Total Relayed | r4anchorpcack-totrelay
> | Total Denied | r4anchorpcack-totdenied
> | Total Discarded | r4anchorpcack-totdiscard
> | Badly Formed | r4anchorpcack-badform
> | Decode Error | r4anchorpcack-decodeerr
> | Unspecified Error | r4anchorpcack-unspecerr
> | Missing Mandatory TLV | r4anchorpcack-missmandtlv
> | TLV Value Invalid | r4anchorpcack-tlvvalinval
> | Unknown TLV | r4anchorpcack-unknowntlv
> | Duplicate TLV Found | r4anchorpcack-duptlvfound
> | No Session Found | r4anchorpcack-nosessfound
> | Admin Prohibited | r4anchorpcack-admprohibit
> | No Resource Drops | r4anchorpcack-noresourcedrop
> | Trans ID Error | r4anchorpcack-transiderr
> ASNPC Statistics / R4 Messages / R4 Location Update Request Msg | Total Sent | r4locupdreq-totsent
> Retransmissions Sent | r4locupdreq-retranssent
> Total Send Failures | r4locupdreq-totsendfail
> Total Received | r4locupdreq-totrec
> Total Accepted | r4locupdreq-totacc
> Total Relayed | r4locupdreq-totrelay
> Total Denied | r4locupdreq-totdenied
> Total Discarded | r4locupdreq-totdiscard
> Badly Formed | r4locupdreq-badform
> Decode Error | r4locupdreq-decodeerr
> Unspecified Error | r4locupdreq-unspecerr
> Missing Mandatory TLV | r4locupdreq-missmandtlv
> TLV Value Invalid | r4locupdreq-tlvvalinval
> Unknown TLV | r4locupdreq-unknowntlv
> Duplicate TLV Found | r4locupdreq-duptlvfound
> No Session Found | r4locupdreq-nosessfound
> Admin Prohibited | r4locupdreq-admprohibit
> No Resource Drops | r4locupdreq-noresourcedrop
> Trans ID Error | r4locupdreq-transiderr
> ASNPC Statistics / R4 Messages / R4 Location Update Response Msg | Total Sent | r4locupdrsp-totsent
> Retransmissions Sent | r4locupdrsp-retranssent
> Total Send Failures | r4locupdrsp-totsendfail
> Total Received | r4locupdrsp-totrec
> Total Accepted | r4locupdrsp-totacc
> Total Relayed | r4locupdrsp-totrelay
> Total Denied | r4locupdrsp-totdenied
> Total Discarded | r4locupdrsp-totdiscard
> Badly Formed | r4locupdrsp-badform
> Decode Error | r4locupdrsp-decodeerr
> Unspecified Error | r4locupdrsp-unspecerr
> Missing Mandatory TLV | r4locupdrsp-missmandtlv
> TLV Value Invalid | r4locupdrsp-tlvvalinval
> Unknown TLV | r4locupdrsp-unknowntlv
> Duplicate TLV Found | r4locupdrsp-duptlvfound
> No Session Found | r4locupdrsp-nosessfound
> Admin Prohibited | r4locupdrsp-admprohibit
> No Resource Drops | r4locupdrsp-noresourcedrop
> Trans ID Error | r4locupdrsp-transiderr
> ASNPC Statistics / R4 Messages / R4 Location Update Confirm Msg | Total Sent | r4locupdcnf-totsent
> Retransmissions Sent | r4locupdcnf-retranssent
> Total Send Failures | r4locupdcnf-totsendfail
> Total Received | r4locupdcnf-totrec
> Total Accepted | r4locupdcnf-totacc
> Total Relayed | r4locupdcnf-totrelay
> Total Denied | r4locupdcnf-totdenied
> Total Discarded | r4locupdcnf-totdiscard
> Badly Formed | r4locupdcnf-badform
> Decode Error | r4locupdcnf-decodeerr
> Unspecified Error | r4locupdcnf-unspecerr
> Missing Mandatory TLV | r4locupdcnf-missmandtlv
> TLV Value Invalid | r4locupdcnf-tlvvalinval
> Unknown TLV | r4locupdcnf-unknowntlv
> Duplicate TLV Found | r4locupdcnf-duptlvfound
> No Session Found | r4locupdcnf-nosessfound
> Admin Prohibited | r4locupdcnf-admprohibit
> No Resource Drops | r4locupdcnf-noresourcedrop
> Trans ID Error | r4locupdcnf-transiderr
> ASNPC Statistics / R4 Messages / R4 PC Relocation Ind Msg | Total Sent | r4pcrelocind-totsent
> | Retransmissions Sent | r4pcrelocind-retranssent
> | Total Send Failures | r4pcrelocind-totsendfail
> | Total Received | r4pcrelocind-totrec
> | Total Accepted | r4pcrelocind-totacc
> | Total Relayed | r4pcrelocind-totrelay
> | Total Denied | r4pcrelocind-totdenied
> | Total Discarded | r4pcrelocind-totdiscard
> | Badly Formed | r4pcrelocind-badform
> | Decode Error | r4pcrelocind-decodeerr
> | Unspecified Error | r4pcrelocind-unspecerr
> | Missing Mandatory TLV | r4pcrelocind-missmandtlv
> | TLV Value Invalid | r4pcrelocind-tlvvalinval
> | Unknown TLV | r4pcrelocind-unknowntlv
> | Duplicate TLV Found | r4pcrelocind-duptlvfound
> | No Session Found | r4pcrelocind-nosessfound
> | Admin Prohibited | r4pcrelocind-admprohibit
> | No Resource Drops | r4pcrelocind-noresourcedrop
> | Trans ID Error | r4pcrelocind-transiderr
> ASNPC Statistics / R4 Messages / R4 PC Relocation Ack Msg | Total Sent | r4pcrelocack-totsent
> Retransmissions Sent | r4pcrelocack-retranssent
> Total Send Failures | r4pcrelocack-totsendfail
> Total Received | r4pcrelocack-totrec
> Total Accepted | r4pcrelocack-totacc
> Total Relayed | r4pcrelocack-totrelay
> Total Denied | r4pcrelocack-totdenied
> Total Discarded | r4pcrelocack-totdiscard
> Badly Formed | r4pcrelocack-badform
> Decode Error | r4pcrelocack-decodeerr
> Unspecified Error | r4pcrelocack-unspecerr
> Missing Mandatory TLV | r4pcrelocack-missmandtlv
> TLV Value Invalid | r4pcrelocack-tlvvalinval
> Unknown TLV | r4pcrelocack-unknowntlv
> Duplicate TLV Found | r4pcrelocack-duptlvfound
> No Session Found | r4pcrelocack-nosessfound
> Admin Prohibited | r4pcrelocack-admprohibit
> No Resource Drops | r4pcrelocack-noresourcedrop
> Trans ID Error | r4pcrelocack-transiderr
> ASNPC Statistics / R4 Messages / R4 Context Request Msg | Total Sent | r4contextreq-totsent
> Retransmissions Sent | r4contextreq-retranssent
> Total Send Failures | r4contextreq-totsendfail
> Total Received | r4contextreq-totrec
> Total Accepted | r4contextreq-totacc
> Total Relayed | r4contextreq-totrelay
> Total Denied | r4contextreq-totdenied
> Total Discarded | r4contextreq-totdiscard
> Badly Formed | r4contextreq-badform
> Decode Error | r4contextreq-decodeerr
> Unspecified Error | r4contextreq-unspecerr
> Missing Mandatory TLV | r4contextreq-missmandtlv
> TLV Value Invalid | r4contextreq-tlvvalinval
> Unknown TLV | r4contextreq-unknowntlv
> Duplicate TLV Found | r4contextreq-duptlvfound
> No Session Found | r4contextreq-nosessfound
> Admin Prohibited | r4contextreq-adminprohib
> No Resource Drops | r4contextreq-noresourcedrop
> Trans ID Error | r4contextreq-transiderr
> ASNPC Statistics / R4 Messages / R4 Context Report Msg | Total Sent | r4contextrpt-totsent
> Retransmissions Sent | r4contextrpt-retranssent
> Total Send Failures | r4contextrpt-totsendfail
> Total Received | r4contextrpt-totrec
> Total Accepted | r4contextrpt-totacc
> Total Relayed | r4contextrpt-totrelay
> Total Denied | r4contextrpt-totdenied
> Total Discarded | r4contextrpt-totdiscard
> Badly Formed | r4contextrpt-badform
> Decode Error | r4contextrpt-decodeerr
> Unspecified Error | r4contextrpt-unspecerr
> Missing Mandatory TLV | r4contextrpt-missmandtlv
> TLV Value Invalid | r4contextrpt-tlvvalinval
> Unknown TLV | r4contextrpt-unknowntlv
> Duplicate TLV Found | r4contextrpt-duptlvfound
> No Session Found | r4contextrpt-nosessfound
> Admin Prohibited | r4contextrpt-adminprohib
> No Resource Drops | r4contextrpt-noresourcedrop
> Trans ID Error | r4contextrpt-transiderr
> ASNPC Statistics / R4 Messages / R4 CMAC Key Count Update Msg | Total Sent | r4cmackeycountupd-totsent
> Retransmissions Sent | r4cmackeycountupd-retranssent
> Total Send Failures | r4cmackeycountupd-totsendfail
> Total Received | r4cmackeycountupd-totrec
> Total Accepted | r4cmackeycountupd-totacc
> Total Relayed | r4cmackeycountupd-totrelay
> Total Denied | r4cmackeycountupd-totdenied
> Total Discarded | r4cmackeycountupd-totdiscard
> Badly Formed | r4cmackeycountupd-badform
> Decode Error | r4cmackeycountupd-decodeerr
> Unspecified Error | r4cmackeycountupd-unspecerr
> Missing Mandatory TLV | r4cmackeycountupd-missmandtlv
> TLV Value Invalid | r4cmackeycountupd-tlvvalinval
> Unknown TLV | r4cmackeycountupd-unknowntlv
> Duplicate TLV Found | r4cmackeycountupd-duptlvfound
> No Session Found | r4cmackeycountupd-nosessfound
> Admin Prohibited | r4cmackeycountupd-adminprohib
> No Resource Drops | r4cmackeycountupd-noresourcedrop
> Trans ID Error | r4cmackeycountupd-transiderr
> ASNPC Statistics / R4 Messages / R4 CMAC Key Count Ack Msg | Total Sent | r4cmackeycountack-totsent
> Retransmissions Sent | r4cmackeycountack-retranssent
> Total Send Failures | r4cmackeycountack-totsendfail
> Total Received | r4cmackeycountack-totrec
> Total Accepted | r4cmackeycountack-totacc
> Total Relayed | r4cmackeycountack-totrelay
> Total Denied | r4cmackeycountack-totdenied
> Total Discarded | r4cmackeycountack-totdiscard
> Badly Formed | r4cmackeycountack-badform
> Decode Error | r4cmackeycountack-decodeerr
> Unspecified Error | r4cmackeycountack-unspecerr
> Missing Mandatory TLV | r4cmackeycountack-missmandtlv
> TLV Value Invalid | r4cmackeycountack-tlvvalinval
> Unknown TLV | r4cmackeycountack-unknowntlv
> Duplicate TLV Found | r4cmackeycountack-duptlvfound
> No Session Found | r4cmackeycountack-nosessfound
> Admin Prohibited | r4cmackeycountack-adminprohib
> No Resource Drops | r4cmackeycountack-noresourcedrop
> Trans ID Error | r4cmackeycountack-transiderr
> ASNPC Statistics / R4 Messages / R4 Unknown Messages | Total Received | r4unknown-totrec
> | Total Accepted | r4unknown-totacc
> | Total Relayed | r4unknown-totrelay
> | Total Denied | r4unknown-totdenied
> | Total Discarded | r4unknown-totdiscard
> | Badly Formed | r4unknown-badform
> | Decode Error | r4unknown-decodeerr
> | Unspecified Error | r4unknown-unspecerr
> | Missing Mandatory TLV | r4unknown-missmandtlv
> | TLV Value Invalid | r4unknown-tlvvalinval
> | Unknown TLV | r4unknown-unknowntlv
> | Duplicate TLV Found | r4unknown-duptlvfound
> | No Session Found | r4unknown-nosessfound
> | Admin Prohibited | r4unknown-admprohibit
> | No Resource Drops | r4unknown-noresourcedrop
> | Trans ID Error | r4unknown-transiderr
> ASNPC Statistics / R4 Messages / General | Total Sessions Connected | total-sessions-connected
> | Unknown TLV |

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> CSCF Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the CSCF schema in WEM Release 12.2.

> CSCF Schema Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> CSCF Schema / CSCF Service Statistics / Calls | Mobile Originating Calls Success Rate | mo-call-succ-rate
> Mobile Terminating Calls Success Rate | mt-call-succ-rate
> Mobile Originating VOICE Calls Success Rate | mo-voice-call-succ-rate
> Mobile Terminating VOICE Calls Success Rate | mt-voice-call-succ-rate
> Mobile Originating VIDEO Calls Success Rate | mo-video-call-succ-rate
> Mobile Terminating VIDEO Calls Success Rate | mt-video-call-succ-rate
> Total Emergency Privacy Calls | emerg-priv-calls
> Total RTCP Packets Sent | rtcp-sent
> Total MSRP Packets Sent | msrp-sent
> Total MSRP Packets Received | msrp-recv
> CSCF Schema / CSCF Registrations / Registration Statistics | 439 FirstHopLackOb (Registration) Received | reg-resp-439rx
> 439 FirstHopLackOb (Registration) Transmitted | reg-resp-439tx
> CSCF Schema / CSCF Registrations / Re-Registration Statistics | 439 FirstHopLackOb (Re-Registration) Received | rereg-resp-439rx
> 439 FirstHopLackOb (Re-Registration) Transmitted | rereg-resp-439tx
> CSCF Schema / CSCF Service Stats / CSCF Message Stats | 413 Request Entity Too Large Received | message-413-rx
> 413 Request Entity Too Large Transmitted | message-413-tx
> CSCF Schema / SIP TCP Connection Statistics | Total TCP Subscribers | sip-tcp-subs
> CSCF Schema / MSRP TCP Connection Statistics | Active Connections | msrp-active-tcp-conn
> Total Connections Closed | msrp-closed-tcp-conn
> Total Successful Outgoing Connections | msrp-succ-tcp-conn-out
> Total Failed Outgoing Connections | msrp-fail-tcp-conn-out
> Total Successful Incoming Connections | msrp-succ-tcp-conn-in
> Total Failed Incoming Connections | msrp-fail-tcp-conn-in
> Total Packets Received | msrp-packet-rx
> Total Packets Sent | msrp-packet-tx
> Total Bytes Received | msrp-bytes-rx
> Total Bytes Sent | msrp-bytes-tx
> Total MSRP Subscribers | msrp-tcp-subs
> CSCF Schema / CSCF SIP Statistics / SIP Response | Received - 439 First Hop Lack Outbound | fhloerrrx
> Transmitted - 439 First Hop Lack Outbound | fhloerrtx
> CSCF Schema / CSCF Statistics / CSCF Session Duration Counters | &lt;1sec | calldur-lt-01sec
> 01..10sec | calldur-01to10sec
> 10..30sec | calldur-10to30sec
> 30..60sec | calldur-30to60sec
> 60..90sec | calldur-60to90sec
> 90..120sec | calldur-90to120sec
> 120..150sec | calldur-120to150sec
> 150..180sec | calldur-150to180sec
> 03..04min | calldur-03to04min
> 04..05min | calldur-04to05min
> 05..06min | calldur-05to06min
> 06..07min | calldur-06to07min
> 07..08min | calldur-07to08min
> 08..09min | calldur-08to09min
> 09..11min | calldur-09to11min
> 11..13min | calldur-11to13min
> 13..15min | calldur-13to15min
> 15..17min | calldur-15to17min
> 17..19min | calldur-17to19min
> 19..21min | calldur-19to21min
> 21..23min | calldur-21to23min
> 23..25min | calldur-23to25min
> 25..27min | calldur-25to27min
> 27..29min | calldur-27to29min
> 29..60min | calldur-29to60min
> &gt;60min | calldur-gt-60min

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> RP Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the RP schema in WEM Release 12.2.

> RP Schema Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> RP / Session Update Send Reason | Always On Indication | sess-always-on-indication

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> CSCF-INTF Schema Bulk Statistic Enhancements
> The following bulk statistics have been added to the CSCF-INTF schema in WEM Release 12.2.

> CSCF-INTF Schema Bulk Statistic Enhancements in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> CSCF_INTF / SIP Response | 422 Session Interval Too Small - Received | sitserrrx
> 422 Session Interval Too Small - Transmitted: | sitserrtx
> 439 First Hop Lack Outbound - Received: | fhloerrrx
> 439 First Hop Lack Outbound - Transmitted | fhloerrtx
> CSCF_INTF / Calls | Mobile Originating Calls Success Rate | mo-call-succ-rate
> Mobile Terminating Calls Success Rate | mt-call-succ-rate
> Mobile Originating VOICE Calls Success Rate | mo-voice-call-succ-rate
> Mobile Terminating VOICE Calls Success Rate | mt-voice-call-succ-rate
> Mobile Originating VIDEO Calls Success Rate | mo-video-call-succ-rate
> Mobile Terminating VIDEO Calls Success Rate | mt-video-call-succ-rate

> Web Element Manager Path

> l | Accounting | Bulk Statistics Configuration | Schema Tab

> l | Accounting | View/Graph Bulk Statistics | Select Counters and Filters Parameters Tab

> Change to Threshold Description for Total HSGW Sessions
> The original entry in the Online Help for this HSGW counter read:
> “Configures the polling interval over which to count the forwarded packets.”
> This has been corrected to: “Configures the polling interval over which to count the total number of HSGW sessions on the system.”
> Web Element Manager Path

> l | Monitor Test Menu| Monitoring Operations Submenu | Thresholds | Descriptive Overview | Thresholds supported by the IMG

> Changes in Data Values to MME Schema Bulk Statistics
> The following mme bulk statistics data values have been changed from Incremental to Gauge.

> MME Bulk Statistic Schema Values Changed to Gauge in WEM Release 12.2
> WEM Bulk Statistic Schema Directory | WEM Display Name | CLI Counter Name
> MME Statistics | Attached Calls | emmcall-attach-currcall
> Maximum Calls | emmcall-attach-maxcall
> Current Calls | emmcall-connect-curcall
> Maximum Calls | emmcall-connect-maxcall
> Current Calls | emmcall-idle-curcall
> Maximum Calls | emmcall-idle-maxcall

> Web Element Manager Path
> On the WEM server: <ems_dir>/server/bsschema/mme_counter.xml

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883