> Bulk Statistics Configuration Mode Commands
> The Bulk Statistics Configuration Mode is used to manage the options for the collection, formatting and delivery of system statistics to remote nodes.
> Refer to the Common Syntax Options section in this chapter for information about formatting the output of bulk statistics.
> Important: Unless otherwise indicated, all statistics are counters. For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
> Overview
> Schema Format String Syntax
> The following defines common syntax block options. These options appear in similar commands and are detailed here for easy reference.
> The schema format string is used to define the structure of generated bulk statistics data. The string may contain static text, dynamic content, and bulk statistic variables, or any combination.
> Static text includes any ASCII characters that are of a fixed value. Static text may also include control characters by using Escape character sequences. Supported Escape character shortcuts are “\n” for new line and “\t” for tab.
> Enclosing an alphanumeric string within double quotation marks (“) allows you to include spaces in the string.
> Variables within the format string must be enclosed within “% and %”, for example, “%var%”. The actual variables supported are command-dependent and are described in the Statistics and Counters Reference.
> Common Statistics
> For a list of the statistics that are common to all schema, refer to the Statistics and Counters Reference.
> aal2 schema
> Configures the ATM adaptation layer 2 (AAL2) bulk statistics schema within an ATM virtual connection by the HNB-GW.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> aal2 schema schema_name format format_string
> no aal2 schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see the Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for ATM adaptation layer 2 (AAL2) bulk statistics collection. Multiple AAL2 schemas can be created to further categorize HNB-GW-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple AAL2 schemas, re-issue the aal2 schema schema_name command using a different schema name.
> Example
> The following command creates a schema called aal2stats1 that records the number of AAL2 uplink packets transmitted and AAL2 downlink packets received by Access Link Control Application Part (ALCAP) service on HNB-GW:
> aal2 schema aal2stats1 format “%uplink-pkts-tx%” “%downlink-pkts-rx%”
> alcap schema
> Configures the Access Link Control Application Part (ALCAP) bulk statistics schema for an ALCAP service on an HNB-GW node.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> alcap schema schema_name format format_string
> no alcap schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for Access Link Control Application Part (ALCAP) service bulk statistics collection on HNB-GW node. Multiple ALCAP schemas can be created to further categorize at AAL2 channel-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple ALCAP schemas, re-issue the alcap schema schema_name command using a different schema name.
> Example
> The following command creates a schema called alcap1stats1 that records the number of AAL2 channels in connecting and connected state on ALCAP service:
> alcap schema alcaplstats1 format “%num-aal2-channels-in-connecting%” “%num-aal2-channels-in-connected-state%”
> apn schema
> Configures the Access Point Name (APN) bulk statistics schema.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> apn schema schema_name format format_string
> no apn schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for APN bulk statistics collection. Multiple APN schemas can be created to further categorize APN-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple APN schemas, re-issue the apn schema schema_name command using a different schema name.
> Example
> The following command creates a schema called apn1stats1 that records the number of sessions currently facilitated by the APN:
> apn schema apn1stats1 format “%sess-curr%”
> asngw schema
> Configures Access Service Gateway (ASN-GW) bulk statistics schema.
> Product
> ASN GW
> Privilege
> Security Administrator, Administrator
> Syntax
> asngw schema schema_name format format_string
> no asngw schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format. as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for ASN-GW bulk statistics collection. Multiple ASN-GW service schemas can be created to further categorize ASN-GW service bulk statistics. All of the schemas are processed at each collection interval. To create multiple ASN-GW service schemas, re-issue the asngw schema schema_name command using a different schema name.
> Example
> To create an ASN-GW schema called asngw_statistics that specifies a schema format of:

> • | VPN context name: vpnname

> • | VPN Context Identifier: vpnid

> • | ASN-GW Service name: servname

> • | ASN-GW Service identifier: servid

> • | Peer IP address: peeripaddr

> Use the following command:
> asngw schema asngw_statistics format “VPN name: %vpnname%\nVPN ID: %vpnid%\nASN-GW Service Name: %servname%\nASN-GW Service Identifier: %servid%\nPeer IP Address: %peeripaddr%”
> bcmcs schema
> Configures Broadcast and Multicast Service (BCMCS) bulk statistics schema.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator
> Syntax
> bcmcs schema schema_name format format_string
> no bcmcs schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for BCMCS bulk statistics collection. Multiple BCMCS schemas can be created to further categorize BCMCS-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple BCMCS schemas, re-issue the bcmcs schema schema_name command using a different schema name.
> Example
> The following command creates a schema named bcmcs1stats1 that records the number of sessions currently facilitated by BCMCS:
> bcmcs schema bcmcs1stats1 format “%sess-curr%”
> card schema
> Configures card bulk statistics schema. These are statistics for circuit cards installed in the ASR 5x00 chassis.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> card schema schema_name format format_string
> no card schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for card bulk statistics collection. Multiple card schemas can be created to categorize card-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple card schemas, re-issue the card schema schema_name command using a different schema name.
> Important: Not supported on all platforms
> Example
> The following command creates a schema called card1stats1 that records the number of processes for all installed cards:
> card schema card1stats1 format “%slot%-%numproc%”
> To create a card-level schema called cardresourcestats that specifies a schema format of:

> • | Chassis slot number: slot

> • | Available Memory: memtotal Memory Used (%): memused

> • | Available CPU (%): cpuidle

> Use the following command:
> card schema cardresourcestats format “Chassis slot number: %slot%\nAvailable Memory: %memtotal%\tMemory Used (%): %memused%\nAvailable CPU (%): %cpuidle%”
> context schema
> Configures context bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> context schema schema_name format format_string
> no context schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema forma as an alphanumeric string of 1 through 3600 characters. For syntax details, see Schema Format String Syntax section.
> Important: For the complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for Context bulk statistics collection. Multiple context schemas can be created to categorize context statistics. All of the schemas are processed at each collection interval. To create multiple context schemas, re-issue the context schema schema_name command using a different schema name.
> Example
> To create a Firewall context schema called sfw_context_stats1 that specifies a schema format of:

> • | Total packets received by firewall: sfw-total-rxpackets

> • | Total packets sent by firewall: sfw-total-txpackets

> • | Total ICMP packets discarded by firewall: fw-icmp-discardpackets

> Use the following command:
> context schema sfw_context_stats1 format “Packets received Rx: %sfw-total-rxpackets%\nPackets Sent Tx:: %sfw-total-txpackets%\nICMP Packets discarded: %fw-icmp-discardpackets%”
> cscf schema
> Configures Call Session Control Function (CSCF) bulk statistics schema.
> Product
> SCM
> Privilege
> Security Administrator, Administrator
> Syntax
> cscf schema schema_name format format_string
> no cscf schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format. as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for CSCF bulk statistics collection. Multiple CSCF-service schemas can be created to categorize CSCF-service bulk statistics. All of the schemas are processed at each collection interval. To create multiple CSCF-service schemas, re-issue the cscf schema schema_name command using a different schema name.
> Example
> To create a CSCF schema called cscf_statistics that specifies a schema format of:

> • | Call attempts received: callattrx

> • | Call attempts transmitted: callatttx

> • | Call successes received: callsuccrx

> • | Call successes transmitted: callsucctx

> • | Call failures received: callfailrx

> • | Call failures transmitted: callfailtx

> Use the following command:
> cscf schema cscf_statistics format “Call Attempts Rx: %callattrx%\nCall Attempts Tx: %callatttx%\nCall Successes Rx: %callsuccrx%\nCall Successes Tx: %callsucctx%\nCall Failures Rx: %callfailrx%\nCall Failures Tx: %callfailtx%”
> cs-network-ranap
> Configures the Radio Access Network Application Part (RANAP) bulk statistics schema in a Circuit Switched (CS) network associated with an HNB-GW node.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> cs-network-ranap schema schema_name format format_string
> no cs-network-ranap schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for RANAP procedure related bulk statistics collection in a CS network associated with HNB-GW in a Femto UMTS network. Multiple CS Networks RANAP schemas can be created to further categorize at CS network or HNB-GW-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple CS Networks RANAP schemas, re-issue the cs-network-ranap schema schema_name command using a different schema name.
> Example
> The following command creates a schema called cs_ranap1stats1 that records the total number of Iu Release Request messages transmitted and total number of Iu Release Command message received by the HNB-GW node:
> cs-network-ranap schema cs_ranaplstats1 format “%iu-rel-req-tx%” “%iu-rel-cmd-rx%”
> cs-network-rtp
> Configures the Real-Time Transport Protocol (RTP) bulk statistics schema in a Circuit Switched (CS) network associated with an HNB-GW node.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> cs-network-rtp schema schema_name format format_string
> no cs-network-rtp schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for RTP procedure related bulk statistics collection in a CS network associated with HNB-GW in a Femto UMTS network. Multiple CS Networks RTP schemas can be created to further categorize at CS network or HNB-GW-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple CS Networks RTP schemas, re-issue the cs-network-rtp schema schema_name command using a different schema name.
> Example
> The following command creates a schema called cs_rtp1stats1 that records the total number of RTP Downlink Packets received and RTP Uplink Packets transmitted by HNB-GW node in an associated CS network:
> cs-network-rtp schema cs_rtplstats1 format “%rtp-uplink-pkts-tx%” “%rtp-downlink-pkts-rx%”
> dcca schema
> Configures Diameter Credit Control Application (DCCA) bulk statistics schema. This command is available only in 9.0 and later releases.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> dcca schema schema_name format format_string
> no dcca schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for DCCA bulk statistics collection.
> default
> Restores the system default for the option specified.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> default { limit | receiver mode | remotefile format | sample-interval | transfer-interval }
> limit
> Restores the memory utilization limit system default: 1000 kilobytes.
> receiver mode
> Restores the behavior for sending files to the receivers to the default value.
> Default: secondary-on-failure
> remotefile format
> Restores the format of remote bulkstats file names to the default value.
> Default: “%date%-%time%”
> sample-interval
> Restores the system default for the local polling interval for statistic sampling.
> Default: 15 minutes
> transfer-interval
> Restores the system default for the time between transfer of data files to receivers.
> Default: 480 minutes
> Usage
> Restore the default values when troubleshooting the system. Setting values to the system defaults places them in well known states as starting points for monitoring for problems.
> Example
> default limit
> default transfer-interval
> diameter-acct schema
> Configures Diameter Accounting bulk statistics schema. This command is available only in 11.0 and later releases.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> diameter-acct schema schema_name format format_string
> no diameter-acct schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for Diameter Accounting bulk statistics collection.
> diameter-auth schema
> Configures Diameter Authentication bulk statistics schema. This command is available only in 11.0 and later releases.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> diameter-auth schema schema_name format format_string
> no diameter-auth schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for Diameter Authentication bulk statistics collection.
> dlci-util schema
> Configures the collection of statistics for the DLCI-Util (DLCI utilization) schema.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> dlci-util schema dlci_schema_name format dlci_schema_format
> no dlci-util schema dlci_schema_name
> no
> Removes the specified schema.
> dlci_schema_name
> Specifies a name for a model collection schema for DLCI utilization statistics. The name must be comprised of an alphanumeric string of 1 to 31 characters.
> format dlci_schema_format
> Specifies the format of the collected DLCI utilization statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters. For syntax details, see the Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for the DLCI-Util schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for DLCI-Util bulk statistics collection in the generated stats report files.. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple schemas can be created to categorize DLCI-Util bulk statistics. All of the schemas are processed at each collection interval. To create multiple DLCI-Util schemas, re-issue the dlci-util schema dlci_schema_name command using a different schema name each time.
> Example
> Include the bulk statistic variable names to create a schema named dlciutilstats_sgsn1 that specifies collection of statistics (a schema format) for:

> • | card

> • | port

> • | path

> • | DS1/E1

> • | DLCI

> • | DLCI utilization snapshot for received packets

> • | DLCI utilization for received packets in the last 5 minutes

> • | DLCI utilization for received packets in the last 15 minutes

> Use the following command:
> gprs schema gprsstats_sgsn1 format “Card: %card%\nPort: %port%\nDLCI in path: %dlci_util_path%\nDS1/E1: %dlci_util_ds1e1%\nDLCI ID: %dlci_util_dlci_no%\nCurrent Rx: %dlci_util_dlci_curr_rx%\nRx in 5 minutes: %dlci_util_dlci_5min_rx%\nRx in 15 minutes: %dlci_util_dlci_15min_rx%\n”
> dpca schema
> Configures Diameter Policy Control Application (DPCA) bulk statistics schema. This command is available only in 9.0 and later releases.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> dpca schema schema_name format format_string
> no dpca schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for DPCA bulk statistics collection.
> ecs schema
> Configures Enhanced Charging Service (ECS) bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> ecs schema schema_name format format_string
> no ecs schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for ECS bulk statistics collection. Multiple ECS schemas can be created to categorize ECS bulk statistics. All of the schemas are processed at each collection interval. To create multiple ECS schemas, re-issue the ecs schema schema_name command using a different schema name.
> egtpc schema
> Configures the enhanced GTP-C statistics schema for naming conventions of data files.
> Product
> P-GW, S-GW
> Privilege
> Administrator
> Syntax
> egtpc schema schema_name format format_string
> no egtpc schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for enhanced GTP-C bulk statistics collection. Multiple eGTP-C service schemas can be created to categorize eGTP-C service bulk statistics. All of the schemas are processed at each collection interval. To create multiple eGTP-C service schemas, re-issue the egtpc schema schema_name command using a different schema name.
> Example
> For an eGTP-C-level schema called egtpcservicestats that specifies a schema format of:

> • | Tunnel - Create Session Request Sent: tun-sent-cresess

> • | Tunnel - Create Session Request Received: tun-recv-cresess

> Use the following command:
> egtpc schema egtpcservicestats format “Number of GTP Tunnel Requests Sent: %tun-sent-cresess%\nNumber of GTP Tunnel Requests Received: %tun-recv-cresess%\n”
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.
> fa schema
> Configures Foreign Agent (FA) bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> fa schema schema_name format format_string
> no fa schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for FA bulk statistics collection. Multiple FA service schemas can be created to categorize FA service bulk statistics. All of the schemas are processed at each collection interval. To create multiple FA service schemas, re-issue the fa schema schema_name command using a different schema name.
> Example
> To create a FA-level schema named faservicestats that separates the date, time, and vpnname by tabs, enter the following command:
> fa schema faservicestats format %date%\t%time%\t%vpnname%
> The schema format appears as follows:
> date time vpnname
> file
> Enters the Bulk Statistics File Configuration mode which supports the configuration of “files” used for grouping bulk statistic configuration information.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] file number
> no
> Removes a previously configured bulk statistic file.
> number
> Specifies a number for the bulkstatistics file as an integer from 1 through 4. This number is how the file is recognized by the system.
> Usage
> Bulk statistics “files” are used to group bulk statistic schema, delivery options, and receiver configuration. Because multiple “files” can be configured, this functionality provides greater flexibility in that it allows you to configure different schemas to go to different receivers. A Maximum of four files can be assigned for bulk statistics collection.
> Executing this command allows you to enter the Bulk Statistics File Configuration Mode. This mode supports all of the commands from the Bulk Statistics Configuration mode except limit, local-directory, sample-interval, and transfer-interval. (these commands are configured globally for all “files”.)
> Important: Use of bulk statistics “files” is optional. If you do not wish to configure bulk statistic “files”, you can perform a standard configuration using the commands in the Bulk Statistic Configuration Mode. Note, however, that the system logically assigns “file 1” to the standard configuration. Therefore, if you wish to configure bulk statistics “files” at a later time, “file 1” will already be used.
> Caution: If the Web Element Manager application is used to collect and process (XML parsing, graphing, etc.) bulk statistics data, “file 1” is used by the Web Element Manager’s default bulk statistics collection information and schemas. To avoid errors in processing by the Web Element Manager, do not configure "file 1" via the CLI. However, it is possible to configure files 1 through 4 using the system’s CLI, regardless of whether or not the Web Element Manager is configured as a receiver. In this case, the bulk statistics data is written to the server but not processed by the Web Element Manager application.
> Example
> The following command creates a bulk statistics file numbered 2 and enters the Bulk Statistics File Configuration Mode:
> file 2
> fng schema
> Configures Femto Network Gateway (FNG) bulk statistics schema.
> Product
> FNG
> Privilege
> Security Administrator, Administrator
> Syntax
> fng schema schema_name format format_string
> no fng schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> footer
> Configures the footer string placed at the end of the generated bulk statistics data files.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> footer format format_string
> no footer format
> no
> Clears the footer format string which results in the default file footer being used in generated data files.
> format format_string
> Specifies the footer format string for use in generated data files as an alphanumeric string from 1 through 2047 characters. The format string syntax is described in the Schema Format String Syntax section. Default: ““ (an empty footer)
> The following variables are supported:
> footer Command Format String Variables

> Variable | Description | Data Type
> date | The date that the collection file was created in YYYYMMDD format where YYYY represents the year, MM represents the month and DD represents the day. | String
> host | The system hostname that created the file | String
> ipaddr | The default management (local context) IP address in ###.###.###.### format. An empty string is inserted if no address is available. | String
> sysuptime | The uptime (in seconds) of the system that created the file. | 32-bit signed
> time | The time that the collection file was created in HHMMSS format where HH represents the hours, MM represents the minutes, and SS represents the seconds. | String

> ‌
> Usage
> Define a unique footer in data files which allows for easy identification of which system generated the data file or any other useful information. The use of the variables is suggested so as to allow for a uniform footer across all systems. The hostname variable should be used to identify the source of the data in the footer and all remaining items can be formatted consistently across all chassis.
> Example
> The following commands define different footer formats:
> footer format northStreet
> footer format “Created on: %date%-%time% by %host%”
> no footer format
> gather-on-standby
> Controls whether or not statistics are gathered when a system is in the standby state.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no | default ] gather-on-standby
> no
> Does not gather bulk statistics when the system is in the standby state.
> default
> Resets this command to its default action of gathering bulk statistics when the system is in the standby state.
> Usage
> Use this command to configure a system to either gather or not gather statistics when the system is in the standby state. This is useful for systems configured for Interchassis Session Recovery (ICSR). See the System Administration Guide for more details on this feature.
> If a chassis transitions to standby state and it has accumulated but not yet transferred bulk statistics data, the previously accumulated data is transferred at the first opportunity. However, no additional statistics gathering takes place.
> Example
> The following command disables gathering statistics when the system is in the standby state:
> no gather-on-standby
> The following command enables the gathering of statistics when the system is in the standby state:
> gather-on-standby
> gprs schema
> Configures the collection of statistics for the GPRS schema.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gprs schema gprs_schema_name format gprs_schema_format
> no gprs schema gprs_schema_name
> no
> Removes the specified schema.
> gprs_schema_name
> Specifies a name for a model collection schema for GPRS statistics. The name must be comprised of an alphanumeric string of 1 to 31 characters.
> format gprs_schema_format
> Specifies the format of the collected GPRS statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters. For syntax details, see the Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for the GPRS schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for GPRS bulk statistics collection in the generated stats report files.. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple GPRS schemas can be created to categorize GPRS bulk statistics. All of the schemas are processed at each collection interval. To create multiple GPRS schemas, re-issue the gprs schema gprs_schema_name command using a different schema name each time.
> Example
> Include the bulk statistic variable names to create a GPRS schema named gprsstats_sgsn1 that specifies collection of statistics (a schema format) for:

> • | context name

> • | GPRS service name

> • | number of LLC packets dropped

> Use the following command:
> gprs schema gprsstats_sgsn1 format “Context Name: %vpnname%\nGPRS Service Name: %servname%\nTotal LLC Packets Dropped: %bssgp-total-usr-req-drop%\n”
> gtpc schema
> Configures GPRS Tunneling Protocol-Control (GTPC) message statistics schema.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gtpc schema gtpc_schema_name format gtpc_schema_format
> no gtpc schema gtpc_schema_name
> no
> Removes the specified schema.
> gtpc_schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format gtpc_schema_format
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for GTPC bulk statistics collection. Multiple GTPC schemas can be created to categorize GTPC bulk statistics. All of the schemas are processed at each collection interval. To create multiple GTPC schemas, re-issue the gtpc schema schema_name command using a different schema name.
> Example
> To create a GTPC-level schema named gtpc_stats that specifies a schema format of:

> • | Context Name: vpnname

> • | GGSN Service Name: servname

> • | Total PDP Contexts Processed: setup-total

> Use the following command:
> gtpc schema gtpc_stats format “Context Name: %vpnname%\nGGSN Service Name: %servname%\nTotal PDP Contexts Processed: %setup-total%\n”
> gtpp schema
> Configures GPRS Tunneling Protocol-Prime (GTPP) statistics schema.
> Product
> GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> gtpp schema gtpp_schema_name format gtpp_schema_format
> no gtpp schema gtpp_schema_name
> no
> Removes the specified schema.
> gtpp_schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format gtpp_schema_format
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for GTPP bulk statistics collection. Multiple GTPP schemas can be created to categorize GTPP bulk statistics. All of the schemas are processed at each collection interval. To create multiple GTPP schemas, re-issue the gtpp schema schema_name command using a different schema name.
> Example
> To create a GTPP schema named gtpp_statistics that specifies a schema format of:

> • | Time: time

> • | Total Redirection Requests Received: redir-rcvd

> Use the following command:
> gtpp schema gtpp_statistics format “Time: %time%\tTotal Redirection Requests Received: %redir-rcvd%\n”
> gtpu schema
> Configures GTP-U bulk statistics schema.
> Product
> GGSN, HNB-GW, P-GW, S-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> gtpu schema schema_name format format_string
> no gtpu schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected GTP-U statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for GTP-U bulk statistics collection in the generated stats report files. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple GTP-U schemas can be created to categorize GTP-U bulk statistics. All of the schemas are processed at each collection interval. To create multiple GTP-U schemas, re-issue the gtpu schema schema_name command using a different schema name each time.
> ha schema
> Configures Home Agent (HA) bulk statistics schema.
> Product
> HA
> Privilege
> Security Administrator, Administrator
> Syntax
> ha schema schema_name format format_string
> no ha schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format. as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for HA bulk statistics collection. Multiple HA service schemas can be created to categorize HA service bulk statistics. All of the schemas are processed at each collection interval. To create multiple HA service schemas, re-issue the ha schema schema_name command using a different schema name.
> Example
> For an HA schema named haservicestats that specifies a schema format of:

> • | Number of HA authentication failures: reply-haauthfail

> • | Number of Mobile Node authentication failures: reply-mnauthfail

> Use the following command:
> ha schema haservicestats format “Number of HA authentication failures: %reply-haauthfail%\nNumber of Mobile Node authentication failures: %reply-mnauthfail%\n”
> header
> Configures the header string placed at the beginning of the generated bulk statistics data files.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> header format format_string
> no header format
> no
> Clears the header format string which results in the default file header being used in generated data files.
> format format_string
> Specifies the header format string for use in generated data files as an alphanumeric string of 1 through 2047 characters. The format string syntax is described in the Schema Format String Syntax section. Default: ““ (an empty header)
> The following variables are supported:
> header Command Format String Variables

> Variable | Description | Data Type
> date | The UTC date that the collection file was created in YYYYMMDD format where YYYY represents the year, MM represents the month and DD represents the day. | String
> date3 | The UTC date that the collection file was created in YYMMDD format where YY represents the year, MM represents the month and DD represents the day. | String
> host | The system hostname that created the file | String
> ipaddr | The default management (local context) IP address in ###.###.###.### format. An empty string is inserted if no address is available. | String
> sysuptime | The uptime (in seconds) of the system that created the file. | 32-bit signed
> time | The time that the collection file was created in HHMMSS format where HH represents the hours, MM represents the minutes, and SS represents the seconds. | String

> ‌
> Usage
> Define a unique header in data files which allows for easy identification as to which system generated the data file or any other useful information.
> Using the variables described above allows for a uniform header across all systems. The hostname variable should be used to identify the source of the data in the header and all remaining items can be formatted consistently across all chassis.
> Example
> The following commands define different header formats:
> header format northStreet
> header format “Created on: %date%-%time% by %host%”
> no header format
> hnbgw-hnbap schema
> Configures bulk statistics schema for HNB-Application Part (HNB-AP) message statistics collection in HNB-GW session instance.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> hnbgw-hnbap schema schema_name format format_string
> no hnbgw-hnbap schema schema_name
> no
> Removes the configured HNB-AP schema.
> schema_name
> Specifies a name for the HNB-AP schema to be used as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies a name for HNB-AP schema format followed by schema variables. format_string must be an alphanumeric string of 1 through 3599 characters. For syntax details, see the Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> This command defines schemas used for HNB-AP statistics collection. Multiple HNB-AP schemas can be created to further categorize bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the hnbgw-hnbap schema schema_name command using a different schema name.
> Example
> The following command creates a schema called hnbap1stats1 that records the number of registered UEs and registered HNBs along with Context name, Context Id, and HNB-GW service name:
> hnbgw-hnbap schema hnbap1stats1 format “%vpnname%-%vpnid%-%servname%-%registered-hnb%-%registered-ue%”
> To create a schema called hnbapuestats that specifies a schema format of:

> • | Number of UEs with CS and PS Core Network Connections: ue-with-ps-cs-conn

> • | Number of UEs in Idle Condition: idle-ue

> Use the following command:
> hnbgw-hnbap schema hnbapuestats format “Number of UEs with CS and PS Core Network Connections: %ue-with-ps-cs-conn%\nNumber of UEs in Idle Condition: %idle-ue%”
> hnbgw-ranap schema
> Configures bulk statistics schema for Radio Access Network-Application Part (RANAP) message statistics collection in HNB-GW session instance.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> hnbgw-ranap schema schema_name format format_string
> no hnbgw-ranap schema schema_name
> no
> Removes the configured RANAP schema.
> schema_name
> Specifies a name for the RANAP schema to be used as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies a name for RANAP schema format, to be used, followed by schema variables. format_string must be an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> This command defines schemas used for RANAP messaging statistics collection. Multiple RANAP schemas can be created to further categorize bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the hnbgw-ranap schem schema_name command using a different schema name.
> Example
> The following command creates a schema called ranap1stats1 that records the number of CS-Direct-Transfer messages sent and received on RANAP along with Context name, Context Id, and HNB-GW service name:
> hnbgw-ranap schema ranap1stats1 format “%vpnname%-%vpnid%-%servname%-%cs-dir-transfer-rx%-%cs-dir-transfer-tx%”
> To create a schema called ranappagingstats that specifies a schema format of:

> • | Number of paging requests sent on RANAP from CS Core Network Connections: cs-paging-req-tx

> • | Number of paging requests sent on RANAP from PS Core Network Connections: ps-paging-req-tx

> Use the following command:
> hnbgw-ranap schema hnbapuestats format “Number of paging requests sent on RANAP from CS Core Network Connections: %cs-paging-req-tx%\nNumber of paging requests sent on RANAP from PS Core Network Connections: %ps-paging-req-tx%”
> hnbgw-rtp schema
> Configures bulk statistics schema for Real-Time Protocol (RTP) message statistics collection in HNB-GW session instance.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> hnbgw-rtp schema schema_name format format_string
> no hnbgw-rtp schema schema_name
> no
> Removes the configured RTP schema.
> schema_name
> Specifies a name for the RTP schema to be used as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies a name for RTP schema format, to be used, followed by schema variables. format_string must be an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> This command defines schemas used for RTP messaging statistics collection. Multiple RTP schemas can be created to further categorize bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the hnbgw-rtp schema schema_name command using a different schema name.
> Example
> The following command creates a schema called rtp1stats1 that records the number of RTP uplink packets dropped and number of RTCP application report messages received on RTP link along with Context name, Context Id, and HNB-GW service name:
> hnbgw-rtp schema rtp1stats1 format “%vpnname%-%vpnid%-%servname%-%rtp-uplink-pkts-dropped%-%rtcp-app-report-rx%”
> hnbgw-rua schema
> Configures bulk statistics schema for RANAP User Adaptation (RUA) protocol message statistics collection in HNB-GW session instance.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> hnbgw-rua schema schema_name format format_string
> no hnbgw-rua schema schema_name
> no
> Removes the configured RUA schema.
> schema_name
> Specifies a name for the RUA schema to be used as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies a name for RUA schema format, to be used, followed by schema variables. format_string must be an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> This command defines schemas used for RUA protocol messaging statistics collection. Multiple RUA schemas can be created to further categorize bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the hnbgw-rua schema schema_name command using a different schema name.
> Example
> The following command creates a schema called rua1stats1 that records the number of CS-Connect messages received and sent on RUA link along with Context name, Context Id, and HNB-GW service name:
> hnbgw-rua schema rua1stats1 format “%vpnname%-%vpnid%-%servname%-%cs-connect-rx%-%cs-connect-tx%”
> hnbgw-sctp schema
> Configures bulk statistics schema for Stream Control Transmission Protocol (SCTP) message statistics collection in HNB-GW session instance.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> hnbgw-sctp schema schema_name format format_string
> no hnbgw-sctp schema schema_name
> no
> Removes the configured SCTP schema.
> schema_name
> Specifies a name for the SCTP schema to be used as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies a name for SCTP schema format, to be used, followed by schema variables. format_string must be an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> This command defines schemas used for SCTP protocol messaging statistics collection. Multiple SCTP schemas can be created to further categorize bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the hnbgw-sctp schema schema_name command using a different schema name.
> Example
> The following command creates a schema called sctp1stats1 that records the number of bytes received from lower layer and number of bytes sent to lower layer over SCTP connection along with Context name, Context Id, and HNB-GW service name:
> hnbgw-sctp schema sctp1stats1 format “%vpnname%-%vpnid%-%servname%-%total-bytes-sent-to-lower-layer%-%total-bytes-rcvd-from-lower-layer%%”
> hsgw schema
> Configures HRPD Serving Gateway (HSGW) bulk statistics schema.
> Product
> HSGW
> Privilege
> Security Administrator, Administrator
> Syntax
> hsgw schema schema_name format format_string
> no hsgw schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected HSGW statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for HSGW bulk statistics collection in the generated stats report files. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple HSGW schemas can be created to categorize HSGW bulk statistics. All of the schemas are processed at each collection interval. To create multiple HSGW schemas, re-issue the hsgw schema schema_name command using a different schema name each time.
> imsa schema
> Configures IP Multimedia System Authorization (IMSA) bulk statistics schema.
> Product
> GGSN, HA, HSGW, IPSG, PDSN, P-GW, S-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> imsa schema schema_name format format_string
> no imsa schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected IMSA statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for IMSA bulk statistics collection in the generated stats report files. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple IMSA schemas can be created to categorize IMSA bulk statistics. All of the schemas are processed at each collection interval. To create multiple IMSA schemas, re-issue the imsa schema schema_name command using a different schema name each time.
> ippool schema
> Configures IP pool bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> ippool schema schema_name format format_string
> no ippool schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for IP pool bulk statistics collection. Multiple IP pool schemas can be created to further categorize IP pool bulk statistics. All of the schemas are processed at each collection interval. To create multiple IP pool schemas, re-issue the ippool schema schema_name command using a different schema name.
> Example
> To create an IP pool schema named ippoolstats that specifies a schema format of:

> • | Number of IP addresses on hold: hold

> • | Number of free IP addresses: free

> Use the following command:
> ippool schema ippoolstats format “Number of IP addresses on hold: %hold%\nNumber of free IP addresses: %free%\n”
> ipsg schema
> Configures IP Services Gateway (IPSG) bulk statistics schema.
> Product
> IPSG
> Privilege
> Security Administrator, Administrator
> Syntax
> ipsg schema schema_name format format_string
> no ipsg schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define the schemas used for IPSG bulk statistics collection. Multiple IPSG schemas can be created to categorize IPSG bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the ipsg schema schema_name command using a different schema name.
> Example
> To create an IPSG schema named ipsgstats that specifies a schema format of:

> • | Context name: vpnname

> • | Service name: servname

> • | Total responses sent: total-rsp-sent

> Use the following command:
> ipsg schema ippoolstats format “Context name: %vpnname%\nService name: %servname%\nTotal responses sent: %total-rsp-sent%\n”
> lac schema
> Configures LAC (L2TP Access Concentrator) bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> lac schema schema_name format format_string
> no lac schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for LAC bulk statistics collection. Multiple LAC schemas can be created to categorize LAC bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the lac schema schema_name command using a different schema name.
> Example
> The following command creates a schema called lac1stats1 that records the number of active subscriber sessions and the number of sessions that failed or were disconnected due to the maximum tunnel limit being reached:
> lac schema lac1stats1 format “%sess-curactive%-%sess-maxtunnel%”
> To create a schema called lacresourcestats that specifies a schema format of:

> • | Number of Successful Session Connections: sess-successful

> • | Number of Session Attempts That Failed: sess-failed

> • | Number of Sessions Currently Active: sess-curative

> Use the following command:
> lac schema lacresourcestats format “Number of Successful Session Connections: %sess-successful%\nNumber of Session Attempts That Failed: %sess-failed%\nNumber of Sessions Currently Active: %sess-curative%”
> limit
> Configures the maximum amount of system memory bulk statistics may utilize.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> limit kilobytes
> kilobytes
> Specifies the maximum amount of memory (in kilobytes) that may be used for bulk statistics as an integer from 1 through 32000. Default: 100
> Usage
> Adjust bulk statics memory usage when considering the sampling interval adjustments.
> Caution: Bulk statistics are stored in Random Access Memory (RAM) on the SMC. In the event of power loss or system failure, the statistics will be lost. If the maximum storage limit has been reached before the system's configured transfer-interval is reached, the oldest information stored in the collection will be overwritten.
> Example
> limit 2048
> lma schema
> Configures the Local Mobility Anchor (LMA) statistics schema for the naming conventions of data files.
> Product
> P-GW
> Privilege
> Administrator
> Syntax
> lma schema schema_name format format_string
> no lma schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name. as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for LMA bulk statistics collection. Multiple LMA service schemas can be created to categorize LMA service bulk statistics. All of the schemas are processed at each collection interval. To create multiple LMA service schemas, re-issue the lma schema schema_name command using a different schema name.
> Example
> For an LMA-level schema called lmaservicestats that specifies a schema format of:

> • | Binding Update Received: bindupd

> • | Binding Update Received - Denied: bindupd-denied

> Use the following command:
> lma schema lmaservicestats format “Number of Binding Updates Received: %bindupd%\nNumber of Binding Updates Received and Denied: %bindupd-denied%\n”
> lns schema
> Configures LNS (L2TP Network Server) bulk statistics schema.
> Product
> LNS
> Privilege
> Security Administrator, Administrator
> Syntax
> lns schema schema_name format format_string
> no lns schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected LNS statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for LNS bulk statistics collection in the generated stats report files. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple LNS schemas can be created to categorize LNS bulk statistics. All of the schemas are processed at each collection interval. To create multiple LNS schemas, re-issue the lns schema schema_name command using a different schema name each time.
> local-directory
> Sets the local directory for storing bulkstats collection files
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> local-directory pathname
> no local-directory
> no
> Delete the setting for local-directory.
> pathname
> Specifies the local path of the directory in which to store bulkstats collection files. This must be an alphanumeric string of 1 through 127 characters. Pathnames are case sensitive.
> Usage
> Use this command to designate a directory on a local file system in which collection files with bulkstats information are stored. The directory specified must already exist. Use the Exec Mode command mkdir to create a directory.
> Example
> To specify that bulkstats collection files are stored in the local directory /flash/bulkstats, enter the following command:
> local-directory /flash/bulkstats
> mag schema
> Configures the Mobile Access Gateway (MAG) statistics schema for naming conventions of data files.
> Product
> HSGW, S-GW
> Privilege
> Administrator
> Syntax
> mag schema schema_name format format_string
> no mag schema schema_name
> no
> Removes the specified schema from MAG bulk statistics generation.
> schema_name
> Specifies the name to use to refer to the schema and associated format string. schema_name must be an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for MAG bulk statistics collection. Multiple MAG service schemas can be created to categorize MAG service bulk statistics. All of the schemas are processed at each collection interval. To create multiple MAG service schemas, re-issue the mag schema schema_name command using a different schema name.
> Example
> For a MAG-level schema called magservicestats that specifies a schema format of:

> • | Binding Update Sent: bindupd

> • | Binding Acknowledgement Received: bindack

> Use the following command:
> mag schema magservicestats format “Number of Binding Updates Sent: %bindupd%\nNumber of Binding Acknowledgements Received: %bindack%\n”
> mipv6ha schema
> Configures MIPv6 HA (home Agent) bulk statistics schema.
> Product
> HA
> Privilege
> Security Administrator, Administrator
> Syntax
> mipv6ha schema schema_name format format_string
> no mipv6ha schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for MIPv6 HA bulk statistics collection. Multiple MIPv6 HA bulk statistics schemas can be created to categorize MIPv6 HA bulk statistics. All of the schemas are processed at each collection interval. To create multiple MIPv6 HA service schemas, re-issue the mipv6ha schema schema_name command using a different schema name.
> Example
> The following command creates a schema called mipv6haservicestats that records the number of authorization attempt failures due to access rejects from AAA:
> mipv6ha schema mipv6haservicestats format “%aaa-actauthfail%”
> mme schema
> Configures MME (Mobility Management Entity) bulk statistics schema.
> Product
> MME
> Privilege
> Security Administrator, Administrator
> Syntax
> mme schema schema_name format format_string
> no mme schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for MME bulk statistics collection. Multiple MME bulk statistics schemas can be created to categorize MME bulk statistics. All of the schemas are processed at each collection interval. To create multiple MME service schemas, re-issue the mme schema schema_name command using a different schema name.
> Example
> The following command creates a schema called mmeservice_s1ap_cfg_transfers that records the total number of S1AP - transmit data - configuration transfers:
> mme schema mmeservice_s1ap_cfg_transfersformat “s1ap-trnsdata-cfg-tfr
> mvs schema
> Configures MVS (Mobile Videoscape) bulk statistics schema.
> Product
> MVG
> Privilege
> Security Administrator, Administrator
> Syntax
> mvs schema schema_name format format_string
> no mvs schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name. as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> nat-realm schema
> Creates and configures Network Address Translation (NAT) realm statistics schema.
> Product
> NAT
> Privilege
> Security Administrator, Administrator
> Syntax
> nat-realm schema schema_name format format_string
> no nat-realm schema schema_name
> schema_name
> Specifies the NAT realm bulk statistics schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for NAT Realm bulk statistics collection. Multiple NAT realm schemas can be created to further categorize NAT realm level bulk statistics. All of the schemas are processed at each collection interval. To create multiple NAT Realm schemas, re-issue the nat-realm schema schema_name command using a different schema name.
> Example
> The following command creates a NAT realm schema with the VPN name, realm name, and flows information:
> nat-realm schema realm1 format “%vpnname% %realmname% %nat-rlm-flows%”
> pcc-af schema
> Configures Policy and Charging Control-Application Function (PCC-AF) service bulk statistics schema.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> pcc-af schema schema_name format format_string
> no pcc-af schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for PCC-AF service bulk statistics collection. Multiple PCC-AF service schemas can be created to categorize PCC-AF service bulk statistics. All of the schemas are processed at each collection interval. To create multiple PCC-AF service schemas, re-issue the pcc-af schema schema_name command using a different schema name.
> Example
> The following command creates a schema called pcc_af1stats1 that records the total number of Rx STR messages received and total number of Rx AAR Accept messages sent along with Context name, Context Id, and PCC-AF service name:
> pcc-af schema pcc_af1stats1 format “%vpnname%-%vpnid%-%servname%-%total-rx-ccai-accept-sent%-%total-rx-aar-accept-sent%”
> pcc-policy schema
> Configures Policy and Charging Control-Policy (PCC-Policy) service bulk statistics schema.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> pcc-policy schema schema_name format format_string
> no pcc-policy schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for PCC-Policy service bulk statistics collection. Multiple PCC-Policy service schemas can be created to categorize PCC-Policy service bulk statistics. All of the schemas are processed at each collection interval. To create multiple PCC-Policy service schemas, re-issue the pcc-policy schema schema_name command using a different schema name.
> Example
> The following command creates a schema called pcc_plcy1stats1 that records the total number of Gx messages sent and total number of Gx CCR messages received along with Context name, Context Id, and PCC-Policy service name:
> pcc-policy schema pcc_plcy1stats1 format “%vpnname%-%vpnid%-%servname%-%total-gx-outbound-msgs%-%total-gx-ccr-rcvd%”
> pcc-sp-endpt schema
> Configures the bulkstats schema at the Sp interface endpoint for PCC procedures with Subscriber Service Controller/Subscriber Policy Register (SSC/SPR).
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> pcc-sp-endpt schema schema_name format format_string
> no pcc-sp-endpt schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for PCC-Sp-Endpoint bulk statistics collection. Multiple PCC-Sp-Endpoint schemas can be created to categorize PCC-Sp-Endpoint bulk statistics. All of the schemas are processed at each collection interval. To create multiple PCC-Sp-Endpoint schemas, re-issue the pcc-sp-endpt schema schema_name command using a different schema name.
> Example
> The following command creates a schema called pcc_sp1stats1 that records the total number of SPRMgr Sh session close and open requests received from PCCMgr and processed by PCC-Sp-Endpoint along with Context name, Context Id, and PCC-Sp-Endpoint name:
> pcc-sp-endpt schema pcc_svc1stats1 format “%vpnname%-%vpnid%-%endpt-name%-%req-open%-%req-close%”
> pcc-service schema
> Configures Policy and Charging Control-Service (PCC-Service) bulk statistics schema.
> Product
> IPCF
> Privilege
> Security Administrator, Administrator
> Syntax
> pcc-service schema schema_name format format_string
> no pcc-service schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for PCC-Service bulk statistics collection. Multiple PCC-Service schemas can be created to categorize PCC-Service bulk statistics. All of the schemas are processed at each collection interval. To create multiple PCC-Service schemas, re-issue the pcc-service schema schema_name command using a different schema name.
> Example
> The following command creates a schema called pcc_svc1stats1 that records the total number of Gx and Gy request processed by PCC-Service along with Context name, Context Id, and PCC-Service name:
> pcc-service schema pcc_svc1stats1 format “%vpnname%-%vpnid%-%servname%-%total-gx-processed%-%total-gy-processed%”
> pdif schema
> Configures Packet Data Interworking Function (PDIF) bulk statistics schema.
> Product
> PDIF
> Privilege
> Security Administrator, Administrator
> Syntax
> pdif schema schema_name format format_string
> no pdif schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3600 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for PDIF bulk statistics collection. Multiple PDIF schemas can be created to categorize PDIF bulk statistics. All of the schemas are processed at each collection interval. To create multiple schemas, re-issue the pdif schema schema_name command using a different schema name.
> Example
> The following command creates a schema called pdifschema1 for the category current active ipv4 sessions:
> pdif schema pdifschema1 format %sess-curactip4%
> pgw schema
> Configures Packet Data Network Gateway (P-GW) bulk statistics schema.
> Product
> P-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> pgw schema schema_name format format_string
> no pgw schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected P-GW statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for P-GW bulk statistics collection in the generated stats report files. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple P-GW schemas can be created to categorize P-GW bulk statistics. All of the schemas are processed at each collection interval. To create multiple P-GW schemas, re-issue the pgw schema schema_name command using a different schema name each time.
> port schema
> Configures port bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> port schema schema_name format format_string
> no port schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format. as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for port bulk statistics collection. Multiple port schemas can be created to categorize port-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple port schemas, re-issue the port schema schema_name command using a different schema name.
> Important: The card variable in the Port schema is not supported on all platforms
> Example
> To create a port-level schema named portstats1 that separates the card/port, bcast_inpackets, and bcast-outpackets variables by hyphens (“-”), enter the following command:
> port schema portstats1 format “%card%/%port% - %bcast_inpackets% - %bcast_outpackets%”
> ppp schema
> Configures Point-to-Point Protocol (PPP) bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> ppp schema schema_name format format_string
> no ppp schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for point-to-point protocol bulk statistics collection. Multiple PPP-service schemas can be created to categorize PPP-service bulk statistics. All of the schemas are processed at each collection interval. To create multiple PPP-service schemas, re-issue the ppp schema schema_name command using a different schema name.
> Example
> To create a ppp-level schema named pppstats that specifies a schema format of:

> • | CHAP: (Challenge Handshake Authentication Protocol)

> • | Auth. Attempts: auth-attempt-chapAuth. Successes: auth-success-chap

> • | PAP: (Password Authentication Protocol)

> • | Auth. Attempts: auth-attempt-papAuth. Successes: auth-success-pap

> Use the following command:
> ppp schema pppstats format “CHAP:\nAuth. Attempts: %auth-attempt-chap%\tAuth. Successes: %auth-success-chap%\nPAP:\nAuth. Attempts: %auth-attempt-pap%\tAuth. Successes: %auth-success-pap%\n”
> ps-network-ranap
> Configures the Radio Access Network Application Part (RANAP) bulk statistics schema in Packet Switched (PS) network associated with an HNB-GW node.
> Product
> HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> ps-network-ranap schema schema_name format format_string
> no ps-network-ranap schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format. as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for RANAP procedure related bulk statistics collection in a PS network associated with HNB-GW in a Femto UMTS network. Multiple PS Networks RANAP schemas can be created to further categorize at PS network or HNB-GW-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple PS Networks RANAP schemas, re-issue the ps-network-ranap schema schema_name command using a different schema name.
> Example
> The following command creates a schema called ps_ranap1stats1 that records the total number of Iu Release Request messages transmitted and total number of Iu Release Command message received by HNB-GW node:
> ps-network-ranap schema ps_ranaplstats1 format “%iu-rel-req-tx%” “%iu-rel-cmd-rx%”
> radius schema
> Configures RADIUS bulk statistics schema.
> Product
> PDSN, GGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> radius schema schema_name format format_string
> no radius schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters that is case sensitive.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for RADIUS bulk statistics collection. Multiple RADIUS schemas can be created to categorize RADIUS bulk statistics. All of the schemas are processed at each collection interval. To create multiple RADIUS schemas, re-issue the radius schema schema_name command using a different schema name.
> Example
> To create a RADIUS schema named radius_statistics that specifies a schema format of:

> • | Server: ipaddr

> • | Authentication Requests Sent: auth-req-sent

> • | Accounting Requests Sent: acc-req-sent

> Use the following command:
> radius schema radius_statistics format “Server: %ipaddr%\nAuthentication Requests Sent: %auth-req-sent%\nAccounting Requests Sent: %acc-req-sent%”
> receiver
> Configures a host system to receive bulkstats information through Trivial File Transfer Protocol (TFTP), File Transfer Protocol (FTP) or SSH File Transfer Protocol (SFTP).
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> receiver { mode { redundant | secondary-on-failure } | ip_address { primary | secondary } [ mechanism { { { ftp | sftp } login user_name [ encrypted ] password pwd } | tftp } } ] }
> no receiver ip_address
> no
> Removes the receiver specified from the list of receivers where data files are sent.
> mode { redundant | secondary-on-failure }
> Determines how bulkstats are delivered to the primary and secondary receivers.
> Default: secondary-on-failure
> redundant: Files are transferred to both the primary and secondary receivers. If either transfer is not currently possible, the file is transferred when possible. The system continues to hold in memory as much data as possible until the data has been successfully transferred to both receivers. Data is only discarded if the in-memory data reaches the configured limit. Refer to the limit command.
> secondary-on-failure: Files are transferred to the secondary receiver if the primary receiver fails. In-memory data is erased once the data is transferred to either the primary or secondary receiver. This is the default behavior.
> ip_address
> Specifies the IP address of the receiver of interest using IPv4 dotted-decimal notation.
> primary | secondary
> Primary and secondary are used to indicate the order in which receivers are connected. The secondary is used when the primary is unreachable.
> primary: indicates the receiver is the primary receiver of data.
> secondary: indicates the receiver is the secondary receiver of data.
> mechanism { { { ftp | sftp } login user_name [ encrypted ] password pwd } | tftp } }
> Specifies the method by which data is transferred to the receiver.
> ftp login user_name [ encrypted ] password pwd: the FTP protocol shall be used for data file transfer. user_name specifies the user to provide for remote system secure logins and must be an alphanumeric string of 1 through 31 characters. The password to use for remote system authentication is specified as pwd and must be from 1 to 31 characters or 1 to 64 characters if the encrypted keyword is also specified.
> sftp login user_name [ encrypted ] password pwd: the SFTP protocol shall be used for data file transfer. user_name specifies the user to provide for remote system secure logins and must be an alphanumeric string of 1 through 31 characters. The password to use for remote system authentication is specified as pwd and must be from 1 to 31 characters or 1 to 64 characters if the encrypted keyword is also specified.
> tftp: the TFTP protocol is to be used to transfer files.
> The encrypted keyword is intended only for use by the system while saving configuration scripts. The system displays the encrypted keyword in the configuration file as a flag that the variable following the password keyword is the encrypted version of the plain text password. Only the encrypted password is saved as part of the configuration file.
> Usage
> Use TFTP methods to reduce transfer times if excessive system resources are being used across the network for transfer of data.
> FTP transfer method allows for login which then provides system logging within the enabled FTP logs.
> The initial connection is attempted to the primary receiver. If the primary receiver is unreachable for any reason, the secondary receiver is used. If the secondary receiver is also unreachable, the system retries after a delay period where it again attempts to connect to the primary receiver followed by the secondary receiver as necessary.
> Important: For redundant receivers, configuration changes to the receivers are applied to all existing and all subsequent data sets pending transfer. If no receiver is configured, bulk statistics will be collected and stored on the system until the maximum amount of memory is used; they will not be transferred to the receiver(s). When the storage limit has been reached the oldest information is overwritten. When a receiver is configured for the primary and secondary target, this command will use both receivers as default if no receiver is specified.
> Example
> receiver 10.2.3.4 primary mechanism tftp
> receiver 10.2.3.5 secondary
> no receiver 10.2.3.4
> remotefile
> Configures the naming convention with support for multiple file format to multiple receivers when storing the data files on the remote receiver(s).
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> remotefile format format_string [ both-receivers | primary-receiver | secondary-receiver ]
> no remotefile format
> no
> Resets the remote file naming convention to the system default.
> format format_string
> Specifies the naming convention format to use as an alphanumeric string of 1 through 127 characters. The format string syntax is described in the Schema Format String Syntax section. Default: “%date%-%time%”
> Important: The remote file naming format should only use static text and bulk statistic variables to avoid any possible file creation issues on the receivers.
> The following variables are supported:
> remote file Command Naming Format Variables

> Variable | Description | Data Type
> date | The UTC date that the collection file was created in YYYYMMDD format where YYYY represents the year, MM represents the month and DD represents the day. | String
> date3 | The UTC date that the collection file was created in YYMMDD format where YY represents the year, MM represents the month and DD represents the day. | String
> host | The system hostname that created the file | String
> sysuptime | The uptime (in seconds) of the system that created the file. | 32-bit signed
> time | The time that the collection file was created in HHMMSS format where HH represents the hours, MM represents the minutes, and SS represents the seconds. | String

> ‌
> both-receivers | primary-receiver | secondary-receiver
> Sets the remote file creation target to both receivers, primary receiver or secondary receiver. Default: Both receivers.
> Usage
> Set the remote file naming format to ensure consistent data file naming across a network or adjusting a single system’s format for easy identification.
> This command specifies whether the format should be used in conjunction with both receivers, only the primary receiver, or only the secondary receiver.
> Important: For redundant receivers, the filenames for the output data files are applied when the information is first gathered. If the name format is modified, the change takes effect for the next data set. The current data set name remains unchanged. even if has not yet been transferred.
> Example
> remotefile format simpleFormat
> remotefile format “%host%-%date%-%time%”
> remotefile format “%host%-%date%-%time%” both-receivers
> remotefile format “%host%-%date%” primary-receiver
> no remotefile format
> rp schema
> Configures R-P bulk statistics schema.
> Product
> PDSN
> Privilege
> Security Administrator, Administrator
> Syntax
> rp schema schema_name format format_string
> no rp schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for R-P bulk statistics collection. Multiple PDSN service schemas can be created to categorize PDSN service bulk statistics. All of the schemas are processed at each collection interval. To create multiple PDSN service schemas, re-issue the rp schema schema_name command using a different schema name.
> Example
> To create an PDSN-level schema called pdsnservicestats that specifies a schema format of:

> • | Date: date

> • | Time: time

> • | Number of Authentication Denials: deny-auth

> Use the following command:
> rp schema rpservicestats format “Date: %date%\nTime: %time%\nNumber of Authentication Denials: %deny-auth%\n”
> sample-interval
> Configures the time interval between collecting local statistics.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> sample-interval minutes
> minutes
> Specifies the frequency (in minutes) of polling for local statistics as an integer from 1 through 1440.
> Usage
> Adjust the sampling interval to tune the system response as shorter periods can cause undue system overhead whereas longer periods have less of a statistical importance when analyzing data.
> The system is shipped from the factory with the sampling interval set to 15 minutes.
> Example
> sample-interval 120
> sccp schema
> Configures the collection of statistics for the SCCP schema.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> sccp schema sccp_schema_name format sccp_schema_format
> no sccp schema sccp_schema_name
> no
> Removes the specified schema.
> sccp_schema_name
> Specifies a name for a model collection schema for SCCP statistics. The name must be comprised of an alphanumeric string of 1 to 31 characters.
> format sccp_schema_format
> Specifies the format of the collected SCCP statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters. For syntax details, see the Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for the SCCP schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for SCCP bulk statistics collection in the generated stats report files.. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple SCCP schemas can be created to categorize SCCP bulk statistics. All of the schemas are processed at each collection interval. To create multiple SCCP schemas, re-issue the sccp schema sccp_schema_name command using a different schema name each time.
> Example
> Include the bulk statistic variable names to create an SCCP schema named sccpstats11 that specifies collection of statistics (a schema format) for:

> • | Subsystem available messages sent from the SCCP

> • | Subsystem available messages received by the SCCP

> Use the following command:
> sccp schema sccpstats11 format “Subsys avail SCCP Tx: %ssa-txed%\nSubsys avail SCCP Rx: %ssa-rcvd%\n”
> schema
> Configures the system-level bulk statistics schema.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> schema schema_name format format_string
> no schema schema_name
> no
> Removes the specified schema.
> schema_name
> Specifies the schema name as an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the schema format as an alphanumeric string of 1 through 3599 characters. For syntax details, see Schema Format String Syntax section.
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for system-level bulk statistics collection. Multiple schemas can be created to categorize system-level bulk statistics. All of the schemas are processed at each collection interval. To create multiple system schemas, re-issue the schema schema_name command using a different schema name.
> Example
> The following command creates a schema called systemstats1 that records the number of current Simple IP and the number of current Mobile IP sessions:
> schema systemstats1 format “%sess-cursipconn% - %sess-curmipconn%”
> To create a system-level schema called bulksysstats that specifies a schema format of:

> • | Number of currently active sessions: sess-curactcall

> • | Number of currently dormant sessions: sess-curdormcall

> Use the following command:
> schema bulksysstats format “Number of currently active sessions: %sess-curactcall%\nNumber of currently dormant sessions: %sess-curdormcall%\n”
> sgs schema
> Configures the collection of statistics for the SGs schema.
> Product
> MME
> Privilege
> Security Administrator, Administrator
> Syntax
> sgs schema schema_name format format_string
> no sgs schema schema_name
> no
> Removes the specified SGs schema from statistics collection.
> schema_name
> Specifies the name to use to refer to the schema and associated format string. schema_name must be an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected SGs statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters. The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for SGs bulk statistics collection in the generated stats report files. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple SGSN schemas can be created to categorize SGSN bulk statistics. All of the schemas are processed at each collection interval. To create multiple SGSN schemas, re-issue the sgs schema sgs_schema_name command using a different schema name each time.
> Example
> Include the bulk statistic variable names to create an SGs schema named stats_SGs_release that specifies a collection of statistics (a schema format) for the total number of release messages transmitted, retransmitted, and received:
> Use the following command:
> sgs schema stats_SGs_release format “Total transmitted: %rel-req-tx%\nTotal retransmitted: %rel-req-retx%\nTotal received: %rel-req-rx%\n”
> sgsn schema
> Configures the collection of statistics for the SGSN schema.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgsn schema schema_name format format_string
> no sgsn schema schema_name
> no
> Removes the specified SGSN schema from statistics collection.
> schema_name
> Specifies the name to use to refer to the schema and associated format string. schema_name must be an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected SGSN statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters. The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for SGSN bulk statistics collection in the generated stats report files. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple SGSN schemas can be created to categorize SGSN bulk statistics. All of the schemas are processed at each collection interval. To create multiple SGSN schemas, re-issue the sgsn schema sgsn_schema_name command using a different schema name each time.
> Example
> Include the bulk statistic variable names to create an SGSN schema named stats_3Gsgsn1 that specifies collection of statistics (a schema format) for the total number of 3G Attaches per LAC/RAC per MCC& MNC:
> Use the following command:
> sgsn schema stats_3Gsgsn1 format “MCC: %mcc%\nMNC: %mnc%\nLAC: %lac%\nRAC: %rac%\nTotal 3G Subs Attached: %3G-attached%\n”
> sgtp schema
> Configures the collection of the SGSN’s GTP-C and GTP-U activity statistics.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> sgtp schema schema_name format format_string
> no sgtp schema schema_name
> no
> Removes the specified SGTP schema from statistics collection.
> schema_name
> Specifies a name for a model collection schema for SGTP statistics. schema_name must be an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected SGTP statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for SGTP bulk statistics collection in the generated stats report files.. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple SGTP schemas can be created to categorize SGTP bulk statistics. All of the schemas are processed at each collection interval. To create multiple SGTP schemas, re-issue the sgtp schema sgtp_schema_name command using a different schema name each time.
> Example
> Include the bulk statistic variable names to create an SGTP schema named sgtpstats_sgsn1 that specifies collection of statistics (a schema format) will be by IuPS service interface and by RNC for the total number of GTP-C Create PDP Context Request messages received.
> Use the following command:
> sgtp schema sgtpstats_sgsn1 format “IuPS Service ID: %iups-service%\nRNC: %rnc-address%\nTotal CPCR Rx: %sgtpc-total-cpc-req%\n”
> sgw schema
> Configures the collection of the S-GW activity statistics.
> Product
> S-GW
> Privilege
> Administrator
> Syntax
> sgw schema schema_name format format_string
> no sgw schema schema_name
> no
> Removes the specified S-GW schema from statistics collection.
> schema_name
> Specifies a name for a model collection schema for S-GW statistics. schema_name must be an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the format of the collected S-GW statistics by identifying the statistics variables and ordering the variables for presentation within the bulk statistics messages. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for S-GW bulk statistics collection in the generated stats report files.. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple S-GW schemas can be created to categorize S-GW bulk statistics. All of the schemas are processed at each collection interval. To create multiple S-GW schemas, re-issue the sgw schema sgw_schema_name command using a different schema name each time.
> Example
> Include the bulk statistic variable names to create an S-GW schema named sgwstats_sgw1 that specifies collection of statistics (a schema format) will be by S-GW service interface for the total number of currently idle and active UEs.
> Use the following command:
> sgw schema sgwstats_sgw1 format “SGW Service ID: %servname%\nTotal Current Idle Ues: %sessstat-totcur-ueidle%\nTotal Current Active Ues: %sessstat-totcur-ueactive%\n”
> show variables
> Displays the bulk statistics variable information based on schema names.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> show variables [ schema_name ] [ obsolete ]
> show variables schema_name
> Displays all valid bulkstat schema statistics, or only the statistics for the specified schema.
> schema_name specifies the name of the schemas available on the system. Following is the list of available schemas in this release.

> • | aal2

> • | alcap

> • | apn

> • | asngw

> • | asnpc

> • | bcmcs

> • | card

> • | closedrp

> • | common

> • | context

> • | cs-network-ranap

> • | cs-network-rtp

> • | cscf

> • | cscfintf

> • | dcca

> • | diameter-acct

> • | diameter-auth

> • | dlci-util

> • | dpca

> • | ecs

> • | egtpc

> • | epdg

> • | fa

> • | fng

> • | gprs

> • | gtpc

> • | gtpp

> • | gtpu

> • | ha

> • | hnbgw-hnbap

> • | hnbgw-ranap

> • | hnbgw-rtp

> • | hnbgw-rua

> • | hnbgw-sctp

> • | hsgw

> • | imsa

> • | ippool

> • | ipsg

> • | lac

> • | lma

> • | lns

> • | mag

> • | map

> • | mipv6ha

> • | mme

> • | mvs

> • | nat-realm

> • | pcc-af

> • | pcc-policy

> • | pcc-service

> • | pcc-sp-endpt

> • | pdg

> • | pdif

> • | pgw

> • | phsgw

> • | phspc

> • | port

> • | ppp

> • | ps-network-ranap

> • | radius

> • | rp

> • | sccp

> • | sgs

> • | sgsn

> • | sgtp

> • | sgw

> • | ss7link

> • | ss7rd

> • | system

> • | vpn

> obsolete
> Displays obsolete (but still available) schema variables. An asterisk (*) is displayed next to schema variables that have been obsoleted.
> Usage
> Use this command to list supported bulk statistic variables. Variables can be listed for a specified schema. If no schema is specified, all supported variables are listed on a per-schema basis.
> Example
> The following command displays the bulkstat variables only for the card schema:
> show variables card
> ss7link schema
> Configures the collection of the SS7 link activity statistics.
> Product
> SGSN
> Privilege
> Security Administrator, Administrator
> Syntax
> ss7link schema schema_name format format_string
> no ss7link schema schema_name
> no
> Removes the specified SS7 Link schema from statistics collection.
> schema_name
> Specifies the name to use to refer to the schema and associated format string. schema_name must be an alphanumeric string of 1 through 31 characters.
> format format_string
> Specifies the naming convention format to use. format_string must be an alphanumeric string of 1 through 3599 characters. The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for SS7 link and linkset bulk statistics collection per SS7 routing domain in a generated stats report file. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple collection schemas can be created to categorize SS7 link bulk statistics. All of the schemas are processed at each collection interval. To create multiple SS7 link schemas, re-issue the ss7link schema ss7link_schema_name command using a different schema name each time.
> Example
> The following command creates a schema called ss7lnk1stats1 that records the changeover orders sent and received per linkset and link and per SS7 routing domain:
> ss7link schema ss7lnk1stats1 format “%ss7rd-number%-%ss7-linkset-id%-%ss7-link-id%-%ss7rd-asp_instance%-%ss7-link-mtp3-changeover-order-tx%-%ss7-link-mtp3-changeover-order-rx%”
> ss7rd schema
> Configures the collection of bulk statistics for SS7 routing domain services, which include the activity statistics for SCTP, MTP, and M3UA data.
> Product
> SGSN, HNB-GW
> Privilege
> Security Administrator, Administrator
> Syntax
> ss7rd schema schema_name format format_string
> no ss7rd schema schema_name
> no
> Removes the specified SS7 routing domain schema from statistics collection.
> schema_name
> Specifies the name to use to refer to the model collection schema and the associated format string.
> schema_name must be an alphanumeric string of 1 to 31 characters.
> format format_string
> Specifies the format of the collected SS7 routing domain statistics by identifying the statistics variables and the ordering of the variables for presentation within the bulk statistics collection report. The format value comprises an alphanumeric string of 1 through 3599 characters.The format string syntax is described by Schema Format String Syntax .
> Important: For a complete list of the statistics that are supported for this schema, refer to the Statistics and Counters Reference.
> Usage
> Use this command to define schemas for collection of SS7 routing domain statistics to be included in the generated stats report file. Usually a schema consists of multiple variables to collect all the statistics for a particular situation. Using double quote marks and text within this command, the reported statistics can be easily identified.
> Multiple collection schemas can be created to categorize SS7 routing domain bulk statistics. All of the schemas are processed at each collection interval. To create multiple SS7 routing domain schemas, re-issue the ss7rd schema ss7rd_schema_name command using a different schema name each time.
> Example
> The following command creates a schema called ss7rd1stats1 that identifies the SS7 routing domain and records the Application Server Process instance in the SS7 routing domain, along with the total number of sent and received SHUTDOWN messages per SS7 routing domain:
> ss7rd schema ss7rd1stats1 format “%ss7rd-number%-%ss7rd-asp_instance%-%ss7rd-sctp-shutdown-tx%-%ss7rd-sctp-shutdown-rx%”
> transfer-interval
> Configures the frequency of transfer of collected statistics to the receiver.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> transfer-interval minutes
> minutes
> Specifies the number of minutes between the transfer of collected statistics to the receivers as an integer from 1 through 999999.
> Usage
> Modify the transfer interval based upon the number of sessions per second. As the number of session requests a second increases it may become necessary to increase the transfer interval to reduce the processing overhead frequency for statistics delivery. This is tempered by the impact reduced resolution of statical data has on usefulness of data when the interval gets larger than the least busy hours and most busy hours of the day.
> The system is shipped from the factory with the transfer interval set to 480 minutes.
> Example
> transfer-interval 1440

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883