> MSEG APN Profile Configuration Mode Commands
> The MSEG APN Profile Configuration Mode allows you to configure Access Point Name(s) (APN) in a Mobile Service Edge Gateway (MSEG) APN profile.
> Important: This configuration mode is not supported in this release. For more information please contact your Cisco account representative.
> apn
> This command allows you to add/remove APN names from an MSEG APN profile.
> Important: This command is not supported in this release. For more information please contact your Cisco account representative.
> Product
> MSEG
> Privilege
> Security Administrator, Administrator
> Syntax
> [ no ] apn apn_name
> no
> If previously configured, deletes the specified APN name in the current MSEG APN profile.
> apn_name
> Specifies the APN to add/remove.
> apn_name must be an alphanumeric string of 1 through 63 characters.
> Usage
> Use this command to add/remove APN names from an MSEG APN profile.
> The APN names configured in the APN profile are wild-cardable strings that are used to match against the APN name in the incoming CPC requests for offload eligibility. APN names are one of the level-one MSEG filters.
> Multiple APN names can be configured in each APN profile to form sets of APN names.
> Example
> The following command adds the APN named test to the current APN profile:
> apn test
> end
> Exits the current configuration mode and returns to the Exec mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> end
> Usage
> Use this command to return to the Exec mode.
> exit
> Exits the current mode and returns to the parent configuration mode.
> Product
> All
> Privilege
> Security Administrator, Administrator
> Syntax
> exit
> Usage
> Use this command to return to the parent configuration mode.

Cisco Systems Inc.
Tel: 408-526-4000
Fax: 408-527-0883