# SNMP MIB Changes in Release 14.0

This chapter identifies objects, traps and conformances added to, modified for, or deprecated from 14.0 SNMP releases.

Topics covered in this chapter are:

- Omissions and Correction
- SNMP MIB Object Changes as of May 31, 2013
- SNMP MIB Alarm Changes as of May 31, 2013
- SNMP MIB Conformance Changes as of May 31, 2013
- SNMP MIB Object Changes as of February 20, 2013
- SNMP MIB Alarm Changes as of February 20, 2013
- SNMP MIB Conformance Changes as of February 20, 2013
- SNMP MIB Object Changes as of November 30, 2012
- SNMP MIB Alarm Changes as of November 30, 2012
- SNMP MIB Conformance Changes as of November 30, 2012
- SNMP MIB Object Changes as of November 7, 2012
- SNMP MIB Alarm Changes as of November 7, 2012
- SNMP MIB Conformance Changes as of November 7, 2012
- SNMP MIB Object Changes as of September 28, 2012
- SNMP MIB Alarm Changes as of September 28, 2012
- SNMP MIB Conformance Changes as of September 28, 2012
- SNMP MIB Object Changes as of August 17, 2012
- SNMP MIB Alarm Changes as of August 17, 2012
- SNMP MIB Conformance Changes as of August 17, 2012
- SNMP MIB Object Changes as of July 31, 2012
- SNMP MIB Alarm Changes as of July 31, 2012
- SNMP MIB Conformance Changes as of July 31, 2012
- SNMP MIB Object Changes as of June 29, 2012
- SNMP MIB Alarm Changes as of June 29, 2012
- SNMP MIB Conformance Changes as of June 29, 2012

Omissions and Corrections

The following lists of items link to changes found in a previous code drop that were omitted from the Release Change Reference or to technical corrections made to previously published content.

Omissions from/corrections to November 7, 2012 Content

- Deprecated SNMP MIB Alarms
- Modified SNMP Conformances

Omissions from/corrections to June 29, 2012 Content

- New SNMP MIB Objects
- New SNMP MIB Alarms

SNMP MIB Object Changes as of May 31, 2013

This section provides information on SNMP MIB object changes in release 14.0.

IMPORTANT:

For more information regarding SNMP MIB objects in this section, refer to the SNMP MIB Reference for this release.

New SNMP MIB Objects

This section identifies new SNMP MIB objects available in release 14.0.
The following objects are new in this release:

- starIfIndex
- starApsOperation
- starLIRcvryErrType
- starLIRcvryErrString
- starSS7CongLevel
- starSS7LocalCong
- starSS7CauseString

Modified SNMP MIB Objects

This section identifies SNMP MIB objects modified in release 14.0.
The following objects have been modified in this release:

- starFanNum
- starFanLocation
- starPortEntry
- starSS7rdid

Deprecated SNMP MIB Objects

This section identifies SNMP MIB objects that are no longer supported in release 14.0.

None for this release.

SNMP MIB Alarm Changes as of May 31, 2013

This section provides information on SNMP MIB alarm changes in release 14.0.

New SNMP MIB Alarms

This section identifies new SNMP MIB alarms available in release 14.0.

- starCdrHDDStart
- starCdrStreamingStart
- starCdrStreamingComplete
- starNPDBConnectionDown
- starNPDBConnectionUp
- starSessMgrCSCFServiceRecoveryComplete
- starLIRcvryError
- starLIRcvryComplete

Modified SNMP MIB Alarms

This section identifies SNMP MIB alarms modified in release 14.0.

- starFanFailed
- starThreshPortHighActivity
- starThreshClearPortHighActivity
- starApsCommandSuccess
- starApsCommandFailure
- starApsSwitchSuccess
- starApsSwitchFailure
- starApsModelMismatch
- starApsFeProtLineFailure
- starApsLossOfRedundancy
- starApsLossOfRedundancyClear
- starSGSNRMMemWarn

Deprecated SNMP MIB Alarms

This section identifies SNMP MIB alarms not supported in release 14.0.

The following alarms are no longer supported. In some instances, their trap numbers (in parentheses) have been reused for other traps.

- starSessMgrFlowCount
- starSessMgrFlowCountClear
- starECSreaddressServerDown(1231)
- starECSreaddressServerUp (1232)

SNMP MIB Conformance Changes as of May 31, 2013

This section provides information on SNMP MIB conformance changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB conformances in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

None for this release.

Modified SNMP Conformances

This section identifies modified SNMP MIB units of conformance available in release 14.0.

None for this release.

SNMP MIB Object Changes as of February 20, 2013

This section provides information on SNMP MIB object changes in release 14.0.

IMPORTANT:

For more information regarding SNMP MIB objects in this section, refer to the SNMP MIB Reference for this release.

New SNMP MIB Objects

This section identifies new SNMP MIB objects available in release 14.0.
The following objects are new in this release:

- starHENBGWMMESCTPAssocDown
- starHENBGWMMESCTPAssocDown
- starHENBGWMMESCTPAllAssocDown
- starHENBGWMMESCTPAllAssocDown
- starNPUMissedARPFrames

Modified SNMP MIB Objects

This section identifies SNMP MIB objects modified in release 14.0.
The following objects have been modified in this release:

- starRedundantPortNum

Deprecated SNMP MIB Objects

This section identifies SNMP MIB objects that are no longer supported in release 14.0.
The following objects have been deprecated in this release:

- starGPRSSportt
- tarGPRSPport
- starGPRSPport
- starGPRSSelfIpAddr
- starGPRSPeerIpAddr

SNMP MIB Alarm Changes as of February 20, 2013

This section provides information on SNMP MIB alarm changes in release 14.0.

None for this release.

SNMP MIB Conformance Changes as of February 20, 2013

This section provides information on SNMP MIB conformance changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB conformances in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

None for this release.

Modified SNMP Conformances

This section identifies modified SNMP MIB units of conformance available in release 14.0.

None for this release.

SNMP MIB Object Changes as of November 30, 2012

This section provides information on SNMP MIB object changes in release 14.0.

New SNMP MIB Objects

This section identifies new SNMP MIB objects in release 14.0.

None for this release.

Modified SNMP MIB Objects

This section identifies modified SNMP MIB objects in release 14.0.

After a review of the Cisco ASR 5x00 SNMP MIB Reference, it was discovered that the external management applications had been documented with Object ID strings that were inconsistent with the MIB files present in the software. This affected all releases through November 7, 2012.

In order to correct this, a new hierarchy diagram has been created for each application, and the OID strings have been corrected for the November 30, 2012 release.

IMPORTANT:

This correction is NOT required for the starOS MIB objects; however, a new hierarchy diagram has been added for clarity.

IMPORTANT:

The OID strings continue to be prefaced with “enterprise” to represent 1.3.6.1.4.1

Application | Previously Documented OID String | Corrected OID String
--- | --- | ---
Content Filtering supports multiple MIBs:
starCFCommonMIB | enterprise.8164.1.100.1.1.x | enterprise.8164.100.1.1.x
starCFCDPMIB | enterprise.8164.1.100.2.1.x | enterprise.8164.100.2.1.x
starCFREMIB | enterprise.8164.1.100.3.1.x | enterprise.8164.100.3.1.x
starCFCCIMIB | enterprise.8164.1.100.4.1.x | enterprise.8164.100.4.1.x
starCFEMSMIB | . | *enterprise.8164.100.5.1.x
*enterprise.8164.100.5.1.x has been added as a placeholder for possible future development
starCFMCRDBSMIB | enterprise.8164.1.100.6.1.x | enterprise.8164.100.6.1.x
IPMS | enterprise.8164.1.102.1.x | enterprise.8164.102.1.x
L-ESS | enterprise.8164.1.101.1.x | enterprise.8164.101.1.x
MUR | enterprise.8164.1.103.1.x | enterprise.8164.103.1.x
PPT (Cisco MIB) | enterprise.9.1.787.1.x | enterprise.9.9.787.0.x
SSC | enterprise.8164.1.201.1.x | enterprise.8164.201.1.x
WEM | enterprise.8164.1.1000.1.x | **enterprise.8164.1.1000.1.2.x
**Note that WEM retains the “1” after 8164 and adds “2” to the string

Deprecated SNMP MIB Objects

This section identifies SNMP MIB objects unsupported in release 14.0.

None for this release.

SNMP MIB Alarm Changes as of November 30, 2012

This section provides information on SNMP MIB alarm changes in release 14.0.

New SNMP MIB Alarms

This section identifies new SNMP MIB alarms available in release 14.0.

After a review of the Cisco ASR 5x00 SNMP MIB Reference, it was discovered that the following traps were present in the MIB files found in the software, but were previously undocumented.

IMPORTANT:

These traps have also been added to Appendix A: Default Trap Severities.

- starGenericLESSHostEnabled
- starGenericLESSHostDisabled
- starGenericLESSProcessFailure
- starGenericLESSProcessStarted

Modified SNMP MIB Alarms

This section identifies SNMP MIB alarms modified in release 14.0.

After a review of the Cisco ASR 5x00 SNMP MIB Reference, it was discovered that the external management applications had been documented with Object ID strings that were inconsistent with the MIB files present in the software. This affected all releases through November 7, 2012.

In order to correct this, a new hierarchy diagram has been created for each product, and the OID strings have been corrected in the documentation dated November 30, 2012.

IMPORTANT:

The OIDs have also been corrected in Appendix A: Default Trap Severities.

IMPORTANT:

This correction is NOT required for the starOS MIB traps; however, a new hierarchy diagram has been added for clarity.

IMPORTANT:

The OID strings continue to be prefaced with “enterprise” to represent 1.3.6.1.4.1

Application | Previously Documented OID String | Corrected OID String
--- | --- | ---
Content Filtering supports multiple MIBS:
starCFCommonMIB | enterprise.8164.1.100.1.2.x | enterprise.8164.100.1.2.x
starCFCDPMIB | enterprise.8164.1.100.2.2.x | enterprise.8164.100.2.2.x
starCFREMIB | enterprise.8164.1.100.3.2.x | enterprise.8164.100.3.2.x
starCFCCIMIB | enterprise.8164.1.100.4.2.x | enterprise.8164.100.4.2.x
starCFEMSMIB | . | enterprise.8164.100.5.2.x
enterprise.8164.100.5.2.x has been added as a placeholder for possible future development
starCFMCRDBSMIB | enterprise.8164.1.100.6.2.x | enterprise.8164.100.6.2.x
IPMS | enterprise.8164.1.102.2.x | enterprise.8164.102.2.x
L-ESS | enterprise.8164.1.101.2.x | enterprise.8164.101.2.x
MUR | enterprise.8164.1.103.2.x | enterprise.8164.103.2.x
PPT (Cisco MIB) | enterprise.9.1.787.2.x | enterprise.9.9.787.1.x
SSC | enterprise.8164.1.201.2.x | enterprise.8164.201.2.x
WEM | enterprise.8164.1.1000.2.x | enterprise.8164.1000.2.x

Deprecated SNMP MIB Alarms

This section identifies SNMP MIB alarms not supported in release 14.0.

Corrected content: In the previous release, three SSC alarms (below) were documented as being no longer supported. This statement was incorrect, and they have been restored to the documentation.

Please continue reading for a list of obsolete alarms for the current release.

- starSSCDBConnectionFailed
- starSSCDBConnectionRestored
- starSSCDBConnRetryExhausted

The following alarms are no longer supported. In some instances, their trap numbers (in parentheses) have been reused for other traps.

- starSSCMaxPendReqAppMgrSysCleared
- starSSCMaxPendReqAppMgrSysCrossed
- starSSCMaxPendReqAppMgrCrossed
- starSSCMaxPendReqAppMgrCleared
- starSSCSprDown
- starSSCSprUp
- starSSCSprCacheDown
- starSSCSprCacheUp
- starSSCPeerStateUp(6)
- starSSCPeerStateDown(7)
- starSSCEmailServerUnreachable(10)
- starSSCEmailServerReachable(11)
- starSSCSmsServerUnreachable(12)
- starSessMgrFlowCount
- starSessMgrFlowCountClear
- starECSreaddressServerDown(1231)
- starECSreaddressServerUp (1232)

SNMP MIB Conformance Changes as of November 30, 2012

This section provides information on SNMP MIB conformance changes in release 14.0.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

None for this release.

Modified SNMP Conformances

This section identifies modified SNMP MIB units of conformance available in release 14.0.

Corrected content: in the previous release of this document, it was stated that the following three SSC entries were removed from the starSSCNotifGroup. This statement was subsequently found to be incorrect.

- starSSCDBConnectionFailed
- starSSCDBConnectionRestored
- starSSCDBConnRetryExhausted

After a review of the Cisco ASR 5x00 SNMP MIB Reference, it was discovered that some of the external management applications had been documented with Object ID strings that were inconsistent with the MIB files present in the software. This affected all releases through November 7, 2012.

In order to correct this, a new hierarchy diagram has been created for each product, and the OID strings have been corrected in the documentation dated November 30, 2012.

IMPORTANT:

This correction is NOT required for the starOS MIB conformances; however, a new hierarchy diagram has been added for clarity.

IMPORTANT:

The OID strings continue to be prefaced with “enterprise” to represent 1.3.6.1.4.1

The most common finding was that MIBGroups and MIBCompliances OID strings were reversed. Although not all applications were affected, the following is the correct OID string for all applications, corrected as per the MIB file, as reflected in the most current user documentation:

Application | OID String
--- | ---
starCFCommonMIB | Possible future development
starCFCDPMIB | Possible future development
starCFREMIB | enterprise.8164.100.3.3.starCFREMIBGroups(1).x enterprise.8164.100.3.3.starCFREMIBCompliances(2).x
starCFCCIMIB | enterprise.8164.100.4.3.starCFCCIMIBGroups(1).x enterprise.8164.100.4.3.starCFCCIMIBCompliances(2).x
starCFEMSMIB | Possible future development
starCFMCRDBSMIB | enterprise.8164.100.6.3.starCFMCRDBSMIBGroups(1).x enterprise.8164.100.6.3.starCFMCRDBSMIBCompliances(2).x
starEMSMIB (WEM) | enterprise.8164.1.1000.3.starEmsMIBCompliances(1).x enterprise.8164.1.1000.3.starEmsMIBGroups(2).x
starIPMSMIB | enterprise.8164.102.3.starIPMSMIBCompliances(1).x enterprise.8164.102.3.starIPMSMIBGroups(2).x
starLESSMIB | enterprise.8164.101.3.starLESSMIBGroups(1).x enterprise.8164.101.3.starLESSMIBCompliances(2).x
starMURMIB | enterprise.8164.103.3.starMURMIBGroups(1).x enterprise.8164.103.3.starMURMIBCompliances(2).x
cPPTMIB | enterprise.9.9.787.2.cPPTMIBGroups(1).x enterprise.9.9.787.2.cPPTMIBCompliances(2).x
starSSCMIB | enterprise.8164.201.3.starSSCMIBGroups(1).x enterprise.8164.201.3.starSSCMIBCompliances(2).x
For the WEM application, see starEMSMIB | .

SNMP MIB Object Changes as of November 7, 2012

This section provides information on SNMP MIB Object changes in release 14.0.

None for this release.

SNMP MIB Alarm Changes as of November 7, 2012

This section provides information on SNMP MIB alarm changes in release 14.0.

New SNMP MIB Alarms

This section identifies new SNMP MIB alarms available in release 14.0.

- starStorageFound
- starStorageNotFound

Modified SNMP MIB Alarms

This section identifies modified SNMP MIB alarms available in release 14.0.

None for this release.

Deprecated SNMP MIB Alarms

This section identifies SNMP MIB alarms not supported in release 14.0.

Corrected content: In the previous release, three SSC alarms (below) were documented as being no longer supported. This statement was incorrect, and they have been restored to the documentation.

The following SSC alarms are no longer supported for 14.0.309:

- starSSCDBConnectionFailed
- starSSCDBConnectionRestored
- starSSCDBConnRetryExhausted

SNMP MIB Conformance Changes as of November 7, 2012

This section provides information on SNMP MIB conformance changes in release 14.0.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

- starStorageFound
- starStorageNotFound
- starSessMgrFlowCount
- starSessMgrFlowCountClear

Modified SNMP Conformances

This section identifies modified SNMP MIB units of conformance available in release 14.0.

The following SSC objects were removed from the starSSCNotifGroup:

- starSSCDBConnectionFailed
- starSSCDBConnectionRestored
- starSSCDBConnRetryExhausted

SNMP MIB Object Changes as of September 28, 2012

This section provides information on SNMP MIB object changes in release 14.0.

New SNMP MIB Objects

This section identifies SNMP MIB objects new in release 14.0.

- starSessMgrFlowInstId
- starSessMgrFlowPDNNo
- starSessMgrFlowMemUsage
- starSessMgrFlowCounter
- starSessMgrTotalFlowCount

Modified SNMP MIB Objects

This section identifies SNMP MIB objects modified in release 14.0.

Previous Behavior:

- The object starCardMode Syntax list ended with activevpc(8).
- The object starPortType Syntax list ended with virtualethernet(10).

Modified Behavior:

- The object starCardMode was modified with the addition of activedpc(9) to the Syntax list.
- The object starPortType was modified with the addition of ether10g(11) to the Syntax list.

Deprecated SNMP MIB Objects

This section identifies deprecated SNMP MIB alarms that are no longer supported in release 14.0.

None for this release.

SNMP MIB Alarm Changes as of September 28, 2012

This section provides information on SNMP MIB alarm changes in release 14.0.

New SNMP MIB Alarms

This section identifies new SNMP MIB alarms available in release 14.0.

- starPCCNtfyIntfPeerUnreachable
- starPCCNtfyIntfPeerReachable
- starIPSecNodePeerDown
- starIPSecNodePeerUp
- starCdrPurged
- starSessMgrFlowCount
- starSessMgrFlowCountClear

The following SSC MIBs were unsupported for the SSC build 14.0.274; but, they are restored for the build 14.0.290:

- starSSCStopObserverFailed
- starSSCStartObserverFailed
- starSSCScpFSFOFailed
- starSSCCacheCleanupFailed
- starSSCDetDBRoleFailed
- starSSCDataGuardBrokerDown
- starSSCStartListnerFailed
- starSSCMonitoringT10Failed

Modified SNMP MIB Alarms

This section identifies SNMP MIB alarms modified in release 14.0.

Previous Behavior:

Trap 1213, starSAEGWSessThreshold, carried the following description: If the thresholding subsystem is configured to run in an 'alarm' model,a starSAEGWSessThresholdClear notification will be generated when the measured value falls below the threshold.

Modified Behavior:

The trap has been renamed to starThreshSAEGWSessions. This change is also reflected in the Conformances. The description has changed to: “If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearSAEGWSessions notification will be generated when the measured value falls below the threshold.”

Previous Behavior:

Trap 1214 was originally named starSAEGWSessThresholdClear.

Modified Behavior:

This trap has been renamed to starThreshClearSAEGWSessions. This change is also reflected in the Conformances.

Deprecated SNMP MIB Alarms

This section identifies SNMP MIB alarms that are no longer supported in release 14.0.

None for this release.

SNMP MIB Conformance Changes as of September 28, 2012

This section identifies MIB Conformance changes in release 14.0.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

None for this release

Modified SNMP Conformances

This section identifies modified SNMP MIB units of conformance available in release 14.0.

The following objects were added to the starSSCNotifGroup:

- starSSCStopObserverFailed
- starSSCUrl
- starSSCStartObserverFailed
- starSSCScpFSFOFailed
- starSSCCacheCleanupFailed
- starSSCDetDBRoleFailed
- starSSCDataGuardBrokerDown
- starSSCStartListnerFailed
- starSSCMonitoringT10Failed

SNMP MIB Object Changes as of August 17, 2012

This section provides information on SNMP MIB object changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB objects in this section, refer to the Cisco ASR 5x00 SNMP MIB Referencefor this release.

New SNMP MIB Objects

This section identifies new SNMP MIB objects available in release 14.0.

- starCLIRemoteIpAddrType

Modified SNMP MIB Objects

This section identifies modified SNMP MIB objects available in release 14.0.

- Object starCLIRemoteIpAddr. Syntax changed from IpAddress to InetAddress. OID string incremented by 1 to 7.
- Object starCLIContext. OID incremented by 1 to 8
- Object starCLIDatabaseUsername. OID incremented by 1 to 9

Deprecated SNMP MIB Objects

This section identifies SNMP MIB objects that are no longer supported in release 14.0.

None in this release.

SNMP MIB Alarm Changes as of August 17, 2012

This section provides information on SNMP MIB alarm changes in release 14.0.

IMPORTANT:

For more information regarding SNMP MIB alarms in this section, refer to the Cisco ASR 5x00 SNMP MIB Referencefor this release.

New SNMP MIB Alarms

This section identifies new SNMP MIB alarms available in release 14.0.

Support has been provided for the following new alarms:

- starHenbgwAccessServiceStart
- starHenbgwAccessServiceStop
- starHenbgwNetworkServiceStart
- starHenbgwNetworkServiceStop
- starECSTotalDNSLearntIPv4Threshold
- starECSTotalDNSLearntIPv4ThresholdClear
- starECSTotalDNSLearntIPv6Threshold
- starECSTotalDNSLearntIPv6ThresholdClear
- starIPSecNodeIpv6PeerDown
- starIPSecNodeIpv6PeerUp
- starLAGGroupDown
- starLAGGroupUp
- starSGSNRMCPUWarn
- starSGSNRMCPUWarnClear
- starSGSNRMCPUOver
- starSGSNRMCPUOverClear
- starSGSNRMMemOver
- starSGSNRMCPUOverClear
- starSGSNRMMemOver
- starSGSNRMMemOverClear
- starSSCGeoFailoverFailed
- starSSCRoleChangeFailed
- starSSCDBConnectionFailed
- starSSCDBConnectionRestored
- starSSCDBConnRetryExhausted

Modified SNMP Alarms

This section identifies SNMP MIB alarms modified in release 14.0.

Support has been added to enable/disable the following MIBs:

- CISCO-PROCESS-MIB
- CISCO-ENTITY-FRU-CONTROL-MIB
- CISCO-ENTITY-DISPLAY-MIB
- CISCO-ENTITY-DISPLAY-MIB
- HOST-RESOURCES-MIB

One of the objects for the alarm starSessionRejectNoResource has been changed. from starServiceVpnID to starServiceVpnName. starServiceVpnID is the index for the table.

The objects starCPUSlot and starCPUNumber have been added to the list of objects for the following alarms:

- starThreshCPUOrbsWarn
- starThreshClearCPUOrbsWarn
- starThreshCPUOrbsCritical
- starThreshClearCPUOrbsCritical

Object starCLIRemoteIpAddrType has been removed from the following alarms:

- starLoginFailure
- starLocalUserAdded
- starLocalUserRemoved
- starLocalUserPrivilegeChanged
- starOsShellAccessed
- starTestModeEntered
- starLicenseFeaturesModified
- starHiddenAccessEnabled
- starHiddenAccessDisabled

Deprecated SNMP Alarms

This section identifies SNMP MIB alarms that are no longer supported in release14.0.

The following SSC alarms are not supported in this release:

- starSSCStopObserverFailed
- starSSCStartObserverFailed
- starSSCScpFSFOFailed
- starSSCCacheCleanupFailed
- starSSCDetDBRoleFailed
- starSSCDataGuardBrokerDown
- starSSCStartListnerFailed
- starSSCMonitoringT10Failed

Modified SNMP Alarms

This section identifies SNMP MIB alarms modified in release 14.0.

Support has been added to enable/disable the following MIBs:

- CISCO-PROCESS-MIB
- CISCO-ENTITY-FRU-CONTROL-MIB
- CISCO-ENTITY-DISPLAY-MIB
- CISCO-ENTITY-DISPLAY-MIB
- HOST-RESOURCES-MIB

One of the objects for the alarm starSessionRejectNoResource has been changed. from starServiceVpnID to starServiceVpnName. starServiceVpnID is the index for the table.

The objects starCPUSlot and starCPUNumber have been added to the list of objects for the following alarms:

- starThreshCPUOrbsWarn
- starThreshClearCPUOrbsWarn
- starThreshCPUOrbsCritical
- starThreshClearCPUOrbsCritical

Object starCLIRemoteIpAddrType has been removed from the following alarms:

- starLoginFailure
- starLocalUserAdded
- starLocalUserRemoved
- starLocalUserPrivilegeChanged
- starOsShellAccessed
- starTestModeEntered
- starLicenseFeaturesModified
- starHiddenAccessEnabled
- starHiddenAccessDisabled

SNMP MIB Conformance Changes as of August 17, 2012

This section provides information on SNMP MIB conformance changes in release 14.0.

IMPORTANT:

For more information regarding SNMP MIB conformances in this section, refer to the Cisco ASR 5x00 SNMP MIB Referencefor this release.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

Object starCLIRemoteIpAddrType has been added to the starChassisGroup Object Group.

Deprecated SNMP MIB Conformances

This section identifies modified SNMP MIB units of conformance not supported in release 14.0.

The following SSC units of conformance are no longer supported in the starSSCNotifGroup Notifications Group:

- starSSCStopObserverFailed
- starSSCStartObserverFailed
- starSSCScpFSFOFailed
- starSSCCacheCleanupFailed
- starSSCDetDBRoleFailed
- starSSCDataGuardBrokerDown
- starSSCStartListnerFailed
- starSSCMonitoringT10Failed

SNMP MIB Object Changes as of July 31, 2012

This section provides information on SNMP MIB object changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB objects in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Objects

This section identifies new SNMP MIB objects available in release 14.0.

None for this release.

Modified SNMP MIB Objects

This section identifies modified SNMP MIB objects available in release 14.0.

- The starCLIEntry object had starCLIRemoteIPAddrType, InetAddressType, and InetAddressType removed from the object sequence while IpAddressed was added.
- Object starCLIRemoteIpAddr had the OID string incremented by 1 to become 7
- Object starCLIContext had the OID string incremented by 1 to become 8
- Object starCLIDatabaseUsername had the OID string incremented by 1 to become 9

Deprecated SNMP MIB Objects

This section identifies SNMP MIB objects that are no longer supported in release14.0.

- starCLIRemoteIpAddrType

SNMP MIB Alarm Changes as of July 31, 2012

This section provides information on SNMP MIB alarm changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB alarms in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Alarms

This section identifies new SNMP MIB alarms available in release 14.0.

- starSAEGWSessThreshold
- starSAEGWSessThresholdClear

Modified SNMP Alarms

This section identifies modified SNMP MIB alarms available in release 14.0.

The description for starAAAArchiveStarted has changed. It now reads: “A AAAArchiveStarted trap will be generated if queue size crosses 15% of maximum number of sessmgr items per instance.”

The following alarms had starCLIRemoteIpAddrType removed from their list of objects:

- starLoginFailure
- starLocalUserAdded
- starLocalUserRemoved
- starLocalUserPrivilegeChanged
- starOsShellAccessed
- starTestModeEntered
- starLicenseFeaturesModified
- starHiddenAccessEnabled
- starHiddenAccessDisabled

Deprecated SNMP Alarms

This section identifies SNMP MIB alarms that are no longer supported in release14.0.

None for this release.

SNMP MIB Conformance Changes as of July 31, 2012

This section provides information on SNMP MIB conformance changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB conformances in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

None for this release.

Modified SNMP Conformances

This section identifies modified SNMP MIB units of conformance available in release 14.0.

- For starChassisGroup: starCLIRemoteIpAddrType was removed.
- For starTrapGroup: starSAEGWSessThreshold and starSAEGWSessThresholdClear were added

SNMP MIB Object Changes as of June 29, 2012

This section provides information on SNMP MIB object changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB objects in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Objects

This section identifies new SNMP MIB objects available in release 14.0.

Omitted Content:The following new Objects were previously documented as new Alarms

- starSGSServiceVpnName
- starSGSServiceServName
- starVLRName
- starVLRIpAddr1
- starVLRIpAddr2
- starVLRPortNum
- starCongestionType
- starCongestionActionProfileName
- starMURSFTPMessage

The following objects are new for this release:

- starChassisPeakCPUUsage
- starCLIRemoteIpAddrType
- IPCF Policy Provisioning Tool (PPT) has changed from the starPPTMIB to the Cisco cPPTMIB structure, thereby creating a new MIB format for this release. The new objects are fully documented in the Cisco SNMP MIB Reference. Refer to the IPCF PPT Application MIB chapter.

Modified SNMP MIB Objects

This section identifies modified SNMP MIB objects available in release 14.0.
The following objects are modified in this release:

- starCPUMemTotal
- starCPUMemUsed
- starCPUMemCached
- StarCLIEntry
- starCLIRemoteIpAddr
- starCLIContext
- starCLIDatabaseUsername

Deprecated SNMP MIB Objects

This section identifies SNMP MIB objects that are no longer supported in release14.0.

None for this release.

SNMP MIB Alarm Changes as of June 29, 2012

This section provides information on SNMP MIB alarm changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB alarms in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Alarms

This section identifies new SNMP MIB alarms available in release 14.0.

Corrected Content: The following entries were incorrectly listed as Alarms, when they should have been listed as new Objects

- starSGSServiceVpnName
- starSGSServiceServName
- starVLRName
- starVLRIpAddr1
- starVLRIpAddr2
- starVLRPortNum
- starCongestionType
- starCongestionActionProfileName
- starMURSFTPMessage

The following alarms are new in this release:

- starVLRAssocDown
- starVLRAssocUp
- starVLRAllAssocDown
- starVLRAllAssocDownClear
- starEnhancedCongestion
- starMURSFTPFailure
- starMURSFTPNormal
- Cisco-Entity-Display-MIB
- Cisco-Entity-Sensor-MIB
- Cisco-Host-Resource-MIB
- Cisco-Process-MIB
- IPCF Policy Provisioning Tool (PPT) has changed from the starPPTMIB to the Cisco cPPTMIB structure, thereby creating a new MIB format for this release.. The new notifications (alarms) are fully documented in the Cisco SNMP MIB Reference. Refer to the IPCF PPT Application MIB chapter and also the Default Trap Severities appendix.

Modified SNMP Alarms

This section identifies modified SNMP MIB alarms available in release 14.0.
The following alarms are modified in this release:

- starAAAArchiveStarted
- starMURDataIdentifier: added rdp(5) to syntax list
- starMURTaskIdentifier: added httphostaggregationminutely(9), httphostaggregationhourly(10) and httpcontentsummary(11) to syntax list
- starMURUnProcessedFilesNormal: severity is now informational.
- starMURKPIThreshCritical: stare is now operational.
- starMURKPIThreshCriticalClear: state is now operational; severity is now informational.
- starMURKPIThreshMajorClear: severity is now informational.
- starMURKPIThreshMinorClear: severity is now informational.
- starMURKPIThreshWarning: severity is now warning.
- starCfCdpProcApiOpFailed is now starCfCdpApiOpFailed
- IF-MIB is disabled by default for this release.
- ENTITY-MIB is disabled by default for this release.
- starLoginFailure
- starEgtpcPathFailureClear
- starLocalUserAdded
- starLocalUserRemoved
- starLocalUserPrivilegeChanged
- starOsShellAccessed
- starTestModeEntered
- starLicenseFeaturesModified
- starHiddenAccessEnabled
- starHiddenAccessDisabled

Deprecated SNMP Alarms

This section identifies SNMP MIB alarms that are no longer supported in release14.0.

- starECSTotalDNSLearntIPv4Threshold
- starECSTotalDNSLearntIPv4ThresholdClear
- starECSTotalDNSLearntIPv6Threshold
- starECSTotalDNSLearntIPv6ThresholdClear
- starIPSecNodeIpv6PeerDown
- starIPSecNodeIpv6PeerUp
- starLAGGroupDown
- starLAGGroupUp

SNMP MIB Conformance Changes as of June 29, 2012

This section provides information on SNMP MIB conformance changes in release14.0.

IMPORTANT:

For more information regarding SNMP MIB conformances in this section, refer to the SNMP MIB Referencefor this release.

New SNMP MIB Conformances

This section identifies new SNMP MIB units of conformance available in release 14.0.

starCLIRemoteIpAddrType

IPCF Policy Provisioning Tool (PPT) has changed to the CiscoMIB structure, thereby creating a new MIB format for this release. The new conformances are fully documented in the Cisco SNMP MIB Reference. Refer to the IPCF PPT Application MIB chapter.

Modified SNMP Conformances

This section identifies modified SNMP MIB units of conformance available in release 14.0.
The following conformances are modified in this release:

- starMURNotifMgmtGroup: starMURSFTPMessage added to the list of objects.
- starMURNotifGroup added the following objects:
  starMURSFTPFailure
  starMURSFTPNormal
- starTrapGroup added the following objects:
  starVLRAssocDown
  starVLRAssocUp
  starVLRAllAssocDown
  starVLRAllAssocDownClear
  starHenbgwAccessServiceStart
  starHenbgwAccessServiceStop
  starHenbgwNetworkServiceStart
  starHenbgwNetworkServiceStop
  starEnhancedCongestion