# Starent Chassis Traps

This chapter describes the traps for the system.

MIB Textual Conventions

The following are the starOS traps.

Information on standards-based traps can be found here: Standards-Based Traps.

enterprise.8164.starentTraps(2)

Object

starCardTempOverheat

Object ID

enterprise.8164.2.1

Description

The card has reached a temperature beyond its safe operating range.

Probable Cause: External temperature is too high; one or more fan failures; blockages that prevent fan air inflow/outflow.

Action to be Taken: Inspect chassis for any item that may be blocking chassis air flow. Verify adjacent equipment is not obstructing air flow. Verify that the fans are running via the CLI/Web Element Manager. Check air filters. Check the chassis maintenance schedule to see if chassis needs routine air filter replacement. Verify room temperature is within acceptable operating conditions.

Clear Condition: This condition is cleared when the card reaches its operating temperature range or is removed from the system.

Condition Clear Alarm: This condition is cleared by a starCardTempOK notification.

Objects

starSlotNum

starCardTemperature
Object

starCardTempOK

Object ID

enterprise.8164.2.2

Description

The temperature of the card is now within its safe operating range. This notification is only generated if the card has previously generated a starCardTempOverheat notification.

Action to be Taken: No action required. The cause for the card overheat condition should be investigated.

Objects

starSlotNum

starCardTemperature
Object

starCardReset

IMPORTANT:

This trap is obsolete.

Object ID

enterprise.8164.2.3

Description

A reset operation has been invoked on the card.

Objects

starSlotNum

starCardType
Object

starCardRebootRequest

Object ID

enterprise.8164.2.4

Description

A reboot operation has been invoked on this card by an administrator. If successful, a subsequent starCardDown trap is typically generated.

Action to be Taken: No action required. If the reboot was not scheduled, the admin logs can be examined to determine who invoked the reboot operation.

Objects

starSlotNum

starCardType
Object

starCardUp

Object ID

enterprise.8164.2.5

Description

The card is up (operational).

Objects

starSlotNum

starCardType
Object

starCardVoltageFailure

Object ID

enterprise.8164.2.6

Description

A voltage regulation failure has been detected this card.

Probable Cause: Problem with incoming power; failure of power filters; hardware issue with card. Note that this is an extremely abnormal condition.

Action to be Taken: Verify that the power supplied to the chassis is operating correctly; use the CLI/Web Element Manager to check the state of the chassis power filters; replace the card.

Clear Condition: This is not a recoverable error except via restarting the card, so the condition is only cleared via a starCardUp or starCardActive notification.

Objects

starSlotNum

starCardType
Object

starCardRemoved

Object ID

enterprise.8164.2.7

Description

A card has been removed from the chassis.

Probable Cause: An operator has physically unlocked and removed a card from the chassis.

Action to be Taken: No action is required. If the card removal was unplanned, the admin logs can identify the time when the card was initially unlocked.

Objects

starSlotNum

starCardType
Object

starCardInserted

Object ID

enterprise.8164.2.8

Description

A card has been inserted into the chassis.

Objects

starSlotNum

starCardType
Object

starCardBootFailed

Object ID

enterprise.8164.2.9

Description

A card has failed to start properly. The card is not operational.

Probable Cause: The system logs should contain additional information about the cause of the boot failure.

Objects

starSlotNum

starCardType
Object

starCardFailed

Object ID

enterprise.8164.2.10

IMPORTANT:

This trap is obsolete.

Description

The card has failed and is no longer operational.

Objects

starSlotNum

starCardType
Object

starCardSWFailed

IMPORTANT:

This trap is obsolete.

Object ID

enterprise.8164.2.11

Description

An unrecoverable software error has occurred on the card.

Objects

starSlotNum
Object

starCardRCCFailed

Object ID

enterprise.8164.2.12

IMPORTANT:

This trap is obsolete.

Description

The RCC has failed.

Probable Cause: A hardware failure on the redundancy crossbar card.

Objects

starSlotNum
Object

starCardMismatch

Object ID

enterprise.8164.2.13

Description

The card does not match its configuration, or the card does not match the slot it was inserted into, or the card is of an unsupported type.

Probable Cause: A card was inserted into a slot which was configured for a different type of card. For example, a Gigabit Ethernet card was inserted into a slot configured for a Fast Ethernet card.

Clear Condition: A starCardUp or starCardActive notification is issued to confirm that this condition has been cleared.

Objects

starSlotNum

starCardType
Object

starCardFailureLEDOn

IMPORTANT:

This trap is obsolete.

Object ID

enterprise.8164.2.14

Description

The failure LED is illuminated on the card.

Objects

starSlotNum

starCardType
Object

starCardFailureLEDOff

IMPORTANT:

This trap is obsolete.

Object ID

enterprise.8164.2.15

Description

The failure LED is no longer illuminated on the card. This notification is only generated if the card has previously generated a starCardFailureLEDOn notification.

Objects

starSlotNum

starCardType
Object

starCardPACMigrateStart

Object ID

enterprise.8164.2.16

Description

A packet processing card migration operation has begun. The first varbind identifies the packet processing card being migrated away from; the second varbind identifies the card being migrated to.

Probable Cause: This is typically caused by an operator action; it can also represent the system recovering from a software or hardware fault.

Clear Condition: A starCardPACMigrateComplete notification is generated when the migration is complete.

Objects

starSlotNum

starSlotNum
Object

starCardPACMigrateComplete

Object ID

enterprise.8164.2.17

Description

A packet processing card migration operation has successfully completed. The first varbind identifies the card that was migrated away from; the second varbind identifies the card that was migrated to.

Objects

starSlotNum

starSlotNum
Object

starCardPACMigrateFailed

Object ID

enterprise.8164.2.18

Description

A packet processing card migration operation has failed. The first varbind identifies the card that was attempted to be migrated away from; the second varbind identifies the card that was being migrated to.

Probable Cause: The packet processing card being migrated to was removed or reset before the migration completed; the migration operation was terminated by an operator; or a software or hardware failure on either packet processing card involved in the migration operation.

Clear Condition: The packet processing card in question will be reset; a starCardUp notification will be generated when the card is operational again.

Objects

starSlotNum

starSlotNum
Object

starCardSPCSwitchoverStart

Object ID

enterprise.8164.2.19

Description

A chassis management card switchover operation has begun. The first varbind identifies the chassis management card being switched away from; the second varbind identifies the card being switched to. Note that since a switchover can cause a momentary loss of communication through the management (SPIO) interface, it is possible that this trap will not be successfully delivered.

Probable Cause: This is typically caused by an operator; it can also represent the system recovering from a software or hardware fault.

Action to be Taken: If the chassis management card switchover was unplanned, the admin logs should be examined for the cause of the switchover. If the cause was a software failure, the system crash logs should be examined.

Clear Condition: Verify the switchover completes successfully.

Clear Condition Alarm: A starCardSPCSwitchoverComplete is generated when the switchover operation has completed.

Objects

starSlotNum

starSlotNum
Object

starCardSPCSwitchoverComplete

Object ID

enterprise.8164.2.20

Description

A chassis management card switchover has completed successfully. The starSlotNum varbind identifies the new primary chassis management card.

Action to be Taken: If the witchover was unplanned, the admin logs should be examined for the cause of the switchover. If the cause was a software failure, the system crash logs should be examined.

Objects

starSlotNum
Object

starCardSPCSwitchoverFailed

Object ID

enterprise.8164.2.21

Description

A chassis management card switchover operation has failed. The first varbind identifies the chassis management card that was attempted to be switched away from; the second varbind identifies the card that was attempted to be switched to.

Probable Cause: The chassis management card being migrated to was removed or reset before the migration completed; the migration operation was terminated by an operator; or a software or hardware failure on either chassis management card.

Action to be Taken: Verify that both chassis management cards have the card locks in the locked position; examine the admin logs for the cause of the failure. If the cause was a software failure, the system crash logs should be examined.

Clear Condition: The chassis management card in question will be reset; a starCardUp notification will be generated when the card is operational again.

Objects

starSlotNum

starSlotNum
Object

starFanFailed

Object ID

enterprise.8164.2.22

Description

One of more fans have failed on the indicated fan controller.

Probable Cause: A hardware failure on the fan tray. The fan tray should be replaced.

Action to be Taken: Verify there is no physical obstruction to the fans or replace the fan tray.

Clear Condition: Verify the fans are running

Condition Clear Alarm: A starFanInserted notification will be generated when the fan tray is replaced.

Objects

starFanNum
Object

starFanRemoved

Object ID

enterprise.8164.2.23

Description

A fan tray has been removed.

Action to be Taken: Replace the fan tray.

Clear Condition: Verify both fan trays are present and operational.

Condition Clear Alarm: A starFanInserted notification will be generated when the fan tray is replaced.

Objects

starFanNum
Object

starFanInserted

Object ID

enterprise.8164.2.24

Description

A fan tray has been inserted.

Objects

starFanNum
Object

starLogThreshold

IMPORTANT:

This trap is obsolete.

Object ID

enterprise.8164.2.25

Description

A system log has reached its maximum size.

Objects

starLogName

starLogCurSize

starLogMaxSize
Object

starCPUBusy

Object ID

enterprise.8164.2.26

Description

The CPU is experiencing very high usage.

Probable Cause: For chassis management card CPUs this typically represents an abnormal amount of management (CLI, SNMP, CORBA) requests. For packet processing cards, this indicates that the system is reaching its capacity.

Action to be Taken: For chassis management cards, this may be a transient condition because of a burst of management activity. Monitor the CPU usage and if it is persistently high, examine the CPU table to determine which management activity is causing the excessive usage. For packet processing cards, this indicates the system is nearing its overall capacity. Monitor CPU usage and if it is persistently high, the system may need additional hardware to keep up with the system load.

Clear Condition: Verify that CPU usage returned to a normal load. This can represent a transient condition; the trap will be periodically repeated if the condition persists.

Objects

starCPUSlot

starCPUNumber
Object

starCPUMemoryLow

Object ID

enterprise.8164.2.27

Description

The CPU is experiencing a low memory condition.

Probable Cause: For chassis management card CPUs this typically represents an abnormal number of management sessions, in particular CLI sessions. For packet processing cards this indicates that the system is reaching its capacity.

Action to be Taken: For chassis management cards, this may be a transient condition because of a burst of management activity. Monitor memory usage and if it is persistently high, examine the CPU table to determine which management activity is causing the excessive usage. Verify that large numbers of CLI sessions are not being generated and, if needed, terminate extra sessions. For packet processing cards, this indicated the system is nearing its overall capacity. Monitor memory usage and if it is persistently high, the system may need additional packet processing cards or additional card memory to keep up with the system load.

Clear Condition: Verify that memory usage has returned to a normal load. This can represent a transient condition; the trap will be periodically repeated if the condition persists.

Objects

starCPUSlot

starCPUNumber
Object

starCPUMemoryFailed

Object ID

enterprise.8164.2.28

Description

The memory on this CPU has failed.

Probable Cause: This indicates a hardware problem.

Action to be Taken: Replace the failing card.

Clear Condition: The card will be reset; a starCardUp will be generated if the card is restored to an operational state.

Objects

starCPUSlot

starCPUNumber
Object

starCPUFailed

Object ID

enterprise.8164.2.29

Description

The CPU has failed.

Probable Cause: This indicates a hardware problem.

Action to be Taken: Replace the failing card.

Clear Condition: The card will be reset; a starCardUp will be generated if the card is restored to an operational state.

Objects

starCPUSlot

starCPUNumber
Object

starCPUWatchDogExpired

Object ID

enterprise.8164.2.30

Description

The watchdog timer has failed on this CPU.

Probable Cause: This could indicate an extremely busy CPU, a software problem, or a hardware issue.

Action to be Taken: Check the admin logs for an indication of the problem. Check the system crash logs for an indication of software problems. If the problem persists, replace the card.

Clear Condition: Verify that a chassis management card switchover or packet processing card migration completes successfully to recover from the failure condition.

Condition Clear Alarm: A starCardUp notification will be generated if the card is restored to an operational state.

Objects

starCPUSlot

starCPUNumber
Object

starNPUARPPoolExhausted

Object ID

enterprise.8164.2.31

Description

The ARP pool on this NPU manager is exhausted. When this occurs, the ARP entry isn't added and traffic to the local device is forwarded through a slower path.

Action To Be Taken: Reduce the total number of directly connected devices or clear ARP entries.

Objects

starNPUMgrNumber
Object

starPowerFilterUnitFailed

IMPORTANT:

This trap is obsolete.

Object ID

enterprise.8164.2.32

Description

A Power Filter Unit (PFU) failed.

Probable Cause: The external power source has failed or has been disconnected, or a hardware failure on the PFU.

Action to be Taken: Verify that the input power to the power filter is operational and repair if needed. Verify that the connections to the power filter are intact and that the power filter is properly inserted into the chassis. Replace the power filter if required.

Clear Condition: Verify that both power filters are operating.

Condition Clear Alarm: A starPowerFilterAvail notification will be generated when the power filter is replaced.

Objects

starPowerNumber
Object

starPowerFilterUnitUnavail

Object ID

enterprise.8164.2.33

Description

A Power Filter Unit (PFU) is unavailable.

Probable Cause: The power filter has been removed from the chassis, or no power is being provided to the PFU.

Action to be Taken: If the power filter removal wasn't planned, verify that the input power to the power filter is operational and repair if needed. Verify that the connections to the power filter are intact and that the power filter is properly inserted into the chassis. Replace the power filter if required.

Clear Condition: Verify that both power filters are operating.

Condition Clear Alarm: A starPowerFilterUnitAvail will be generated when the power filter is replaced.

Objects

starPowerNumber
Object

starPowerFilterUnitAvail

Object ID

enterprise.8164.2.34

Description

A Power Filter Unit (PFU) is available. This typically means that a PFU has been inserted into the chassis or has its power source restored.

Action to be Taken: No action required.

Objects

starPowerNumber
Object

starAlertsDisabled

Object ID

enterprise.8164.2.37

Description

The sending of SNMP traps has been disabled because too many alerts were generated within the defined window type.

Probable Cause: Either a large number of SNMP notifications are being generated, or the configured threshold which limits the number of notifications is set too aggressively.

Actions to be Taken: Examine the admin logs and the SNMP trap logs to determine the source of the large number of traps and take appropriate actions; verify that the configured limit for the rate at which traps will be sent is appropriate for your environment.

Clear Condition Alarm: When the rate of SNMP notifications goes down, a starAlertsEnabled notification is generated.

Objects

starMaxAlertsPerTime

starWindowTime
Object

starAlertsEnabled

Object ID

enterprise.8164.2.38

Description

The sending of SNMP Traps has been re-enabled.
Object

starAAAAuthServerUnreachable

Object ID

enterprise.8164.2.39

Description

The Authentication, Authorization and Accounting (AAA) server cannot be reached.

Probable Cause: The AAA server is down, or there is a network issue preventing communication with the AAA server.

Actions to be Taken: Restore the AAA server to an operational status. Verify that the AAA server is reachable by performing a 'ping' operation from the CLI in the appropriate context. Check the admin logs for notification of communication problems.

Clear Condition: Verify that communication to the AAA authentication server has been restored.

Condition Clear Alarm: When this condition clears, a starAAAAuthServerReachable notification will be generated. Note that if in a AAA group all the configured RADIUS servers are detected as down, their state is brought back to Active before the deadtime expiry period so that call setup signaling with AAA can proceed for subsequent requests. Therefore, when the last active authentication server in the group is detected as being down, a starAAAAuthServerUnreachable notification is generated. When the server state changes to Active, a starAAAAuthServerReachable notification is generated. This behavior is the same when there is only one RADIUS server configured.

Objects

radiusAuthServerIndex

radiusAuthServerAddress
Object

starAAAAuthServerReachable

Object ID

enterprise.8164.2.40

Description

The Authentication, Authorization and Accounting (AAA) server is now reachable. This can be the result of a system startup, the configuration of a new server, or a previously unreachable server becoming reachable.

Action to be Taken: No Action Required.

Objects

radiusAuthServerIndex

radiusAuthServerAddress
Object

starAAAAuthServerMisconfigured

Object ID

enterprise.8164.2.41

Description

The Authentication, Authorization and Accounting (AAA) server has been misconfigured. This server is not usable until this condition is repaired.

Action to be Taken: Examine the system configuration and correct the misconfiguration. See the user documentation for details on AAA configuration.

Clear Condition: Verify that communication to the AAA authentication server has been restored.

Condition Clear Alarm: When this condition clears, a starAAAAuthServerReachable notification will be generated.

Objects

radiusAuthServerIndex

radiusAuthServerAddress
Object

starAAAAccServerUnreachable

Object ID

enterprise.8164.2.42

Description

The Authentication, Authorization and Accounting (AAA) server cannot be reached.

Probable Cause: The AAA server is down, or there is a network issue preventing communication with the AAA server.

Actions to be Taken: Restore the AAA server to an operational status; Verify that the AAA server is reachable by performing a 'ping' operation from the CLI in the appropriate context. Check the admin logs for notification of communication problems.

Clear Condition: Verify that communication to the AAA accounting server has been restored.

Condition Clear Alarm: When this condition clears a starAAAAccServerReachable notification will be generated. Note that if in a AAA group all the configured RADIUS servers are detected as down, their state is brought back to active before the deadtime expiry period so that call setup signaling with AAA can proceed for subsequent requests. Therefore, when the last Active Accounting server in the group is detected as being down, a starAAAAccServerUnreachable notification is generated. When the server state changes to Active, a starAAAAccServerReachable is generated. This behavior is the same when there is only one RADIUS server configured.

Objects

radiusAccServerIndex

radiusAccServerAddress
Object

starAAAAccServerReachable

Object ID

enterprise.8164.2.43

Description

The Authentication, Authorization and Accounting (AAA) server is now reachable. This can be the result of a system startup, the configuration of a new server, or a previously unreachable server becoming reachable. Note that since Accounting servers are not responding to 'hello'-type messages, it is not always possible to accurately determine when an accounting server is reachable. A server may be declared 'reachable' when the chassis is ready to start using the server, but before any acknowledgement is actually received from the server. Once accounting information actually is sent to the server a starAAAAccServerUnreachable will be generated if the server does not properly respond.

Action to be Taken: No Action Required.

Objects

radiusAccServerIndex

radiusAccServerAddress
Object

starAAAAccServerMisconfigured

Object ID

enterprise.8164.2.44

Description

The Authentication, Authorization and Accounting (AAA) server has been misconfigured. This server is not usable until this condition is repaired.

Action to be Taken: Examine the system configuration and correct the misconfiguration. See the user documentation for details on AAA configuration.

Clear Condition: Verify that communication to the AAA authentication server has been restored.

Condition Clear Alarm: When this condition clears, a starAAAAccServerReachable notification will be generated.

Objects

radiusAccServerIndex

radiusAccServerAddress
Object

starLogMsg

Object ID

enterprise.8164.2.45

Description

A log message. This trap is used only for debugging.

Objects

starLogText
Object

starPDSNServiceStart

Object ID

enterprise.8164.2.46

Description

A PDSN service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starPDSNServiceStop

Object ID

enterprise.8164.2.47

Description

A PDSN service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the PDSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PDSN service is operational.

Condition Clear Alarm: A starPDSNServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starHAServiceStart

Object ID

enterprise.8164.2.48

Description

An HA service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starHAServiceStop

Object ID

enterprise.8164.2.49

Description

An HA service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of resources (packet processing cards) to support the running configuration.

Action to be Taken: If the PDSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PDSN service is operational.

Condition Clear Alarm: A starHAServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starFAServiceStart

Object ID

enterprise.8164.2.50

Description

An FA service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starFAServiceStop

Object ID

enterprise.8164.2.51

Description

An FA service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the FA service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the FA service is operational.

Condition Clear Alarm: A starFAServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starCLISessionStart

Object ID

enterprise.8164.2.52

Description

An interactive CLI session has started.

Condition Clear Alarm: A starCLISessionEnd notification will be sent when the CLI session is terminated.

Objects

starCLIUsername

starCLIPrivs

starCLITtyname
Object

starCLISessionEnd

Object ID

enterprise.8164.2.53

Description

An interactive CLI session has ended. The CLI session may have been terminated by the CLI user; the session may have expired due to an idle timeout, or a session timeout; or the session may have been terminated by operator intervention.

Objects

starCLIUsername

starCLIPrivs

starCLITtyname
Object

starCritTaskFailed

Object ID

enterprise.8164.2.54

Description

A critical task has failed and the appropriate recovery steps begun. The card containing the failed task will be restarted; migration/recovery operations will proceed.

Probable Cause: Software error.

Actions to be Taken: Examine the admin logs for an indication of the source of the failure.

Clear Condition: Verify that a chassis management card switchover or card migration completes to recover from this condition.

Condition Clear Alarm: A starCardUp notification will be generated when the card restarts.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU
Object

starCardActive

Object ID

enterprise.8164.2.55

Description

The card is now active.

Objects

starSlotNum

starCardType
Object

starLACServiceStart

Object ID

enterprise.8164.2.56

Description

A LAC service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starLACServiceStop

Object ID

enterprise.8164.2.57

Description

A LAC service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the LAC service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the LAC service is operational.

Condition Clear Alarm: A starLACServiceStart notification will be generated when the service restarts.

Objects

starServiceVpnName

starServiceServName
Object

starLNSServiceStart

Object ID

enterprise.8164.2.58

Description

A LNS service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starLNSServiceStop

Object ID

enterprise.8164.2.59

Description

A LNS service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the LNS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the LNS service is operational.

Condition Clear Alarm: A starLNSServiceStart notification will be generated when the service restarts.

Objects

starServiceVpnName

starServiceServName
Object

starCardDown

Object ID

enterprise.8164.2.60

Description

The card is now down.

Probable Cause: The card was shut down by an operator; the card was removed by an operator; or a hardware or software fault caused the card to shut down. In the latter case an additional notification is generated with the specific failure.

Action to be Taken: If the card shutdown was not planned, verify that the card is present in the system and its card lock is in the locked position. Check the admin logs for the cause of the card shutdown.

Clear Condition: Verify that a chassis management card switchover/card migration completes to recover from the card shutdown.

Condition Clear Alarm: A starCardUp notification is generated when the card is restarted.

Objects

starSlotNum

starCardType
Object

starDsx3LineStatusChange

Object ID

enterprise.8164.2.61

Description

As defined by RFC2496, this trap (mib-2.10.30.15.0 1) is sent when there is a change in the value of a Dsx3LineStatus instance. If the line status change is the result of a line status change at a lower level (i.e. ds1), then no traps for the ds3 are sent.

Objects

dsx3LineStatus

dsx3LineStatusLastChange
Object

starDsx1LineStatusChange

Object ID

enterprise.8164.2.62

Description

As defined by RFC2496, this trap (mib-2.10.18.15.0 1) is sent when there is a change in the value of a Dsx1LineStatus instance. If the line status change is the result of a line status change at a higher level (i.e. ds3), then no traps for the ds1 are sent.

Objects

dsx1LineStatus

dsx1LineStatusLastChange
Object

starGGSNServiceStart

Object ID

enterprise.8164.2.63

Description

A GGSN Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starGGSNServiceStop

Object ID

enterprise.8164.2.64

Description

A GGSN Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the GGSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the GGSN service is operational.

Condition Clear Alarm: A starGGSNServiceStart notification will be generated when the service restarts.

Objects

starServiceVpnName

starServiceServName
Object

starLicenseExceeded

Object ID

enterprise.8164.2.65

Description

The licenses session limit has been exceeded; note that a small number of sessions are permitted beyond the licensed limit.

Probable Cause: System usage has exceeded the capacity of the license installed, the license installed does not match the identification of the system. No license is installed.

Action to be Taken: Verify that the proper license is installed on the system, verify that the SPCs present in the system match those identified in the software license. If required, install an additional higher-capacity license.

Clear condition: This condition is cleared when usage goes under the licensed limit.

Condition clear alarm: This condition is cleared by a starLicenseUnderLimit notification.

Objects

starLicensedSessions

starCurrentSessions

starServiceType
Object

starSubscriberLimit

Object ID

enterprise.8164.2.66

Description

The specified service has reached its configured limit for number of subscribers.

Action to be Taken: Verify that the configured subscriber limit is correct. Configure additional services, or configure the existing service to permit a larger number of subscribers.

Objects

starServiceVpnName

starServiceServName

starServiceSubLimit

starServiceSubCurrent

starServiceType
Object

starSessionRejectNoResource

Object ID

enterprise.8164.2.67

Description

A session setup was rejected because of a lack of available resources.

Probable Cause: The system has reached its maximum capacity based on the number of available packet processing cards/CPUs/memory.

Actions to be Taken: Examine the system CPU table to determine if there is abnormal system usage or if the system is reaching its capacity. If this condition persists, additional processing cards or memory may be required. Note that there is a configuration threshold which can be setup to monitor the number of NORESOURCE rejects.

Objects

starServiceType

starServiceVpnName
Object

starLongDurTimerExpiry

Object ID

enterprise.8164.2.68

Description

The long duration timer has expired for the identified subscriber.

Action to be Taken: No action is typically required. If an abnormal number of expiries occur, verify that the configuration expiry time is correct.

Objects

starSubContext

starSubMSID

starSubName

starSubTimerDuration

starSubLongDurTimeoutAction

starSubSetupTime

starSubHomeAddr

starSubHomeAddrv6
Object

starClosedRPServiceStart

Object ID

enterprise.8164.2.69

Description

Closed RP Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starClosedRPServiceStop

Object ID

enterprise.8164.2.70

Description

Closed RP Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the Closed RP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the Closed RP service is operational.

Condition Clear Alarm: A starClosedRPServiceStart notification will be generated when the service restarts.

Objects

starServiceVpnName

starServiceServName
Object

starGtpcPathFailure

Object ID

enterprise.8164.2.71

Description

GTP Control Path Failure.

Objects

starSessGGSNVpnName

starSessGGSNServName

starSessGGSNPeerAddr
Object

starGtpuPathFailure

Object ID

enterprise.8164.2.72

Description

GTP Data Path Failure.

Objects

starSessGGSNVpnName

starSessGGSNServName

starSessGGSNPeerAddr
Object

starManagerFailure

Object ID

enterprise.8164.2.73

Description

Software manager failure.

Probable Cause: A software failure. The failing manager will be restarted.

Action to be Taken: Examine the admin and crash logs for more information about the failure.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU
Object

starEISServerAlive

Object ID

enterprise.8164.2.74

Description

EIS Server alive.

Objects

starEISServerVPNID

starEISServerAddr
Object

starEISServerDead

Object ID

enterprise.8164.2.75

Description

EIS Server down.

Probable Cause: The remote EIS server is down or there is a network error making it unreachable.

Condition Clear Alarm: A starEISServerAlive notification will be generated when this condition is cleared.

Objects

starEISServerVPNID

starEISServerAddr
Object

starCgfAlive

Object ID

enterprise.8164.2.76

Description

GTPP CGF Server is alive.

Objects

starSessGGSNVpnName

starSessGGSNPeerPort

starSessGGSNPeerAddr
Object

starCgfDead

Object ID

enterprise.8164.2.77

Description

GTPP CGF Server is dead.

Probable Cause: The remote CGF server is down or there is a network error making it unreachable.

Action to be Taken: Verify that the CGF server is functioning properly, or verify network connectivity to the CGF server.

Clear Condition: This condition is cleared when the CGF server becomes reachable.

Condition Clear Alarm: A starCgfServerAlive notification will be generated when this condition is cleared.

Objects

starSessGGSNVpnName

starSessGGSNPeerPort

starSessGGSNPeerAddr
Object

starStorageServerAlive

Object ID

enterprise.8164.2.78

Description

GTPP Storage Server is alive.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr
Object

starStorageServerDead

Object ID

enterprise.8164.2.79

Description

GTPP Storage Server is dead.

Probable Cause: The remote storage server is down. There is a network error making it unreachable.

Action to be Taken: Verify that the storage server is functioning properly, or verify network connectivity to the storage server.

Clear Condition: This condition is cleared when the storage server becomes reachable.

Condition Clear Alarm: A starStorageServerAlive notification is generated when this condition is cleared.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr
Object

starGgsnInitiatedUpdtFailed

Object ID

enterprise.8164.2.80

Description

GGSN initiated update PDP context response failed.

Probable Cause: This can happen if there is an inter-SGSN handoff and the new SGSN is not listed in GGSN service and its PLMN policy is set to reject unknown SGSNs.

Action to be Taken: List the SGSN address in the GGSN service.

Condition Clear Alarm: N/A

Objects

starSessGGSNVpnName

starSessGGSNServName

starSessGGSNSubsName

starSessGGSNAPNName

starSessGGSNImsi

starSessGGSNPeerAddr
Object

starCongestion

Object ID

enterprise.8164.2.81

Description

A congestion condition has occurred.

Probable Cause: This is the result of an operator-configured congestion threshold being reached. This can be due to high usage of the resource being monitored which indicates that the system is reaching its peak capacity, or could be caused by the incorrect configuration of the congestion thresholds.

Actions to be Taken: Verify that the congestion thresholds are correct, if the congested state is seem repeatedly, or, for sustained periods of time, additional system capacity may need to be brought online.

Clear Condition: This condition is cleared when the use of the specific resource falls below the configured limit.

Condition Clear Alarm: A starCongestionClear notification is sent when there are no congestion conditions for a service type.

Objects

starServiceType

starCongestionPolicy

starCongestionResourceType
Object

starCongestionClear

Object ID

enterprise.8164.2.82

Description

A congestion condition has cleared.

Objects

starServiceType
Object

starServiceLossPTACs

Object ID

enterprise.8164.2.83

Description

A service loss condition has occurred due to packet processing card failure or removal.

Probable Cause: Multiple packet processing cards are no longer available due to failure, removal, or other operator action; or, configuration changes have been made which eliminated the availability of redundant cards.

Action to be Taken: Bring additional packet processing cards online to match the number of configured cards, or update the configuration to require fewer active cards.

Clear Condition: This condition is cleared when the number of active packet processing cards reaches or exceeds the configured number.

Objects

starCardMode

starPTACConfig

starPTACActive
Object

starServiceLossLC

Object ID

enterprise.8164.2.84

Description

A service loss condition has occurred due to LC failure or removal.

Probable Cause: Multiple line cards (LCs) are no longer available due to failure, removal, or operator action.

Action to be Taken: Bring additional LCs online to match the number of configured cards, or update the configuration to require fewer active LCs.

Clear Condition: This condition is cleared when the number of active line cards reaches or exceeds the configured number.

Objects

starCardType

starSlotNum

starSlotNum
Object

starServiceLossSPIO

Object ID

enterprise.8164.2.85

Description

A service loss condition has occurred due to SPIO failure or removal. Since the SPIO contains the ports used for SNMP access, this notification cannot normally be delivered as an SNMP trap. The notification will be logged and stored in the historical trap list, and if the system is configured to send INFORM PDUs the notification might be delivered at a later time.

Probable Cause: Both SPIOs are no longer available due to failure, removal, or operator action.

Action to be Taken: Bring at least one SPIO online.

Clear Condition: This condition is cleared when a SPIO is made active.
Object

starIPSPAllAddrsFree

Object ID

enterprise.8164.2.86

Description

All IP addresses are now free on the IP Pool Sharing Protocol (IPSP) primary HA.

Probable Cause: IP Pool Sharing Protocol (IPSP) is running between two HAs (a primary and a secondary). The primary HA has now released the last address that was in use. This presumably is done in preparation for taking the primary HA out of server.

Action to be Taken: Perform the desired maintenance on the primary HA that required taking the device out of service.

Objects

starContextName

starInterfaceName
Object

starPCFUnreachable

Object ID

enterprise.8164.2.87

Description

A PCF that the system communicates with is no longer reachable.

Probable Cause: The PCF has failed or is otherwise unavailable, or a network connectivity problem makes it unreachable.

Action to be Taken: If the PCF outage was unplanned, restart/reset the PCF, and verify network connectivity.

Objects

starContextName

starPCFAddress
Object

starDhcpAlive

Object ID

enterprise.8164.2.88

Description

DHCP server alive.

Objects

starSessGGSNVpnName

starSessGGSNPeerPort

starSessGGSNPeerAddr
Object

starDhcpDead

Object ID

enterprise.8164.2.89

Description

DHCP server dead.

Probable Cause: The remote DHCP server is down or there is a network error making it unreachable.

Action to be Taken: Verify that the DHCP server is functioning properly; verify network connectivity to the DHCP server.

Clear Condition: The condition is cleared when the DHCP server becomes reachable, or if the configuration is changed to not use this server.

Condition Clear Alarm: A starDhcpAlive notification is generated when the server becomes reachable.

Objects

starSessGGSNVpnName

starSessGGSNPeerPort

starSessGGSNPeerAddr
Object

starNTPPeerUnreachable

Object ID

enterprise.8164.2.90

Description

NTP peer unreachable.

Probable Cause: The NTP server is down or unavailable, or there is a network connectivity issue that prevents access to the NTP server.

Action to be Taken: Verify that the NTP server is running properly; verify that the connection to the NTP server is functioning.

Clear Condition: This condition is cleared when the NTP server becomes reachable.

Condition Clear Alarm: This condition is cleared by a starNTPPeerReachable notification.

Objects

starPeerAddress
Object

starNTPSyncLost

Object ID

enterprise.8164.2.91

Description

NTP synchronization lost.

Probable Cause: All configured NTP servers are no longer available, or some/all NTP servers have been un-configured by an operator.

Action to be Taken: Verify that the NTP server(s) are running properly and that the network connections to the NTP servers are available. Check the configured of the NTP servers for correctness. If needed, configure additional NTP servers.

Clear Condition: This condition is cleared when any (one) NTP server becomes reachable.

Condition Clear Alarm: This condition is cleared by a starNTPSyncEstablished notification.
Object

starL2TPTunnelDownPeerUnreachable

Object ID

enterprise.8164.2.92

Description

L2TP tunnel down due to peer unreachable.

Probable Cause: Misconfiguration of the peer router address or inability to route to the peer.

Action to be Taken: Verify the peer address is correct; verify that the peer is operational; verify network connectivity to the peer.

Objects

starL2TPLocalTunnelID

starL2TPPeerTunnelID

starL2TPContextName

starL2TPServiceName

starL2TPServiceTypeName

starL2TPLocalAddress

starL2TPPeerAddress
Object

starCardStandby

Object ID

enterprise.8164.2.93

Description

The card is now in standby mode.

Objects

starSlotNum

starCardType
Object

starLicenseUnderLimit

Object ID

enterprise.8164.2.94

Description

Usage is now under the licensed session limit.

Objects

starLicensedSessions

starCurrentSessions

starServiceType
Object

starIPSECPriTunDown

Object ID

enterprise.8164.2.95

Description

IPSEC primary tunnel is down

Objects

starIPSECContextName

starIPSECGroupName

starIPSECTunLocalIPAddr

starIPSECTunRemoteIPAddr
Object

starIPSECPriTunUp

Object ID

enterprise.8164.2.96

Description

IPSEC primary tunnel is up

Objects

starIPSECContextName

starIPSECGroupName

starIPSECTunLocalIPAddr

starIPSECTunRemoteIPAddr
Object

starIPSECSecTunDown

Object ID

enterprise.8164.2.97

Description

IPSEC secondary tunnel down

Objects

starIPSECContextName

starIPSECGroupName

starIPSECTunLocalIPAddr

starIPSECTunRemoteIPAddr
Object

starIPSECSecTunUp

Object ID

enterprise.8164.2.98

Description

IPSEC secondary tunnel is up

Objects

starIPSECContextName

starIPSECGroupName

starIPSECTunLocalIPAddr

starIPSECTunRemoteIPAddr
Object

starIPSECTunSwitchFail

Object ID

enterprise.8164.2.99

Description

IPSEC tunnel switchover failed or unable to be attempted.

Objects

starIPSECContextName

starIPSECGroupName
Object

starIPSECTunSwitchComplete

Object ID

enterprise.8164.2.100

Description

IPSEC tunnel switchover complete

Objects

starIPSECContextName

starIPSECGroupName

starIPSECTunLocalIPAddr

starIPSECTunRemoteIPAddr
Object

starNwReachServerAlive

Object ID

enterprise.8164.2.101

Description

Nw reachable server alive

Objects

starNwReachName

starNwReachSrvrAddr
Object

starNwReachServerDead

Object ID

enterprise.8164.2.102

Description

Nw Reachable Server is dead.

Probable Cause: The remote server is down or there is a network error making it unreachable. A starNwReachServerAlive notification will be generated when this condition is cleared.

Objects

starNwReachName

starNwReachSrvrAddr
Object

starStorageServerUnackedGcdrVolPurge

Object ID

enterprise.8164.2.103

Description

GTPP storage server has performed un-acked GCDRs volume purge.

Probable Cause: GTPP storage server has purged un-acked GCDRs after hitting the max allowed configured limit on un-acked GCDR in the backup database.

Action to be Taken: Check for the unacked file generated for these GCDRs.

Clear Condition: There is no clear condition for this notification.

Condition Clear Alarm: There is no clear alarm for this notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr
Object

starStorageServerUnackedGcdrFileGen

Object ID

enterprise.8164.2.104

Description

GTPP storage server has exported the unacked GCDRs to file from backup db.

Probable Cause: GTPP storage server has generated and saved all the unacked GCDRs to file.

Action to be Taken: Operator needs to FTP the generated file.

Clear Condition: There is no clear condition for this notification.

Condition Clear Alarm: There is no clear alarm for this notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr
Object

starNTPPeerReachable

Object ID

enterprise.8164.2.105

Description

NTP peer reachable.

Probable Cause: The NTP server is reachable. This could indicate a newly configured NTP server (including an initial configuration on system startup) or could indicate a previously unreachable server has become reachable.

Action to be Taken: No action required.

Objects

starPeerAddress
Object

starNTPSyncEstablished

Object ID

enterprise.8164.2.106

Description

NTP Synchronization Established.

Probable Cause: An NTP server is available when previously no server was available. This could indicate a newly configured NTP server (including an initial configuration on system startup) or could indicate that one or more previously unreachable server(s) has become reachable.

Action to be Taken: No action required.
Object

starSIPServiceStart

Object ID

enterprise.8164.2.107

Description

A SIP service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starSIPServiceStop

Object ID

enterprise.8164.2.108

Description

A SIP service has stopped.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starVIMServiceStart

Object ID

enterprise.8164.2.109

Description

A VIM service has started.

Action to be Taken: No action required.

Syntax

starServiceVpnName

starServiceServName
Object

starVIMServiceStop

Object ID

enterprise.8164.2.110

Description

A VIM service has stopped. This is because an application is out-of-service, or vim is down, or there is no app. server.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starCHATCONFServiceStart

Object ID

enterprise.8164.2.111

Description

A CHAT/CONF service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starCHATCONFServiceStop

Object ID

enterprise.8164.2.112

Description

A CHAT/CONF service has stopped. This is because of application out-of-service or if chatconf is down or no app. server.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starSIPRouteNomatch

Object ID

enterprise.8164.2.113

Description

SIP session has failed since there is no match in the routing table with matching prefix.

Action to be Taken: Operator has to configure with matching prefix if required.

Objects

starSIPRouteVpnName

starSIPRouteVmgName

starSIPRouteAsName

starSIPRouteDestPartyNum

starSIPRouteReqNum
Object

starL3AddrUnreachable

Object ID

enterprise.8164.2.114

Description

An L3 address is unreachable through the specific slot and port.

Action to be Taken: No action required.

Objects

starL3Address

starPortSlot

starPortNum
Object

starSWUpgradeStart

Object ID

enterprise.8164.2.115

Description

An operator has begun to upgrade the software on the chassis.
Object

starSWUpgradeComplete

Object ID

enterprise.8164.2.116

Description

An operator-initiated software upgrade has been completed.
Object

starSWUpgradeAborted

Object ID

enterprise.8164.2.117

Description

An operator-initiated software upgrade has been aborted.
Object

starBGPPeerSessionUp

Object ID

enterprise.8164.2.118

Description

The BGP peer session to the specified IP address is operational. This may indicate the initial configuration of a new peer, the initial connectivity after a system restart, or the restoration of connectivity after a starBGNPeerSessionDown event.

Action to be Taken: No action required.

Objects

starContextName

starBGPPeerIPAddress
Object

starBGPPeerSessionDown

Object ID

enterprise.8164.2.119

Description

The BGP peer session to the specified IP address is no longer operational.

Probable Cause: The BGP peer is not-operational; the network between the chassis and the BGP peer is experiencing an outage; or LC failure(s) on the chassis.

Action to be Taken: Verify the BGP peer is operational; verify network connectivity to the BGP peer.

Clear Condition Alarm: A starBGPPeerSessionUp notification is generated when connectivity is reestablished.

Objects

starContextName

starBGPPeerIPAddress
Object

starSRPActive

Object ID

enterprise.8164.2.120

Description

The SRP chassis status is now active.

Action to be Taken: No action is required.

Objects

starContextName

starSRPIPAddress
Object

starSRPStandby

Object ID

enterprise.8164.2.121

Description

The SRP chassis status is now Standby.

Action to be Taken: No action is required.

Objects

starContextName

starSRPIPAddress
Object

starBGPPeerReachable

Object ID

enterprise.8164.2.122

Description

The monitored BGP peer is now reachable. This notification can represent the initial detection of the peer's state, or the re-connection to a peer after a starBGPPeerDown notification.

Action to be Taken: No action is required.

Objects

starContextName

starSRPIPAddress

starUDPPortNum

starBGPPeerIPAddress
Object

starBGPPeerUnreachable

Object ID

enterprise.8164.2.123

Description

The monitored BGP peer is now unreachable.

Action to be Taken:V erify that the BGP Peer is running and is properly configured. Verify the network link to the BGP Peer.

Clear Condition: This condition is cleared when communication with the BGP peer is reestablished.

Condition Clear Alarm: This condition is cleared by a starBGPPeerReachable notification.

Objects

starContextName

starSRPIPAddress

starUDPPortNum

starBGPPeerIPAddress
Object

starSRPAAAReachable

Object ID

enterprise.8164.2.124

Description

The SRP AAA monitor has found a reachable AAA server. This notification can represent the initial detection of an AAA server, or the restoration of reachability after a starSRPAAAUnreachable notification. This notification is only generated if there was previously no reachable AAA server.

Action to be Taken: No action required.

Objects

starContextName

starSRPIPAddress

starUDPPortNum
Object

starSRPAAAUnreachable

Object ID

enterprise.8164.2.125

Description

The SRP AAA monitor has determined that all AAA servers are unreachable.

Action to be Taken: Verify the state of the configured AAA server(s) and restart them if required. Verify the network link to the AAA Server(s). Configure additional AAA servers if required.

Clear Condition: This condition is cleared when communication with any single AAA service is (re)established.

Condition Clear Alarm: This condition is cleared by a starSRPAAAReachable notification.

Objects

starContextName

starSRPIPAddress

starUDPPortNum
Object

starHASwitchoverInitiated

Object ID

enterprise.8164.2.126

Description

An HA Switchover operation has been initiated by an operator.

Action to be Taken: Verify that the switchover was a planned operator action.

Objects

starContextName

starSRPIPAddress
Object

starSRPCheckpointFailure

Object ID

enterprise.8164.2.127

Description

The system has detected that a checkpoint messaged failed to be sent successfully to the standby HA. If the active HA were to fail, this information will be lost.

Action to be Taken: Verify the communication path to the standby HA.

Objects

starContextName

starSRPIPAddress
Object

starSRPConfigOutOfSync

Object ID

enterprise.8164.2.128

Description

The system has detected that the standby HA has a different configuration than the active HA. In the event of a failure of the active HA, it is possible that the standby HA is not configured properly to be able to take over.

Action to be Taken: Update the configuration of the standby HA to match the active HA.

Clear Condition: This condition is cleared when the active HA confirms that the standby HA has a configuration.

Condition Clear Alarm: This condition is cleared by a starSRPConfigInSync notification.

Objects

starContextName

starSRPIPAddress
Object

starSRPConfigInSync

Object ID

enterprise.8164.2.129

Description

The system has detected that the standby HA has a matching configuration as the active HA. This notification is generated only after a starSRPConfigOutOfSync notification.

Action to be Taken: No action required.

Objects

starContextName

starSRPIPAddress
Object

starGESwitchFailure

Object ID

enterprise.8164.2.130

Description

A failure of an internal Gigabit Ethernet switch has been detected. If it is possible to determine the slow containing the failed switch it is identified in starSlotNum, otherwise starSlotNum is 0.

Action to be Taken: If this condition persists, the identified card needs to be replaced.

Objects

starSlotNum
Object

starSIPRouteServerAvailable

Object ID

enterprise.8164.2.131

Description

SIP route server is available.

Action to be Taken: No action required.

Objects

starSIPRouteServerVpnName

starSIPRouteServerVmgName

starSIPRouteServerAsName

starSIPRouteServerIpAddr
Object

starSIPRouteServerUnavailable

Object ID

enterprise.8164.2.132

Description

SIPsession has failed since the route server is unavailable.

Action to be Taken: Operator has to check the reason for the unavailability of the server and act accordingly.

Objects

starSIPRouteServerVpnName

starSIPRouteServerVmgName

starSIPRouteServerAsName

starSIPRouteServerIpAddr
Object

starFMDMaxCallRateReached

Object ID

enterprise.8164.2.133

Description

FMD max call rate reached.

Action to be Taken: Increase the value of fmd-max-call-rate or set no fmd-max-call-rate.

Condition Clear Alarm: This condition is cleared by a starFMDCallRateUnderControl notification

Objects

starVIMServiceVpnName

starVIMServiceInstanceId

starVIMServiceFMDMaxCallRate

starVIMServiceFMDContinuousLoadCount
Object

starFMDCallRateUnderControl

Object ID

enterprise.8164.2.134

Description

FMD call rate is under control.

Action to be Taken: No action required.

Objects

starVIMServiceVpnName

starVIMServiceInstanceId

starVIMServiceFMDMaxCallRate

starVIMServiceFMDContinuousLoadCount
Object

starStorageServerCPUBusy

Object ID

enterprise.8164.2.135

Deseceiption

GTPP Storage Server is experiencing high CPU usage. The usage has exceeded an operator-configure value. Note that this is an external server.

Probable Cause: The amount of information being sent to the storage server is approaching the server's capacity, the storage server has other tasks running on it which are taking CPU time, a problem with the Storage Server is causing the CPU to be abnormally busy.

Condition Clear Alarm: This condition is cleared by a starStorageServerCPUNormal notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshPct

starThreshMeasuredPct

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerCPUNormal

Object ID

enterprise.8164.2.136

Description

GTPP Storage Server CPU usage has returned to a normal range. Note that this is an external server.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshPct

starThreshMeasuredPct

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerDiskSpaceLow

Object ID

enterprise.8164.2.137

Description

GTPP Storage Server is experiencing low available disk space. The available disk space has gone below an operator-configure value. Note that this is an external server.

Description

Probable Cause: This can be caused by an improper configuration, or by the failure or removal of other cards in the system.

Condition Clear Alarm: This condition is cleared by a starStorageServerDiskSpaceOK notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshGB

starThreshMeasuredGB

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerDiskSpaceOK

Object ID

enterprise.8164.2.138

Description

Available disk space for GTPP Storage Server is now in a normal range. Note that this is an external server.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshPct

starThreshMeasuredPct

starGSSClusterName

starGSSClusterNodeName
Object

starCardSPOFAlarm

Object ID

enterprise.8164.2.139

Description

The identified card is a Single Point of Failure (SPOF). There is no redundant card available to take over in the event of a failure.

Probable Cause: This can be caused by an improper configuration, or by the failure or removal of other cards in the system.

Action to be Taken: Install or configure additional redundant cards.

Condition Clear Alarm: A starCardSPOFClear notification will be generated is a redundant card becomes available. Notifications like starCardDown could also obsolete this notification.

Objects

starSlotNum

starCardType
Object

starCardSPOFClear

Object ID

enterprise.8164.2.140

Description

The identified card is no longer a Single Point of Failure (SPOF).

Objects

starSlotNum

starCardType
Object

starStorageServerOldGcdrPending

Object ID

enterprise.8164.2.141

Description

GCDR files on the storage server have been unprocessed since the configured threshold value of time period. Note that this is an external server.

Description

Probable Cause: No action has been taken long for the GCDR files generated by Storage Server.

Condition Clear Alarm: This condition is cleared by a starStorageServerOldGcdrCleared notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshInt

starThreshMeasuredInt

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerOldGcdrCleared

Object ID

enterprise.8164.2.142

Description

GCDR files on the storage server have been processed and he threshold condition is now clear.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshInt

starGSSClusterName

starGSSClusterNodeName
Object

starLoginFailure

Object ID

enterprise.8164.2.143

Description

A login failure occurred attempting to establish a CLI or FTP session.

Objects

starCLITtyname

starCLIType

starCLIRemoteIpAddr

starCLIRemoteIpAddrType
Object :

starIPSGServiceStart

Object ID

enterprise.8164.2.144

Description

A IP Services Gateway (IPSG) service has started.

Objects

starServiceVpnName

starServiceServName
Object

starIPSGServiceStop

Object ID

enterprise.8164.2.145

Description

A IP Services Gateway (IPSG) service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the IPSG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the IPSG service is operational.

Condition Clear Alarm: A starIPSGServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starHAUnreachable

Object ID

enterprise.8164.2.146

Description

A monitored HA is unreachable from the identified FA Service.

Condition Clear Alarm: A starHAReachable notification will be generated when the HA becomes reachable.

Objects

starServiceVPNName

starServiceServName

starServiceFAIpAddr

starServiceHAIpAddr
Object

starHAReachable

Object ID

enterprise.8164.2.147

Description

A monitored HA is now reachable. A starHAReachable notification is only generated for monitored HA's which previously were marked unreachable.

Objects

starServiceVPNName

starServiceServName

starServiceFAIpAddr

starServiceHAIpAddr
Object

starASNGWServiceStart

Object ID

enterprise.8164.2.148

Description

A WiMAX ASN Gateway (ASNGW) service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starASNGWServiceStop

Object ID

enterprise.8164.2.149

Description

A WiMAX ASN Gateway (ASNGW) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the ASNGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Condition Clear Alarm: A starASNGWServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starTaskFailed

Object ID

enterprise.8164.2.150

Description

A non-critical task has failed and the appropriate recovery steps begun. The failing task will be restarted.

Probable Cause: Software error.

Actions to be Taken: Examine the admin logs for an indication of the source of the failure.

Clear Condition: Verify that the task has been restarted.

Condition Clear Alarm: A starTaskRestart notification will be generated when task has successfully restarted.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU
Object

starTaskRestart

Object ID

enterprise.8164.2.151

Description

A non-critical task has restarted after an earlier failure.

Actions to be Taken: None.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU
Object

starCSCFServiceStart

Object ID

enterprise.8164.2.152

Description

A CSCF Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starCSCFServiceStop

Object ID

enterprise.8164.2.153

Description

A CSCF Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the CSCF service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the CSCF service is operational.

Condition Clear Alarm: A starCSCFServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starDhcpServiceStarted

Object ID

enterprise.8164.2.154

Description

A DHCP Service has started.

Action to be Taken: No action required.

Objects

starSessGGSNVpnName

starSessGGSNPeerPort

starSessGGSNPeerAddr
Object

starDhcpServiceStopped

Object ID

enterprise.8164.2.155

Description

A DHCP Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the DHCP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the DHCP service is operational.

Condition Clear Alarm: A starDHCPServiceStart notification will be generated when the service is restarted.

Objects

starSessGGSNVpnName

starSessGGSNPeerPort

starSessGGSNPeerAddr
Object

starContFiltDBError

Object ID

enterprise.8164.2.156

Description

The Content Filtering OPTCMDB file error displayed with an error code.

Action to be Taken: If no OPTCMDB file is found in the specified directory, then place an OPTCMDB-FULL file in the directory and give an upgrade command. If the error is related to a merge/loading failure then give an upgrade command with a new inc/full database file.

Condition Clear Alarm: This condition is cleared by a starContFiltDBErrorClear notification.

Objects

starContFiltCFFilename

starContFiltCFErrorCode
Object

starContFiltDBErrorClear

Object ID

enterprise.8164.2.157

Description

The Content Filtering OPTCMDB file error was removed.

Action to be Taken: No action required.

Objects

starContFiltCFFilename

starContFiltCFErrorCode
Object

starBLDBError

Object ID

enterprise.8164.2.158

Description

The Blacklisting OPTBLDB file error displayed with an error code.

Action to be Taken: If there is no or there is an invalid OPTBLDB file in the specified directory then place a OPTBLDB_FULL file in the directory and give an upgrade command.

Condition Clear Alarm: This condition is cleared by a starBLDBErrorClear notification.

Objects

starBLFilename

starBLErrorCode
Object

starBLDBErrorClear

Object ID

enterprise.8164.2.159

Description

The Blacklisting OPTBLDB file error removed

Objects

starBLFilename

starBLErrorCode
Object

starContFiltDBUpgradeError

Object ID

enterprise.8164.2.160

Description

The Content Filtering OPTCMDB file error displayed with an error code.

Action to be Taken: Place a valid OPTCMDB-FULL file or OPTCMDB_INCR file in the directory and give an upgrade command.

Condition Clear Alarm: This condition is cleared by a starContFiltDBUpgradeErrorClear notification.

Objects

starContFiltCFUpgradeFilename

starContFiltCFUpgradeErrorCode
Object

starContFiltDBUpgradeErrorClear

Object ID

enterprise.8164.2.161

Description

The Content Filtering OPTCMDB file error removed.

Action to be Taken: No action required.

Objects

starContFiltCFUpgradeFilename

starContFiltCFUpgradeErrorCode
Object

starBLDBUpgradeError

Object ID

enterprise.8164.2.162

Description

The Blacklisting OPTBLDB file error displayed with an error code.

Action to be Taken: No action required

Condition Clear Alarm: This condition is cleared by a starBLDBUpgradeErrorClear notification.

Objects

starBLUpgradeFilename

starBLUpgradeErrorCode
Object

starBLDBUpgradeErrorClear

Object ID

enterprise.8164.2.163

Description

The Blacklisting OPTBLDB file error is removed.

Action to be Taken: No action required.

Objects

starBLUpgradeFilename

starBLUpgradeErrorCode
Object

starIPSECDynTunUp

Object ID

enterprise.8164.2.164

Description

IPSEC dynamic tunnel up.

Action to be Taken: No action required.

Objects

starIPSECContextName

starIPSECPolicyName

starIPSECDynPolicyType

starIPSECPolicyPayloadType

starIPSECLocalGateway

starIPSECRemoteGateway
Object

starIPSECDynTunDown

Object ID

enterprise.8164.2.165

Description

IPSEC dynamic tunnel down.

Objects

starIPSECContextName

starIPSECPolicyName

starIPSECDynPolicyType

starIPSECDynPolicyPayloadType

starIPSECLocalGateway

starIPSECRemoteGateway

.
Object

starHeartbeat

Object ID

enterprise.8164.2.166

Description

Periodic SNMP heartbeat. A starHeartbeat notification can be generated periodically if the system is configured to do so. These notifications serve only to validate that there is communication to external entities which sink SNMP notifications
Object

starOverloadSystem

Object ID

enterprise.8164.2.167

Description

A system-wide congestion overload condition has occurred.

Probable Cause: This is the result of an operator-configured congestion overload value reached. This notification indicated a chassis-wide overload condition, typically overall system usage reaching some fraction of capacity. Once this limit is reached, the configured behavior is taken. This will cause certain older and/or dormant calls to be dropped in favor of newer calls. Note that this is similar to, but different from, the starCongestion notification. Typically the 'overload' condition will be configured to trigger at an earlier point.

Actions to be Taken: Verify that the congestion overload thresholds are correct; if the congested state is seen repeatedly, or for sustained periods of time, additional system capacity may need to be brought online.

Clear Condition: This system is cleared when the use of the specific resource falls below the configured limit.

Condition Clear Alarm: A starOverloadSystemClear notification is sent when the system overload condition is clear.

Objects

starCongestionResourceType
Object

starOverloadSystemClear

Object ID

enterprise.8164.2.168

Description

A system-wide congestion overload condition has cleared
Object

starOverloadService

Object ID

enterprise.8164.2.169

Description

A service-specific congestion overload condition has occurred.

Probable Cause: This is the result of an operator-configured congestion overload value reached. This notification indicated a service-specific overload condition, typically the use of the service reaching some fraction of capacity. Once this limit is reached, the configured behavior is taken. This will cause certain older and/or dormant calls to be dropped in favor of newer calls. Note that this is similar to, but different than, the starCongestion notification. Typically the 'overload' condition will be configured to trigger at an earlier point. Since this is a service-specific notification, it is possible to receive multiple notifications for different services.

Action to be Taken: Verify that the congestion overload thresholds are correct; if the congested state is seem repeatedly, or for sustained periods of time, additional system capacity may need to be brought online.

Clear Condition: This system is cleared when the use of the specific resource falls below the configured limit.

Condition Clear Alarm: A starOverloadServiceClear notification is sent when the service-specific overload condition is clear.

Objects

starCongestionResourceType

starServiceVpnName

starServiceServName
Object

starOverloadServiceClear

Object ID

enterprise.8164.2.170

Description

A service-specific congestion overload condition has cleared

Objects

starServiceVpnName

starServiceServName
Object

starStorageServerClusterStateChange

Object ID

enterprise.8164.2.171

Description

GTPP Storage Server cluster state has been changed. GTPP Storage Server may have gone offline from all the nodes or switchover has been occurred. Note that this is an external server.

Probable Cause: GTPP Storage Server cluster hardware/software component failure, or maintenance of GTPP Storage Server is in progress.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSClusterName

starGSSClusterRgName

starGSSClusterRsName

starGSSClusterNodeState

starGSSClusterPrevOnlineNode
Object

starStorageServerCluswitchOver

Object ID

enterprise.8164.2.172

Description

GTPP Storage Server switchover from current online node to next available node in cluster. Note that this is an external server.

Probable Cause: GTPP storage server cluster hardware/software component failure or maintenance of GTPP storage server is in progress.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSClusterName

starGSSClusterRgName

starGSSClusterFromNode

starGSSClusterToNode
Object

starStorageServerClusPathFail

Object ID

enterprise.8164.2.173

Description

GTPP Storage Server cluster disk path failure has been occurred. Note that this is an external server.

Probable Cause: Fiber-optic cable may have been damaged or pulled out or disk fault may have been occurred.

Condition Clear Alarm: This condition is cleared by a starStorageServerClusPathOK notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSDiskPath

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerClusPathOK

Object ID

enterprise.8164.2.174

Description

GTPP Storage Server cluster disk path failure has been restored. Note that this is an external server.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSDiskPath

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerClusInterCFail

Object ID

enterprise.8164.2.175

Description

GTPP Storage Server cluster transport path (Interconnect) failure observed. Note that this is an external server.

Probable Cause: Interconnect interface may have been failed, or interconnect interface cable may have been pulled out.

Condition Clear Alarm: This condition is cleared by a starStorageServerClusInterCOK notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSTransportPath

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerClusInterCOK

Object ID

enterprise.8164.2.176

Description

GTPP Storage Server cluster transport path (Interconnect) failure has been restored to an operational state. Note that this is an external server.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSTransportPath

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerClusIntfFail

Object ID

enterprise.8164.2.177

Description

GTPP Storage Server cluster disk path failure has occurred. Note that this is an external server.

Probable Cause: Interface may have been failed, interface cable may have been pulled out.

Condition Clear Alarm: This condition is cleared by a starStorageServerClusIntfOK notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSIPMPGroupName

starGSSInterfaceName

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerClusIntfOK

Object ID

enterprise.8164.2.178

Description

GTPP Storage Server cluster GE Interface has been restored.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSIPMPGroupName

starGSSInterfaceName

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerMemLow

Object ID

enterprise.8164.2.179

Description

GTPP Storage Server is experiencing a low memory condition.

Description

Probable Cause: The amount of free memory used by storage server is approaching the server's capacity.

Condition Clear Alarm: This condition is cleared by a starStorageServerMemNormal notification.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshMB

starThreshMeasuredMB

starGSSClusterName

starGSSClusterNodeName
Object

starStorageServerMemNormal

Object ID

enterprise.8164.2.180

Description

GTPP Storage Server Memory usage has returned to a normal range. Note that this is an external server.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starThreshMB

starThreshMeasuredMB

starGSSClusterName

starGSSClusterNodeName
Object

starPDIFServiceStart

Object ID

enterprise.8164.2.181

Description

A PDIF Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starPDIFServiceStop

Object ID

enterprise.8164.2.182

Description

A PDIF Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (packet processing cards) to support the running configuration.

Action to be Taken: If the shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running on the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PDIF Service is operational.

Condition Clear Alarm: A starPDIFServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starSessMgrRecoveryComplete

Object ID

enterprise.8164.2.183

Description

A Sess Mgr Recovery Complete.

Probable Cause: This is typically caused by session manager task fails and successfully completed recovery.

Action to be Taken: No action required.

Objects

starCPUSlot

starCPUNumber
Object

starDiameterPeerDown

Object ID

enterprise.8164.2.184

Description

A Diameter peer is down.

Problem Cause: The Diameter peer has failed, or a network connectivity problem prevents reaching the peer.

Condition Clear Alarm: A starDiameterPeerUp notification will be generated when the peer is up.

Objects

starDiameterVpnName

starDiameterPeerAddr

starDiameterEndpointName
Object

starDiameterPeerUp

Object ID

enterprise.8164.2.185

Description

A Diameter peer is up. This notification is only generated for peers which have previously been declared down.

Objects

starDiameterVpnName

starDiameterPeerAddr

starDiameterEndpointName
Object

starDiameterServerUnreachable

Object ID

enterprise.8164.2.186

Description

A Diameter server is down.

Problem Cause: The Diameter server has failed, or a network connectivity issue prevents reaching the server.

Condition Clear Alarm: A starDiameterServerReachable notification will be generated when the server is reachable.

Objects

starServiceVpnName

starDiameterPeerAddr

starDiameterEndpointName
Object

starDiameterServerReachable

Object ID

enterprise.8164.2.187

Description

A Diameter server is up. This notification is only generated for servers which have previously been declared unreachable.

Objects

starServiceVpnName

starDiameterPeerAddr

starDiameterEndpointName
Object

starCDRFileRemoved

Object ID

enterprise.8164.2.188

Description

A Charging Data Record (CDR) file has been deleted from the system due to a lack of available storage space. When required, the system deletes old files to make space for new files. This notification is only generated when specifically enabled on the system.

Probable Cause: CDR files are not being moved off the system, or these files are not being deleted after they have been transferred.

Objects

starCDRFilename
Object

starCSCFPeerServerReachable

Object ID

enterprise.8164.2.189

Description

A peer server is reachable

Objects

starServiceVPNName

starServiceServName

starServicePeerServerName
Object

starCSCFPeerServerUnreachable

Object ID

enterprise.8164.2.190

Description

A peer server is reachable

Objects

starServiceVPNName

starServiceServName

starServicePeerServerName
Object

starCLIConfigMode

Object ID

enterprise.8164.2.192

Description

An interactive CLI session has an “enter configuration” mode for the specified context. Thus the CLI user can potentially start entering configuration commands that could impact the entire system. Note that this notification is not enabled by default; it is only generated if the system is specifically configured to enable it.

Objects

starCLIUsername

starCLIContext
Object

starSGSNServiceStart

Object ID

enterprise.8164.2.194

Description

A SGSN Service has started.

Objects

starServiceVpnName

starServiceServName
Object

starSGSNServiceStop

Object ID

enterprise.8164.2.195

Description

A SGSN Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the SGSN service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the SGSN service is operational.

Condition Clear Alarm: A starSGSNServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName,

starServiceServName
Object

starM3UAPCUnavailable

Object ID

enterprise.8164.2.196

Description

M3UA route to the point code becomes unavailable.

Probable Cause: Received destination unavailable (DUNA) message, or SCTP association is down, or remote peer server is down.

Action to be taken: Verify that the peer server is up.

Condition Clear Alarm: A starM3UAPCAvailable notification will be generated when the remote peer identified by the point code becomes reachable.

Objects

starSS7rdId

starSS7Pc

starSS7M3UAPsId

starSS7CauseString
Object

starM3UAPCAvailable

Object ID

enterprise.8164.2.197

Description

M3UA route to the point code becomes available.

Probable Cause: Received a destination available (DAVA) message. SCTP Association is up. Remote peer server is up.

A starM3UAPCAvailable message is generated only after a starM3UAPCUnavailable message was generated.

Objects

starSS7M3UAPsId

starSS7Pc

starSS7rdId

starSS7CauseString
Object

starThreshCPUUtilization

Object ID

enterprise.8164.2.200

Description

The overall CPU utilization for the identified processor has exceeded its configured threshold value for the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCPUUtilization notification will be generated when the measured value falls below the threshold.

Objects

starCPUSlot

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshClearCPUUtilization

Object ID

enterprise.8164.2.201

Description

The threshold condition is now clear.

Objects

starCPUSlot

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshCPUMemory

Object ID

enterprise.8164.2.202

Description

The amount of available memory for the identified processor has fallen below the configured threshold value.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCPUMemory notification will be generated when the measured value falls below the threshold.

Objects

starCPUSlot

starCPUNumber

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCPUMemory

Object ID

enterprise.8164.2.203

Description

The threshold condition is now clear.

Objects

starCPUSlot

starCPUNumber

starThreshInt

starThreshMeasuredInt
Object

starThreshLicense

Object ID

enterprise.8164.2.204

Description

The percentage available, licensed subscribers has fallen below the configured threshold value.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearLicense notification will be generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct

starServiceType
Object

starThreshClearLicense

Object ID

enterprise.8164.2.205

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt

starServiceType
Object

starThreshSubscriberTotal

Object ID

enterprise.8164.2.206

Description

The total number of subscribers is above the configured threshold value.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearSubscriberTotal notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearSubscriberTotal

Object ID

enterprise.8164.2.207

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshSubscriberActive

Object ID

enterprise.8164.2.208

Description

The total number of active subscribers is above the configured threshold value.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearSubscriberActive notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearSubscriberActive

Object ID

enterprise.8164.2.209

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPortRxUtil

Object ID

enterprise.8164.2.210

Description

The Rx utilization of the port has exceeded the configured threshold value during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortRxUtil notification will be generated when the measured value falls below the threshold.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshClearPortRxUtil

Object ID

enterprise.8164.2.211

Description

The threshold condition is now clear.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshPortTxUtil

Object ID

enterprise.8164.2.212

Description

The Tx utilization of the port has exceeded the configured threshold value during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortTxUtil notification will be generated when the measured value falls below the threshold.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshClearPortTxUtil

Object ID

enterprise.8164.2.213

Description

The threshold condition is now clear.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshPortHighActivity

Object ID

enterprise.8164.2.214

Description

The number of seconds of 'high activity' time on the port has exceeded the configured threshold value during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortHighActivity notification is generated when the measured value falls below the threshold.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshClearPortHighActivity

Object ID

enterprise.8164.2.215

Description

The threshold condition is now clear.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshAAAAuthFail

Object ID

enterprise.8164.2.216

Description

The number of AAA authentication failures has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAuthFail notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearAAAAuthFail

Object ID

enterprise.8164.2.217

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshAAAAuthFailRate

Object ID

enterprise.8164.2.218

Description

The percentage of AAA authentication requests which failed has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAuthFailRate notification will be generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearAAAAuthFailRate

Object ID

enterprise.8164.2.219

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshAAAAcctFail

Object ID

enterprise.8164.2.220

Description

The number of AAA accounting failures has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user -configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAcctFail notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearAAAAcctFail

Object ID

enterprise.8164.2.221

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshAAAAcctFailRate

Object ID

enterprise.8164.2.222

Description

The percentage of AAA accounting requests which failed has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAcctFailRate notification will be generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearAAAAcctFailRate

Object ID

enterprise.8164.2.223

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshAAARetryRate

Object ID

enterprise.8164.2.224

Description

The percentage of AAA requests which has to be retried has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAARetryRate notification will be generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearAAARetryRate

Object ID

enterprise.8164.2.225

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshCallSetup

Object ID

enterprise.8164.2.226

Description

The number of call setup operations has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCallSetup notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCallSetup

Object ID

enterprise.8164.2.227

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshCallSetupFailure

Object ID

enterprise.8164.2.228

Description

The number of call setup operations which failed has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCallSetupFailure notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCallSetupFailure

Object ID

enterprise.8164.2.229

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshCallRejectNoResource

Object ID

enterprise.8164.2.230

Description

The number of call setup operations which were rejected due to a no resource condition has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCallRejectNoResource notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCallRejectNoResource

Object ID

enterprise.8164.2.231

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPacketsFilteredDropped

Object ID

enterprise.8164.2.232

Description

The number of user data packets filtered has exceeded the configured threshold for the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in an alarm mode, a starThreshClearPacketsFilteredDropped notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPacketsFilteredDropped

Object ID

enterprise.8164.2.233

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPacketsForwarded

Object ID

enterprise.8164.2.234

Description

The number of user data packets forwarded has exceeded the configured threshold for the current monitoring period.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPacketsForwarded notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPacketsForwarded

Object ID

enterprise.8164.2.235

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshSessCPUThroughput

Object ID

enterprise.8164.2.236

Description

The total session throughout for the specified processor has exceeded the configured threshold for the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearSessCPUThroughput notification will be generated when the measured value falls below the threshold.

Objects

starCPUSlot

starCPUNumber

starThreshMB

starThreshMeasuredMB
Object

starThreshClearSessCPUThroughput

Object ID

enterprise.8164.2.237

Description

The threshold condition is now clear.

Objects

starCPUSlot

starCPUNumber

starThreshMB

starThreshMeasuredMB
Object

starThreshIPPoolAvail

Object ID

enterprise.8164.2.238

Description

The available IP pool addresses in a context has fallen below the configured threshold.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPPoolAvail notification will be generated when the measured value falls below the threshold.

Objects

starIPPoolContext

starIPPoolGroup

starThreshPct

starThreshMeasuredPct
Object

starThreshClearIPPoolAvail

Object ID

enterprise.8164.2.239

Description

The threshold condition is now clear.

Objects

starIPPoolContext

starIPPoolGroup

starThreshPct

starThreshMeasuredPct
Object

starThreshCPUUtilization10Sec

Object ID

enterprise.8164.2.240

Description

The CPU utilization of 10 second measurement for the identified processor has exceeded for configured threshold value for the current monitoring period.

Objects

starCPUSlot

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshClearCPUUtilization10Sec

Object ID

enterprise.8164.2.241

Description

The threshold condition is now clear.

Objects

starCPUSlot

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshCPULoad

Object ID

enterprise.8164.2.242

Description

The CPU load for the identified processor has exceeded for configured threshold value for the current monitoring period.

Objects

starCPUSlot

starCPUNumber

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCPULoad

Object ID

enterprise.8164.2.243

Description

The threshold condition is now clear.

Objects

starCPUSlot

starCPUNumber

starThreshInt

starThreshMeasuredInt
Object

starThreshCPUMemUsage

Object ID

enterprise.8164.2.244

Description

The CPU mem usage for the identified processor has exceeded for configured threshold value for the current monitoring period.

Objects

starCPUSlot

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshClearCPUMemUsage

Object ID

enterprise.8164.2.245

Description

The threshold condition is now clear.

Objects

starCPUSlot

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshPDSNSessions

Object ID

enterprise.8164.2.246

Description

The total number of PDSN sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDSNSessions

Object ID

enterprise.8164.2.247

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshGGSNSessions

Object ID

enterprise.8164.2.248

Description

The total number of GGSN sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearGGSNSessions

Object ID

enterprise.8164.2.249

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshHASessions

Object ID

enterprise.8164.2.250

Description

The total number of HA sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHASessions

Object ID

enterprise.8164.2.251

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshLNSSessions

Object ID

enterprise.8164.2.252

Description

The total number of L2TP LNS sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearLNSSessions

Object ID

enterprise.8164.2.253

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServicePDSNSessions

Object ID

enterprise.8164.2.254

Description

The total number of PDSN sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServicePDSNSessions

Object ID

enterprise.8164.2.255

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceGGSNSessions

Object ID

enterprise.8164.2.256

Description

The total number of GGSN sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceGGSNSessions

Object ID

enterprise.8164.2.257

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceHASessions

Object ID

enterprise.8164.2.258

Description

The total number of HA sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceHASessions

Object ID

enterprise.8164.2.259

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceLNSSessions

Object ID

enterprise.8164.2.260

Description

The total number of L2TP LNS sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceLNSSessions

Object ID

enterprise.8164.2.261

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshIPPoolHold

Object ID

enterprise.8164.2.262

Description

The percentage IP pool addresses in HOLD state in a context has gone above the configured threshold.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearIPPoolHold

Object ID

enterprise.8164.2.263

Description

The threshold condition is now clear.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshIPPoolUsed

Object ID

enterprise.8164.2.264

Description

The percentage IP pool addresses in USED state in a context has gone above the configured threshold.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearIPPoolUsed

Object ID

enterprise.8164.2.265

Description

The threshold condition is now clear.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshIPPoolRelease

Object ID

enterprise.8164.2.266

Description

The percentage IP pool addresses in RELEASE state in a context has gone above the configured threshold.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct

starThreshMeasuredInt
Object

starThreshClearIPPoolRelease

Object ID

enterprise.8164.2.267

Description

The threshold condition is now clear.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshIPPoolFree

Object ID

enterprise.8164.2.268

Description

The percentage IP pool addresses in HOLD state in a context has gone below the configured threshold.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearIPPoolFree

Object ID

enterprise.8164.2.269

Description

The threshold condition is now clear.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshAAAAcctArchive

Object ID

enterprise.8164.2.270

Description

The AAA accounting archive size has gone above the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearAAAAcctArchive

Object ID

enterprise.8164.2.271

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPortSpecRxUtil

IMPORTANT:

This alarm is obsolete.

Object ID

enterprise.8164.2.272

Description

The Rx utilization of the port has exceeded the configured threshold value during the current monitoring period.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortSpecRxUtil notification will be generated when the measured value falls below the threshold.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshClearPortSpecRxUtil

IMPORTANT:

This alarm is obsolete.

Object ID

enterprise.8164.2.273

Description

The threshold condition is now clear.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshPortSpecTxUtil

IMPORTANT:

This alarm is obsolete.

Object ID

enterprise.8164.2.274

Description

The Tx utilization of the port has exceeded the configured threshold value during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPortSpecTxUtil notification will be generated when the measured value falls below the threshold.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshClearPortSpecTxUtil

IMPORTANT:

This trap is obsolete.

Object ID

enterprise.8164.2.275

Description

The threshold condition is now clear.

Objects

starPortSlot

starPortNum

starThreshPct

starThreshMeasuredPct
Object

starThreshHACallSetupRate

Object ID

enterprise.8164.2.276

Description

The per-context HA call setup rate (calls per second) has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in 'alarm' mode, a starThreshClearHACallSetupRate notification will be generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHACallSetupRate

Object ID

enterprise.8164.2.277

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starThreshInt

starThreshMeasuredInt
Object

starThreshHASvcCallSetupRate

Object ID

enterprise.8164.2.278

Description

The per-service HA Call setup rate (calls per second) has gone above the configured threshold.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcCallSetupRate notification will be generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHASvcCallSetupRate

Object ID

enterprise.8164.2.279

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshHASvcRegReplyError

Object ID

enterprise.8164.2.280

Description

The per-service HA Reg Reply Error count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcRegReplyError notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHASvcRegReplyError

Object ID

enterprise.8164.2.281

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshHASvcReregReplyError

Object ID

enterprise.8164.2.282

Description

The per-service HA Rereg Reply Error count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcReregReplyError notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHASvcReregReplyError

Object ID

enterprise.8164.2.283

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshHASvcDeregReplyError

Object ID

enterprise.8164.2.284

Description

The per-service HA Dereg Reply Error count has gone above the configured threshold

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearHASvcDeregReplyError notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHASvcDeregReplyError

Object ID

enterprise.8164.2.285

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshFASvcRegReplyError

Object ID

enterprise.8164.2.286

Description

The Per-Service FA Reg Reply Error count has gone above the configured threshold

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearFASvcRegReplyError notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearFASvcRegReplyError

Object ID

enterprise.8164.2.287

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPDSNCallSetupRate

Object ID

enterprise.8164.2.288

Description

The Per-Context PDSN Call Setup Rate (calls per second) has gone above the configured threshold

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNCallSetupRate notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDSNCallSetupRate

Object ID

enterprise.8164.2.289

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starThreshInt

starThreshMeasuredInt
Object

starThreshPDSNSvcCallSetupRate

Object ID

enterprise.8164.2.290

Description

The Per-Service PDSN Call Setup Rate (calls per second) has gone above the configured threshold

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNSvcCallSetupRate notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDSNSvcCallSetupRate

Object ID

enterprise.8164.2.291

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPDSNSvcA11RRPFailure

Object ID

enterprise.8164.2.292

Description

The Per-Service PDSN A11 RRP Failure count has gone above the configured threshold

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNSvcA11RRPFailure notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDSNSvcA11RRPFailure

Object ID

enterprise.8164.2.293

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPDSNSvcA11RRQMsgDiscard

Object ID

enterprise.8164.2.294

Description

The Per-Service PDSN A11 RRQ Msg Discard count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode a starThreshClearPDSNSvcA11RRQMsgDiscard notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDSNSvcA11RRQMsgDiscard

Object ID

enterprise.8164.2.295

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPDSNSvcA11RACMsgDiscard

Object ID

enterprise.8164.2.296

Description

The Per-Service PDSN A11 RAC Msg Discard count has gone above the configured threshold

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode a starThreshClearPDSNSvcA11RACMsgDiscard notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDSNSvcA11RACMsgDiscard

Object ID

enterprise.8164.2.297

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPDSNSvcA11PPPSendDiscard

Object ID

enterprise.8164.2.298

Description

The Per-Service PDSN A11 PPP Send Discard count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDSNSvcA11PPPSendDiscard notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDSNSvcA11PPPSendDiscard

Object ID

enterprise.8164.2.299

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshAAAMgrQueue

Object ID

enterprise.8164.2.300

Description

The Per-AAA Manager internal request queue usage has gone above the configured threshold

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAMgrQueue is generated when the measured value falls below the threshold.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starThreshClearAAAMgrQueue

Object ID

enterprise.8164.2.301

Description

The threshold condition is now clear.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starThreshCPUOrbsWarn

Object ID

enterprise.8164.2.302

Description

The ORBs task has exceeding the CPU usage configured as a warning.

Objects

starCPUSlot,

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshClearCPUOrbsWarn

Object ID

enterprise.8164.2.303

Description

The threshold condition is now clear.

Objects

starCPUSlot,

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshCPUOrbsCritical

Object ID

enterprise.8164.2.304

Description

The ORBs task has exceeded the CPU usage configured as a critical error

Objects

starCPUSlot,

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshClearCPUOrbsCritical

Object ID

enterprise.8164.2.305

Description

The threshold condition is now clear

Objects

starCPUSlot,

starCPUNumber

starThreshPct

starThreshMeasuredPct
Object

starThreshRPSetupFailRate

Object ID

enterprise.8164.2.306

Description

The RP call setup failure rate has exceeded the configured threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearRPSetupFailRate

Object ID

enterprise.8164.2.307

Description

The threshold condition is now clear

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshPPPSetupFailRate

Object ID

enterprise.8164.2.308

Description

The PPP call setup failure rate has exceeded the configured threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearPPPSetupFailRate

Object ID

enterprise.8164.2.309

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshStorageUtilization

Object ID

enterprise.8164.2.310

Description

The utilization of a mass storage device has exceeded the configured threshold.

Objects

starStorageSlot

starStorageName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearStorageUtilization

Object ID

enterprise.8164.2.311

Description

The threshold condition is now clear.

Objects

starStorageSlot

starStorageName

starThreshPct

starThreshMeasuredPct
Object

starThreshDCCAProtocolErrors

Object ID

enterprise.8164.2.312

Description

The number of DCCA protocol errors has exceeded the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearDCCAProtocolErrors

Object ID

enterprise.8164.2.313

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshDCCABadAnswers

Object ID

enterprise.8164.2.314

Description

The number of DCCA BadAnswers has exceeded the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearDCCABadAnswers

Object ID

enterprise.8164.2.315

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshDCCAUnknownRatingGroup

Object ID

enterprise.8164.2.316

Description

The number of DCCA UnknownRatingGroup has exceeded the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearDCCAUnknownRatingGroup

Object ID

enterprise.8164.2.317

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshDCCARatingFailed

Object ID

enterprise.8164.2.318

Description

The number of DCCA RatingFailed has exceeded the configured threshold

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearDCCARatingFailed

Object ID

enterprise.8164.2.319

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshIPSECIKERequests

Object ID

enterprise.8164.2.320

Description

The number of IPSEC IKE requests seen for this HA service has exceeded the configured threshold.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in an alarm mode, a starThreshClearIPSECIKERequests notification will be generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearIPSECIKERequests

Object ID

enterprise.8164.2.321

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshIPSECIKEFailures

Object ID

enterprise.8164.2.322

Description

The number of IPSEC IKE failures seen for this HA service has exceeded the configured threshold.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECIKEFailures notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearIPSECIKEFailures

Object ID

enterprise.8164.2.323

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshIPSECIKEFailRate

Object ID

enterprise.8164.2.324

Description

The rate of IPSEC IKE failures (as a percentage of total requests) seen for this HA service has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECIKEFailRate notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearIPSECIKEFailRate

Object ID

enterprise.8164.2.325

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshPct

starThreshMeasuredPct
Object

starThreshIPSECTunSetup

Object ID

enterprise.8164.2.326

Description

The number of IPSEC tunnels setup over the last measurement period for this HA service has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECTunSetup notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearIPSECTunSetup

Object ID

enterprise.8164.2.327

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshIPSECTunEstabl

Object ID

enterprise.8164.2.328

Description

The current number of IPSEC tunnels established for this HA service has exceeded the configured threshold.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECTunEstabl notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearIPSECTunEstabl

Object ID

enterprise.8164.2.329

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshIPSECCallReqRej

Object ID

enterprise.8164.2.330

Description

The number of IPSEC Rejected Call Requests has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold. Reject Call Requests indicate that an IPSEC Manager has reached its maximum allowable number of IPSEC tunnels.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearIPSECTunnelsTotal notification is generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearIPSECCallReqRej

Object ID

enterprise.8164.2.331

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcRouteFailure

Object ID

enterprise.8164.2.332

Description

The Per-Service CSCF Route failure count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCSCFSvcRouteFailure notification will be generated when the measured value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcRouteFailure

Object ID

enterprise.8164.2.333

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshContFiltRating

Object ID

enterprise.8164.2.334

Description

The number of Content Filtering Rating operations performed has gone above the configured threshold value.

Probable Cause: This is a user configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearContFiltRating notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearContFiltRating

Object ID

enterprise.8164.2.335

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshContFiltBlock

Object ID

enterprise.8164.2.336

Description

The number of Content Filtering Block operations performed has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearContFiltBlock notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearContFiltBlock

Object ID

enterprise.8164.2.337

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshCDRFileSpace

Object ID

enterprise.8164.2.338

Description

The CDR file space usage is above the configured threshold percentage.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in an alarm mode, a starThreshClearCDRFileSpaceOverLimit notification is generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearCDRFileSpace

Object ID

enterprise.8164.2.339

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshEDRFileSpace

Object ID

enterprise.8164.2.340

Description

The EDR file space usage is above the configured threshold percentage.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearEDRFileSpaceOverLimit notification generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearEDRFileSpace

Object ID

enterprise.8164.2.341

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshPDIFCurrSess

Object ID

enterprise.8164.2.342

Description

The chassis-wide count of current PDIF sessions has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDIFCurrSess notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDIFCurrSess

Object ID

enterprise.8164.2.343

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPDIFCurrActSess

Object ID

enterprise.8164.2.344

Description

The chassis-wide count of current PDIF active sessions has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearPDIFCurrActSess notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDIFCurrActSess

Object ID

enterprise.8164.2.345

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshCDRFlowControl

Object ID

enterprise.8164.2.346

Description

The number of Charging Data Record (CDR) records which have been discarded at an ACSMGR due to flow control has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold. This threshold potentially indicates an overload condition due which prevents processing CDR messages at the same rate as the incoming packets.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearCDRFlowControl notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCDRFlowControl

Object ID

enterprise.8164.2.347

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWSessTimeout

Object ID

enterprise.8164.2.348

Description

ASNGW session timeout has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearASNGWSessTimeout notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWSessTimeout

Object ID

enterprise.8164.2.349

Description

Threshold condition is now clear

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWSessSetupTimeout

Object ID

enterprise.8164.2.350

Description

ASNGW session setup timeout has exceeded the configured threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGWSessSetupTimeout notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWSessSetupTimeout

Object ID

enterprise.8164.2.351

Description

Threshold condition is now clear

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWAuthFail

Object ID

enterprise.8164.2.352

Description

Number of ASNGW authentication failures has exceeded the configured threshold in the current monitoring period.

Probable Cause: This is a-user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearASNGWAuthFail notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWAuthFail

Object ID

enterprise.8164.2.353

Description

Threshold conditrion is now clear

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWR6InvNai

IMPORTANT:

This object is obsolete.

Object ID

enterprise.8164.2.354

Description

Number of ASNGW Invalid NAI has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGWR6InvNai notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWR6InvNai

IMPORTANT:

This object is obsolete.

Object ID

enterprise.8164.2.355

Description

Threshold condition is now clear

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWMaxEAPRetry

Object ID

enterprise.8164.2.356

Description

Number of ASNGW EAP retries has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearASNGWMaxEAPRetry notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWMaxEAPRetry

Object ID

enterprise.8164.2.357

Description

Threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWNWEntryDenial

Object ID

enterprise.8164.2.358

Description

Number of ASNGW network entry denials has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGWNWEntryDenial notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWNWEntryDenial

Object ID

enterprise.8164.2.359

Description

Threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWHandoffDenial

Object ID

enterprise.8164.2.360

Description

Number of ASNGW handoff denials has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshASNGWHandoffDenial notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWHandoffDenial

Object ID

enterprise.8164.2.361

Description

Threshold condition is now clear

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshSGSNSessions

Object ID

enterprise.8164.2.362

Description

The total number of SGSN sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearSGSNSessions notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearSGSNSessions

Object ID

enterprise.8164.2.363

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceSGSNSessions

Object ID

enterprise.8164.2.364

Description

The total number of SGSN sessions in a service is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearPerServiceSGSNSessions notification is generated when the value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceSGSNSessions

Object ID

enterprise.8164.2.365

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshSGSNPdpSessions

Object ID

enterprise.8164.2.366

Description

The total number of SGSN PDP sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearSGSNPdpSessions notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearSGSNPdpSessions

Object ID

enterprise.8164.2.367

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceSGSNPdpSessions

Object ID

enterprise.8164.2.368

Description

The total number of SGSN PDP sessions in a service is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearPerServiceSGSNPdpSessions notification is generated when the value falls below the threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceSGSNPdpSessions

Object ID

enterprise.8164.2.369

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshFWDosAttack

Object ID

enterprise.8164.2.370

Description

The cumulative number of FW Denial of Service attacks has exceeded the configured threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDoSAttack notification is generated when the value falls below the threshold.

Description

starThreshInt

starThreshMeasuredInt
Object

starThreshClearFWDosAttack

Object ID

enterprise.8164.2.371

Description

Threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshFWDropPacket

Object ID

enterprise.8164.2.372

Description

The cumulative number of FW dropped packets has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDropPacket notification is generated when the value falls below the threshold.

Description

starThreshInt

starThreshMeasuredInt
Object

starThreshClearFWDropPacket

Object ID

enterprise.8164.2.373

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshFWDenyRule

Object ID

enterprise.8164.2.374

Description

The cumulative number of FW Deny-Rules has exceeded the threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDenyRule notification is generated when the value falls below the threshold.

Description

starThreshInt

starThreshMeasuredInt
Object

starThreshClearFWDenyRule

Object ID

enterprise.8164.2.375

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshFWNoRule

Object ID

enterprise.8164.2.376

Description

The cumulative number of FW No Rules has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If thresholding is configured to run in alarm mode, a starThreshClearFWDenyRule notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearFWNoRule

Object ID

enterprise.8164.2.377

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWSessTimeout

Object ID

enterprise.8164.2.378

Description

The PHSGW session timeout has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWSessTimeout

Object ID

enterprise.8164.2.379

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWSessSetupTimeout

Object ID

enterprise.8164.2.380

Description

The PHSGW session setup timeout has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWSessSetupTimeout

Object ID

enterprise.8164.2.381

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWAuthFail

Object ID

enterprise.8164.2.382

Description

The number of PHSGW authentication failures has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWAuthFail

Object ID

enterprise.8164.2.383

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWMaxEAPRetry

Object ID

enterprise.8164.2.384

Description

The number of PHSGW Maximum EAP Retry has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWMaxEAPRetry

Object ID

enterprise.8164.2.385

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWNWEntryDenial

Object ID

enterprise.8164.2.386

Description

The number of PHSGW Network Entry Denial has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWNWEntryDenial

Object ID

enterprise.8164.2.387

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWHandoffDenial

Object ID

enterprise.8164.2.388

Description

The number of PHSGW Handoff Denial has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWHandoffDenial

Object ID

enterprise.8164.2.389

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshASNGWSessions

Object ID

enterprise.8164.2.390

Description

The total number of ASNGW sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: A starThreshClearASNGWSessions notification is generated when the value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearASNGWSessions

Object ID

enterprise.8164.2.391

Description

Threshold condition is now clear

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceASNGWSessions

Object ID

enterprise.8164.2.392

Description

The total number of PDSN sessions in a service is above the configured threshold value.

Possible Cause: This is a user-configurable threshold.

Condition Clear Alarm: A starThreshClearPerServiceASNGWSessions notification is generated when the value falls below the threshold.

Objects

starServiceVPNName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceASNGWSessions

Object ID

enterprise.8164.2.393

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSPCSessSetupTimeout

Object ID

enterprise.8164.2.394

Description

The PHSPC session setup timeout has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSPCSessSetupTimeout

Object ID

enterprise.8164.2.395

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSPCSleepModeTimeout

Object ID

enterprise.8164.2.396

Description

The PHSPC idle mode timeout has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSPCSleepModeTimeout

Object ID

enterprise.8164.2.397

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSPCSmEntryDenial

Object ID

enterprise.8164.2.398

Description

The number of PHSPC sm entry denial has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSPCSmEntryDenial

Object ID

enterprise.8164.2.399

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshSGWSessions

Object ID

enterprise.8164.2.408

Description

The total number of SGW sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearSGWSessions

Object ID

enterprise.8164.2.409

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPGWSessions

Object ID

enterprise.8164.2.410

Description

The total number of PGW sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPGWSessions

Object ID

enterprise.8164.2.411

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshLMASessions

Object ID

enterprise.8164.2.412

Description

The total number of LMA sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearLMASessions

Object ID

enterprise.8164.2.413

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshMAGSessions

Object ID

enterprise.8164.2.414

Description

The total number of MAG sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearMAGSessions

Object ID

enterprise.8164.2.415

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshFNGCurrSess

Object ID

enterprise.8164.2.416

Description

The chassis-wide count of current FNG sessions has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm model, a starThreshClearFNGCurrSess notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearFNGCurrSess

Object ID

enterprise.8164.2.417

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshFNGCurrActSess

Object ID

enterprise.8164.2.418

Description

The chassis-wide count of current FNG active sessions has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearFNGCurrActiveSess notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearFNGCurrActSess

Object ID

enterprise.8164.2.419

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWEAPOLAuthFailure

Object ID

enterprise.8164.2.420

Description

The number of PHSGW EAPOL auth failures has exceeded the configured threshold value. If the thresholding subsystem is configured to run in alarm mode, a starThreshPHSGWEAPOLAuthFailure notification will be generated when the measured value falls below the threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWEAPOLAuthFailure

Object ID

enterprise.8164.2.421

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPHSGWMaxEAPOLRetry

Object ID

enterprise.8164.2.422

Description

The number of PHSGW max EAPOL retry has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPHSGWMaxEAPOLRetry

Object ID

enterprise.8164.2.423

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshHSGWSessions

Object ID

enterprise.8164.2.424

Description

The total number of HSGW sessions is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshNAPTPortChunks

Object ID

enterprise.8164.2.425

Description

The NAT port chunks utilization of NAT pool is above the configured threshold value.

Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearNAPTPortChunks notification will be generated when the measured value exceeds the threshold.

Objects

starIPPoolContext

starIPPoolName

starThreshInt

starThreshMeasuredInt
Object

starThreshPDGCurrSess

Object ID

enterprise.8164.2.426

Description

The chassis-wide count of current PDG sessions has gone above the configured threshold value.

Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDGCurrSess notification will be generated when the measured value falls below the threshold.

Object ID

enterprise.8164.2.427

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPDGCurrActSess

Object ID

enterprise.8164.2.428

Description

The chassis-wide count of current PDG active sessions has gone above the configured threshold value.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearPDGCurrActiveSess notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPDGCurrActSess

Object ID

enterprise.8164.2.429

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshNATPortChunks

Object ID

enterprise.8164.2.430

Description

The NAT port chunks utilization of NAT pool is above the configured threshold value.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearNAPTPortChunks notification will be generated when the measured value exceeds the threshold.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearNATPortChunks

Object ID

enterprise.8164.2.431

Description

The threshold condition is now clear.

Objects

starIPPoolContext

starIPPoolName

starThreshPct

starThreshMeasuredPct
Object

starThreshGPRSSessions

Object ID

enterprise.8164.2.432

Description

The total number of GPRS sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearGPRSSessions

Object ID

enterprise.8164.2.433

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceGPRSSessions

Object ID

enterprise.8164.2.434

Description

The total number of GPRS sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceGPRSSessions

Object ID

enterprise.8164.2.435

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshGPRSPdpSessions

Object ID

enterprise.8164.2.436

Description

The total number of GPRS PDP sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearGPRSPdpSessions

Object ID

enterprise.8164.2.437

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServiceGPRSPdpSessions

Object ID

enterprise.8164.2.438

Description

The total number of GPRS PDP sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServiceGPRSPdpSessions

Object ID

enterprise.8164.2.439

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcRegRcvdRate

Object ID

enterprise.8164.2.446

Description

The Per-Service CSCF Registration Per Interval count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcRegRcvdRate

Object ID

enterprise.8164.2.447

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcTotalActiveReg

Object ID

enterprise.8164.2.448

Description

The per-service CSCF Total Active Registrations count has gone above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcTotalActiveReg

Object ID

enterprise.8164.2.449

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcCallsPerInterval

Object ID

enterprise.8164.2.450

Description

The Per-Service CSCF Calls Per Interval count has gone above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcCallsPerInterval

Object ID

enterprise.8164.2.451

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcTotalActiveCalls

Object ID

enterprise.8164.2.452

Description

The Per-Service CSCF Total Active Calls count has gone above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcTotalActiveCalls

Object ID

enterprise.8164.2.453

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcTotalCallFailure

Object ID

enterprise.8164.2.454

Description

The per-service CSCF Total Call Failure count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcTotalCallFailure

Object ID

enterprise.8164.2.455

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcErrorNoResource

Object ID

enterprise.8164.2.456

Description

The per-service CSCF No Resource Failure count has gone above the configured threshold.

Probable Cause: This is a user configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcErrorNoResource

Object ID

enterprise.8164.2.457

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcErrorTcp

Object ID

enterprise.8164.2.458

Description

The per-service CSCF Tcp Failure count has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcErrorTcp

Object ID

enterprise.8164.2.459

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcErrorPresence

Object ID

enterprise.8164.2.460

Description

The Per-Service CSCF Presence failure count has gone above the configured threshold. Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcErrorPresence

Object ID

enterprise.8164.2.461

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshCSCFSvcErrorRegAuth

Object ID

enterprise.8164.2.462

Description

The Per-Service CSCF Reg-Auth failure count has gone above the configured threshold. Probable Cause: This is a user-configurable threshold.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCSCFSvcErrorRegAuth

Object ID

enterprise.8164.2.463

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshBGPRoutes

Object ID

enterprise.8164.2.464

Description

The total number of BGP routes is above the configured threshold value.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearBGPRoutes notification will be generated when the measured value falls below the threshold.

Objects

starContextName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearBGPRoutes

Object ID

enterprise.8164.2.465

Description

The threshold condition is now clear.

Objects

starContextName

starThreshPct

starThreshMeasuredPct
Object

starThreshPCCPolicySessions

Object ID

enterprise.8164.2.466

Description

The total number of PCC-Policy sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPCCPolicySessions

Object ID

enterprise.8164.2.467

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServicePCCPolicySessions

Object ID

enterprise.8164.2.468

Description

The total number of PCC-Policy sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServicePCCPolicySessions

Object ID

enterprise.8164.2.469

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPCCQuotaSessions

Object ID

enterprise.8164.2.470

Description

The total number of PCC-Quota sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPCCQuotaSessions

Object ID

enterprise.8164.2.471

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServicePCCQuotaSessions

Object ID

enterprise.8164.2.472

Description

The total number of PCC-Quota sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServicePCCQuotaSessions

Object ID

enterprise.8164.2.473

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshPCCAFSessions

Object ID

enterprise.8164.2.474

Description

The total number of PCC-AF sessions is above the configured threshold value.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPCCAFSessions

Object ID

enterprise.8164.2.475

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServicePCCAFSessions

Object ID

enterprise.8164.2.476

Description

The total number of PCC-AF sessions in a service is above the configured threshold value.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServicePCCAFSessions

Object ID

enterprise.8164.2.477

Description

The threshold condition is now clear.

Objects

starServiceVpnName

starServiceServName

starThreshInt

starThreshMeasuredInt
Object

starThreshNPUUtilization

Object ID

enterprise.8164.2.478

Description

The overall NPU utilization for the identified processor is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

If the thresholding subsystem is configured to run in alarm mode, a starThreshClearNPUUtilization notification will be generated when the measured value falls below the threshold.

Objects

starNPUSlot

starThreshPct

starThreshMeasuredPct
Object

starThreshClearNPUUtilization

Object ID

enterprise.8164.2.479

Description

The threshold condition is now clear.

Objects

starNPUSlot

starThreshPct

starThreshMeasuredPct
Object

starThreshDnsLookupFailure

Object ID

enterprise.8164.2.480

Description

The Total number of DNS lookup failures is above the configured threshold value.

Probable Cause: This is a user-configurable threshold.

If the thresholding subsystem is configured to run in alarm mode, a starThreshClearDnsLookupFailure notification will be generated when the measured value falls below the threshold.

Objects

starContextName

starThreshPct

starThreshMeasuredPct
Object

starThreshClearDnsLookupFailure

Object ID

enterprise.8164.2.481

Description

The threshold condition is now clear.

Objects

starContextName

starThreshPct

starThreshMeasuredPct
Object

starThreshDiameterRetryRate

Object ID

enterprise.8164.2.482

Description

The percentage of Diameter requests to be retried has exceeded the configured threshold.

Probable Cause: This is a user-configurable threshold.

If the thresholding subsystem is configured to run in an alarm mode, a starThreshClearDiameterRetryRate notification will be generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearDiameterRetryRate

Object ID

enterprise.8164.2.483

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshHNBGWHnbSess

Object ID

enterprise.8164.2.484

Description

The chassis-wide count of current HNBGW HNB sessions has gone above the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHNBGWHnbSess

Object ID

enterprise.8164.2.485

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshHNBGWUeSess

Object ID

enterprise.8164.2.486

Description

The chassis-wide count of current HNBGW UE sessions has gone above the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHNBGWUeSess

Object ID

enterprise.8164.2.487

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshHNBGWIuSess

Object ID

enterprise.8164.2.488

Description

The chassis-wide count of current HNBGW IU sessions has gone above the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearHNBGWIuSess

Object ID

enterprise.8164.2.489

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshPerServicePDGSessions

Object ID

enterprise.8164.2.491

Description

he total number of PDG sessions in a service is above the configured threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearPerServicePDGSessions

Object ID

enterprise.8164.2.492

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshSystemCapacity

Object ID

enterprise.8164.2.493

Description

The System resource capacity has exceeded the configured threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearSystemCapacity

Object ID

enterprise.8164.2.494

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshTpoRtoTimeout

Object ID

enterprise.8164.2.495

Description

The total number of TPO RTO timeouts is above the configured threshold.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearTpoRtoTimeout notification will be generated when the measured value falls below the threshold.

Objects

starThreshClearTpoRtoTimeout

starThreshMeasuredInt
Object

starThreshHNBGWIuSess

Object ID

enterprise.8164.2.496

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshTpoDnsFailure

Object ID

enterprise.8164.2.497

Description

The total number of TPO DNS query failure is above the configured threshold.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearTpoDnsFailure notification will be generated when the measured value falls below the threshold.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshClearTpoDnsFailure

Object ID

enterprise.8164.2.498

Description

The threshold condition is now clear.

Objects

starThreshPct

starThreshMeasuredPct
Object

starThreshTpoLowCompressionGain

Object ID

enterprise.8164.2.499

Description

The total number of TPO low compression gain is above the configured threshold.

Probable Cause: This is a user-configurable threshold. If the thresholding subsystem is configured to run in alarm mode, a starThreshClearTpoLowCompressionGain notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearTpoLowCompressionGain

Object ID

enterprise.8164.2.500

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshEPDGCurrSess

Object ID

enterprise.8164.2.501

Description

The chassis-wide count of current EPDG sessions has gone above the configured threshold.

Probable Cause: This is a user-configurable threshold

If the thresholding subsystem is configured to run in alarm mode, a starThreshClearEPDGCurrSess notification will be generated when the measured value falls below the threshold.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshClearEPDGCurrSess

Object ID

enterprise.8164.2.502

Description

The threshold condition is now clear.

Objects

starThreshInt

starThreshMeasuredInt
Object

starThreshCardTemperatureNearPowerOffLimit
Object ID

enterprise.8164.2.503

Description

On a given card, the distance between the poweroff/reset point and current temperature on card is smaller than the setted threshold during the current monitoring period.

Probable Cause: This is a user-configurable threshold. Possible reasons for this alarm:

- External temperature is too high.
- One or more fan failures.
- Blockages the prevent fan air inflow/outflow.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearCardTemperaturePowerOffLimit notification will be generated when the measured temperature falls, making the distance between the poweroff/reset point and current temperature larger than the set threshold.

Objects

starSlotNum

starThreshInt

starThreshMeasuredInt
Object

starThreshClearCardTemperaturePowerOffLimit

Object ID

enterprise.8164.2.504

Description

On a given card, the distance between the poweroff/reset point and current temperature on card is larger than the set clear point.

Objects

starSlotNum

starThreshInt

starThreshMeasuredInt
Object

starThreshAAAAcctArchiveQueue-1

Object ID

enterprise.8164.2.505

Description

The Per-Sessmgr Archive queue usage is above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAcctArchiveQueue-1 notification will be generated when the measured value falls below the threshold.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starThreshClearAAAAcctArchiveQueue-1

Object ID

enterprise.8164.2.506

Description

The threshold condition is now clear.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starThreshAAAAcctArchiveQueue-2

Object ID

enterprise.8164.2.507

Description

The Sessmgr Archive queue usage is above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAcctArchiveQueue-2 notification will be generated when the measured value falls below the threshold.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starThreshClearAAAAcctArchiveQueue-2

Object ID

enterprise.8164.2.508

Description

The threshold condition is now clear.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starThreshAAAAcctArchiveQueue-3

Object ID

enterprise.8164.2.509

Description

The Sessmgr Archive queue usage is above the configured threshold.

Probable Cause: This is a user-configurable threshold.

Condition Clear Alarm: If the thresholding subsystem is configured to run in alarm mode, a starThreshClearAAAAcctArchiveQueue-3 notification will be generated when the measured value falls below the threshold.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starThreshClearAAAAcctArchiveQueue-3

Object ID

enterprise.8164.2.510

Description

The threshold condition is now clear.

Objects

starTaskInstance

starThreshPct

starThreshMeasuredPct
Object

starOSPFNeighborDown

Object ID

enterprise.8164.2.1001

Description

An OSPF neighbor is down.

Condition Clear Alarm: A starOSPFNeighborFull notification will be generated when the neighbor is restored.

Objects

starContextName

starInterfaceName

starInterfaceIPAddress

starOSPFNeighborRouterID

starOSPFFromState

starOSPFToState
Object

starOSPFNeighborFull

Object ID

enterprise.8164.2.1002

Description

An OSPF neighbor is full. A starOSPFNeighborFull notification is only sent for neighbors which had previously been declared down via a starOSPFNeighborDown notification.

Objects

starContextName

starInterfaceName

starInterfaceIPAddress

starOSPFNeighborRouterID
Object

starM3UAPSDown

Object ID

enterprise.8164.2.1004

Description

The M3UA Peer Server is unavailable.

Probable Cause: All related Peer Server Processes(PSPs) are in the ASP-Down state for this peer server.

Condition Clear Alarm: A starM3UAPSActive notification will be generated when the peer server becomes reachable as at least one PSP is in ASP-Active state.

Objects

starSS7rdId

starSS7M3UAPsID
Object

starM3UAPSActive

Object ID

enterprise.8164.2.1005

Description

Peer Server is available and application traffic is active. This state implies that at least one PSP is in the ASP-Active state. A starM3UAPSActive notification is only generated for application services which were previously declared down via a starM3UAPSDown notification

Objects

starSS7rdId

starSS7M3UAPsID
Object

starM3UAPSPDown

Object ID

enterprise.8164.2.1006

Description

ASP Down message received from the remote M3UA peer indicates the adaptation layer at the remote peer is not ready to receive DATA, SSNM, RKM or ASPTM messages.

Probable Cause: SCTP association is down or remote peer server is down.

Condition Clear Alarm: A starM3UAPSPUp notification will be generated when the remote ASP is available.

Objects

starSS7rdId

starSS7M3UAPspID

starSS7CauseString
Object

starM3UAPSPUp

Object ID

enterprise.8164.2.1007

Description

ASP Up message from remote M3UA Peer indicates the adaptation layer at the remote peer is ready to receive ASPSM/ASPTM messages for all routing keys the ASP is configured to serve. Up message is only generated after a previous down message.

Objects

starSS7rdId

starSS7M3UAPspId

starSS7M3UAPsId

starSS7CauseString
Object

starSCCPSspRcvd

Object ID

enterprise.8164.2.1008

Description

Subsystem Prohibited message was received from a peer.

Probable Cause: This is sent by the peer SCCP layer when one of its apps (subsystems), such as the HLR, is out of commission.

Action to be Taken: Receiving node needs to update the translation tables so that traffic can be directed to a backup system if available.

Condition Clear Alarm: A starSCCPSspClear notification is generated when this condition is cleared.

Objects

starSccpNwId

starSS7Pc

starSccpSsn
Object

starSCCPSspClear

Object ID

enterprise.8164.2.1009

Description

Subsystem Available received from a peer This indicates a previously prohibited node is now available.

Objects

starSccpNwId

starSS7Pc

starSccpSsn
Object

starSGSNRNCReset

Object ID

enterprise.8164.2.1010

Description

SGSN has received a Radio Network Controller reset event. SGSN will clean up all the lu connections.

IMPORTANT:

This event is not generated for RNC Reset the first time the system boots up.

Objects

starSessSGSNVpnName

starSessSGSNServName

starSessSGSNMcc

starSessSGSNMnc

starSessSGSNRncId
Object

starSGSNHLRReset

Object ID

enterprise.8164.2.1011

Description

Home Location Register (HLR) reset event received. SGSN will mark all subscribers served by this HLR so the subscription record can be fetched again on subsequent activity.

Objects

starSessSGSNVpnName

starSessSGSNServName

starSessSGSNhlrNum
Object

starSGSNGtpcPathFailure

Object ID

enterprise.8164.2.1012

Description

No response received from peer GSN as several messages have timed out. The control path to the GSN is down.

Probable Cause: Remote GSN is down.

Condition Clear Alarm: A starSGSNGtpcPathFailureClear alarm is generated when the GSN becomes reachable.

Objects

starSGTPVpnName

starSGTPServName

starSGTPPeerAdd

starSGTPPeerPort

starSGSNSelfAddr

starSGSNSelfPort
Object

starSGSNFtpcPathFailureClear

Object ID

enterprise.8164.2.1013

Description

The path to the peer GSN which was down is now available. Generated only for GSNs which had previously been down.

Objects

starSGTPVpnName

starSGTPServName

starSGTPPeerAddr
Object

starSGSNGtpuPathFailure

Object ID

enterprise.8164.2.1014

Description

No response received for Echo Request sent from SGSN. Data path failure detected toward GSN or RNC.

Probable Cause: Remote GSN is down.

Action to be Taken: Check if peer RNC or GSN is up.

Condition Clear Alarm: A starSGSNGtpuPathFailureClear message is generated when the remote GSN becomes available again.

Objects

starSGTPVpnName

starSGTPNServName

starSGTPPeerAddr

tarSGTPPeerPort

starSGSNSelfAddr

starSGSNSelfPort
Object

starSGSNGtpuPathFailureClear

Object ID

enterprise.8164.2.1015

Description

The data path toward the peer GSN or RNC is now available. A path failure clear notification will only be sent for peers which had previously generated a path failure notification.

Objects

starSGTPVpnName,

starSGTPServName

starSGTPPeerAddr

starSGTPPeerPort

starSGSNSelfAddr

starSGSNSelfPor
Object

starMTP3LinkOutofService

Object ID

enterprise.8164.2.1016

Description

Message Transfer Part (MTP3) Link out of service.

Probable Cause: Physical link is down, Layer 2 SSCOP/MTP2 is down, or link was deactivated by operator.

Condition Clear Alarm: A starMTP3LinkInService message is generated when the link is restored.

Objects

starSS7rdId

starSS7MTP3LinkSetId

starSS7MTP3LinkId
Object

starMTP3LinkinService

Object ID

enterprise.8164.2.1017

Description

MTP3 link is now in service.

Objects

starSS7rdId

starSS7MTP3LinkSetId

starSS7MP3LinkId
Object

starMTP3LinkSetUnAvailable

Object ID

enterprise.8164.2.1018

Description

MTP3 Linkset Unavailable message.

Probable Cause: All links in linkset are down or linkset was deactivated by operator.

Condition Clear Alarm: A starMTP3LinkSetAvailable message is generated when the previously down linkset is restored.

Objects

starSS7rdId

starSS7MTP3LinkSetId
Object

starMTP3LinkSetAvailable

Object ID

enterprise.8164.2.1019

Description

MTP3 linkset is now available

Objects

starSS7rdId

starSS7MTP3LinkSetId
Object

starSCTPAssociationFail

Object ID

enterprise.8164.2.1020

Description

M3UA SCTP association establishment failure.

Probable Cause: Peer is down, or network is down, or the endpoint configuration is incorrect at our end.

Condition Clear Alarm: A starSCTPAssociationEstablished message is sent when a previously failed association is restored.

Objects

starSS7rdId

starSS7M3UAPspId

starSS7M3UAPsId
Object

starSCTPAssociationEstablished

Object ID

enterprise.8164.2.1021

Description

M3UA SCTP association established successfully. This message is only generated for peers which previously generated an Association Fail message.

Objects

starSS7rdId

starSS7M3UAPspId

starSS7M3UAPsId
Object

starSCTPPathDown

Object ID

enterprise.8164.2.1022

Description

SCTP path is down.

Probable Cause: Peer is down. Network to the remote server is down. The endpoint configuration is incorrect at our end.

Condition Clear Alarm: A starSCTPPathUp notification is generated when the path is restored.

Objects

starSS7rdId

starSS7M3UAPspId

starSS7M3UAPsId

starSS7SCTPPeerAddr

starSS7SCTPSelfAddr

starSS7SCTPPeerPort

starSS7SCTPSelfPort

starSS7CauseString
Object

starSCTPPathUp

Object ID

enterprise.8164.2.1023

Description

SCTP path up. This notification is only generated for peers which had previously generated an SCTP path down notification.

Objects

starSS7rdId

starSS7M3UAPspId

starSS7M3UAPsId

starSS7SCTPSelfAddr

starSS7SCTPSelfPort

starSS7SCTPPeerAddr

starSS7SCTPSelfAddr

starSS7SCTPPeerPort

starSS7CauseString
Object

starPortDown

Object ID

enterprise.8164.2.1024

Description

Physical port status is down.

Probable Cause: Network is down. Port is disconnected.

Condition Clear Alarm: A starPortUp notification is generated when the port is restored.

Objects

starPortSlot

starPortNum

starPortType
Object

starPortUp

Object ID

enterprise.8164.2.1025

Description

Physical port is up. This notification is only generated for a physical port with a previous starPortDown notification.

Objects

starPortSlot

starPortNum

starPortType
Object

starBSReachable

Object ID

enterprise.8164.2.1026

Description

The base station that the IMG communicates with is now reachable.

Objects

starContextName

starASNGWServiceName

starBSAddress
Object

starBSUnreachable

Object ID

enterprise.8164.2.1027

Description

The base station that the IMG communicates with is not reachable.

Probable Cause: The base station has failed or the network has connectivity problems.

Action to be Taken: If the outage was unplanned, reboot the base station and verify network connectivity.

Condition Clear Alarm: A starBSReachable notification is generated when the base station is reconnected.

Objects

starContextName

starASNGWServiceName

starBSAddress
Object

starSystemStartup

Object ID

enterprise.8164.2.1028

Description

The system has completed a reboot/startup

Objects

starChassisType

starChassisDescription

starChassisSWRevision
Object

starMTP3PCUnavailable

Object ID

enterprise.8164.2.1029

Description

MTP3 route to the point code is unavailable.

Probable Cause: All links within the linkset become unavailable. Remote peer is down.

Condition Clear Alarm: A starMTP3PCAvailable message is generated when the route to the point code is reestablished.

Objects

starSS7rdId

starSS7Pc

starSS7MTP3LinkSetId
Object

starMTP3PCAvailable

Object ID

enterprise.8164.2.1030

Description

MTP3 route to the point code available

Objects

starSS7rdId

starSS7Pc

starSS7MTP3LinkSetId
Object

starSS7PCUnavailable

Object ID

enterprise.8164.2.1031

Description

SS7 point code unavailable.

Probable Cause: All MTP3 and M3UA routes to the point code are unavailable.

Condition Clear Alarm: A starSS7PCAvailable message is generated when the route is reestablished.

Objects

starSS7rdId

starSS7Pc
Object

starSS7PCAvailable

Object ID

enterprise.8164.2.1032

Description

SS7 point code available.

Probable Cause: One of the M3UA or MTP3 routes is back up.

Action to be Taken: No action required.

Objects

starSS7rdId

starSS7Pc
Object

starASNPCServiceStart

Object ID

enterprise.8164.2.1033

Description

A WiMAX ASN Paging Controller (ASNPC) Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starASNPCServiceStop

Object ID

enterprise.8164.2.1034

Description

A WiMAX ASN Paging Controller (ASNPC) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the ASNPC service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the ASNPC service is operational.

Objects

starServiceVpnName

starServiceServName
Object

starDiameterCapabilitiesExchangeFailure

Object ID

enterprise.8164.2.1035

Description

Capability negotiations have failed and connections are down.

Probable Cause: Connections have been torn down due to an error in the Capability Exchange Answer received from the peer.

Objects

starDiameterVpnName

starDiameterPeerAddr

starDiameterEndpointName
Object

starDiameterCapabilitiesExchangeSuccess

Object ID

enterprise.8164.2.1036

Description

Diameter server is up. This notification is only generated for a server that has been previously declared unreachable

Objects

starDiameterVpnName

starDiameterPeerAddr

starDiameterEndpointName
Object

starSRPConnDown

Object ID

enterprise.8164.2.1037

Description

SRP system connection is down and active system is now without a standby and therefore unable to perform an SRP switchover.

Probable Cause: Network connectivity problem.

Action to be Taken: Verify standby system is operational and check the network connections are up.

Clear Condition: A starSRPConnUp notification is generated when condition is cleared.

Objects

starContextName

starSRPIpAddress
Object

starSRPConnUP

Object ID

enterprise.8164.2.1038

Description

SRP connection is restored. This notification is only generated after a previous connection loss was reported.

Objects

starContextName

starSRPIpAddress
Object

starDiameterIpv6PeerDown

Object ID

enterprise.8164.2.1039

Description

A Diameter peer is down. This Diameter peer is reached using an IPv6 address. For IPv4-connected Diameter peers, a starDiameterPeerDown notification would be generated.

Probable Cause: The Diameter peer has failed, or a network connectivity prevents reaching the peer.

Condition Clear Alarm: A starDiameterPeerUp notification will be generated when the peer is up.

Objects

starDiameterVpnName

starDiameterPeerAddrIpv6

starDiameterEndpointName
Object

starDiameterIpv6PeerUp

Object ID

enterprise.8164.2.1040

Description

A Diameter peer is up. This Diameter peer is reached using an IPv6 address. This notification is only generated for peers which have previously been declared down. For IPv4-connected Diameter peers, a starDiameterPeerUp notification would be generated.

Objects

starDiameterVpnName

starDiameterPeerAddrIpv6

starDiameterEndpointName
Object

starIPMSServerUnreachable

Object ID

enterprise.8164.2.1041

Description

An IPMS server is unreachable.

Probable Cause: The IPMS server has failed, or a network connectivity issue prevents reaching the server.

Condition Clear Alarm: A starIPMSServerReachable notification will be generated when the server becomes reachable.
Object

starIPMSServerReachable

Object ID

enterprise.8164.2.1042

Description

An IPMS server is reachable. A starIPMSServerReachable notification is only generated for servers which had previously been declared unreachable

Objects

starIPMSServerVpnName

starIPMSServerAddr
Object

starCertShortLifetime

Object ID

enterprise.8164.2.1043

Description

A certificate is approaching its expiration. The certificate is still valid, but should be updated with a new certificate.

Action to be Taken: A new certificate should be created and configured on the system.

Objects

starCertSerialNumber

starCertIssuer

starCertExpiryTime
Object

starCertExpired

Object ID

enterprise.8164.2.1044

Description

A certificate has expired. The certificate is no longer valid.

Action to be Taken: A new certificate should be created and configured on the system.

Condition Clear Alarm: A starCertValid notification is sent when a new, valid, certificate is configured.

Objects

starCertSerialNumber

starCertIssuer

starCertExpiryTime
Object

starCertValid

Object ID

enterprise.8164.2.1045

Description

A valid certificate has been configured. This notification is only generated if a starCertExpired had been previously generated.

Objects

starCertSerialNumber

starCertIssuer

starCertExpiryTime
Object

starFTPPushFail

Object ID

enterprise.8164.2.1046

Description

An FTP push operation has failed for the specified file to the specified server.

Objects

starFTPServVpnName

starFTPServIpAddr

starFileName

starFileApplication
Object

starFTPServSwitch

Object ID

enterprise.8164.2.1047

Description

An FTP server switchover has been performed; that is, the system has determined that an external FTP server is unreachable, and is not using an alternate FTP server

Objects

starFTPServVpnName

starFTPServIpAddr

starFTPServIpAddr

starFileApplication
Object

starSDHSectionDown

Object ID

enterprise.8164.2.1048

Description

The SDH interface on this port is down. The starSDHOperState identifies the specific issue.

Condition Clear Alarm: This condition is cleared by a starSDHSectionUp notification

Objects

starSDHSlot

starSDHPort

starSDHOperState
Object

starSDHSectionUp

Object ID

enterprise.8164.2.1049

Description

The SDH interface on this port is now up. A starSDHSectionUp notification is only generated if a starSDHSectionDown was previously generated for this port.

Objects

starSDHSlot

starSDHPort
Object

starSDHPathHopDown

Object ID

enterprise.8164.2.1050

Description

The identified SDH Path is down. The value of starSDHPathOperState identifies the specific failure bits.

Objects

starSDHPathSlot

starSDHPathPort

starSDHPathNum

starSDHPathOperState
Object

starSDHPathHopUp

Object ID

enterprise.8164.2.1051

Description

The identified SDH Path is up.

Objects

starSDHPathSlot

starSDHPathPort

starSDHPathNum
Object

starSDHLopDown

Object ID

enterprise.8164.2.1052

Description

The identified E1 Tributary on this port is down. The value of starE1TribOperStateLOP identifies the specific failure bits.

Condition Clear Alarm: This condition is cleared by a starSDHLopDown notification

Objects

starE1TribSlot

starE1TribPort

starE1TribPath

starE1TribTug2

starE1TribTu12

starE1TribOperStateLOP
Object

starSDHLopUp

Object ID

enterprise.8164.2.1053

Description

The identified E1 Tributary on this port is now up. A starE1TributaryUp notification is only generated if a starSDHLopDown was previously generated for this E1 tributary.

Objects

starE1TribSlot

starE1TribPort

starE1TribPath

starE1TribTug2

starE1TribTu12
Object

starSS7PCCongested

Object ID

enterprise.8164.2.1056

Description

SS7 point code is congested; all the routes to this point-code are congested.

Probable Cause: All the routes (both M3UA and MTP3) to this point code have become congested.

Condition Clear Alarm: A starSS7PCCongestionCleared notification will be generated when the congestion gets cleared for any one of the routes.

Objects

starSS7rdId

starSS7Pc

starSS7CongLevel

starSS7LocalCong
Object

starSS7PCCongestionCleared

Object ID

enterprise.8164.2.1057

Description

SS7 Point code is congested; all the routes to this point-code are congested.

Objects

starSS7rdId

starSS7Pc

starSS7CongLevel

starSS7LocalCong
Object ID

enterprise.8164.2.1058

Description

A PHS-GW Service has started

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starPHSGWServiceStop

Object ID

enterprise.8164.2.1059

Description

A PHS-GW Service has stopped

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the PHS-GW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PHS-GW service is operational

Condition Clear Alarm: A starPHSGWServiceStart notification will be generated when the service is restarted

Objects

starServiceVpnName

starServiceServName
Object

starGPRSServiceStart

Object ID

enterprise.8164.2.1060

Description

A GPRS Service has started

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starGPRSServiceStop

Object ID

enterprise.8164.2.1061

Description

A GPRS Service has stopped.

In unusual cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.This can also happen due to some misconfiguration of the service parameters.

Action to be Taken: If the GPRS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the GPRS service is operational.

Condition Clear Alarm: A starGPRSServiceStart notification will be generated when the service is restarted

Objects

starServiceVpnName

starServiceServName
Object

starGPRSNseDown

Object ID

enterprise.8164.2.1062

Description

Network Service Entity (NSE) is down.

Possible Cause: The last NSVC (Network Service virtual circuit in the NSE is down.

Condition Clear Alarm: A starGPRSNseUp will be generated when at least one NSVC in the NSE comes up.

Objects

starGPRSNsei
Object

starGPRSNseUp

Object ID

enterprise.8164.2.1063

Description

Network Service Entity (NSE) is up.

The first NSVC (Network Service virtual circuit in the NSE is up.

Condition Clear Alarm: A starGPRSNseUp notification is generated only when a previous starGPRSNseDown has been generated.

Objects

starGPRSNsei
Object

starGPRSNsvcDown

Object ID

enterprise.8164.2.1064

Description

Network Service Entity Virtual Circuit (NSVC) is down.

Probable Cause: NS_ALIVE heartbeat messages sent from the Serving GPRS Support Node (SGSN) were not acknowledged by the Base Station Subsystem (BSS) for a configured number of maximum retries. This trap is generated only when an NSVC goes down due to reasons other than physical port failure. A separate trap is generated for a physical port failure event.

Condition Clear Alarm: A starGPRSNsvcUp will be generated when the NSVC is restored.

Objects

starGPRSNsei

starGPRSNsvci
Object

starGPRSNsvcUp

Object ID

enterprise.8164.2.1065

Description

A Network Service Entity Virtual Circuit (NSVC) comes up. An starGPRSNsvcUp trap is generated only when a previous starGPRSNsvcDown was generated

Objects

starGPRSNsei

starGPRSNsvci
Object

starGPRSBvcDown

Object ID

enterprise.8164.2.1066

Description

Base Station Subsystem (BSS) GPRS (General Packet Radio Service) Protocol (BSSGP) Virtual Circuit (BVC) is down.

Probable Cause: All Network Service Entity Virtual Circuits (NSVC) associated with this BVC are down.

Condition Clear Alarm: A starGPRSBvcUp will be generated when the BVC is available.

Objects

starGPRSNsei

starGPRSBvci
Object

starGPRSBvcUp

Object ID

enterprise.8164.2.1067

Description

Base Station Subsystem (BSS) GPRS ((General Packet Radio Service) Protocol (BSSGP) Virtual Circuit (BVC) is up

Probable Cause: At least one NSVC associated with the BVC becomes available. A starGPRSBvcUp is generated only when a previous starGPRSBvcDown has been generated.

Objects

starGPRSNsei

starGPRSBvci
Object

starSDHE1TribDown

Object ID

enterprise.8164.2.1068

Description

The identified E1 Tributary on this port is down.

Condition Clear Alarm: This condition is cleared by a starSDHTugUp notification

Objects

starE1TribSlot

starE1TribPort

starE1TribPath

starE1TribTug2

starE1TribTu12

starE1TribOperState
Object

starSDHE1TribUp

Object ID

enterprise.8164.2.1069

Description

The condition is cleared.

Objects

starE1TribSlot

starE1TribPort

starE1TribPath

starE1TribTug2

starE1TribTu12
Object

starSDHFractE1LMIDown

Object ID

enterprise.8164.2.1070

Description

The identified fractional E1 Tributary on this port is down.

Objects

starFractE1TribSlot

starFractE1TribPort

starFractE1TribPath

starFractE1TribTug2

starFractE1TribTu12

starFractE1TribTimeslots
Object

starSDHFractE1LMIUp

Object ID

enterprise.8164.2.1071

Description

The condition is cleared.

Objects

starFractE1TribSlot

starFractE1TribPort

starFractE1TribPath

starFractE1TribTug2

starFractE1TribTu12
Object

starPHSPCServiceStart

Object ID

enterprise.8164.2.1072

Description

A PHS-PC Service has started

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starPHSPCServiceStop

Object ID

enterprise.8164.2.1073

Description

A PHS-PC Service has stopped

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration

Action to be Taken: If the PHS-PC service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PHS-PC service is operational.

Condition Clear Alarm: A starPHSPCServiceStart notification will be generated when the service is restarted.

Objects

starIPMSServerVpnName

starIPMSServerAddr
Object

starM3UAPSPCongested

Object ID

enterprise.8164.2.1074

Description

Peer Server Process (PSP) link is congested when the congestion queue size rises above the threshold limit.

Probable Cause: No Stream Control Transmission Protocol (SCTP) acknowledgement from peer server due to packet loss, or an acknowledgement with zero window size.

Condition Clear Alarm: A starM3UAPSPCongestionCleared notification will be generated when the congestion queue size goes below the threshold limit.

Objects

starSS7rdId

starSS7M3UAPsId

starSS7M3UAPspId

starSS7Pc

starSS7CongLevel
Object

starM3UAPSPCongestionCleared

Object ID

enterprise.8164.2.1075

Description

Peer Server Process (PSP) link Congestion gets cleared when the congestion queue size goes below the threshold limit. A starM3UAPSPCongestionCleared notification is generated only when a previous starM3UAPSPCongested is generated.

Objects

starSS7rdId

starSS7M3UAPsId

starSS7M3UAPspId

starSS7Pc

starSS7CongLevel
Object

starStorageFailed

Object ID

enterprise.8164.2.1076

Description

The specified storage device has failed. This storage device is now out of service and cannot be used to store additional data. This notification is currently only generated for failures on the hard drive attached to the SMC card.

Probable Cause: A hardware failure on the device, or a hardware failure on the card to which the device is attached.

Action to be Taken: Replace the card.

Condition Clear Alarm: A starCardRemoved notification will be generated when the card is removed from the chassis.

Objects

starStorageSlot

starStorageName
Object

starRaidFailed

Object ID

enterprise.8164.2.1077

Description

The specified raid array has failed. The raid array can no longer be used to store data.

Probable Cause: Hardware failure(s) on the devices within the raid array; or hardware failure(s) on the card(s) to which the devices are attached; or the removal of the cards containing devices in the array; or operator action which disabled the raid array.

Condition Clear Alarm: A starRaidStarted notification will be generated when the raid array is online.

Objects

starStorageName
Object

starRaidStarted

Object ID

enterprise.8164.2.1078

Description

The specific raid array has resumed operation. This notification is only generated if a starRaidFailed notification was previously generated for this array.

Objects

starStorageName
Object

starRaidDegraded

Object ID

enterprise.8164.2.1079

Description

The specified raid array is running in a degraded state. This typically means one of the member devices has failed or become unavailable. The raid array continues to function and can read/store data, but may not be operating in a redundant manner.

Probable Cause: Hardware failure(s) on the devices within the raid array; hardware failure(s) on the card(s) to which the devices are attached; the removal of the cards containing devices in the array; operator action which disabled the raid array.

The first variable binding, starStorageName, is indicating the raid array name. The second variable binding, starStorageSlot, is the disk card number where the failure happens. The third varbind, which is also the second starStorageName, is the name of the disk where the fail happens.

Condition Clear Alarm: A starRaidRecovered notification will be generated when the raid array is fully recovered.

Objects

starStorageName

starStorageSlot

starStorageName
Object

starRaidRecovered

Object ID

enterprise.8164.2.1080

Description

The specific raid array has been recovered and is running in its normal redundant state. This notification is only generated if a starRaidDegraded notification was previously generated for this array. As to the variable bindings, please refer to the trap starRaidDegraded.

Objects

starStorageName

starStorageSlot

starStorageName
Object

starPGWServiceStart

Object ID

enterprise.8164.2.1081

Description

A Packet Data Network Gateway (PGW) Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starPGWServiceStop

Object ID

enterprise.8164.2.1082

Description

A Packet Data Network Gateway (PGN) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the PGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PGW service is operational.

Condition Clear Alarm: A starPGWServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starSGWServiceStart

Object ID

enterprise.8164.2.1083

Description

A Serving Gateway (SGW) Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starSGWServiceStop

Object ID

enterprise.8164.2.1084

Description

A Serving Gateway (SGW) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the SGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the SGW service is operational.

Condition Clear Alarm: A starSGWServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starEGTPServiceStart

Object ID

enterprise.8164.2.1085

Description

An Evolved GPRS Tunneling Protocol (EGTP) Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starEGTPServiceStop

Object ID

enterprise.8164.2.1086

Description

An Evolved GPRS Tunneling Protocol (EGTP) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the configuration.

Action to be Taken: If the EGTP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the EGTP service is operational.

Objects

starServiceVpnName

starServiceServName
Object

starLMAServiceStart

Object ID

enterprise.8164.2.1087

Description

A Local Mobility Anchor (LMA) Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starLMAServiceStop

Object ID

enterprise.8164.2.1088

Description

A Local Mobility Anchor (LMA) service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the LMA service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the LMA service is operational.

Objects

starServiceVpnName

starServiceServName
Object

starMAGServiceStart

Object ID

enterprise.8164.2.1089

Description

A Mobile Access Gateway (MAG) Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starMAGServiceStop

Object ID

enterprise.8164.2.1090

Description

A MAG Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the MAG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the MAG service is operational.

Condition Clear Alarm: A starMAGServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starMMEServiceStart

Object ID

enterprise.8164.2.1091

Description

A Mobility Management Entity (MME) Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starMMEServiceStop

Object ID

enterprise.8164.2.1092

Description

A Mobility Management Entity (MME) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources (packet processing cards) to support the running configuration.

Action to be Taken: If the MME service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the MME service is operational.

Condition Clear Alarm: A starMMEServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starHSGWServiceStart

Object ID

enterprise.8164.2.1093

Description

A HRPD Serving Gateway (HSGW) Service has started.

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starHSGWServiceStop

Object ID

enterprise.8164.2.1094

Description

A HRPD Servi g Gateway (HSGW) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of resources (packet processing cards) to support the running configuration.

Action to be Taken: If the HSGW service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the HSGW service is operational.

Conditio Clear Alarm: A starHSGWServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starCPUBusyClear

Object ID

enterprise.8164.2.1095

Description

The CPU is no longer busy.

Objects

starCPUSlot

starCPUNumber
Object

starCPUMemoryLowClear

Object ID

enterprise.8164.2.1096

Description

The CPU is no longer experiencing a low memory condition.

Objects

starCPUSlot

starCPUNumber
Object

starFNGServiceStart

Object ID

enterprise.8164.2.1097

Description

A FNG Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starFNGServiceStop

Object ID

enterprise.8164.2.1098

Description

A FNG Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the FNG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running on the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the FNG service is operational.

Condition Clear Alarm: A starFNGServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starManagerRestart

Object ID

enterprise.8164.2.1099

Description

The identified manager task has been restarted.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU
Object

starConfigurationUpdate

Object ID

enterprise.8164.2.1100

Description

The configuration of the chassis has been changed. This notification is generated based on a periodic polling of the chassis, It is not real-time generated based on individual changes. The configuration change could have been made via CLI sessions, CORBA management operations, or other methods. This notification is not generated by default; it is only generated if the configuration polling mechanism is specifically enabled.
Object

starPDGServiceStart

Object ID

enterprise.8164.2.1101

Description

A PDG Service has started

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starPDGServiceStop

Object ID

enterprise.8164.2.1102

Description

A PDG Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the PDG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PDG service is operational.

Condition Clear Alarm: A starPDGServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starDynPkgLoadError

Object ID

enterprise.8164.2.1103

Description

The Dynamic rater package error displayed with an error code.

Condition Clear Alarm: This condition is cleared by a starDynPkgLoadErrorClear notification.

Objects

starDynPkgFilename

starDynCFErrorCode
Object

starDynPkgLoadErrorClear

Object ID

enterprise.8164.2.1104

Description

The error condition was removed.

Objects

starDynPkgFilename

starDynCFErrorCode
Object

starDynPkgUpgradeError

Object ID

enterprise.8164.2.1105

Description

The Dynamic rater package error displayed with an error code. This condition is cleared by a starDynPkgUpgradeErrorClear notification.

Objects

starDynPkgUpgradeFilename

starDynCFUpgradeErrorCode
Object

starDynPkgUpgradeErrorClear

Object ID

enterprise.8164.2.1106

Description

The Dynamic Rater package error was removed.

Objects

starDynPkgUpgradeFilename

starDynCFUpgradeErrorCode
Object

starCSCFPeerServerUnavailable

Object ID

enterprise.8164.2.1107

Description

Peer server is unavailable

Objects

starCSCFPeerServerVpnName

starCSCFPeerServerSvcName

starCSCFPeerServerName
Object

starCSCFPeerServerOutofService

Object ID

enterprise.8164.2.1108

Description

Peer server is out-of-service

Objects

starCSCFPeerServerVpnName

starCSCFPeerServerSvcName

starCSCFPeerServerName
Object

starCSCFPeerServerInService

Object ID

enterprise.8164.2.1109

Description

Peer server unavailable and/or out of service condition has been cleared.

Objects

starCSCFPeerServerVpnName

starCSCFPeerServerSvcName

starCSCFPeerServerName
Object

starServiceLossPTACsClear

Object ID

enterprise.8164.2.1110

Description

Service Loss condition is now cleared.

Objects

starCardMode
Object

starServiceLossLCClear

Object ID

enterprise.8164.2.1111

Description

Service Loss condition is now cleared.

Objects

starCardMode
Object

starEgtpcPathFailure

Object ID

enterprise.8164.2.1112

Description

EGTP Control Path Failure. No response received for GTPV2 request sent from MME or SGW or PGW.

Probable Cause: Remote peer MME or SGW or PGW is down.

Condition Clear Alarm: A StarEgtpcPathFailureClear notification will be generated when the control path to the remote peer MME or SGW or PGW becomes available.

Objects

starEGTPVpnName

starEGTPServName

starEGTPInterfaceType

starEGTPSelfAddr

starEGTPPeerAddr

starEGTPPeerOldRstCnt

starEGTPPeerNewRstCnt

starEGTPPeerSessCnt

starEGTPFailureReason
Object

starEgtpcPathFailureClear

Object ID

enterprise.8164.2.1113

Description

EGTP Control Path Failure condition is no longer valid.

Objects

starEGTPVpnName

starEGTPServName

starEGTPInterfaceType

starEGTPSelfAddr

starEGTPPeerAddr

starEGTPPeerOldRstCnt

starEGTPPeerSessCnt
Object

starCscfSessResourceCongestion

Object ID

enterprise.8164.2.1114

Description

A congestion condition has occurred at Session Manager for Cscf Service.

Probable Cause: This is the result of an operator-configured congestion threshold being reached for CSCF Service at Session Manager. This can be due to high usage of the resource being monitored which indicates that the IMG is reaching its peak capacity, or could be caused by the incorrect configuration of the congestion thresholds.

Actions to be Taken: Verify that the congestion thresholds are correct; if the congested state is seem repeatedly, or for sustained periods of time, additional system capacity may need to be brought online.

Condition Clear Alarm: A starCscfSessResourceCongestionClear notification is sent when there are no congestion conditions for CSCF service in that Session Manager instance.

This system is cleared when the use of the specific resource falls below the configured limit.

Objects

starSmgrId

starCongestionPolicy

starCscfSessCongestionResourceType
Object

starCscfSessResourceCongestionClear

Object ID

enterprise.8164.2.1115

Description

A congestion condition has cleared.

Objects

starSmgrId
Object

starOSPFv3NeighborDown

Object ID

enterprise.8164.2.1116

Description

An OSPFv3 neighbor is down

Objects

starContextName

starInterfaceName

starInterfaceIPAddress

starOSPFNeighborRouterID

starOSPFFromState

starOSPFToState
Object

starOSPFv3NeighborFull

Object ID

enterprise.8164.2.1117

Description

An OSPFv3 neighbor is full.

Condition Clear Alarm: A starOSPFv3NeighborFull notification is only sent for neighbors which had previously been declared down via a starOSPFv3NeighborDown notification.

Objects

starContextName

starInterfaceName

starInterfaceIPAddress

starOSPFNeighborRouterID
Object

starServiceLossSPIOClear

Object ID

enterprise.8164.2.1118

Description

Service Loss condition has been cleared.

Objects

starCardMode
Object

starEgtpuPathFailure

Object ID

enterprise.8164.2.1119

Description

No response received for GTP-U ECHO requests. Data path failure detected towards peer EPC Node. Check if the peer RNC or GSN is up.

Probable Cause: Remote EPC node is down.

Condition Clear Alarm: A starEgtpuPathFailureClear notification will be generated when the data path towards the peer node is available.

Objects

starEGTPVpnName

starEGTPServName

starEGTPSelfAddr

starEGTPPeerAddr

starEGTPSelfPort

starEGTPPeerPort

starEGTPPeerSessCnt
Object

starEgtpuPathFailureClear

Object ID

enterprise.8164.2.1120

Description

The data path to the peer EPC node which was down is now available A starEgtpuPathFailureClear notification is only generated for nodes which had previously generated a starEgtpuPathFailure notification.

Objects

starEGTPVpnName

starEGTPServName

starEGTPSelfAddr

starEGTPPeerAddr

starEGTPSelfPort

starEGTPPeerPort
Object

starStorageServerCDRLoss

Object ID

enterprise.8164.2.1121

Description

GTPP Storage Server is experiencing CDR Loss greater than the configured threshold value at the GSS.

Objects

starSessGGSNVpnName

starSessGGSNPeerAddr

starGSSCDRLossConfigured

starGSSCDRLossMeasured

starGSSClusterName

starGSSClusterNodeName
Object

starHNBGWServiceStart

Object ID

enterprise.8164.2.1122

Description

A Home Node B Gateway (HNB GW) Service has started

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starHNBGWServiceStop

Object ID

enterprise.8164.2.1123

Description

A Home Node B Gateway (PGN) Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of packet processing card resources to support the running configuration

Action to be Taken: If the HNB GW service shutdown was not planned, examine the ad min logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure

Clear Condition: Verify that the HNB GW service is operational

Condition Clear Alarm: A starHNBGWServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starSystemReboot

Object ID

enterprise.8164.2.1124

Description

The system has rebooted by the operator. If successful, a subsequent starSystemStartup trap is typically generated.

Action to be Taken: No action required. If the reboot was not scheduled the admin logs can be examined to determine who invoked the reboot operation.

Objects

starChassisType

starChassisDescription

starChassisSWRevision
Object

starLicenseAboutToExpire

Object ID

enterprise.8164.2.1125

Description

A license is about to expire

Action to be Taken: A new license should be created and configured on the system before the grace period is over.

Objects

starLicenseKey

starLicenseExpiryDate

starLicenseDaysRemaining
Object

starLicenseExpired

Object ID

enterprise.8164.2.1126

Description

A license is in the grace period and should be updated with a new license.

Action to be Taken: A new license should be created and configured on the system.

Objects

starLicenseKey

starLicenseExpiryDate

starLicenseDaysAfterExpiry
Object

starPCCPolicyServiceStart

Object ID

enterprise.8164.2.1127

Description

A PCC-Policy Service has started

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starPCCPolicyServiceStop

Object ID

enterprise.8164.2.1128

Description

A PCC-Policy Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the PCC-Policy service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PCC-Policy service is operational.

Condition Clear Alarm: A starPCCPolicyServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starPCCQuotaServiceStart

Object ID

enterprise.8164.2.1129

Description

A PCC-Quota Service has started.

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starPCCQuotaServiceStop

Object ID

enterprise.8164.2.1130

Description

A PCC-Quota Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the PCC-Quota service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PCC-Quota service is operational.

Condition Clear Alarm: A starPCCQuotaServiceStart notification will be generated when the service is restarted

Objects

starServiceVpnName

starServiceServName
Object

starPCCAFServiceStart

Object ID

enterprise.8164.2.1131

Description

A PCC-AF Service has started.

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starPCCAFServiceStop

Object ID

enterprise.8164.2.1132

Description

A PCC-AF Service has stopped.

Probable Cause: This is typically caused by operator intervention. In rare cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the PCC-AF service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the PCC-AF service is operational.

Condition Clear Alarm: A starPCCAFServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starSPRServerUnreachable

Object ID

enterprise.8164.2.1133

Description

The Subscriber Profile Repository (SPR) server cannot be reached.

Probable Cause: The SPR server is down, or there is a network issue preventing communication with the SPR server.

Action to be Taken: Restore the SPR server to an operational status; Verify that the SPR server is reachable by performing a 'ping' operation from the CLI in the appropriate context. Check the admin logs for notification of communication problems.

Clear Condition: Verify that communication to the SPR authentication server has been restored.

Condition Clear Alarm: When this condition clears a starSPRServerReachable notification will be generated.

Objects

starSPRServerIpAddr
Object

starSPRServerReachable

Object ID

enterprise.8164.2.1134

Description

The Subscriber Profile Repository (SPR) server is now reachable. This can be the result of a system startup, the configuration of a new server, or a previously unreachable server becoming reachable.

Action to be Taken: No Action Required.

Objects

starSPRServerIpAddr
Object

starGSServiceStart

Object ID

enterprise.8164.2.1135

Description

A GS Service has started

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starGSServiceStop

Object ID

enterprise.8164.2.1136

Description

A GS Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the GS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Objects

starServiceVpnName

starServiceServName
Object

starMAPServiceStart

Object ID

enterprise.8164.2.1137

Description

A MAP Service has started

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starMAPServiceStop

Object ID

enterprise.8164.2.1138

Description

A MAP Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Objects

starServiceVpnName

starServiceServName
Object

starIUPSServiceStart

Object ID

enterprise.8164.2.1139

Description

An IUPS Service has started.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starIUPSServiceStop

Object ID

enterprise.8164.2.1140

Description

An IUPS Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the IUPS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the IUPS service is operational.

Objects

starServiceVpnName

starServiceServName
Object

starSGTPServiceStart

Object ID

enterprise.8164.2.1141

Description

A SGTP Service has started

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starSGTPServiceStop

Object ID

enterprise.8164.2.1142

Description

A SGTP Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the SGTP service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the SGTP service is operational.

Objects

starServiceVpnName

starServiceServName
Object

starEPDGServiceStart

Object ID

enterprise.8164.2.1143

Description

A EPDG Service has started

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName
Object

starEPDGServiceStop

Object ID

enterprise.8164.2.1144

Description

A EPDG service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the EPDG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the EPDG service is operational.

Condition Clear Alarm: A starEPDGServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starApsCommandSuccess

Object ID

enterprise.8164.2.1145

Description

APS Command Succes Status.

Objects

starSlotNum

starPortSlot

starIfIndex

starPortType

starApsOperation
Object

starApsCommandFailure

Object ID

enterprise.8164.2.1146

Description

APS Command Failure Status.

Objects

starSlotNum

starPortSlot

starIfIndex

starPortType

starApsOperation
Object

starApsSwitchSuccess

Object ID

enterprise.8164.2.1147

Description

APS Switch Command Status.

Objects

starSlotNum

starPortSlot

starIfIndex

starPortType

starApsOperation
Object

starApsSwitchFailure

Object ID

enterprise.8164.2.1148

Description

APS Switch Command failure status.

Objects

starSlotNum

starPortSlot

starIfIndex

starPortType

starApsOperation
Object

starApsModeMismatch

Object ID

enterprise.8164.2.1149

Description

APS Mode Mismatch Status

Objects

starSlotNum

starCardType

starPortSlot
Object

starApsChannelMismatch

Object ID

enterprise.8164.2.1150

Description

APS channel mismatch Status.

Objects

starSlotNum

starCardType

starPortSlot
Object

starApsByteMismatch

Object ID

enterprise.8164.2.1151

Description

APS byte mismatch status.

Objects

starSlotNum

starCardType

starPortSlot
Object

starApsFeProtLineFailure

Object ID

enterprise.8164.2.1152

Description

APS FE port line failure status.

Objects

starSlotNum

starCardType

starSlotNum

starSlotNum
Object

starApsLossOfRedundancy

Object ID

enterprise.8164.2.1153

Description

APS Loss of Redundancy Status.

Objects

starSlotNum

starCardType

starSlotNum

starSlotNum
Object

starApsLossOfRedundancyClear

Object ID

enterprise.8164.2.1154

Description

APS Redundancy Restored Status.

Objects

starSlotNum

starCardType

starSlotNum

starSlotNum
Object

starHNBGWSGSNRanapReset

Object ID

enterprise.8164.2.1155

Description

HNBGW has received RANAP Reset event from SGSN.

Objects

starSessHNBGWVpnName

starSessHNBGWServName

starSessHNBGWPsNwName

starSessHNBGWSgsnPtCd
Object

starHNBGWMSCRanapReset

Object ID

enterprise.8164.2.1156

Description

HNBGW has received RANAP Reset event from MSC.

Objects

starServiceVpnName

starSessHNBGWServName

starSessHNBGWCsNwName

starSessHNBGWMscPtCd
Object

starALCAPNodeReset

Object ID

enterprise.8164.2.1157

Description

HNBGW has received ALCAP Node Reset from MGW.

Objects

starSessALCAPVpnName

starSessALCAPServName

starSessALCAPNodeName
Object

starALCAPPathReset

Object ID

enterprise.8164.2.1158

Description

HNBGW has received ALCAP Path Reset from MGW.

This event is sent by MGW on detection of certain failures. MGW can also provide CLI to send the event.

HNBGW will terminate all the cs calls impacted due to the path reset.

Objects

starSessALCAPVpnName

starSessALCAPServName

starSessALCAPNodeName

starSessALCAPPathId
Object

starALCAPPathBlock

Object ID

enterprise.8164.2.1159

Description

HNBGW has received ALCAP Path Block from MGW.

Objects

starSessALCAPVpnName

starSessALCAPServName

starSessALCAPPathId
Object

starALCAPPathUnBlock

Object ID

enterprise.8164.2.1160

Description

ALCAP Unblock received from MGW.

Objects

starSessALCAPVpnName

starSessALCAPServName

starSessALCAPPathId
Object

starSGSServiceStart

Object ID

enterprise.8164.2.1161

Description

An SGS Service has started.

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starSGSServiceStop

Object ID

enterprise.8164.2.1162

Description

An SGS Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of packet processing card resources to support the running configuration.

Action to be Taken: If the SGS service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured packet processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the SGS service is operational.

Condition Clear Alarm: A starSGSServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starMMES1AssocFail

Object ID

enterprise.8164.2.1163

Description

An S1 Association between an MME service and an eNodeB has failed.

Action to be Taken: If the shutdown of the eNodeB was not planned, determine the health/status of the eNodeB. If available, verify the health of the network between the two elements.

Clear Condition: The condition is cleared when the S1 Association is reestablished.

Objects

starMMES1AssocVpnName

starMMES1AssocServName

starMMES1AssocENBID
Object

starMMES1AssocSetup

Object ID

enterprise.8164.2.1164

Description

An S1 Association between an MME service and an eNodeB has been established. Normally a starMMES1AssocSetup notification would be generated only for an associated which had previously failed, but optionally this notification can be generated for any association setup.

Objects

starMMES1AssocVpnName

starMMES1AssocServName

starMMES1AssocENBID
Object

starBNGServiceStart

Object ID

enterprise.8164.2.1165

Description

A BNG Service has started.

Action to be Taken: No action required

Objects

starServiceVpnName

starServiceServName
Object

starBNGServiceStop

Object ID

enterprise.8164.2.1166

Description

A BNG Service has stopped.

Probable Cause: This is typically caused by operator intervention. In unusual cases it can be caused by the loss of packet processing card resources to support the running configuration.

Action to be Taken: If the BNG service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured processing cards are present and running in the system. Check the crash logs for an indication of a software failure.

Condition Clear Alarm: A starBNGServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starMMES1AssocFail

Object ID

enterprise.8164.2.1167

Description

An S1 Association between an MME service and an eNodeB has failed.

Action to be Taken: If the shutdown of the eNodeB was not planned, determine the health/status of the eNodeB. If available, verify the health of the network between the two elements.

Clear Condition: The condition is cleared when the S1 Association is reestablished.

Condition Clear Alarm: A starMMES1AssocEstab notification will be generated when the S1 association is re-established

Objects

starMMES1AssocVpnName

starMMES1AssocServName

starMMES1AssocENBID
Object

starMMES1AssocSetup

Object ID

enterprise.8164.2.1168

Description

An S1 Association between an MME service and an eNodeB has been established. Normally a starMMES1AssocSetup notification would be generated only for an associated which had previously failed, but optionally this notification can be generated for any association setup.

Objects

starMMES1AssocVpnName

starMMES1AssocServName

starMMES1AssocENBID
Object

starMVGPeerDown

Object ID

enterprise.8164.2.1169

Description

A MVG peer is down.

Problem Cause: The MVG peer has failed, or a network connectivity prevents reaching the peer.

Condition Clear Alarm: A starMVGPeerUp notification will be generated when the peer is up.

Objects

starServiceVpnName

starPeerAddress

starMVGEndpointName

starMVGCauseCode

starMVGProtocolType
Object

starMVGPeerUp

Object ID

enterprise.8164.2.1170

Description

An MVG peer is up. This notification is only generated for peers which have previously been declared down.

Objects

starServiceVpnName

starPeerAddress

starMVGEndpointName

starMVGCauseCode

starMVGProtocolType
Object

starPCCNtfyIntfPeerUnreachable

Object ID

enterprise.8164.2.1173

Description

The IPCF Event Notification Interface peer cannot be reached.

Probable Cause: The Event Notification server on SPR is down or the IP-address/port configuration does not match with the server.

Actions to be Taken: Check the Event Notification server on SPR and ensure it is running. Ensure that IP-address port combination on IPCF match the server side configurations

Condition Clear Alarm: When this condition clears, a starNtfyIntfPeerReachable notification will be generated.

Objects

starPCCNtfyIntfPeerName
Object

starPCCNtfyIntfPeerReachable

Object ID

enterprise.8164.2.1174

Description

The Notification Interface peer can be reached.

Action to be Taken: No action required.

Objects

starPCCNtfyIntfPeerName
Object

starIPSecNodePeerDown

Object ID

enterprise.8164.2.1175

Description

A Node Service peer has stopped responding

Action to be Taken: No Action Required.

Probable Cause: The IPSec Node peer has failed, or a network connectivity prevents reaching the peer.

Condition Clear Alarm: A starIPSecNodePeerUp notification will be generated when the peer is up.

Objects

starServiceVpnName

starServiceServName

starPeerAddress
Object

starIPSecNodePeerUp

Object ID

enterprise.8164.2.1176

Description

A Node Service peer is back online.

Action to be Taken: No action required.

Objects

starServiceVpnName

starServiceServName

starPeerAddress
Object

starCdrPurged

Object ID

enterprise.8164.2.1178

Description

CDR’s purged

Objects

starSessGGSNVpnName

starSessGGSNAPNName

starSessGTPPGroupName
Object

starCdrHDDStart

Object ID

enterprise.8164.2.1239

Description

CDRs are being written to the HDD

Probable Cause: All CGF servers under mentioned gtpp group are down.

Action to be Taken: Bring CGF server(s) up and verify that servers are functioning properly or change the storage mode.

Clear Condition: The condition is cleared when CGF server(s) are reachable.

Condition Clear Alarm: starCdrStreamingStart alarm would be generated if CDR(s) were written on HDD when all CGF servers under mentioned gtpp group were down.

Objects

starServiceVpnName

starSessGTPPGroupName
Object

starCdrStreamingStart

Object ID

enterprise.8164.2.1240

Description

CDR streaming is started

Probable Cause: CGF server(s) are up and CDR streaming is started.

Action to be Taken: NA

Clear Condition: All CDRs are streamed.

Condition Clear Alarm: starCdrStreamingComplete alarm will be generated on streaming completion.

Objects

starServiceVpnName

starSessGTPPGroupName
Object

starCdrStreamingComplete

Object ID

enterprise.8164.2.1241

Description

CDR streaming is Completed

Probable Cause: All CDRs written on HDD due to CGF server down have been streamed.

Action to be Taken: NA

Clear Condition: NA

Condition Clear Alarm: NA

Objects

starServiceVpnName

starSessGTPPGroupName
Object

starLocalUserAdded

Object ID

enterprise.8164.2.1180

Description

A local user was added to the system.

Probable Cause: A command was issued which resulted in a new user being added to the local user database. If this was not a planned action then further investigation is advised.

Objects

starContextName

starCLIUsername

starCLITtyname

starCLIRemoteIpAddrType.

starCLIRemoteIpAddr

starCLIDatabaseUsername

starCLIPrivs
Object

starLocalUserRemoved

Object ID

enterprise.8164.2.1181

Description

A local user was removed from the system.

Probable Cause: A command was issued which resulted in an existing user being removed from the local user database. If this was not a planned action then further investigation is advised.

Objects

starContextName

starCLIUsername

starCLITtyname

starCLIRemoteIpAddrType.

starCLIRemoteIpAddr

starCLIDatabaseUsername
Object

starLocalUserPrivilegeChanged

Object ID

enterprise.8164.2.1182

Description

A local user's privileges were modified.

Probable Cause: A command was issued which resulted in an existing user's privileges being modified. If this was not a planned action then further investigation is advised.

Objects

starCLIUsername

starCLITtyname

starCLIRemoteIpAddr

starCLIDatabaseUsername

starCLIPrivs

starCLIRemoteIpAddrType.
Object

starOsShellAccessed

Object ID

enterprise.8164.2.1183

Description

A user has accessed the operating system (OS) shell.

Probable Cause: A command was issued which resulted in a user's access to the operating system shell. If this was not a planned action then further investigation is advised.

Objects

starContextName

starCLIUsername

starCLITtyname

starCLIRemoteIpAddr

starCLIRemoteIpAddrType.
Object

starTestModeEntered

Object ID

enterprise.8164.2.1184

Description

A user has entered the StarOS Test Mode.

Probable Cause: A command was issued which resulted in a user entering the CLI test command mode. The test command mode is only intended for maintenance and diagnostic activity and access could result in major service disruptions. If this was not a planned action the user should exit from test mode.

Objects

starContextName

starCLIUsername

starCLITtyname

starCLIRemoteIpAddr

starCLIRemoteIpAddrType
Object

starLicenseFeaturesModified

Object ID

enterprise.8164.2.1185

Description

A user has manually modified the StarOS license feature set through the CLI.

Probable Cause: A command was issued which resulted in a user modifying the set of licensed features. This ability was only intended for maintenance and diagnostic activityand could result in major service disruptions. If this action was not intentional, the user should restore the original license feature set.

Objects

starContextName

starCLIUsername

starCLITtyname

starCLIRemoteIpAddr

starCLIRemoteIpAddrType.
Object

starHiddenAccessEnabled

Object ID

enterprise.8164.2.1186

Description

An administrator has explicitly enabled the use of hidden test commands.

Probable Cause: A command was configured which resulted in users having access to the specific test commands which may have been previously unavailable. If this action was not intentional, the user should disable access to the hidden test commands.

Objects

starContextName

starCLIUsername

starCLITtyname

starCLIRemoteIpAddr

starCLIRemoteIpAddrType.
Object

starHiddenAccessDisabled

Object ID

enterprise.8164.2.1187

Description

An administrator has explicitly disabled the use of hidden test commands.

Probable Cause: A command was configured which resulted in users no longer having access to specific test commands which may have been previously available. If this action was not intentional, the user should re-enable access to the hidden test commands.

Objects

starContextName

starCLIUsername

starCLITtyname

starCLIRemoteIpAddr

starCLIRemoteIpAddrType
Object

starLawfulInterceptChanged

Object ID

enterprise.8164.2.1188

Description

Original Lawful Intercept configured by Admin is changed by Admin.

Objects

starCLIUsername
Object

starMMES1PathFail

Object ID

enterprise.8164.2.1189

Description

An S1 Path between an MME service and an eNodeB has failed.

Action to be Taken: If the shutdown of the eNodeB was not planned, determine the health/status of the eNodeB. If available, verify the health of the network between the two elements.

Condition Clear Alarm: A starMMES1PathEstab notification will be generated when the S1 path is re-established.

Objects

starMMES1PathVpnName

starMMES1PathServName

starMMES1PathENBID

starMMES1PathSelfAddr

starMMES1PathSelfPort

starMMES1PathPeerAddr

starMMES1PathPeerPort
Object

starMMES1PathSetup

Object ID

enterprise.8164.2.10

Description

An S1 Path between an MME service and an eNodeB has been established. Normally a starMMES1PathSetup notification would be generated only for a path which had previously failed, but optionally this notification can be generated for any path setup.

Objects

starMMES1PathVpnName

starMMES1PathServName

starMMES1PathENBID

starMMES1PathSelfAddr

starMMES1PathSelfPort

starMMES1PathPeerAddr

starMMES1PathPeerPort
Object

starHenbgwAccessServiceStart

Object ID

enterprise.8164.2.1193

Description

A HENBGW Access Service has started. No action required

Objects

starServiceVpnName

starServiceServName
Object

starHenbgwAccessServiceStop

Object ID

enterprise.8164.2.1194

Description

A HENBGW Access Service has stopped.

Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the HENBGW Access service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the HENBGW Access service i s operational.

Condition Clear Alarm: A starHenbgwAccessServiceStart notification will be generated when the service is restarted.

Objects

starServiceVpnName

starServiceServName
Object

starHenbgwNetworkServiceStart

Object ID

enterprise.8164.2.1195

Description

A HENBGW Network Service has started

Objects

starServiceVpnName,

starServiceServName
Object

starHenbgwNetworkServiceStop

Object ID

enterprise.8164.2.1196

Description

A HENBGW Network Service has stopped.

Probable Cause: This is typically caused by operator invention. In unusual cases it can be caused by the loss of hardware resources to support the running configuration.

Action to be Taken: If the HENBGW Network service shutdown was not planned, examine the admin logs for an indication of the failure. Verify that all configured PACs/PSCs are present and running in the system. Check the crash logs for an indication of a software failure.

Clear Condition: Verify that the HENBGW Network service is operational.

Condition Clear Alarm: A starHenbgwNetworkServiceStart notification will be generated when the service is restarte

Objects

starServiceVpnName,

starServiceServName
Object

starAAAArchiveStarted

Object ID

enterprise.8164.2.1197

Description

AAA Archive started for sessmgr instance.

A AAAArchiveStarted trap will be generated if queue size crosses 15% of maximum number of sessmgr items per instance.

Objects

starTaskInstance
Object

starECSTotalDNSLearntIPv4Threshold

Object ID

enterprise.8164.2.1198

Description

DNS Learnt IPv4 entries exceed the threshold limit (high water mark) configured. For IPv4 Max IP entries = 512,00. Alarm Cleared when the IPv4 entries go below the Lower Water Mark configured

Objects

starECSTotalDNSLearntIPThresholdInstance

starECSTotalDNSLearntIPThresholdconfigured

starECSTotalDNSLearntIPThresholdmeasured
Object

starECSTotalDNSLearntIPv4ThresholdClear

Object ID

enterprise.8164.2.1199

Description

DNS Learnt IPv6 entries exceed the threshold limit (high water mark) configured. For IPv4 Max IP entries = 256,00.

Action to be Taken: None required. Alarm is cleared when the IPv6 entries go below the Lower Water Mark configured.

Objects

starECSTotalDNSLearntIPThresholdInstance

starECSTotalDNSLearntIPThresholdconfigured

starECSTotalDNSLearntIPThresholdmeasured
Object

starECSTotalDNSLearntIPv6Threshold

Object ID

enterprise.8164.2.1200

Description

DNS Learnt IPv4 entries reach below the threshold limit (lower water mark) configured.

Objects

starECSTotalDNSLearntIPThresholdInstance

starECSTotalDNSLearntIPThresholdconfigured

starECSTotalDNSLearntIPThresholdmeasured
Object

starECSTotalDNSLearntIPv6ThresholdClear

Object ID

enterprise.8164.2.1201

Description

DNS Learnt IPv6 entries reach below the threshold limit (lower water mark) configured.

Objects

starECSTotalDNSLearntIPThresholdInstance

starECSTotalDNSLearntIPThresholdconfigured

starECSTotalDNSLearntIPThresholdmeasured

Object

starIPSecNodeIpv6PeerDown

Object ID

enterprise.8164.2.1202

Description

A Node Service peer has stopped responding. This peer is reached using an IPv6 address. For IPv4-connected peers, a starIPSecNodePeerDown notification would be generated.

Problem Cause: The IPSec Node peer has failed, or a network connectivity problem exists.

Condition Clear Alarm: A starIPSecNodeIpv6PeerUp notification will be generated when the peer is up.

Objects

starServiceVpnName

starServiceServName

starPeerAddressIpv6
Object

starIPSecNodeIpv6PeerUp

Object ID

enterprise.8164.2.1203

Description

A Node Service peer is back online. This peer is reached using an IPv6 address. For IPv4-connected peers, a starIPSecNodePeerUp notification would be generated.

Objects

starServiceVpnName

starServiceServName

starPeerAddressIpv6
Object

starLAGGroupDown

Object ID

enterprise.8164.2.1204

Description

LAG group status is Down. This notification is only generated for master physical port and a previous 'starLAGGroupUp' notification was previously generated.

Action to be Taken: No action required. The cause for the LAG down should be investigated.

Objects

starPortSlot

starPortNum

starLAGPartner
Object

starLAGGroupUp

Object ID

enterprise.8164.2.1205

Description

LAG group status is up. This notification is only generated for master physical port.

Action to be Taken: No action required.

Objects

starPortSlot

starPortNum

starLAGPartner
Object

starVLRAssocDown

ObjectID

enterprise.8164.2.1206

Description

Probable Cause: The VLR Association has failed, or a network connectivity issue prevents reaching the VLR.

Condition Clear Alarm: A starVLRAssocUp notification will be generated when the VLR association is up.

Objects

starSGSServiceVpnName

starSGSServiceServName

starVLRName

starVLRIpAddr1
Object

starVLRAssocUp

Object ID

enterprise.8164.2.1207

Description

A VLR Association is up. This notification is only generated for Associations which have previously been declared down.

Objects

starSGSServiceVpnName

starSGSServiceServName

starVLRName

starVLRIpAddr1
Object

starVLRAllAssocDown

Object ID

enterprise.8164.2.1208

Description

All the VLR Associations are down.

Probable Cause: All the VLR Associations have failed, or network connectivity prevents reaching the VLRs.

Condition Clear Alarm: A starVLRAllAssocUp notification will be generated when all the VLR associations are up.

Objects

starSGSServiceVpnName

starSGSServiceServName
Object

starVLRAllAssocDownClear

Object ID

enterprise.8164.2.1209

Description

VLR has at least one association up. This notification is only generated for all the associations which were previously declared down.

Objects

starSGSServiceVpnName

starSGSServiceServName
Object

starEnhancedCongestion

Object ID

enterprise.8164.2.1210

Description

A congestion condition has occurred.

Probable Cause: This is the result of an operator-configured congestion threshold being reached.

This can be due to high usage of the resource being monitored which indicates that the IMG is reaching its peak capacity, or could be caused by the incorrect configuration of the congestion thresholds.

Actions to be Taken: Verify that the congestion thresholds are correct. If the congested state is seen repeatedly, or for sustained periods of time, additional system capacity may need to be brought online.This system is cleared when the use of the specific resource falls below the configured limit.

Condition Clear Alarm: A starCongestionClear notification is sent when there are no congestion conditions for a service type

Objects

starServiceType

starCongestionPolicy

starCongestionResourceType

starCongestionType

starCongestionActionProfileName
Object

starSGSNRNCNoResetAck

Object ID

enterprise.8164.2.1212

Description

SGSN has not received an Radio Network Controller(RNC) reset-ack event. This event is generated on expiry of all retransmission for RNC Reset and non-receipt of Reset-Ack

Action to be Taken: No action required.

Objects

starSessSGSNVpnName

starSessSGSNServName

starSessSGSNMcc

starSessSGSNMnc

starSessSGSNRncId
Object

starThreshSAEGWSessions.

IMPORTANT:

This was previously starSAEGWSessThreshold prior to build 45548. The “clear” notification was starSAEGWSessThresholdClear.

Object ID

enterprise.8164.2.1213

Description

The total number of SAEGW sessions is above the configured threshold value.

Probable Cause: This is a user configurable threshold. If the thresholding subsystem is configured to run in an 'alarm' model, a starThreshClearSAEGWSessions notification will be generated when the measured value falls below the threshold

Objects

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMCPUWarn

Object ID

enterprise.8164.2.1215

Description

The CPU usage is going into Warning level. This event is generated when current CPU usage reaches 90% of allocated limit.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMCPUWarnClear

Object ID

enterprise.8164.2.1216

Description

The CPU usage is coming back to normal once warned. This event is generated when current CPU usage reaches 50% of allocated limit after warning.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMMemWarn

Object ID

enterprise.8164.2.1217

Description

The Memory usage for the proclet is going in Warning level. This event is generated when current memory usage exceeds allocated limit

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMMemWarnClear

Object ID

enterprise.8164.2.1218

Description

The memory usage for the proclet is coming back to normal once warned. This event is generated when current memory usage reaches below 90% of allocated limit once warned.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMCPUOver

Object ID

enterprise.8164.2.1219

Description

The CPU usage is going into Overlaod level. This event is generated when current CPU usage reaches 50% more of allocated limit

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMCPUOverClear

Object ID

enterprise.8164.2.1220

Description

The CPU usage is back to normal level.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMMemOver

Object ID

enterprise.8164.2.1221

Description

The Memory usage of the task is going in Overload level. This event is generated when current Memory usage reached twice allocated limit.

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSGSNRMMemOverClear

Object ID

enterprise.8164.2.1222

Description

The memory usage for a proclet reached normal after overload. This event is generated when current Memory usage reaches 50% of allocated limit once overloaded

Objects

starTaskFacilityName

starTaskInstance

starTaskCard

starTaskCPU

starThreshInt

starThreshMeasuredInt
Object

starSessMgrFlowCount

Object ID

enterprise.8164.2.1223

Description

Session Manager Flows counting, This event is genereted when the number of flows in a session manager instance goes beyond configured threshold. It will also print the PDN number, memory usage, and the sess manager instance number.

Objects

starSessMgrFlowInstId

starSessMgrFlowPDNNo

starSessMgrFlowMemUsage

starSessMgrFlowCounter

starSessMgrTotalFlowCount
Object

Object ID

enterprise.8164.2.1224

Description

Clear Session Manager Flows Counting Trap, This event is genereted when the number of flows in a session manager instance goes below the configured threshold. It will also print the PDN number, memory usage, and sess manager instance number.

Objects

starSessMgrFlowInstId

starSessMgrFlowPDNNo

starSessMgrFlowMemUsage

starSessMgrFlowCounter

starSessMgrTotalFlowCount
Object

starStorageFound

Object ID

enterprise.8164.2.1225

Description

The specified storage device is found and mounted successfully on the card. This notification only generated to the storage device for which the starStorageNotFound notification was generated.

Objects

starStorage Slot

starStorage name
Object

starStorageNotFound

Object ID

enterprise.8164.2.1226

Description

The specified storage device not found on the card. This notification is currently only generated for failures to access the specified storage device on the card.

Probable Cause: The storage device is not accessible on the card.

Action to be Taken: Verify the storage device on the card is attached correctly.

Condition Clear Alarm: A starStorageFound notification will be generated when the storage device is mounted on the card.

Objects

starStorage Slot

starStorage name
Object

starHENBGWMMESCTPAssocDown

Object ID

enterprise.8164.2.1227

Description

A HENBGW MME SCTP Association is down.

Probable Cause:The HENBGW MME SCTP Association has failed, or a network connectivity prevents reaching the MME.

Condition Clear Alarm: A starHENBGWMMESCTPAssocUp notification will be generated when the HENBGW MME SCTP association is up.

Objects

starHENBGWServiceVpnName

starHENBGWServiceServName

starHENBGWServiceLogicalENBId

starHENBGWServiceMMEServName

starHENBGWServicePeerAddr

starHENBGWServicePeerPort
Object

starHENBGWMMESCTPAssocDown

Object ID

enterprise.8164.2.1228

Description

A HENBGW MME SCTP Association is up. This notification is only generated for Association which have previously been declared down, optionally this notification can be generated for any association up.

Objects

starHENBGWServiceVpnName

starHENBGWServiceServName

starHENBGWServiceLogicalENBId

starHENBGWServiceMMEServName

starHENBGWServicePeerAddr

starHENBGWServicePeerPort
Object

starHENBGWMMESCTPAllAssocDown

Object ID

enterprise.8164.2.1229

Description

All the HENBGW MME SCTP Associations are down.

Probable Cause: All the HENBGW MME SCTP Associations has failed, or network connectivity prevents reaching the MMEs.

Condition Clear Alarm: A starHENBGWMMESCTPAllAssocDownClear notification will be generated when at least one HENBGW MME SCTP association is up.

Objects

starHENBGWServiceVpnName

starHENBGWServiceServName
Object

starHENBGWMMESCTPAllAssocDownClear

Object ID

enterprise.8164.2.1230

Description

HENBGW MME SCTP at least one association is up. This notification is only generated for all the Association which have previously been declared down.

Objects

starHENBGWServiceVpnName

starHENBGWServiceServName
Object

starNPUMissedARPFrames

Object ID

enterprise.8164.2.1233

Description

This trap will be raised when NPU misses the ARP and packets route to kernel. This will print the slot number CPU number and NPU number.

Objects

starNPUSlotNumber

starNPUCPUNumber

starNPUNPUNumber
Object

starNPUMissedARPFramesClear

Object ID

enterprise.8164.2.1234

Description

This clear trap will be raised when NPU misses the ARP and packets route to kernel recovers. This will print the slot number CPU number and NPU number.

Objects

starNPUSlotNumber

starNPUCPUNumber

starNPUNPUNumber
Object

starSessMgrCSCFServiceRecoveryComplete

Object ID

enterprise.8164.2.1236

Description

Indicates that the CSCF Service had completed recovery.

This trap is generated when all the calls are recovered and the listen socket becomes active to accept packets

Objects

starServiceVpnName

starServiceServName

starTaskInstance

starCPUSlot

starCPUNumber
Object

starLIRcvryError

Object ID

enterprise.8164.2.1245

Description

"This trap will be raised when Lawful Intercepts cannot be saved or recovered to/from backup. This will print the type of error and error string.

Objects

starLIRcvryErrType

starLIRcvryErrString
Object

starLIRcvryComplete

Object ID

enterprise.8164.2.1246

Description

This trap will be raised when Lawful Intercepts are successfully recovered.

Standards-Based Traps

The following traps are defined in RFC 1157, Simple Network Management Protocol (SNMP) and are supported by the system:

- linkDown. The Interface Index for this trap is the IfIndex for the physical port, not the logical interface.
- linkUp. The Interface Index for this trap is the IfIndex for the physical port, not the logical interface.
- authenticationFailure.
- enterprisepecific.