# ACS Bandwidth Policy Configuration Mode Commands

The ACS Bandwidth Policy Configuration Mode is used to create and manage Active Charging Service (ACS) Bandwidth Policies.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
flow limit-for-bandwidth

This command allows you to configure the flow limit-for-bandwidth parameter for the current bandwidth policy.
Platform:

ASR 5000

ASR 5500
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    flow limit-for-bandwidth
    id bandwidth_id group-id group_idno flow limit-for-bandwidth
    id bandwidth_id

no

If previously configured, removes the specified flow limit-for-bandwidth configuration in the current bandwidth policy.
id bandwidth_id

Specifies ID for the current bandwidth policy.

bandwidth_id must be an integer from 1 through 65535.
group-id group_id

Specifies group ID for the current bandwidth policy.

group_id must be an integer from 1 through 65535.
Usage:

Use this command to configure the flow limit-for-bandwidth configuration for a bandwidth policy.
Example:
The following command configures the Flow Limit-for-Bandwidth configuration with bandwidth policy ID test123 and group ID 123:

    flow limit-for-bandwidth
    id test123 group-id 123

group-id

This command allows you to configure the group ID for the current bandwidth policy.
Platform:

ASR 5000

ASR 5500
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    group-id group_id direction { downlink | uplink } peak-data-rate peak_data_rate peak-burst-size peak_burst_size violate-action { discard | lower-ip-precedence } [ committed-data-rate committed_data_rate committed-burst-size committed_burst_size [ exceed-action { discard | lower-ip-precedence } ] ]{ default | no } group-id group_id direction { downlink | uplink }

default

Configures this command with default settings for the specified group ID.
no

If previously configured, removes the specified group ID configuration from the current bandwidth policy.
group_id

Specifies the group ID.

group_id must be an integer from 1 through 65535.
direction { downlink | uplink }

Specifies the direction for which bandwidth will be controlled.
peak-data-rate peak_data_rate

Specifies the peak data rate, in bits per second.

peak_data_rate must be an integer from 1 through 4294967295.

Default: 0
peak-burst-size peak_burst_size

Specifies the peak burst size, in bytes.

peak_burst_size must be an integer from 1 through 4294967295.

Default: 0
violate-action { discard | lower-ip-precedence }

Specifies the action to be taken if Peak Data Rate is surpassed.

- discard: Specifies to discard the packet
- lower-ip-precedence: Specifies to lower IP precedence of the packet

committed-data-rate committed_data_rate

Specifies the committed Data Rate, in bits per second. This can also be used to specify the Guaranteed Bit Rate (GBR) for Network Controlled QoS (NCQoS) without exceed-action.

committed_data_rate must be an integer from 1 through 4294967295.

Default: 0
committed-burst-size committed_burst_size

Specifies the committed burst size, in bytes.

committed_burst_size must be an integer from 1 through 4294967295.

Default: 0
exceed-action { discard | lower-ip-precedence }

Specifies the action to be taken if Committed Data Rate is surpassed.

- discard: Specifies to discard the packet.
- lower-ip-precedence: Specifies to lower IP precedence of the packet.

Usage:

Use this command to configure the Group ID for an bandwidth policy.
Example:
The following command configures the group ID 111 to control bandwidth in the downlink direction specifying peak data rate of 10000 bits per second and peak burst size of 10000 bytes while specifying the action to be taken on violation as discard:

    group-id 111 direction
    downlink peak-data-rate 10000 peak-burst-size 10000 violate-action discard