# show ipv6

This chapter describes the outputs of the show ipv6 command.
show ipv6 interface summary
Table 1. show ipv6 interface summary Command Output Descriptions

Field | Description
--- | ---
Intf name | Interface name
Intf Type | Interface type
Description
Router Advertisement | Displays whether the system is sending router advertisements. Options are either enabled or disabled.
IP State | Displays the IP state (UP/DOWN) and binding detail
MTU | The subscriber’s maximum transmission unit (MTU) size in octets.
IPv6 Link-Local Address: | Displays the IPv6 link-local address
IPv6 Global Unicast Address: | Displays the ipv6 Global Unicast Address address

show ipv6 neighbors
Table 2. show ipv6 neighbors Command Output Descriptions

Field | Description
--- | ---
Address | IPv6 address from table
Type | Interface type: Broadcast (Ethernet) Loopback
Link address | MAC address
Flags | One of the following flag codes: I = Incomplete R = Reachable M = Permanent S = Stale D = Delay P = Probe F = Failed
Interface | Interface name

show ipv6 route
Table 3. show ipv6 route Command Output Descriptions

Field | Description
--- | ---
Destination | Designating ipv6 address prefix/length
Next hop | Address of the directly connected next hop interface
Protocol | Connected Unconnected
Prec | Number of precedence bits set
Cost | Number of router hops to destination address
Interface | Name of the next hop interface
Total Route Count | Total number of routes Number connected Number of static routes