# ACS Group-of-Objects Configuration Mode Commands

The ACS Group-of-Objects Configuration Mode is used to configure groups of Active Charging Service (ACS) objects.

IMPORTANT:

This configuration mode is available only in 10.2 and later releases.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
member-object

This command allows you to add or remove objects from the current group-of-objects.

IMPORTANT:

A maximum of 128 objects can be added to a group-of-objects.
Platform:

ASR 5000

ASR 5500
Product:

ACS
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] member-object object

no

If previously added, removes the specified member object from the current group-of-objects.
object

Specifies the member object to add to or remove from the current group-of-objects.

object must be an alpha and/or numeric string of 1 through 63 characters.
Usage:

Use this command to add or remove member objects from a group-of-objects.
Example:
The following command adds the object test to the current group-of-objects:

    member-object test