# show operator-policy

This chapter describes the output of the show operator-policy command.
show operator-policy full name

Displays detailed configuration information for a specific operator policy configured on the system. While operator policies can be configured on SGSN, MME, and S-GW products, the information provided below only applies to SGSN.
Table 1. show operator-policy full name Command Output Descriptions

Field | Description
--- | ---
Operator Policy Name | The name of the operator policy you chose to view.
Call Control Profile Name | The name of the call control profile associated with this operator policy (only one call control profile per operator policy) or none-associated if no profile has been associated with this operator policy.
Validity | Indicates whether the profile name listed above already exists (Valid) or has not been created yet (Invalid).
APN Remap Table Name | The name of the access point name (APN) remap table associated with this operator policy (only one APN remap table per operator policy) or none-associated if no APN remap table has been associated with this operator policy.
Validity | Indicates whether the APN remap table name listed above already exists (Valid) or has not been created yet (Invalid).
IMEI Range | A range of international mobile equipment identity numbers associated with this operator policy or none-associated if no ranges have been associated with this operator policy. Up to 10 IMEI ranges can be associated with an operator policy.
IMEI Profile Name | The name of the IMEI profile associated with the IMEI number range above or none if no profile is associated with this range.
Include/Exclude | Indicates whether the IMEI range is associated with an IMEI profile (Include) or not associated with any IMEI profile (Exclude).
APN Associations | If no APN parameters are associated with this operator policy, this entry appears with the value none-associated.
APN NI
APN Profile Name | The name of the APN profile associated with the APN network identifier show above.
Validity | Indicates whether the APN profile name listed above already exists (Valid) or has not been created yet (Invalid).
APN OI
APN Profile Name | The name of the APN profile associated with the APN operator identifier show above.
Validity | Indicates whether the APN profile name listed above already exists (Valid) or has not been created yet (Invalid).
Default APN
APN Profile Name | The name of the APN profile associated with the default access point name.
Validity | Indicates whether the APN profile name listed above already exists (Valid) or has not been created yet (Invalid).