# show alarm

This chapter includes the show alarm command output tables.
show alarm outstanding all verbose
Table 1. show alarm outstanding all verbose Command Output Descriptions

Field | Description
--- | ---
Severity (Sev) | If an alarm is present, the system will indicate that one of the following alarm levels has been triggered: Minor (MN): This alarm is triggered when a high temperature is detected on a card causing the fan tray to switch to high speed. Major (MJ): This alarm is triggered on the following conditions: A hardware failure was detected on a card that will cause it to be taken off-line One of the Power Filter Units has failed or was removed. One or more of the fans on either the upper or lower fan tray have failed. Either the upper or lower fan trays have been removed. Critical (CR): This alarm is triggered when events cause a degradation in service (i.e. the system is supporting a large number of subscribers and Processing Cards are removed thus reducing the amount of available CPU and memory resources).
Object | Describes the object that triggered the alarm event
Event | Describes the event that triggered the alarm condition.
Timestamp | Lists the date and time that the alarm condition was triggered.
Alarm ID | The internal system ID of the alarm.

show alarm statistics
Table 2. show alarm statistics Command Output Descriptions

Field | Description
--- | ---
Current Outstanding Alarms | The alarm conditions that are currently active.
Cumulative Totals | The number of alarms that have occurred since the system was last booted.