# MVS Schema Statistics

The MVS (Mobile Videoscape) schema provides operational statistics that can be used for monitoring and troubleshooting the Mobile Video Gateway.
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the MVS Schema

Variables | Description | Data Type
--- | --- | ---
currflows-paced | Description: The number of current video flows paced. For video pacing. This variable is proprietary. Trigger: The charging action event increments this statistic. Availability: Video pacing, which is part of ECS (Enhanced Charging Services), generates this statistic. Type: Gauge | Int32
ttl-flows-paced | Description: The total number of video flows paced. For video pacing. This variable is proprietary. Trigger: The charging action event increments this statistic. Availability: Video pacing, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
ttl-flows-optimized | Description: The total number of TCP flows optimized. For TPO. This variable is proprietary. Trigger: This variable gets triggered when TPO is enabled on the flow. Availability: TPO, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
avrg-goodput | Description: The average goodput of optimized TCP flows in kbps. For TPO. This variable is proprietary. Trigger: This variable gets triggered when TPO is enabled on the flow. Availability: TPO, which is part of ECS (Enhanced Charging Services), generates this statistic. Type: Gauge | Int32
avrg-conn-setup-time-ms | Description: The average connection setup time of Optimized TCP flows in milliseconds. For TPO. This variable is proprietary. Trigger: This variable gets triggered when TPO is enabled on the flow. Availability: TPO, which is part of ECS (Enhanced Charging Services), generates this statistic. Type: Gauge | Int32
avrg-goodput-cong-avoid | Description: The average goodput of optimized TCP flows during congestion avoidance in kbps. For TPO. This variable is proprietary. Trigger: This variable gets triggered when TPO is enabled on the flow. Availability: TPO, which is part of ECS (Enhanced Charging Services), generates this statistic. Type: Gauge | Int32
tcplm-video-avrg-rtt-ms | Description: The average video round trip time in milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-avrg-rtt-ms | Description: The average non-video round trip time in milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-avrg-rate | Description: The average video bit rate in kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-avrg-rate | Description: The average non-video bit rate in kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-lt-50ms | Description: The number of average video round trip times less than 50 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-50-69ms | Description: The number of average video round trip times between 50 and 69 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-70-89ms | Description: The number of average video round trip times between 70 and 89 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-90-109ms | Description: The number of average video round trip times between 90 and 109 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-110-129ms | Description: The number of average video round trip times between 110 and 129 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-130-149ms | Description: The number of average video round trip times between 130 and 149 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-150-169ms | Description: The number of average video round trip times between 150 and 169 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-170-189ms | Description: The number of average video round trip times between 170 and 189 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-190-209ms | Description: The number of average video round trip times between 190 and 209 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-210-229ms | Description: The number of average video round trip times between 210 and 229 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-230-249ms | Description: The number of average video round trip times between 230 and 249 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-gteq-250ms | Description: The number of average video round trip times greater than or equal to 250 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-lt-250ms | Description: The number of average video round trip times less than 250 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-250-289ms | Description: The number of average video round trip times between 250 and 289 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-290-329ms | Description: The number of average video round trip times between 290 and 329 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-330-369ms | Description: The number of average video round trip times between 330 and 369 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-370-409ms | Description: The number of average video round trip times between 370 and 409 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-410-449ms | Description: The number of average video round trip times between 410 and 449 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-450-489ms | Description: The number of average video round trip times between 450 and 489 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-490-529ms | Description: The number of average video round trip times between 490 and 529 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-530-569ms | Description: The number of average video round trip times between 530 and 569 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-570-609ms | Description: The number of average video round trip times between 570 and 609 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-610-649ms | Description: The number of average video round trip times between 610 and 649 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-gteq-650ms | Description: The number of average video round trip times greater than or equal to 650 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-lt-650ms | Description: The number of average video round trip times less than 650 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-650-749ms | Description: The number of average video round trip times between 650 and 749 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-750-849ms | Description: The number of average video round trip times between 750 and 849 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-850-949ms | Description: The number of average video round trip times between 850 and 949 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-950-1049ms | Description: The number of average video round trip times between 950 and 1049 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-1050-1149ms | Description: The number of average video round trip times between 1050 and 1149 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-1150-1249ms | Description: The number of average video round trip times between 1150 and 1249 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-1250-1349ms | Description: The number of average video round trip times between 1250 and 1349 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-1350-1449ms | Description: The number of average video round trip times between 1350 and 1449 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-1450-1549ms | Description: The number of average video round trip times between 1450 and 1549 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-1550-1649ms | Description: The number of average video round trip times between 1550 and 1649 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rtt-gteq-1650ms | Description: The number of average video round trip times greater than or equal to 1650 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-lt-50ms | Description: The number of average non-video round trip times less than 50 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-50-69ms | Description: The number of average non-video round trip times between 50 and 69 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-70-89ms | Description: The number of average non-video round trip times between 70 and 89 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-90-109ms | Description: The number of average non-video round trip times between 90 and 109 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-110-129ms | Description: The number of average non-video round trip times between 110 and 129 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-130-149ms | Description: The number of average non-video round trip times between 130 and 149 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-150-169ms | Description: The number of average non-video round trip times between 150 and 169 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-170-189ms | Description: The number of average non-video round trip times between 170 and 189 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-190-209ms | Description: The number of average non-video round trip times between 190 and 209 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-210-229ms | Description: The number of average non-video round trip times between 210 and 229 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-230-249ms | Description: The number of average non-video round trip times between 230 and 249 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-gteq-250ms | Description: The number of average non-video round trip times greater than or equal to 250 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-lt-250ms | Description: The number of average non-video round trip times less than 250 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-250-289ms | Description: The number of average non-video round trip times between 250 and 289 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-290-329ms | Description: The number of average non-video round trip times between 290 and 329 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-330-369ms | Description: The number of average non-video round trip times between 330 and 369 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-370-409ms | Description: The number of average non-video round trip times between 370 and 409 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-410-449ms | Description: The number of average non-video round trip times between 410 and 449 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-450-489ms | Description: The number of average non-video round trip times between 450 and 489 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-490-529ms | Description: The number of average non-video round trip times between 490 and 529 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-530-569ms | Description: The number of average non-video round trip times between 530 and 569 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-570-609ms | Description: The number of average non-video round trip times between 570 and 609 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-610-649ms | Description: The number of average non-video round trip times between 610 and 649 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-gteq-650ms | Description: The number of average non-video round trip times greater than or equal to 650 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-lt-650ms | Description: The number of average non-video round trip times less than 650 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-650-749ms | Description: The number of average non-video round trip times between 650 and 749 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-750-849ms | Description: The number of average non-video round trip times between 750 and 849 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-850-949ms | Description: The number of average non-video round trip times between 850 and 949 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-950-1049ms | Description: The number of average non-video round trip times between 950 and 1049 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-1050-1149ms | Description: The number of average non-video round trip times between 1050 and 1149 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-1150-1249ms | Description: The number of average non-video round trip times between 1150 and 1249 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-1250-1349ms | Description: The number of average non-video round trip times between 1250 and 1349 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-1350-1449ms | Description: The number of average non-video round trip times between 1350 and 1449 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-1450-1549ms | Description: The number of average non-video round trip times between 1450 and 1549 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-1550-1649ms | Description: The number of average non-video round trip times between 1550 and 1649 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rtt-gteq-1650ms | Description: The number of average non-video round trip times greater than or equal to 1650 milliseconds. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-lt-20kbps | Description: The number of average video bit rates less than 20 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-20-39kbps | Description: The number of average video bit rates between 20 and 39 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-40-59kbps | Description: The number of average video bit rates between 40 and 59 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-60-79kbps | Description: The number of average video bit rates between 60 and 79 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-80-99kbps | Description: The number of average video bit rates between 80 and 99 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-100-119kbps | Description: The number of average video bit rates between 100 and 119 kbps. For TCP link monitoring. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-120-139kbps | Description: The number of average video bit rates between 120 and 139 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-140-159kbps | Description: The number of average video bit rates between 140 and 159 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-160-179kbps | Description: The number of average video bit rates between 160 and 179 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-180-199kbps | Description: The number of average video bit rates between 180 and 199 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-200-219kbps | Description: The number of average video bit rates between 200 and 219 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-gteq-220kbps | Description: The number of average video bit rates between greater than or equal to 220 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-lt-220kbps | Description: The number of average video bit rates between less than 220 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-220-259kbps | Description: The number of average video bit rates between 220 and 259 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-260-299kbps | Description: The number of average video bit rates between 260 and 299 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-300-339kbps | Description: The number of average video bit rates between 300 and 339 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-340-379kbps | Description: The number of average video bit rates between 340 and 379 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-380-419kbps | Description: The number of average video bit rates between 380 and 419 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-420-459kbps | Description: The number of average video bit rates between 420 and 459 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-460-499kbps | Description: The number of average video bit rates between 460 and 499 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-500-539kbps | Description: The number of average video bit rates between 500 and 539 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-540-579kbps | Description: The number of average video bit rates between 540 and 579 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-580-619kbps | Description: The number of average video bit rates between 580 and 619 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-gteq-620kbps | Description: The number of average video bit rates greater than or equal to 620 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-lt-620kbps | Description: The number of average video bit rates less than 620 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-620-719kbps | Description: The number of average video bit rates between 620 and 719 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-720-819kbps | Description: The number of average video bit rates between 720 and 819 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-820-919kbps | Description: The number of average video bit rates between 820 and 919 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-920-1019kbps | Description: The number of average video bit rates between 920 and 1019 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-1020-1119kbps | Description: The number of average video bit rates between 1020 and 1119 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-1120-1219kbps | Description: The number of average video bit rates between 1120 and 1219 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-1220-1319kbps | Description: The number of average video bit rates between 1220 and 1319 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-1320-1419kbps | Description: The number of average video bit rates between 1320 and 1419 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-1420-1519kbps | Description: The number of average video bit rates between 1420 and 1519 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-1520-1619kbps | Description: The number of average video bit rates between 1520 and 1619 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-video-rate-gteq-1620kbps | Description: The number of average video bit rates greater than or equal to 1620 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-lt-20kbps | Description: The number of average non-video bit rates less than 20 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-20-39kbps | Description: The number of average non-video bit rates between 20 and 39 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-40-59kbps | Description: The number of average non-video bit rates between 40 and 59 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-60-79kbps | Description: The number of average non-video bit rates between 60 and 79 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-80-99kbps | Description: The number of average non-video bit rates between 80 and 99 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-100-119kbps | Description: The number of average non-video bit rates between 100 and 119 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-120-139kbps | Description: The number of average non-video bit rates between 120 and 139 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-140-159kbps | Description: The number of average non-video bit rates between 140 and 159 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-160-179kbps | Description: The number of average non-video bit rates between 160 and 179 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-180-199kbps | Description: The number of average non-video bit rates between 180 and 199 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-200-219kbps | Description: The number of average non-video bit rates between 200 and 219 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-gteq-220kbps | Description: The number of average non-video bit rates between greater than or equal to 220 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-lt-220kbps | Description: The number of average non-video bit rates between less than 220 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-220-259kbps | Description: The number of average non-video bit rates between 220 and 259 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-260-299kbps | Description: The number of average non-video bit rates between 260 and 299 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-300-339kbps | Description: The number of average non-video bit rates between 300 and 339 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-340-379kbps | Description: The number of average non-video bit rates between 340 and 379 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-380-419kbps | Description: The number of average non-video bit rates between 380 and 419 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-420-459kbps | Description: The number of average non-video bit rates between 420 and 459 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-460-499kbps | Description: The number of average non-video bit rates between 460 and 499 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-500-539kbps | Description: The number of average non-video bit rates between 500 and 539 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-540-579kbps | Description: The number of average non-video bit rates between 540 and 579 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-580-619kbps | Description: The number of average non-video bit rates between 580 and 619 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-gteq-620kbps | Description: The number of average non-video bit rates greater than or equal to 620 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-lt-620kbps | Description: The number of average non-video bit rates less than 620 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-620-719kbps | Description: The number of average non-video bit rates between 620 and 719 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-720-819kbps | Description: The number of average non-video bit rates between 720 and 819 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-820-919kbps | Description: The number of average non-video bit rates between 820 and 919 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-920-1019kbps | Description: The number of average non-video bit rates between 920 and 1019 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-1020-1119kbps | Description: The number of average non-video bit rates between 1020 and 1119 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-1120-1219kbps | Description: The number of average non-video bit rates between 1120 and 1219 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-1220-1319kbps | Description: The number of average non-video bit rates between 1220 and 1319 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-1320-1419kbps | Description: The number of average non-video bit rates between 1320 and 1419 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-1420-1519kbps | Description: The number of average non-video bit rates between 1420 and 1519 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-1520-1619kbps | Description: The number of average non-video bit rates between 1520 and 1619 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
tcplm-nonvideo-rate-gteq-1620kbps | Description: The number of average non-video bit rates greater than or equal to 1620 kbps. For TCP link monitoring. This variable is proprietary. Trigger: This variable get triggered when TCP link monitoring is enabled and the flow is identified as a non-video flow. Availability: TCP link monitoring, which is part of ECS (Enhanced Charging Services), generates this statistic. | Int32
ttl_vbytes_mp4_ios | Description: The total video bytes for MP4 containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_mp4_android | Description: The total video bytes for MP4 containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_mp4_laptop | Description: The total video bytes for MP4 containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_mp4_unk_ue | Description: The total video bytes for MP4 containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_flv_ios | Description: The total video bytes for FLV (Flash Video) containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_flv_android | Description: The total video bytes for FLV (Flash Video) containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_flv_laptop | Description: The total video bytes for FLV (Flash Video) containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_flv_unk_ue | Description: The total video bytes for FLV (Flash Video) containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_cntnr_ios | Description: The total video bytes for other containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_cntnr _android | Description: The total video bytes for other containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_cntnr _laptop | Description: The total video bytes for other containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_cntnr _unk_ue | Description: The total video bytes for other containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_mp4_ios | Description: The total video duration for MP4 containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_mp4_android | Description: The total video duration for MP4 containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_mp4_laptop | Description: The total video duration for MP4 containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_mp4_ unk_ue | Description: The total video duration for MP4 containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_flv_ios | Description: The total video duration for FLV (Flash Video) containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_flv_android | Description: The total video duration for MP4 containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_flv_laptop | Description: The total video duration for MP4 containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_flv_unk_ue | Description: The total video duration for MP4 containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_cntnr_ios | Description: The total video duration for other containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_cntnr_android | Description: The total video duration for other containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_cntnr_laptop | Description: The total video duration for other containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_cntnr_unk_ue | Description: The total video duration for other containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_mp4_ios | Description: The total video bytes for MP4 containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_mp4_android | Description: The total video bytes for MP4 containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_mp4_laptop | Description: The total video bytes for MP4 containers for laptops. For video analytics. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_mp4_unk_ue | Description: The total video bytes for MP4 containers for other devices. For video analytics. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_flv_ios | Description: The total video bytes for FLV (Flash Video) containers for iPhone/iPad/iPod (iOS) devices. For video analytics. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_flv_android | Description: Total video bytes for MP4 containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_flv_laptop | Description: The total video bytes for MP4 containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_flv_unk_ue | Description: The total video bytes for MP4 containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_cntnr_ios | Description: The total video bytes for other containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_cntnr_android | Description: The total video bytes for other containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_cntnr_laptop | Description: The total video bytes for other containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_cntnr_unk_ue | Description: The total video bytes for other containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_mp4_ios | Description: The total videos for MP4 containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_mp4_android | Description: The total videos for MP4 containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_mp4_laptop | Description: The total videos for MP4 containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_mp4_unk_ue | Description: The total videos for MP4 containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_flv_ios | Description: The total videos for FLV (Flash Video) containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_flv_android | Description: The total videos for MP4 containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_flv_laptop | Description: The total videos for MP4 containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_flv_unk_ue | Description: The total videos for MP4 containers for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_cntnr_ios | Description: The total videos for other containers for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_cntnr_android | Description: The total videos for other containers for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_cntnr_laptop | Description: The total videos for other containers for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_cntnr_unk_ue | Description: The total videos for other container for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_gprs_ios | Description: The total video bytes for GPRS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_gprs_android | Description: The total video bytes for GPRS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_gprs_laptop | Description: The total video bytes for GPRS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_gprs_unk_ue | Description: The total video bytes for GPRS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_umts_ios | Description: The total video bytes for UMTS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_umts_android | Description: The total video bytes for UMTS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_umts_laptop | Description: The total video bytes for UMTS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_umts_unk_ue | Description: The total video bytes for UMTS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_lte_ios | Description: The total video bytes for LTE Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_lte_android | Description: The total video bytes for LTE Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_lte_laptop | Description: The total video bytes for LTE Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_lte_unk_ue | Description: The total video bytes for LTE Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_hspa_ios | Description: The total video bytes for HSPA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_hspa_android | Description: The total video bytes for HSPA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_hspa_laptop | Description: The total video bytes for HSPA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_hspa_unk_ue | Description: The total video bytes for HSPA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_wlan_ios | Description: The total video bytes for WLAN Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_wlan_android | Description: The total video bytes for WLAN Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_wlan_laptop | Description: The total video bytes for WLAN Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_wlan_unk_ue | Description: The total video bytes for WLAN Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_cdma_ios | Description: The total video bytes for CDMA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_cdma_android | Description: The total video bytes for CDMA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_cdma_laptop | Description: The total video bytes for CDMA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_cdma_unk_ue | Description: The total video bytes for CDMA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_rat_ios | Description: The total video bytes for other Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_rat_android | Description: The total video bytes for other Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_rat_laptop | Description: The total video bytes for other Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vbytes_unk_rat_unk_ue | Description: The total video bytes for other Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_gprs_ios | Description: The total video duration for GPRS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_gprs_android | Description: The total video duration for GPRS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_gprs_laptop | Description: The total video duration for GPRS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_gprs_unk_ue | Description: The total video duration for GPRS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_umts_ios | Description: The total video duration for UMTS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_umts_android | Description: The total video duration for UMTS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_umts_laptop | Description: The total video duration for UMTS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_umts_unk_ue | Description: The total video duration for UMTS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_lte_ios | Description: The total video duration for LTE Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_lte_android | Description: The total video duration for LTE Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_lte_laptop | Description: The total video duration for LTE Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_lte_unk_ue | Description: The total video duration for LTE Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_hspa_ios | Description: The total video duration for HSPA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_hspa_android | Description: The total video duration for HSPA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_hspa_laptop | Description: The total video duration for HSPA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_hspa_unk_ue | Description: The total video duration for HSPA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_wlan_ios | Description: The total video duration for WLAN Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_wlan_android | Description: The total video duration for WLAN Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_wlan_laptop | Description: The total video duration for WLAN Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_wlan_unk_ue | Description: The total video duration for WLAN Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_cdma_ios | Description: The total video duration for CDMA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_cdma_android | Description: The total video duration for CDMA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_cdma_laptop | Description: The total video duration for CDMA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_cdma_unk_ue | Description: The total video duration for CDMA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_rat_ios | Description: The total video duration for other Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_rat_android | Description: The total video duration for other Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_rat_laptop | Description: The total video duration for other Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_vduration_unk_rat_unk_ue | Description: The total video duration for other Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_gprs_ios | Description: The total video bytes sent for GPRS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_gprs_android | Description: The total video bytes sent for GPRS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_gprs_laptop | Description: The total video bytes sent for GPRS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_gprs_unk_ue | Description: The total video bytes sent for GPRS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_umts_ios | Description: The total video bytes sent for UMTS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_umts_android | Description: The total video bytes sent for UMTS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_umts_laptop | Description: The total video bytes sent for UMTS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_umts_unk_ue | Description: The total video bytes sent for UMTS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_lte_ios | Description: The total video bytes sent for LTE Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_lte_android | Description: The total video bytes sent for LTE Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_lte_laptop | Description: The total video bytes sent for LTE Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_lte_unk_ue | Description: The total video bytes sent for LTE Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_hspa_ios | Description: The total video bytes sent for HSPA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_hspa_android | Description: The total video bytes sent for HSPA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_hspa_laptop | Description: The total video bytes sent for HSPA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_hspa_unk_ue | Description: The total video bytes sent for HSPA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_wlan_ios | Description: The total video bytes sent for WLAN Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_wlan_android | Description: The total video bytes sent for WLAN Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_wlan_laptop | Description: The total video bytes sent for WLAN Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_wlan_unk_ue | Description: The total video bytes sent for WLAN Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_cdma_ios | Description: The total video bytes sent for CDMA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_cdma_android | Description: The total video bytes sent for CDMA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_cdma_laptop | Description: The total video bytes sent for CDMA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_cdma_unk_ue | Description: The total video bytes sent for CDMA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_rat_ios | Description: The total video bytes sent for other Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_rat_android | Description: The total video bytes sent for other Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_rat_laptop | Description: The total video bytes sent for other Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_txbytes_unk_rat_unk_ue | Description: The total video bytes sent for other Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_gprs_ios | Description: The total video sessions on time for GPRS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_gprs_android | Description: The total video sessions on time for GPRS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_gprs_laptop | Description: The total video sessions on time for GPRS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_gprs_unk_ue | Description: The total video sessions on time for GPRS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_umts_ios | Description: The total video sessions on time for UMTS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_umts_android | Description: The total video sessions on time for UMTS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_umts_laptop | Description: The total video sessions on time for UMTS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_umts_unk_ue | Description: The total video sessions on time for UMTS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_lte_ios | Description: The total video sessions on time for LTE Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_lte_android | Description: The total video sessions on time for LTE Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_lte_laptop | Description: The total video sessions on time for LTE Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_lte_unk_ue | Description: The total video sessions on time for LTE Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_hspa_ios | Description: The total video sessions on time for HSPA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_hspa_android | Description: The total video sessions on time for HSPA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_hspa_laptop | Description: The total video sessions on time for HSPA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_hspa_unk_ue | Description: The total video sessions on time for HSPA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_wlan_ios | Description: The total video sessions on time for WLAN Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_wlan_android | Description: The total video sessions on time for WLAN Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_wlan_laptop | Description: The total video sessions on time for WLAN Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_wlan_unk_ue | Description: The total video sessions on time for WLAN Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_cdma_ios | Description: The total video sessions on time for CDMA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_cdma_android | Description: The total video sessions on time for CDMA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_cdma_laptop | Description: The total video sessions on time for CDMA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_cdma_unk_ue | Description: The total video sessions on time for CDMA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_unk_rat_ios | Description: The total video sessions on time for other Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_unk_rat_android | Description: The total video sessions on time for other Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_unk_rat_laptop | Description: The total video sessions on time for other Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_session_time_unk_rat_unk_ue | Description: The total video sessions on time for other Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_gprs_ios | Description: The total TCP video flow count for GPRS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_gprs_android | Description: The total TCP video flow count for GPRS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_gprs_laptop | Description: The total TCP video flow count for GPRS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_gprs_unk_ue | Description: The total TCP video flow count for GPRS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_umts_ios | Description: The total TCP video flow count for UMTS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_umts_android | Description: The total TCP video flow count for UMTS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_umts_laptop | Description: The total TCP video flow count for UMTS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_umts_unk_ue | Description: The total TCP video flow count for UMTS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_lte_ios | Description: The total TCP video flow count for LTE Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_lte_android | Description: The total TCP video flow count for LTE Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_lte_laptop | Description: The total TCP video flow count for LTE Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_lte_unk_ue | Description: The total TCP video flow count for LTE Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_hspa_ios | Description: The total TCP video flow count for HSPA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_hspa_android | Description: The total TCP video flow count for HSPA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_hspa_laptop | Description: The total TCP video flow count for HSPA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_hspa_unk_ue | Description: The total TCP video flow count for HSPA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_wlan_ios | Description: The total TCP video flow count for WLAN Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_wlan_android | Description: The total TCP video flow count for WLAN Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_wlan_laptop | Description: The total TCP video flow count for WLAN Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_wlan_unk_ue | Description: The total TCP video flow count for WLAN Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_cdma_ios | Description: The total TCP video flow count for CDMA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_cdma_android | Description: The total TCP video flow count for CDMA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_cdma_laptop | Description: The total TCP video flow count for CDMA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_cdma_unk_ue | Description: The total TCP video flow count for CDMA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_unk_rat_ios | Description: The total TCP video flow count for other Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_unk_rat_android | Description: The total TCP video flow count for other Radio Access Type for Android devices. For video analytics. This variable is proprietary. | Int64
ttl_video_tcp_flow_unk_rat_laptop | Description: The total TCP video flow count for other Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_tcp_flow_unk_rat_unk_ue | Description: The total TCP video flow count for other Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_gprs_ios | Description: The total video object count for GPRS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_gprs_android | Description: The total video object count for GPRS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_gprs_laptop | Description: The total video object count for GPRS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_gprs_unk_ue | Description: The total video object count for GPRS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_umts_ios | Description: The total video object count for UMTS Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_umts_android | Description: The total video object count for UMTS Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_umts_laptop | Description: The total video object count for UMTS Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_umts_unk_ue | Description: The total video object count for UMTS Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_lte_ios | Description: The total video object count for LTE Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_lte_android | Description: The total video object count for LTE Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_lte_laptop | Description: The total video object count for LTE Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_lte_unk_ue | Description: The total video object count for LTE Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_hspa_ios | Description: The total video object count for HSPA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_hspa_android | Description: The total video object count for HSPA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_hspa_laptop | Description: The total video object count for HSPA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_hspa_unk_ue | Description: The total video object count for HSPA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_wlan_ios | Description: The total video object count for WLAN Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_wlan_android | Description: The total video object count for WLAN Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_wlan_laptop | Description: The total video object count for WLAN Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_wlan_unk_ue | Description: The total video object count for WLAN Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_cdma_ios | Description: The total video object count for CDMA Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_cdma_android | Description: The total video object count for CDMA Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_cdma_laptop | Description: The total video object count for CDMA Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_cdma_unk_ue | Description: The total video object count for CDMA Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_rat_ios | Description: The total video object count for other Radio Access Type for iPhone/iPad/iPod (iOS) devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_rat_android | Description: The total video object count for other Radio Access Type for Android devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_rat_laptop | Description: The total video object count for other Radio Access Type for laptops. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
ttl_video_count_unk_rat_unk_ue | Description: The total video object count for other Radio Access Type for other devices. For video analytics. This variable is proprietary. Trigger: This variable get triggered for each downloaded video when the video information is timed out from the MVG cache. Availability: Video analytics generates this statistic. | Int64
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.