# show fa-service

Table 1. show fa-service name Command Output Descriptions

Field | Description
--- | ---
Service name | The name of the FA service for which the information are displayed.
Context | The name of the context in which this service is configured.
Bind | Status of connectivity of this service with context and IP address.
Max Subscribers | The number of subscribers are allowed to configure in this service.
Local IP Address | IP address to which this service is bound and communicate with HA.
Local IP Port | The port number on which this service is to communicate with HA.
Lifetime | The maximum time that the FA session can exist before it becomes expired.
Registration Timeout | The maximum duration of inactivity for a session registration before it becomes expired.
Advt Lifetime | Lifetime for an advertisement message.
Advt Interval | Interval between two advertisement messages.
Num Advt | The total number of advertisement messages broadcasted.
Advt Prefix Length Extn | Indicates the setting of prefix extension length in advertisement message.
Reverse Tunnel | Status of reverse tunnel.
GRE Encapsulation | Status of Generic Routing Encapsulation (GRE).
Optimize Tunnel Reassembly | Status of tunnel reassembly optimization.
Allow Priv Addr w/o Rev Tunnel | Status of setting to allow private addresses without reverse tunnelling.
Dynamic MIP Key Update | Status of setting to update dynamic MIP key.
Ignore Dynamic MIP Key | Status of setting to ignore dynamic MIP keys.
Remove MN-AAA/MN-FAC extns | Status of setting to remove MN-AAA and/or MN-FA extensions from messages.
Standalone FA service | Show the standalone FA service status. If “Enabled” system performs as a standalone FA only.
Proxy MIP | Status of Proxy Mobile IP support.
Proxy MIP Max Retransmissions | Total number of retransmission for Proxy Mobile IP support.
Proxy MIP Retrans Timeout | Timeout duration in seconds between two of retransmissions for Proxy MIP support.
Proxy MIP Renew Percent Time: | Percentage of timeout duration. Once this much percent of timeout duration exhausted the Proxy MIP message will be retransmitted. For example, If retransmission timeout is set for 4 secs. and renew percent time is configured for 75%, the Proxy MIP messages will be retransmitted after 3 seconds.
SPI(s) | The configured Security Parameter Index (SPI) number between FA and HA.
FAHA
Remote Addr | IP address of HA.
Hash Algorithm: | Hashing algorithm applicable for HA.
SPI Num | SPI number set for HA.
Replay Protection: | Type of reply protection enabled for reply messages.
Timestamp Tolerance | Total variation allowed in timestamp mismatch.
HA Monitoring: | Status of HA monitoring configuration.
GRE Sequence Numbers | Status of GRE sequence number setting in messages.
GRE Sequence Mode | Specifies the GRE sequence mode.
GRE reorder Timeout | Total timeout duration for GRE reorder.
GRE Checksum | Status of GRE Checksum setting in messages.
GRE Checksum Verification | Status of GRE Checksum verification setting.
Registration Revocation | Status of registration revocation setting.
Reg-Revocation I Bit | Status of I-bit setting for registration revocation.
Reg-Revocation Max Retries | Maximum number of retries allowed for registration revocation.
Reg-Revocation Timeout | Total duration allowed between two retries for registration revocation.
Reg-Rev on InternalFailure | Specifies whether registration revocation will be triggered on internal failure or not.
Default Subscriber | Name of the default subscriber.
Max sessions | Maximum number of subscriber sessions allowed.
Max challenge len | Length of challenge key for subscriber authentication.
Challenge Window | total number of windows opened for challenge.
Service Status | Status of this service.
MN-AAA Auth Policy | Specifies the lookup criteria for authentication policy between MN and AAA in RRP. Possible settings are: alwaysignore-after-handoffinit-reginit-reg-except-handoffrenew-and-dereg-noauthrenew-reg-noauth
Optimize-Retries | Status of setting for optimized retries when authentication policy is not received for MN and AAA.
MN-HA Auth Policy | Specifies the lookup criteria for authentication policy between MN and HA in RRP.
AAA Distributed MIP Keys Override | Specifies the setting for the FA service to override dynamic keys from AAA with static keys to support MIP registration with HAs which do not support dynamic keys.
Newcall Policy | Specify that new call policy enabled or disabled to handle new calls.
Idle Timeout Mode | Idle timeout mode allowed for this service.
Ignore Stale Challenge | Status of setting to ignore old/stale challenge messages.
Limit Reg Lifetime | Status of setting to limit registration lifetime.
Dynamic HA Failover | Status of setting to handle dynamic HA failovers.
AAA HA override | Status of setting to override HA settings if received from AAA.
HA Failover | Status of setting to handle HA failovers.
Retrans Timeout | Timeout duration between two retransmission of probe on HA failover.
Retries Before Swtichover | Total number of retries before switching to another HA.
Maximum retries | Total number of retries allowed.
Load Balance | Status of setting to handle HA performance issues or HAa failovers by load balancing.
HA Monitoring | Status of setting to monitor HA.
Inactivity Timeout | Timeout duration after which a probe message will be sent to HA.
Monitor Reply Timeout | Timeout duration to wait for reply from HA after which a probe message will be resent to HA.
Maximum retries | Total number of retries allowed.