# APN Schema Statistics

The APN schema provides operational statistics that can be used for monitoring and troubleshooting the following products: GGSN, P-GW.
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistics Variables in the APN Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the APN configuration. This is a key variable. Type: Information | String
vpnid | The identification number of the context configured on the system that is currently facilitating the APN configuration. This is an internal reference number. This is a key variable. Type: Information | Int32
apn | The name of the APN for which statistics are displayed. This is a key variable. Type: Information | String
uplnk-bytes | The number of bytes sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int64
dnlnk-bytes | The number of bytes sent from the APN towards MS on the GTP interface. Type: Counter | Int64
uplnk-pkts | The number of IP packets sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
dnlnk-pkts | The number of IP packets sent from the APN towards MS on the GTP interface. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
uplnk-bytes-drop | The number of bytes sent from the APN towards Internet/PDN on the Gi interface dropped. Type: Counter | Int64
dnlnk-bytes-drop | The number of bytes sent from the APN towards MS on the GTP interface dropped. Type: Counter | Int64
uplnk-drop | The number of IP packets sent from the APN towards Internet/PDN on the Gi interface dropped. Type: Counter | Int32
dnlnk-drop | The number of IP packets sent from the APN towards MS on the GTP interface dropped. Type: Counter | Int32
bad-hdr | The total number of IP packets received and dropped due to bad header. Type: Counter | Int32
ttl-excd | The number of IP packets dropped because they were received with a TTL value of 0. Type: Counter | Int32
frag-sent | The number of times IP packets were fragmented before sending on the GTP tunnel. Type: Counter | Int32
frag-fail | The number of packets which failed in fragmentation. Type: Counter | Int32
inacl-drop | The number of IP packets received that were dropped due to ACL filtering. Type: Counter | Int32
outacl-drop | The number of outbound IP packets that were dropped due to ACL filtering. Type: Counter | Int32
inexcd-mbr-pkt-drop | Data Statistics – IP input excd MBR packets dropped Type: Counter | Int32
outexcd-mbr-pkt-drop | Data Statistics – IP output excd MBR packets dropped Type: Counter | Int32
inexcd-gbr-pkt-drop | Data Statistics – IP input excd GBR packets dropped Type: Counter | Int32
outexcd-gbr-pkt-drop | Data Statistics – IP output excd GBR packets dropped Type: Counter | Int32
inexcd-ambr-pkt-drop | Data Statistics – IP in excd APN packets AMBR dropped Type: Counter | Int32
outexcd-ambr-pkt-drop | Data Statistics – IP out excd APN packets AMBR dropped Type: Counter | Int32
inmisc-pkt-drop | Data Statistics – IP input misc packets dropped Type: Counter | Int32
outmisc-pkt-drop | Data Statistics – IP output misc packets dropped Type: Counter | Int32
inexcd-mbr-byte-drop | Data Statistics – IP input excd MBR bytes dropped Type: Counter | Int32
outexcd-mbr-byte-drop | Data Statistics – IP output excd MBR bytes dropped Type: Counter | Int32
inexcd-gbr-byte-drop | Data Statistics – IP input excd GBR bytes dropped Type: Counter | Int32
outexcd-gbr-byte-drop | Data Statistics – IP output excd GBR bytes dropped Type: Counter | Int32
inexcd-ambr-byte-drop | Data Statistics – IP in excd APN AMBR bytes dropped Type: Counter | Int32
outexcd-ambr-byte-drop | Data Statistics – IP out excd APN AMBR bytes dropped Type: Counter | Int32
inmisc-byte-drop | Data Statistics – IP input misc bytes dropped Type: Counter | Int32
outmisc-byte-drop | Data Statistics – IP output misc bytes dropped Type: Counter | Int32
bad-src-addr | The number of IP packets received for which a source violation was detected resulting in the packets being dropped. Type: Counter | Int32
addr-stat | The total number of PDP contexts facilitated by the APN that used static IP addresses. Type: Counter | Int32
addr-lpool | The total number of PDP contexts facilitated by the APN that were allocated IP addresses from pools configured locally. Type: Counter | Int32
addr-rad | The total number of PDP contexts facilitated by the APN that were allocated IP addresses from a RADIUS server. Type: Counter | Int32
addr-dhcp | The total number of PDP contexts facilitated by the APN that were allocated IP addresses from DHCP. Type: Counter | Int32
addr-dhcp-rly | The total number of PDP contexts facilitated by the APN that were allocated IP addresses by DHCP Relay. Type: Counter | Int32
addr-no-alloc | The total number of PDP contexts facilitated by the APN that were not allocated IP addresses. Type: Counter | Int32
sess-curr | The number of PDP contests currently facilitated by the APN. Type: Gauge | Int32
sess-curr-all | The total number of PDP contexts currently being facilitated by the entire system. Type: Gauge | Int32
sess-tot | The total number of PDP contexts facilitated by the APN. Type: Counter | Int32
sess-tot-all | The total number of PDP contexts that have been facilitated by the entire system. Type: Counter | Int32
att-pdp-ctxt | The total CPC req per APN Type: Counter | Int32
att-deact-pdp-ggsn | The total DPC Req Tx per APN Type: Counter | Int32
succ-deact-pdp-ggsn | The total DPC Req Tx Accepted Type: Counter | Int32
att-deact-pdp-ms | The total DPC Req Rx per APN Type: Counter | Int32
succ-deact-pdp-ms | The total Deactivate PDP Context Req successful from MS. Type: Counter | Int32
dyn-ipv4-attempt | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were attempted. Type: Counter | Int32
dyn-ipv6-attempt | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were attempted. Type: Counter | Int32
dyn-ipv4-success | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. Type: Counter | Int32
dyn-ipv6-success | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. Type: Counter | Int32
data-fromuseravg-bps | The sum of average data rate in bits per seconds (bps) from all the users under this VPN. Type: Gauge | Int64
data-touseravg-bps | The sum of average data rate in bps towards all the users under this VPN. Type: Gauge | Int64
data-fromusersust-bps | The sustained data rate in bps from the user. Type: Gauge | Int64
data-tousersust-bps | The sustained data rate in bps towards the user. Type: Gauge | Int64
data-fromuseravg-pps | The average data rate in packets per seconds (pps) from the user. Type: Gauge | Int64
data-touseravg-pps | The average data rate in pps towards the user. Type: Gauge | Int64
data-fromusersust-pps | The sustained data rate in pps from the user. Type: Gauge | Int64
data-tousersust-pps | The sustained data rate in pps towards the user. Type: Gauge | Int64
qosconv-pkts-uplnk | The number of packets with Conversational QoS sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int32
qosconv-pkts-dnlnk | The number of packets with Conversational QoS sent from the APN towards MS on the GTP interface. Type: Counter | Int32
qosstrm-pkts-uplnk | The number of packets with Streaming QoS sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int32
qosstrm-pkts-dnlnk | The number of packets with Streaming QoS sent from the APN towards MS on the GTP interface. Type: Counter | Int32
qosint1-pkts-uplnk | The number of packets with Interactive QoS for priority 1 sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int32
qosint1-pkts-dnlnk | The number of packets with Interactive QoS for priority 1 sent from the APN towards MS on the GTP interface. Type: Counter | Int32
qosint2-pkts-uplnk | The number of packets with Interactive QoS for priority 2 sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int32
qosint2-pkts-dnlnk | The number of packets with Interactive QoS for priority 2 sent from the APN towards MS on the GTP interface. Type: Counter | Int32
qosint3-pkts-uplnk | The number of packets with Interactive QoS for priority 3 sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int32
qosint3-pkts-dnlnk | The number of packets with Interactive QoS for priority 3 sent from the APN towards MS on the GTP interface. Type: Counter | Int32
qosint-pkts-uplnk | Total number of packets with Interactive QoS for all priorities (priority 1, 2, and 3) sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int32
qosint-pkts-dnlnk | Total number of packets with Interactive QoS for all priorities (priority 1, 2, and 3) sent from the APN towards MS on the GTP interface. Type: Counter | Int32
qosback-pkts-uplnk | The number of packets with Background QoS sent from the APN towards Internet/PDN on the Gi interface. Type: Counter | Int32
qosback-pkts-dnlnk | The number of packets with Background QoS sent from the APN towards MS on the GTP interface. Type: Counter | Int32
auth-req-sent | The total authentication requests sent from the APN towards AAA on Ga interface. Type: Counter | Int32
auth-acc-rcvd | The total authentication accept messages received by the APN on Ga Interface from AAA. Type: Counter | Int32
auth-timeout | The total authentication requests that timed out. Type: Counter | Int32
acc-req-sent | The total accounting requests sent from the APN towards AAA on Ga interface. Type: Counter | Int32
acc-rsp-rcvd | The total accounting response messages received by the APN on Ga Interface from AAA. Type: Counter | Int32
acc-req-timeout | The total accounting requests that timed out. Type: Counter | Int32
act-defbear | The total number of active default bearers. Type: Gauge | Int32
act-dedbear | The total number of active dedicated bearers. Type: Gauge | Int32
setup-defbear | The total number of default bearers setup. Type: Counter | Int32
setup-dedbear | The total number of dedicated bearers setup. Type: Counter | Int32
rel-defbear | The total number of released default bearers. Type: Counter | Int32
rel-dedbear | The total number of released dedicated bearers. Type: Counter | Int32
rel-fail-defbear | The total number of default bearers with release failures. Type: Counter | Int32
rel-fail-dedbear | The total number of dedicated bearers with release failures. Type: Counter | Int32
rej-defbear | The total number of rejected default bearers. Type: Counter | Int32
rej-dedbear | The total number of rejected dedicated bearers. Type: Counter | Int32
mod-uebear | The total number of UE-initiated modified bearers. Type: Counter | Int32
mod-nwbear | The total number of network-initiated modified bearers. Type: Counter | Int32
ue-init-modfail | The total number of failed UE-initiated modified bearers. Type: Counter | Int32
nw-init-modfail | The total number of failed network-initiated modified bearers. Type: Counter | Int32
pdn-ipv4-actsess | The total number of active IPv4 sessions. Type: Gauge | Int32
pdn-ipv4-setupsess | The total number of IPv4 session setup. Type: Counter | Int32
pdn-ipv4-relsess | The total number of released IPv4 sessions. Type: Counter | Int32
pdn-ipv6-actsess | The total number of active IPv6 sessions. Type: Gauge | Int32
pdn-ipv6-setupsess | The total number of IPv6 session setup. Type: Counter | Int32
pdn-ipv6-relsess | The total number of released IPv6 sessions. Type: Counter | Int32
pdn-ipv4v6-actsess | The total number of active IPv4-in-IPv6 sessions. Type: Gauge | Int32
pdn-ipv4v6-setupsess | The total number of IPv4-in-IPv6 session setup. Type: Counter | Int32
pdn-ipv4v6-relsess | The total number of released IPv4-in-IPv6 sessions. Type: Counter | Int32
addr-ipv6-stateless-autocnf | The total number of allocated IPv6 addresses from stateless auto-configuration. Type: Counter | Int32
qci1-actbear | The total number of QCI1 active bearers. Type: Gauge | Int32
qci1-setupbear | The total number of QCI1 bearers setup. Type: Counter | Int32
qci1-relbear | The total number of QCI1 released bearers. Type: Counter | Int32
qci1-uplinkpkt-fwd | The total number of QCI1 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci1-dwlinkpkt-fwd | The total number of QCI1 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci1-uplinkbyte-fwd | The total number of QCI1 uplink bytes forwarded. Type: Counter | Int64
qci1-dwlinkbyte-fwd | The total number of QCI1 downlink bytes forwarded. Type: Counter | Int64
qci1-uplinkpkt-drop | The total number of QCI1 uplink packets dropped. Type: Counter | Int32
qci1-dwlinkpkt-drop | The total number of QCI1 downlink packets dropped. Type: Counter | Int32
qci1-uplinkbyte-drop | The total number of QCI1 uplink bytes dropped. Type: Counter | Int64
qci1-dwlinkbyte-drop | The total number of QCI1 downlink bytes dropped. Type: Counter | Int64
qci2-actbear | The total number of QCI2 active bearers. Type: Gauge | Int32
qci2-setupbear | The total number of QCI2 bearers setup. Type: Counter | Int32
qci2-relbear | The total number of QCI2 released bearers. Type: Counter | Int32
qci2-uplinkpkt-fwd | The total number of QCI2 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci2-dwlinkpkt-fwd | The total number of QCI2 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci2-uplinkbyte-fwd | The total number of QCI2 uplink bytes forwarded. Type: Counter | Int64
qci2-dwlinkbyte-fwd | The total number of QCI2 downlink bytes forwarded. Type: Counter | Int64
qci2-uplinkpkt-drop | The total number of QCI2 uplink packets dropped. Type: Counter | Int32
qci2-dwlinkpkt-drop | The total number of QCI2 downlink packets dropped. Type: Counter | Int32
qci2-uplinkbyte-drop | The total number of QCI2 uplink bytes dropped. Type: Counter | Int64
qci2-dwlinkbyte-drop | The total number of QCI2 downlink bytes dropped. Type: Counter | Int64
qci3-actbear | The total number of QCI3 active bearers. Type: Gauge | Int32
qci3-setupbear | The total number of QCI3 bearers setup. Type: Counter | Int32
qci3-relbear | The total number of QCI3 released bearers. Type: Counter | Int32
qci3-uplinkpkt-fwd | The total number of QCI3 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci3-dwlinkpkt-fwd | The total number of QCI3 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci3-uplinkbyte-fwd | The total number of QCI3 uplink bytes forwarded. Type: Counter | Int64
qci3-dwlinkbyte-fwd | The total number of QCI3 downlink bytes forwarded. Type: Counter | Int64
qci3-uplinkpkt-drop | The total number of QCI3 uplink packets dropped. Type: Counter | Int32
qci3-dwlinkpkt-drop | The total number of QCI3 downlink packets dropped. Type: Counter | Int32
qci3-uplinkbyte-drop | The total number of QCI3 uplink bytes dropped. Type: Counter | Int64
qci3-dwlinkbyte-drop | The total number of QCI3 downlink bytes dropped. Type: Counter | Int64
qci4-actbear | The total number of QCI4 active bearers. Type: Gauge | Int32
qci4-setupbear | The total number of QCI4 bearers setup. Type: Counter | Int32
qci4-relbear | The total number of QCI4 released bearers. Type: Counter | Int32
qci4-uplinkpkt-fwd | The total number of QCI4 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci4-dwlinkpkt-fwd | The total number of QCI4 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci4-uplinkbyte-fwd | The total number of QCI4 uplink bytes forwarded. Type: Counter | Int64
qci4-dwlinkbyte-fwd | The total number of QCI4 downlink bytes forwarded. Type: Counter | Int64
qci4-uplinkpkt-drop | The total number of QCI4 uplink packets dropped. Type: Counter | Int32
qci4-dwlinkpkt-drop | The total number of QCI4 downlink packets dropped. Type: Counter | Int32
qci4-uplinkbyte-drop | The total number of QCI4 uplink bytes dropped. Type: Counter | Int64
qci4-dwlinkbyte-drop | The total number of QCI4 downlink bytes dropped. Type: Counter | Int64
qci5-actbear | The total number of QCI5 active bearers. Type: Gauge | Int32
qci5-setupbear | The total number of QCI5 bearers setup. Type: Counter | Int32
qci5-relbear | The total number of QCI5 released bearers. Type: Counter | Int32
qci5-uplinkpkt-fwd | The total number of QCI5 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci5-dwlinkpkt-fwd | The total number of QCI5 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci5-uplinkbyte-fwd | The total number of QCI5 uplink bytes forwarded. Type: Counter | Int64
qci5-dwlinkbyte-fwd | The total number of QCI5 downlink bytes forwarded. Type: Counter | Int64
qci5-uplinkpkt-drop | The total number of QCI5 uplink packets dropped. Type: Counter | Int32
qci5-dwlinkpkt-drop | The total number of QCI5 downlink packets dropped. Type: Counter | Int32
qci5-uplinkbyte-drop | The total number of QCI5 uplink bytes dropped. Type: Counter | Int64
qci5-dwlinkbyte-drop | The total number of QCI5 downlink bytes dropped. Type: Counter | Int64
qci6-actbear | The total number of QCI6 active bearers. Type: Gauge | Int32
qci6-setupbear | The total number of QCI6 bearers setup. Type: Counter | Int32
qci6-relbear | The total number of QCI6 released bearers. Type: Counter | Int32
qci6-uplinkpkt-fwd | The total number of QCI6 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci6-dwlinkpkt-fwd | The total number of QCI6 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci6-uplinkbyte-fwd | The total number of QCI6 uplink bytes forwarded. Type: Counter | Int64
qci6-dwlinkbyte-fwd | The total number of QCI6 downlink bytes forwarded. Type: Counter | Int64
qci6-uplinkpkt-drop | The total number of QCI6 uplink packets dropped. Type: Counter | Int32
qci6-dwlinkpkt-drop | The total number of QCI6 downlink packets dropped. Type: Counter | Int32
qci6-uplinkbyte-drop | The total number of QCI6 uplink bytes dropped. Type: Counter | Int64
qci6-dwlinkbyte-drop | The total number of QCI6 downlink bytes dropped. Type: Counter | Int64
qci7-actbear | The total number of QCI7 active bearers. Type: Gauge | Int32
qci7-setupbear | The total number of QCI7 bearers setup. Type: Counter | Int32
qci7-relbear | The total number of QCI7 released bearers. Type: Counter | Int32
qci7-uplinkpkt-fwd | The total number of QCI7 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci7-dwlinkpkt-fwd | The total number of QCI7 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci7-uplinkbyte-fwd | The total number of QCI7 uplink bytes forwarded. Type: Counter | Int64
qci7-dwlinkbyte-fwd | The total number of QCI7 downlink bytes forwarded. Type: Counter | Int64
qci7-uplinkpkt-drop | The total number of QCI7 uplink packets dropped. Type: Counter | Int32
qci7-dwlinkpkt-drop | The total number of QCI7 downlink packets dropped. Type: Counter | Int32
qci7-uplinkbyte-drop | The total number of QCI7 uplink bytes dropped. Type: Counter | Int64
qci7-dwlinkbyte-drop | The total number of QCI7 downlink bytes dropped. Type: Counter | Int64
qci8-actbear | The total number of QCI8 active bearers. Type: Gauge | Int32
qci8-setupbear | The total number of QCI8 bearers setup. Type: Counter | Int32
qci8-relbear | The total number of QCI8 released bearers. Type: Counter | Int32
qci8-uplinkpkt-fwd | The total number of QCI8 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci8-dwlinkpkt-fwd | The total number of QCI8 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci8-uplinkbyte-fwd | The total number of QCI8 uplink bytes forwarded. Type: Counter | Int64
qci8-dwlinkbyte-fwd | The total number of QCI8 downlink bytes forwarded. Type: Counter | Int64
qci8-uplinkpkt-drop | The total number of QCI8 uplink packets dropped. Type: Counter | Int32
qci8-dwlinkpkt-drop | The total number of QCI8 downlink packets dropped. Type: Counter | Int32
qci8-uplinkbyte-drop | The total number of QCI8 uplink bytes dropped. Type: Counter | Int64
qci8-dwlinkbyte-drop | The total number of QCI8 downlink bytes dropped. Type: Counter | Int64
qci9-actbear | The total number of QCI9 active bearers. Type: Gauge | Int32
qci9-setupbear | The total number of QCI9 bearers setup. Type: Counter | Int32
qci9-relbear | The total number of QCI9 released bearers. Type: Counter | Int32
qci9-uplinkpkt-fwd | The total number of QCI9 uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci9-dwlinkpkt-fwd | The total number of QCI9 downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
qci9-uplinkbyte-fwd | The total number of QCI9 uplink bytes forwarded. Type: Counter | Int64
qci9-dwlinkbyte-fwd | The total number of QCI9 downlink bytes forwarded. Type: Counter | Int64
qci9-uplinkpkt-drop | The total number of QCI9 uplink packets dropped. Type: Counter | Int32
qci9-dwlinkpkt-drop | The total number of QCI9 downlink packets dropped. Type: Counter | Int32
qci9-uplinkbyte-drop | The total number of QCI9 uplink bytes dropped. Type: Counter | Int64
qci9-dwlinkbyte-drop | The total number of QCI9 downlink bytes dropped. Type: Counter | Int64
nonstdqci-nongbr-actbear | The total number of non-standard QCI, non-GBR active bearers. Type: Gauge | Int32
nonstdqci-nongbr-setupbear | The total number of non-standard QCI, non-GBR bearers setup. Type: Counter | Int32
nonstdqci-nongbr-relbear | The total number of non-standard QCI, non-GBR released bearers. Type: Counter | Int32
nonstdqci-nongbr-uplinkpkt-fwd | The total number of non-standard QCI, non-GBR uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
nonstdqci-nongbr-dwlinkpkt-fwd | The total number of non-standard QCI, non-GBR downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
nonstdqci-nongbr-uplinkbyte-fwd | The total number of non-standard QCI, non-GBR uplink bytes forwarded. Type: Counter | Int64
nonstdqci-nongbr-dwlinkbyte-fwd | The total number of non-standard QCI, non-GBR downlink bytes forwarded. Type: Counter | Int64
nonstdqci-nongbr-uplinkpkt-drop | The total number of non-standard QCI, non-GBR uplink packets dropped. Type: Counter | Int32
nonstdqci-nongbr-dwlinkpkt-drop | The total number of non-standard QCI, non-GBR downlink packets dropped. Type: Counter | Int32
nonstdqci-nongbr-uplinkbyte-drop | The total number of non-standard QCI, non-GBR uplink bytes dropped. Type: Counter | Int64
nonstdqci-nongbr-dwlinkbyte-drop | The total number of non-standard QCI, non-GBR downlink bytes dropped. Type: Counter | Int64
nonstdqci-gbr-actbear | The total number of non-standard QCI, GBR active bearers. Type: Gauge | Int32
nonstdqci-gbr-setupbear | The total number of non-standard QCI, GBR bearers setup. Type: Counter | Int32
nonstdqci-gbr-relbear | The total number of non-standard QCI, GBR released bearers. Type: Counter | Int32
nonstdqci-gbr-uplinkpkt-fwd | The total number of non-standard QCI, GBR uplink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
nonstdqci-gbr-dwlinkpkt-fwd | The total number of non-standard QCI, GBR downlink packets forwarded. Type: Counter | v12.2 and earlier:Int32 v12.3/14.0 and later: Int64
nonstdqci-gbr-uplinkbyte-fwd | The total number of non-standard QCI, GBR uplink bytes forwarded. Type: Counter | Int64
nonstdqci-gbr-dwlinkbyte-fwd | The total number of non-standard QCI, GBR downlink bytes forwarded. Type: Counter | Int64
nonstdqci-gbr-uplinkpkt-drop | The total number of non-standard QCI, GBR uplink packets dropped. Type: Counter | Int32
nonstdqci-gbr-dwlinkpkt-drop | The total number of non-standard QCI, GBR downlink packets dropped. Type: Counter | Int32
nonstdqci-gbr-uplinkbyte-drop | The total number of non-standard QCI, GBR uplink bytes dropped. Type: Counter | Int64
nonstdqci-gbr-dwlinkbyte-drop | The total number of non-standard QCI, GBR downlink bytes dropped. Type: Counter | Int64
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.