# show apn-remap-table

This chapter describes the output of the show apn-remap-table command.

show apn-remap-table full name

This command provides detailed configuration and functional information for a specified apn-remap-table. Only those settings which are configured will be displayed in the output of this command.
Table 1. show apn-remap-table full name Command Output Descriptions

Field | Description
--- | ---
Default APN | Displays the network identifier to be used when the normal APN selection process fails. This setting is configured using the apn-selection-default command. Up to four individual default APN configurations will be displayed if configured.
Require Subscription APN | Indicates if this APN name must be included in the subscription data for the default APN feature to function.
Use Default APN when no APN is requested | Indicates that the default APN should be used if no APN is requested in the subscription record.
Use Default APN when DNS Query fails | Indicates that the default APN should be used if the DNS query fails.
Fallback APN to use when Default APN not present in subscription | Indicates the dummy APN to be used when the default APN is not present in the subscription.
Fallback APN in First subscription record when Default APN not present | Indicates whether to use the APN from the first subscription record when the configured default APN is not available.
Use APN from Single Subscription record | Indicates whether to use the APN from the subscription record if it is the only record available and normal APN selection fails.
APN selection mode when APN requested not present | Indicates the default APN selection mode, either first-in-subscription or lowest-context-id. This setting is configured using the apn-selection-default command.
APN to use when no APN is requested | Indicates the APN that will be used when no APN is requested. This setting is configured using the blank-apn command.
Charging Characteristic APN Overide Entry n | Displays a charging characteristics-based APN override group entry and associated settings. This group of settings is configured using the cc command.
Match Charging Characteristics Behavior | Indicates the charging characteristic behavior bit value.
Match Charging Characteristics Profile-Index | Indicates the index value for this charging characteristic profile.
Match Requested APN | Identifies the “old” APN network identifier of that is configured to be overridden/remapped.
APN to use for overriding | Identifies the “new” APN network identifier to which the APN will be remapped.
Wildcard APN for IPv4 | Identifies the configuration of the wildcard APN feature for IPv4 PDP contexts.
Wildcard APN for IPv6 | Identifies the configuration of the wildcard APN feature for IPv6 PDP contexts.
Wildcard APN for IPv4v6 | Identifies the configuration of the wildcard APN feature for dual IPv4v6 PDP contexts.
Wildcard APN for PPP | Identifies the configuration of the wildcard APN feature for PPP contexts.
APN remap Entryn | Displays an APN remap group entry and associated settings.
Match Input NI wildcard | Identifies the "old" APN network identifier that is being mapped for replacement.
Remap Input NI to | Identifies the new (target) network identifier to use.
Match Input OI wildcard | Identifies the “old” APN operator identifier that is being mapped for replacement.
Remap Input OI to | Identifies the new (target) operator identifier to use.
Replace wildcard MCC in Input OI with | Identifies the new (target) MCC value to use. This is specified using the value-for-oi-mcc keyword.
Replace wildcard MNC in Input OI with | Identifies the new (target) MNC value to use. This is specified using the value-for-oi-mnc keyword.