# ACS IMSI Pool Configuration Mode Commands

The ACS IMSI Pool Configuration Mode is used to define a pool of subscriber International Mobile Station Identifier (IMSI) numbers within the ACS Configuration Mode. IMSI pool configuration facilitates creation of rules to handle the packets coming from or going to a group of subscriber of IMSI numbers within an access policy.

IMPORTANT:

The commands or keywords/variables that are available are dependent on platform type, product version, and installed license(s).
end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.
imsi

This command allows you to add/remove an individual or a range of subscriber IMSI numbers from the current IMSI pool.
Platform:

ASR 5000

ASR 5500
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    [ no ] imsi { imsi_number | range start_imsi to end_imsi }

no

If added previously, removes the specified subscriber IMSI number(s) from the current IMSI pool.
imsi_number

Specifies an IMSI number to add to the current IMSI pool.

imsi_number must be an IMSI number, and must be a sequence of hexadecimal digits between 1 and 15.
start_imsi to end_imsi

Specifies a range of IMSI numbers to add to the current IMSI pool.

start_imsi specifies the starting IMSI number of the range and must be less than end_imsi.

end_imsi specifies the ending IMSI number of the range and must be greater than start_imsi.
Usage:

Use this command to add an individual or range of subscriber IMSI numbers to an IMSI pool. Up to 10 sets of IMSI numbers can be configured in each IMSI pool.
Example:
The following command adds IMSI numbers from 310150987654321 to 310150987656879 to the current IMSI pool:

    imsi range 310150987654321
    to 310150987656879