# show lma-service

This chapter describes the outputs of the show lma-service command.
show lma-service statistics
Table 1. show lma-service statistics Command Output Descriptions

Field | Description
--- | ---
MIP AAA Authentication
Attempts | The total number of MIP AAA authentication attempts made by this system or the specified service.
Success | The total number of MIP AAA authentication attempts that were successful made by this system or the specified service.
Total Failures | The total number of MIP AAA authentication attempts that failed made by this system or the specified service.
Actual Auth Failures | The total number of actual MIP AAA authentication failures received by this system or the specified service.
Failures | The total number of failures received by this system or the specified service.
Misc Auth Failures | The total number of miscellaneous MIP AAA authentication failures received this system or the specified service.
Binding Updates Received
Total Received | The total number of all binding updates received by this system or the specified service.
Total Accepted | The total number of all binding updates received and accepted by this system or the specified service.
Total Denied | The total number of all binding updates received and denied by this system or the specified service.
Total Discarded | The total number of all binding updates received and discarded by this
Initial Binding Update Requests
Received | The total number of all initial binding updates received by this system or the specified service.
Accepted | The total number of initial binding updates received and accepted by this system or the specified service.
Denied | The total number of initial binding updates received and denied by this system or the specified service.
Refresh Binding Update Requests
Received | The total number of all refresh binding updates received by this system or the specified service.
Accepted | The total number of refresh binding update requests received and accepted by this system or the specified service.
Denied | The total number of refresh binding update requests received and denied by this system or the specified service.
DeReg Requests
Received | The total number of all deregistration request binding updates received by this system or the specified service.
Accepted | The total number of deregistration request binding updates received and accepted by this system or the specified service.
Denied | The total number of deregistration request binding updates received and denied by this system or the specified service.
Handoff Requests
Received | The total number of all handoff request binding updates received by this system or the specified service.
Accepted | The total number of handoff request binding updates received and accepted by this system or the specified service.
Denied | The total number of handoff request binding updates received and denied by this system or the specified service.
Binding Acknowledgements Sent
Total | The total number of all binding update acknowledgements sent by this system or the specified service.
Accepted Reg | The total number of accepted registration binding update acknowledgements sent by this system or the specified service.
Accepted DeReg | The total number of accepted deregistration binding update acknowledgements sent by this system or the specified service.
Denied | The total number of denied binding update acknowledgements sent by this system or the specified service.
Send Error | The total number of send error binding update acknowledgements sent by this system or the specified service.
Binding Update Deny Reasons
Insufficient Resources | The total number of binding update deny messages, due to insufficient resources, sent by this system or the specified service.
Mismatched ID | The total number of binding update deny messages, due to mismatched IDs, sent by this system or the specified service.
MN Auth Failure | The total number of binding update deny messages, due to a mobile node authentication failure condition, sent by this system or the specified service.
Admin Prohibited | The total number of binding update deny messages, due to requiring a message ID, sent by this system or the specified service.
Msg ID Required | The total number of binding update deny messages, due to requiring a message ID, sent by this system or the specified service.
DAD Failed | The total number of binding update deny messages, due to DAD failure, sent by this system or the specified service.
Not Home Subnet | The total number of binding update deny messages, due to an incorrect home subnet, sent by this system or the specified service.
Sequence Out Of Window | The total number of binding update deny messages, due to sequence out of window, sent by this system or the specified service.
Reg Type Change Disallowed | The total number of binding update deny messages, due to a disallowed registration type change, sent by this system or the specified service.
Unspecified Reason | The total number of binding update deny messages, due to an unspecified reason, sent by this system or the specified service.
Service-Authorization Failed | The total number of binding update deny messages, due to a service authorization failure, sent by this system or the specified service.
Proxy Reg Not Enabled | The total number of binding update deny messages, due to a proxy registration not enabled error, sent by this system or the specified service.
Timestamp Mismatch | The total number of binding update deny messages, due to a timestamp mismatch error, sent by this system or the specified service.
Timestamp Lower Than Expected | The total number of binding update deny messages, due to a timestamp lower than expected reason, sent by this system or the specified service.
Missing MN-ID Option | The total number of binding update deny messages, due to a missing MN-ID option, sent by this system or the specified service.
Missing HNP Option | The total number of binding update deny messages, due to a missing HNP option, sent by this system or the specified service.
Missing Access Tech Option | The total number of binding update deny messages, due to a missing access technology option, sent by this system or the specified service.
Missing Handoff Ind Option | The total number of binding update deny messages, due to a missing handoff indicator option, sent by this system or the specified service.
Not Authorized For HNP | The total number of binding update deny messages, due to a not authorized for HNP reason, sent by this system or the specified service.
Not LMA For Mobile | The total number of binding update deny messages, due to a missing LMA for the MN reason, sent by this system or the specified service.
Not Authorized For Proxy Reg | The total number of binding update deny messages, due to a not authorized for proxy registration reason, sent by this system or the specified service.
BCE Prefix Do Not Match | The total number of binding update deny messages, due to a BCE prefix not matching, sent by this system or the specified service.
GRE Key Option Required | The total number of binding update deny messages, due to a GRE key option required reason, sent by this system or the specified service.
MCOA Unknown CoA: | The total number of binding update deny messages, due to a MCOA unknown CoA reason, sent by this system or the specified service.
Update Denied - Insufficient Resource Reasons
No Session Manager | The total number of binding update deny messages, due to insufficient resources - no session manager, sent by this system or the specified service.
No Memory | The total number of binding update deny messages, due to insufficient resources - no memory, sent by this system or the specified service.
Session Manager Rejected | The total number of binding update deny messages, due to insufficient resources - session manager rejected, sent by this system or the specified service.
Input-Q Exceeded | The total number of binding update deny messages, due to insufficient resources - input queue exceeded, sent by this system or the specified service.
Simul Bindings Exceeded | The total number of binding update deny messages, due to insufficient resources - simultaneous bindings exceeded, sent by this system or the specified service.
Address Alloc Failed | The total number of binding update deny messages, due to insufficient resources - address allocation failed, sent by this system or the specified service.
Update Denied - Admin Prohibited Reasons
MN-AAA Auth Option Missing | The total number of binding update deny messages, due to an administrator prohibited - MN-AAA auth option missing condition, sent by this system or the specified service.
H-bit Not Set | The total number of binding update deny messages, due to an administrator prohibited - H-bit not set condition, sent by this system or the specified service.
Invalid MN-AAA Option SPI | The total number of binding update deny messages, due to an administrator prohibited - invalid MN-AAA option SPI condition, sent by this system or the specified service.
Invalid MN-HA Option SPI | The total number of binding update deny messages, due to an administrator prohibited - invalid MN-HA option SPI condition, sent by this system or the specified service.
Congestion Control Denied | The total number of binding update deny messages, due to an administrator prohibited - congestion control denied condition, sent by this system or the specified service.
Policy Rejected | The total number of binding update deny messages, due to an administrator prohibited - policy rejected condition, sent by this system or the specified service.
HoA Not Authorized | The total number of binding update deny messages, due to an administrator prohibited - HoA not authorized condition, sent by this system or the specified service.
No Permission | The total number of binding update deny messages, due to an administrator prohibited - no permission condition, sent by this system or the specified service.
Bad Request | The total number of binding update deny messages, due to an administrator prohibited - bad request condition, sent by this system or the specified service.
Binding Updates Discard Reasons
Congestion Discarded | The total number of binding update discarded messages, due to congestion, sent by this system or the specified service.
Checksum Error | The total number of binding update discarded messages, due to checksum error(s), sent by this system or the specified service.
Initial Auth Pending | The total number of binding update discarded messages, due to an initial authentication pending condition, sent by this system or the specified service.
Session Not Found | The total number of binding update discarded messages, due to a session not found condition, sent by this system or the specified service.
HAMGR Not Ready | The total number of binding update discarded messages, due to an HA manager not found condition, sent by this system or the specified service.
Decode Failure | The total number of binding update discarded messages, due to a decode failure, sent by this system or the specified service.
Invalid Buffer Length | The total number of binding update discarded messages, due to an invalid buffer length, sent by this system or the specified service.
Revocation Pending | The total number of binding update discarded messages, due to pending revocations, sent by this system or the specified service.
Binding Revocation
Sent | The total number of binding revocations sent by this system or the specified service.
Retries Sent | The total number of binding revocation retries sent by this system or the specified service.
Ack Rcvd | The total number of binding revocation acknowledgements received by this system or the specified service.
Not Acknowledged | The total number of binding revocations sent, but not acknowledged, by this system or the specified service.
Rcvd | The total number of binding revocations received by this system or the specified service.
Ack Sent | The total number of binding revocation acknowledgements sent by this system or the specified service.
Sent Revocation Trigger Reasons
Unspecified | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Unspecified” revocation trigger reason.
Administrative Reason | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Administrative Reason” revocation trigger reason.
Inter-MAG Handoff-Same ATT | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Inter-MAG Handoff-Same ATT” revocation trigger reason.
Inter-MAG - Unknown Handoff | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Inter-MAG - Unknown Handoff” revocation trigger reason.
Inter-MAG Handoff-Diff ATT | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Inter-MAG Handoff-Diff ATT” revocation trigger reason.
Per-Peer Policy | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with a “Per-Peer Policy” revocation trigger reason.
Revoking Node Local Policy | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with a “Revoking Node Local Policy” revocation trigger reason.
User Initiated Session Term | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with a “User Initiated Session Term” revocation trigger reason.
Access Network Session Term | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Access Network Session Term” revocation trigger reason.
Out-of Sync BCE State | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Out-of Sync BCE State” revocation trigger reason.
Unknown | The total number of Binding Revocation Indication (BRI) messages sent by the LMA with an “Unknown” revocation trigger reason.
Received Revocation ACK Status
Success | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Success” status.
Partial-Success | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Partial-Success” status.
Binding-Does-Not-Exist | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Binding-Does-Not-Exist” status.
No IPv4-HoA-Bind | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “No IPv4-HoA-Bind” status.
Global-Revoc-Not-Authorized | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Global-Revoc-Not-Authorized” status.
Revoc-MN-ID-Required | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Revoc-MN-ID-Required” status.
Revoc-Failed-MN-Attached | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Revoc-Failed-MN-Attached” status.
Trigger-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Trigger-Not-Supported” status.
Proxy-Bind-Rev-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Proxy-Bind-Rev-Not-Supported” status.
Revoc-Func-Not-Supported | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with a “Revoc-Func-Not-Supported” status.
Unknown | The total number of Binding Revocation Acknowledgement (BRA) messages received by the LMA with an “Unknown” status.
Binding Revocation ACK Discarded
Total | The total number of binding revocation acknowledgements received and discarded by this system or the specified service.
Session Not Found | The total number of binding revocation acknowledgements received and discarded, due to a session not found condition, by this system or the specified service.
Badly Formed Request | The total number of binding revocation acknowledgements received and discarded, due to a badly formed request condition, by this system or the specified service.
Decode Error | The total number of binding revocation acknowledgements received and discarded, due to a decode error condition, by this system or the specified service.
Checksum Error | The total number of binding revocation acknowledgements received and discarded, due to a checksum error condition, by this system or the specified service.
Invalid Message Type | The total number of binding revocation acknowledgements received and discarded, due to a invalid memory type condition, by this system or the specified service.
HAMGR Not Ready | The total number of binding revocation acknowledgements received and discarded, due to a HAMGR not ready condition, by this system or the specified service.
Matching Request Not Found | The total number of binding revocation acknowledgements received and discarded, due to a matching request not found condition, by this system or the specified service.
Invalid Buffer Length | The total number of binding revocation acknowledgements received and discarded, due to a invalid buffer length condition, by this system or the specified service.
Tunnel Data Received
Total Packets | The total number of tunnel packets received by this system or the specified service.
6in6 | The total number of IPv6-in-IPv6 tunnel packets received by this system or the specified service.
4in6 | The total number of IPv4-in-IPv6 tunnel packets received by this system or the specified service.
IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel packets received by this system or the specified service.
IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel packets received by this system or the specified service.
4in4 | The total number of IPv4-in-IPv4 tunnel packets received by this system or the specified service.
6in4 | The total number of IPv6-in-IPv4 tunnel packets received by this system or the specified service.
IPv4 UDP (IPv4) | The total number of IPv4-in-IPv4 UDP tunnel packets received by this system or the specified service.
IPv4 UDP (IPv6) | The total number of IPv6-in-IPv4 UDP tunnel packets received by this system or the specified service.
Total Bytes | The total number of tunnel bytes received by this system or the specified service.
6in6 | The total number of IPv6-in-IPv6 tunnel bytes received by this system or the specified service.
4in6 | The total number of IPv4-in-IPv6 tunnel bytes received by this system or the specified service.
IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel bytes received by this system or the specified service.
IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel bytes received by this system or the specified service.
4in4 | The total number of IPv4-in-IPv4 tunnel bytes received by this system or the specified service.
6in4 | The total number of IPv6-in-IPv4 tunnel bytes received by this system or the specified service.
IPv4 UDP (IPv4) | The total number of IPv4-in-IPv4 UDP tunnel bytes received by this system or the specified service.
IPv4 UDP (IPv6) | The total number of IPv6-in-IPv4 UDP tunnel bytes received by this system or the specified service.
Errors
Protocol Type Error | The total number of protocol type data errors received by this system or the specified service.
Invalid Pkt Length | The total number of invalid packet length data errors received by this system or the specified service.
No Session Found | The total number of no session found data errors received by this system or the specified service.
Tunnel Data Sent
Total Packets | The total number of tunnel packets sent by this system or the specified service.
6in6 | The total number of IPv6-in-IPv6 tunnel packets sent by this system or the specified service.
4in6 | The total number of IPv4-in-IPv6 tunnel packets sent by this system or the specified service.
IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel packets sent by this system or the specified service.
IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel packets sent by this system or the specified service.
4in4 | The total number of IPv4-in-IPv4 tunnel packets sent by this system or the specified service.
6in4 | The total number of IPv6-in-IPv4 tunnel packets sent by this system or the specified service.
IPv4 UDP (IPv4) | The total number of IPv4-in-IPv4 UDP tunnel packets sent by this system or the specified service.
IPv4 UDP (IPv6) | The total number of IPv6-in-IPv4 UDP tunnel packets sent by this system or the specified service.
Total Bytes | The total number of tunnel bytes sent by this system or the specified service.
6in6 | The total number of IPv6-in-IPv6 tunnel bytes sent by this system or the specified service.
4in6 | The total number of IPv4-in-IPv6 tunnel bytes sent by this system or the specified service.
IPv6 GRE (IPv4) | The total number of IPv4-in-IPv6 GRE tunnel bytes sent by this system or the specified service.
IPv6 GRE (IPv6) | The total number of IPv6-in-IPv6 GRE tunnel bytes sent by this system or the specified service.
4in4 | The total number of IPv4-in-IPv4 tunnel bytes sent by this system or the specified service.
6in4 | The total number of IPv6-in-IPv4 tunnel bytes sent by this system or the specified service.
IPv4 UDP (IPv4) | The total number of IPv4-in-IPv4 UDP tunnel bytes sent by this system or the specified service.
IPv4 UDP (IPv6) | The total number of IPv6-in-IPv4 UDP tunnel bytes sent by this system or the specified service.
Tunnel ICMPV6 Packets
Packet Too Big Rcvd | The total number of tunnel ICMP packets - too big received by this system or the specified service.
Packet Too Big Dropped | The total number of tunnel ICMP packets - too big dropped by this system or the specified service.
Packet Too Big Relayed | The total number of tunnel ICMP packets - too big relayed by this system or the specified service.
Total Disconnects
Lifetime expiry | The total number of disconnects due to lifetime expiry initiated by this system or the specified service.
Deregistrations | The total number of disconnects due to deregistrations initiated by this system or the specified service.
Admin Drops | The total number of disconnects due to admin drops initiated by this system or the specified service.
Other Reasons | The total number of disconnects due to “other reasons” initiated by this system or the specified service.