# show gs-service

This chapter includes the show gs-service command output tables.
show gs-service all
Table 1. show gs-service all Command Output Descriptions

Field | Description
--- | ---
Service name | The Gs service that is running in this session.
State | Status of the Gs service.
Context | The name of the context in which Gs service is running.
SGSN Number | The E.164 number for the SGSN to associate with the Gs service.
SSN | Indicates the subsystem number configured or not. If configured it indicates SSN.
Self SCCP Network Id | Indicates the SCCP network identifier configured or not. If configured it indicates SSCP network identifier.
T6-1 Timeout | Indicates the retransmission timer (T6-1) value to guard the location update. Default: 10 seconds Range: 10 to 90 seconds
T8 Timeout | Indicates the retransmission timer (T8) value to guard the explicit IMSI detach from the GPRS service procedure. Default: 4 seconds Range: 1 to 30 seconds
T9 Timeout | Indicates the retransmission timer (T9) value to guard the explicit IMSI detach from the non-GPRS service procedure. Default: 4 seconds Range: 1 to 30 seconds
T10 Timeout | Indicates the retransmission timer (T10) value to guard the implicit IMSI detach from the non-GPRS service procedure. Default: 4 seconds Range: 1 to 30 seconds
T12-1 Timeout | Indicates the retransmission timer value (T12-1) in minutes to control the resetting of SGSN-Reset variable procedure. Default: 54 minutes (plus 8 seconds for transmission delay) Range: 0 to 380 minutes
T12-2 Timeout | Indicates the retransmission timer (T10) value to guard the SGSN reset procedure. Default: 4 seconds Range: 1 to 30 seconds
Max N8 Retries | Indicates the maximum retransmission allowed for procedure for explicit IMSI detach message from GPRS service (N8). Default: 2 retries Range: 0 to 10 retries
Max N9 Retries | Indicates the maximum retransmission allowed for procedure for explicit IMSI detach message from non-GPRS service (N9). Default: 2 retries Range: 0 to 10 retries
Max N10 Retries | Indicates the maximum retransmission allowed for procedure for implicit IMSI detach message from non-GPRS service (N10). Default: 2 retries Range: 0 to 10 retries
Max N12 Retries | Indicates the maximum retransmission allowed for N12 procedure for sending BSSAP+ Reset Indication message (N12). Default: 2 retries Range: 0 to 10 retries
GS Service Configurations
LAC Id | Indicates the subscriber location area code identifier configured in Gs service. Range: 1 through 65535
Pool Type | Type of pool area (non-pool area or pool area) configured in Gs service. Possible values are: Non Pool Area Pool Area
Pool Area/ Non Pool Area name | Name of the configured Non-pool area or pool area in Gs service.
Pool Area Configurations
Pool Area Name | Name of the configured pool area in Gs service.
Default Vlr | Name of the default VLR attached to this pool area.
LAC in Pool Area | Indicates the subscriber location area code identifier configured in this pool area. Range: 1 through 65535
VLR Hash Type | Indicates the type of hash configured for this pool area. Possible values are: Value Range
Value / Range | Indicates the value of hash or range of hash.
Vlr Name | Name of the VLR attached to this pool area.
Non-Pool Area Configurations
Non-Pool Area Name | Name of the configured non-pool area in Gs service.
Vlr Name | Name of the VLR attached to this non-pool area.
LAC in Pool Area | Indicates the subscriber location area code identifier configured in this non-pool area. Range: 1 through 65535
VLR Configurations
VLR Name | Name of the VLR attached to this Gs service.
ISDN Numbe | Indicates the E.164 ISDN number of configured VLR.
SSN | Indicates the subsystem number configured or not. If configured it indicates SSN.
Point Code | Indicates the configured point code address for VLR in SS7 address format.a
SGSN Reset | Indicates whether SGSN reset function is allowed or not. Possible values are: TRUE FALSE