# show location-service

This chapter describes the output of the show location-service command.

show location-service service all

Displays configuration information for all Location services configured on the system.
Table 1. show location-service service all Command Output Descriptions

Field | Description
--- | ---
Service name | The name of the Location service configured on the system.
Context | The name of the context in which this Location service is configured on the system.
Status | The state of the Location service, either STARTED or NOT STARTED. The status will display STARTED if a valid diameter endpoint is associated with this locations service
Diameter endpoint | The Diameter endpoint configured for this Location service.
Diameter dictionary | The Diameter dictionary configured for this Location service.
Map Service | The MAP service configured for this Location service.

show location-service statistics all

Displays SGs service statistics for all SGs services configured on the system.
Table 2. show location-service statistics all Command Output Descriptions

Field | Description
--- | ---
Message Stats
PL Request | The total number of Provide Location Request messages received.
PL Answer | The total number of Provide Location Answers sent.
PLR Retries | Not used in this release.
PLA Timeouts | Not used in this release.
PLA Dropped | The total number of times a Provide Location Answer could not be sent even though a paging answer is received.
LR Request | Not used in this release.
LR Answer | Not used in this release.
LRR Retries | Not used in this release.
LRA Timeouts | Not used in this release.
LRA Dropped | Not used in this release.
Message Error Stats
Unauthorized Requestion Network | The total number of times the requesting GMLC’s network was not authorized to request UE location information (Error code: 5490).
Unreachable User | The total number of times a PLR was received for a user which could not be reached (Error code: 4221)
User Unknown | The total number of times the PLR was received for an unknown user (Error code: 5001).
Suspended User | The total number of times the PLR was received for a user who is suspended in the MME (Error code: 4222).
Positioning Denied | The total number of times the positioning procedure was denied (Error code: 4224).
Detached User | The total number of times where the PLR was received for a detached user (Error code: 4223).
Positioning Failed | The total number of times the positioning procedure failed (Error code: 4225).
Unreachable LCS Client | The total number of times the GLMC indicated that the LCS Client was not known or could not be reached (Error code: 4226).
Other Errors | The total number of PLA messages received with other error result codes.