# Sample NAT Configuration

The following is a sample NAT configuration.

    configure

       license
    key "\

    VER=1|C1M=SanDiskSDCFJ-4096|C1S=116904I0207E3107|DOI=1258470708|DOE=12\

    HG=100000|FHE=Y|SIG=MC4CFQCf9f7bAibGKJWq69JaJMd5XowxVwIVALDFfUHAEUTokw"

       aaa
    default-domain subscriber radius

       aaa
    last-resort context subscriber radius

       gtpp
    single-source

       system
    hostname ABC123DEF456

       autoconfirm

       clock
    timezone asia-calcutta

       crash
    enable encrypted url abc123def456ghi789

       card
    1

          mode
    active psc

          exit

       card
    2

          mode
    active psc

          exit

       card
    4

          mode
    active psc

          exit

       require
    session recovery

       require
    active-charging

       context
    local

          interface
    SPIO1

             ip
    address 1.2.3.4 255.255.255.0

             exit

          server
    ftpd

             exit

          ssh
    key abc123def456ghi789abc123def456ghi789 len 777 type v2-dsa

          server
    sshd

             subsystem
    sftp

             exit

          server
    telnetd

             exit

          subscriber
    default

             exit

          administrator
    admin encrypted password abc123def456ghi789 ftp

          aaa
    group default

             exit

          gtpp
    group default

             exit

          ip
    route 0.0.0.0 0.0.0.0 2.3.4.5 SPIO1

          exit

       port
    ethernet 24/1

          no
    shutdown

          bind
    interface SPIO1 local

          exit

       ntp

          enable

          server
    10.6.1.1

          exit

       snmp
    engine-id local 123007e123275a8c123ff07ca49

       active-charging
    service service_name

          nat
    allocation-failure send-icmp-dest-unreachable

          host-pool
    host1

             ip
    range 3.4.5.6 to 4.5.6.7

             exit

          host-pool
    host2

             ip
    range 5.6.7.8 to 6.7.8.9

             exit

          host-pool
    host3

             ip
    range 7.8.9.0 to 8.9.0.1

             exit

          ruledef
    ip_any

             ip
    any-match = TRUE

             exit

          ruledef
    rt_ftp

             tcp
    either-port = 21

             rule-application
    routing

             exit

          ruledef
    rt_ftp_data

             tcp
    either-port = 20

             rule-application
    routing

             exit

          ruledef
    rt_http

             tcp
    either-port = 80

             rule-application
    routing

             exit

          ruledef
    rt_rtp

             rtp
    any-match = TRUE

             rule-application
    routing

             exit

          ruledef
    rt_rtsp

             tcp
    either-port = 554

             rule-application
    routing

             exit

          access-ruledef
    fw_icmp

             icmp
    any-match = TRUE

             exit

          access-ruledef
    fw_tcp

             tcp
    any-match = TRUE

             exit

          access-ruledef
    fw_udp

             udp
    any-match = TRUE

             exit

          edr-format
    nbr_format1

             attribute
    sn-correlation-id priority 1

             rule-variable
    ip subscriber-ip-address priority 2

             attribute
    subscriber-ipv4-address priority 19

             attribute
    subscriber-ipv6-address priority 20

             attribute
    sn-fa-correlation-id priority 3

             attribute
    radius-fa-nas-ip-address priority 4

             attribute
    radius-fa-nas-identifier priority 5

             attribute
    radius-user-name priority 6

             attribute
    radius-calling-station-id priority 7

             attribute
    sn-nat-ip priority 8

             attribute
    sn-nat-port-block-start priority 9

             attribute
    sn-nat-port-block-end priority 10

             attribute
    sn-nat-binding-timer priority 11

             attribute
    sn-nat-subscribers-per-ip-address priority 12

             attribute
    sn-nat-realm-name priority 13

             attribute
    sn-nat-gmt-offset priority 14

             attribute
    sn-nat-port-chunk-alloc-dealloc-flag priority 15

             attribute
    sn-nat-port-chunk-alloc-time-gmt priority 16

             attribute
    sn-nat-port-chunk-dealloc-time-gmt priority 17

             attribute
    sn-nat-last-activity-time-gmt priority 18

             exit

          udr-format
    udr_format

             attribute
    sn-start-time format MM/DD/YYYY-HH:MM:SS localtime
    priority 1

             attribute
    sn-end-time format MM/DD/YYYY-HH:MM:SS localtime
     priority 2

             attribute
    sn-correlation-id priority 4

             attribute
    sn-content-vol bytes uplink priority 6

             attribute
    sn-content-vol bytes downlink priority 7

             attribute
    sn-fa-correlation-id priority 8

             attribute
    radius-fa-nas-ip-address priority 9

             attribute
    radius-fa-nas-identifier priority 10

             attribute
    radius-user-name priority 11

             attribute
    sn-content-vol pkts uplink priority 12

             attribute
    sn-content-vol pkts downlink priority 13

             attribute
    sn-group-id priority 14

             attribute
    sn-content-id priority 15

             exit

          charging-action
    ca_nothing

             content-id
    20

             exit

          bandwidth-policy
    bw1

             exit

          bandwidth-policy
    bw2

             exit

          rulebase
    base_1

             tcp
    packets-out-of-order timeout 30000

             billing-records
    udr udr-format udr_format

             action
    priority 1 ruledef ip_any charging-action ca_nothing

             route
    priority 1 ruledef rt_ftp analyzer ftp-control

             route
    priority 10 ruledef rt_ftp_data analyzer ftp-data

             route
    priority 20 ruledef rt_rtsp analyzer rtsp

             route
    priority 30 ruledef rt_rtp analyzer rtp

             route
    priority 40 ruledef rt_http analyzer http

             route
    priority 50 ruledef rt_h323 analyzer h323

             rtp
    dynamic-flow-detection

             bandwidth
    default-policy bw1

             fw-and-nat
    default-policy base_1

             exit

          rulebase
    base_2

             action
    priority 1 ruledef ip_any charging-action ca_nothing

             route
    priority 1 ruledef rt_ftp analyzer ftp-control

             route
    priority 10 ruledef rt_ftp_data analyzer ftp-data

             route
    priority 40 ruledef rt_http analyzer http

             bandwidth
    default-policy bw2

             fw-and-nat
    default-policy base_2

             exit

          rulebase
    default

             exit

          fw-and-nat
    policy base_1

             access-rule
    priority 1 access-ruledef fw_tcp permit nat-realm nat_pool1

             access-rule
    priority 2 access-ruledef fw_udp permit nat-realm nat_pool2

             firewall
    tcp-first-packet-non-syn reset

             nat
    policy ipv4-only default-nat-realm nat_pool3

             firewall
    policy ipv4-and-ipv6

             nat
    binding-record edr-format nbr_format1 port-chunk-allocation
    port-chunk-release

             exit

          fw-and-nat
    policy base_2

             access-rule
    priority 10 access-ruledef fw_tcp permit nat-realm nat_pool2

             access-rule
    priority 20 access-ruledef fw_udp permit nat-realm nat_pool1

             access-rule
    priority 25 access-ruledef fw_icmp permit bypass-nat

             nat
    policy ipv4-only default-nat-realm nat_pool3

             firewall
    policy ipv4-and-ipv6

             exit

          nat
    tcp-2msl-timeout 120

          exit

       context
    pdsn

          interface
    pdsn

             ip
    address 9.0.1.2 255.255.255.0

             exit

          ssh
    key abc123def456ghi789abc123def456ghi789 len 461

          server
    sshd

             subsystem
    sftp

             exit

          subscriber
    default

             ip
    access-group css-1 in

             ip
    access-group css-1 out

             ip
    context-name isp

             mobile-ip
    send accounting-correlation-info

             active-charging
    rulebase base_1

             exit

          aaa
    group default

             exit

          gtpp
    group default

             exit

          pdsn-service
    pdsn

             spi
    remote-address 9.0.1.2 spi-number 256 encrypted secret abc123def456ghi789
    timestamp-tolerance 0

             spi
    remote-address 9.0.1.2 spi-number 256 encrypted secret abc123def456ghi789
    timestamp-tolerance 0

             spi
    remote-address 9.0.1.2 spi-number 9999 encrypted secret abc123def456ghi789
    timestamp-tolerance 0

             authentication
    pap 1 chap 2 allow-noauth

             bind
    address 0.1.2.3

             exit

          edr-module
    active-charging-service

             file
    name NBR_nat current-prefix Record rotation time 45 headers
    edr-format-name

             exit

          exit

       context
    isp

          ip
    access-list css

             redirect
    css service service_name

             ip
    any any

             exit

          ip
    pool nat_pool1 range 20.20.20.0 20.20.20.99 napt-users-per-ip-address
    10 max-chunks-per-user 5 port-chunk-size 128 send-nat-binding-update

          ip
    pool nat_pool2 range 30.30.30.0 30.30.30.99 nat-one-to-one
    on-demand nat-binding-timer 60 send-nat-binding-update

          ip
    pool nat_pool3 40.40.40.0 255.255.255.0 napt-users-per-ip-address
    5 max-chunks-per-user 5 port-chunk-size 64 send-nat-binding-update

          ip
    pool pool1 11.22.33.44 255.255.0.0 public 0

          interface
    isp

             ip
    address 22.33.44.55 255.255.255.0

             exit

          subscriber
    default

             exit

          aaa
    group default

             exit

          gtpp
    group default

             exit

          ip
    route 0.0.0.0 0.0.0.0 33.44.55.66 isp

          exit

       context
    radius

          interface
    radius

             ip
    address 44.55.66.77 255.255.255.0

             exit

          subscriber
    default

             exit

          subscriber
    name test7-sub

             ip
    access-group css in

             ip
    access-group css out

             ip
    context-name isp

             active-charging
    rulebase base_1

             exit

          subscriber
    name test9-sub

             ip
    access-group css in

             ip
    access-group css out

             ip
    context-name isp1

             active-charging
    rulebase base_2

             exit

          domain
    test7.com default subscriber test7-sub

          domain
    test9.com default subscriber test9-sub

          radius
    change-authorize-nas-ip 44.55.66.77 encrypted key abc123def456ghi789
    port 4000

          aaa
    group default

             radius
    attribute nas-ip-address address 44.55.66.77

             radius
    dictionary custom9

             radius
    server 55.66.77.88 encrypted key abc123def456ghi port 1645

             radius
    accounting server 55.66.77.88 encrypted key abc12 port 1646

             exit

          gtpp
    group default

             exit

          diameter
    endpoint abc.star.com

             origin
    host abc.star.com address 44.55.66.77

             peer
    minid realm star.com address 55.66.77.88

             exit

          exit

       bulkstats
    collection

       bulkstats
    mode

          sample-interval
    1

          transfer-interval
    15

          file
    1

             remotefile
    format /localdisk/ABC.bulkstat

             receiver
    66.77.88.99 primary mechanism ftp login root encrypted password
    34dab256a700e2a8

             exit

          exit

       port
    ethernet 17/1

          no
    shutdown

          bind
    interface pdsn pdsn

          exit

       port
    ethernet 17/2

          no
    shutdown

          bind
    interface isp isp

          exit

       port
    ethernet 17/3

          no
    shutdown

          bind
    interface radius radius

          exit

       port
    ethernet 17/4

          no
    shutdown

          exit

       port
    ethernet 17/5

          no
    shutdown

          exit

       end