# show sgtp

This chapter describes the outputs of the show sgtp command.
show sgtp-service ggsn-table
Table 1. show sgtp-service ggsn-table Command Output Descriptions

Field | Description
--- | ---
GTP | Indicates the GTP version. Possible values are: 0: GTP-v0 1: GTP-v1
Status | Indicates the status of the GTP session. Possible values are: I: Inactive A: Active
GTPC Echo | Indicates the status of the GTPC echo. Possible values are: D: Disabled E: Enabled
PLMN Type | Indicates the type of Public Land Mobile Network area. Possible values are: H: Home networks F: Foreign networks U: Unknown networks
SGTPC Stats | Indicates the availability of the SGTPC statistics. Possible values are: A: Available U: Unavailable
Service ID | Indicates the SGTP service identifier.
GGSN Address | Indicates the IP address of GGSN service.
Restart Counter | Indicates the restart counter of SGTP service.
No. of restart | Indicates the total number of restarts happened for SGTP session.
Curr sessions | Total number of SGTP session currently running.
Max sessions | Indicates the maximum number of SGTP session allowed.

show sgtp-service sgsn-table
Table 2. show sgtp-service sgsn-table Command Output Descriptions

Field | Description
--- | ---
GTP | Indicates the GTP version. Possible values are: 0: GTP-v0 1: GTP-v1
GTPC Echo | Indicates the status of the GTPC echo. Possible values are: D: Disabled E: Enabled
PLMN Type | Indicates the type of Public Land Mobile Network area. Possible values are: H: Home networks F: Foreign networks U: Unknown networks
SGTPC Stats | Indicates the availability of the SGTPC statistics. Possible values are: A: Available U: Unavailable
Service ID | Indicates the SGTP service identifier.
SGSN Address | Indicates the IP address of SGGSN service.