# show cs-network

This chapter includes the show cs-network command output tables.
show cs-network all status
Table 1. show cs-network all status Command Output Descriptions

Field | Description
--- | ---
CS Network name | Indicates the name of the Circuit Switched (CS) network instance for which status is displayed.
Associated SCCP-Network | Indicates the name of the Signalling Connection Control Part (SCCP) network service instance which in associated with referecned CS network instance.
Associated Alcap-Service | Indicates the name of the Access Link Control Application Protocol (ALCAP) service instance which in associated with referecned CS network instance.
Alcap Context Name | Indicates the name of the context in which ALCAP service instance is configured.
Associated RTP Pool | Indicates the name of the RTP IP pool configured and associated with referecned CS network instance for RTP stream management.
RTP Pool Context Name | Indicates the name of the context in which RTP IP pool is configured for RTP stream management.
MSC Point Code | Indicates the address of MSC in SS7 point code notation which is serving the referenced CS network instance.
Status | Indicates the status of MSC which is serving the referenced CS network instance.
Network Status | Indicates the status of network in which the referenced CS network instance is placed.
RTP IP Addresses | Indicates the session manager instances and associated IP pools with them for RTP stream management support.
NRI | Indicates the Network Resource Identication (NRI) bit configuration status for the referenced CS network.
IDNNS | Indicates the Intra-Domain NAS Node Selector (IDNNS) configuration status for the referenced CS network to transport the NRI value.
Lac range <nnn> to <nnn> MSC Point-code <x.x.x> | Indicates the mapping configured between MSC point-code and range of LAC for multiple MSC selection without Iu-Flex in CS network.
CORE NODE MAP | Indicates the core node mapping configuration status for the referenced CS network.
Initiated Ranap Reset | Indicates if the HNB-GW Initiated RANAP Reset function is enabled or disabled. IMPORTANT: Before StarOS 14.0 release, this counter was displayed in `show hnbgw-service` command outputs.
Ranap Reset Ack Timer | The timer value, in seconds, that defines how long the HNB-GW waits for a RESET ACK message from the MSC after transmitting a RESET message. This setting is used only if the HNB-GW Initiated RANAP Reset function is enabled. IMPORTANT: Before StarOS 14.0 release, this counter was displayed in `show hnbgw-service` command outputs.
Ranap Reset Maximum Retransmissions | Sets the maximum number of retries allowed for the HNB-GW to transmit a RANAP RESET message to the MSC if the RESET ACK timer expires. This setting is used only if the HNB-GW Initiated RANAP Reset function is enabled. IMPORTANT: Before StarOS 14.0 release, this counter was displayed in `show hnbgw-service` command outputs.
Ranap Reset Guard Timer | The timer that the HNB-GW starts after receiving a RESET message from the CS core network. While this timer is running, the HNB-GW discards any new RESET messages that it receives. IMPORTANT: Before StarOS 14.0 release, this counter was displayed in `show hnbgw-service` command outputs.
Global RNC-Id | This group displays the information related to global Radio Network Controller settings for use by the CS core network for HNB-GW service(s) on a chassis. It is configured under the PLMN-ID.
MCC | The Mobile Country Code defined for use with this HNB-GW service. It consists of the first 3 digits of the Available Radio Network PLMN ID.
MNC | The Mobile Network Code defined for use with this HNB-GW service. It consists of the last 3 digits of the Available Radio Network PLMN ID.
Id | The Radio Network Controller ID provided to HNBs for use by the CS core network for this HNB-GW service. It is configured under the PLMN-ID

show cs-network statistics ranap-only
Table 2. show cs-network statistics ranap-only Command Output Descriptions

Field | Description
--- | ---
RANAP | This group displays the statistics of RANAP in a CS network on chassis.
Initial UE Tx | Total number of initial UE requests transmitted.
Direct Transfer Rx | Total number of Direct Transfer requests received.
Direct Transfer Tx | Total number of Direct Transfer responses sent.
Reset Rx | Total number of RESET requests received.
Reset Tx | Total number of RESET responses sent.
Reset Ack Rx | Total number of RESET Ack requests received.
Reset Ack Tx | Total number of responses against RESET Ack request sent.
Reset Resource Rx | Total number of RESET RESOURCE requests received.
Reset Resource Tx | Total number of RESET RESOURCE responses sent.
Reset Resource Ack Rx | Total number of RESET RESOURCE Ack requests received.
Reset Resource Ack Tx | Total number of responses against RESET RESOURCE Ack request sent.
Iu Release Request Tx | Total number of Iu RELEASE requests sent.
Iu Release Command Rx | Total number of Iu RELEASE command received.
Iu Release Complete Tx | Total number of Iu RELEASE Complete response sent.
Paging Request Rx | Total number of Paging rquests received.
RAB Assignment Request Rx | Total number of RAB assignment requests received.
RAB Setup/Mod Rx | Total number of RAB setup or modification requests received.
RAB Release Rx | Total number of RAB Release requests received.
RAB Assignment Response Tx | Total number of responses against RAB assignment requests sent.
RAB Setup/Mod Success Tx | Total number of RAB setup or modification Success response sent.
Total RAB Setup/Mod Fail Tx | Total number of RAB setup or modification Fail response sent.
RAB Setup/Mod Fail(Local) Tx | Total number of RAB setup or modification Fail response sent where RAB setup or modification failed due to local reason/cause.
RAB Release Success Tx | Total number of RAB Release Success response sent.
Total RAB Release Fail Tx | Total number of RAB Release Success response sent.
RAB Release Fail(Local) Tx | Total number of RAB Release Fail response sent where RAB Release failed due to local reason/cause.
RAB Queued Tx | Total number of RAB messages quesed for transmission.
RAB Setup/Mod Timer Exp | Total number of instances where RAB setup/modification timer expired before process of request.
RAB Release Timer Exp | Total number of instances where RAB Reelase timer expired before process of request.
RAB Set/Mod/Rel Local Fail | This group displays the total number of RAB setup or modification or release requests failed due to local reason/cause.
Local Failure Cause | This group idendifies the local cause for RAB setup or modification or release request failure.
Radio Network Layer Cause | This group idendifies the total number of RAB setup or modification or release request failure due to error in radio network layer.
Invalid Rab Id | Total number of RAB setup or modification or release requests failed due to invalid RAB id in radio network layer.
Interaction With Other Proc | Total number of RAB setup or modification or release requests failed as system was interacting with another process.
Transport Layer Cause | This group idendifies the total number of RAB setup or modification or release request failure due to error in Transport layer.
Sig Trans Res Fail | Total number of RAB setup or modification or release requests failed due to Sig trans Resource failure in transport layer.
Iu Tran Conn failed to Estab | Total number of RAB setup or modification or release requests failed where Iu Transmission connection failed to establish in transport layer.
Protocol Layer Cause | This group idendifies the total number of RAB setup or modification or release request failure due to error in Protocol layer.
Transfer syntax error | Total number of RAB setup or modification or release requests failed due to transfer syntax error in Protocol layer.
Asn error(Reject) | Total number of RAB setup or modification or release requests failed due to ASN (Reject) syntax error in Protocol layer.
Asn error | Total number of RAB setup or modification or release requests failed due to ASN syntax error in Protocol layer.
Msg not comp with Rcvr state | Total number of RAB setup or modification or release requests failed as message was not compatible with Recovery state in Protocol layer.
Semantic error | Total number of RAB setup or modification or release requests failed due to semantic error in Protocol layer.
Asn error(Falsely const msg) | Total number of RAB setup or modification or release requests failed due to ASN error (falsely constructed messages) in Protocol layer.
Miscellaneous Cause | This group idendifies the total number of RAB setup or modification or release request failure due to miscellaneous cause (not listed in this table).
No Resource Available | Total number of RAB setup or modification or release requests failed due to non availability of resourcse.
Unspecified | Total number of RAB setup or modification or release request failure due to sunspecified cause (not listed in this table).
<codec_name> Codec | This group displays the total number of RAB setup or modification or release request failure grouped in Codec name <codec_name>. Following groups are supported: UMTS AMR Codec UMTS AMR2 Codec Other Codec No Codec Unknown Codec
RAB Setup/Mod Rx | Total number of RAB setup or modification requests received for specific codec.
RAB Setup/Mod Success Tx | Total number of RAB setup or modification sucess messages sent for specific codec.
RAB Release Rx | Total number of RAB Release requests received for specific codec.
Total RAB Setup/Mod Fail Tx | Total number of RAB setup or modification failure messages sent for specific codec.
RAB Setup/Mod Fail(Local) Tx | Total number of RAB setup or modification failure messages sent for specific codec where RAB setup or modification failed due to local reason/cause.
RAB Release Success Tx | Total number of RAB Release success messages sent for specific codec.
Total RAB Release Fail Tx | Total number of RAB Release fail messages sent for specific codec.
RAB Release Fail(Local) Tx | Total number of RAB Release fail messages sent for specific codec where RAB setup or modification failed due to local reason/cause.
RAB Queued Tx | Total number of RAB messages queued for processing or transmission.
Relocation Request Rx | Total number of RAB Relocation request received by system for this CS network.
RAB Setup Rx | Total number of RAB Relocation setup request received by system for this CS network.
Relocation Request ACK Tx | Total number of RAB Relocation Ack messages sent agains setup request received by system for this CS network.
RAB Setup Success Tx | Total number of RAB setup success messages sent agains setup request received by system for this CS network.
Total RAB Setup Fail Tx | Total number of RAB setup fail messages sent agains setup request received by system for this CS network.
RAB Setup Fail(Local) Tx | Total number of RAB setup failure messages sent from this system where RAB setup or modification failed due to local reason/cause.
Local Failure Cause | This group idendifies the local cause for RAB setup or modification or release request failure.
Radio Network Layer Cause | This group idendifies the total number of RAB setup or modification or release request failure due to error in radio network layer.
Invalid Rab Id | Total number of RAB setup or modification or release requests failed due to invalid RAB id in radio network layer.
Interaction With Other Proc | Total number of RAB setup or modification or release requests failed as system was interacting with another process.
Transport Layer Cause | This group idendifies the total number of RAB setup or modification or release request failure due to error in Transport layer.
Sig Trans Res Fail | Total number of RAB setup or modification or release requests failed due to Sig trans Resource failure in transport layer.
Iu Tran Conn failed to Estab | Total number of RAB setup or modification or release requests failed where Iu Transmission connection failed to establish in transport layer.
Protocol Layer Cause | This group idendifies the total number of RAB setup or modification or release request failure due to error in Protocol layer.
Transfer syntax error | Total number of RAB setup or modification or release requests failed due to transfer syntax error in Protocol layer.
Asn error(Reject) | Total number of RAB setup or modification or release requests failed due to ASN (Reject) syntax error in Protocol layer.
Asn error | Total number of RAB setup or modification or release requests failed due to ASN syntax error in Protocol layer.
Msg not comp with Rcvr state | Total number of RAB setup or modification or release requests failed as message was not compatible with Recovery state in Protocol layer.
Semantic error | Total number of RAB setup or modification or release requests failed due to semantic error in Protocol layer.
Asn error(Falsely const msg) | Total number of RAB setup or modification or release requests failed due to ASN error (falsely constructed messages) in Protocol layer.
Miscellaneous Cause | This group idendifies the total number of RAB setup or modification or release request failure due to miscellaneous cause (not listed in this table).
No Resource Available | Total number of RAB setup or modification or release requests failed due to non availability of resourcse.
Unspecified | Total number of RAB setup or modification or release request failure due to sunspecified cause (not listed in this table).
<codec_name> Codec | This group displays the total number of RAB Setup request grouped in Codec name <codec_name>.
RAB Setup Rx | Total number of RAB setup requests received for specific codec.
RAB Setup Success Tx | Total number of RAB setup sucess messages sent for specific codec.
Total RAB Setup Fail Tx | Total number of RAB setup failure messages sent for specific codec.
RAB Setup Fail(Local) Tx | Total number of RAB setup failure messages sent for specific codec where RAB setup failed due to local reason/cause.
Relocation Detect Tx | Total number of RAB Relocation Detect messages sent by system in this CS network.
Relocation Required Tx | Total number of RAB Relocation Required request messages sent by system in this CS network.
Fwd SRNS Context Request Tx | Total number of FWD SRNS Context request messages sent by system in this CS network.
Relocation Prep Failure Rx | Total number of Relocation Preparation failure response messages sent by system in this CS network.
Relocation Cancel Tx | Total number of Relocation cancle command messages received by system in this CS network.
Relocation Command Rx | Total number of Relocation command messages received by system in this CS network.
Srns Context Request Rx | Total number of SRNS Context Request messages received by system in this CS network.
Srns Context Response Tx | Total number of response sent for SRNS Context Request messages received by system in this CS network.

show cs-network statistics sccp-only
Table 3. show cs-network statistics sccp-only Command Output Descriptions

Field | Description
--- | ---
SCCP | This group displays the statistics of SCCP in a CS network on chassis.
SCCP Connection Request Rx | Total number of SCCP connection Request received by HNB-GW from the Core Node. This counter changes when Core Node initiates SCCP connection during Relocation.
SCCP Connection Request Tx | Total number of SCCP connection Request sent by HNB-GW towards the CN after getting RUA Connect Request for a Registered UE. This counter changes when RUA Connect Request sent for a Registered UE.
SCCP Connection Confirm Rx | Total number of SCCP Connection Confirmation messages received by HNB-GW from the Core Node. This counter changes when CN sends the SCCP connection confirmation for a requested SCCP Connection Request.
SCCP Connection Confirm Tx | Total number of SCCP Connection Confirmation response messages sent by HNB-GW to the Core Node. This counter changes when HNB-GW sends the SCCP connection confirmation response for a requested SCCP Connection Request to CN.
SCCP Connection Reject Rx | Total number of SCCP Connection Reject messages received by HNB-GW from the Core Node. This counter changes when Core node Rejects the SCCP Conn Request due to some parameter mismatch, etc.
SCCP Connection Reject Tx | Total number of SCCP Connection Rejection response messages sent by HNB-GW to the Core Node. This counter changes when HNBGW initiates the tear Down on receiving RUA disconnect from HNB which doesn't contain RANAP Iu-release complete message and other failure scenarios.
SCCP Connection Data Rx | Total data received by HNB-GW over SCCP connection between HNB-GW and Core Node. This counter changes when CN sends the data towards HNB-GW over SCCP connection.
SCCP Connection Data Tx | Total data sent by HNB-GW over SCCP connection between HNB-GW and Core Node. This counter changes when HNB-GW sends the data towards CN over SCCP connection.
SCCP Disconnect Rx | Total number of SCCP Disconnect messages received by HNB-GW from Core Node. This counter changes when CN initiate tear-down procedure for SCCP connection.
SCCP Disconnect Tx | Total number of SCCP Disconnect response messages sent by HNB-GW to Core Node. This counter changes when HNBGW initiates the tear-down procedure on receiving RUA disconnect from HNB which doesn't contain RANAP Iu-release complete message and other failure scenarios.
SCCP Uni Data Rx | Total Connection-less data, like paging, received by HNB-GW over SCCP connection between HNB-GW and Core Node. This counter changes when CN sends any connection-less data, like paging, towards HNB-GW over SCCP connection.
SCCP Uni Data Tx | Total Connection-less data, RANAP Reset, RANAP reset Resource, sent by HNB-GW over SCCP connection between HNB-GW and Core Node. This counter changes when HNB-GW sends or forward any Connection-less data, like RANAP reset, RANAP Reset Resource, towards CN over SCCP connection.