# PDG Schema Statistics

The PDG schema provides operational statistics that can be used for monitoring and troubleshooting the following products: PDG/TTG
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the PDG Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | Description: The name of the context currently facilitating the service processing the subscriber session. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | String
vpnid | Description: The identification number of the context currently facilitating the service processing the subscriber session. This is an internal reference number. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | Int32
svcname | Description: The service name for which PDG statistics are being displayed. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | String
svcid | Description: The service ID for which PDG statistics are being displayed. This is a key variable. This variable is proprietary. Availability: IPSec/SSL. | Int32
bindaddress | Description: The bind IP address for this PDG service. This variable is proprietary. Availability: IPSec/SSL. | String
state | Description: System-wide PDG state identified by the following codes: inservice(1): The PDG service is started (active). outofservice(2): The PDG service is not started. It is in the initial state (inactive). This variable is proprietary. Availability: IPSec/SSL. | String
sess-ttlcursess | Description: Number of total current sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
sess-curact | Description: Number of currently active PDG sessions. This variable is proprietary. Trigger: Increments on receiving a new call request from the UE. For IPSec, it increments after receiving an IKE_INIT message from the UE. For SSL, it increments after the SSL tunnel is established. Availability: IPSec/SSL. Type: Gauge | Int32
sess-curdorm | Description: Number of currently dormant PDG sessions. This variable is proprietary. Trigger: For SSL, it represents those subscribers wherein the TCP connection is up but the SSL tunnel is not yet up. Availability: SSL. Type: Gauge | Int32
sess-curactipv4 | Description: Number of currently active IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
sess-curdormipv4 | Description: Number of currently dormant IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
sess-curactipv6 | Description: Number of currently active IPv6 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
sess-curdormipv6 | Description: Number of currently dormant IPv6 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
sess-curdiripipv4 | Description: Number of current direct IP IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
sess-curttgipv4 | Description: Number of current TTG IPv4 sessions. This variable is proprietary. Availability: IPSec/SSL. Type: Gauge | Int32
sess-ttldiripipv4 | Description: Total number of direct IP IPv4 sessions. This variable is proprietary. Trigger: Increments upon successful IPv4 PDG mode call setup. Availability: IPSec/SSL. Type: Gauge | Int32
sess-ttlttgipv4 | Description: Total number of TTG IPv4 sessions. This variable is proprietary. Trigger: Increments upon successful IPv4 TTG mode call setup. Availability: IPSec/SSL. | Int32
sess-diripipv4succ | Description: Number of direct IP IPv4 successful sessions. This variable is proprietary. Trigger: Increments upon successful IPv4 PDG mode call setup. Availability: IPSec/SSL. | Int32
sess-diripipv4attempt | Description: Number of direct IP IPv4 attempted sessions. This variable is proprietary. Trigger: Increments upon receiving an IKE_INIT message from the UE in IPsec and a TCP SYN message from the UE in SSL. Availability: IPSec/SSL. | Int32
sess-diripipv4attemptfail | Description: Number of direct IP IPv4 attempted sessions that failed. This variable is proprietary. Trigger: Increments upon a session setup timeout and authentication failure scenario in PDG mode IPv4 call setup. Availability: IPSec/SSL. | Int32
sess-ttgipv4succ | Description: Number of direct TTG IPv4 successful sessions. This variable is proprietary. Trigger: Increments upon a successful IPv4 TTG mode call setup. Availability: IPSec/SSL. | Int32
sess-ttgipv4attempt | Description: Number of direct TTG IPv4 attempted sessions. This variable is proprietary. Trigger: Increments upon receiving an IKE_INIT message from the UE in IPsec and a TCP SYN message from the UE in SSL TTG mode. Availability: IPSec/SSL. | Int32
sess-ttgipv4attemptfail | Description: Number of direct TTG IPv4 attempted sessions that failed. This variable is proprietary. Trigger: Increments upon a session setup timeout and authentication failure scenario in PDG mode IPv4 call setup. Availability: IPSec/SSL. | Int32
sess-ttlsetup | Description: Total number of sessions set up. This variable is proprietary. Trigger: Increments upon sending a successful IKE_AUTH CFG response to the UE in IPSec, and upon a successful call setup with an MT_CLOSE message sent to the UE in SSL. Availability: IPSec/SSL. | Int32
sess-ttlattempt | Description: Total number of session attempted. This variable is proprietary. Trigger: Increments upon receiving an IKE_INIT message from the UE in IPsec and a TCP SYN message in SSL TTG mode. Availability: IPSec/SSL. | Int32
sess-ttlattemptfail | Description: Total number of session attempts failed. This variable is proprietary. Trigger: Increments upon session setup timout and authentication failure scenario or a resource unavailable scenario where the subscriber allocation fails. Availability: IPSec/SSL. | Int32
sess-ttldisc | Description: Total number of sessions disconnected. Trigger: Increments after call is up during re-authentication failure (IPSec only) and the SSL or IPSec tunnel goes down. This variable is proprietary. | Int32
sess-ttldisclocal | Description: Total number of sessions disconnected locally. This variable is proprietary. Trigger: Increments by unavailable resources and session setup timeout. Availability: IPSec/SSL. | Int32
sess-ttldiscremote | Description: Total number of sessions disconnected remotely. This variable is proprietary. Trigger: Increments on UE-initiated call tear down after call setup. Availability: IPSec/SSL. | Int32
sess-discbeforeconn | Description: Sessions remotely disconnected before connected. This variable is proprietary. Trigger: Increments on UE-initiated call tear down before call setup. Availability: IPSec/SSL. | Int32
sess-ttlfastreauthsucc | Description: Total fast re-authentication successes. This variable is proprietary. Trigger: Increments upon re-authetication success scenario. Includes both fast re-authentication and pseudoname re-authentication. Availability: IPSec. | Int32
sess-ttlfastreauthattempt | Description: Total fast re-authentication attempts. This variable is proprietary. Trigger: Increments upon receiving the re-auth ID in the IKE-AUTH message from the UE. Includes both fast re-authentication and pseudoname re-authentication. Availability: IPSec. | Int32
sess-ttlfastreauthattemptfail | Description: Total fast re-authentication attempts that failed. This variable is proprietary. Trigger: Increments upon a re-authentication success scenario from the AAA server. Includes both fast re-authentication and pseudoname re-authentication. Availability: IPSec. | Int32
sess-ttlreauthorizesucc | Description: Total reauthorization attempts that succeeded. This variable is proprietary. Trigger: Increments upon receiving an authorize success message from the AAA server. Availability: IPSec. | Int32
sess-ttlreauthorizeattempt | Description: Total reauthorization attempts. This variable is proprietary. Trigger: Increments upon sending an authorize request message to the AAA server. Availability: IPSec. | Int32
sess-ttlreauthorizeattemptfail | Description: Total reauthorization attempts that failed. This variable is proprietary. Trigger: Increments upon an authorization failure with the AAA server or if the IPsec tunnel goes down during authorization. Availability: IPSec. | Int32
sess-ttlprimaryaaasucc | Description: Total primary AAA sessions that succeeded. This variable is proprietary. Trigger: Increments upon receiving an access accept message from the AAA server. (Increments only during primary authentication if multiple authentication is supported in IPSec). Availability: IPSec/SSL. | Int32
sess-ttlprimaryaaaattempt | Description: Total primary AAA sessions attempted. This variable is proprietary. Trigger: Increments upon receiving an IKE -AUTH message from the UE in IPSec and an MT-AUTH message from the UE in SSL. Availability: IPSec/SSL. | Int32
sess-ttlprimaryaaaattemptfail | Description: Total primary AAA sessions that failed. This variable is proprietary. Trigger: Increments on an authentication failure and if the SSL or IPSec tunnel goes down during authentication. Availability: IPSec/SSL. | Int32
sess-ttlexternalaaasucc | Description: Total external AAA sessions that succeeded. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server in a multiple authentication scenario. Availability: IPSec. | Int32
sess-ttlexternalaaaattempt | Description: Total external AAA sessions that attempted. This variable is proprietary. Trigger: Increments upon receiving an IKE-AUTH (ANOTHER-AUTH-FOLLOWS) message from the UE in a multiple authentication scenario. Availability: IPSec. | Int32
sess-ttlexternalaaaattemptfail | Description: Total external AAA sessions that failed. This variable is proprietary. Trigger: Increments upon receiving an authentication failure from the AAA server or an IPsec tunnel tear down in a multiple authentication scenario. Availability: IPSec. | Int32
sess-ttleapauthsucc | Description: Total of successful EAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server for the second phase authentication using EAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
sess-ttleapauthfail | Description: Total of failed EAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication failure message from the AAA server for the second phase authentication using EAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
sess-ttlpapauthsucc | Description: Total of successful PAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server for the second phase authentication using PAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
sess-ttlpapauthfail | Description: Total of failed PAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication failure message from the AAA server for the second phase authentication using PAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
sess-ttlchapauthsucc | Description: Total of successful CHAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication success message from the AAA server for the second phase authentication using CHAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
sess-ttlchapauthfail | Description: Total of failed CHAP authorizations. This variable is proprietary. Trigger: Increments upon receiving an authentication failure message from the AAA server for the second phase authentication using CHAP. (Applicable only in a multiple authentication scenario.) Availability: IPSec. | Int32
sess-discremote | Description: Number of sessions terminated by a remote disconnect. This variable is proprietary. Trigger: A TCP failure scenario in SSL PDG and SSL TTG after the call is in the CONNECTED state. A UE-initiated session disconnect in IPSec PDG and IPSec TTG after the call is in the CONNECTED state. Availability: IPSec/SSL. | Int32
sess-attemptfaildiscremote | Description: Number of sessions terminated by a Session Attempt Failed disconnect reason due to a remote disconnect. Trigger: A TCP failure scenario in SSL PDG and SSL TTG before the call is in the CONNECTED state. A UE-initiated session disconnect in IPSec PDG and IPSec TTG before the call is in the CONNECTED state. Availability: IPSec/SSL. | Int32
sess-discadmin | Description: Number of sessions terminated because of an admin release. This variable is proprietary. Trigger: Incremented for all sessions in a CONNECTED state that are cleared due to an Admin Disconnect disconnect reason. Availability: IPSec/SSL. | Int32
sess-attemptfaildiscadmin | Description: Number of sessions terminated by a Session Attempt Failed disconnect reason due to an admin disconnect. This variable is proprietary. Trigger: Incremented for all session setups that failed due to an admin disconnect before the session is in a CONNECTED state. Availability: IPSec/SSL. | Int32
sess-discidletimeout | Description: Number of sessions terminated because of idle timer timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discabstimeout | Description: Number of sessions terminated because of absolute timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-disclongdur | Description: Number of sessions terminated because of long duration timer timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discsesssetuptimeout | Description: Number of sessions terminated because of Session Manager session setup timeout. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discnonexistpcrf | Description: Number of sessions terminated because of non-existence of PCRF. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discnoresource | Description: Number of sessions terminated because of no resources. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discauthfail | Description: Number of sessions terminated because of AAA authentication failure. This variable is proprietary. Trigger: Incremented on receiving an Access-Reject message, an invalid AAA attribute in an Access-Accept message, an AAA timeout message, a missing AAA attribute in an Access-Accept message, an invalid W-APN format, or an invalid NAI format. Also incremented in PDG mode if W-APN is not configured. Availability: IPSec/SSL. | Int32
sess-discreauthfail | Description: Number of sessions terminated because of a session re-authetication failure. This variable is proprietary. Trigger: Incremented for all AAA failures during fast re-authentication or pseudonym re-authentication. Availability: IPSec. | Int32
sess-discflowaddfail | Description: Number of sessions terminated because of flow add failure. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discinvdestctx | Description: Number of sessions terminated because of invalid destination context. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discsourceviol | Description: Number of sessions terminated because of source IP address violation. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discgtp | Description: Number of sessions terminated because of a GTP failure. This variable is proprietary. Trigger: Incremented for all GTP path failures or DPC requests from the GGSN. Availability: IPSec/SSL (TTG only). | Int32
sess-attemptfaildiscgtp | Description: Number of session attempts failed because of GTP failure. This variable is proprietary. Trigger: Incremented for all session setups failed due to CPC failure/timeout. Availability: IPSec/SSL (TTG only). | Int32
sess-discdupreq | Description: Number of sessions terminated because of duplicate requests. This variable is proprietary. Trigger: Incremented on receiving a new call when a previous call exists in the CONNECTED state with the same IMSI and APN on the same Session Manager. When this occurs, the original call is cleared. Availability: IPSec/SSL (TTG only). | Int32
sess-attemptfaildiscdupreq | Description: Number of session attempts failed because of duplicate requests. This variable is proprietary. Trigger: Incremented on receiving a new call when a previous call exists in the CONNECTED state with the same IMSI and APN on the same Session Manager. When this occurs, the original call is cleared. Availability: IPSec/SSL (TTG only). | Int32
sess-discaddrfail | Description: Number of sessions terminated because of an address assignment failure. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-discmisc | Description: Number of sessions terminated because of miscellaneous reasons. This variable is proprietary. Trigger: Incremented for all SSL failures and all remaining disconnect reasons (for example, for IPSec, no-response or remote-error-notification). Availability: IPSec/SSL. | Int32
sess-attemptfaildiscmisc | Description: Number of session attempts failed because of miscellaneous reasons. This variable is proprietary. Trigger: Incremented for all session setup failures due to SSL failures (for example, handshake failures, ssl-alert, ssl-bad-message), or an unknown APN case in which the TTG is unable to resolve the APN and all remaining disconnect reasons before the call is in the CONNECTED state. Availability: IPSec/SSL. | Int32
sess-ttlbytessent | Description: Total number of bytes sent. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-ttlbytesrcvd | Description: Total number of bytes received. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-ttlpktsent | Description: Total number of packets sent. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-ttlpktrcvd | Description: Total number of packets received. This variable is proprietary. Availability: IPSec/SSL. | Int32
sess-ttlpktviolations | Description: Total number of packet violations. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-rxttlsrvrpassthru | Description: Total number of EAP messages received from the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-rxsuccsrvrpassthru | Description: Total number of EAP-Success messages received from the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-rxfailsrvrpassthru | Description: Total number of EAP-Failure messages received from the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-rxchalsrvrpassthru | Description: Total number of EAP challenge messages sent to the EAP server in pass-through mode. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-txttlsrv | Description: Total number of EAP messages transmitted to the EAP server. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-txinitrequest | Description: Total number of EAP request messages forwarded to the EAP server for initial request. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-txreqfwd | Description: Total number of EAP messages transmitted to the EAP server for forward request. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-rxmobilepassthru | Description: Total number of EAP messages transmitted to the EAP server in pass-through mode for mobile node. This variable is proprietary. Availability: IPSec/SSL. | Int32
eap-rxmobilediscarded | Description: Total number of EAP messages transmitted to the EAP server that were discarded. This variable is proprietary. Availability: IPSec/SSL. | Int32
mt-txdatabyteuplink | Description: SSL micro-tunneling: Uplink data bytes sent. This variable is proprietary. Availability: SSL. | Int64
mt-databyteuplinkdropped | Description: SSL micro-tunneling: Uplink data bytes dropped. This variable is proprietary. Availability: SSL. | Int64
mt-uldroppedd-nonconnectedstate | Description: SSL micro-tunneling: Uplink data bytes dropped due to non-connected state. This variable is proprietary. Availability: SSL. | Int64
mt-uldroppedd-transstackbuffoverflow | Description: SSL micro-tunneling: Uplink data bytes dropped due to transport stack buffer over flow. This variable is proprietary. Availability: SSL. | Int64
mt-uldroppedd-incorrectdestip | Description: SSL micro-tunneling: Uplink data bytes dropped due to incorrect destination IP address. This variable is proprietary. Availability: SSL. | Int64
mt-uldroppedd-transtackfailed | Description: SSL micro-tunneling: Uplink data bytes dropped due to transport stack failed to send. This variable is proprietary. Availability: SSL. | Int64
mt-uldroppedd-sessnotfoundforsockid | Description: SSL micro-tunneling: Uplink data bytes dropped due to session not found for sock-id. This variable is proprietary. Availability: SSL. | Int64
mt-txdatabytedownlink | Description: SSL micro-tunneling: Downlink data bytes sent. This variable is proprietary. Availability: SSL. | Int64
mt-rxttlopenreq | Description: SSL micro-tunneling: Total OPEN requests received. This variable is proprietary. Availability: SSL. | Int32
mt-rxopenreqprocessed | Description: SSL micro-tunneling: OPEN requests processed. This variable is proprietary. Availability: SSL. | Int32
mt-rxopenreqdropped | Description: SSL micro-tunneling: OPEN requests dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlopenresp | Description: SSL micro-tunneling: Total OPEN responses sent. This variable is proprietary. Availability: SSL. | Int32
mt-txopenrespaccept | Description: SSL micro-tunneling: OPEN responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-txopenresprej | Description: SSL micro-tunneling: OPEN responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-rxopenresp | Description: SSL micro-tunneling: OPEN responses received. This variable is proprietary. Availability: SSL. | Int32
mt-rxttlnamreq | Description: SSL micro-tunneling: Total NAM requests received. This variable is proprietary. Availability: SSL. | Int32
mt-rxnamreqprocessed | Description: SSL micro-tunneling: NAM requests processed. This variable is proprietary. Availability: SSL. | Int32
mt-rxnamreqdropped | Description: SSL micro-tunneling: NAM requests dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlnamresp | Description: SSL micro-tunneling: Total NAM responses sent. This variable is proprietary. Availability: SSL. | Int32
mt-txnamrespaccept | Description: SSL micro-tunneling: NAM responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-txnamresprej | Description: SSL micro-tunneling: NAM responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-rxnamresp | Description: SSL micro-tunneling: NAM responses received. This variable is proprietary. Availability: SSL. | Int32
mt-rxttlauthreq | Description: SSL micro-tunneling: Total AUTH requests received. This variable is proprietary. Availability: SSL. | Int32
mt-rxauthreqprocessed | Description: SSL micro-tunneling: AUTH requests processed. This variable is proprietary. Availability: SSL. | Int32
mt-rxauthreqdropped | Description: SSL micro-tunneling: AUTH requests dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlauthresp | Description: SSL micro-tunneling: Total AUTH responses sent. This variable is proprietary. Availability: SSL. | Int32
mt-txauthrespaccept | Description: SSL micro-tunneling: AUTH responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-txauthresprej | Description: SSL micro-tunneling: AUTH responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-rxauthresp | Description: SSL micro-tunneling: AUTH responses received. This variable is proprietary. Availability: SSL. | Int32
mt-rxttlrecvreq | Description: SSL micro-tunneling: Total RECV requests received. This variable is proprietary. Availability: SSL. | Int32
mt-rxrecvreqprocessed | Description: SSL micro-tunneling: RECV requests processed. This variable is proprietary. Availability: SSL. | Int32
mt-rxrecvreqdropped | Description: SSL micro-tunneling: RECV requests dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlrecvresp | Description: SSL micro-tunneling: Total RECV responses sent. This variable is proprietary. Availability: SSL. | Int32
mt-txrecvrespaccept | Description: SSL micro-tunneling: RECV responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-txrecvresprej | Description: SSL micro-tunneling: RECV responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-rxrecvresp | Description: SSL micro-tunneling: RECV responses received. This variable is proprietary. Availability: SSL. | Int32
mt-rxttlclosereq | Description: SSL micro-tunneling: Total CLOSE requests received. This variable is proprietary. Availability: SSL. | Int32
mt-rxclosereqprocessed | Description: SSL micro-tunneling: CLOSE requests processed. This variable is proprietary. Availability: SSL. | Int32
mt-rxclosereqdropped | Description: SSL micro-tunneling: CLOSE requests dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlclosereq | Description: SSL micro-tunneling: Total CLOSE requests sent. This variable is proprietary. Availability: SSL. | Int32
mt-txclosereqdispatch | Description: SSL micro-tunneling: CLOSE requests dispatched. This variable is proprietary. Availability: SSL. | Int32
mt-rxttlcloseresp | Description: SSL micro-tunneling: Total CLOSE responses received. This variable is proprietary. Availability: SSL. | Int32
mt-rxcloserespaccept | Description: SSL micro-tunneling: CLOSE responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-rxcloseresprej | Description: SSL micro-tunneling: CLOSE responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-rxcloserespdropped | Description: SSL micro-tunneling: CLOSE responses dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlcloseresp | Description: SSL micro-tunneling: Total CLOSE responses sent. This variable is proprietary. Availability: SSL. | Int32
mt-txcloserespaccept | Description: SSL micro-tunneling: CLOSE responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-txcloseresprej | Description: SSL micro-tunneling: CLOSE responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-rxttlsendreq | Description: SSL micro-tunneling: Total SEND requests received. This variable is proprietary. Availability: SSL. | Int32
mt-rxsendreqprocessed | Description: SSL micro-tunneling: SEND requests processed. This variable is proprietary. Availability: SSL. | Int32
mt-rxsendreqdropped | Description: SSL micro-tunneling: SEND requests dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlsendreq | Description: SSL micro-tunneling: Total SEND requests sent. This variable is proprietary. Availability: SSL. | Int32
mt-txsendreqdispatch | Description: SSL micro-tunneling: SEND requests dispatched. This variable is proprietary. Availability: SSL. | Int32
mt-rxttlsendresp | Description: SSL micro-tunneling: Total SEND responses received. This variable is proprietary. Availability: SSL. | Int32
mt-rxsendrespaccept | Description: SSL micro-tunneling: SEND responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-rxsendresprej | Description: SSL micro-tunneling: SEND responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-rxsendrespdropped | Description: SSL micro-tunneling: SEND responses dropped. This variable is proprietary. Availability: SSL. | Int32
mt-txttlsendresp | Description: SSL micro-tunneling: Total SEND responses sent. This variable is proprietary. Availability: SSL. | Int32
mt-txsendrespaccept | Description: SSL micro-tunneling: SEND responses accepted. This variable is proprietary. Availability: SSL. | Int32
mt-txsendresprej | Description: SSL micro-tunneling: SEND responses rejected. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-cannotcreatconn | Description: SSL micro-tunneling: OPEN Reject sent: cannot create connection. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-protonotsupported | Description: SSL micro-tunneling: OPEN Reject sent: protocol not supported. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-permdenied | Description: SSL micro-tunneling: OPEN Reject sent: permission denied. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-cannotcreatesockid | Description: SSL micro-tunneling: OPEN Reject sent: cannot create sock-id. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-badparam | Description: SSL micro-tunneling: OPEN Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-addrport-alreadyused | Description: SSL micro-tunneling: OPEN Reject sent: address or port already used. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-cannotconnectserver | Description: SSL micro-tunneling: OPEN Reject sent: cannot connect the server. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-hostnameunknown | Description: SSL micro-tunneling: OPEN Reject sent: hostname is unknown. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-authrequired | Description: SSL micro-tunneling: OPEN Reject sent: authentication required. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-undefined | Description: SSL micro-tunneling: OPEN Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-openrejtx-reserved | Description: SSL micro-tunneling: OPEN Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-namrejtx-versionnotsupported | Description: SSL micro-tunneling: OPEN Reject sent: version not supported. This variable is proprietary. Availability: SSL. | Int32
mt-namrejtx-servercannotcreateauth | Description: SSL micro-tunneling: OPEN Reject sent: server cannot create an authentication process. This variable is proprietary. Availability: SSL. | Int32
mt-namrejtx-badparameters | Description: SSL micro-tunneling: OPEN Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-namrejtx-undefined | Description: SSL micro-tunneling: NAM Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-namrejtx-reserved | Description: SSL micro-tunneling: NAM Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-authrejtx-authidunknown | Description: SSL micro-tunneling: AUTH Reject sent: the auth-id is unknown. This variable is proprietary. Availability: SSL. | Int32
mt-authrejtx-cannotconntoauthserver | Description: SSL micro-tunneling: AUTH Reject sent: cannot connect to authentication server. This variable is proprietary. Availability: SSL. | Int32
mt-authrejtx-badparam | Description: SSL micro-tunneling: AUTH Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-authrejtx-undefined | Description: SSL micro-tunneling: AUTH Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-authrejtx-reserved | Description: SSL micro-tunneling: AUTH Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-recvrejtx-sockidunknown | Description: SSL micro-tunneling: RECV Reject sent: the sock-id is unknown. This variable is proprietary. Availability: SSL. | Int32
mt-recvrejtx-connlost | Description: SSL micro-tunneling: RECV Reject sent: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
mt-recvrejtx-permissiondenied | Description: SSL micro-tunneling: RECV Reject sent: permission denied. This variable is proprietary. Availability: SSL. | Int32
mt-recvrejtx-badparameters | Description: SSL micro-tunneling: RECV Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-recvrejtx-undefined | Description: SSL micro-tunneling: RECV Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-recvrejtx-unreserved | Description: SSL micro-tunneling: RECV Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-closerejtx-sockidunknown | Description: SSL micro-tunneling: RECV Reject sent: the sock-id is unknown. This variable is proprietary. Availability: SSL. | Int32
mt-closerejtx-connlost | Description: SSL micro-tunneling: CLOSE Reject sent: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
mt-closerejtx-badparameters | Description: SSL micro-tunneling: CLOSE Reject sent: the bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-closerejtx-undefined | Description: SSL micro-tunneling: CLOSE Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-closerejtx-unreserved | Description: SSL micro-tunneling: CLOSE Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-closerejrx-sockidunknown | Description: SSL micro-tunneling: CLOSE Reject received: sock-id unknown. This variable is proprietary. Availability: SSL. | Int32
mt-closerejrx-connlost | Description: SSL micro-tunneling: CLOSE Reject received: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
mt-closerejrx-badparameters | Description: SSL micro-tunneling: CLOSE Reject received: bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-closerejrx-undefined | Description: SSL micro-tunneling: CLOSE Reject received: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-closerejrx-unreserved | Description: SSL micro-tunneling: CLOSE Reject received: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejtx-sockidunknown | Description: SSL micro-tunneling: SEND Reject sent: sock-id unknown. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejtx-connlost | Description: SSL micro-tunneling: SEND Reject sent: the connection is lost. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejtx-permissiondenied | Description: SSL micro-tunneling: SEND Reject sent: permission denied. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejtx-badparam | Description: SSL micro-tunneling: SEND Reject sent: bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejtx-undefined | Description: SSL micro-tunneling: SEND Reject sent: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejtx-reserved | Description: SSL micro-tunneling: SEND Reject sent: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejrx-sockidunknown | Description: SSL micro-tunneling: SEND Reject received: sock-id unknown. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejrx-connlost | Description: SSL micro-tunneling: SEND Reject received: connection is lost. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejrx-permissiondenied | Description: SSL micro-tunneling: SEND Reject received: permission denied. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejrx-badparam | Description: SSL micro-tunneling: SEND Reject received: bad parameters. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejrx-undefined | Description: SSL micro-tunneling: SEND Reject received: undefined. This variable is proprietary. Availability: SSL. | Int32
mt-sendrejrx-reserved | Description: SSL micro-tunneling: SEND Reject received: reserved. This variable is proprietary. Availability: SSL. | Int32
mt-pktdiscardstat-unknownversion | Description: SSL micro-tunneling: Packets discarded statistics: unknown version. This variable is proprietary. Availability: SSL. | Int32
mt-pktdiscardstat-unknownmsgtype | Description: SSL micro-tunneling: Packets discarded statistics: unknown message type. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-open-decodefaildropped | Description: SSL micro-tunneling: Packets discarded statistics: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-open-decodefailrej | Description: SSL micro-tunneling: Packets discarded statistics: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-open-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: OPEN: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-open-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: OPEN: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respopen-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP OPEN: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respopen-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP OPEN: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-close-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-close-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-close-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-close-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: CLOSE: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respclose-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP CLOSE: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respclose-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP CLOSE: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-nam-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: NAM: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-nam-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: NAM: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-nam-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: NAM: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-nam-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: NAM: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respnam-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP NAM: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respnam-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP NAM: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-auth-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: AUTH: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-auth-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: AUTH: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-auth-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: AUTH: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-auth-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: AUTH: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respauth-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP AUTH: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respauth-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP AUTH: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-recv-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RECV: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-recv-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: RECV: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-recv-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RECV: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-recv-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: RECV: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-resprecv-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP RECV: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-resprecv-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP RECV: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-send-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: SEND: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-send-decodefailrej | Description: SSL micro-tunneling: Messages denied statistics: SEND: decoding failed, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-send-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: SEND: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-send-uknownctxtrej | Description: SSL micro-tunneling: Messages denied statistics: SEND: unknown context, rejected. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respsend-decodefaildropped | Description: SSL micro-tunneling: Messages denied statistics: RESP SEND: decoding failed, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respsend-uknownctxtdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP SEND: unknown context, dropped. This variable is proprietary. Availability: SSL. | Int32
mt-msgdenied-respunknowncommdropped | Description: SSL micro-tunneling: Messages denied statistics: RESP to unknown command dropped. This variable is proprietary. Availability: SSL. | Int32
utcp_access_raw_pkts_to_stack | Not supported in this release. | Int64
utcp_nw_raw_pkts_to_stack | Not supported in this release. | Int64
utcp_access_raw_bytes_to_stack | Not supported in this release. | Int64
utcp_access_raw_pkts_from_stack | Not supported in this release. | Int64
utcp_nw_raw_pkts_from_stack | Not supported in this release. | Int64
utcp_access_raw_bytes_from_stack | Not supported in this release. | Int64
utcp_nw_raw_bytes_from_stack | Not supported in this release. | Int64
utcp_access_sockets_opened | Not supported in this release. | Int64
utcp_nw_sockets_opened | Not supported in this release. | Int64
utcp_access_sockets_open_fail | Not supported in this release. | Int64
utcp_nw_sockets_open_fail | Not supported in this release. | Int64
utcp_access_connect_attempt | Not supported in this release. | Int64
utcp_nw_connect_attempt | Not supported in this release. | Int64
utcp_access_listening_socket | Not supported in this release. | Int64
utcp_nw_listening_socket | Not supported in this release. | Int64
utcp_access_listen_fail | Not supported in this release. | Int64
utcp_nw_listen_fail | Not supported in this release. | Int64
utcp_access_bind_success | Not supported in this release. | Int64
utcp_nw_bind_success | Not supported in this release. | Int64
utcp_access_bind_fail | Not supported in this release. | Int64
utcp_nw_bind_fail | Not supported in this release. | Int64
utcp_access_accept_success | Not supported in this release. | Int64
utcp_nw_accept_success | Not supported in this release. | Int64
utcp_access_accept_fail | Not supported in this release. | Int64
utcp_nw_accept_fail | Not supported in this release. | Int64
utcp_access_send_success | Not supported in this release. | Int64
utcp_nw_send_success | Not supported in this release. | Int64
utcp_access_send_fail | Not supported in this release. | Int64
utcp_nw_send_fail | Not supported in this release. | Int64
utcp_access_send_partial | Not supported in this release. | Int64
utcp_nw_send_partial | Not supported in this release. | Int64
utcp_access_sendto_success | Not supported in this release. | Int64
utcp_nw_sendto_success | Not supported in this release. | Int64
utcp_access_sendto_fail | Not supported in this release. | Int64
utcp_nw_sendto_fail | Not supported in this release. | Int64
utcp_access_sendto_partial | Not supported in this release. | Int64
utcp_nw_sendto_partial | Not supported in this release. | Int64
utcp_access_recv_attempt | Not supported in this release. | Int64
utcp_nw_recv_attempt | Not supported in this release. | Int64
utcp_access_recv_fail | Not supported in this release. | Int64
utcp_nw_recv_fail | Not supported in this release. | Int64
utcp_access_recvfrom_attempt | Not supported in this release. | Int64
utcp_nw_recvfrom_attempt | Not supported in this release. | Int64
utcp_access_current_open_sockets | Not supported in this release. | Int32
utcp_nw_current_open_sockets | Not supported in this release. | Int32
utcp_access_current_alloc_tcpvect | Not supported in this release. | Int32
utcp_nw_current_alloc_tcpvect | Not supported in this release. | Int32
utcp_access_tcpinsegs | Not supported in this release. | Int64
utcp_nw_tcpinsegs | Not supported in this release. | Int64
utcp_access_tcpinbytes | Not supported in this release. | Int64
utcp_nw_tcpinbytes | Not supported in this release. | Int64
utcp_access_tcpinerrs | Not supported in this release. | Int64
utcp_nw_tcpinerrs | Not supported in this release. | Int64
utcp_access_tcpinretransseg | Not supported in this release. | Int64
utcp_nw_tcpinretransseg | Not supported in this release. | Int64
utcp_access_tcpinretransbytes | Not supported in this release. | Int64
utcp_nw_tcpinretransbytes | Not supported in this release. | Int64
utcp_access_tcpoutsegs | Not supported in this release. | Int64
utcp_nw_tcpoutsegs | Not supported in this release. | Int64
utcp_access_tcpoutrsts | Not supported in this release. | Int64
utcp_nw_tcpoutrsts | Not supported in this release. | Int64
utcp_access_tcpretranssegs | Not supported in this release. | Int64
utcp_nw_tcpretranssegs | Not supported in this release. | Int64
utcp _access_tcpretransbytes | Not supported in this release. | Int64
utcp_nw_tcpretransbytes | Not supported in this release. | Int64
utcp_access_tcpinpartialretransseg | Not supported in this release. | Int64
utcp_nw_tcpinpartialretransseg | Not supported in this release. | Int64
utcp_access_tcpinpartialretransbytes | Not supported in this release. | Int64
utcp_nw_tcpinpartialretransbytes | Not supported in this release. | Int64
utcp_access_tcpinoooseg | Not supported in this release. | Int64
utcp_nw_tcpinoooseg | Not supported in this release. | Int64
utcp_access_tcpinooobytes | Not supported in this release. | Int64
utcp_nw_tcpinooobytes | Not supported in this release. | Int64
utcp_access_tcpinoooretransseg | Not supported in this release. | Int64
utcp_nw_tcpinoooretransseg | Not supported in this release. | Int64
utcp_access_tcpinoooretransbytes | Not supported in this release. | Int64
utcp_nw_tcpinoooretransbytes | Not supported in this release. | Int64
utcp_access_tcpinooosuccessseg | Not supported in this release. | Int64
utcp_nw_tcpinooosuccessseg | Not supported in this release. | Int64
utcp_access_tcpinooosuccessbytes | Not supported in this release. | Int64
utcp_nw_tcpinooosuccessbytes | Not supported in this release. | Int64
utcp_access_tcpincsumerrseg | Not supported in this release. | Int64
utcp_nw_tcpincsumerrseg | Not supported in this release. | Int64
utcp_access_tcpincsumerrbytes | Not supported in this release. | Int64
utcp_nw_tcpincsumerrbytes | Not supported in this release. | Int64
utcp_access_tcpactiveopens | Not supported in this release. | Int64
utcp_nw_tcpactiveopens | Not supported in this release. | Int64
utcp_nw_tcppassiveopens | Not supported in this release. | Int64
utcp_access_tcpattemptfails | Not supported in this release. | Int64
utcp_nw_tcpattemptfails | Not supported in this release. | Int64
utcp_access_tcpestabresets | Not supported in this release. | Int64
utcp_nw_tcpestabresets | Not supported in this release. | Int64
utcp_access_tcpcurrestab | Not supported in this release. | Int64
utcp_nw_tcpcurrestab | Not supported in this release. | Int64
utcp_access_ipinreceives | Not supported in this release. | Int64
utcp_nw_ipinreceives | Not supported in this release. | Int64
utcp_access_ipinhdrerrors | Not supported in this release. | Int64
utcp_nw_ipinhdrerrors | Not supported in this release. | Int64
utcp_access_ipinunknownprotos | Not supported in this release. | Int64
utcp_nw_ipinunknownprotos | Not supported in this release. | Int64
utcp_access_ipindiscards | Not supported in this release. | Int64
utcp_nw_ipindiscards | Not supported in this release. | Int64
utcp_access_ipinaddrerrors | Not supported in this release. | Int64
utcp_nw_ipinaddrerrors | Not supported in this release. | Int64
utcp_access_ipoutrequests | Not supported in this release. | Int64
utcp_nw_ipoutrequests | Not supported in this release. | Int64
utcp_access_ipoutdiscards | Not supported in this release. | Int64
utcp_nw_ipoutdiscards | Not supported in this release. | Int64
utcp_access_ipoutnoroutes | Not supported in this release. | Int64
utcp_nw_ipoutnoroutes | Not supported in this release. | Int64
utcp_access_ipreasmtimeout | Not supported in this release. | Int64
utcp_nw_ipreasmtimeout | Not supported in this release. | Int64
utcp_access_ipreasmoks | Not supported in this release. | Int64
utcp_nw_ipreasmoks | Not supported in this release. | Int64
utcp_access_ipreasmfails | Not supported in this release. | Int64
utcp_nw_ipreasmfails | Not supported in this release. | Int64
utcp_access_ipfragoks | Not supported in this release. | Int64
utcp_nw_ipfragoks | Not supported in this release. | Int64
utcp_access_ipfragfails | Not supported in this release. | Int64
utcp_nw_ipfragfails | Not supported in this release. | Int64
utcp_access_ipfragcreates | Not supported in this release. | Int64
utcp_nw_ipfragcreates | Not supported in this release. | Int64
utcp_access_iproutingdiscards | Not supported in this release. | Int64
utcp_nw_iproutingdiscards | Not supported in this release. | Int64
utcp_access_udpnoports | Not supported in this release. | Int64
utcp_nw_udpnoports | Not supported in this release. | Int64
utcp_access_udpinerrors | Not supported in this release. | Int64
utcp_nw_udpinerrors | Not supported in this release. | Int64
utcp_access_udpindatagrams | Not supported in this release. | Int64
utcp_nw_udpindatagrams | Not supported in this release. | Int64
utcp_access_udpoutdatagrams | Not supported in this release. | Int64
utcp_nw_udpoutdatagrams | Not supported in this release. | Int64
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.