# show session

This chapter describes the output of the show session command variants.
show session counters historical all
Table 1. show session counters historical all Command Output Descriptions

Header | Description
--- | ---
Intv | The identification number of the sample interval.
Timestamp | The approximate time the data was gathered. It is in the format YYYY:MM:DD:HH:MM:SS.
Number of Calls
Arrived | Displays data for “total calls arrived” counters.
Rejected | Displays data for “total calls rejected” counters.
Connected | Displays data for “total calls connected” counters.
Disconn | Displays data for “total calls disconnected” counters.
Failed | Displays data for “total calls failed” counters.
Handoffs | Displays data for “total handoffs” counters.
Renewals | Displays data for “total renewal” counters.
(A+R+D+F+H+R) CallOps | Displays data for all call operations. This is a calculated value based on the following formula: (arrived + rejected + disconnected + failed + handoffs + renewals)

show session disconnect-reasons
Table 2. show session disconnect-reasons Header Descriptions

Field | Description
--- | ---
Session Disconnect Statistics
Total Disconnects | The total number of sessions disconnected since the system was started or since the last time that session disconnect reasons was cleared.
Disconnect Reason | The reason sessions were disconnected. Only reasons that have disconnects associated with them are listed.
Num Disc | The number of sessions disconnected for the reason.
Percentage | The percentage of total disconnects.

show session disconnect-reasons verbose
Table 3. show session disconnect-reasons verbose Header Descriptions

Header | Description
--- | ---
Total Disconnects | The total number of sessions disconnected since the system was started or since the last time that session disconnect reasons was cleared.
Disconnect Reason | The reason sessions were disconnected. Only reasons that have disconnects associated with them are listed unless the verbose keyword is specified.
Num Disc | The number of sessions disconnected for the reason.
Percentage | The percentage of total disconnects.

In the following table, the indicator number at the end of the disconnect field name will vary depending upon the software build in which the show session disconnect-reason command is issued.
Table 4. show session disconnect-reasons Fields Descriptions

Field | Description
--- | ---
Unknown (0) | The total number of sessions disconnected due to unknown reason.
Admin-disconnect (1) | The total number of sessions disconnected due to any of the following reasons: Sessions disconnected when the Administrator issues the clear subscribers all CLI command. Sessions disconnected by ECS due to any of the following reasons: Bearer does not contain active rules—when the last bearer has no rules left as part of some PCRF trigger. Charging-action has the flow action parameter configured as terminate-session. Sessions disconnected by Diameter Credit Control Application (DCCA) due to any of the following reasons: Result code 4010 or 4012 is received at the command level, and for CCR-Initial and CCR-Update Credit Control Failure Handling (CCFH) is configured as Terminate or Retry-and-Terminate. Result code 5003 or 5030 is received at the command level. Abort-Session-Request message is received.
Remote-disconnect (2) | The total number of sessions disconnected by the remote system.
Local-disconnect (3) | The total number of sessions disconnected by local system.
No-resource (4) | The total number of sessions disconnected due to non-availability of resources.
Service-limit-exceeded (5) | The total number of sessions disconnected due to exceed in service limit.
PPP-LCP-negotiation-failed (6) | The total number of sessions disconnected due to LCP negotiation failed.
PPP-LCP-no-response (7) | The total number of sessions disconnected due to no response in PPP-LCP session.
PPP-LCP-loopback-detected (8) | The total number of sessions disconnected due to loop back detected in PPP-LCP.
PPP-LCP-max-retry-reached (9) | The total number of sessions disconnected due to maximum retries in PPP-LCP session.
PPP-LCP-echo-failed (10) | The total number of sessions disconnected due to PPP-LCP echo not received.
PPP-Auth-failed (11) | The total number of sessions disconnected due to authorization failed in PPP.
PPP-Auth-failed-no-AAA-response (12) | The total number of sessions disconnected due to authorization failed by no response on AAA server.
PPP-Auth-failed-no-peer-response (13) | The total number of sessions disconnected due to PPP authorization failed on no peer response.
PPP-Auth-failed-max-retry-reached (14) | The total number of sessions disconnected due to PPP authorization failed and reaching maximum retries limit.
Invalid-AAA-attr-in-auth-response (15) | The total number of sessions disconnected due to invalid AAA attributes in authorization response.
Could-not-apply-subscriber-ACL (16) | The total number of sessions disconnected due to inability in applying subscriber's Access Control List (ACL).
Could-not-provide-service (17) | The total number of sessions disconnected due to service is not available.
AAA-return-IP-address-not-valid (18) | The total number of sessions disconnected due to return IP address from AAA server is invalid.
Pool-IP-address-not-valid (19) | The total number of sessions disconnected due to IP address in pool is invalid.
PPP-IPCP-negotiation-failed (20) | The total number of sessions disconnected due to PPP-IPCP negotiation failed.
PPP-IPCP-no-response (21) | The total number of sessions disconnected due to no response in PPP-IPCP.
PPP-IPCP-max-retry-reached (22) | The total number of sessions disconnected due to maximum retries in PPP-IPCP session.
No-IPV4-address-for-subscriber (23) | The total number of sessions disconnected due to no IPv4 address are available for subscriber.
Inactivity-timeout (24) | The total number of sessions disconnected due to system time out limit for silence (ideal) reached.
Absolute-timeout (25) | The total number of sessions disconnected due to timeout in complete session.
Max-data-limit-exceeded (26) | The total number of sessions disconnected due to maximum data limit exceeded.
Invalid-source-IPV4-address (27) | The total number of sessions disconnected due to invalid IPv4 address of subscriber.
MSID-auth-failed (28) | The total number of sessions disconnected due to MSID authentication failed.
MSID-auth-failed-no-aaa-response (29) | The total number of sessions disconnected due to MSID authentication failed and/or no response from AAA server.
A11-max-retry-reached (30) | The total number of sessions disconnected due to maximum limit for retries reached for A11 interface.
A11-lifetime-expired (31) | The total number of sessions disconnected due to A11 interface lifetime expired.
A11-msg-integrity-failure (32) | The total number of sessions disconnected due to failure in message integrity in A11 interface.
PPP-LCP-remote-disconnect (33) | The total number of sessions disconnected due to PPP-LCP remote disconnect.
Session-setup-timeout (34) | The total number of sessions disconnected due to timeout in setting up of session.
PPP-keepalive-failure (35) | The total number of sessions disconnected due to PPP keepalive attribute failure.
Flow-add-failed (36) | The total number of sessions disconnected due to fail in adding flow to session.
Call-type-detection-failed (37) | The total number of sessions disconnected due to failure in call type detection.
Wrong-ipcp-params (38) | The total number of sessions disconnected due to IPCP parameters are wrong.
MIP-remote-dereg (39) | The total number of sessions disconnected due to de-registration of Mobile IP on remote system.
MIP-lifetime-expiry (40) | The total number of sessions disconnected due to expiry of Mobile IP life time.
MIP-proto-error (41) | The total number of sessions disconnected due to protocol error in Mobile IP.
MIP-auth-failure (42) | The total number of sessions disconnected due to Mobile IP authentication failure.
MIP-reg-timeout (43) | The total number of sessions disconnected due to registration request timeout.
Invalid-dest-context (44) | The total number of sessions disconnected due to invalid destination context.
Source-context-removed (45) | The total number of sessions disconnected due to source context is removed from system.
Destination-context-removed (46) | The total number of sessions disconnected due to destination context is removed from system.
Required-service-address-unavailable (47) | The total number of sessions disconnected due to unavailability of required service address.
demux-mgr-failed-could-not-restart (48) | The total number of sessions disconnected due to failure in demux-mgr.
internal-error (49) | The total number of sessions disconnected due to some internal system error.
AAA-context-removed (50) | The total number of sessions disconnected due to AAA context is removed from system.
invalid-service-type (51) | The total number of sessions disconnected due to invalid service type.
mip-relay-req-failed (52) | The total number of sessions disconnected due to failure in Mobile IP relay request.
mip-rcvd-relay-failure (53) | The total number of sessions disconnected due to failure in Mobile IP received.
ppp_restart_inter_pdsn_handoff (54) | The total number of sessions disconnected due to restart in inter PDSN handoff.
gre-key-mismatch (55) | The total number of sessions disconnected due to mismatch in Generic Routing Encapsulation (GRE) key.
invalid-tunnel-context (56) | The total number of sessions disconnected due to invalid Tunnel context.
no-peer-lns-address (57) | The total number of sessions disconnected due to no peer LNS address
failed-tunnel-connect (58) | The total number of sessions disconnected due to failure in Tunnel connect.
l2tp-tunnel-disconnect-remote (59) | The total number of sessions disconnected due to tunnel disconnected by remote system.
l2tp-tunnel-timeout (60) | The total number of sessions disconnected due to tunnel timeout.
l2tp-protocol-error-remote (61) | The total number of sessions disconnected due to protocol error on remote system.
l2tp-protocol-error-local (62) | The total number of sessions disconnected due to protocol error on local system.
l2tp-auth-failed-remote (63) | The total number of sessions disconnected due to authorization failed on remote system.
l2tp-auth-failed-local (64) | The total number of sessions disconnected due to authorization failed on local system
l2tp-try-another-lns-from-remote (65) | The total number of sessions disconnected due to remote system tried for another LNS.
l2tp-no-resource-local (66) | The total number of sessions disconnected due to non-availability of resource on local system.
l2tp-no-resource-remote (67) | The total number of sessions disconnected due to non-availability of resource on remote system.
l2tp-tunnel-disconnect-local (68) | The total number of sessions disconnected due to tunnel disconnected on local system.
l2tp-admin-disconnect-remote (69) | The total number of sessions disconnected by administrator on remote system.
l2tpmgr-reached-max-capacity (70) | The total number of sessions disconnected due to L2TP Manager logging facility reached to maximum logging capacity.
MIP-Reg-Revocation (71) | The total number of sessions disconnected due to a failure in Mobile IP registration revocation.
path-failure (72) | The total number of sessions disconnected due to path failure in connecting session.
Dhcp-Relay-IP-Validation-Failed (73) | The total number of sessions disconnected due to a failure with the validation of the IP addresses with DHCP relay method.
Gtp-unknown-pdp-addr-or-pdp-type (74) | The total number of sessions disconnected due to unknown PDP address or PDP type.
Gtp-all-dynamic-pdp-addr-occupied (75) | The total number of sessions disconnected due to all dynamic PDP addresses are occupied and no PDP address is available to allocate.
Gtp-no-memory-is-available (76) | The total number of sessions disconnected due to out of memory problem.
dhcp-relay-static-ip-addr-not-allowed (77) | The total number of sessions disconnected due to the mobile requesting the use of a static IP address when static IP address requests are not allowed.
dhcp-no-ip-addr-allocated (78) | The total number of sessions disconnected as no IP address is allocated on DHCP Server.
dhcp-ip-addr-allocation-tmr-exp (79) | The total number of sessions disconnected due to time expired for IP address allocation on DHCP Server.
dhcp-ip-validation-failed (80) | The total number of sessions disconnected due to a failure with the validation of the IP address. This occurs because the IP address returned by DHCP Server is not present in the static pool in the destination context.
dhcp-static-addr-not-allowed (81) | The total number of sessions disconnected due to a failure with IP address in the static pool on destination context is not allowed by DHCP Server.
dhcp-ip-addr-not-available-at-present (82) | The total number of sessions disconnected due to non availability of IP address on DHCP Server.
dhcp-lease-expired (83) | The total number of sessions disconnected due to expiration of IP address lease time.
lpool-ip-validation-failed (84) | The total number of sessions disconnected due to validation failure of IP address in IP pool.
lpool-static-ip-addr-not-allowed (85) | The total number of sessions disconnected due to specified static IP address is not allowed in IP pool.
static-ip-validation-failed (86) | The total number of sessions disconnected due to a failure in validation of static IP address on remote system.
static-ip-addr-not-present (87) | The total number of sessions disconnected due to allocated static address is removed or not available.
static-ip-addr-not-allowed (88) | The total number of sessions disconnected due to prohibition of defined static IP address.
radius-ip-validation-failed (89) | The total number of sessions disconnected due to a failure in IP address validation on RADIUS.
radius-ip-addr-not-provided (90) | The total number of sessions disconnected due to IP address is not provided by RADIUS.
invalid-ip-addr-from-sgsn (91) | The total number of sessions disconnected due to invalid IP address received from SGSN.
no-more-sessions-in-aaa (92) | The total number of sessions disconnected due to sessions cleared in AAA.
ggsn-aaa-auth-req-failed (93) | The total number of sessions disconnected due to authentication request failure between GGSN and AAA server.
conflict-in-ip-addr-assignment (94) | The total number of sessions disconnected due to conflict in IP address assignment.
apn-removed (95) | The total number of sessions disconnected due to APN removed during session.
credits-used-bytes-in (96) | The total number of sessions disconnected due to exceeding the incoming data/bytes credit.
credits-used-bytes-out (97) | The total number of sessions disconnected due to exceeding the outgoing data/bytes credit.
credits-used-bytes-total (98) | The total number of sessions disconnected due to exceeding the total data/bytes credit.
prepaid-failed (99) | The total number of sessions disconnected due to a failure in processing prepaid account information.
l2tp-ipsec-tunnel-failure (100) | The total number of sessions disconnected due to the IPSec tunnel being failed to connect.
l2tp-ipsec-tunnel-disconnected (101) | The total number of sessions disconnected due to the IPSec tunnel being disconnected.
mip-ipsec-sa-inactive (102) | The total number of sessions disconnected due to in active security association (sa) of IPSec for specific Mobile IP address.
Long-duration-timeout (103) | The total number of sessions disconnected due to the expiration of the configured long-duration timer.
proxy-mip-registration-failure (104) | The total number of Proxy Mobile IP sessions disconnected due to Registration failures.
proxy-mip-binding-update (105) | The total number of Proxy Mobile IP sessions disconnected due to errors occurring during binding updates.
proxy-mip-inter-pdsn-handoff-require-ip-address (106) | The total number of Proxy Mobile IP sessions disconnected due to the mobile not providing the IP address it was assigned during IPCP negotiations resulting from inter-PDSN handoffs.
proxy-mip-inter-pdsn-handoff-mismatched-address (107) | The total number of Proxy Mobile IP sessions disconnected due to the mobile providing an IP address other than what it was assigned during IPCP negotiations resulting from inter-PDSN handoffs.
Local-purge (108) | The total number of sessions disconnected due to a locally-initiated purge.
failed-update-handoff (109) | The total number of sessions disconnected due to failure in update handoff.
closed_rp-handoff-complete (110) | The total number of sessions disconnected due to handoff completed.
closed_rp-duplicate-session (111) | The total number of sessions disconnected due to duplicate session.
closed_rp-handoff-session-not-found (112) | The total number of sessions disconnected due to hand off session not found.
closed_rp-handoff-failed (113) | The total number of sessions disconnected due to handoff failed for session.
pcf-monitor-keep-alive-failed (114) | The total number of sessions disconnected due to the expiration of the configured max-inactivity timer indicating that the PCF was unavailable.
call-internal-reject (115) | The total number of sessions disconnected due to call rejected internally.
call-restarted (116) | The total number of sessions disconnected due to call restarted on unknown reason.
a11-mn-ha-auth-failure (117) | The total number of sessions disconnected due to failure in authentication between Mobile node and Home Agent (HA).
a11-badly-formed (118) | The total number of sessions disconnected as A11 interface is formed badly.
a11-t-bit-not-set (119) | The total number of sessions disconnected due to t-bit is not set in interface.
a11-unsupported-vendor-id (120) | The total number of sessions disconnected due to unsupported vendor Id in interface.
a11-mismatched-id (121) | The total number of sessions disconnected due to mismatched Id in A11 interface.
mipha-dup-home-addr-req (122) | The total number of sessions disconnected due to duplicate home address request on HA.
mipha-dup-imsi-session (123) | The total number of sessions disconnected due to duplicate IMSI in session on HA.
ha-unreachable (124) | The total number of sessions disconnected due to unreachable HA.
IPSP-addr-in-use (125) | The total number of sessions disconnected due to IP Pool Sharing Protocol address is in use/not free on HA.
mipfa-dup-home-addr-req (126) | The total number of sessions disconnected due to duplicate home address request on FA.
mipha-ip-pool-busyout (127) | The total number of sessions disconnected due to IP pool busyout.
inter-pdsn-handoff (128) | The total number of sessions disconnected due to inter-PDSN handoff failure.
active-to-dormant (129) | The total number of sessions disconnected due to system enters to dormant state from active state.
ppp-renegotiation (130) | The total number of sessions disconnected due to failure/conflict in PPP renegotiation.
active-start-parameter-change (131) | The total number of sessions disconnected due to change in start parameters.
accounting-tariff-boundary (132) | The total number of sessions disconnected due to the closure of an accounting record based configured tariff time.
a11-disconnect-no-active-stop (133) | The total number of sessions disconnected due to A11 interface is not active or stopped.
nw-reachability-failed-reject (134) | The total number of sessions disconnected due to failure in network reachability and request rejected.
nw-reachability-failed-redirect (135) | The total number of sessions disconnected due to failure in network reachability and request redirected.
container-max-exceeded (136) | The total number of sessions disconnected due to the closure of an accounting record based on the configured maximum number of container changes being exceeded.
static-addr-not-allowed-in-apn (137) | The total number of sessions disconnected due to static IP address is not allowed in APN.
static-addr-required-by-radius (138) | The total number of sessions disconnected due to static IP address required by RADIUS.
static-addr-not-allowed-by-radius (139) | The total number of sessions disconnected due to static IP address is not allowed by RADIUS.
mip-registration-dropped (140) | The total number of sessions disconnected due to registration dropped for Mobile IP address.
counter-rollover (141) | The total number of sessions disconnected due to counter rollover.
constructed-nai-auth-failed (142) | The total number of sessions disconnected due to authentication failure in subscriber’s Network Access Identifier (NAI).
inter-pdsn-service-optimize-handoff-disabled (143) | The total number of sessions disconnected due to disabled inter-PDSN service optimization handoff.
gre-key-collision (144) | The total number of sessions disconnected due to collision in Generic Routing Encapsulation (GRE) key.
inter-pdsn-service-optimize-handoff-triggered (145) | The total number of sessions disconnected when inter PDSN service optimization handoff triggered.
intra-pdsn-handoff-triggered (146) | The total number of sessions disconnected when intra-PDSN service optimization handoff triggered.
delayed-abort-timer-expired (147) | The total number of sessions disconnected due to abort timer duration expired.
Admin-AAA-disconnect (148) | The total number of sessions disconnected as AAA server disconnected Administratively.
Admin-AAA-disconnect-handoff (149) | The total number of sessions disconnected due to AAA handoff disconnected Administratively.
PPP-IPV6CP-negotiation-failed (150) | The total number of sessions disconnected due to IPv6CP negotiation failed.
PPP-IPV6CP-no-response (151) | The total number of sessions disconnected due to no response during IPv6CP negotiation.
PPP-IPV6CP-max-retry-reached (152) | The total number of sessions disconnected due to maximum retries failed on IPv6CP negotiation.
PPP-Restart-Invalid-source-IPV4-address (153) | The total number of sessions disconnected due to PPP restarted by invalid Pv4 address of source.
a11-disconnect-handoff-no-active-stop (154) | The total number of sessions disconnected due to handoff in A11 interface is not active or stopped.
call-restarted-inter-pdsn-handoff (155) | The total number of sessions disconnected due to call restarted during inter PDSN handoff.
call-restarted-ppp-termination (156) | The total number of sessions disconnected due to call restarted on PPP termination.
mipfa-resource-conflict (157) | The total number of sessions disconnected due to resource conflict on FA.
failed-auth-with-charging-svc (158) | The total number of sessions disconnected due to authentication failure in charging services.
mipha-dup-imsi-session-purge (159) | The total number of sessions disconnected due to clearing of duplicate IMSI in session on HA.
mipha-rev-pending-newcall (160) | The total number of sessions disconnected due to revival of pending new calls.
volume-quota-reached (161) | The total number of sessions disconnected due to allocated data quota volume reached.
duration-quota-reached (162) | The total number of sessions disconnected due to time-out reached.
gtp-user-auth-failed (163) | The total number of sessions disconnected due to a failure in user/subscriber authentication.
MIP-Reg-Revocation-no-lcp-term (164) | The total number of sessions disconnected due to termination of an MIP Session for a Revocation being received from the HA and the PDSN is not configured to send a LCP Terminate Request.
MIP-private-ip-no-rev-tunnel (165) | The total number of sessions disconnected due to no reverse tunnel for MIP.
Invalid-Prepaid-AAA-attr-in-auth-response (166) | The total number of sessions disconnected due to invalid Prepaid attribute in authentication response.
mipha-prepaid-reset-dynamic-newcall (167) | The total number of MIP HA sessions disconnected due to receiving MIP registration with a home address of 0.0.0.0.
gre-flow-control-timeout (168) | The total number of RP sessions disconnected due to the PCF not removing flow control for a specified amount of time if GRE flow control for RP sessions is enabled.
mip-paaa-bc-query-not-found (169) | The total number of sessions that were disconnected because the binding cache was not found.
mipha-dynamic-ip-addr-not-available (170) | The total number of MIP HA sessions that were disconnected because a dynamic IP address was not available.
a11-mismatched-id-on-handoff (171) | The total number of sessions disconnected due to a mismatched ID in the A11 interface during a handoff.
a11-badly-formed-on-handoff (172) | The total number of sessions disconnected because the A11 interface is formed badly during a handoff.
a11-unsupported-vendor-id-on-handoff (173) | The total number of sessions disconnected due to unsupported vendor Id in the A11 interface during a handoff.
a11-t-bit-not-set-on-handoff (174) | The total number of sessions disconnected due to t-bit is not set in the A11 interface during a handoff.
MIP-Reg-Revocation-i-bit-on (175) | The total number of Mobile IP sessions disconnected at the PDSN/FA due to Revocation received from HA (with I bit set).
a11-RRQ-Deny-Max-Count (176) | The total number of sessions disconnected due to failures in processing A11-Registration-Request despite retries of the message by the PCF.
Dormant-Transition-During-Session-Setup (177) | The total number of sessions disconnected because they entered the dormant state during session setup.
PPP-Rem-Reneg-Disc-Always-Cfg (178) | The total number of PPP sessions disconnected because they were renegotiated by the remote side by sending LCP Conf-req/nak/ack and the “always” option was used for the remote-renegotiation disconnect command/attribute.
PPP-Rem-Reneg-Disc-NAI-MSID-Mismatch (179) | The total number of PPP sessions disconnected because they were renegotiated by the remote side by sending LCP Conf-req/nak/ack and the “nai-prefix-msid-mismatch” option was used for the remote-renegotiation disconnect command/attribute.
mipha-subscriber-ipsec-tunnel-down (180) | The total number of subscribers disconnected because the IPSec tunnel facilitating their sessions went down.
mipha-subscriber-ipsec-tunnel-failed (181) | The total number of subscribers disconnected because an IPSec tunnel failed to be established.
mipha-subscriber-ipsecmgr-death (182) | The total number of subscribers disconnected because the IPSec Manager software task facilitating their sessions crashed.
flow-is-deactivated (183) | The total number of sessions disconnected because their respective flow was deactivated.
ecs-license-exceeded (184) | The total number of sessions disconnected because the licensed session capacity for the Enhanced Charging Service feature has been exceeded.
IPSG-Auth-failed (185) | The total number of sessions disconnected because IPSG authentication failed.
driver-initiated (186) | The total number of sessions disconnected due to driver initiation.
ims-authorization-failed (187) | The total number of sessions disconnected because of IMS authorization failures.
service-instance-released (188) | The total number of sessions disconnected because they were released by the service instances facilitating them.
flow-released (189) | The total number of sessions disconnected because their respective flows were released.
ppp-renego-no-ha-addr (190) | The total number of sessions disconnect because no HA address was supplied during PPP renegotiation.
intra-pdsn-handoff (191) | The total number of sessions disconnected during an intra-PDSN service handoff.
overload-disconnect (192) | The total number of sessions disconnected because the configured overload-disconnect threshold has been exceeded.
css-service-not-found (193) | The total number of sessions because the CSS service specified for handling the session was not found.
Auth-failed (194) | This is not supported at this time.
dhcp-client-sent-release (195) | The total number of sessions disconnected because the DHCP client sent a release.
dhcp-client-sent-nak (196) | The total number of sessions disconnected because the DHCP client sent a negative acknowledge message.
msid-dhcp-chaddr-mismatch (197) | The total number of sessions disconnected because the DHCP Client Hardware (MAC) Address (CHADDR) does not match with MSID of the ASN-GW session.
link-broken(198) | The total number of sessions disconnected because the link between the SGSN and the GGSN is broken resulting in the termination of ongoing Diameter Credit-Control sessions with the DIAMETER_LINK_BROKEN termination-cause.
prog-end-timeout(199) | The total number of sessions disconnected because the allowed BCMCS program limit time expires.
qos-update-wait-timeout(200) | The total number of sessions disconnected because the PDSN failed to update QoS for them.
css-synch-cause(201) | The total number of sessions disconnected because the session-audit between the ACS Manager task and Session Manager disconnects any dangling sessions in the Session Manager.
Gtp-context-replacement(202) | The total number of sessions disconnected due to GTP context replacement.
PDIF-Auth-failed(203) | The total number of sessions disconnected due to PDIF authentication process unable to set up a secure IPSec tunnel to subscriber.
l2tp-unknown-apn(204) | The total number of sessions disconnected due to unknown APN in L2TP message.
ms-unexpected-network-reentry(205) | The total number of sessions disconnected due unexpected network reentry by MS in WiMAX network.
r6-invalid-nai(206) | The total number of sessions disconnected due invalid NAI in R6 message in WiMAX network.
eap-max-retry-reached(207) | The total number of sessions disconnected due maximum retry limit for EAP authentication exhausted in WiMAX network.
vbm-hoa-session-disconnected(208) | vbm-hoa-session-disconnected
vbm-voa-session-disconnected(209) | vbm-voa-session-disconnected
in-acl-disconnect-on-violation(210) | in-acl-disconnect-on-violation
eap-msk-lifetime-expiry(211) | The total number of sessions disconnected due to EAP Master Session Key lifetime expiry in WiMAX network.
eap-msk-lifetime-too-low(212) | The total number of sessions disconnected due to EAP Master Session Key lifetime is too less to allow session.
inter-service-handoff(213) | The total number of sessions disconnected due to inter-service handoff in WiMAX network.
r6-max-retry-reached(214) | The total number of sessions disconnected due to maximum retry limit for R6 message exhausted in WiMAX network.
r6-nwexit-recd(215) | The total number of sessions disconnected due to network exit message received on R6 interface in WiMAX network.
r6-dereg-req-recd(216) | The total number of sessions disconnected due to de-registration message received on R6 interface in WiMAX network.
r6-remote-failure(217) | The total number of sessions disconnected due to remote peer failure on R6 interface in WiMAX network.
r6r4-protocol-errors(218) | The total number of sessions disconnected due to protocol error on R6 and/or R4 interface in WiMAX network.
wimax-qos-invalid-aaa-attr(219) | The total number of sessions disconnected due to invalid AAA attributes for QoS to a subscriber in WiMAX network.
npu-gre-flows-not-available(220) | The total number of sessions disconnected due to requested NPU GRE flow is not available for a subscriber in WiMAX network.
r4-max-retry-reached(221) | The total number of sessions disconnected due to maximum retry limit for R4 message exhausted in WiMAX network.
r4-nwexit-recd(222) | The total number of sessions disconnected due to network exit message received on R4 interface in WiMAX network.
r4-dereg-req-recd(223) | The total number of sessions disconnected due to de-registration message received on R4 interface in WiMAX network.
r4-remote-failure(224) | The total number of sessions disconnected due to remote peer failure on R4 interface in WiMAX network.
ims-authorization-revoked(225) | The total number of sessions disconnected due to IMS authorization revoked.
ims-authorization-released(226) | The total number of sessions disconnected due to IMS authorization released.
ims-auth-decision-invalid(227) | The total number of sessions disconnected due to invalid IMS authorization decision.
mac-addr-validation-failed(228) | The total number of sessions disconnected due to MAC address validation failure in WiMAX network.
excessive-wimax-pd-flows-configured(229) | The total number of sessions disconnected due to excessive packet data flows are configured in WiMAX network.
sgsn-cancel-location-subs-withdrawn(230) | The total number of sessions disconnected due to cancellation of the request to location substitution withdrawn.
sgsn-cancel-location-update(231) | The total number of sessions disconnected because the cancellation of the location update.
sgsn-mnr-expiry(232) | The total number of sessions disconnected due to manager expiry.
sgsn-identity-failure(233) | The total number of sessions disconnected due to identity check failure.
sgsn-security-failure(234) | The total number of sessions disconnected due to security verification failure.
sgsn-auth-failure(235) | The total number of sessions disconnected due to authentication failure.
sgsn-glu-failure(236) | The total number of sessions disconnected due to GLU failure.
sgsn-implicit-detach(237) | The total number of sessions disconnected due to an implicit detach.
sgsn-subscriber-moved-to-different-smgr-instanc(238) | The total number of sessions disconnected due to subscriber moving to a different SMGR instance.
sgsn-subscriber-moved-to-peer-sgsn(239) | The total number of sessions disconnected due to subscriber moving to a peer SGSN.
sgsn-dns-failure-inter-rau(240) | The total number of sessions disconnected due to DNS failure during Inter-RAU.
sgsn-context-response-failure(241) | The total number of sessions disconnected due to context response failure.
sgsn-hlr-not-found-for-imsi(242) | The total number of sessions disconnected due to HLR not found for particular IMSI.
sgsn-ms-init-detach(243) | The total number of sessions disconnected due to MS initiated detach.
sgsn-roaming-not-allowed(244) | The total number of sessions disconnected because MS was not allowed to roam.
sgsn-duplicate-context(245) | The total number of sessions disconnected due to duplicate context.
hss-profile-update-failed(246) | The total number of sessions disconnected due to failure of profile update.
inactive-without-activating-any-pdp(247) | The total number of sessions disconnected where session is inactive and no PDP context is activated from this session.
asnpc-idle-mode-timeout(248) | The total number of sessions disconnected due to configured idle mode timeout duration is exhausted for ASN paging controller in WiMAX network.
asnpc-idle-mode-exit(249) | The total number of sessions disconnected due to idle mode exit message for ASN paging controller in WiMAX network.
asnpc-idle-mode-entry-auth-failed(250) | The total number of sessions disconnected due to authentication failure during idle mode entry for ASN paging controller in WiMAX network.
asngw-invalid-qos-configuration(251) | The total number of sessions disconnected due to invalid QoS configuration for subscriber in WiMAX network.
sgsn-dsd-allgprswithdrawn(252) | The total number of sessions disconnected due to the SGSN receiving a DSD message, from the HLR, with “All GPRS subscription withdrawn” flag set to true. The SGSN responds as if receiving a cancel location (subscription withdrawn) and clears the subscriber fully using this disconnect reason.
r6-pmk-key-change-failure(253) | The total number of sessions disconnected due to primary master key change failure on R6 interface in WiMAX network.
sgsn-illegal-me(254) | The total number of sessions disconnected because the ME was illegal.
sess-termination-timeout(255) | The total number of sessions disconnected due to failure monitored through BS monitor keep-alive probe.
sgsn-sai-failure(256) | The total number of sessions disconnected due to error in SGSN attachment in registration state.
sgsn-rnc-removal(257) | The total number of sessions disconnected due to error in SGSN inbound SRNS in registration state.
sgsn-rai-removal(258) | The total number of sessions disconnected due to error in Update PDP Context Response message for direct tunnel functionality. Direct tunnel functionality at GGSN was expecting some fields which were not received in the Update PDP Context Response message. Hence, GGSN was not able to establish tunnel appropriately with SGSN or RNC.
sgsn-init-deact(259) | The total number of sessions disconnected at SGSN due to unknown PDP context.
ggsn-init-deact(260) | The total number of sessions disconnected at SGSN due to PDP authentication failed.
hlr-init-deact(261) | The total number of sessions disconnected at SGSN due to duplicate PDP context
ms-init-deact(262) | The total number of sessions disconnected at SGSN due to no response from GGSN.
sgsn-detach-init-deact(263) | The total number of sessions disconnected at SGSN due to failed response from GGSN.
sgsn-rab-rel-init-deact(264) | The total number of sessions disconnected at SGSN due to unknown APN.
sgsn-iu-rel-init-deact(265) | The total number of sessions disconnected at SGSN due to service request initiated deactivation.
sgsn-gtpu-path-failure(266) | The total number of sessions disconnected at SGSN due to attachment procedure initiated abort.
sgsn-gtpc-path-failure(267) | The total number of sessions disconnected at SGSN due to ISRAU initiated abort procedure.
sgsn-local-handoff-init-deact(268) | The total number of sessions disconnected at SGSN due to unknown APN.
sgsn-remote-handoff-init-deact(269) | The total number of sessions disconnected at SGSN due to MM context cleanup initiated abort procedure.
sgsn-gtp-no-resource(270) | The total number of sessions disconnected at SGSN due to unknown abort procedure.
sgsn-rnc-no-resource(271) | The total number of sessions disconnected at SGSN due to abort procedure started by guard timeout.
sgsn-odb-init-deact(272) | The total number of sessions disconnected at SGSN due to abort procedure initiated on DHCP IP validate request.
sgsn-invalid-ti(273) | The total number of sessions disconnected due to id mismatch in MIPv6 session.
sgsn-actv-rejected-due-to-rnc(274) | The total number of sessions disconnected as AAA session id not-found
sgsn-apn-restrict-vio(275) | The total number of sessions disconnected due to security associate rekeying failure.
sgsn-actv-rejected-by-sgsn(276) | The total number of sessions disconnected due to failure in relocation in ASN-PC service.
sgsn-abnormal-deact(277) | The total number of sessions disconnected due to failure in paging controller relocation in ASN PC service.
sgsn-actv-rejected-by-ggsn(278) | The total number of sessions disconnected due to mismatch in authentication policy.
sgsn-err-ind(279) | The total number of sessions disconnected as DELETE MS ENTRY message received by the ASN Paging Controller.
asngw-non-anchor-prohibited(280) | The total number of sessions disconnected due to non-anchor ASN GW being prohibited.
asngw-im-entry-prohibited(281) | The total number of sessions disconnected due to unknown reason.
Session-idle-mode-entry-timeout(282) | The total number of sessions disconnected Administratively.
session-idle-mode-exit-timeout(283) | The total number of sessions disconnected by remote system
asnpc-ms-power-down-nwexit(284) | The total number of sessions disconnected by local system.
asnpc-r4-nwexit-recd(285) | The total number of sessions disconnected due to non-availability of resources.
sgsn-iu-rel-before-call-est(286) | The total number of sessions disconnected because of Iu Release during call establishment when service limits exceeded.
ikev2-subscriber-ipsecmgr-death(287) | The total number of sessions disconnected due to LCP negotiation failed.
All-dynamic-pool-addr-occupied(288) | The total number of sessions disconnected due to no response in PPP-LCP session.
mipv6ha-ip-addr-not-available(289) | The total number of sessions disconnected due to loop back detected in PPP-LCP.
bs-monitor-keep-alive-failed(290) | The total number of sessions disconnected due to failure monitored through BS monitor keep-alive probe.
sgsn-attach-in-reg-state(291) | The total number of SGSN sessions disconnected due to an error in the SGSN attachment during the registration state.
sgsn-inbound-srns-in-reg-state(292) | The total number of SGSN sessions disconnected due to an error in the SGSN inbound SRNS in a registration state.
dt-ggsn-tun-reestablish-failed(293) | The total number of SGSN sessions disconnected due to error in Update PDP Context Response message for direct tunnel functionality. Direct tunnel functionality at GGSN was expecting some fields which were not received in the Update PDP Context Response message. Hence, the GGSN was not able to establish a tunnel appropriately with the SGSN or the RNC.
sgsn-pdp-unknown(294) | The total number of SGSN sessions disconnected due to an unknown PDP context.
sgsn-pdp-auth-failure(295) | The total number of SGSN sessions disconnected because the PDP authentication failed.
sgsn-duplicate-pdp-context(296) | The total number of SGSN sessions disconnected due to duplicate PDP contexts.
sgsn-no-rsp-from-ggsn(297) | The total number of SGSN sessions disconnected because the SGSN does note receive a response from the GGSN.
sgsn-failure-rsp-from-ggsn(298) | The total number of SGSN sessions disconnected due to failed response from the GGSN.
sgsn-apn-unknown(299) | The total number of SGSN sessions disconnected due to an unknown APN.
sgsn-pdp-status-mismatch(300) | The total number of SGSN sessions disconnected due to deactivation initiated by a service request.
sgsn-attach-on-attch-init-abort(301) | The total number of SGSN sessions disconnected due to an attachment procedure-initiated abort.
sgsn-iu-rel-in-israu-init-abort(302) | The total number of SGSN sessions disconnected due to an ISRAU-initiated abort procedure.
sgsn-smgr-init-abort(303) | The total number of SGSN sessions disconnected because the SessMgr initiates an abort.
sgsn-mm-ctx-cleanup-init-abort(304) | The total number of SGSN sessions disconnected due to the MM context cleanup-initiated abort procedure.
sgsn-unknown-abort(305) | The total number of SGSN sessions disconnected due to an unknown abort procedure.
sgsn-guard-timeout-abort(306) | The total number of SGSN sessions disconnected because the abort procedure was started by the guard timer timeout.
vpn-bounce-dhcpip-validate-req(307) | The total number of SGSN sessions disconnected because the abort procedure was initiated upon receiving a DHCP IP validate request.
mipv6-id-mismatch(308) | The total number of sessions disconnected due to id mismatch in MIPv6 session.
aaa-session-id-not-found(309) | The total number of sessions disconnected as AAA session id not-found
x1/x5-max-retry-reached(310) | The total number of sessions disconnected due to security associate rekeying failure.
x1-nwexit-recd(311) | The total number of sessions disconnected due to failure in relocation in ASN-PC service.
x1-dereg-req-recd(312) | The total number of sessions disconnected due to failure in paging controller relocation in ASN PC service.
x1-remote-failure(313) | The total number of sessions disconnected due to mismatch in authentication policy.
x1x2-protocol-errors(314) | The total number of sessions disconnected as DELETE MS ENTRY message received by the ASN Paging Controller.
x2/x6-max-retry-reached(315) | The total number of sessions disconnected because the ASNGW TID entry was not found.
x2/x6-nwexit-recd(316) | The total number of sessions disconnected due to network exit message received on X2 interface in PHS network.
x2-dereg-req-recd(317) | The total number of sessions disconnected due to deregistration request received on X2 interface in PHS network.
x2-remote-failure(318) | The total number of sessions disconnected by remote system due to failure on X2 interface in PHS network.
x1-pmk-key-change-failure(319) | The total number of sessions disconnected due to primary master key change failure on X1 interface in PHS network.
SA-Rekeying-Failure(320) | The total number of sessions disconnected due to security associate rekeying failure.
Sess-sleep-mode-entry-timeout(321) | The total number of sessions disconnected due to session sleep mode entry timeout on PHS GW.
phsgw-non-anchor-prohibited(322) | The total number of sessions disconnected due to non-anchor PHS GW being prohibited.
asnpc-pc-relocation-failed(323) | The total number of sessions disconnected due to failure in relocation in ASN-PC service.
asnpc-pc-relocation(324) | The total number of sessions disconnected due to failure in paging controller relocation in ASN PC service.
auth_policy_mismatch(325) | The total number of sessions disconnected due to mismatch in authentication policy.
ike/ipsec-sa-lifetime-expired(326) | The total number of sessions disconnected due to IKE/IPsec security associate lifetime timer expiration.
asnpc-del-ms-entry-recd(327) | The total number of sessions disconnected as DELETE MS ENTRY message received by the ASN Paging Controller.
phspc-sleep-mode-timeout(328) | The total number of sessions disconnected due to sleep mode timeout by the PHS Paging Controller.
phspc-sleep-mode-exit(329) | The total number of sessions disconnected due to sleep mode exit by the PHS Paging Controller.
phspc-sleep-mode-entry-auth-failed(330) | The total number of sessions disconnected due to failed sleep mode entry authorization by the PHS Paging Controller.
phspc-ms-power-down-nwexit(331) | The total number of sessions disconnected due to ms power down network exit message received by the PHS Paging Controller.
phspc-x6-nwexit-recd(332) | The total number of PHS Paging Controller sessions disconnected due to network exit message received from X2 interface in PHS network.
invalid-nat-config(333) | The total number of sessions disconnected due to the following reasons: 1. SessMgr and ACSMgr are running in non-optimized mode. 2. An undefined NAT pool is configured for subscriber. NAT must be disabled if ACS is not running in optimized mode.
asngw-tid-entry-not-found(334) | The total number of sessions disconnected because the ASNGW TID entry was not found.
No-NAT-IP-Addr-for-subscriber(335) | The total number of sessions disconnected due to NAT IP address being unavailable during call setup for allocation to a subscriber.
excessive-phs-pd-flows-configured(336) | The total number of sessions disconnected due to configuration of excessive PHS pd flows.
phsgw-invalid-qos-configuration(337) | The total number of sessions disconnected due to invalid QoS configuration for subscriber in PHS network.
Interim-Update(338) | The total number of sessions disconnected due to Interim Update.
sgsn-inbound-attach-abort-radio-status-bad-lost(339) | The total number of SGSN sessions disconnected because the inbound attach requests aborted due to poor radio status or lost radio connections.
sgsn-inbound-irau-abort-radio-status-bad-lost(340) | The total number of SGSN sessions disconnected due to inbound IRAU requests aborting as the radio status was poor or the radio connection lost.
ike-keep-alive-failed(341) | The total number of sessions disconnected due to IKE keepalive failure.
sgsn-attach-abort-ms-suspend(342) | The total number of SGSN sessions disconnected due to attach requests aborting because MS was in suspend mode.
sgsn-inbound-irau-abort-ms-suspend(343) | The total number of SGSN sessions disconnected due to IRAU requests aborted when MS was in suspend mode.
duplicate-session-detected(344) | The total number of sessions disconnected due to detection of duplicate sessions for the same session id.
sgsn-xid-response-failure(345) | The total number of SGSN sessions disconnected due to XID response failure.
sgsn-nse-cleanup(346) | The total number of SGSN sessions disconnected due to record cleanup or reset on the network service entity (NSE).
sgsn-gtp-req-failure(347) | The total number of SGSN sessions disconnected due to failure of the GTPP request.
sgsn-imsi-mismatch(348) | The total number of SGSN sessions disconnected due to mismatches of the IMSIs.
sgsn-bvc-blocked(349) | The total number of SGSN sessions disconnected because the BSSGP Virtual Connection (BVC) was blocked.
sgsn-attach-on-inbound-irau(350) | The total number of SGSN sessions disconnected as the session was attached on inbound IRAU requests.
sgsn-attach-on-outbound-irau(351) | The total number of SGSN sessions disconnected while the session was attached on outbound IRAU requests.
sgsn-incorrect-state(352) | The total number of SGSN sessions disconnected due to incorrect state of network elements.
sgsn-t3350-expiry(353) | The total number of SGSN sessions disconnected due to expiry of the T-3350 timer.
sgsn-page-timer-expiry(354) | The total number of SGSN sessions disconnected due to expiry of the paging timer.
phsgw-tid-entry-not-found(355) | The total number of SGSN sessions disconnected due to local purging of PDP contexts.
sgsn-pdp-local-purge(357) | The total number of SGSN sessions disconnected due to local purging of PDP contexts.
sgsn-offload-phase2(360) | With Iu/Gb flex enabled, this is the total number of SGSN sessions disconnected when the subscribers has been forcefully cleared via phase2 offloading from one SGSN to another SGSN within the SGSN pool.
Remote-error-notification(362) | The total number of sessions disconnected due to remote error notification.
no-response(363) | The total number of sessions disconnected due to no response from any of the network entity.
PDG-Auth-failed(364) | The total number of sessions disconnected due to re-authorization failure at any stage.
mme-s1AP-send-failed(365) | The total number of sessions disconnected due to message sent on S1AP interface failed.
mme-egtpc-connection-failed(366) | The total number of sessions disconnected as connection between MME and eGTP service/node failed due to any reason.
mme-egtpc-create-session-failed(367) | The total number of sessions disconnected as session creation failed between MME and eGTP service/node.
mme-authentication-failure(368) | The total number of sessions disconnected as authentication procedure failed between MME and HSS.
mme-ue-detach(369) | The total number of sessions disconnected as UE detached explicitly.
mme-mme-detach(370) | The total number of sessions disconnected on serving MME due to detach procedure occurred between anchored MME and service MME.
mme-hss-detach(371) | The total number of sessions disconnected due to DETACH procedure started from HSS.
mme-pgw-detach(372) | The total number of sessions disconnected due to DETACH procedure started from P-GW.
mme-sub-validation-failure(373) | The total number of sessions disconnected as subscriber validation failed at MME or HSS during authentication procedure.
mme-hss-connection-failure(374) | The total number of sessions disconnected due to connection failure between MME and associated HSS during authentication procedure.
mme-hss-user-unknown(375) | The total number of sessions disconnected by MME service due to UNKNOWN USER response from HSS during authentication procedure.
dhcp-lease-mismatch-detected(376) | The total number of sessions disconnected due to mismatch in DHCP lease time mismatch.
nemo-link-layer-down(377) | The total number of disconnected sessions due to the NEMO (Network Mobility) link layer being down.
sgsn-offload-phase3(379) | With Iu/Gb flex enabled, this is the total number of SGSN sessions disconnected when the subscribers has been forcefully cleared via phase3 offloading from one SGSN to another SGSN within the SGSN pool.
mbms-bearer-service-disconnect(380) | The total number of sessions disconnected due to disconnect in MBMS bearer service.
disconnect-on-violation-odb(381) | The total number of sessions disconnected due to violation on Operator Determined Barring (ODB) of services.
disconn-on-violation-focs-odb(382) | The total number of sessions disconnected due to violation on Operator Determined Barring (ODB) of Free-of-Charge Service (FOCS).
CSCF-REG-Admin-disconnect(383) | The total number of CSCF sessions disconnected through CLI registration clearing by administrator.
CSCF-REG-User-disconnect(384) | The total number of CSCF sessions disconnected by UE with an explicit deregister message.
CSCF-REG-Inactivity-timeout(385) | The total number of CSCF sessions disconnected due to registration expiry.
CSCF-REG-Network-disconnect(386) | The total number of CSCF sessions disconnected due to network-initiated deregistration.
CSCF-Call-Admin-disconnect(387) | The total number of CSCF sessions disconnected through CLI call clearing by administrator.
CSCF-Call-User-disconnect(388) | The total number of CSCF sessions disconnected by UE using BYE message.
CSCF-CALL-Local-disconnect(389) | The total number of CSCF sessions disconnected locally due to some processing failure, task death, recovery failure, etc.
CSCF-CALL-No-Resource(390) | The total number of CSCF sessions disconnected because locally due to congestion caused by max calline/flow usage from high cpu/memory utilization in sessmgr.
CSCF-CALL-No-Response(391) | The total number of CSCF sessions disconnected due to response timeout (SIP response code 408).
CSCF-CALL-Inactivity-timeout(392) | The total number of CSCF sessions disconnected due to session timer timeout
CSCF-CALL-Media-Auth-Failure(393) | The total number of CSCF sessions disconnected due to media authorization failure.
CSCF-REG-No-Resource(394) | The total number of CSCF sessions disconnected because register message is rejected due to congestion caused by max calline/flow usage from high cpu/memory utilization in sessmgr.
ms-unexpected-idle-mode-entry(395) | The total number of sessions disconnected while MS unexpectedly started the IDLE mode procedure and enters the Idle mode.
Re-Auth-failed(396) | The total number of sessions disconnected during re-authentication when MS started activation after coming out of idle mode.
sgsn-pdp-nse-cleanup(397) | The total number of SGSN sessions disconnected because the NSE configured in the GPRS service is removed and there are PDP contexts associated with the subscribers attached in this NSE.
sgsn-mm-ctxt-gtp-no-resource(398) | The total number of SGSN sessions disconnected because an SGTP service could not be assigned to an MM context.
unknown-apn(399) | The total number of sessions disconnected due to invalid and/or unknown APN name received from AAA or subscriber template.
gtpc-path-failure(400) | The total number of sessions disconnected due to failure of GTP-C interface path between two nodes.
gtpu-path-failure(401) | The total number of sessions disconnected due to failure of GTP-U interface path between two nodes.
actv-rejected-by-ggsn(402) | The total number of sessions disconnected due as session activation procedure, started by an MS which was in idle mode, was rejected by GGSN.
sgsn-pdp-gprs-camel-release(403) | The total number of PDP activation failures due to release from CAMEL. This counter is visible but not yet fully supported.
sgsn-check-imei-failure(404) | The total number of of Attaches / RAUs rejected due to failure in the IMEI checking (i.e. due either to black listing or to grey listing and an SGSN operator policy is configured with deny-grey-list).
sgsn-sndcp-init-deact(405) | The total number of PDP contexts deactivated upon receiving a cleanup indication from the SNDCP layer.
sgsn-pdp-inactivity-timeout(406) | The total number of subscribers detached or PDP context(s) deactivated due to subscriber inactivity during a configured (in the SGSN operator policy) time.
No-IPV6-address-for-subscriber(410) | The total number of disconnects due to No-IPv6-address-for-subscriber.
prefix-registration-failure(411) | The total number of disconnects due to prefix-registration-failure.
disconnect-from-policy-server(412) | The total number of sessions disconnected due to disconnect from policy server.
s6b-auth-failed (413) | The total number of subscriber sessions disconnected due to failure of authentication over S6b interface with HSS. This support is added for interoperability of GGSN with P-GW and HA.
gtpc-err-ind(414) | The total number of sessions disconnected due to a GTP control plane error indication message.
gtpu-err-ind(415) | The total number of sessions disconnected due to a GTP user plane error indication message.
invalid-pdn-type(416) | The total number of sessions disconnected due to an invalid PDN-type error.
aaa-auth-req-failed(417) | The total number of sessions disconnected due to a AAA authentication request failure.
apn-denied-no-subscription (418) | The total number of subscriber sessions disconnected due to denial of APN as requested APN was not subscribed to subscriber.
sgw-context-replacement(419) | The total number of sessions disconnected due to an S-GW context replacement.
dup-static-ip-addr-req (420) | The total number of subscriber sessions disconnected due to new session request received with duplicate IP address at GGSN. This support is added for interoperability of GGSN with P-GW and HA.
apn-restrict-violation (421) | The total number of subscriber sessions disconnected due to violation of level of restriction to ensure controlled co-existence of the Primary PDP Contexts in APN.
invalid-wapn(422) | The total number of sessions disconnected due to invalid or no W-APN details received from the UE.
ttg-nsapi-allocation-failed(423) | The total number of TTG sessions disconnected due to an NSAPI (Network Service Access Point Identifier) allocation failure.
mandatory-gtp-ie-missing(424) | The total number of sessions disconnected due to the unavailability of a mandatory GTP Information-Element during PDP context creation.
aaa-unreachable(425) | The total number of sessions disconnected due to unreachable AAA server.
asngw-service-flow-deletion(426) | Sent in the Accounting-Stop message for the particular service flow when that service flow is deleted by the Network- or MS-initiated service flow detection procedure.
CT-PMIP-RRQ-NVSE-Value-Change(427) | he total number of disconnects resulting from a PMIP (Proxy-MIP) registration request (RRQ) returning an NVSE (Normal/Vendor organization Special Extension) value change [WiMAX].
tcp-read-failed (428) | The total number of disconnected IP-CAN sessions due to a TCP read failure.
tcp-write-failed (429) | The total number of disconnected IP-CAN sessions due to a TCP write failure.
ssl-handshake-failed (430) | The total number of disconnected SSL ssessions due to a handshake failure.
ssl-renegotiate-failed (431) | The total number of disconnected SSL ssessions due to a renegotiation failure.
ssl-bad-message (432) | The total number of disconnected SSL ssessions due to corrupted messages.
ssl-alert-received (433) | The total number of disconnected SSL ssessions due to an alert.
ssl-disconnect (434) | The total number of SSL disconnections.
ssl-migration (435) | The total number of SSL migrations.
sgsn-ard-failure(436) | The total number of session disconnects due to ARD (access restriction data) subscription restriction received from the HLR.
sgsn-camel-release(437) | The total number of session disconnects experienced by the SGSN when Detach/Attach Rejects were due to explicit “Release GPRS” received from the CAMEL component GSM-SCF or due to failures during CAMEL handling.
sgsn-egtpc-connection-failed(438) | Replaced by sgsn-egtpc-create-session-failed(439) in Release 14.0.
sgsn-egtpc-create-session-failed(439) | Supported in Release 14.0 The total number of session disconnects occurring when the S4-SGSN is not able to establish a PDP context when the SGW returned a failure cause in “Create Session Response” or the SGW did not respond at all to “Create Session Request”. Counter
sgsn-hss-detach(440) | Replaced by sgsn-cancel-location-subs-withdrawn(230) in Release 14.0.
sgsn-hss-connection-failure(441) | Replaced by sgsn-glu-failure(236) in Release 14.0
sgsn-pgw-detach(442) | Not yet supported.
sgsn-s5-s8-no-support-for-apn(443) | Supported in Release 14.0. The total number of session disconnects resulting from the S4-SGSN's inability to establish a PDP context for an APN in the following scenario: An EPS subscription is used for a subscriber. The SGSN tries to find an S5 / S8 address of the PGW for the requested APN. The DNS response does not contain an S5/S8 address. The PDP activation is rejected.
sgsn-no-rab-for-gbr-bearer(444) | Not yet supported. In development for future use.
sgsn-sgw-selection-failure(445) | Supported in Release 14.0. The total number of session disconnects resulting from the S4-SGSN’s inability to establish a PDP context in the following scenario: Either EPS or GPRS subscription is used. S4-SGSN chooses S4 interface for PDP activation because The UE is EPC-capable. EGTP service is configured. Operator Policy does not override the core-nw-interface to Gn. The SGSN successfully resolves P-GW address (S5/S8 address) for the APN requested. The SGSN tries S-GW resolution. If the DNS response fails and no local S-GW is configured for the RAI, then the PDP activation is reected with this disconnect reason.
sgsn-pgw-selection-failure(446) | Supported in Release 14.0. The total number of sessions disconnected by the S4-enabled SGSN when the P-GW DNS resolution fails due to any cause other than the DNS response does not contain an S5/S8 address.
wimax-hotlining-status-change(447) | The total number of disconnects resulting from a status change in the Hotlining-Capabilities sub-attribute in the WiMAX-Capabilities attribute.
ggsn-no-rsp-from-sgsn(448) | The total number of sessions disconnected on GGSN node due to no response received from SGSN for a request.
diameter-protocol-error(449) | The total number of sessions disconnected on IPCF node due to an error in Diameter protocol (such as, CCR-I parse failure).
diameter-request-timeout(450) | The total number of sessions disconnected on IPCF node due to Diameter (RAR/ASR) request timeout on IPCF node.
operator-policy(451) | The total number of session disconnected on IPCF node due to parameters configured by operator for PCC policy.
spr-connection-error(452) | The total number of sessions disconnected on IPCF node due to an error in connection between SSC and IPCF node or non-availability of SSC.
mipha-dup-wimax-session(453) | The total number of WiMAX session disconnects resulting from duplicate Mobile IP Home Agent (MIPHA) logins.
invalid-version-attr(454) | This disconnect reason is set, if there is mismatch of WiMAX-Release version supported by ASNGW and that supported by AAA. This statistic is incremented when there is a mismatch of WiMAX-Release version supported by ASNGW and that supported by AAA. AAA sends WiMAX release in Radius packet. This statistic is cumulative for all ASNGW services configured on the system.
sgsn-zone-code-failure(455) | The total number of session disconnects experienced by the SGSN due to verification failure during the zone-code checking procedure.
invalid-qci(456) | The total number of session disconnects resulting from the receipt of invalid QoS class identifiers (QCIs). This error is returned if an invalid QCI is used in certain operations such as create bearer, which expects a QCI. A QCI is deemed invalid if it is not a standard QCI (1-9) or the QCI is not defined in the QCI table associated with the service.
no_rules(457) | This session disconnect counter increases for eGCDR when the call is terminated because of the PCRF deleting a rulebase through RAR.
sgsn-rnc-no-dual-pdp-init-pdp-deact(458) | Indicates the number of times the SGSN has deactivated a PDP because the MS/UE has roamed into an area where the RNC does not support dual PDP types. Deactivation would have been done with cause code “reactivation required”.
mme-init-ctxt-setup-failure (459) | The total number of session disconnects resulting from context setup failures in the ENodeB during EMM/ECM procedures.
mme-driver-initiated (460) | The total number of session disconnects resulting from the default value for mme-sessions.
mme-s1ap-connection-down (461) | The total number of session disconnects resulting from S1AP connection failures.
mme-s1ap-reset-recd (462) | The total number of session disconnects resulting from partial or full resets received for the S1 connection.
mme-s6a-response-timeout (463) | The total number of session disconnects resulting from requests to the HSS that timed out (AIR or ULR).
mme-s13-response-timeout (464) | The total number of session disconnects resulting from EIR query time outs.
mme-Illegal-equipment (465) | The total number of session disconnects resulting from EIR query failures.
mme-unexpected-attach (466) | The total number of session disconnects resulting from older sessions getting disconnected due to the UE executing an ATTACH procedure.
mme-sgw-selection-failure (467) | The total number of session disconnects resulting from failed selections of S-GWs for the UE’s current location.
mme-pgw-selection-failure (468) | The total number of session disconnects resulting from failed selections of P-GWs for default APNs.
mme-reselection-to-sgsn (469) | The total number of session disconnects resulting from a context request from an SGSN relocated call to 3G.
mme-relocation-to-sgsn (470) | The total number of session disconnects resulting from calls transitioned to an SGSN using handover signaling.
mme-reselection-to-mme (471) | The total number of session disconnects resulting from a context request from an MME relocated call to a different MME.
mme-relocation-to-mme (472) | The total number of session disconnects resulting from calls transitioned to an MME using handover signaling.
mme-tau-attach-collision (473) | The total number of session disconnects resulting from processing a TAU request with a foreign GUTI that cleared an existing session on the MME.
mme-old-sgsn-resolution-failure (474) | The total number of session disconnects resulting from calls setup using a PTMSI that failed due to failure in resolution of the old SGSN context.
mme-old-mme-resolution-failure (475) | The total number of session disconnects resulting from calls setup using a foreign GUTI that failed due to a failure in resolution of the old MME context.
mme-reloc-ho-notify-timeout (476) | The total number of session disconnects resulting from a handover based session origination failure due to an ho-notify timeout.
mme-reloc-ho-req-ack-timeout (477) | The total number of session disconnects resulting from a handover based session origination failure due to an ho-request-ack timeout.
mme-create-session-timeout (478) | The total number of session disconnects resulting from a create session request to the S-GW that timed out.
mme-create-session-failure (479) | The total number of session disconnects resulting from a create session request to the S-GW that returned a failure response.
mme-s11-path-failure (480) | The total number of session disconnects resulting from a call cleared due to an S11 path failure.
mme-policy-no-ue-irat (481) | The total number of session disconnects resulting from a call cleared due to policy restrictions on inter-rat handovers.
mme-x2-handover-failed (482) | The total number of session disconnects resulting from a call cleared due to failures in x2 handovers.
mme-attach-restrict (483) | The total number of session disconnects resulting from an operator policy based attach restriction.
mme-regional-zone-code (484) | The total number of session disconnects resulting from the UE being in a zone code where the UE is not allowed to roam.
mme-no-response-from-ue (485) | The total number of session disconnects resulting from the maximum retransmission of a NAS message during session setup.
mme-sgw-relocation-failed (486) | The total number of session disconnects resulting from an S-GW relocation procedure failing.
mme-implicit-detach (487) | The total number of session disconnects resulting from the UE being implicitly detached due to inactivity.
sgsn-detach-notify (488) | Replaced by sgsn-isr-mme-init-detach(505) in Release 14.0.
policy-initiated-release(489) in StarOS 12.1 and earlier releases | .
emergency-inactivity-timeout (489) in StarOS 12.2 and later releases | The total number of sessions disconnected due to emergency inactivity timeout. The emergency session inactivity timeout is set on an APN configured as an emergency APN for VoLTE-based E911 support.
gy-result-code-system-failure (490) in StarOS 12.1 and earlier releases | The total number of sessions disconnected due to failure result codes received from the Online Charging Server that resulted in system failure on the GTP side.
policy-initiated-release(490) in StarOS 12.2 and later releases | The total number of times that a call disconnect occurs due to a Gx-initiated bearer release. For example, this disconnect reason may be used if there are any errors in the manner of the policy or rule configurations.
emergency-inactivity-timeout (491) in StarOS 12.1 and earlier releases | The total number of sessions disconnected due to emergency inactivity timeout. The emergency session inactivity timeout is set on an APN configured as an emergency APN for VoLTE-based E911 support.
gy-result-code-system-failure (491) in StarOS 12.2 and later releases | The total number of sessions disconnected due to failure result codes received from the Online Charging Server that resulted in system failure on the GTP side.
mme-zone-code-validation-failed (492) | The total number of session disconnects resulting from the UE being in a zone code where the UE is not allowed to roam.
sgsn-pgw-init-deact(493) | Supported in Release 14.0. The total number of session disconnects resulting from an initial deactivation between the SGSN and the P-GW when the P-GW sends “Delete Bearer Request” to deactivate a PDP or a PDP bundle.
s6b-ip-validation-failed(494) | Not supported in releases 12.0 or 12.2 - in development for future use.
sgsn-failure-rsp-from-sgw(495) | Supported in Release 14.0. The total number of session disconnects resulting from the SGSN receiving a failure response from the S-GW. This occurs in any of the following scenarios: The UE has successfully attached and activated the PDP contexts through the S4 interface and then the UE does a RAU to a new RA. During this RAU, the SGSN will do S-GW selection for the new RA. If the SGSN selects a new S-GW for this RA and sends “Create Session Request” to the new S-GW to setup a tunnel. But the new S-GW does not respond or the responds with a failure cause. The SGSN deactivates the PDP with this disconnect cause. In the case of a new-SGSN RAU without S-GW relocation, the new-SGSN sends "Modify Bearer Req" to inform the S-GW that the UE has moved to the new-SGSN but the SGSN does not receive any response from the S-GW. During intra-SGSN RAU with a change in the PLMN but without a change in the S-GW. In this case, SGSN will send "Modify Bearer Req" to inform the S-GW of the change in PLMN ID but SGSN does not receive any response from the S-GW. During intra-SGSN 3G-to-2G or 2G-to-3G inter-RAT RAU without an S-GW change. In this case, the SGSN sends "Modify Bearer Req" to inform the S-GW of the change in RAT type but the SGSN dpes not receive any response from the S-GW.
tcp-remote-close (496) | The total number of sessions disconnected due to a TCP FIN (finished sending) message received from the UE.
tcp-reset-received (497) | The total number of sessions disconnected due to a TCP RST (reset) message received from the UE.
tcp-socket-error (498) | The total number of sessions disconnected due to a socket error received from the trek stack at the access-side TCP socket connection between the UE and the TTG.
ptmsi-signature-mismatch(499) | The number of times the SGSN was unable to validate the P-TMSI signature, present in the Attach Request, against the PTMSI-SIGNATURE stored in SGSN. The SGSN sent an Attach Reject to MS if it did not match. This occurs when the GPRS service is configured to reject Attaches with mismatching P-TMSI-signature. This configuration is used to prevent collision of 2 Attach procedures from 2 subscribers with the same P-TMSI and then quickly enforces an IMSI Attach.
camel-invalid-configuration(500) | Supported in Release14.0. The number of times the SGSN has encountered an invalid Customized Applications for Mobile network Enhanced Logic (CAMEL) configuration. This condition typically occurs when a subscriber moves from 3G service to 2G service or vice versa and the CAMEL service is associated only in the source service but not in the target service. In such cases, RAU requests are rejected with disconnect reason "camel-invalid-configuration".
4Gto3G-context-replacement(501) | Supported in Release14.0. The total number of times a PGW call has been cleared when a new call request came on GGSN and PGW already had a call with the same IMSI. ISR is enabled.
mme-isr-sgsn-init-detach(502) | Supported in Release14.0. The total number of times an MME, with IRS enabled, deletes a subscriber to detach the UE after receiving an S3 Detach Notification from the SGSN with cause code “complete detach”.
sgsn-isr-addl-ptmsi-rai(503) | Supported in Release14.0. The total number times the SGSN has disconnected a session because the SGSN has sent an additional P-TMSI Attach request during ISR. This cause is used to peg the clearing of stale contexts. This can occur in the following scenario: The UE is registered with both the MME and the SGSN and ISR is active. Due to one of the reasons mentioned in Annex J.6 of TS 23.401, ISR is deactivated at the UE but has not deactivated at either the SGSN or the MME which means the UE’s last point of attachment at the time of ISR deactivation is the MME. Now the UE does a RAU to the SGSN. The UE will send old-RAI mapped from the GUTI (since the ISR is deactivated and the UE’s last point of attachment was the MME) and also an additional RAI / P-TMSI which is the P-TMSI/RAI given by the SGSN at the time of ISR activation in step 1. This additional P-TMSI / RAI helps the SGSN to locate the stale UE context and clean it up. (The SGSN received a RAU with an old-RAI mapped from the GUTI so the SGSN needs to build a fresh UE context by fetching information from the MME - “Context Req/Rsp/Ack”.)
sgsn-sgw-dbr-cause-isr-deact(504) | Supported in Release14.0. The number of times “Delete Bearer Requests” occurred between the SGSN and the S-GW due to ISR being deactivated. This occurs when the SGSN locally deactivate PDP contexts after receiving “Delete Bearer Requests” with cause “ISR Deactivation” from the S-GW.
sgsn-isr-mme-init-detach(505) | Supported in Release14.0. The number of times Init Detach occurred between the SGSN and the MME with ISR activated. This occurs when the SGSN receives “S3 Detach Notification” with cause “Complete Detach” from the MME.
mme-sgw-dbr-cause-isr-deact(506) | Supported in Release14.0. The number of times Delete Bearer Requests occurred between MME and SGW due to ISR being deactivated.
sgsn-ptmsi-crunch(507) | Supported in Release 14.0. The total number of sessions disconnected by the SGSN when there is a shortage of P-TMSIs which can occur when the number of possible subscribers per SessMgr has increased (with a PSC3) but the number of local NRI has not been increased in the configuration.
3Gto4G-context-replacement(508) | Supported in Release14.0. The total number of times a GGSN call has been cleared when a new call request came on PGW and GGSN already had a call with the same IMSI. Idle mode Signaling Reduction (ISR) is enabled.
sgsn-actv-reject-on-dns-failure(509) | Never used. Removed in Release 14.0.
mme-no-eps-bearers-activated(509) | Supported in Release14.0. The number of times the MME has rejected a TAU Attach Request due to any of the following reasons: EPS Context Status IE value = 0 ( which implies no EPS bearers were active in UE). The SGSN Context Response received by the MME did not have any PDP Contexts or the Response which included the PDP Contexts encountered basic decoding issues (like incorrectly encoded APN, etc.).

show session progress
Table 5. show session progress Command Output Descriptions

Field | Description
--- | ---
In-progress calls | The number of calls that are currently in progress (active, dormant, being set up, or being disconnected) and being processed by either the system (if no keywords were used), a specific PDSN service (if the pdsn-service keyword was used), or a specific PCF (if the pcf keyword was used).
In-progress active calls | The total number of active sessions.
In-progress dormant calls | The total number of dormant sessions.
In-progress always-on calls | The number of calls that have always on enabled.
In-progress calls @ ARRIVED state | The total number of sessions that are at the onset of the registration process.
In-progress calls @ LCP-NEG state | The total number of sessions that are in the Link Control Protocol (LCP) negotiation phase of the registration process.
In-progress calls @ LCP-UP state | The total number of sessions that have just completed the Link Control Protocol (LCP) negotiation phase of the registration process.
In-progress calls @ AUTHENTICATING state | The total number of sessions that are in the process of being authenticated.
In-progress calls @ BCMCS SERVICE AUTHENTICATING state | The total number of BCMCS sessions that are in the process of being authenticated.
In-progress calls @ MBMS UE AUTHORIZING state | The total number of MBMS sessions currently in UE authorization state.
In-progress calls @ MBMS BEARER AUTHORIZING state | The total number of MBMS sessions currently in bearer authorization state.
In-progress calls @ AUTHENTICATED state | The total number of sessions that have just completed the authentication phase of the registration process.
In-progress calls @ L2TP-LAC CONNECTING state | The number of calls that have an L2TP tunnel in the process of being brought up.
In-progress calls @ DHCP PENDING state | The total number of DHCP calls that are currently in pending state.
In-progress calls @ IPCP-UP state | The total number of sessions that have just completed the Internet Protocol Control Protocol (IPCP) phase of the registration process.
In-progress calls @ NON-ANCHOR CONNECTED state | Indicates the total number of WiMAX sessions being processed by this Session Manager instance that are currently being in connected state in non-anchor mode.
In-progress calls @ SIMPLE IPv4 CONNECTED state | The total number of IPv4 data sessions that are currently connected.
In-progress calls @ SIMPLE IPv6 CONNECTED state | The total number of IPv6 data sessions that are currently connected.
In-progress calls @ SIMPLE-IP CONNECTED state | The total number of Simple IP data sessions that are currently connected.
In-progress calls @ MOBILE-IP CONNECTED state | The total number of Mobile IP data sessions that are currently connected.
In-progress calls @ PROXY-MOBILE-IP CONNECTED state | The total number of Proxy Mobile IP data sessions that are currently connected.
In-progress calls @ HA-IPSEC CONNECTED state | The number of calls that have negotiated IP Security.
In-progress calls @ L2TP-LAC CONNECTED state | The number of calls that are passing data through an L2TP tunnel.
In-progress calls @ HNBGW CONNECTED state | The number of UMTS-Femto calls conencted to HNB-GW.
In-progress calls @ PDP-TYPE- IPv4 CONNECTED state | The total number of PDP-type IPv4 data sessions that are currently connected.
In-progress calls @ PDP-TYPE- IPv6 CONNECTED state | The total number of PDP-type IPv6 data sessions that are currently connected.
In-progress calls @ PDP-TYPE-IP CONNECTED state | The total number of PDP contexts of type IP that are currently connected. This field applies to GGSN only.
In-progress calls @ PDP-TYPE-PPP CONNECTED state | The total number of PDP contexts of type PPP that are currently connected. This field applies to GGSN only.
In-progress calls @ BCMCS CONNECTED state | The total number of BCMCS sessions currently connected.
In-progress calls @ PCC CONNECTED state | The total number of IP-CAN sessions currently in connected state.
In-progress calls @ MBMS UE CONNECTED state | The total number of MBMS sessions currently in UE connected state.
In-progress calls @ MBMS BEARER CONNECTED state | The total number of MBMS sessions currently in bearer connected state.
In-progress calls @ IPSG CONNECTED state | The total number of IPSG sessions currently connected.
In-progress calls @ ASNPC CONNECTED state | Indicates the number of ASN Paging Controller calls that are currently connected.
In-progress calls @ CSCF-REGISTERING state | Total number of CSCF sessions which are in registration processing state.
In-progress calls @ CSCF-REGISTERED state | Total number of cscf sessions which are in registered state.
In-progress calls @ CSCF-CALL-ARRIVED state | Total number of CSCF sessions which are processing the newly arrived CSCF calls (i.e., processing initial Invite, waiting for provisional response, waiting for final response, etc.).
In-progress calls @ CSCF-CALL-CONNECTING state | Total number of CSCF sessions which are in call connecting state (waiting for ACK).
In-progress calls @ CSCF-CALL-CONNECTED state | Total number of CSCF sessions which are in call connected state.
In-progress calls @ CSCF-CALL-DISCONNECTING state | Total number of CSCF sessions which are in call disconnecting state (i.e., processing BYE , waiting for BYE response, etc.).
In-progress calls @ MME ATTACHED state | Indicates the number of MME subscriber session currently attached.
In-progress calls @ DISCONNECTING state | The total number of sessions that are in the process of disconnecting.

show session recovery status verbose
Table 6. show session recovery status verbose Output Descriptions

Field | Description
--- | ---
Last Status Update | The duration from the last time the Resource Manager did a health check on the session managers. This is informational info only, and does not reflect the last time a subscriber was checkpointed.
cpu | This indicates the card and slot number of the CPU listed.
state | Indicates the state of the specified CPU. This is either Active or Standby.
sessmgr | This lists the number of Session Managers in the active and standby state on the specified CPU.
aaamgr | Indicates the number of AAA managers in the active and standby state on the specified CPU.
demux active | Indicates the number of demux managers on the CPU.
status | This indicates the session recovery state for the specified CPU. This can be one of the following values: Good (Demux) Demux With Non-Demux Non-Demux With Demux Pair on Processing Cards SESSMGR Not Ready Missing AAAMGR No Standby Good SESSMGR Not Ready Too Few Standby Good Unknown

show session subsystem facility a11mgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) and A11 Manager (A11Mgr) task itself (not from the perspective of subscribers).
Table 7. show session subsystem facility a11mgr Command Output Descriptions

Field | Description
--- | ---
A11Mgr | The A11 Manager task instance number. Since multiple A11 Manager tasks can be operating simultaneously in the system, each one is assigned an instance number.
Total calls arrived | Indicates the total number of sessions received by this A11 Manager instance for processing.
Total calls rejected | Indicates the total number of sessions that were rejected by this A11 Manager instance.
Total calls demultiplexed | Indicates the total number of sessions that were successfully setup by this by this A11 Manager instance.
Total dereg reply sent | Indicates the total number of sessions that were successfully de-registered, or disconnected, by this by this A11 Manager instance.
Current active calls | Indicates the total number of active sessions currently being facilitated by this A11 Manager instance.
Total active services | The total number of PDSN services that are currently facilitating subscriber sessions.

show session subsystem facility aaamgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) and AAA Manager (AAAMgr) task itself (not from the subscriber perspective).
Table 8. show session subsystem facility aaamgr all Command Output Descriptions

Field | Description
--- | ---
AAA Manager | The AAA Manager task instance number. Since multiple AAA Manager tasks can be operating simultaneously in the system, each one is assigned an instance number.
Total aaa requests | The total number of AAA requests received by this AAAMgr instance for processing.
Current aaa requests | The number of AAA requests that this AAAMgr instance is currently processing.
Total aaa auth requests | The total number of AAA authentication requests that were received by this AAAMgr instance.
Current aaa auth requests | The number of AAA authentication requests that this AAAMgr instance is currently processing.
Total aaa auth probes | The total number of Authorization Probes that this AAAMgr instance has initiated.
Current aaa auth probes | The number of Authorization Probe requests that this AAAMgr instance is currently processing.
Total aaa auth keepalive | The total number of AAA authentication keepalive requests that were sent by this AAAMgr instance.
Current aaa auth keepalive | The number of AAA authentication keepalive requests that this AAAMgr instance is currently processing.
Total aaa acct requests | The total number of AAA accounting requests that were received by this AAAMgr instance.
Current aaa acct requests | The number of AAA accounting requests that this AAAMgr instance is currently processing.
Total aaa acct keepalive | The total number of AAA accounting keepalive requests that were sent by this AAAMgr instance.
Current aaa acct keepalive | The number of AAA accounting keepalive requests that this AAAMgr instance is currently processing.
Total aaa auth success | The total number of successful AAA authentications facilitated by this AAAMgr instance.
Total aaa no-auth null-username | The total number of AAA authentication requests dropped because of a null user name, or because there is no RADIUS null-username configured.
Total aaa auth failure | The total number of failed AAA authentications facilitated by this AAAMgr instance.
Total aaa auth purged | The total number of AAA authentication requests received by this AAAMgr instance that failed to get a response from the AAA server.
Total aaa auth cancelled | The total number of canceled AAA authentication requests facilitated by this AAAMgr instance.
Total auth keepalive success | The total number of successful authentication keepalives facilitated by this AAAMgr instance.
Total auth keepalive failure | The total number of failed authentication keepalives facilitated by this AAAMgr instance.
Total auth keepalive purged | The total number of authentication keepalive requests received by this AAAMgr instance that failed to get a response from the AAA server.
Total aaa auth DMU challenged | The total number of AAA authentication requests that were challenged for Dynamic Mobile Keying update.
aaa request (used/max) | The total number of AAA requests used and the maximum allowed for this AAAMgr instance.
Total Diameter auth requests | The total number of AAA authentication requests of the type Diameter authentication protocol facilitated by this AAAMgr instance.
Current Diameter auth requests | The number of AAA authentication requests of the type Diameter authentication protocol currently being processed by this AAAMgr instance.
Total Diameter auth requests retried | The total number of AAA authentication requests of the type Diameter authentication protocol that this AAAMgr instance retried. Retries occur when the AAAMgr instance does not receive a response from the AAA server to an initial request. The AAAMgr instance retries a request triggered by a timeout value configured under the AAA group.
Total Diameter auth requests dropped | The total number of AAA authentication requests of the type Diameter authentication protocol dropped by this AAAMgr instance due to the AAA server being unavailable or the system being out of memory.
Total radius auth requests | The total number of RADIUS authentication requests received by this AAAMgr instance.
Current radius auth requests | The number of RADIUS authentication requests currently being processed by this AAAMgr instance.
Total radius auth requests retried | The total number of RADIUS authentication requests processed by this AAAMgr instance that were retried.
Total radius auth responses dropped | The total number of RADIUS authentication responses dropped by the AAAMgr instance.
Total local auth requests | The total number of authentication requests received by this AAAMgr instance for locally configured subscribes.
Current local auth requests | The number of authentication requests currently being processed by this AAAMgr instance for locally configured subscribes.
Total pseudo auth requests | The total number of AAA requests for user profiles received by this AAAMgr instance.
Current pseudo auth requests | The number of current pending AAA requests for user profiles in this AAAMgr instance.
Total null-username auth requests (rejected) | The total number of AAA requests for un-attempted user profiles received by this AAAMgr instance.
Total aaa acct completed | The total number of AAA accounting requests received by this AAAMgr instance that were delivered successfully to the AAA server.
Total aaa acct purged | The total number of AAA accounting requests received by this AAAMgr instance that had to be purged because the storage limit of pending accounting requests had been exceeded.
Total acct keepalive success | The total number of successful accounting keepalives facilitated by this AAAMgr instance.
Total acct keepalive timeout | The total number of failed accounting keepalives facilitated by this AAAMgr instance.
Total acct keepalive purged | The total number of accounting keepalive requests received by this AAAMgr instance that failed to get a response from the AAA server.
Total aaa acct cancelled | The total number of AAA accounting requests received by this AAAMgr instance that were cancelled.
Total Diameter acct requests | The total number of AAA accounting requests of the type Diameter accounting protocol facilitated by this AAAMgr instance. This includes active and deleted requests.
Current Diameter acct requests | The number of AAA accounting requests of the type Diameter accounting protocol currently being processed by this AAAMgr instance.
Total Diameter acct requests retried | The total number of AAA accounting requests of the type Diameter accounting protocol that this AAAMgr instance retried. Retries occur when the AAAMgr instance does not receive a response from the AAA server to an initial request. The AAAMgr instance retries a request triggered by a timeout value configured under the AAA group.
Total diameter acct requests dropped | The total number of dropped AAA accounting requests of the type Diameter accounting protocol.
Total diameter acct responses dropped | The total number of dropped AAA accounting responses of the type Diameter accounting protocol.
Total diameter acct cancelled | The total number of cancelled AAA accounting requests of the type Diameter accounting protocol.
Total diameter acct purged | The total number of purged AAA accounting requests of the type Diameter accounting protocol.
Total radius acct requests | The total number of AAA accounting requests received by this AAAMgr instance for which the RADIUS protocol was used to deliver the accounting message to the AAA server.
Current radius acct requests | The number of AAA accounting requests currently being processed by this AAAMgr instance for which the RADIUS protocol is being used to deliver the accounting message to the AAA server.
Total radius acct cancelled | The total number of cancelled RADIUS accounting requests received by this AAAMgr instance.
Total radius acct purged | The total number of RADIUS accounting requests received by this AAAMgr instance that had to be purged because the storage limit of pending accounting requests had been exceeded.
Total radius acct requests retried | The total number of AAA accounting requests received by this AAAMgr instance for which the RADIUS protocol was used to deliver the accounting message to the AAA server that were retried.
Total radius acct responses dropped | The total number of RADIUS accounting responses dropped by the AAAMgr instance.
Total radius sec acct requests | The total number of AAA secondary accounting requests received by this AAAMgr instance for which the RADIUS protocol was used to deliver the accounting message to the AAA server.
Current radius sec acct requests | The number of AAA secondary accounting requests currently being processed by this AAAMgr instance for which the RADIUS protocol is being used to deliver the accounting message to the AAA server.
Total radius sec acct cancelled | The total number of cancelled RADIUS secondary accounting requests received by this AAAMgr instance.
Total radius sec acct purged | The total number of RADIUS secondary accounting requests received by this AAAMgr instance that had to be purged because the storage limit of pending accounting requests had been exceeded.
Total radius sec acct requests retried | The total number of AAA secondary accounting requests received by this AAAMgr instance for which the RADIUS protocol was used to deliver the accounting message to the AAA server that were retried.
Total gtpp acct requests | The total number of AAA accounting requests received by this AAAMgr instance for which the GTPP protocol was used to deliver the accounting message to the Charging Gateway Function (CGF).
Current gtpp acct requests | The current number of AAA accounting requests being processed by this AAAMgr instance for which the GTPP protocol is being used to deliver the accounting message to the Charging Gateway Function (CGF).
Total gtpp acct cancelled | The total number of accounting requests that were cancelled.
Total gtpp acct purged | The total number of accounting requests that were purged.
Total gtpp sec acct requests | The total number of secondary G-CDR requests being processed by this AAAMgr instance for which the GTPP protocol is being used to deliver the accounting message to the Charging Gateway Function (CGF). It counts total secondary G-CDRs generated by this AAAMgr instance.
Total gtpp sec acct purged | The total number of secondary G-CDR requests being processed and purged by this AAAMgr instance for which the GTPP protocol is being used to deliver the accounting message to the Charging Gateway Function (CGF). It counts total secondary G-CDRs purged by this AAAMgr instance.
Total null acct requests | The total number of AAA accounting requests received by this AAAMgr instance that were not required to be delivered to a AAA server.
Current null acct requests | The current number of AAA accounting requests being processed by this AAAMgr instance that are not required to be delivered to a AAA server.
Total aaa acct sessions | The total number of AAA accounting sessions facilitated by this AAAMgr instance.
Current aaa acct sessions | The number of AAA accounting sessions currently being facilitated by this AAAMgr instance.
Total aaa acct archived | The total number of AAA accounting requests received by this AAAMgr instance that initially failed to be delivered to a AAA server, and was subsequently archived for later transmission.
Current aaa acct archived | The current number of AAA accounting requests being processed by this AAAMgr instance that initially failed to be delivered to a AAA server and is currently archived for later transmission.
Current recovery archives | The number of AAA state records being maintained within the AAAMgr. They are used to generate accounting stops when a session manager fails or to recover the call in the Session Manager.
Current valid recovery records | The number of valid call recovery records that exist for current sessions.
Total aaa sockets opened | The total number of communication sockets opened by the AAAMgr instance for the purposes of communication with AAA servers.
Current aaa sockets open | The current number of communication sockets open by the AAAMgr instance for communication with AAA servers.
Total aaa requests pend socket open | The total number of AAA requests received by this AAAMgr instance that had to wait in queue while a socket to the AAA server was being opened.
Current aaa requests pend socket open | The number of AAA requests received by this AAAMgr instance that are currently waiting in queue while a socket to the AAA server is being opened.
Total radius requests pend server max-outstanding | The total number of RADIUS requests received by this AAAMgr instance that had to wait in queue because the limit of the number of outstanding RADIUS messages had been reached.
Current radius requests pend server max-outstanding | The number of RADIUS requests received by this AAAMgr instance that are currently waiting in queue because the limit of the number of outstanding RADIUS messages has been reached.
Total aaa radius coa requests | The total number of RADIUS Change Authorization Requests received from the RADIUS server.
Total aaa radius dm requests | The total number of RADIUS Disconnect Requests Received from the RADIUS server.
Total aaa radius coa acks | The total number of RADIUS Change Authorization Acknowledgement sent to the RADIUS server.
Total aaa radius dm acks | The total number of RADIUS Disconnect Acknowledgments sent to the RADIUS Server.
Total aaa radius coa naks | The total number of RADIUS Change Authorization Negative Acknowledgement sent to the RADIUS server.
Total aaa radius dm naks | The total number of RADIUS Disconnect Negative Acknowledgments sent to the RADIUS Server.
Total radius charg auth | The total number of authentication requests sent to the RADIUS charging server.
Total radius charg auth purg | The total number of RADIUS charging authentication requests purged.
Current radius charg auth | The total number of current authentication requests sent to the RADIUS charging server.
Total radius charg auth succ | The total number of successful authentication requests sent to the RADIUS charging server.
Total radius charg auth fail | The total number of access reject received from the RADIUS charging server.
Total radius charg auth cancel | The total number of accounting authorization request that were cancelled.
Total radius charg acct | The total number of accounting requests sent to the RADIUS charging server.
Current radius charg acct | The total number of current accounting requests sent to the RADIUS charging server
Total radius charg acct succ | The total number of accounting responses from the RADIUS charging server.
Total radius charg acct cancel | The total number of accounting requests that were cancelled.
Total gtpp charg | The total number of GTPP accounting requests sent to the server.
Current gtpp charg | The total number of current GTPP requests sent to the charging server.
Total gtpp charg success | The total number of successful GTPP accounting responses from the charging server.
Total gtpp charg failure | The total number of failed GTPP accounting requests from the charging server.
Total gtpp charg cancelled | The total number of cancelled GTPP accounting requests from the charging server.
Total gtpp charg purged | The total number of purged GTPP accounting requests.
Total radius charg acct purg | The total number of accounting requests purged.
Total gtpp sec charg | The total number of secondary eG-CDR charging requests being processed by this AAAMgr instance for which the GTPP protocol is being used to deliver the charging message to the Charging Gateway Function (CGF). It counts total secondary eG-CDRs generated by this AAAMgr instance.
Total gtpp sec charg purged | The total number of secondary eG-CDRs charging requests being processed and purged by this AAAMgr instance for which the GTPP protocol is being used to deliver the charging message to the Charging Gateway Function (CGF) . It counts total secondary eG-CDRs purged by this AAAMgr instance
Total prepaid online requests | The total number of prepaid online requests.
Current prepaid online requests | The number of prepaid online requests that this AAAMgr instance is currently processing.
Total prepaid online success | The total number of prepaid online requests succeed.
Current prepaid online failure | The number of failed prepaid online requests that this AAAMgr instance is currently processing.
Total prepaid online retried | The total number of prepaid online requests retried.
Total prepaid online cancelled | The total number of prepaid online requests cancelled.
Current prepaid online purged | The total prepaid online cancelled.
Total aaamgr purged requests | The total number of purged AAAMgr requests.
SGSN: Total mm records | Total number of Mobility Management (MM) records in database of this AAAMgr instance for SGSN service.
SGSN: Total pdp records | Total number of PDP context records in database of this AAAMgr instance for SGSN service.
SGSN: Total auth records | Total number of authentication records in database of this AAAMgr instance for SGSN service.
MME: Total extension records | Total number of extension records in database of this AAAMgr instance for MME service.
MME: Total apn records | Total number of APN records in database of this AAAMgr instance for MME service.
MME: Total apn extension records | Total number of extended APN records in database of this AAAMgr instance for MME service.
MME: Total auth records | Total number of authentication records in database of this AAAMgr instance for MME service.
MME: Total auth extension records | Total number of extended authentication records in database of this AAAMgr instance for MME service.
Current active subscriber traces | Total number of subscribers currently enabled with Subscriber Tracing function in database of this AAAMgr instance for MME service.

show session subsystem facility aaaproxy all

IMPORTANT:

These statistics are from the perspective of the Session manager (SessMgr) and AAA Proxy Manager (AAAProxyMgr) task itself (not from the perspective of subscribers).
Table 9. show session subsystem facility aaaproxy all Command Output Descriptions

Field | Description
--- | ---
Total gtpp requests | The total number of GTPP requests sent.
Current gtpp requests | The total number of outstanding GTPP requests waiting for response from CGF/storage server.
Total GCDRs | The total number of G-CDRs sent.
Current GCDRs | The total number of outstanding G-CDRs waiting for response from CGF/storage server.
Total G-MB-CDRs | The total number of G-MB-CDRs sent.
Current G-MB-CDRs | The total number of outstanding G-MB_CDRs waiting for response from CGF/storage server.
Total SCDRs | The total number of S-CDRs sent.
Current SCDRs | The total number of outstanding S-CDRs waiting for response from CGF/storage server.
Total MCDRs | The total number of M-CDRs sent.
Current MCDRs | The total number of outstanding M-CDRs waiting for response from CGF/storage server.
Total S-SMO-CDRs | The total number of S-SMO-CDRs sent.
Current S-SMO-CDRs | The total number of outstanding S-SMO-CDRs waiting for response from CGF/storage server.
Total S-SMT-CDRs | The total number of S-SMT-CDRs sent.
Current S-SMT-CDRs | The total number of outstanding S-SMT-CDRs waiting for response from CGF/storage server.
Total SMBMSCDRs | The total number of outstanding SMBMS CDRs waiting for response from CGF/storage server.
Total SGW-CDRs | The total number of outstanding S-GW CDRs waiting for response from CGF/storage server.
Total WLAN-CDRs | The total number of outstanding WLANGW CDRs waiting for response from CGF/storage server.
Total sockets opened | The total number of sockets opened.
Current sockets opened | The total number of sockets waiting to open.
Total files closed | The total number of files that have been already closed.
Current Open files | The number of files that are currently open and still in use.

show session subsystem facility asngwmgr all

IMPORTANT:

These statistics are from the perspective of the Session manager (SessMgr) and ASNGW Manager (ASNGWMgr) task itself (not from the perspective of subscribers).
Table 10. show session subsystem facility asngwmgr all Command Output Descriptions

Field | Description
--- | ---
ASNGW Managers | Total number of active ASN GW Managers.
Total active services | Total number of active ASN GW services.
Anchor Session | Specifies the subsystem statistics for ASN GW service sessions in anchored mode.
Non-Anchor Session | Specifies the subsystem statistics for ASN GW service sessions in non-anchored mode.
Total calls arrived | Indicates the total number of sessions received by this ASN Gateway Manager instance for processing.
Total calls rejected | Indicates the total number of sessions that were rejected by this ASN Gateway Manager instance.
Total calls demultiplexed | Indicates the total number of sessions that were successfully setup by this by this ASN Gateway Manager instance.
Total dereg reply sent | Indicates the total number of sessions that were successfully de-registered, or disconnected, by this ASN Gateway Manager instance.
Total control pkts relayed | Indicates the total number of R6 control packets relayed via demux manager.
Current active calls | Indicates the total number of active sessions currently being facilitated by this ASN Gateway Manager instance.
Total active services | The total number of ASN Gateway services that are currently facilitating subscriber sessions.

show session subsystem facility asnpcmgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) and ASN-PC Manager (ASNPCMgr) task itself (not from the subscriber perspective).
Table 11. show session subsystem facility asngwmgr all Command Output Descriptions

Field | Description
--- | ---
ASNPC Managers | Total number of active ASN PC Manager instances.
Total active services | Total number of active ASN PC services.
Total calls arrived | Indicates the total number of sessions received by this ASN PC Manager instance for processing.
Total calls rejected | Indicates the total number of sessions that were rejected by this ASN PC Manager instance.
Total calls demultiplexed | Indicates the total number of sessions that were successfully setup by this by this ASN PC Manager instance.
Total calls released | Indicates the total number of sessions that were successfully de-registered, or disconnected, by this ASN PC Manager instance.
Total control pkts relayed | Indicates the total number of R6 control packets relayed via demux manager.
Current active calls | Indicates the total number of active sessions currently being facilitated by this ASN Gateway Manager instance.
context name | Indicates the name of the context where ASN PC service is configured.

show session subsystem facility egtpinmgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) and EGTP Ingress Demux Manager (EGTPCinMgr) task itself (not from the subscriber perspective).
Table 12. show session subsystem facility egtpinmgr Command Output Descriptions

Field | Description
--- | ---
EGTPINMgr | The EGTP Ingress Demux Manager task instance number. Since multiple EGTP Manager tasks can be operating simultaneously in the system, each one is assigned an instance number.
Total calls arrived | Indicates the total number of sessions received by this EGTP Manager instance for processing.
Total calls rejected | Indicates the total number of sessions that were rejected by this EGTP Manager instance.
Total calls demultiplexed | Indicates the total number of sessions that were successfully setup by this by this EGTP Manager instance.
Total SGSNs | Indicates the total number of SGSNs available for facilitating subscriber sessions.
Total Active SGSNs | The total number of SGSNs that are currently facilitating subscriber sessions.
Total active services | The total number of EGTP services that are currently facilitating subscriber sessions.

show session subsystem facility famgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) and FA Manager (FAMgr) task itself (not from the subscriber perspective).
Table 13. show session subsystem facility famgr Command Output Descriptions

Field | Description
--- | ---
FAMgr | The FA Manager task instance number. Since multiple FA Manager tasks can be operating simultaneously in the system, each one is assigned an instance number.
Total calls arrived | Indicates the total number of sessions received by this FA Manager instance for processing.
Total calls rejected | Indicates the total number of sessions that were rejected by this FA Manager instance.
Total calls demultiplexed | Indicates the total number of sessions that were successfully setup by this by this FA Manager instance.
Total dereg reply sent | Indicates the total number of sessions that were successfully de-registered, or disconnected, by this by this FA Manager instance.
Current active calls | Indicates the total number of active sessions currently being facilitated by this FA Manager instance.
Total active services | The total number of FA services that are currently facilitating subscriber sessions.

show session subsystem facility gtpcmgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) and GTPC Manager (GTPCMgr) task itself (not from the subscriber perspective).

IMPORTANT:

This command is not suppo.rted release 14.0 onwards. Look for new command “show session subsystem facility egtpinmgr all” instead.
Table 14. show session subsystem facility gtpcmgr Command Output Descriptions

Field | Description
--- | ---
GTPCMgr | The GTPC Manager task instance number. Since multiple GTPC Manager tasks can be operating simultaneously in the system, each one is assigned an instance number.
Total calls arrived | Indicates the total number of sessions received by this GTPC Manager instance for processing.
Total calls rejected | Indicates the total number of sessions that were rejected by this GTPC Manager instance.
Total calls demultiplexed | Indicates the total number of sessions that were successfully setup by this by this GTPC Manager instance.
Total SGSNs | Indicates the total number of SGSNs available for facilitating subscriber sessions.
Total Active SGSNs | The total number of SGSNs that are currently facilitating subscriber sessions.
Current active calls | Indicates the total number of active sessions currently being facilitated by this GTPC Manager instance.
Total active services | The total number of GTPC services that are currently facilitating subscriber sessions.

show session subsystem facility hamgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) and HA Manager (HAMgr) task itself (not from the subscriber perspective).
Table 15. show session subsystem facility hamgr all Command Output Descriptions

Field | Description
--- | ---
HAMgr | The HA Manager task instance number. Since multiple HA Manager tasks can be operating simultaneously in the system, each one is assigned an instance number.
Total calls arrived | Indicates the total number of sessions received by this HA Manager instance for processing.
Total calls rejected | Indicates the total number of sessions that were rejected by this HA Manager instance.
Total calls demultiplexed | Indicates the total number of sessions that were successfully setup by this by this HA Manager instance.
Total dereg reply sent | Indicates the total number of sessions that were successfully de-registered, or disconnected, by this by this HA Manager instance.
Current active calls | Indicates the total number of active sessions currently being facilitated by this HA Manager instance.
Total active services | The total number of HA services that are currently facilitating subscriber sessions.

show session subsystem facility mmedemux

IMPORTANT:

These statistics are from the perspective of the MME Demux Manager (MMEDemuxr) task itself (not from the subscriber perspective).
Table 16. show session subsystem facility mmedemux Output Descriptions

Field | Description
--- | ---
MME Demux Managers | The total number of MME managers running on a chassis.
Total number of packets received | The total number of packets received and processed for EPS session by the MME Demux manager.
Total number of packets received (IPSec) | The total number of encrypted packets received and processed for EPS session by the MME Demux manager.
Total number of packets dropped | The total number of packets received but dropped by the MME Demux manager.
Total number of packets dropped (Assurance Violation) | The total number of packets received but dropped due to not being encrypted.
Total number of octets received | The total number of packets received and processed for EPS session by the MME Demux manager.
Total number of octets received (IPSec) | The total number of encrypted octets received and processed for EPS session by the MME Demux manager.
Total number of octets dropped | The total number of octets received but dropped by the MME Demux manager.
Total number of octets dropped (Assurance Violation) | The total number of octets received but dropped due to not being encrypted.
Total Services | The total number of MME services managed by the MME Demux Manager.
Total Services (IPSec) | The total number of IPSec-enabled MME services managed by the MME Demux Manager.
Enodeb Associations | The total number of eNodeBs connected/associated with MME services managed by the MME Demux Manager.
Enodeb Associations (IPSec) | The total number of IPSec-enabled eNodeBs connected/associated with MME services managed by the MME Demux Manager.

show session subsystem facility mmemgr all

IMPORTANT:

These statistics are from the perspective of the MME Manager (MMEMgr) task itself (not from the subscriber perspective).
Table 17. show session subsystem facility mmemgr all Output Descriptions

Field | Description
--- | ---
MME Managers | Indicates the total number of MME managers running on a chassis.
SCTP Statistics | This group displays the statistics captured over the SCTP interface and processed by this MME manager.
Transmitted SCTP Data | This sub-group displays the statistics of the total data processed and transmitted over SCTP interface by this MME manager.
Init Chunks | Indicates the total SCTP packets with INIT transmitted over SCTP interface by this MME manager.
Init Ack Chunks | Indicates the total SCTP packets with INIT-ACK transmitted over SCTP interface by this MME manager.
Shutdown Chunks | Indicates the total SCTP packets with SHUTDOWN transmitted over SCTP interface by this MME manager.
Shutdown Ack Chunks | Indicates the total SCTP packets with SHUTDOWN-ACK transmitted over SCTP interface by this MME manager.
Cookie Chunks | Indicates the total SCTP packets with COOKIE transmitted over SCTP interface by this MME manager.
Cookie Ack Chunks | Indicates the total SCTP packets with COOKIE-ACK transmitted over SCTP interface by this MME manager.
Data Chunks | Indicates the total SCTP packets with DATA transmitted over SCTP interface by this MME manager.
Data Ack Chunks | Indicates the total SCTP packets with DATA-ACK transmitted over SCTP interface by this MME manager.
Shutdown Complete Chunks | Indicates the total SCTP packets with SHUTDOWN-COMPLETE transmitted over SCTP interface by this MME manager.
Heartbeat Chunks | Indicates the total SCTP packets with HEARTBEAT transmitted over SCTP interface by this MME manager.
HeartBeat Ack Chunks | Indicates the total SCTP packets with HEARTBEAT-ACK transmitted over SCTP interface by this MME manager.
Abort Chunks | Indicates the total SCTP packets with ABORT transmitted over SCTP interface by this MME manager.
Error Chunks | Indicates the total SCTP packets with ERROR transmitted over SCTP interface by this MME manager.
Received SCTP Data | This sub-group displays the statistics of the total data received over SCTP interface and processed by this MME manager.
Init Chunks | Indicates the total SCTP packets with INIT received over SCTP interface by this MME manager.
Init Ack Chunks | Indicates the total SCTP packets with INIT-ACK received over SCTP interface by this MME manager.
Shutdown Chunks | Indicates the total SCTP packets with SHUTDOWN received over SCTP interface by this MME manager.
Shutdown Ack Chunks | Indicates the total SCTP packets with SHUTDOWN-ACK received over SCTP interface by this MME manager.
Cookie Chunks | Indicates the total SCTP packets with COOKIE received over SCTP interface by this MME manager.
Cookie Ack Chunks | Indicates the total SCTP packets with COOKIE-ACK received over SCTP interface by this MME manager.
Data Chunks | Indicates the total SCTP packets with DATA received over SCTP interface by this MME manager.
Data Ack Chunks | Indicates the total SCTP packets with DATA-ACK received over SCTP interface by this MME manager.
Shutdown Complete Chunks | Indicates the total SCTP packets with SHUTDOWN-COMPLETE received over SCTP interface by this MME manager.
Heartbeat Chunks | Indicates the total SCTP packets with HEARTBEAT received over SCTP interface by this MME manager.
HeartBeat Ack Chunks | Indicates the total SCTP packets with HEARTBEAT-ACK received over SCTP interface by this MME manager.
Abort Chunks | Indicates the total SCTP packets with ABORT received over SCTP interface by this MME manager.
Error Chunks | Indicates the total SCTP packets with ERROR received over SCTP interface by this MME manager.
Retransmitted SCTP Data | This sub-group displays the statistics of the total data processed and retransmitted over SCTP interface by this MME manager.
Init Chunks | Indicates the total SCTP packets with INIT retransmitted over SCTP interface by this MME manager.
Shutdown Chunks | Indicates the total SCTP packets with SHUTDOWN retransmitted over SCTP interface by this MME manager.
Shutdown Ack Chunks | indicates the total SCTP packets with SHUTDOWN-ACK retransmitted over SCTP interface by this MME manager.
Cookie Chunks | Indicates the total SCTP packets with COOKIE retransmitted over SCTP interface by this MME manager.
Data Chunks | Indicates the total SCTP packets with DATA transmitted over SCTP interface by this MME manager.
Total Bytes Sent To Lower Layer | Indicates the total bytes processed and sent to lower layer over SCTP interface by this MME manager.
Total Bytes Received From Lower Layer | Indicates the total bytes received from lower layer over SCTP interface by this MME manager for processing.
Total Packets Sent To Lower Layer | Indicates the total packets processed and sent to lower layer over SCTP interface by this MME manager.
Total Packets Received From Lower Layer | Indicates the total packets received from lower layer over SCTP interface by this MME manager for processing.
S1AP Statistics | This group displays the statistics captured over S1-AP interface and processed by this MME manager received or transmitted from/to eNodeB.
Transmitted S1AP Data | This sub-group displays the statistics of the total data processed and transmitted over S1-AP interface by this MME manager to eNodeB.
S1 Setup Response | Indicates the total number of S1 SETUP RESPONSE messages for S1 setup procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
S1 Setup Failure | Indicates the total number of S1 SETUP FAILURE messages for S1 setup procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
Reset | Indicates the total number of S1 RESET messages for S1 reset procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
Reset Acknowledge | Indicates the total number of S1 RESET-ACK messages for S1 reset procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
Overload Start | Indicates the total number of OVERLOAD-START messages for S1 overload start procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
Overload Stop | Indicates the total number of OVERLOAD-START messages for S1 overload start procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
MME Dir Information Transfer | Indicates the total number of MME DIRECT INFORMATION TRANSFER messages for MME Direct Information Transfer procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
Paging | Indicates the total number of PAGING messages for paging procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
EnodeB Configuration Update Acknowledge | Indicates the total number of ENB CONFIGURATION UPDATE ACK messages for eNB Configuration Update procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
EnodeB Configuration Update Failure | Indicates the total number of ENB CONFIGURATION UPDATE FAILURE messages for eNB Configuration Update procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
S1AP Encode Failure | Indicates the total number of failure occurred during S1AP encode procedure and S1AP ENCODE FAILURE messages processed and transmitted over S1-AP interface by this MME manager to eNodeB.
Received S1AP Data | This sub-group displays the statistics of the total data received over S1-AP interface by this MME manager from eNodeB.
S1 Setup Request | Indicates the total number of S1 SETUP REQUEST messages for S1 setup procedure received over S1-AP interface by this MME manager from eNodeB.
Reset | Indicates the total number of S1 RESET messages for S1 reset procedure received over S1-AP interface by this MME manager from eNodeB.
Reset Acknowledge | Indicates the total number of S1 RESET-ACK messages for S1 reset procedure received over S1-AP interface by this MME manager from eNodeB.
EnodeB Dir Information Transfer | Indicates the total number of ENB DIRECT INFORMATION TRANSFER messages for eNB Direct Information Transfer procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
EnodeB Configuration Update | Indicates the total number of ENB CONFIGURATION UPDATE messages for eNB Configuration Update procedure processed and transmitted over S1-AP interface by this MME manager to eNodeB.
S1AP Decode Failure | Indicates the total number of failure occurred during S1AP decoding procedure by eNodeB and S1AP DECODE FAILURE messages received over S1-AP interface by this MME manager from eNodeB.
S1AP Unexpected Event | Indicates the total number of failure occurred due to unexpected events during S1AP procedure at eNodeB and S1AP UNEXPECTED EVENT messages received over S1-AP interface by this MME manager from eNodeB.
Total Services | Indicates the total number of MME services managed by this MME Manager.
Total Services (IPSec) | Indicates the total number of IPSec-enabled MME services managed by this MME Manager.
Enodeb Associations | Indicates the total number of eNodeBs connected/associated with MME services managed by this MME Manager.
Enodeb Associations (IPSec) | Indicates the total number of IPSec-enabled eNodeBs connected/associated with MME services managed by this MME Manager.

show session subsystem facility sessmgr all

IMPORTANT:

These statistics are from the perspective of the Session Manager (SessMgr) task itself (not from the subscriber perspective).
Table 18. show session subsystem facility sessmgr all Output Descriptions

Field | Description
--- | ---
SessMgr | Displays the Session Manager task instance number. Since multiple Session Manager tasks can be operating simultaneously in the system, each one is assigned an instance number.
Total calls arrived | The total number of calls for which registration requests were received by this Session Manager instance.
Total calls rejected | The total number of calls that were rejected by this Session Manager instance.
Total calls connected | The total number of calls that are connected (including active, dormant, being set up, and being disconnected) by this Session Manager instance.
Total calls failed | The total number of calls processed by this Session Manager instance which have failed.
Total calls disconnected | The total number of calls that were disconnected by this Session Manager instance.
Total handoffs | The total number of calls that are handed off by this Session Manager instance.
Total renewals | The total number of call that were reprocessed by this Session Manager instance.
Total active-to-idle transitions | The total number of call sessions passed through active mode to idle mode.
Total idle-to-active transitions | The total number of call sessions passed through idle mode to active mode.
Total auth successes | The total number of successful authentications for calls being processed by this Session Manager instance.
Total auth failure | The total number of failed authentications for calls being processed by this Session Manager instance.
Current aaa active sessions | The total number of calls being processed by this Session Manager instance for which there are active AAA authentication and/or accounting sessions.
Current aaa deleting sessions | The total number of calls being processed by this Session Manager instance for which the AAA accounting is being terminated.
Current aaa acct pending | The total number of calls being processed by this Session Manager instance for which there are pending AAA authentication and/or accounting sessions.
aaa acct items (used/max) | The total number of AAA accounting items used and the maximum allowed by this Session Manager instance.
aaa buffer (used in MB/max in MB) | The AAA buffer space used and the maximum allowed in megabytes for this Session Manager instance.
Total aaa cancel auth | The total number of canceled AAA authentication requests for this Session Manager instance.
Total aaa acct purged | The total number of AAA accounting requests received by this Session Manager instance that had to be purged because the storage limit of pending accounting requests had been exceeded.
Total radius acct purged | The total number of RADIUS accounting requests received by this Session Manager instance that had to be purged because the storage limit of pending accounting requests had been exceeded.
Total LCP up | The total number of calls being processed by this Session Manager instance that have completed the Link Control Protocol (LCP) phase of the registration process.
Total IPCP up | The total number of calls being processed by this Session Manager instance that have completed the Internet Protocol Control Protocol (IPCP) phase of the registration process.
Total IPv6CP up | The total number of calls being processed by this Session Manager instance that have completed the Internet Protocol version 6 (IPv6) phase of the registration process.
Total source violation | The total number of source violations experienced for all calls being processed by this Session Manager instance.
Total keepalive failure | The total number of keep-alive failures experienced for all calls being processed by this Session Manager instance.
Empty fwd pkt sessions | The total number of calls that were processed by this session manager instance for which there were no data packets being sent to the subscriber.
Empty rev pkt sessions | The total number of calls that were processed by this session manager instance for which there were no data packets being received from the subscriber.
Total 3gpp2 prepaid sess | The total number of 3gpp2 prepaid sessions on the system.
Current 3gpp2 prepaid sess | The current number of active 3gpp2 prepaid sessions on the system.
Total 3gpp2 online auth requests | The total number of 3gpp2 sessions requesting authentication on the system.
Total 3gpp2 online auth success | The total number of authenticated 3gpp2 active sessions on the system.
Total 3gpp2 online auth failures | The total number of 3gpp2 sessions that had authentication failures.
Total 3gpp2 online prepaid errors | The total number of prepaid 3gpp2 sessions that incurred errors.
Total 3gpp2 prepaid initial auth errors | The total number of prepaid initial 3gpp2 sessions that had authentication errors.
Total Rfc3261 subscribers | Total number of subscribers registered in CSCF Rfc3261 service.
Total Proxy Cscf subscribers | Total number of subscribers registered in Proxy-CSCF service.
Total Serving Cscf subscribers | Total number of subscribers registered in Serving-CSCF service.
Total Proxy-Serving cscf subscribers | Total number of subscribers registered in Collapsed Proxy-Serving-CSCF service.
Total voice-push sessions | The total number of voice-push sessions.
Current voice-push sessions | The current number of active voice-push sessions.
Total voice-push-filt sessions | The total number of voice-push-filt sessions.
Current voice-push-filt sessions | The current number of voice-push-filt sessions.
Total non-voice-push sessions | The total number of non-voice-push session.
Current non-voice-push sessions | The current number of non-voice-push sessions
Total undetermined sessions | The total number of undetermined sessions.
Current undetermined sessions | The current number of undetermined sessions.
Intra-ASNGW HO attempted | The total number of inter-BS (Intra-ASN GW) handovers attempted by system.
Intra-ASNGW HO succeeded | The total number of inter-BS (Intra-ASN GW) handover attempts succeeded.
Inter-ASNGW HO attempted | The total number of inter-ASN GW handovers attempted by system.
Inter-ASNGW HO succeeded | The total number of inter-ASN GW handover attempts succeeded.
ASNPC IM Entry attempted | The total number of idle mode entry attempted by Paging Controller.
ASNPC IM Entry Succeeded | The total number of idle mode entry by Paging Controller succeeded.
ASNPC IM Exit attempted | The total number of idle mode exit attempted by Paging Controller.
ASNPC IM Exit Succeeded | The total number of idle mode exit by Paging Controller succeeded.
ASNPC LU attempted | The total number of location updates attempted by Paging Controller.
ASNPC LU Succeeded | The total number of location updates by Paging Controller succeeded.
ASNPC Paging Triggered | The total number of pagings triggered by Paging Controller.
ASN Ctrl packets received | The total number of control packets received for ASN GW service session.
ASN Ctrl packets runt received | The total number of control packets with run-time error discarded for ASN GW service session.
ASN Ctrl packets csum received | The total number of control packets with checksum error discarded for ASN GW service session.
ASN Ctrl packets no-flow discarded | The total number of control packets (without any flow) discarded for ASN GW service session.
ASNGW data pkts stored (during paging) | The total number of data packets stored during paging.
ASNGW data pkts flushed (during paging) | The total number of data packets flushed during paging.
CRP-RP handoff attempted | The total number of Closed RP to RP handoffs that were attempted.
CRP-RP handoff succeeded | The total number of Closed RP to RP handoffs that succeeded.
RP-CRP handoff attempted | The total number of RP to Closed RP handoffs that were attempted.
RP-CRP handoff succeeded | The total number of RP to Closed RP handoffs that succeeded.
Current active subscriber traces | Total number of subscribers currently enabled with Subscriber Tracing function in database of this SessMgr instance for MME service.
Data statistics | This table categorizes the number of Receive and Transmit packets into packet size ranges. These statistics are totals for all calls being processed by this Session Manager instance.
In-Progress Call Duration Statistics | This table categorizes the total number of calls being processed by this Session Manager according to various time durations ranging from less than ( < ) 1 minute to greater than ( > ) 24 hours.
Setup Time Statistics | This table categorizes the amount of time it took to set up calls according to various time durations ranging from less than ( < ) 100 ms to greater than ( > ) 18 seconds.
Total SGSN Fast Path statistics update | Total number of updates for statistical information from NPU in fast path support. The title of this counter is valid in release 12.2 and earlier versions.
Total Gtpu Fast Path statistics update | Total number of updates for statistical information from NPU in fast path support. The title of this counter is valid in release 14.0 and later versions.
Total SGSN Fast Path out-of-order statistics updates | Total number of updates for out of order packet statistics from NPU in fast path support. The title of this counter is valid in release 12.2 and earlier versions.
Total Gtpu Fast Path out-of-order statistics updates | Total number of updates for out of order packet statistics from NPU in fast path support. The title of this counter is valid in release 14.0 and later versions.
Total SGSN Fast Path statistics updates lost | Total number of packets lost for statistical updates from NPU in fast path support. The title of this counter is valid in release 12.2 and earlier versions.
Total Gtpu Fast Path statistics updates lost | Total number of packets lost for statistical updates from NPU in fast path support. The title of this counter is valid in release 14.0 and later versions.
Total SGSN Fast Path packets lost | Total number of lost packets of all types from NPU in fast path support. The title of this counter is valid in release 12.2 and earlier versions.
Total Gtpu Fast Path packets lost | Total number of lost packets of all types from NPU in fast path support. The title of this counter is valid in release 14.0 and later versions.
Total SGSN Fast Path bytes lost | Total number of lost bytes from NPU in fast path support. The title of this counter is valid in release 12.2 and earlier versions.
Total Gtpu Fast Path bytes lost | Total number of lost bytes from NPU in fast path support. The title of this counter is valid in release 14.0 and later versions.
Total SGSN Fast Path packets received | Total number of all type of packets received from NPU in fast path support. The title of this counter is valid in release 12.2 and earlier versions.
Total Gtpu Fast Path packets received | Total number of all type of packets received from NPU in fast path support. The title of this counter is valid in release 14.0 and later versions.
Total SGSN Fast Path bytes received | Total number of all type of bytes received from NPU in fast path support. The title of this counter is valid in release 12.2 and earlier versions.
Total Gtpu Fast Path bytes received | Total number of all type of bytes received from NPU in fast path support. The title of this counter is valid in release 14.0 and later versions.
In-progress calls | The number of calls that are currently in progress (active, dormant, being set up, or being disconnected) and being processed by either the system (if no keywords were used), a specific PDSN service (if the pdsn-service keyword was used), or a specific PCF (if the pcf keyword was used).
In-progress active calls | The total number of active sessions being processed by this Session Manager instance.
In-progress dormant calls | The total number of dormant sessions being processed by this Session Manager instance.
In-progress always-on calls | The total number of always-on sessions being processed by this Session Manager instance.
In-progress calls @ MBMS UE AUTHORIZING state | The total number of MBMS sessions currently in UE authorization state.
In-progress calls @ MBMS BEARER AUTHORIZING state | The total number of MBMS sessions currently in bearer authorization state.
In-progress calls @ ARRIVED state | The total number of sessions being processed by this Session Manager instance that are at the onset of the registration process.
In-progress calls @ LCP-NEG state | The total number of sessions being processed by this Session Manager instance that are in the Link Control Protocol (LCP) negotiation phase of the registration process.
In-progress calls @ LCP-UP state | The total number of sessions being processed by this Session Manager instance that have just completed the Link Control Protocol (LCP) negotiation phase of the registration process.
In-progress calls @ AUTHENTICATING state | The total number of sessions being processed by this Session Manager instance that are in the process of being authenticated.
In-progress calls @ AUTHENTICATED state | The total number of sessions being processed by this Session Manager instance that have just completed the authentication phase of the registration process.
In-progress calls @ L2TP-LAC CONNECTING state | The number of calls that have an L2TP tunnel in the process of being brought up.
In-progress calls @ IPCP-UP state | The total number of sessions being processed by this Session Manager instance that have just completed the Internet Protocol Control Protocol (IPCP) phase of the registration process.
In-progress calls @ NON-ANCHOR CONNECTED state | The total number of WiMAX sessions being processed by this Session Manager instance that are currently being in connected state in non-anchor mode.
In-progress calls @ SIMPLE-IP CONNECTED state | The total number of Simple IP data sessions being processed by this Session Manager instance that are currently being supported.
In-progress calls @ MOBILE-IP CONNECTED state | The total number of Mobile IP data sessions being processed by this Session Manager instance that are currently being supported.
In-progress calls @ PROXY-MOBILE-IP CONNECTED state | The total number of Proxy Mobile IP data sessions being processed by this Session Manager instance that are currently being supported.
In-progress calls @ L2TP-LAC CONNECTED state | The number of calls that are passing data through an L2TP tunnel.
In-progress calls @ PDP-TYPE-IP CONNECTED state | The total number of PDP contexts of type IP that are currently connected. This field applies to GGSN only.
In-progress calls @ PDP-TYPE-PPP CONNECTED state | The total number of PDP contexts of type PPP that are currently connected. This field applies to GGSN only.
In-progress calls @ BCMCS CONNECTED state | The total number of BCMCS sessions currently in connected state.
In-progress calls @ MBMS UE CONNECTED state | The total number of MBMS sessions currently in UE connected state.
In-progress calls @ MBMS BEARER CONNECTED state | The total number of MBMS sessions currently in bearer connected state.
In-progress calls @ ASNPC CONNECTED state | The number of ASN Paging Controller calls that are currently connected.
In-progress calls @ DISCONNECTING state | The total number of sessions being processed by this Session Manager instance that are in the process of disconnecting.
In-progress calls @ CSCF-REGISTERING state | Total number of CSCF sessions which are in registration processing state.
In-progress calls @ CSCF-REGISTERED state | Total number of cscf sessions which are in registered state.
In-progress calls @ CSCF-CALL-ARRIVED state | Total number of CSCF sessions which are processing the newly arrived CSCF calls (i.e., processing initial Invite, waiting for provisional response, waiting for final response, etc.).
In-progress calls @ CSCF-CALL-CONNECTING state | Total number of CSCF sessions which are in call connecting state (waiting for ACK).
In-progress calls @ CSCF-CALL-CONNECTED state | Total number of CSCF sessions which are in call connected state.
In-progress calls @ CSCF-CALL-DISCONNECTING state | Total number of CSCF sessions which are in call disconnecting state (i.e., processing BYE , waiting for BYE response, etc.).
In-progress calls @ MME ATTACHED state | Indicates the number of MME subscriber session currently attached.
User Data statistics | This section indicates the Data octets and Data packets received and send by a user.
Data octets from User | The number of Data octets send from the user.
Data octets to User | The number of Data octets received by the user.
Data packets from User | The number of Data packets send from the user.
Data packets to User | The number of Data packets received by the user.

show session trace statistics
Table 19. show session trace statistics Command Output Descriptions

Field | Description
--- | ---
Network Element Status | Specifies if session traces are enabled for the listed network elements.
Number of current trace sessions | The total number of session traces currently active.
Total trace sessions activated | The total number of session traces activated.
Total number of trace session activation failures | The total number of session activation failures.
Total number of trace recording sessions triggered | The total number of trace recording sessions triggered
Total number of messages traced | The total number of messages traced for the activated session traces.
Number of messages dropped
No memory | The total number of messages dropped due to a no memory condition.
No trace recording session | The total number of messages dropped due to a failure to receive the start trigger.
Interface not traced | The total number of messages dropped due to the messages being received on interfaces not part of the trace interface list.
Total number of file generated | The total number of session trace files generated.
Number of files deleted
No space | The total number of files deleted due to a lack of space on the storage device.
Number of current TCE connections | The total number of trace collection entity connections currently configured.
Total number of TCE connections | The total number of trace collection entity connections configured.
Total number of files uploaded to all TCEs | The total number of files uploaded to all trace collection entities.

show session trace subscriber

The full command is as follows:

    show session trace
    subscriber network-element <type> trace-ref <id>

Table 20. show session trace subscriber Command Output Descriptions

Field | Description
--- | ---
Trace reference | The trace reference ID for the trace displayed. The ID is the MCC (3 digits), followed by the MNC (3 digits), then the trace ID number (3 byte octet string).
Activation time | The date and time when the trace was initiated.
IMEI or IMSI | The subscriber identification. IMEI: The International Mobile Equipment Identification number of the subscriber’s UE. IMSI: The International Mobile Subscriber Identification (IMSI) which is the 3-digit MCC (Mobile Country Code), 2 or 3-digit MNC (Mobile Network Code), and the MSIN (Mobile Subscriber Identification Number).
Actively Tracing | Specifies if the trace is currently active.
Trace Recording Session Reference | The current active trace recording session reference number.
Recording start time | The date and time when the session trace recording started.
Total number of trace recording sessions triggered | The total number of trace recording sessions initiated.
Total number of messages traced | The total number of messages traced for this trace reference.
Number of messages dropped
No memory | The total number of messages dropped due to a no memory condition.
No trace recording session | The total number of messages dropped due to a failure to receive the start trigger.
Interface not traced | The total number of messages dropped due to the messages being received on interfaces not part of the trace interface list.
Total number of files created | The total number of trace recording files created.
Number of files deleted
No space | The total number of files deleted due to a lack of space on the storage device.
Traced Interfaces | List of interfaces configured for the session trace.
Trace Triggers | Identifies the triggers used by this subscriber.