# Remote Server List Configuration Mode Commands

The Remote Server List Configuration Mode manages the list of server addresses to which a context has access.

IMPORTANT:

Available commands or keywords/variables vary based on platform type, product version, and installed license(s).
address

Configures or removes an IP address to a remote server.
Platform:

ASR 5000

ASR 5500
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    address remote-ip-address netmask ip_netmaskno address remote-ip-address netmask ip_netmask

no

Removes the specified IP address from the Remote Server List.
remote-ip-address netmask ip_netmask

Specifies the IP address and netmask of the remote server in IPv4 dotted-decimal or IPv6 colon-separated-hexadecimal notation.
Usage:

Use this command to create and maintain a list of remote servers accessible by this context.
Example:

    address 193.154.78.9
    netmask 255.255.255.0

end

Exits the current configuration mode and returns to the Exec mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    end

Usage:

Use this command to return to the Exec mode.
exit

Exits the current mode and returns to the parent configuration mode.
Product:

All
Privilege:

Security Administrator, Administrator
Syntax

    exit

Usage:

Use this command to return to the parent configuration mode.