# VLAN-NPU Schema Statistics

The VLAN-NPU schema provides operational statistics that can be used for monitoring and troubleshooting the following products: All
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the VLAN-NPU Schema

Variables | Description | Data Type
--- | --- | ---
slot-no | Description: The slot number of the interface card. Type: Information | Int32
port-no | Description: The port number on an interface card. Type: Information | Int32
vpnname | Description: The name of the VPN associated with the interface. Type: Information | String
vpnid | Description: The identification number of the context configured on the system that is associated with this interface. This is an internal reference number. Type: Information | Int32
interface | Description: Internal number that uniquely identifies an interface. Type: Information | Int32
interfacename | Description: The name assigned to the interface by the user. Type: Information | String
interfacetype | Description: The integer corresponding to the interface type (media) supported by the interface. [0 = Unknown] [1 = Ethernet] [2 = PVC] [3 = Loopback] [4 = Tunnel] Type: Information | Int32
ip-addr | Description: The primary IP address of the interface. Type: Information | String
ip-addr-s1 | Description: The first secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s2 | Description: The second secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s3 | Description: The third secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s4 | Description: The fourth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s5 | Description: The fifth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s6 | Description: The sixth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s7 | Description: The seventh secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s8 | Description: The eight secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s9 | Description: The ninth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s10 | Description: The tenth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s11 | Description: The eleventh secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s12 | Description: The twelfth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s13 | Description: The thirteenth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s14 | Description: The fourteenth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s15 | Description: The fifteenth secondary IP address associated with this slot/port. Type: Information | String
ip-addr-s16 | Description: The sixteenth secondary IP address associated with this slot/port. Type: Information | String
unicast-rx-frames | Description: The total number of received Unicast frames (IPv4 and IPv6). Trigger: Increments whenever a Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
unicast-rx-bytes | Description: The total number of received Unicast bytes (IPv4 and IPv6). Trigger: Increments whenever a Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
unicast-tx-frames | Description: The total number of transmitted Unicast frames (IPv4 and IPv6). Trigger: Increments whenever a Unicast packet is transmitted over an interface Availability: Existing interface Type: Counter | Int64
unicast-tx-bytes | Description: The total number of transmitted Unicast bytes (IPv4 and IPv6). Trigger: Increments whenever a Unicast packet is transmitted over an interface Availability: Existing interface Type: Counter | Int64
multicast-rx-frames | Description: The total number of received Multicast frames (IPv4 and IPv6). Trigger: Increments whenever a Multicast packet is received on an interface Availability: Existing interface Type: Counter | Int64
multicast-rx-bytes | Description: The total number of received Multicast bytes (IPv4 and IPv6). Trigger: Increments whenever a Multicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
multicast-tx-frames | Description: The total number of transmitted Multicast frames (IPv4 and IPv6). Trigger: Increments whenever a Multicast packet is transmitted over an interface Availability: Existing interface Type: Counter | Int64
multicast-tx-bytes | Description: The total number of transmitted Multicast bytes (IPv4 and IPv6). Trigger: Increments whenever a Multicast packet is transmitted over an interface Availability: Existing interface Type: Counter | Int64
broadcast-rx-frames | Description: The total number of received Broadcast frames (IPv4 and IPv6). Trigger: Increments whenever a Broadcast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
broadcast-rx-bytes | Description: The total number of received Broadcast bytes (IPv4 and IPv6). Trigger: Increments whenever a Broadcast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
broadcast-tx-frames | Description: The total number of transmitted Broadcast frames (IPv4 and IPv6). Trigger: Increments whenever a Broadcast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
broadcast-tx-bytes | Description: The total number of transmitted Broadcast bytes (IPv4 and IPv6). Trigger: Increments whenever a Broadcast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ipv4-unicast-rx-frames | Description: The total number of received Unicast frames (IPv4 only). Trigger: Increments whenever an IPv4 Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv4-unicast-rx-bytes | Description: The total number of received Unicast bytes (IPv4 only). Trigger: Increments whenever an IPv4 Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv4-unicast-tx-frames | Description: The total number of transmitted Unicast frames (IPv4 only). Trigger: Increments whenever an IPv4 Unicast packet is transmitted over an interface Availability: Existing interface Type: Counter | Int64
ipv4-unicast-tx-bytes | Description: The total number of transmitted Unicast bytes (IPv4 only). Trigger: Increments whenever an IPv4 Unicast packet is transmitted over an interface Availability: Existing interface Type: Counter | Int64
ipv4-non-unicast-rx-frames | Description: The total number of received non-Unicast frames (IPv4 only). Trigger: Increments whenever an IPv4 non-Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv4-non-unicast-rx-bytes | Description: The total number of received non-Unicast bytes (IPv4 only). Trigger: Increments whenever an IPv4 non-Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv4-non-unicast-tx-frames | Description: The total number of transmitted non-Unicast frames (IPv4 only). Trigger: Increments whenever an IPv4 non-Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ipv4-non-unicast-tx-bytes | Description: The total number of transmitted non-Unicast bytes (IPv4 only). Trigger: Increments whenever an IPv4 non-Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ipv6-unicast-rx-frames | Description: The total number of received Unicast frames (IPv6 only). Trigger: Increments whenever an IPv6 Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv6-unicast-rx-bytes | Description: The total number of received Unicast bytes (IPv6 only). Trigger: Increments whenever an IPv6 Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv6-unicast-tx-frames | Description: The total number of transmitted Unicast frames (IPv6 only). Trigger: Increments whenever an IPv6 Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ipv6-unicast-tx-bytes | Description: The total number of transmitted Unicast bytes (IPv6 only). Trigger: Increments whenever an IPv6 Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ipv6-non-unicast-rx-frames | Description: The total number of received non-Unicast frames (IPv6 only). Trigger: Increments whenever an IPv6 non-Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv6-non-unicast-rx-bytes | Description: The total number of received non-Unicast bytes (IPv6 only). Trigger: Increments whenever an IPv6 non-Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv6-non-unicast-tx-frames | Description: The total number of transmitted non-Unicast frames (IPv6 only). Trigger: Increments whenever an IPv6 non-Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ipv6-non-unicast-tx-bytes | Description: The total number of transmitted non-Unicast bytes (IPv6 only). Trigger: Increments whenever an IPv6 non-Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
fragment-rcvd-rx-frames | Description: The total number of fragments received in frames (IPv4 and IPv6). Trigger: Increments whenever IPv6/IPv4 fragment frames are received over an interface. Availability: Existing interface Type: Counter | Int64
fragment-rcvd-rx-bytes | Description: The total number of fragments received in bytes (IPv4 and IPv6). Trigger: Increments whenever IPv6/IPv4 fragment bytes are received over an interface. Availability: Existing interface Type: Counter | Int64
pkt-reassembled-rx-frames | Description: The total number of received frames with reassembled packets. Trigger: Increments whenever reassembled packets are received on an interface. Availability: Existing interface Type: Counter | Int64
pkt-reassembled-rx-bytes | Description: The total number of received bytes associated with reassembled packets. Trigger: Increments whenever reassembled packets are received on an interface. Availability: Existing interface Type: Counter | Int64
fragment-to-kernel-rx-frames | Description: The total number of received fragment frames handed to the kernel (IPv4 and IPv6). Trigger: Increments whenever fragmented frames are received by the kernel from an interface. Availability: Existing interface Type: Counter | Int64
fragment-to-kernel-rx-bytes | Description: The total number of received fragment bytes handed to the kernel (IPv4 and IPv6). Trigger: Increments whenever fragmented bytes are received by the kernel from an interface. Availability: Existing interface Type: Counter | Int64
hardware-error-rx-frames | Description: The total number of received frames associated with hardware errors. Trigger: Increments whenever a packet associated with a hardware error is received. Availability: Existing interface Type: Counter | Int64
hardware-error-rx-bytes | Description: The total number of received bytes associated with hardware errors. Trigger: Increments whenever a packet associated with a hardware error is received on an interface. Availability: Existing interface Type: Counter | Int64
port-nonoper-rx-frames | Description: The total number of received frames associated with a non-operable port indicator. Trigger: Increments whenever a packet associated with a non-operable port indicator is received on an interface. Availability: Existing interface Type: Counter | Int64
port-nonoper-rx-bytes | Description: The total number of received bytes associated with a non-operable port indicator. Trigger: Increments whenever a packet associated with a non-operable port indicator is received on an interface. Availability: Existing interface Type: Counter | Int64
port-nonoper-tx-frames | Description: The total number of transmitted frames associated with a non-operable port indicator. Trigger: Increments whenever a packet associated with a non-operable port indicator is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
port-nonoper-tx-bytes | Description: The total number of transmitted bytes associated with a non-operable port indicator. Trigger: Increments whenever a packet associated with a non-operable port indicator is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
srcmac-multicast-rx-frames | Description: The total number of frames associated with Multicast packets that include source MAC addresses. Trigger: Increments whenever a Multicast packet containing a source MAC address is received on an interface. Availability: Existing interface Type: Counter | Int64
srcmac-multicast-rx-bytes | Description: The total number of bytes associated with Multicast packets that include source MAC addresses. Trigger: Increments whenever a Multicast packet containing a source MAC address is received on an interface. Availability: Existing interface Type: Counter | Int64
unknown-vlan-tag-rx-frames | Description: The total number of received frames associated with an unknown VLAN tag. Trigger: Increments whenever a packet associated with an unknown VLAN tag is received over an interface. Availability: Existing interface Type: Counter | Int64
unknown-vlan-tag-rx-bytes | Description: The total number of received bytes associated with an unknown VLAN tag. Trigger: Increments whenever a packet associated with an unknown VLAN tag is received over an interface. Availability: Existing interface Type: Counter | Int64
other-protocol-rx-frames | Description: The total number of received frames for non-IP packets. Trigger: Increments whenever a non-IP packet is received on an interface. Availability: Existing interface Type: Counter | Int64
other-protocol-rx-bytes | Description: The total number of received bytes for non-IP packets. Trigger: Increments whenever a non-IP packet is received on an interface. Availability: Existing interface Type: Counter | Int64
not-ipv4-rx-frames | Description: The total number of received non-IPv4 frames. Trigger: Increments whenever a non-IPv4 packet is received on an interface. Availability: Existing interface Type: Counter | Int64
not-ipv4-rx-bytes | Description: The total number of received non-IPv4 bytes. Trigger: Increments whenever a non-IPv4 packet is received on an interface. Availability: Existing interface Type: Counter | Int64
bad-ipv4-hdr-rx-frames | Description: The total number of received frames for packets having bad IPv4 headers. Trigger: Increments whenever a packet containing a bad IPv4 header is received on an interface. Availability: Existing interface Type: Counter | Int64
bad-ipv4-hdr-rx-bytes | Description: The total number of received bytes associated with packets having bad IPv4 headers. Trigger: Increments whenever a packet containing a bad IPv4 header is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv4-mru-excd-rx-frames | Description: The total number of received frames for packets where the IPv4 Maximum Receive Unit (MRU) has been exceeded. Trigger: Increments whenever a packet with a byte count that exceeds the MRU is received on an interface. Availability: Existing interface Type: Counter | Int64
ipv4-mru-excd-rx-bytes | Description: The total number of received bytes for packets where the IPv4 MRU has been exceeded. Trigger: Increments whenever a packet with a byte count that exceeds the MRU is received on an interface. Availability: Existing interface Type: Counter | Int64
tcp-tiny-fragment-rx-frames | Description: The total number of received TCP frames containing tiny fragments. This may be an indication of a fragmentation attack designed to circumvent user-defined filtering rules. Trigger: Increments whenever a TCP packet containing tiny fragments is received on an interface. Availability: Existing interface Type: Counter | Int64
tcp-tiny-fragment-rx-bytes | Description: The total number of received TCP bytes containing tiny fragments. Trigger: Increments whenever a TCP packet containing tiny fragments is received on an interface. Availability: Existing interface Type: Counter | Int64
tcp-tiny-fragment-tx-frames | Description: The total number of transmitted TCP frames containing tiny fragments. Trigger: Increments whenever a TCP packet containing tiny fragments is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
tcp-tiny-fragment-tx-bytes | Description: The total number of transmitted TCP bytes containing tiny fragments. Trigger: Increments whenever a TCP packet containing tiny fragments is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
no-acl-match-rx-frames | Description: The total number of received frames having no Access Control List (ACL) matches. Trigger: Increments whenever a packet that could not be matched via an ACL is received on an interface. Availability: Existing interface Type: Counter | Int64
no-acl-match-rx-bytes | Description: The total number of received bytes having no Access Control List (ACL) matches. Trigger: Increments whenever a packet that could not be matched via an ACL is received on an interface. Availability: Existing interface Type: Counter | Int64
no-acl-match-tx-frames | Description: The total number of transmitted frames having no Access Control List (ACL) matches. Trigger: Increments whenever a packet that could not be matched via an ACL is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
no-acl-match-tx-bytes | Description: The total number of transmitted bytes having no Access Control List (ACL) matches. Trigger: Increments whenever a packet that could not be matched via an ACL is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
acl-filtered-rx-frames | Description: The total number of received frames that have been filtered via an ACL. Trigger: Increments whenever a packet that has been filtered via an ACL is received on an interface. Availability: Existing interface Type: Counter | Int64
acl-filtered-rx-bytes | Description: The total number of received bytes that have been filtered via an ACL. Trigger: Increments whenever a packet that has been filtered via an ACL is received on an interface. Availability: Existing interface Type: Counter | Int64
acl-filtered-tx-frames | Description: The total number of transmitted frames that have been filtered via an ACL. Trigger: Increments whenever a packet that has been filtered via an ACL is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
acl-filtered-tx-bytes | Description: The total number of transmitted bytes that have been filtered via an ACL. Trigger: Increments whenever a packet that has been filtered via an ACL is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ttl-expired-rx-frames | Description: The total number of received frames having an expired Time To Live (TTL). Trigger: Increments whenever a packet having an expired TTL is received on an interface. Availability: Existing interface Type: Counter | Int64
ttl-expired-rx-bytes | Description: The total number of received bytes having an expired Time To Live (TTL). Trigger: Increments whenever a packet having an expired TTL is received on an interface. Availability: Existing interface Type: Counter | Int64
flow-lookup-twice-rx-frames | Description: The number of frames over which flow lookup happened twice (IPv4 and IPv6). Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
flow-lookup-twice-rx-bytes | Description: The number of bytes over which flow lookup happened twice (IPv4 and IPv6). Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
unknown-ipv4-class-rx-frames | Description: The number of received IPv4 frames where the class is “unknown”. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
unknown-ipv4-class-rx-bytes | Description: The number of received IPv4 bytes where the class is “unknown”. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-ip-rx-frames | Description: The number of received IP too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-ip-rx-bytes | Description: The number of received IP too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-icmp-rx-frames | Description: The number of received Internet Control Message Protocol (ICMP) too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-icmp-rx-bytes | Description: The number of received ICMP too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-icmp-tx-frames | Description: The number of transmitted ICMP too short frames. Trigger: Increments when such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-icmp-tx-bytes | Description: The number of transmitted ICMP too short bytes. Trigger: Increments when such bytes are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-igmp-rx-frames | Description: The number of received Internet Group Management Protocol (IGMP) too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-igmp-rx-bytes | Description: The number of received IGMP too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-igmp-tx-frames | Description: The number of transmitted IGMP too short frames. Trigger: Increments when such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-igmp-tx-bytes | Description: The number of transmitted IGMP too short bytes. Trigger: Increments when such bytes are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-tcp-rx-frames | Description: The number of received TCP too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-tcp-rx-bytes | Description: The number of received TCP too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-tcp-tx-frames | Description: The number of transmitted TCP too short frames. Trigger: Increments when such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-tcp-tx-bytes | Description: The number of transmitted TCP too short bytes. Trigger: Increments when such bytes are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-udp-rx-frames | Description: The number of received UDP too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-udp-rx-bytes | Description: The number of received UDP too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-udp-tx-frames | Description: The number of transmitted UDP too short frames. Trigger: Increments when such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-udp-tx-bytes | Description: The number of transmitted UDP too short bytes. Trigger: Increments when such bytes are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
too-short-ipip-rx-frames | Description: The number of received IP-in-IP (IPIP) too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-ipip-rx-bytes | Description: The number of received IPIP too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-gre-rx-frames | Description: The number of received Generic Routing Encapsulation (GRE) too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-gre-rx-bytes | Description: The number of received GRE too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-gre-key-rx-frames | Description: The number of received GRE key too short frames. Trigger: Increments when such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
too-short-gre-key-rx-bytes | Description: The number of received GRE key too short bytes. Trigger: Increments when such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
dont-frag-discard-tx-frames | Description: The number of transmitted frames having the Don't Fragment Discard tag. Trigger: Increments when such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
dont-frag-discard-tx-bytes | Description: The number of transmitted bytes having the Don't Fragment Discard tag. Trigger: Increments when such bytes are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
frag-packets-tx-frames | Description: The number of transmitted frames associated with fragmented packets. Trigger: Increments when such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
frag-packets-tx-bytes | Description: The number of transmitted frames associated with fragmented packets. Trigger: Increments when such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
frag-frags-tx-frames | Description: The number of transmitted fragment frames in fragmented packets. Trigger: Increments whenever such frames are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
frag-frags-tx-bytes | Description: The number of transmitted fragment bytes in fragmented packets. Trigger: Increments whenever such bytes are transmitted over an interface. Availability: Existing interface Type: Counter | Int64
ipv4-vlan-dropped-rx-frames | Description: The number of received IPv4 VLAN dropped frames. Trigger: Increments whenever such frames are received on an interface. Availability: Existing interface Type: Counter | Int64
ipv4-vlan-dropped-rx-bytes | Description: The number of received IPv4 VLAN dropped bytes. Trigger: Increments whenever such bytes are received on an interface. Availability: Existing interface Type: Counter | Int64
ipsec-natt-keepalive-rx-frames | Description: The total number of received frames associated with IPSec Network Address Translation - Traversal (NAT-T) keepalive packets. Trigger: Increments whenever a NAT-T keepalive packet is received on an interface. Availability: Existing interface Type: Counter | Int64
ipsec-natt-keepalive-rx-bytes | Description: The total number of received bytes associated with IPSec NAT-T keepalive packets. Trigger: Increments whenever a NAT-T keepalive packet is received on an interface. Availability: Existing interface Type: Counter | Int64
mpls-flow-not-found-rx-frames | Description: The total number of received frames for MPLS packets with Flow Not Found indicators. Trigger: Increments whenever an MPLS packet with a Flow Not Found indicator is received on an interface. Availability: Existing interface Type: Counter | Int64
mpls-flow-not-found-rx-bytes | Description: The total number of received bytes for MPLS packets with Flow Not Found indicators. Trigger: Increments whenever an MPLS packet with a Flow Not Found indicator is received on an interface. Availability: Existing interface Type: Counter | Int64
mpls-unicast-rx-frames | Description: The total number of received frames for MPLS Unicast packets. Trigger: Increments whenever an MPLS Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
mpls-unicast-rx-bytes | Description: The total number of received bytes for MPLS Unicast packets. Trigger: Increments whenever an MPLS Unicast packet is received on an interface. Availability: Existing interface Type: Counter | Int64
mpls-unicast-tx-frames | Description: The total number of transmitted frames for MPLS Unicast packets. Trigger: Increments whenever an MPLS Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
mpls-unicast-tx-bytes | Description: The total number of transmitted bytes for MPLS Unicast packets. Trigger: Increments whenever an MPLS Unicast packet is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
less-than-17-rx-frames | Description: The total number of frames received for packets containing less than 17 bytes. Trigger: Increments whenever a packet containing less than 17 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
less-than-17-rx-bytes | Description: The total number of bytes received for packets containing less than 17 bytes. Trigger: Increments whenever a packet containing less than 17 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
less-than-17-tx-frames | Description: The total number of frames transmitted for packets containing less than 17 bytes. Trigger: Increments whenever a packet containing less than 17 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
less-than-17-tx-bytes | Description: The total number of bytes transmitted for packets containing less than 17 bytes. Trigger: Increments whenever a packet containing less than 17 bytes is transmitted the interface. Availability: Existing interface Type: Counter | Int64
17-to-64-rx-frames | Description: The total number of frames received for packets containing between 17 and 64 bytes. Trigger: Increments whenever a packet containing between 17 and 64 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
17-to-64-rx-bytes | Description: The total number of bytes received for packets containing between 17 and 64 bytes. Trigger: Increments whenever a packet containing between 17 and 64 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
17-to-64-tx-frames | Description: The total number of frames transmitted for packets containing between 17 and 64 bytes. Trigger: Increments whenever a packet containing between 17 and 64 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
17-to-64-tx-bytes | Description: The total number of bytes transmitted for packets containing between 17 and 64 bytes. Trigger: Increments whenever a packet containing between 17 and 64 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
65-to-127-rx-frames | Description: The total number of frames received for packets containing between 64 and 127 bytes. Trigger: Increments whenever a packet containing between 64 and 127 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
65-to-127-rx-bytes | Description: The total number of bytes received for packets containing between 64 and 127 bytes. Trigger: Increments whenever a packet containing between 64 and 127 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
65-to-127-tx-frames | Description: The total number of frames transmitted for packets containing between 64 and 127 bytes. Trigger: Increments whenever a packet containing between 64 and 127 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
65-to-127-tx-bytes | Description: The total number of bytes transmitted for packets containing between 64 and 127 bytes. Trigger: Increments whenever a packet containing between 64 and 127 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
128-to-255-rx-frames | Description: The total number of frames received for packets containing between 128 and 255 bytes. Trigger: Increments whenever a packet containing between 128 and 255 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
128-to-255-rx-bytes | Description: The total number of bytes received for packets containing between 128 and 255 bytes. Trigger: Increments whenever a packet containing between 128 and 255 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
128-to-255-tx-frames | Description: The total number of frames transmitted for packets containing between 128 and 255 bytes. Trigger: Increments whenever a packet containing between 128 and 255 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
128-to-255-tx-bytes | Description: The total number of bytes transmitted for packets containing between 128 and 255 bytes. Trigger: Increments whenever a packet containing between 128 and 255 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
256-to-511-rx-frames | Description: The total number of frames received for packets containing between 256 and 511 bytes. Trigger: Increments whenever a packet containing between 256 and 511 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
256-to-511-rx-bytes | Description: The total number of bytes received for packets containing between 256 and 511 bytes. Trigger: Increments whenever a packet containing between 256 and 511 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
256-to-511-tx-frames | Description: The total number of frames transmitted for packets containing between 256 and 511 bytes. Trigger: Increments whenever a packet containing between 256 and 511 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
256-to-511-tx-bytes | Description: The total number of bytes transmitted for packets containing between 256 and 511 bytes. Trigger: Increments whenever a packet containing between 256 and 511 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
512-to-1023-rx-frames | Description: The total number of frames received for packets containing between 512 and 1023 bytes. Trigger: Increments whenever a packet containing between 512 and 1023 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
512-to-1023-rx-bytes | Description: The total number of bytes received for packets containing between 512 and 1023 bytes. Trigger: Increments whenever a packet containing between 512 and 1023 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
512-to-1023-tx-frames | Description: The total number of frames transmitted for packets containing between 512 and 1023 bytes. Trigger: Increments whenever a packet containing between 512 and 1023 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
512-to-1023-tx-bytes | Description: The total number of bytes transmitted for packets containing between 512 and 1023 bytes. Trigger: Increments whenever a packet containing between 512 and 1023 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
1024-to-2047-rx-frames | Description: The total number of frames received for packets containing between 1024 and 2047 bytes. Trigger: Increments whenever a packet containing between 1024 and 2047 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
1024-to-2047-rx-bytes | Description: The total number of bytes received for packets containing between 1024 and 2047 bytes. Trigger: Increments whenever a packet containing between 1024 and 2047 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
1024-to-2047-tx-frames | Description: The total number of frames transmitted for packets containing between 1024 and 2047 bytes. Trigger: Increments whenever a packet containing between 1024 and 2047 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
1024-to-2047-tx-bytes | Description: The total number of bytes transmitted for packets containing between 1024 and 2047 bytes. Trigger: Increments whenever a packet containing between 1024 and 2047 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
2048-to-4095-rx-frames | Description: The total number of frames received for packets containing between 2048 and 4095 bytes. Trigger: Increments whenever a packet containing between 2048 and 4095 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
2048-to-4095-rx-bytes | Description: The total number of bytes received for packets containing between 2048 and 4095 bytes. Trigger: Increments whenever a packet containing between 2048 and 4095 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
2048-to-4095-tx-frames | Description: The total number of frames transmitted for packets containing between 2048 and 4095 bytes. Trigger: Increments whenever a packet containing between 2048 and 4095 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
2048-to-4095-tx-bytes | Description: The total number of bytes transmitted for packets containing between 2048 and 4095 bytes. Trigger: Increments whenever a packet containing between 2048 and 4095 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
4096-to-4500-rx-frames | Description: The total number of frames received for packets containing between 4096 and 4500 bytes. Trigger: Increments whenever a packet containing between 4096 and 4500 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
4096-to-4500-rx-bytes | Description: The total number of bytes received for packets containing between 4096 and 4500 bytes. Trigger: Increments whenever a packet containing between 4096 and 4500 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
4096-to-4500-tx-frames | Description: The total number of frames transmitted for packets containing between 4096 and 4500 bytes. Trigger: Increments whenever a packet containing between 2048 and 4095 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
4096-to-4500-tx-bytes | Description: The total number of bytes transmitted for packets containing between 4096 and 4500 bytes. Trigger: Increments whenever a packet containing between 4096 and 4500 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
greater-than-4500-rx-frames | Description: The total number of frames received for packets containing more than 4500 bytes. Trigger: Increments whenever a packet containing more than 4500 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
greater-than-4500-rx-bytes | Description: The total number of bytes received for packets containing more than 4500 bytes. Trigger: Increments whenever a packet containing between 4096 and 4500 bytes is received on an interface. Availability: Existing interface Type: Counter | Int64
greater-than-4500-tx-frames | Description: The total number of frames transmitted for packets containing more than 4500 bytes. Trigger: Increments whenever a packet containing more than 4095 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64
greater-than-4500-tx-bytes | Description: The total number of bytes transmitted for packets containing more than 4500 bytes. Trigger: Increments whenever a packet containing more than 4500 bytes is transmitted over an interface. Availability: Existing interface Type: Counter | Int64