# WEM Changes in Release 14.0

This chapter identifies features and functionality added to, modified for, or deprecated from 14.0 Web Element Manager (WEM) software releases.

Topics covered in this chapter are:

- WEM Feature Changes as of November 7, 2012
- WEM Feature Changes as of September 28, 2012
- WEM Feature Changes as of August 17, 2012
- WEM Feature Changes as of July 31, 2012
- WEM Feature Changes as of June 29, 2012

WEM Feature Changes as of November 7, 2012

This section provides information on WEM feature changes in release 14.0.

IMPORTANT:

Some of the features in this section may also be documented in the WEB Element Manager Installation and Admininstration Guide for this release.

New WEM Features

This section identifies any new WEM features available in release 14.0.

None for this release.

Modified WEM Features

This section identifies WEM features modified in release 14.0 and contains two types of modifications: enhancements and behavior changes. Feature enhancements are modifications based on customer change requests. Feature behavior changes are modifications based on software error corrections (bug fixes) or other code fixes that result in a change in feature behavior.

Feature Enhancements

Change requests have resulted in the following enhancements:

High Availability Configuration Documentation Modification

Previous Behavior: in the “Uninstalling WEM with VCS” section of the WEB Element Manager Installation and Administration Guide, the instructions read:

Offline the WEM Application service resource on active node:

    $ hares -offline <wem application
    resource name> -sys <node1>

    $ hagrp
    -disable <resource group name> -sys <node1>

Modified Behavior: This has been modified to read:

Offline the WEM Application service resource on active node:

    $ hares -offline <wem application
    resource name> -sys <node1>

Behavior Changes Based on Code Modifications

Code changes have resulted in the following enhancements:

P2P Bulkstat Schema Modifications

Previous Behavior: The P2P schema counter selection process was impacting WEM performance.

Modified Behavior: Instead of maintaining five counters for every protocol, there are now only five counters in the P2P schema. To fetch the required information, the Peer-to-Peer protocol names are now used as the filter value in the Bulkstatistics Report Configuration GUI.

The counters are as follows:

- Duration
- Uplink Bytes
- Downlink Bytes
- Uplink Packets
- Downlink Packets

The protocols are subject to change. Currently supported protocols are as follows:

- actsync
- aiminiants
- p2p
- applejuice
- ares
- armagettron
- battlefld
- bittorrent
- blackberry
- callofduty
- citrix
- clubpenguin
- comodounite
- crossfire
- ddlink
- directconnect
- dofus
- ebuddy
- edonkey
- facebook
- facetime
- fasttrack
- feidian
- ficall
- fiesta
- filetopia
- flash
- florensia
- freenet
- fring
- funshion
- gadugadu
- gamekit
- gmail
- gnutella
- goober
- gotomeeting
- gtalk
- gtalk-audio
- gtalk-unclassified
- gtalk-video
- guildwars
- halflife2
- hamachivpn
- iax
- icecast
- imesh
- imo
- implus
- iplayer
- iptv
- irc
- isakmp
- iskoot
- itunes
- jabber
- kakaotalk
- kakaotalk-audio
- kakaotalk-unclassified
- kontiki
- manolito
- maplestory
- meebo
- mgcp
- mig33
- mojo
- msn
- msn-audio
- msn-unclassified
- msn-video
- msrp
- mute
- mypeople
- mypeople-audio
- mypeople-unclassified
- myspace
- nateontalk
- nateontalk-audio
- nateontalk-unclassified
- naverline
- naverline-audio
- naverline-unclassified
- netflix
- netmotion
- nimbuzz
- octoshape
- off
- ogg
- oovoo
- openft
- openvpn
- operamini
- orb
- oscar
- oscar-audio
- oscar-unclassified
- oscar-video
- paltalk
- pando
- pandora
- pcanywhere
- popo
- pplive
- ppstream
- ps3
- qq
- qq-audio
- qq-unclassified
- qq-video
- qqgame
- qqlive
- quake
- quicktime
- rdp
- rdt
- rfactor
- rmstream
- scydo
- secondlife
- shoutcast
- skinny
- skype
- skype-audio
- skype-unclassified
- skype-video
- slingbox
- sopcast
- soulseek
- splashfighter
- spotify
- ssdp
- stealthnet
- steam
- stun
- tango
- tango-audio
- tango-unclassified
- tango-video
- teamspeak
- teamviewer
- thunder
- tor
- truphone
- tunnelvoice
- tvants
- tvuplayer
- twitter
- ultrabac
- usenet
- uusee
- veohtv
- viber
- viber-audio
- viber-unclassified
- vpnx
- vtun
- warcft3
- webex
- whatsapp
- wii
- winmx
- winny
- wmstream
- wofkungfu
- wofwarcraft
- xbox
- xdcc
- yahoo
- yahoo-audio
- yahoo-unclassified
- yahoo-video
- yourfreetunnel
- zattoo

The Online Help has been updated accordingly.

The WEM path is Accounting Menu\View/Graph Bulk Statistics\Bulk Statistics Report Configuration Screen - Counter Selection Tab.

WEM Process Monitoring (WEMPM) Bulkstat Counter Support

Previous Behavior: Online Help support was not available for the WEMPM bulkstat schema.

Modified Behavior: WEM Online Help has been updated to support the following WEMPM schema counters:
Table 1. WEM Process Monitoring Bulkstat Schema Statistics

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
Accounting Menu/View Graph Bulk Statistics/WEM PM Statistics/Processes | HTTPD Server process ID | httpd-server-pid
HTTPD server process CPU usage (%) | httpd-server-cpu-usage
HTTPD server virtual memory (KB) | httpd-server-virtual-mem
HTTPD server memory usage (%) | httpd-server-memory
HTTPD server start time | httpd-server-start-time
HTTPD server elapsed time | httpd-server-elapsed-time
HTTPD server Number of LWP's | httpd-server-lwps
Database server process ID | db-server-pid
Database server process CPU usage (%) | db-server-cpu-usage
Database server virtual memory (KB) | db-server-virtual-mem
Database Server memory usage (%) | db-server-memory
Database server start time | db-server-start-time
Database server elapsed time | db-server-elapsed-time
Database server Number of LWP's | db-server-lwps
WEM Server process ID | wem-server-pid
WEM Server process CPU usage (%) | wem-server-cpu-usage
WEM Server process virtual memory usage (KB | wem-server-virtual-mem
WEM Server Process memory usage (%) | wem-server-memory
WEM Server start time | wem-server-start-time
WEM Server Elapsed time | wem-server-elapsed-time
WEM server Number of LWP's | wem-server-lwps
Script server process ID | script-server-pid
Script server process CPU usage (%) | script-server-cpu-usage
Script server virtual memory (KB | script-server-virtual-mem
Script server memory usage (%) | script-server-memory
Script server start time | script-server-start-time
Script server elapsed time | script-server-elapsed-time
Script server Number of LWP's | script-server-lwps
Bulkstat server process ID | bsserver-server-pid
Bulkstat server process CPU usage (%) | bsserver-server-cpu-usage
Bulkstat server virtual memory (KB) | bsserver-server-virtual-mem
Bulkstat server memory usage (%) | bsserver-server-memory
Bulkstat server start time | bsserver-server-start-time
Bulkstat server elapsed time | bsserver-server-elapsed-time
Bulkstat server Number of LWP's | bsserver-server-lwps
Bulkstat parser process ID | bsparser-server-pid
Bulkstat parser process CPU usage (%) | bsparser-server-cpu-usage
Bulkstat parser virtual memory (KB | bsparser-server-virtual-mem
Bulkstat parser memory usage (%) | bsparser-server-memory
Bulkstat parser start time | bsparser-server-start-time
Bulkstat parser elapsed time | bsparser-server-elapsed-time
Bulkstat parser Number of LWP's | bsparser-server-lwps
NorthBound server process ID | nb-server-pid
NorthBound Server process CPU usage (%) | nb-server-cpu-usage
NorthBound Server virtual memory (KB | nb-server-virtual-mem
NorthBound Server memory usage (%) | nb-server-memory
NorthBound Server start time | nb-server-start-time
NorthBound server elapsed time | nb-server-elapsed-time
NorthBound server Number of LWP's | nb-server-lwps
Notification Service process ID | notif-service-pid
Notification Service process CPU usage (%) | notif-service-cpu-usage
Notification Service virtual memory (KB | notif-service-virtual-mem
Notification Service memory usage (%) | notif-service-memory
Notification Service start time | notif-service-start-time
Notification Service elapsed time | notif-service-elapsed-time
Notification Service Number of LWP's | notif-service-lwps
Accounting Menu/View Graph Bulk Statistics/WEM PM Statistics/Utilization | Total CPU usage on system (%) | sys-total-cpu
Total Swap usage of System (%) | sys-swap-usage
Accounting Menu/View Graph Bulk Statistics/WEM PM Statistics/Disk Usage | Device Name | server-devicename
Mount Point | server-mountpoint
Total number of block allocated (KB | server-totblk
Total number of block available (KB) | server-totavailableblk
WEM server number of block allocated (KB) | wem-server-blkallocated
WEM directory disk usage (%) | wem-disk-usage
DB server number of block allocated (KB) | db-server-blkallocated
Database directory Disk usage (%) | db-disk-usage
FTP server number of block allocated (KB) | ftp-server-blkallocated
FTP directory disk usage (%) | ftp-disk-usage
BS archive number of block allocated (KB) | bs-archive-blkallocated
Bulkstat archive Disk usage (%) | bs-archive-disk-usage
CF DB server number of block allocated (KB) | cfdb-server-blkallocated
Content filtering disk usage (%) | cf-disk-usage
Free disk space (%) | free-disk

The WEM Online Help path is 1. Accounting Menu\View Graph Bulk Statistics\Dialog Boxes\WEMPM_Schema_Statistics

Online Help Modifications

Previous Behavior: In the WEM Online Help system, there was no support for PROFAPP bulkstat counters; the Accounting Menu\View and/or Graph Bulk Statistics\Dialog Boxes\Bulk Statistics Report Configuration Dialog Box - Plot Parameters Tab page was outdated and not hyperlinked to the appropriate schema page, and the individual schema pages were found to be inconsistent in appearance.
Modified Behavior: A new help page was added for PROFAPP counters. The WEM Help path is: Accounting Menu\View and/or Graph Bulk Statistics\Dialog Boxes\PROFAPP Schema Statistics.

IMPORTANT:

PROFAPP counters, along with other SSC counters for SHAPP and ENAPP, are fully documented in the Cisco ASR 5000 Series Subscriber Service Controller Installation and Administration Guide.

The Bulk Statistics Report Configuration Dialog Box - Select Counters & Filter Parameters Tab has been updated to include all schemas, and hyperlinks to the schema pages are now provided. The WEM Help path is Accounting Menu\View and/or Graph Bulk Statistics\Dialog Boxes\Bulk Statistics Report Configuration Dialog Box - Plot Parameters Tab

All bulkstat schema pages have been standardized based on the content found in the xml files in the server/bsschema directory. WEM Help path is Accounting Menu\View and/or Graph Bulk Statistics\Dialog Boxes\<Schema name>.

WEM Feature Changes as of September 28, 2012

This section provides information on WEM feature changes in release 14.0.

IMPORTANT:

Some of the features in this section may also be documented in the WEB Element Manager Installation and Admininstration Guide for this release.

New WEM Features

This section identifies any new WEM features available in release 14.0.

None for this release.

Modified WEM Features

This section identifies WEM features modified in release 14.0 and contains two types of modifications: enhancements and behavior changes. Feature enhancements are modifications based on customer change requests. Feature behavior changes are modifications based on software error corrections (bug fixes) or other code fixes that result in a change in feature behavior.

Feature Enhancements

Change requests have resulted in the following enhancements:

Add User Screen Enhancements

Previous Behavior:Admins had to create new users without the benefit of any default options in the Add User screen.

Modified Behavior: Two new enhancements have been made for this release that support default options in the Add User screen.

1. A Default Map combo box has been added which is populated with all the topology maps that have been created by logged-in users. The topology map is the default view when a user opens WEM, so this combo box allows the Admin to select the appropriate map when creating a new user. If the default map for a user is changed in the Modify User screen, the new entry is added to the map table for that particular user.
2. This enhancement also adds a new section to the dialog box so the Admin can create a default profile for each user type - Inspector, Operator, Config Administrator or Security Administrator - and save the profile. When a new user is added, the Admin can load a profile based on the user’s privilege level and the appropriate fields are populated based on the defaults set for that user privilege.

All fields can be saved as part of a profile with the exception of Context Name, IMG List User ID and Password. The profile enhancement is not supported on the Modify User screen.

The Online Help has been updated to support these changes.

WEM path is Security Menu\User Administration\Add User - General Tab

Customized E-Mail Enhancement

Previous Behavior: Admins were not able to send emails to individual users.

Modified Behavior: A new button marked Email has been added to the User Administration screen so the WEM Admin is now able to send custom notifications to the user community at large, including attachments.

WEM path is Security Menu\User Administration Screen - WEM Users Tab

Bulk Statistics Configuration Screen Enhancements

Previous Behavior: Configured schemas were not easily identified apart from unconfigured schemas. They tended to become harder to identify as more schemas were configured.

Modified Behavior: The Bulk Statistics Configuration - Schema Tab is now divided into two tables. The upper table lists the available bulk statistics schemas on the selected network element (NE). Available schema types vary depending on the type of network services enabled and configured on a given chassis.

Schemas are added to the lower table, in the Configured Schemas panel, as they are configured, and the schema is deleted from the list of available schemas in the upper table.

The Online Help has been updated to support these changes.

WEM help path is Accounting Menu\Bulk Statistics Configuration - Schema Tab

WEM GUI Screens ID Enhancements

Previous Behavior: Users had to type in a WEM screen identifier at the start of each logon session to identify a particular WEM among multiple WEM GUI screens.

Modified Behavior: Now the Admin can identify a WEM at installation time in much the same way as a Hostname. The text is saved as a parameter in img.html and imgdebug.html files. If the flag value for imgdebug.html is set to True, then the WEM Identifier text field is automatically populated at login time. The flag is set to False by default.

WEM path to enable flag values is \users\ems\client\imgdebug.html and \users\ems\client\img.html

Update User Privilege Enhancement

Previous Behavior: Admins could only change a user’s access privilege by deleting and recreating the user.

Modified Behavior: Select the appropriate privilege level from the drop-down box on the Modify User screen.

The Online Help has been updated to support this change.

WEM path is Security Menu\User Administration Screen - Modify User

P2P Voice Bulkstat Counters Enhancement

Previous Behavior: A number of P2P voice counters were unsupported after an upgrade from 12.0.

Modified Behavior: The counters are now supported, but “voice” in the original counters has been changed to “audio” in the following list:

- p2p-skype-audio-duration
- p2p-msn-audio-duration
- p2p-oscar-audio-duration
- p2p-gtalk-audio-duration
- p2p-yahoo-audio-duration

Inspector-Level SNMP Privilege Enhancement

Previous Behavior: Users at the Inspector level were able to change the SNMP forwarding settings on the WEM side. This did not affect the security integrity on the chassis side.

Modified Behavior: This has been corrected.

WEM path is Security Menu\User Administration Screen - WEM Users Tab

Behavior Changes Based on Code Modifications

Code modifications in this release have resulted in the following changes:

WEM GUI Sub-Menu Default View Modification

Previous Behavior: Generic configuration and exec mode commands screens are used by many users to do configuration and to execute show clis on the chassis.

This has lowered the usage of existing configuration and performance (show cli) screens available in WEM. Many screens from the configuration, performance, system info, and monitor/test menus were out of sync with the current cli.

Modified Behavior: A large number of sub-menus that were visible in WEM prior to version 14.0 for the above menus are not visible by default in versions from 14.0. For 14.0 and later, sub-menus not visible by default can be made visible administratively by means of a flag set in the menu.xml file. This process is described in the “Config File Parameters” chapter in the Web Element Manager Installation and Administration Guide and in the WEM Online Help.

WEM specific screens like Configuration Backup, Software Upgrade etc. are not added in menu.xml and hence they would always be visible.

The following table shows the default sub-menu options that were visible for version 12 and prior and compares them with the visible defaults for Version 14. The intention is to make it easier to transition from versions prior to 14.0.

The Online Help is maintained for full backwards-compatibility.
Table 2. Sub-Menus Visible by Default

Menu | Default Sub-Menus Prior to Version 14.0 | Default Sub-Menus from Version 14.0
--- | --- | ---
System | Front View | Front View
Rear View | Rear View
Hardware Information | Hardware Information
Hardware Inventory | Software Version Information
Hardware Version | CPU Information
Card Diagnostics | Port Information
Card Hardware | Port Utilization
Software Version Information | Support Detail
CPU Information | .
Task Information | .
Port Information | .
Port Utilization | .
Power Information | .
Resource Information | .
Support Detail | .
Configuration | NE Configuration | NE List
System | System
PDSN | Save/Load Configuration
GGSN | Configuration Backup
PDIF | Context Administration
Context Provisioning | Event Logging
Content Filtering | Session/Feature License
IMS | SNMP Configuration
SSL | Software Upgrade
CORBA | Syslog
Save/Load COnfiguration | Clock Configuration
CSS | .
UDR/EDR | .
Configuration Backup | .
Context Administration | .
Event Logging | .
Session/Feature License | .
SNMP Configuration | .
Software Upgrade | .
Syslog | .
Global Configuration | .
QoS NPU | .
NTP Configuration | .
Clock Configuration | .
ROHC Profile Configuration | .
Certificate Configuration | .
Performance | Exec Mode Commands | Exec Mode Commands
PDSN | WEM Server Statistics
GGSN | .
SGSN | .
PDIF | .
PHS | .
SSl | .
Active Charging | .
IMS | .
Content Filtering | .
Port Counters | .
IP Access Group Stats | .
IP Interface Stats | .
IPv6 Interface Summary | .
L2TP Information | .
SNMP Stats | .
Prepaid Stats | .
Subscriber information | .
Update CSCF Subscriber | .
Access Flow Stats | .
ROHC Stats | .
RADIUS | .
PPP | .
QoS NPU | .
Session | .
IP Security | .
Mobile IP | .
WEM Server Statistics | .
SRP | .
WEM Server Stats | .
Subscriber information | .
Monitor/Test | Monitoring Operations | Monitoring Operations
Test Operations | .

Screen Output Modification for “WEM Identifier” Prompt

Previous Behavior:There was no on-screen prompt to enter the WEM Identifier (WEM ID) during installation.

Modified Behavior:The following on-screen text has been added to prompt for a WEM ID:

    Enter WEM Identifier text:

WEM Process Monitoring Bulkstat Counter Support

Previous Behavior: Support was not available for the WEM Process Monitoring bulkstat schema.

Modified Behavior: The following table describes the WEM Process Monitoring bulkstat schema counters.

Online Help support for these counters is to follow in October.
Table 3. WEM Process Monitoring Bulkstat Schema Statistics

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
Accounting Menu/View Graph Bulk Statistics/WEM PM Statistics/Processes | HTTPD Server process ID | httpd-server-pid
HTTPD server process CPU usage (%) | httpd-server-cpu-usage
HTTPD server virtual memory (KB) | httpd-server-virtual-mem
HTTPD server memory usage (%) | httpd-server-memory
HTTPD server start time | httpd-server-start-time
HTTPD server elapsed time | httpd-server-elapsed-time
HTTPD server Number of LWP's | httpd-server-lwps
Database server process ID | db-server-pid
Database server process CPU usage (%) | db-server-cpu-usage
Database server virtual memory (KB) | db-server-virtual-mem
Database Server memory usage (%) | db-server-memory
Database server start time | db-server-start-time
Database server elapsed time | db-server-elapsed-time
Database server Number of LWP's | db-server-lwps
WEM Server process ID | wem-server-pid
WEM Server process CPU usage (%) | wem-server-cpu-usage
WEM Server process virtual memory usage (KB | wem-server-virtual-mem
WEM Server Process memory usage (%) | wem-server-memory
WEM Server start time | wem-server-start-time
WEM Server Elapsed time | wem-server-elapsed-time
WEM server Number of LWP's | wem-server-lwps
Script server process ID | script-server-pid
Script server process CPU usage (%) | script-server-cpu-usage
Script server virtual memory (KB | script-server-virtual-mem
Script server memory usage (%) | script-server-memory
Script server start time | script-server-start-time
Script server elapsed time | script-server-elapsed-time
Script server Number of LWP's | script-server-lwps
Bulkstat server process ID | bsserver-server-pid
Bulkstat server process CPU usage (%) | bsserver-server-cpu-usage
Bulkstat server virtual memory (KB) | bsserver-server-virtual-mem
Bulkstat server memory usage (%) | bsserver-server-memory
Bulkstat server start time | bsserver-server-start-time
Bulkstat server elapsed time | bsserver-server-elapsed-time
Bulkstat server Number of LWP's | bsserver-server-lwps
Bulkstat parser process ID | bsparser-server-pid
Bulkstat parser process CPU usage (%) | bsparser-server-cpu-usage
Bulkstat parser virtual memory (KB | bsparser-server-virtual-mem
Bulkstat parser memory usage (%) | bsparser-server-memory
Bulkstat parser start time | bsparser-server-start-time
Bulkstat parser elapsed time | bsparser-server-elapsed-time
Bulkstat parser Number of LWP's | bsparser-server-lwps
NorthBound server process ID | nb-server-pid
NorthBound Server process CPU usage (%) | nb-server-cpu-usage
NorthBound Server virtual memory (KB | nb-server-virtual-mem
NorthBound Server memory usage (%) | nb-server-memory
NorthBound Server start time | nb-server-start-time
NorthBound server elapsed time | nb-server-elapsed-time
NorthBound server Number of LWP's | nb-server-lwps
Notification Service process ID | notif-service-pid
Notification Service process CPU usage (%) | notif-service-cpu-usage
Notification Service virtual memory (KB | notif-service-virtual-mem
Notification Service memory usage (%) | notif-service-memory
Notification Service start time | notif-service-start-time
Notification Service elapsed time | notif-service-elapsed-time
Notification Service Number of LWP's | notif-service-lwps
Accounting Menu/View Graph Bulk Statistics/WEM PM Statistics/Utilization | Total CPU usage on system (%) | sys-total-cpu
Total Swap usage of System (%) | sys-swap-usage
Accounting Menu/View Graph Bulk Statistics/WEM PM Statistics/Disk Usage | Device Name | server-devicename
Mount Point | server-mountpoint
Total number of block allocated (KB | server-totblk
Total number of block available (KB) | server-totavailableblk
WEM server number of block allocated (KB) | wem-server-blkallocated
WEM directory disk usage (%) | wem-disk-usage
DB server number of block allocated (KB) | db-server-blkallocated
Database directory Disk usage (%) | db-disk-usage
FTP server number of block allocated (KB) | ftp-server-blkallocated
FTP directory disk usage (%) | ftp-disk-usage
BS archive number of block allocated (KB) | bs-archive-blkallocated
Bulkstat archive Disk usage (%) | bs-archive-disk-usage
CF DB server number of block allocated (KB) | cfdb-server-blkallocated
Content filtering disk usage (%) | cf-disk-usage
Free disk space (%) | free-disk

Online Help Support for ASR 5500

Previous Behavior: Certain Online Help screens did not support the ASR 5500 chassis.

Modified Behavior: WEM online help has been updated to support the ASR 5500. The following System Information Menu screens are modified:

- Port Information Dialog Box
- Port Utilization Dialog Box
- CPU Information Dialog Box
- Chassis Front View
- Chassis Rear View

WEM help path is Accounting Menu\[ Port Information\Dialog Box | Port Utilization\Dialog Box | CPU Information\Dialog Box | Front Rear Image Views\Dialog Box ]

Resource Information Online Help Modification

Previous Behavior: The Online Help for the Resource Info dialog box-Session Tab showed “Unknown” when the Help button was pressed.

Modified Behavior: This now shows “HNBGW” instead of “Unknown.”
WEM help path is System Info Menu\Resource Information\Resource Info dialog box-Session Tab

PHS Gateway Online Help Counter Name Modification

Previous Behavior: The counter name Total X1/X2?X6 Data Messages was incorrect for the Online Help.

Modified Behavior: This has been changed to read Total X1/X2 Data Messages

WEM help path is Performance Menu/PHS/PHS Gateway Statistics/Dialog Boxes/PHS Gateway Statistics Dialog Box - General tab.

MAP Online Help Modification

Previous Behavior:

1. The counter map-hlr-reset-rcvd is missing from the Online Help for the MAP Bulkstat Schema Statistics screen.
2. The MAP schema is missing from the Online Help for the Bulkstatistics Configuration screen.

Modified Behavior:

1. Online Help support has been added for counter map-hlr-reset-rcvd. The WEM name is HLR Reset Rx: The total number of HLR reset indicators received by MAP. WEM help path is Accounting Menu\View_Graph Bulk Statistics/Dialog Boxes\MAP Schema Statistics.
2. Online Help support has been added for MAP Bulkstatistics Configuration.

WEM help path is Accounting Menu\Bulk Statistics Configuration\Dialog Boxes\MAP Parameters Dialog Box.

PDSN Subscriber Online Help Modification

Previous Behavior: Online Help was not provided for the PDSN Subscriber Access Flow screen.

Modified Behavior: Online Help support has now been added.

WEM help path is Performance Menu\Subscriber Information\Dialog Boxes\PDSN Dialog Boxes\PDSN Subscriber Information Dialog Box - Access Flows Tab.

HSGW Online Help Modification

Previous Behavior: Online Help was not provided for the HSGW Bulkstat Configuration screen.

Modified Behavior: Online Help support has now been added.

WEM help path is Accounting Menu\Bulk Statistics Configuration\Dialog Boxes\HSGW Parameters Dialog Box.

Diameter-Acct/Diameter-Auth Online Help Modification

Previous Behavior: Online Help was not provided for the Diameter-Acct and Diameter-Auth bulkstat configuration screens.

Modified Behavior: Online Help support has now been added.

WEM help path is Accounting Menu\Bulk Statistics Configuration\Dialog Boxes\Diameter-Acct Parameters Dialog Box and Diameter-Auth Parameters Dialog Box.

Diameter-Acct/Diameter-Auth Filter Modification

Previous Behavior: Group was part of the filters list for Diameter-Auth and Diameter-Acct while IP Address and Port were not.

Modified Behavior: Group has been removed from the filters list for Diameter-Auth and Diameter-Acct and IP Address and Port have been added.

WEM Online Help has been updated to reflect these changes.

WEM help path is Accounting Menu\Bulk Statistics Configuration\Diameter-Acct Parameters Dialog Box and Diameter-Auth Parameters Dialog Box.

APN Configuration Online Help Modification

Previous Behavior: Online help was not provided for the ACS Tab for the Add APN Configuration Dialog Box and APN Configuration Dialog Box screens.

Modified Behavior: Online help has been added for the Add APN Configuration Dialog Box - ACS Tab and the APN Configuration Dialog Box - ACS Tab screens.

The Online Help page for the Add APN Configuration Dialog Box has been updated. No change is required for the Modify APN Configuration Dialog Box help page.

WEM help path is Configuration Menu\GGSN Submenu\APN\Dialog Boxes\[ Add APN Configuration Dialog Box | Add APN Configuration Dialog Box - ACS Tab | APN Configuration Dialog Box - ACS Tab ].

WEM Feature Changes as of August 17, 2012

This section provides information on WEM feature changes in release 14.0.

IMPORTANT:

Some of the features in this section may also be documented in the WEB Element Manager Installation and Admininstration Guide for this release.

New WEM Features

This section identifies new WEM features available in release 14.0.

None for this release

Modified WEM Features

This section identifies WEM features modified in release 14.0 and contains two types of modifications: enhancements and behavior changes. Feature enhancements are modifications based on customer change requests. Feature behavior changes are modifications based on software error corrections (bug fixes) or other code fixes that result in a change in feature behavior.

Feature Enhancements

Change requests have resulted in the following enhancements:

Saved Bulk Statistics Reports Enhancement

WEM has the capacity to save multiple report configurations. Previously these reports were not saved in any particular order making it difficult to manage large numbers of configurations. With this enhancement, reports are now saved alphabetically.

WEM path is Accounting Menu\View Graph Bulk Statistics\Select Counters and Filter Parameters tab.

Behavior Changes Based on Code Modifications

Code modifications in this release have resulted in the following changes:

New System Schema Counters

The following table describes the new System schema coounters. These same counters are also described in the WEM Help system.
Table 4. System Schema Bulkstats

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
System Schema\CC Message Error Statistics | Permanent Failures | cc-msgerr-permfailure
Transient Failures | cc-msgerr-transfailure
System Schema\CCA Result Code 2xxx Stats | Result Code 2001 | cca-2001-rc
Result Code 2002 | cca-2002-rc
System Schema\CCA Result Code 4xxx Stats | Result Code 4001 | cca-4001-rc
Result Code 4002 | cca-4002-rc
Result Code 4011 | cca-4011-rc
Result Code 4012 | cca-4012-rc
System Schema\CCA Result Code 5xxx Stats | Result Code 5001 | cca-5001-rc
Result Code 5002 | cca-5002-rc
Result Code 5003 | cca-5003-rc
Result Code 5004 | cca-5004-rc
Result Code 5005 | cca-5005-rc
Result Code 5006 | cca-5006-rc
All Other Result Codes | cca-other-rc
System Schema\Session Disconnect Reasons | sgsn-pgw-init-deact | disc-reason-493
s6b-ip-validation-failed | disc-reason-494
sgsn-failure-rsp-from-sgw | disc-reason-495
tcp-remote-close | disc-reason-496
tcp-reset-received | disc-reason-497
tcp-socket-error | disc-reason-498
sgsn-ptmsi-crunch | disc-reason-499
3Gto4G-context-replacement | disc-reason-500
4Gto3G-context-replacement | disc-reason-501
mme-isr-sgsn-init-detach | disc-reason-502
sgsn-isr-addl-ptmsi-rai | disc-reason-503
sgsn-sgw-dbr-cause-isr-deact | disc-reason-504
sgsn-isr-mme-init-detach | disc-reason-505
mme-sgw-dbr-cause-isr-deact | disc-reason-506
ptmsi-signature-mismatch | disc-reason-507
camel-invalid-configuration | disc-reason-508
mme-no-eps-bearers-activated | disc-reason-509
System Schema\Number of Active Sessions | IPSG | ipsg-activedata
SAEGW | saegw-activedata
System Schema\Connection Statistics | CDMA EVDORA Total Calls Arrived | sess-num-calls-arrived-evdora
CDMA EVDORA Total Calls Disconnected | sess-num-calls-disconnected-evdora
CDMA EVDORA Total Sessions | sess-total-sessions-evdora
System Schema\IKEv2 Detail Statistics | Total IKEv2 CHILD_SA Delete Payload Multiple SPI Received | ikev2-csa-delmultspircv

WEM Performance Requirements

WEM will now support a maximum of 100 chassis for bulkstats reporting and 100 simultaneous web clients. Refer to the Overview chapter in the Cisco Web Element Manager Installation and Administration Guide.

Enhancement to WEM Help System for Process Management Screens

Online Help has been added for a new Historical Statistics tab to the WEM Process Monitoring Screen.

The WEM Help path is Monitor\Test Menu\Monitoring Operations Submenu\WEM Process Monitoring\Dialog Boxes\WEM Process Monitoring Dialog Box - Historical Statistics Tab.

Users can graph these historical statistics locally using the Accounting\View Graph Bulk StatisticsDialog Boxes\Bulk Statistics Report Configuration Dialog Box page and selecting the new option WEM PM from the Subsystem dropdown box. Then continue configuring the report as normal.

System Bulkstat Counter Data-Type Changes

The following System bulkstat counters have had their Data-Type value changed from Int32 to Int64:

- cc-badans-auth-appid
- cc-badans-sessid
- cc-badans-cc-req-num
- cc-badans-cc-req-type
- cc-badans-origin-host
- cc-badans-origin-realm
- cc-badans-parsemsg-err
- cc-badans-parsemscc-err
- cc-badans-misc-err

Mobility Unified Reporting System (MUR) Support in WEM Help System

Support has been provided to configure MUR as a Network Element (System Device) through the Configuration Menu\NE List options in WEM. MUR alarms can be forwarded to and displayed in WEM GUI screens through the Alarm Management and Monitor\Test menus. Various pages have now been updated in the WEM Help system as follows:

Menu Path | Page Title
--- | ---
Configuration Menu\NE List\Procedures | Procedure: Adding a Network Element (System Device) Modifying a Network Element (System Device)
Configuration Menu\NE List\Dialog Boxes | NE List Dialog Box NE List Dialog Box - SSC/MUR Tab Add NE Dialog Box Add NE Dialog Box - SSC/MUR Tab Modify NE Dialog Box Modify NE Dialog Box - SSC/MUR Tab
Alarm Management Menu\Current Alarm View\Dialog Boxes | Current Alarm View Set Alarm Filter Configuration Dialog Box Set Alarm Forwarding Filter Dialog Box
Alarm Management Menu\Pending Alarm Menu\Dialog Boxes | Pending Alarm View Window
Alarm management Menu\Historical Alarm View\Dialog Boxes | Set Historical Alarm Filter - Alarm Database Dialog Box
Monitor Test Menu\Monitoring Operations Submenu\EMS Server Process Monitoring\Dialog Boxes | WEM Process Monitoring Dialog Box

New SGS Schema Counters

The following table describes the new SGS schema counters. These same counters are also described in the WEM Help system.

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
SGS/SGS-AP Statistics/Paging Request | Tx | pag-req-tx
ReTx | pag-req-retx
Rx | pag-req-rx
SGS/SGS-AP Statistics/Paging Reject | Tx | pag-rej-tx
ReTx | pag-rej-retx
Rx | pag-rej-rx
SGS/SGS-AP Statistics/Service Request | Tx | service-req-tx
ReTx | service-req-retx
Rx | service-req-rx
SGS/SGS-AP Statistics/Downlink Unitdata | Tx | dl-ud-tx
ReTx | dl-ud-retx
Rx | dl-ud-rx
SGS/SGS-AP Statistics/Uplink Unitdata | Tx | ul-ud-tx
ReTx | ul-ud-retx
Rx | ul-ud-rx
SGS/SGS-AP Statistics/Location Update Request | Tx | localupd-req-tx
ReTx | localupd-req-retx
Rx | localupd-req-rx
SGS/SGS-AP Statistics/Location Update Accept | Tx | localupd-accept-tx
ReTx | localupd-accept-retx
Rx | localupd-accept-rx
SGS/SGS-AP Statistics/Location Update Reject | Tx | localupd-rej-tx
ReTx | localupd-rej-retx
Rx | localupd-rej-rx
SGS/SGS-AP Statistics/TMSI Reallocation Complete | Tx | tmsi-reloc-tx
ReTx | tmsi-reloc-retx
Rx | tmsi-reloc-rx
SGS/SGS-AP Statistics/Alert Request | Tx | alert-req-tx
ReTx | alert-req-retx
Rx | alert-req-rx
SGS/SGS-AP Statistics/Alert Ack | Tx | alert-ack-tx
ReTx | alert-ack-retx
Rx | alert-ack-rx
SGS/SGS-AP Statistics/Alert Reject | Tx | alert-rej-tx
ReTx | alert-rej-retx
Rx | alert-rej-rx
SGS/SGS-AP Statistics/UE Activity Indication | Tx | ue-actind-tx
ReTx | ue-actind-retx
Rx | ue-actind-rx
SGS/SGS-AP Statistics/EPS Detach Indication | Tx | eps-detind-tx
ReTx | eps-detind-retx
Rx | eps-detind-rx
SGS/SGS-AP Statistics/EPS Detach Ack | Tx | eps-detack-tx
ReTx | eps-detack-retx
Rx | eps-detack-rx
SGS/SGS-AP Statistics/IMSI Detach Indication | Tx | imsi-detind-tx
ReTx | imsi-detind-retx
Rx | imsi-detind-rx
SGS/SGS-AP Statistics/IMSI Detach Ack | Tx | imsi-detack-tx
ReTx | imsi-detack-retx
Rx | imsi-detack-rx
SGS/SGS-AP Statistics/Reset Indication | Tx | reset-ind-tx
ReTx | reset-ind-retx
Rx | reset-ind-rx
SGS/SGS-AP Statistics/Reset Ack | Tx | reset-ack-tx
ReTx | reset-ack-retx
Rx | reset-ack-rx
SGS/SGS-AP Statistics/MM Information Request | Tx | mm-inforeq-tx
ReTx | mm-inforeq-retx
Rx | mm-inforeq-rx
SGS/SGS-AP Statistics/Release Request | Tx | rel-req-tx
ReTx | rel-req-retx
Rx | rel-req-rx
SGS/SGS-AP Statistics/Status | Tx | status-tx
ReTx | status-retx
Rx | status-rx
SGS/SGS-AP Statistics/UE Unreachable | Tx | ue-unreach-tx
ReTx | ue-unreach-retx
Rx | ue-unreach-rx
SGS/SGS-AP Statistics/Unknown MSG | Tx | unk-msg-tx
ReTx | unk-msg-retx
Rx | unk-msg-rx

New ASNGW Schema Counters

The following table describes the new ASNGW schema counters. These same counters are also described in the WEM Help system.

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
ASNGW Schema Statistics/R6 Capability Ack Msg | Total Sent | r6capabilityack-totsent
Retransmissions Sent | r6capabilityack-retranssent
Total Send Failures | r6capabilityack-totsendfail
Total Received | r6capabilityack-totrec
Total Accepted | r6capabilityack-totacc
Total Relayed | r6capabilityack-totrelay
Total Denied | r6capabilityack-totdenied
Total Discarded | r6capabilityack-totdiscard
Badly Formed | r6capabilityack-badform
Decode Error | r6capabilityack-decodeerr
Unspecified Error | r6capabilityack-unspecerr
Missing Mandatory TLV | r6capabilityack-missmandtlv
TLV Value Invalid | r6capabilityack-tlvvalinval
Unknown TLV | r6capabilityack-unknowntlv
Duplicate TLV Found | r6capabilityack-duptlvfound
No Session Found | r6capabilityack-nosessfound
Admin Prohibited | r6capabilityack-admprohibit
No Resource Drops | r6capabilityack-noresourcedrop
Transaction Id. Error | r6capabilityack-transiderr

WEM Feature Changes as of July 31, 2012

This section provides information on WEM feature changes in release 14.0.

IMPORTANT:

Some of the features in this section may also be documented in the WEB Element Manager Installation and Admininstration Guide for this release.

New WEM Features

None for this release.

Modified WEM Features

This section identifies WEM features modified in release 14.0 and contains two types of modifications: enhancements and behavior changes. Feature enhancements are modifications based on customer change requests. Feature behavior changes are modifications based on software error corrections (bug fixes) or other code fixes that result in a change in feature behavior.

Enhancements

The following enhancements are supported in this release:

Enhancement to PS/CS Filtering

Previously, Packet-Switched and Circuit-Switched counters were fetched and displayed filtered only on a per-network basis.

A new key variable, dest-pt-code, provides a new option to filter reports based on the Destination Point Code (DPC) of an MSC in the core network connected with a specific HNB-GW. Dest-pt-code has been added to the following bulkstat schemas: cs-network-rtp, cs-nw-ranap, cs-nw-sccp, ps-nw-ranap, ps-nw-sccp and ps-nw-gtpu.

The WEM path to the Bulk Statistics Report Configuration screen is Accounting Menu/View Graph Bulk Statistics/Dialog Boxes/Bulk Statistics Report Configuration Dialog Box - Select Counters Tab.

Enhancement to Blacklisting

This enhancement supports North American Blacklisting requirements by adding support for the IWF database to the existing support for the NCMEC database. One or both can be enabled and configured as required.

The following instructions can be used regardless of whether the installation is done via the GUI or the Console. Refer to the relevant section in the Installing the WEM Software chapter in the WEM Installation and Configuration Guide for further information.
Table 5. Content Filtering/Blacklisting Configuration Parameters

CFEMS Server Configuration
Content Filtering / Blacklisting Configuration
Enable Content Filtering | Content Filtering is enabled by default | Enabled
Enable Blacklisting | Blacklisting is enabled by default. For North American installations, support is required for both the IWF and NCMEC blacklisting databases. Users can enable blacklisting for one or both databases at prompts during the installation regardless of whether you use the GUI or the command line for the installation. | Enabled
Blacklisting Configuration
NCMEC Database Configuration:
URL | Enter the cumulative.csv file path at NCMEC. | Null
User Name | Enter the username required for authentication at the NCMEC site. | Null
Password | Enter the password required for authentication at the NCMEC site. | Null
Import interval(Hrs) | Enter the cumulative.csv file import interval in hours. | 24
Export to CDP interval(Hrs) | Enter the time interval in hours for Content Filtering Server to export OPTCMDB-BL to CDP. The range is from1 to 5 hours. | 2
IWF Database Configuration:
IWF Database Import Path | Provide the path for the IWF database. | Null
Import Interval | Enter the import interval in hours | 24
Master Content Rating Database (MCRDBS):
MCRDBS Host Name | Enter the host name for an MCRDBS server in the field provided. | Null
MCRDBS Host IP Address | Enter the host IP address of the MCRDBS to which Content Filtering server statistics files are to be sent. | Null
MCRDBS User Name | Enter a username for the MCRDBS in the field provided. | Null
MCRDBS Password | Enter a password for the MCRDBS user in the field provided. The password is case sensitive. | Null
Full Database Import Interval(Hrs) | Enter the time interval in hours for Content Filtering Server to import various databases from MCRDBS (Databases: SFMDB). The range is from 2 to 4320 hours. | 24
Full Database Import Path | Enter the path to locate the SFMDB files in MCRDBS. For example: <Mcrdbs server path>/cfems/<cfems ip address>/sfmdb | Null
Incremental Database Import Interval(Hrs) | Enter the time interval in hours for Content Filtering Server to import various databases from MCRDBS (Databases: SFMDB-INC). The range is from 2 to 720 hours. | 24
Incremental Database Import Path | Enter the path to locate the SFMDB-INC files in MCRDBS. For example: <MCRDBS server path>/cfems/<cfems ip address>/sfmincdb | Null
Full Database Backup Limit (number) | Enter the backup limit for full databases. | 4
Incremental Database Backup Limit (Days) | Enter the backup limit in days for incremental databases. | 30
Archive Database Files | Select 1 if you want to archive the database files. | 1

PS-NW-GTPU Bulkstat Schema

This is a new schema created to support the PS/CS filter enhancement. The following table describes the new counters. These same counters are also described in the WEM Help system.
Table 6. PS-NW-GTPU Bulkstat Schema Statistics

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
Accounting Menu/Bulkstatistics Configuration/Vew Graph Bulk Statistics/PS NW GTPU | GTPU Packet Rx | gtpu-pkt-rx
GTPU Packet Tx | gtpu-pkt-tx
GTPU Bytes Rx | gtpu-bytes-rx
GTPU Bytes Tx | gtpu-bytes-tx

PS-NW-SCCP Bulkstat Schema

This is a new schema created to support the PS/CS filter enhancement. The following table describes the new counters. These same counters are also described in the WEM Help system.
Table 7. PS-NW-SCCP Bulkstat Schema Statistics

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
Accounting Menu/Bulkstatistics Configuration/Vew Graph Bulk Statistics/PS NW SCCP | SCCP Connection Request Rx | sccp-conn-req-rx
SCCP Connection Request Tx | sccp-conn-req-tx
SCCP Connection Confirm Rx | sccp-conn-cfm-rx
SCCP Connection Confirm Tx | sccp-conn-cfm-tx
SCCP Connection Reject Rx | sccp-conn-rej-rx
SCCP Connection Reject Tx | sccp-conn-rej-tx
SCCP Connection Data Rx | sccp-con-data-rx
SCCP Connection Data Tx | sccp-con-data-tx
SCCP Disconnect Rx | sccp-disconnect-rx
SCCP Disconnect Tx | sccp-disconnect-tx
SCCP Uni Data Rx | sccp-uni-data-rx
SCCP Uni Data Tx | sccp-uni-data-tx

CS-NW-SCCP Bulkstat Schema

This is a new schema created to support the PS/CS filter enhancement. The following table describes the new counters. These same counters are also described in the WEM Help system.
Table 8. CS-NW-SCCP Bulkstat Schema Statistics

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
Accounting Menu/Bulkstatistics Configuration/Vew Graph Bulk Statistics/CS NW SCCP | SCCP Connection Request Rx | sccp-conn-req-rx
SCCP Connection Request Tx | sccp-conn-req-tx
SCCP Connection Confirm Rx | sccp-conn-cfm-rx
SCCP Connection Confirm Tx | sccp-conn-cfm-tx
SCCP Connection Reject Rx | sccp-conn-rej-rx
SCCP Connection Reject Tx | sccp-conn-rej-tx
SCCP Connection Data Rx | sccp-con-data-rx
SCCP Connection Data Tx | sccp-con-data-tx
SCCP Disconnect Rx | sccp-disconnect-rx
SCCP Disconnect Tx | sccp-disconnect-tx
SCCP Uni Data Rx | sccp-uni-data-rx
SCCP Uni Data Tx | sccp-uni-data-tx

Behavior Changes Based on Code Modifications

Code modifications in this release have resulted in the following changes:

New CS-NW-RANAP Bulkstat Counter

The following table describes new counters added to the existing cs-nw-ranap bulkstat schema. These same counters are also described in the WEM Help system.
Table 9. CS-NW-RANAP Bulkstat Schema Statistics

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
Accounting Menu/Bulkstatistics Configuration/Vew Graph Bulk Statistics/CS-NW-RANAP Statistics | RAB Time | rab-time

New MVS Schema Counters

The following table describes new counters added to the existing MVS schema. These same counters are also described in the WEM Help system.
Table 10. MVS Bulkstat Schema Counters

Directory Path | WEM Display Name | CLI Display Name
--- | --- | ---
Accounting Menu/Bulkstatistics Configuration/Vew Graph Bulk Statistics/MVS Schema Statistics/Video Analysis Statistics | Total video object count for FLV | ttl-video-flv
Total Video Object Gunzipped | ttl-video-gzipped
Total Video Object Count for MP4 | ttl-video-mp4
Total Video Bytes Received count for Gzip | video-ttl-gzip-rxbytes
Total Video Bytes Transmitted for Gzip | video-ttl-gzip-txbytes

WEM Feature Changes as of June 29, 2012

This section provides information on WEM feature changes in release 14.0.

IMPORTANT:

Some of the features in this section may also be documented in the WEB Element Manager Installation and Admininstration Guide for this release.

New WEM Features

This section identifies new WEM features available in release 14.0.

Support for CISCO ASR 5500

WEM provides monitoring of the ASR 5500 chassis as follows:
Table 11. WEM Support for the ASR 5500

WEM Menu Path | Feature Support
--- | ---
Topology Support
. | A new icon representing the ASR 5500 has been created. Drag the icon to the correct location on the topology map.
Online Help Support
. | Support for the ASR 5500 is being added to the existing Online Help project on an ongoing basis.
System Info Menu
Front View | Opens a stylized chassis front view with the following information: Upper Bezel: Displays the Cisco logo and the legend ASR 5500 Fabric and Storage Cards (FSC) and System Status Cards (SSC) populating slots 11 - 20. LEDs indicate the current status of each card. Hovering over any card also initiates a status popup message.
Rear View | Opens a stylized chassis Rear view with the following information: System Location: Displays the ASR 5500 chassis name. Management I/O (MIO) and Data Processing Cards (DPC) populating slots 1 - 10. LEDs indicate the current status of each card. Hovering over any card also initiates a status popup message.
CPU Information - Graph Button | Opens the Graph Configuration dialog box - Counter Selection tab. Any ASR 5500 cards present are supported in the Categories pane for polling.
Port Information | Opens the Port Information dialog box. A new label IMG Type supports the ASR 5500. The Card Type field supports the MIO card to display MIO port information.
Port Utilization | Opens the Port Utilization dialog box. A new label IMG Type supports the ASR 5500. The Card Type field supports the MIO card to display MIO port utilization.
Port Utilization - Graph Button | Opens the Graph Configuration dialog box - Counter Selection tab. The counter type Average Port Utilization is supported for the MIO.
Monitor/Test Menu
Port Monitoring | Port monitoring is supported for the ASR 5500, but the Port Monitoring menu option is hidden in the default WEM GUI topology for this release. To turn on port monitoring, refer to the section Hide and Unhide Menu Option using the menu.xml File below.
Monitoring Operations - Auto Discovery | Auto-Discovery is supported for the ASR 5500

Mobility Unified Reporting System (MUR) Support in WEM

Previous Behavior: There was no mechanism to forward MUR alarms to WEM for display.

Modified Behavior: MUR can be configured as a Network Element (NE) in WEM and WEM can receive MUR alarms for display. The following menu items have been modified:
Table 12. WEM Support for MUR Alarms

WEM Menu Path | Feature Support
--- | ---
Online Help Support
. | Support is being added to the existing Online Help project on an ongoing basis.
Configuration Menu
NE List: Add Button | The NE Type combo box now includes MUR as a Network Element.
NE List | Shows a list of created NEs. The first tab is always an IMG tab. The second tab can be either SSC or MUR depending on which NE is selected from the list when both are configured.
Alarm Management Menu
Current Alarm View | A radio button has been added to fetch only MUR alarms when selected.
Historical Alarm View\Alarm Database | A radio button has been added to display the MUR(s) in the NE list and the MUR alarm names.
Pending Alarm View | When the NE radio button is selected, “All MUR” and “MUR” can be found in the drop-down list. Selecting “MUR” allows you to select any MUR from the list.

Hide and Unhide Menu Option Using the menu.xml File

Administrators can hide or unhide any menu items to control access for WEM users. This is done by setting the flag in the menu.xml file to hide = Y/N.

This is described with an example in the menu.xml section in the WEM Configuration File appendix in theWEB Element Manager Installation and Admininstration Guide..

Northbound Server Included in Basic WEM License

Formerly available only as a separately licensed feature, Northbound server support is now included in the basic WEM license.

NEBS/Non-Nebs Hardware/Software Support Combinations

Combinations of tested and supported NEBS-compliant and Non-NEBS-compliant servers, operating systems, storage servers, and cluster software are tabled in the WEM Port and Hardware Information chapter of the WEB Element Manager Installation and Admininstration Guide.

Diameter_Auth Bulkstat Schema

Diameter_Auth is a new schema for this release.
Table 13. Diameter_Auth Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
Diameter Auth Statistics | Total DE Requests | der-req-id-sent
Total DE Answers | der-req-aka-chal-sen
DER Retries | der-req-retried
DEA Challenge Received | dea-chal-rcvd
DEA Accept | dea-acpt-rcvd
DEA Timeouts | dea-timeout
DEA Bad Authentication | dea-badauth
DEA Malformed | dea-malformed
DEA Malformed AVP | dea-malformed-avp
DEA Dropped | dea-dropped
RAR | rar-req-rcvd
RAA | raa-ans-accpt-sent
Total AA Requests | aar-req-sent
STR | str-req-sent
STR - Retries | str-req-retried
STA | sta-ans-accpt-rcvd
ASR | asr-req-rcvd
ASA | asa-rsp-accpt-sent
ASA Rej Sent | asa-rsp-rej-sent
REQ Write Error | req-sock-write-err
RSP Write Error | rsp-sock-write-err
Any Read Error | any-sock-read-err
REM Disconnect | rem-disconnect
LOC Disconnect | loc-disconnect

Diameter_Acct Bulkstat Schema

Diameter_Acct is a new schema for this release.
Table 14. Diameter_Acct Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
Diameter Acct Statistics/ | Total AC Requests | req-sent
Total Request Retried | req-retried
Total AC Answers | rsp-rcvd
Request Timeout | req-timeout
Bad Answers | rsp-bad-resp
Malformed | rsp-malformed
ACA-Dropped | rsp-dropped
ACR-Start Present | start-sent
ACR-Stop Present | stop-sent
ACR-Interim Present | interim-sent
ACR-StartRetries | start-retries
ACR-StopRetries | stop-retries
ACA-InterimTimeouts | interim-retries

MVS Bulkstat Schema

MVS is a new schema for this release.
Table 15. MVS Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
MVS Statistics/Video Pacing | Current Flows Paced | currflows-paced
Total Flows Paced | ttlflows-paced
MVS Statistics/TPO | Total Flows Optimized | ttlflows-optimized
Average Goodput (kbps | avrg-goodput
Average Connection Setup Time (msec) | avrg-conn-setup-time-ms
Average Goodput During Congestion Avoidance (kbps) | avrg-goodput-cong-avoid
MVS Statistics/Dynamic Transrating | Average Input Video Bit Rate | ttl-video-transrated
Transrated Sorenson H263 Connections | ttl-transrated-h263-conns
Transrated H264 Connections | ttl-transrated-h264-conns
Average Input Video Bit Rate (kbps | avrg-video-rxbitrate
Average Output Video Bit Rate (kbps) | avrg-video-txbitrate
Average Transrating Reduction (percentage) | avrg-video-rate-reduction
H264 Output Video Bit Rate | video-h264-txbitrate
SH263 Input Video Data Bytes | video-ttl-h263-rxbytes
SH263 Input Video Bit Rate | video-h263-rxbitrate
H264 Input Video Bit Rate | video-h264-rxbitrate
SH263 Output Video Bit Rate | video-h263-txbitrate
SH263 Bit Rate Reduction | h263-bitrate-reduction
H264 Bit Rate Reduction | h264-bitrate-reduction
H264 Input Video Data Bytes | video-ttl-h264-rxbytes
SH263 Output Video Data Bytes | video-ttl-h263-txbytes
H264 Output Video Data Bytes | video-ttl-h264-txbytes
MVS Statistics/TCP Link Monitoring | Average Video RTT (msec) | tcplm-video-avrg-rtt-ms
. | Average RTT (msec) for Video and Non-Video | tcplm-ttl-avrg-rtt-ms
. | Average Video Bit Rate (kbps) | tcplm-video-avrg-rate
. | Average Video and Non-Video Bit Rate (kbps | tcplm-ttl-avrg-rate
. | Number of Average Video RTT less than 50 msec | tcplm-video-rtt-lt-50ms
. | Number of Average Video RTT between 50 and 69 msec | tcplm-video-rtt-50-69ms
. | Number of Average Video RTT between 70 and 89 msec | tcplm-video-rtt-70-89ms
. | Number of Average Video RTT between 90 and 109 msec | tcplm-video-rtt-90-109ms
. | Number of Average Video RTT between 110 and 129 msec | tcplm-video-rtt-110-129ms
. | Number of Average Video RTT between 130 and 149 msec | tcplm-video-rtt-130-149ms
. | Number of Average Video RTT between 150 and 169 msec | tcplm-video-rtt-150-169ms
. | Number of Average Video RTT between 170 and 189 msec | tcplm-video-rtt-170-189ms
. | Number of Average Video RTT between 190 and 209 msec | tcplm-video-rtt-190-209ms
. | Number of Average Video RTT between 210 and 229 msec | tcplm-video-rtt-210-229ms
. | Number of Average Video RTT between 230 and 249 msec | tcplm-video-rtt-230-249ms
. | Number of Average Video RTT greater than or equal 250 msec | tcplm-video-rtt-gteq-250ms
. | Number of Average Video RTT less than 250 msec | tcplm-video-rtt-lt-250ms
. | Number of Average Video RTT between 250 and 289 msec | tcplm-video-rtt-250-289ms
. | Number of Average Video RTT between 290 and 329 msec | tcplm-video-rtt-290-329ms
. | Number of Average Video RTT between 330 and 369 msec | tcplm-video-rtt-330-369ms
. | Number of Average Video RTT between 370 and 409 msec | tcplm-video-rtt-370-409ms
. | Number of Average Video RTT between 410 and 449 msec | tcplm-video-rtt-410-449ms
. | Number of Average Video RTT between 450 and 489 msec | tcplm-video-rtt-450-489ms
. | Number of Average Video RTT between 490 and 529 msec | tcplm-video-rtt-490-529ms
. | Number of Average Video RTT between 530 and 569 msec | tcplm-video-rtt-530-569ms
. | Number of Average Video RTT between 570 and 609 msec | tcplm-video-rtt-570-609ms
. | Number of Average Video RTT between 610 and 649 msec | tcplm-video-rtt-610-649ms
. | Number of Average Video RTT greater than or equal 650 msec | tcplm-video-rtt-gteq-650ms
. | Number of Average Video RTT less than 650 msec | tcplm-video-rtt-lt-650ms
. | Number of Average Video RTT between 650 and 749 msec | tcplm-video-rtt-650-749ms
. | Number of Average Video RTT between 750 and 849 msec | tcplm-video-rtt-750-849ms
. | Number of Average Video RTT between 850 and 949 msec | tcplm-video-rtt-850-949ms
. | Number of Average Video RTT between 950 and 104 msec | tcplm-video-rtt-950-1049ms
. | Number of Average Video RTT between 1050 and 1149 msec | tcplm-video-rtt-1050-1149ms
. | Number of Average Video RTT between 1150 and 1249 msec | tcplm-video-rtt-1150-1249ms
. | Number of Average Video RTT between 1250 and 1349 msec | tcplm-video-rtt-1250-1349ms
. | Number of Average Video RTT between 1350 and 1449 msec | tcplm-video-rtt-1350-1449ms
. | Number of Average Video RTT between 1450 and 1549 msec | tcplm-video-rtt-1450-1549ms
. | Number of Average Video RTT between 1550 and 1649 msec | tcplm-video-rtt-1550-1649ms
. | Number of Average Video RTT greater than or equal 1650 msec | tcplm-video-rtt-gteq-1650ms
. | Number of Average Video and Non-Video RTT less than 50 msec | tcplm-ttl-rtt-lt-50ms
. | Number of Average Video and Non-Video RTT between 50 and 69 msec | tcplm-ttl-rtt-50-69ms
. | Number of Average Video and Non-Video RTT between 70 and 89 msec | tcplm-ttl-rtt-70-89ms
. | Number of Average Video and Non-Video RTT between 90 and 109 msec | tcplm-ttl-rtt-90-109ms
. | Number of Average Video and Non-Video RTT between 110 and 129 msec | tcplm-ttl-rtt-110-129ms
. | Number of Average Video and Non-Video RTT between 130 and 149 msec | tcplm-ttl-rtt-130-149ms
. | Number of Average Video and Non-Video RTT between 150 and 169 msec | tcplm-ttl-rtt-150-169ms
. | Number of Average Video and Non-Video RTT between 170 and 189 msec | tcplm-ttl-rtt-170-189ms
. | Number of Average Video and Non-Video RTT between 190 and 209 msec | tcplm-ttl-rtt-190-209ms
. | Number of Average Video and Non-Video RTT between 210 and 229 msec | tcplm-ttl-rtt-210-229ms
. | Number of Average Video and Non-Video RTT between 230 and 249 msec | tcplm-ttl-rtt-230-249ms
. | Number of Average Video and Non-Video RTT greater than or equal 250 msec | tcplm-ttl-rtt-gteq-250ms
. | Number of Average Video and Non-Video RTT less than 250 msec | tcplm-ttl-rtt-lt-250ms
. | Number of Average Video and Non-Video RTT between 250 and 289 msec | tcplm-ttl-rtt-250-289ms
. | Number of Average Video and Non-Video RTT between 290 and 329 msec | tcplm-ttl-rtt-290-329ms
. | Number of Average Video and Non-Video RTT between 330 and 369 msec | tcplm-ttl-rtt-330-369ms
. | Number of Average Video and Non-Video RTT between 370 and 409 msec | tcplm-ttl-rtt-370-409ms
. | Number of Average Video and Non-Video RTT between 410 and 449 msec | tcplm-ttl-rtt-410-449ms
. | Number of Average Video and Non-Video RTT between 450 and 489 msec | tcplm-ttl-rtt-450-489ms
. | Number of Average Video and Non-Video RTT between 490 and 529 msec | tcplm-ttl-rtt-490-529ms
. | Number of Average Video and Non-Video RTT between 530 and 569 msec | tcplm-ttl-rtt-530-569ms
. | Number of Average Video and Non-Video RTT between 570 and 609 msec | tcplm-ttl-rtt-570-609ms
. | Number of Average Video and Non-Video RTT between 610 and 649 msec | tcplm-ttl-rtt-610-649ms
. | Number of Average Video and Non-Video RTT greater than or equal 650 msec | tcplm-ttl-rtt-gteq-650ms
. | Number of Average Video and Non-Video RTT less than 650 msec | tcplm-ttl-rtt-lt-650ms
. | Number of Average Video and Non-Video RTT between 650 and 749 msec | tcplm-ttl-rtt-650-749ms
. | Number of Average Video and Non-Video RTT between 750 and 849 msec | tcplm-ttl-rtt-750-849ms
. | Number of Average Video and Non-Video RTT between 850 and 949 msec | tcplm-ttl-rtt-850-949ms
. | Number of Average Video and Non-Video RTT between 950 and 1049 | tcplm-ttl-rtt-950-1049ms
. | Number of Average Video and Non-Video RTT between 1050 and 1149 msec | tcplm-ttl-rtt-1050-1149ms
. | Number of Average Video and Non-Video RTT between 1150 and 1249 msec | tcplm-ttl-rtt-1150-1249ms
. | Number of Average Video and Non-Video RTT between 1250 and 1349 msec | tcplm-ttl-rtt-1250-1349ms
. | Number of Average Video and Non-Video RTT between 1350 and 1449 msec | tcplm-ttl-rtt-1350-1449ms
. | Number of Average Video and Non-Video RTT between 1450 and 1549 msec | tcplm-ttl-rtt-1450-1549ms
. | Number of Average Video and Non-Video RTT between 1550 and 1649 msec | tcplm-ttl-rtt-1550-1649ms
. | Number of Average Video and Non-Video RTT greater than or equal 1650 msec | tcplm-ttl-rtt-gteq-1650ms
. | Number of Average Video Rate less than 20 kbps | tcplm-video-rate-lt-20kbps
. | Number of Average Video Rate between 20 and 39 kbps | tcplm-video-rate-20-39kbps
. | Number of Average Video Rate between 40 and 59 kbps | tcplm-video-rate-40-59kbps
. | Number of Average Video Rate between 60 and 79 kbps | tcplm-video-rate-60-79kbps
. | Number of Average Video Rate between 80 and 99 kbps | tcplm-video-rate-80-99kbps
. | Number of Average Video Rate between 100 and 119 kbps | tcplm-video-rate-100-119kbps
. | Number of Average Video Rate between 120 and 139 | tcplm-video-rate-120-139kbps
. | Number of Average Video Rate between 140 and 159 kbps | tcplm-video-rate-140-159kbps
. | Number of Average Video Rate between 160 and 179 kbps | tcplm-video-rate-160-179kbps
. | Number of Average Video Rate between 180 and 199 kbps | tcplm-video-rate-180-199kbps
. | Number of Average Video Rate between 200 and 219 kbps | tcplm-video-rate-200-219kbps
. | Number of Average Video Rate greater than or equal 220 kbps | tcplm-video-rate-gteq-220kbps
. | Number of Average Video Rate less than 220 kbps | tcplm-video-rate-lt-220kbps
. | Number of Average Video Rate between 220 and 259 kbps | tcplm-video-rate-220-259kbps
. | Number of Average Video Rate between 260 and 299 kbps | tcplm-video-rate-260-299kbps
. | Number of Average Video Rate between 300 and 339 kbps | tcplm-video-rate-300-339kbps
. | Number of Average Video Rate between 340 and 379 kbps | tcplm-video-rate-340-379kbps
. | Number of Average Video Rate between 380 and 419 kbps | tcplm-video-rate-380-419kbps
. | Number of Average Video Rate between 420 and 459 kbps | tcplm-video-rate-420-459kbps
. | Number of Average Video Rate between 460 and 499 kbps | tcplm-video-rate-460-499kbps
. | Number of Average Video Rate between 500 and 539 kbps | tcplm-video-rate-500-539kbps
. | Number of Average Video Rate between 540 and 579 kbps | tcplm-video-rate-540-579kbps
. | Number of Average Video Rate between 580 and 619 kbps | tcplm-video-rate-580-619kbps
. | Number of Average Video Rate greater than or equal 620 kbps | tcplm-video-rate-gteq-620kbps
. | Number of Average Video Rate less than 620 kbps | tcplm-video-rate-lt-620kbps
. | Number of Average Video Rate between 620 and 719 kbps | tcplm-video-rate-620-719kbps
. | Number of Average Video Rate between 720 and 819 kbps | tcplm-video-rate-720-819kbps
. | Number of Average Video Rate between 820 and 919 kbps | tcplm-video-rate-820-919kbps
. | Number of Average Video Rate between 920 and 1019 kbps | tcplm-video-rate-920-1019kbps
. | Number of Average Video Rate between 1020 and 1119 kbps | tcplm-video-rate-1020-1119kbps
. | Number of Average Video Rate between 1120 and 1219 kbps | tcplm-video-rate-1120-1219kbps
. | Number of Average Video Rate between 1220 and 1319 kbps | tcplm-video-rate-1220-1319kbps
. | Number of Average Video Rate between 1320 and 1419 kbps | tcplm-video-rate-1320-1419kbps
. | Number of Average Video Rate between 1420 and 1519 kbps | tcplm-video-rate-1420-1519kbps
. | Number of Average Video Rate between 1520 and 1619 kbps | tcplm-video-rate-1520-1619kbps
. | Number of Average Video Rate greater than or equal 1620 kbps | tcplm-video-rate-gteq-1620kbps
. | Number of Average Video and Non-Video Rate less than 20 kbps | tcplm-ttl-rate-lt-20kbps
. | Number of Average Video and Non-Video Rate between 20 and 39 kbps | tcplm-ttl-rate-20-39kbps
. | Number of Average Video and Non-Video Rate between 40 and 59 kbps | tcplm-ttl-rate-40-59kbps
. | Number of Average Video and Non-Video Rate between 60 and 79 kbps | tcplm-ttl-rate-60-79kbps
. | Number of Average Video and Non-Video Rate between 80 and 99 kbps | tcplm-ttl-rate-80-99kbps
. | Number of Average Video and Non-Video Rate between 100 and 119 kbps | tcplm-ttl-rate-100-119kbps
. | Number of Average Video and Non-Video Rate between 120 and 139 kbps | tcplm-ttl-rate-120-139kbps
. | Number of Average Video and Non-Video Rate between 140 and 159 kbps | tcplm-ttl-rate-140-159kbps
. | Number of Average Video and Non-Video Rate between 160 and 179 kbps | tcplm-ttl-rate-160-179kbps
. | Number of Average Video and Non-Video Rate between 180 and 199 kbps | tcplm-ttl-rate-180-199kbps
. | Number of Average Video and Non-Video Rate between 200 and 219 kbps | tcplm-ttl-rate-200-219kbps
. | Number of Average Video and Non-Video Rate greater than or equal 220 kbps | tcplm-ttl-rate-gteq-220kbps
. | Number of Average Video and Non-Video Rate less than 220 kbps | tcplm-ttl-rate-lt-220kbps
. | Number of Average Video and Non-Video Rate between 220 and 259 kbps | tcplm-ttl-rate-220-259kbps
. | Number of Average Video and Non-Video Rate between 260 and 299 kbps | tcplm-ttl-rate-260-299kbps
. | Number of Average Video and Non-Video Rate between 300 and 339 kbps | tcplm-ttl-rate-300-339kbps
. | Number of Average Video and Non-Video Rate between 340 and 379 kbps | tcplm-ttl-rate-340-379kbps
. | Number of Average Video and Non-Video Rate between 380 and 419 kbps | tcplm-ttl-rate-380-419kbps
. | Number of Average Video and Non-Video Rate between 420 and 459 kbps | tcplm-ttl-rate-420-459kbps
. | Number of Average Video and Non-Video Rate between 460 and 499 kbps | tcplm-ttl-rate-460-499kbps
. | Number of Average Video and Non-Video Rate between 500 and 539 kbps | tcplm-ttl-rate-500-539kbps
. | Number of Average Video and Non-Video Rate between 540 and 579 kbps | tcplm-ttl-rate-540-579kbps
. | Number of Average Video and Non-Video Rate between 580 and 619 kbps | tcplm-ttl-rate-580-619kbps
. | Number of Average Video and Non-Video Rate greater than or equal 620 kbps | tcplm-ttl-rate-gteq-620kbps
. | Number of Average Video and Non-Video Rate between 620 and 719 kbps | tcplm-ttl-rate-620-719kbps
. | Number of Average Video and Non-Video Rate between 720 and 819 kbps | tcplm-ttl-rate-720-819kbps
. | Number of Average Video and Non-Video Rate between 820 and 919 kbps | tcplm-ttl-rate-820-919kbps
. | Number of Average Video and Non-Video Rate between 920 and 1019 kbps | tcplm-ttl-rate-920-1019kbps
. | Number of Average Video and Non-Video Rate between 1020 and 1119 kbps | tcplm-ttl-rate-1020-1119kbps
. | Number of Average Video and Non-Video Rate between 1120 and 1219 kbps | tcplm-ttl-rate-1120-1219kbps
. | Number of Average Video and Non-Video Rate between 1220 and 1319 kbps | tcplm-ttl-rate-1220-1319kbps
. | Number of Average Video and Non-Video Rate between 1320 and 1419 kbps | tcplm-ttl-rate-1320-1419kbps
. | Number of Average Video and Non-Video Rate between 1420 and 1519 kbps | tcplm-ttl-rate-1420-1519kbps
. | Number of Average Video and Non-Video Rate between 1520 and 1619 kbps | tcplm-ttl-rate-1520-1619kbps
. | Number of Average Video and Non-Video Rate greater than or equal 1620 kbps | tcplm-ttl-rate-gteq-1620kbps
MVG Statistics/Video Analysis Statistics | Total Video bytes for MP4 container for Iphone/Ipad (iOS) | ttl_vbytes_mp4_ios
. | Total Video bytes for MP4 container for android devices | ttl_vbytes_mp4_android
. | Total Video bytes for MP4 container for laptop | ttl_vbytes_mp4_laptop
. | Total Video bytes for MP4 container for Other devices | ttl_vbytes_mp4_unk_ue
. | Total Video bytes for flash container for Iphone/Ipad (iOS | ttl_vbytes_flv_ios
. | Total Video bytes for MP4 container for androidTotal Video bytes for MP4 container for android | ttl_vbytes_flv_android
. | Total Video bytes for MP4 container for laptopTotal Video bytes for MP4 container for laptop | ttl_vbytes_flv_laptop
. | Total Video bytes for MP4 container for other devicesTotal Video bytes for MP4 container for other devices | ttl_vbytes_flv_unk_ue
. | Total Video bytes for other container for Iphone/Ipad (iOS)Total Video bytes for other container for Iphone/Ipad (iOS | ttl_vbytes_unk_cntnr_ios
. | Total Video bytes for other container for android " columnName="ttl_vbytes_unk_cntnr_android | ttl_vbytes_unk_cntnr_android
. | Total Video bytes for other container for laptop | ttl_vbytes_unk_cntnr_laptop
. | Total Video duration for other container for other devices | ttl_vbytes_unk_cntnr_unk_ue
. | Total Video duration for MP4 container for Iphone/Ipad (iOS | ttl_vduration_mp4_ios
. | Total Video duration for MP4 container for android devices | ttl_vduration_mp4_android
. | Total Video duration for MP4 container for laptop | ttl_vduration_mp4_laptop
. | Total Video duration for MP4 container for Other devices | ttl_vduration_mp4_unk_ue
. | Total Video duration for flash container for Iphone/Ipad (iOS | ttl_vduration_flv_ios
. | Total Video duration for MP4 container for android | ttl_vduration_flv_android
. | Total Video duration for MP4 container for laptop | ttl_vduration_flv_laptop
. | Total Video duration for MP4 container for other devices | ttl_vduration_flv_unk_ue
. | Total Video duration for other container for Iphone/Ipad (iOS | ttl_vduration_unk_cntnr_ios
. | Total Video duration for other container for android | ttl_vduration_unk_cntnr_android
. | Total Video duration for other container for laptop | ttl_vduration_unk_cntnr_laptop
. | Total Video duration for other container for other devicesTotal Video duration for other container for other devices | ttl_vduration_unk_cntnr_unk_ue
. | Total Video bytes for MP4 container for Iphone/Ipad (iOS)" columnName="ttl_txbytes_mp4_ios | ttl_txbytes_mp4_ios
. | Total Video bytes for MP4 container for android devices | ttl_txbytes_mp4_android
. | Total Video bytes for MP4 container for laptop | ttl_txbytes_mp4_laptop
. | Total Video bytes for MP4 container for Other devices | ttl_txbytes_mp4_unk_ue
. | Total Video bytes for flash container for Iphone/Ipad (iOS | ttl_txbytes_flv_ios
. | Total Video bytes for MP4 container for android | ttl_txbytes_flv_android
. | Total Video bytes for MP4 container for laptop | ttl_txbytes_flv_laptop
. | Total Video bytes for MP4 container for other devices | ttl_txbytes_flv_unk_ue
. | Total Video bytes for other container for Iphone/Ipad (iOS | ttl_txbytes_unk_cntnr_ios
. | Total Video bytes for other container for android | ttl_txbytes_unk_cntnr_android
. | Total Video bytes for other container for laptop | ttl_txbytes_unk_cntnr_laptop
. | Total Video bytes for other container for other devices | ttl_txbytes_unk_cntnr_unk_ue
. | Total Videos for MP4 container for Iphone/Ipad (iOS | ttl_video_count_mp4_ios
. | Total Videos for MP4 container for android devices | ttl_video_count_mp4_android
. | Total Videos for MP4 container for laptop | ttl_video_count_mp4_laptop
. | Total Videos for MP4 container for Other devices | ttl_video_count_mp4_unk_ue
. | Total Videos for flash container for Iphone/Ipad (iOS | ttl_video_count_flv_ios
. | Total Videos for MP4 container for android | ttl_video_count_flv_android
. | Total Videos for MP4 container for laptop | ttl_video_count_flv_laptop
. | Total Videos for MP4 container for other devices | ttl_video_count_flv_unk_ue
. | Total Videos for other container for Iphone/Ipad (iOS | ttl_video_count_unk_cntnr_ios
. | Total Videos for other container for android | ttl_video_count_unk_cntnr_android
. | Total Videos for other container for laptop | ttl_video_count_unk_cntnr_laptop
. | Total Videos for other container for other devices | ttl_video_count_unk_cntnr_unk_ue
. | Total video bytes for gprs rat type on Iphone/Ipad (iOS) devices | ttl_vbytes_gprs_ios
. | Total video bytes for gprs rat type on android devices | ttl_vbytes_gprs_android
. | Total video bytes for gprs rat type for laptop devices | ttl_vbytes_gprs_laptop
. | Total video bytes for gprs rat type for any other kind of UE | ttl_vbytes_gprs_unk_ue
. | Total video bytes for umts rat type on ios UE | ttl_vbytes_umts_ios
. | Total video bytes for umts rat type on android UE | ttl_vbytes_umts_android
. | Total video bytes for umts rat type for laptop UE | ttl_vbytes_umts_laptop
. | Total video bytes for umts rat type for any other kind of UE | ttl_vbytes_umts_unk_ue
. | Total video bytes for lte rat type on ios UE | ttl_vbytes_lte_ios
. | Total video bytes for lte rat type on android UE | ttl_vbytes_lte_android
. | Total video bytes for lte rat type for laptop UE | ttl_vbytes_lte_laptop
. | Total video bytes for lte rat type for any other kind of UE | ttl_vbytes_lte_unk_ue
. | Total video bytes for hspa rat type on ios UE | ttl_vbytes_hspa_ios
. | Total video bytes for hspa rat type on android UE | ttl_vbytes_hspa_android
. | Total video bytes for hspa rat type for laptop UE | ttl_vbytes_hspa_laptop
. | Total video bytes for hspa rat type for any other kind of UE | ttl_vbytes_hspa_unk_ue
. | Total video bytes for wlan rat type on ios UE | ttl_vbytes_wlan_ios
. | Total video bytes for wlan rat type on android UE | ttl_vbytes_wlan_android
. | Total video bytes for wlan rat type for laptop UE | ttl_vbytes_wlan_laptop
. | Total video bytes for wlan rat type for any other kind of UE | ttl_vbytes_wlan_unk_ue
. | Total video bytes for cdma rat type on ios UE | ttl_vbytes_cdma_ios
. | Total video bytes for cdma rat type on android UE | ttl_vbytes_cdma_android
. | Total video bytes for cdma rat type for laptop UE | ttl_vbytes_cdma_laptop
. | Total video bytes for cdma rat type for any other kind of UE | ttl_vbytes_cdma_unk_ue
. | Total video bytes for other rat type on ios UE | ttl_vbytes_unk_rat_ios
. | Total video bytes for other rat type on android UE | ttl_vbytes_unk_rat_android
. | Total video bytes for other rat type for laptop UE | ttl_vbytes_unk_rat_laptop
. | Total video bytes for other rat type for any other kind of UE | ttl_vbytes_unk_rat_unk_ue
. | Total video duration for gprs rat type on ios UE | ttl_vduration_gprs_ios
. | Total video duration for gprs rat type on android UE | ttl_vduration_gprs_android
. | Total video duration for gprs rat type on laptop UE | ttl_vduration_gprs_laptop
. | Total video duration for gprs rat type on any other kind of UE | ttl_vduration_gprs_unk_ue
. | Total video duration for umts rat type on ios UE | ttl_vduration_umts_ios
. | Total video duration for umts rat type on android UE | ttl_vduration_umts_android
. | Total video duration for umts rat type on laptop UE | ttl_vduration_umts_laptop
. | Total video duration for umts rat type on any other kind of UE | ttl_vduration_umts_unk_ue
. | Total video duration for lte rat type on ios UE | ttl_vduration_lte_ios
. | Total video duration for lte rat type on android UE | ttl_vduration_lte_android
. | Total video duration for lte rat type on laptop UE | ttl_vduration_lte_laptop
. | Total video duration for lte rat type on any other kind of UE | ttl_vduration_lte_unk_ue
. | Total video duration for hspa rat type on ios UE | ttl_vduration_hspa_ios
. | Total video duration for hspa rat type on android UE | ttl_vduration_hspa_android
. | Total video duration for hspa rat type on laptop UE | ttl_vduration_hspa_laptop
. | Total video duration for hspa rat type on any other kind of UE | ttl_vduration_hspa_unk_ue
. | Total video duration for wlan rat type on ios UE | ttl_vduration_wlan_ios
. | Total video duration for wlan rat type on android UE | ttl_vduration_wlan_android
. | Total video duration for wlan rat type on laptop UE | ttl_vduration_wlan_laptop
. | Total video duration for wlan rat type on any other kind of UE | ttl_vduration_wlan_unk_ue
. | Total video duration for cdma rat type on ios UE" columnName="ttl_vduration_cdma_ios | ttl_vduration_cdma_ios
. | Total video duration for cdma rat type on android UE | ttl_vduration_cdma_android
. | Total video duration for cdma rat type on laptop UE | ttl_vduration_cdma_laptop
. | Total video duration for cdma rat type on any other kind of UE | ttl_vduration_cdma_unk_ue
. | Total video duration for other rat type on ios UE | ttl_vduration_unk_rat_ios
. | Total video duration for other rat type on android UE | ttl_vduration_unk_rat_android
. | Total video duration for other rat type on laptop UE | ttl_vduration_unk_rat_laptop
. | Total video duration for other rat type on any other kind of UE | ttl_vduration_unk_rat_unk_ue
. | Total bytes sent for gprs rat type for ios UE | ttl_txbytes_gprs_ios
. | Total bytes sent for gprs rat type for android UE | ttl_txbytes_gprs_android
. | Total bytes sent for gprs rat type for laptop UE | ttl_txbytes_gprs_laptop
. | Total bytes sent for gprs rat type for any other kind of UE" | ttl_txbytes_gprs_unk_ue
. | Total bytes sent for umts rat type for ios UE | ttl_txbytes_umts_ios
. | Total bytes sent for umts rat type for android UE | ttl_txbytes_umts_android
. | Total bytes sent for umts rat type for laptop UE | ttl_txbytes_umts_laptop
. | Total bytes sent for umts rat type for any other kind of UE | ttl_txbytes_umts_unk_ue
. | Total bytes sent for lte rat type for ios UE | ttl_txbytes_lte_ios
. | Total bytes sent for lte rat type for android UE | ttl_txbytes_lte_android
. | Total bytes sent for lte rat type for laptop UE | ttl_txbytes_lte_laptop
. | Total bytes sent for lte rat type for any other kind of UE | ttl_txbytes_lte_unk_ue
. | Total bytes sent for hspa rat type for ios UE | ttl_txbytes_hspa_ios
. | Total bytes sent for hspa rat type for android UE" | ttl_txbytes_hspa_android
. | Total bytes sent for hspa rat type for laptop UE | ttl_txbytes_hspa_laptop
. | Total bytes sent for hspa rat type for any other kind of UE | ttl_txbytes_hspa_unk_ue
. | Total bytes sent for wlan rat type for ios UE | ttl_txbytes_wlan_ios
. | Total bytes sent for wlan rat type for android UE | ttl_txbytes_wlan_android
. | Total bytes sent for wlan rat type for laptop UE | ttl_txbytes_wlan_laptop
. | Total bytes sent for wlan rat type for any other kind of UE | ttl_txbytes_wlan_unk_ue
. | Total bytes sent for cdma rat type for ios UE | ttl_txbytes_cdma_ios
. | Total bytes sent for cdma rat type for android UE | ttl_txbytes_cdma_android
. | Total bytes sent for cdma rat type for laptop UE | ttl_txbytes_cdma_laptop
. | Total bytes sent for cdma rat type for any other kind of UE" | ttl_txbytes_cdma_unk_ue
. | Total bytes sent for other rat type for ios UE | ttl_txbytes_unk_rat_ios
. | Total bytes sent for other rat type for android UE | ttl_txbytes_unk_rat_android
. | Total bytes sent for other rat type for laptop UE | ttl_txbytes_unk_rat_laptop
. | Total bytes sent for other rat type for any other kind of UE | ttl_txbytes_unk_rat_unk_ue
. | Total video session on time for gprs rat type for ios UE | ttl_video_session_time_gprs_ios
. | Total video session on time for gprs rat type for android UE | ttl_video_session_time_gprs_android
. | Total video session on time for gprs rat type for laptop UE | ttl_video_session_time_gprs_laptop
. | Total video session on time for gprs rat type for any other kind of UE | ttl_video_session_time_gprs_unk_ue
. | Total video session on time for umts rat type for ios UE | ttl_video_session_time_umts_ios
. | Total video session on time for umts rat type for android UE | ttl_video_session_time_umts_android
. | Total video session on time for umts rat type for laptop UE | ttl_video_session_time_umts_laptop
. | Total video session on time for umts rat type for any other kind of UE | ttl_video_session_time_umts_unk_ue
. | Total video session on time for lte rat type for ios UE | ttl_video_session_time_lte_ios
. | Total video session on time for lte rat type for android UE | ttl_video_session_time_lte_android
. | Total video session on time for lte rat type for laptop UE | ttl_video_session_time_lte_laptop
. | Total video session on time for lte rat type for any other kind of UE | ttl_video_session_time_lte_unk_ue
. | Total video session on time for hspa rat type for ios UE | ttl_video_session_time_hspa_ios
. | Total video session on time for hspa rat type for android UE | ttl_video_session_time_hspa_android
. | Total video session on time for hspa rat type for laptop UE | ttl_video_session_time_hspa_laptop
. | Total video session on time for hspa rat type for any other kind of UE | ttl_video_session_time_hspa_unk_ue
. | Total video session on time for wlan rat type for ios UE | ttl_video_session_time_wlan_ios
. | Total video session on time for wlan rat type for android UE | ttl_video_session_time_wlan_android
. | Total video session on time for wlan rat type for laptop UE | ttl_video_session_time_wlan_laptop
. | Total video session on time for wlan rat type for any other kind of UE | ttl_video_session_time_wlan_unk_ue
. | Total video session on time for cdma rat type for ios UE | ttl_video_session_time_cdma_ios
. | Total video session on time for cdma rat type for android UE | ttl_video_session_time_cdma_android
. | Total video session on time for cdma rat type for laptop UE | ttl_video_session_time_cdma_laptop
. | Total video session on time for cdma rat type for any other kind of UE | ttl_video_session_time_cdma_unk_ue
. | Total video session on time for other rat type for ios UE | ttl_video_session_time_unk_rat_ios
. | Total video session on time for other rat type for android UE | ttl_video_session_time_unk_rat_android
. | Total video session on time for other rat type for laptop UE | ttl_video_session_time_unk_rat_laptop
. | Total video session on time for other rat type for any other kind of UE | ttl_video_session_time_unk_rat_unk_ue
. | Total video tcp flow count for gprs rat type on ios UE | ttl_video_tcp_flow_gprs_ios
. | Total video tcp flow count for gprs rat type on android UE | ttl_video_tcp_flow_gprs_android
. | Total video tcp flow count for gprs rat type on laptop UE | ttl_video_tcp_flow_gprs_laptop
. | Total video tcp flow count for gprs rat type on any other kind of UE | ttl_video_tcp_flow_gprs_unk_ue
. | Total video tcp flow count for umts rat type on ios UE | ttl_video_tcp_flow_umts_ios
. | Total video tcp flow count for umts rat type on android UE | ttl_video_tcp_flow_umts_android
. | Total video tcp flow count for umts rat type on laptop UE | ttl_video_tcp_flow_umts_laptop
. | Total video tcp flow count for umts rat type on any other kind of UE | ttl_video_tcp_flow_umts_unk_ue
. | Total video tcp flow count for lte rat type on ios UE | ttl_video_tcp_flow_lte_ios
. | Total video tcp flow count for lte rat type on android UE | ttl_video_tcp_flow_lte_android
. | Total video tcp flow count for lte rat type on laptop UE | ttl_video_tcp_flow_lte_laptop
. | Total video tcp flow count for lte rat type on any other kind of UE | ttl_video_tcp_flow_lte_unk_ue
. | Total video tcp flow count for hspa rat type on ios UE | ttl_video_tcp_flow_hspa_ios
. | Total video tcp flow count for hspa rat type on android UE | ttl_video_tcp_flow_hspa_android
. | Total video tcp flow count for hspa rat type on laptop UE | ttl_video_tcp_flow_hspa_laptop
. | Total video tcp flow count for hspa rat type on any other kind of UE | ttl_video_tcp_flow_hspa_unk_ue
. | Total video tcp flow count for wlan rat type on ios UE | ttl_video_tcp_flow_wlan_ios
. | Total video tcp flow count for wlan rat type on android UE | ttl_video_tcp_flow_wlan_android
. | Total video tcp flow count for wlan rat type on laptop UE | ttl_video_tcp_flow_wlan_laptop
. | Total video tcp flow count for wlan rat type on any other kind of UE | ttl_video_tcp_flow_wlan_unk_ue
. | Total video tcp flow count for cdma rat type on ios UE | ttl_video_tcp_flow_cdma_ios
. | Total video tcp flow count for cdma rat type on android UE | ttl_video_tcp_flow_cdma_android
. | Total video tcp flow count for cdma rat type on laptop UE | ttl_video_tcp_flow_cdma_laptop
. | Total video tcp flow count for cdma rat type on any other kind of UE | ttl_video_tcp_flow_cdma_unk_ue
. | Total video tcp flow count for other rat type on ios UE | ttl_video_tcp_flow_unk_rat_ios
. | Total video tcp flow count for other rat type on android UE | ttl_video_tcp_flow_unk_rat_android
. | Total video tcp flow count for other rat type on laptop UE | ttl_video_tcp_flow_unk_rat_laptop
. | Total video tcp flow count for other rat type on any other kind of UE | ttl_video_tcp_flow_unk_rat_unk_ue
. | Total video object count for gprs rat type on ios UE" | ttl_video_count_gprs_ios
. | Total video object count for gprs rat type on android UE | ttl_video_count_gprs_android
. | Total video object count for gprs rat type on laptop UE | ttl_video_count_gprs_laptop
. | Total video object count for gprs rat type on any other kind of UE | ttl_video_count_gprs_unk_ue
. | Total video object count for umts rat type on ios UE | ttl_video_count_umts_ios
. | Total video object count for umts rat type on android UE | ttl_video_count_umts_android
. | Total video object count for umts rat type on laptop UE | ttl_video_count_umts_laptop
. | Total video object count for umts rat type on any other kind of UE | ttl_video_count_umts_unk_ue
. | Total video object count for lte rat type on ios UE | ttl_video_count_lte_ios
. | Total video object count for lte rat type on android UE | ttl_video_count_lte_android
. | Total video object count for lte rat type on laptop UE | ttl_video_count_lte_laptop
. | Total video object count for lte rat type on any other kind of UE | ttl_video_count_lte_unk_ue
. | Total video object count for hspa rat type on ios UE | ttl_video_count_hspa_ios
. | Total video object count for hspa rat type on android UE | ttl_video_count_hspa_android
. | Total video object count for hspa rat type on laptop UE | ttl_video_count_hspa_laptop
. | Total video object count for hspa rat type on any other kind of UE | ttl_video_count_hspa_unk_ue
. | Total video object count for wlan rat type on ios UE | ttl_video_count_wlan_ios
. | Total video object count for wlan rat type on android UE | ttl_video_count_wlan_android
. | Total video object count for wlan rat type on laptop UE | ttl_video_count_wlan_laptop
. | Total video object count for wlan rat type on any other kind of UE | ttl_video_count_wlan_unk_ue
. | Total video object count for cdma rat type on ios UE | ttl_video_count_cdma_ios
. | Total video object count for cdma rat type on android UE | ttl_video_count_cdma_android
. | Total video object count for cdma rat type on laptop UE | ttl_video_count_cdma_laptop
. | Total video object count for cdma rat type on any other kind of UE | ttl_video_count_cdma_unk_ue
. | Total video object count for other rat type on ios UE | ttl_video_count_unk_rat_ios
. | Total video object count for other rat type on android UE | ttl_video_count_unk_rat_android
. | Total video object count for other rat type on laptop UE | ttl_video_count_unk_rat_laptop
. | Total video object count for other rat type on any other kind of UE | ttl_video_count_unk_rat_unk_ue

PCC-APP Bulkstat Schema

PCC-APP is a new schema for this release.
Table 16. PCC-APP Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
PCC APP Service Statistics Summary/Messages Statistics | Inbound Messages | total-rx-inbound-msgs
Outbound messages | total-rx-outbound-msgs
AAR Messages | total-rx-aar-rcvd
Accepted AAR Messages | total-rx-aar-accept-sent
STR Messages | total-rx-str-rcvd
Accepted STR Messages | total-rx-srt-accept-sent
RAR Messages | total-rx-rar-sent
RAA Messages | total-rx-raa-rcvd
ASR Messages | total-rx-asr-sent
ASA Messages | total-rx-asa-rcvd

DLCI_UTIL Bulkstat Schema

DLCI_UTIL is a new schema for this release.
Table 17. DLCI_UTIL Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
DLCI Utilization Statistics | Path | dlci_util_path
E1T1 | dlci_util_ds1e1
Timeslot | dlci_util_timeslot
DLCI | dlci_util_dlci_no
DLCI Utilization Statistics/Average DLCI Utilization (Kbps | Current RX | dlci_util_dlci_curr_rx
Current TX | dlci_util_dlci_curr_tx
5min Rx | dlci_util_dlci_5min_rx
5min Tx | dlci_util_dlci_5min_tx
15min Rx | dlci_util_dlci_15min_rx
15min Tx | dlci_util_dlci_15min_tx

EGTPC Bulk Statistics Enhancements

The following counters were added to the EGTPC Bulkstat Schema:
Table 18. EGTPC Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Display Name
--- | --- | ---
EGTPC Schema/Tunnel/Create Ind Data Forwarding Tunnel Response | Accepted RX | tun-recv-creinddatafwdngrspaccept

SGW Bulk Statistics Enhancements

The following changes were made to the SGW Bulkstat Schema:
Table 19. SGW Schema Statistics

Schema Directory Path | Wem Display Name | CLI Display Name
--- | --- | ---
Obsolete Counters
. | . | intersgwhaovstat-intra-intramme-success
intersgwhaovstat-intra-intramme-fail
intersgwhaovstat-intra-intermme-success
intersgwhaovstat-intra-intermme-fail
New Counters
PDN PLMN Statistics/Home PDNs | PDNs active | plmnstat-home-pdn-active
PDNs setup | plmnstat-home-pdn-setup
PDNs released | plmnstat-home-pdn-released
PDN PLMN Statistics/Roaming PDNs | PDNs active. | plmnstat-roam-pdn-active
PDNs setup | plmnstat-roam-pdn-setup
PDNs released. | plmnstat-roam-pdn-released
PDN PLMN Statistics/Visiting PDNs | PDNs active. | plmnstat-vist-pdn-active
PDNs setup | plmnstat-vist-pdn-setup
PDNs released | plmnstat-vist-pdn-released
Source Violation | Packets Dropped | srcviolatestat-packets-dropped
Bytes Dropped | srcviolatestat-bytes-dropped
Session Level Statistics/Current/CurrentPDNs Per PDN-Type | ipv4 | sessstat-totcur-pdn-ipv4
ipv6 | sessstat-totcur-pdn-ipv6
ipv4v6 | sessstat-totcur-pdn-ipv4v6
IPV4 PDN Data Statistics | Pkts to user | ipv4-pdn-to-user-pkt
Bytes to user | ipv4-pdn-to-user-byte
Packets from user | ipv4-pdn-from-user-pkt
Bytes from user | ipv4-pdn-from-user-byte
IPV6 PDN Data Statistics | Pkts to user | ipv6-pdn-to-user-pkt
Bytes to user | ipv6-pdn-to-user-byte
Packets from user | ipv6-pdn-from-user-pkt
Bytes from user | ipv6-pdn-from-user-byte
IPV4V6 PDN Data Statistics | IPV4 Pkts to user | ipv4v6-pdn-ipv4-to-user-pkt
IPV4 Bytes to user | ipv4v6-pdn-ipv4-to-user-byte
IPV4 Packets from user | ipv4v6-pdn-ipv4-from-user-pkt
IPV4 Bytes from user | ipv4v6-pdn-ipv4-from-user-byte
IPV6 Pkts to user | ipv4v6-pdn-ipv6-to-user-pkt
IPV6 Bytes to user | ipv4v6-pdn-ipv6-to-user-byte
IPV6 Packets from user | ipv4v6-pdn-ipv6-from-user-pkt
IPV6 Bytes from user | ipv4v6-pdn-ipv6-from-user-byte
SGW Statistics/Session Level Statistics/Paging Statistics | DDN Notifications Throttled | ddn-notifications-throttled
SGW Statistics/Session Level Statistics/Intra-SGW Handover Statistics/Intra-MME | Intra-MME | intrasgwhaovstat-intramme
Success | intrasgwhaovstat-intramme-success
Fail | intrasgwhaovstat-intramme-fail
SGW Statistics/Session Level Statistics/Intra-SGW Handover Statistics/Inter-MME | Inter-MME | intrasgwhaovstat-intermme
Success | intrasgwhaovstat-intermme-success
Fail | intrasgwhaovstat-intermme-fail
SGW Statistics/Session Level Statistics/Idle Mode Signaling Reduction (ISR) Statistics | ISR Active Subscribers By Current Idle State | sessstat-isr-curr-idle-sess
ISR Active Subscribers By Current Active State | sessstat-isr-curr-active-sess
SGW Statistics/Session Level Statistics/Idle Mode Signaling Reduction (ISR) Statistics/Total ISR Activations | From MME | sessstat-isr-activations-mme
From S4-SGSN | sessstat-isr-activations-s4sgsn
SGW Statistics/Session Level Statistics/Idle Mode Signaling Reduction (ISR) Statistics/Total ISR Deactivations | From MME | sessstat-isr-deactivations-mme
From S4-SGSN | sessstat-isr-deactivations-s4sgsn
Due to Call Clear | sessstat-isr-deactivations-callclear
SGW Statistics/Session Level Statistics/Bearer Level Statistics | Total Bearers Attempted | totepsbearsetup-attempt
SGW Statistics/Data Statistics For Traffic Policing/Downlink | Bytes Dropped | trafpol-downlnk-bytes-dropped
Packets Dropped | trafpol-downlnk-pkts-dropped
Bytes Green | trafpol-downlnk-bytes-green
Packets Green | trafpol-downlnk-pkts-green
Bytes Red | trafpol-downlnk-bytes-red
Packets Red | trafpol-downlnk-pkts-red
Bytes Yellow | trafpol-downlnk-bytes-yellow
Packets Yellow | trafpol-downlnk-pkts-yellow
Bytes Low IP Prec | trafpol-downlnk-bytes-low_ip_prec
Packets Low IP Prec | trafpol-downlnk-pkts-low_ip_prec
Bytes Transmitted | trafpol-downlnk-bytes-xmitted
Packets Transmitted | trafpol-downlnk-pkts-xmitted
SGW Statistics/Data Statistics For Traffic Policing/Uplink | Bytes Dropped | trafpol-uplnk-bytes-dropped
Packets Dropped | trafpol-uplnk-pkts-dropped
Bytes Green | trafpol-uplnk-bytes-green
Packets Green | trafpol-uplnk-pkts-green
Bytes Red | trafpol-uplnk-bytes-red
Packets Red | trafpol-uplnk-pkts-red
Bytes Yellow | trafpol-uplnk-bytes-yellow
Packets Yellow | trafpol-uplnk-pkts-yellow
Bytes Low IP Prec | trafpol-uplnk-bytes-low_ip_prec
Packets Low IP Prec | trafpol-uplnk-pkts-low_ip_prec
Bytes Transmitted | trafpol-uplnk-bytes-xmitted
Packets Transmitted | trafpol-uplnk-pkts-xmitted

CSCF Bulk Statistics Enhancements

The following counters were added to the CSCF Bulkstat Schema:
Table 20. CSCF Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
CSCF Statistics/CSCF Session Duration Counters | &lt;1sec | calldur-lt-01sec
01..10sec | calldur-01to10sec
10..30sec | calldur-10to30sec
30..60sec | calldur-30to60sec
60..90sec | calldur-60to90sec
90..120sec | calldur-90to120sec
120..150sec | calldur-120to150sec
150..180sec | calldur-150to180sec
150..180sec | calldur-150to180sec
03..04min | calldur-03to04min
04..05min | calldur-04to05min
05..06min | calldur-05to06min
06..07min | calldur-06to07min
07..08min | calldur-07to08min
08..09min | calldur-08to09min
09..11min | calldur-09to11min
11..13min | calldur-11to13min
13..15min | calldur-13to15min
15..17min | calldur-15to17min
17..19min | calldur-17to19min
19..21min | calldur-19to21min
21..23min | calldur-21to23min
23..25min | calldur-23to25min
25..27min | calldur-25to27min
27..29min | calldur-27to29min
29..60min | calldur-29to60min
&gt;60min | calldur-gt-60min
CSCF Service Statistics/Calls | Mobile Originating Calls Success Rate | mo-call-succ-rate
Mobile Terminating Calls Success Rate | mt-call-succ-rate
Mobile Originating VOICE Calls Success Rate | mo-voice-call-succ-rate
Mobile Terminating VOICE Calls Success Rate | mt-voice-call-succ-rate
Mobile Originating VIDEO Calls Success Rate | mo-video-call-succ-rate
Mobile Terminating VIDEO Calls Success Rate | mt-video-call-succ-rate
Total Emergency Privacy Calls | emerg-priv-calls
Total RTCP Packets Sent | rtcp-sent
Total MSRP Packets Sent | msrp-sent
Total MSRP Packets Received | msrp-recv
CSCF Service Statistics/MSRP TCP Connection Statistics | Active Connections | msrp-active-tcp-conn
Total Connections Closed | msrp-closed-tcp-conn
Total Successful Outgoing Connections | msrp-succ-tcp-conn-out
Total Failed Outgoing Connections | msrp-fail-tcp-conn-out
Total Successful Incoming Connections | msrp-succ-tcp-conn-in
Total Failed Incoming Connections | msrp-fail-tcp-conn-in
Total Packets Received | msrp-packet-rx
Total Packets Sent | msrp-packet-tx
Total Bytes Received | msrp-bytes-rx
Total Bytes Sent | msrp-bytes-tx
Total MSRP Subscribers | msrp-tcp-subs
CSCF Service Statistics/CSCF Registrations/Registration Statistics | 439 FirstHopLackOb (Registration) Received | reg-resp-439rx
439 FirstHopLackOb (Registration) Transmitted | reg-resp-439tx
CSCF Service Statistics/CSCF Registrations/Re-Registration Statistics | 439 FirstHopLackOb (Re-Registration) Received | rereg-resp-439rx
439 FirstHopLackOb (Re-Registration) Transmitted | rereg-resp-439tx
CSCF Service Statistics/CSCF Message Statistics | 413 Request Entity Too Large Received | message-413-rx
413 Request Entity Too Large Transmitted | message-413-tx
CSCF Service Statistics/SIP TCP Connection Statistics | Total TCP Subscribers | sip-tcp-subs
CSCF Service Statistics/SIP Response | Received - 439 First Hop Lack Outbound | fhloerrrx
Transmitted - 439 First Hop Lack Outbound | fhloerrtx

HSGW Bulk Statistics Enhancements

The following counters were added to the HSGW Bulkstat Schema:
Table 21. HSGW Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
HSGW Statistics/Session Level Statistics/Total Current Pdns Per Pdn-type | IPv4 | sessstat-totcur-pdn-ipv4
IPv6 | sessstat-totcur-pdn-ipv6
IPv4v6 | sessstat-totcur-pdn-ipv4v6
HSGW Statistics/Data Statistics/IPV4 PDN Data Statistics | Pkts to User | ipv4-pdn-to-user-pkt
Bytes to User | ipv4-pdn-to-user-byte
Pkts from User | ipv4-pdn-from-user-pkt
Bytes from User | ipv4-pdn-from-user-byte
HSGW Statistics/Data Statistics/IPV6 PDN Data Statistics | Pkts to User | ipv6-pdn-to-user-pkt
Bytes to User | ipv6-pdn-to-user-byte
Pkts from User | ipv6-pdn-from-user-pkt
Bytes from User | ipv6-pdn-from-user-byte
HSGW Statistics/Data Statistics/IPV4V6 PDN Data Statistics | IPv4 Pkts to User | ipv4v6-pdn-ipv4-to-user-pkt
IPv4 Bytes to User | ipv4v6-pdn-ipv4-to-user-byte
IPv4 Pkts from User | ipv4v6-pdn-ipv4-from-user-pkt
IPv4 Bytes from User | ipv4v6-pdn-ipv4-from-user-byte
IPv6 Pkts to User | ipv4v6-pdn-ipv6-to-user-pkt
IPv6 Bytes to User | ipv4v6-pdn-ipv6-to-user-byte
IPv6 Pkts from User | ipv4v6-pdn-ipv6-from-user-pkt
IPv6 Bytes from User | ipv4v6-pdn-ipv6-from-user-byte

PGW Bulk Statistics Enhancements

The following counters were added to the PGW Bulkstat Schema:
Table 22. PGW Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
PGW Statistics/Subscriber Data Statistics/IPV4 PDN Data Statistics | Bytes from User | ipv4-pdn-from-user-byte
Pkts from User | ipv4-pdn-from-user-pkt
Bytes to User | ipv4-pdn-to-user-byte
Pkts to User | ipv4-pdn-to-user-pkt
PGW Statistics/Subscriber Data Statistics/IPV6 PDN Data Statistics | Bytes from User | ipv6-pdn-from-user-byte
Pkts from User | ipv6-pdn-from-user-pkt
Bytes to User | ipv6-pdn-to-user-byte
Pkts to User | ipv6-pdn-to-user-pkt
PGW Statistics/Subscriber Data Statistics/IPV4V6 PDN Data Statistics | Ipv4 Bytes from User | ipv4v6-pdn-ipv4-from-user-byte
Ipv4 Pkts from User | ipv4v6-pdn-ipv4-from-user-pkt
Ipv4 Bytes to User | ipv4v6-pdn-ipv4-to-user-byte
Ipv4 Pkts to User | ipv4v6-pdn-ipv4-to-user-pkt
Ipv6 Bytes from User | ipv4v6-pdn-ipv6-from-user-byte
Ipv6 Pkts from User | ipv4v6-pdn-ipv6-from-user-pkt
Ipv6 Bytes to User | ipv4v6-pdn-ipv6-to-user-byte
Ipv6 Pkts to User | ipv4v6-pdn-ipv6-to-user-pkt
PGW Statistics/Subscriber Session Statistics/Total Bearers Rejected/Total Bearers Modification Failure | Syntact Error in TFT | sessstat-bearmodfail-uesyntft

CSCFINTF Bulk Statistics Enhancements

The following counters were added to the CSCFINTF bulkstat schema:
Table 23. CSCFINTF Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
CSCF INTF Statistics/SIP Response | 422 Session Interval Too Small - Received | sitserrrx
422 Session Interval Too Small - Transmitted | sitserrtx
439 First Hop Lack Outbound - Received | fhloerrrx
439 First Hop Lack Outbound - Transmitted | fhloerrtx
CSCF INTF Statistics/Calls | Mobile Originating Calls Success Rate | mo-call-succ-rate
Mobile Terminating Calls Success Rate | mt-call-succ-rate
Mobile Originating VOICE Calls Success Rate | mo-voice-call-succ-rate
Mobile Terminating VOICE Calls Success Rate | mt-voice-call-succ-rate
Mobile Originating VIDEO Calls Success Rate | mo-video-call-succ-rate
Mobile Terminating VIDEO Calls Success Rate | mt-video-call-succ-rate

System Bulk Statistics Enhancements

The following changes were made to the System Bulkstat Schema:
Table 24. System Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Counter Name
--- | --- | ---
Obsolete Statistics
. | Storage Device Name | storage-name
New Statistics
System Statistics/Session Managers/User Data Statistics | UMTS Data Packets to User | sess-txpackets-umts
UMTS Data Octets to User | sess-txbytes-umts
UMTS Data Packets from User | sess-rxpackets-umts
UMTS Data Octets from User | sess-rxbytes-umts
GPRS Data Packets to User | sess-txpackets-gprs
GPRS Data Octets to User | sess-txbytes-gprs
GPRS Data Packets from User | sess-rxpackets-gprs
GPRS Data Octets from User | sess-rxbytes-gprs
LTE Data Packets to User | sess-txpackets-lte
LTE Data Octets to User | sess-txbytes-lte
LTE Data Packets from User | sess-rxpackets-lte
LTE Data Octets from User | sess-rxbytes-lte
eHRPD Data Packets to User | sess-txpackets-ehrpd
eHRPD Data Octets to User | sess-txbytes-ehrpd
eHRPD Data Packets from User | sess-rxpackets-ehrpd
eHRPD Data Octets from User | sess-rxbytes-ehrpd
System Statistics/Session Managers/Connection Statistics | CDMA 1X RTT Total Sessions | sess-total-sessions-1xrtt
CDMA 1X RTT Total Calls Arrived | sess-num-calls-arrived-1xrtt
CDMA 1X RTT Total Calls Disconnected | sess-num-calls-disconnected-1xrtt
CDMA EVDO Total Sessions | sess-total-sessions-evdorev0
CDMA EVDO Total Calls Arrived | sess-num-calls-arrived-evdorev0
CDMA EVDO Total Calls Disconnected | sess-num-calls-disconnected-evdorev0
CDMA EVDO Rev-a Total Sessions | sess-total-sessions-evdoreva
CDMA EVDO Rev-a Total Calls Arrived | sess-num-calls-arrived-evdoreva
CDMA EVDO Rev-a Total Calls Disconnected | sess-num-calls-disconnected-evdoreva
System Statistics/ASNPC Statistics | IM Exit Recd | asnpc-imexitresponsetopaging
No Response to Paging | asnpc-noresponsetopaging
System Statistics/CC Message Error Statistics | Permanent Failures | cc-msgerr-permfailure
Transient Failures | cc-msgerr-transfailure
System Statistics/CCA Result Code 2xxx Stats | Result Code 2001 | cca-2001-rc
Result Code 2002 | cca-2002-rc
System Statistics/CCA Result Code 4xxx Stats | Result Code 4001 | cca-4001-rc
Result Code 4002 | cca-4002-rc
Result Code 4003 | cca-4011-rc
Result Code 4004 | cca-4012-rc
System Statistics/CCA Result Code 5xxx Stats | Result Code 5001 | cca-5001-rc
Result Code 5002 | cca-5002-rc
Result Code 5003 | cca-5003-rc
Result Code 5004 | cca-5004-rc
Result Code 5005 | cca-5005-rc
Result Code 5006 | cca-5006-rc
All Other Result Codes | cca-other-rc
System Statistics/Session Disconnect Reasons | sgsn-pgw-init-deact | disc-reason-493
s6b-ip-validation-failed | disc-reason-494
sgsn-failure-rsp-from-sgw | disc-reason-495
tcp-remote-close | disc-reason-496
tcp-reset-received | disc-reason-497
tcp-socket-error | disc-reason-498
sgsn-ptmsi-crunch | disc-reason-499
3Gto4G-context-replacement | disc-reason-500
4Gto3G-context-replacement | disc-reason-501
mme-isr-sgsn-init-detach | disc-reason-502
sgsn-isr-addl-ptmsi-rai | disc-reason-503
sgsn-sgw-dbr-cause-isr-deact | disc-reason-504
sgsn-isr-mme-init-detach | disc-reason-505
mme-sgw-dbr-cause-isr-deact | disc-reason-506
ptmsi-signature-mismatch | disc-reason-507
camel-invalid-configuration | disc-reason-508
System Statistics/Number of Active Sessions | IPSG | ipsg-activedata
SAEGW | saegw-activedata
System Statistics/Session Managers/Connection Statistics | CDMA EVDORA Total Calls Arrived | sess-num-calls-arrived-evdora
CDMA EVDORA Total Calls Disconnected | sess-num-calls-disconnected-evdora
CDMA EVDORA Total Sessions | sess-total-sessions-evdora

CSCF Bulk Statistics Enhancements

The following counters were added to the CSCF Bulkstat Schema:
Table 25. CSCF Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Display Name
--- | --- | ---
CSCF Service Statistics/Calls | Total SRTP Packets Sent | srtp-sent
Total SRTP Packets Received | srtp-recv
Total SRTCP Packets Sent | srtcp-sent
Total SRTCP Packets Received | srtcp-recv

EGTPC Bulk Statistics Enhancements

The following counters were added to the EGTPC Bulkstat Schema:
Table 26. EGTPC Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Display Name
--- | --- | ---
EGTPC Statistics/Alert MME Acknowledge | Total RX | mobility-recv-alertmmeack
Total RX Accepted | mobility-recv-alertmmeackaccept
Total RX Denied | mobility-recv-alertmmeackdenied
Retrans RX | mobility-recv-retransalertmmeack
Total TX | mobility-sent-alertmmeack
Total TX Accepted | mobility-sent-alertmmeackaccept
Total TX Denied | mobility-sent-alertmmeackdenied
Retrans TX | mobility-sent-retransalertmmeack
EGTPC Statistics/Alert MME Notification | Total RX | mobility-recv-alertmmenotf
Retrans RX | mobility-recv-retransalertmmenotf
Total TX" | mobility-sent-alertmmenotf
Retrans TX | mobility-sent-retransalertmmenotf
EGTPC Statistics/CS Paging Indication | Total RX | mobility-recv-cspagingind
Total TX | mobility-sent-cspagingind
EGTPC Statistics/Detach Acknowledge | Total RX | mobility-recv-detachack
Total RX Accepted | mobility-recv-detachackaccept
Total RX Denied | mobility-recv-detachackdenied
Total TX | mobility-sent-detachack
Total TX Accepted | mobility-sent-detachackaccept
Total TX Denied | mobility-sent-detachackdenied
EGTPC Statistics/Detach Notification | Total RX | mobility-recv-detachnotf
Retrans RX | mobility-recv-retransdetachnotf
Total TX | mobility-sent-detachnotf
Retrans TX | mobility-sent-retransdetachnotf
EGTPC Statistics/UE Activity Acknowledge | Total RX | mobility-recv-ueactivityack
Total RX Accepted | mobility-recv-ueactivityackaccept
Total RX Denied | mobility-recv-ueactivityackdenied
Retrans RX | mobility-recv-retransueactivityack
Total TX | mobility-sent-ueactivityack
Total TX Accepted | mobility-sent-ueactivityackaccept
Total TX Denied | mobility-sent-ueactivityackdenied
Retrans TX | mobility-sent-retransueactivityack
EGTPC Statistics/UE Activity Notification | Total RX | mobility-recv-ueactivitynotf
Retrans RX | mobility-recv-retransueactivitynotf
Total TX | mobility-sent-ueactivitynotf
Retrans TX | mobility-sent-retransueactivitynotf
EGTPC Statistics/Tunnel Management Messages/Change Notification Request | Initial RX | tun-recv-changenotfreq
Initial TX | tun-sent-changenotfreq
Retrans RX | tun-recv-retranschangenotfreq
Retrans TX | tun-sent-retranschangenotfreq
EGTPC Statistics/Tunnel Management Messages/Change Notification Response | Initial RX | tun-recv-changenotfresp
Accepted RX | tun-recv-changenotfrespaccept
Denied RX | tun-recv-changenotfrespdenied
Initial TX | tun-sent-changenotfresp
Accepted TX" | tun-sent-changenotfrespaccept
Denied TX | tun-sent-changenotfrespdenied
Retrans TX | tun-sent-retranschangenotfresp
EGTPC Statistics/Tunnel /Downlink Data Notification Response | Initial TX | tun-sent-dlinknotifack
Accepted TX | tun-sent-dlinknotifackaccept
Denied TX | tun-sent-dlinknotifackdenied
EGTPC Statistics/SRVCC Messages/PS to CS Cancel Acknowledge | Initial RX | srvcc-recv-pstocscancelack
Accepted RX | srvcc-recv-pstocscanelackaccept
Denied RX | srvcc-recv-pstocscancelackdenied
EGTPC Statistics/SRVCC Messages/PS to CS Complete Acknowledge | Initial TX | srvcc-sent-pstocscmpack
Accepted TX | srvcc-sent-pstocscmpackaccept
Denied TX | srvcc-sent-pstocscmpackdenied
Retrans TX | srvcc-sent-retranspstocscmpack
EGTPC Statistics/SRVCC Messages/PS to CS Complete Notification | Initial RX | srvcc-recv-pstocscmpnotf
Retrans RX | srvcc-recv-retranspstocscmpnotf

MME Bulk Statistics Enhancements

The following counters were added to the MME Bulkstat Schema:
Table 27. MMEBulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Display Name
--- | --- | ---
MME Statistics/NW Initiated Service Request Events | Attempted | ecmevent-nw-srvcreq-attempt
Success | ecmevent-nw-srvcreq-success
Failure | ecmevent-nw-srvcreq-failure
MME Statistics/UE Initiated Service Request Events | Attempted | ecmevent-ue-srvcreq-attempt
Success | ecmevent-ue-srvcreq-success
Failure | ecmevent-ue-srvcreq-failure
MME Statistics/Total EMM Control Messages/Sent | EPS Non-EPS Not Allowed | emm-msgtx-eps-non-eps-not-allowed
No EPS Service in this PLMN | emm-msgtx-no-eps-svc-plmn
tau - no eps service in plmn | emm-msgtx-tau-no-eps-svc-plmn
MME Statistics/Total ESM Control Messages/Sent | Bearer Alloc Reject - Authentication Failed | esm-msgtx-brralloc-rej-auth-failed
Bearer Alloc Reject - Service Opt Not Subscribed | esm-msgtx-brralloc-rej-svc-not-subscribed
Bearer Alloc Reject - Service Opt Not Supported | esm-msgtx-brralloc-rej-svc-not-supported
Bearer Modify Reject - Authentication Failed | esm-msgtx-brrmod-rej-auth-failed
Bearer Modify Reject - Service Opt Not Subscribed | esm-msgtx-brrmod-rej-svc-not-subscribed
Bearer Modify Reject - Service Opt Not Supported | esm-msgtx-brrmod-rej-svc-not-supported
PDN Connectivity Reject - Authentication Failed | esm-msgtx-pdncon-rej-auth-failed
PDN Connectivity Reject - Service Opt Not Subscribed | esm-msgtx-pdncon-rej-svc-not-subscribed
PDN Connectivity Reject - Service Opt Not Supported | esm-msgtx-pdncon-rej-svc-not-supported
MME Statistics/ESM Events/PDN IPv4 Connections | Attempted | esmevent-pdncon-ipv4-attempt
Success | esmevent-pdncon-ipv4-success
Failures | esmevent-pdncon-ipv4-failure
MME Statistics/ESM Events/PDN IPv6 Connections | Attempted | esmevent-pdncon-ipv6-attempt
Success | esmevent-pdncon-ipv6-success
Failures | esmevent-pdncon-ipv6-failure
MME Statistics/ECM Statistics/Paging Initiation Events | Success at TAI List | paging-tai-list-success
MME Statistics/ECM Events/Paging Initiation Events | Last EnodeB Success | ecmevent-lastenb-success
Last TAI Success | ecmevent-lasttai-success
MME Statistics/Bearer Statistics | Currrent Connected Bearers | connected-brr-current
Maximum Connected Bearers | connected-brr-max
Current Idle Bearers | idle-brr-current
Maximum Idle Bearers | idle-brr-max
Total Current Bearers | tot-brr-current
Total Maximum Bearers | tot-brr-max
MME Statistics/PDN Statistics | Current Connected PDNs | connected-pdn-current
Maximum Connected PDNs | connected-pdn-max
Current Idle PDNs | idle-pdn-current
Maximum Idle PDNs | idle-pdn-max
Total Current PDNs | tot-pdn-current
Total Maximum PDNs | tot-pdn-max

GTPC Bulk Statistics Enhancements

The following counters were added to the GTPC Bulkstat Schema:
Table 28. GTPC Bulkstat Schema Statistics

Schema Directory Path | Wem Display Name | CLI Display Name
--- | --- | ---
GTPC Statistics/Session Statistics | Current - IPv4v6 | current-ipv4v6
Setup - IPv4v6 | setup-ipv4v6

Modified WEM Features

This section identifies WEM features modified in release 14.0 and contains two types of modifications: enhancements and behavior changes. Feature enhancements are modifications based on customer change requests. Feature behavior changes are modifications based on software error corrections (bug fixes) or other code fixes that result in a change in feature behavior.

Feature Enhancements

Change requests have resulted in the following enhancements:

Keepalive Parameter Edits Support Client-Server Reconnection

Sometimes after a client-server connection is broken, WEM displays the message that the client cannot reconnect. This problem is caused by incorrect keepalive settings in the Client Session parameters found in the nms.cfg file.

Resetting the keepalive to Minimum = 0, Maximum = 8600 and Default = 60 will allow the client to reconnect shortly after it is returned to the network.

There is more about the nms.cfg file in the Configuration File Parameters chapter in the Web Element Manager Installation and Administration Guide.

Inspector-Level Security Enhancements

Previously, Inspector-level users had unauthorized access to the following screens: Alarm Forwarding, System Alarm History and Outstanding Alarms.

The Add, Modify, Delete, and Clear buttons for these screens have now been disabled for Inspector-level users.

openSSL Version Upgrade

Previous secure communication vulnerabilities that may have existed with earlier versions of openSSL have been addressed by upgrading to openSSL 0.9.8s.

Process Monitoring Converts WEM Statistics to XML Format

WEM monitors itself and generates some statistics - CPU usage, memory usage, disk usage, etc. Prior to this enhancement, these statistics were only displayed in a WEM table.

With this enhancement, these historical statistics can now be collected and parsed into xml files so customers can poll the data and display it in their performance management system.

The collection process is disabled by default. To enable, follow the WEM path Monitor/Test Menu/Monitoring Operations/WEM Process Monitoring/Historical Statistics.

To enable collection, click the checkbox, select a poll interval and click Apply.

Users can select the required counters and fetch the historical statistics report through the Accounting/View_Graph Bulk Statistics menu.

For more information, click the Help button on the Historical Statistics tab.

Behavior Changes Based on Code Modifications

Code modifications in this release have resulted in the following changes:

Modified Data-Type for System Schema Counters

The following WEM counters have had their data-type changed from Int32 to Int64:

- cc-badans-auth-appid
- cc-badans-sessid
- cc-badans-cc-req-num
- cc-badans-cc-req-type
- cc-badans-origin-host
- cc-badans-origin-realm
- cc-badans-parsemsg-err
- cc-badans-parsemscc-err
- cc-badans-misc-err