# GTP-C Schema Statistics

The GTP-C schema provides operational statistics that can be used for monitoring and troubleshooting the following products: GGSN, P-GW, S-GW.
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the GTP-C Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the service. This is a key variable. Type: Information | String
vpnid | The identification number of the context configured on the system that is currently facilitating the service. This is an internal reference number. This is a key variable. Type: Information | Int32
servname | The name of the service for which the statistics are displayed. This is a key variable. Type: Information | String
setup-current | The total number of current sessions setup Type: Gauge | Int32
current-ip | The total number of current IPv4 Sessions Type: Gauge | Int32 14.0 and later: Int64
current-ppp | The total number of current PPP sessions Type: Gauge | Int32 14.0 and later: Int64
current-ipv6 | The total number of current IPv6 Sessions Type: Gauge | Int32 14.0 and later: Int64
current-ipv4v6 | The total number of current IPv4v6 Sessions Type: Gauge | Int32 14.0 and later: Int64
current-ntwkinitd | The total number of current Network initiated Sessions Type: Gauge | Int32 14.0 and later: Int64
setup-total | The total number of PDP contexts setup. Type: Counter | Int32 14.0 and later: Int64
setup-ip | The total number of IP PDP contexts setup. Type: Counter | Int32 14.0 and later: Int64
setup-ppp | The total number of PPP PDP contexts setup. Type: Counter | Int32 14.0 and later: Int64
setup-ipv6 | The total number of IPv6 sessions Type: Counter | Int32 14.0 and later: Int64
setup-ipv4v6 | The total number of IPv4v6 sessions Type: Counter | Int32 14.0 and later: Int64
setup-sgsn | The total number of SGSN initiated sessions Type: Counter | Int32 14.0 and later: Int64
setup-ggsn | The total number of GGSN initiated sessions Type: Counter | Int32 14.0 and later: Int64
released-total | The total number of PDP contexts released. Type: Counter | Int32 14.0 and later: Int64
dyn-ipv4-attempt | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were attempted. Type: Counter | Int32 14.0 and later: Int64
dyn-ipv6-attempt | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were attempted. Type: Counter | Int32 14.0 and later: Int64
dyn-ipv4v6-attempt | The total number of IPv4v6 PDP contexts requesting dynamically assigned IP addresses that were attempted. Type: Counter | Int32 14.0 and later: Int64
dyn-ipv4-success | The total number of IPv4 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. Type: Counter | Int32 14.0 and later: Int64
dyn-ipv6-success | The total number of IPv6 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. Type: Counter | Int32 14.0 and later: Int64
dyn-ipv4v6-success | The total number of IPv4v6 PDP contexts requesting dynamically assigned IP addresses that were successfully setup. Type: Counter | Int32 14.0 and later: Int64
echo-req-rx | The total number of GTPC echo requests received. Type: Counter | Int32 14.0 and later: Int64
echo-req-tx | The total number of GTPC echo requests transmitted. Type: Counter | Int32 14.0 and later: Int64
gtpu-echo-req-rx | The total number of GTPU echo requests received. Type: Counter | Int32 14.0 and later: Int64
gtpu-echo-req-tx | The total number of GTPU echo requests transmitted. Type: Counter | Int32 14.0 and later: Int64
echo-rsp-tx | The total number of GTPC echo responses transmitted. Type: Counter | Int32 14.0 and later: Int64
echo-rsp-rx | The total number of GTPC echo responses received. Type: Counter | Int32 14.0 and later: Int64
gtpu-echo-rsp-tx | The total number of GTPU echo responses transmitted. Type: Counter | Int32 14.0 and later: Int64
gtpu-echo-rsp-rx | The total number of GTPU echo responses received. Type: Counter | Int32 14.0 and later: Int64
cpc-total | The total number of Create PDP Context Request messages received. This is the sum of GTPC v0 and GTP v1 messages. Type: Counter | Int32 14.0 and later: Int64
cpc-v0 | The total number of Create PDP Context Request messages received that used GTPC version 0. Type: Counter | Int32 14.0 and later: Int64
cpc-v1 | The total number of Create PDP Context Request messages received that used GTPC version 1. Type: Counter | Int32 14.0 and later: Int64
cpc-sec | The total number of Activate Secondary PDP Context Request received. Type: Counter | Int32 14.0 and later: Int64
cpc-retrans | The total number of re-transmitted Create PDP Context Request messages received from the SGSN for either the primary or secondary PDP contexts. Type: Counter | Int32 14.0 and later: Int64
cpc-accept | The total number of Create PDP Context Response messages transmitted containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
cpc-deny | The total number of “reject” Create PDP Context Response messages transmitted. Type: Counter | Int32 14.0 and later: Int64
cpc-discard | The total number of Create PDP Context Request messages received from the SGSN(s) that were discarded. Type: Counter | Int32 14.0 and later: Int64
upc-rx | The total number of Update PDP Context Request messages received from the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
upc-rx-accept | The total number of Update PDP Context Response messages transmitted to the SGSN(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
upc-rx-deny | The total number of “reject” Update PDP Context Response messages transmitted to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
upc-rx-discard | The total number of Update PDP Context Request messages received from SGSN(s) that were discarded Type: Counter | Int32 14.0 and later: Int64
upc-tx | The total number of Update PDP Context Request messages transmitted to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
upc-tx-accept | The total number of Update PDP Context Response messages sent to the SGSN(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
upc-tx-deny | The total number of “reject” Update PDP Context Response messages sent to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
upc-tx-dt-upd | The total number of Update PDP Context Response messages sent to SGSN(s) for direct tunnel update. Type: Counter | Int32 14.0 and later: Int64
dpc-rx | The total number of Delete PDP Context Request messages received from the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
dpc-rx-accept | The total number of Delete PDP Context Response messages transmitted containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
dpc-rx-deny | The total number of “reject” Delete PDP Context Response messages transmitted. Type: Counter | Int32 14.0 and later: Int64
dpc-rx-discard | The total number of Delete PDP Context Request messages received from the SGSN(s) that were discarded Type: Counter | Int32 14.0 and later: Int64
dpc-tx | The total number of Delete PDP Context Request messages transmitted to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
dpc-tx-accept | The total number of Delete PDP Context Response messages received from the SGSN(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
dpc-tx-deny | The total number of “reject” Delete PDP Context Response messages received from the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
cpc-aa | The total number of Create AA (anonymous access) PDP Context Request messages received. Type: Counter | Int32 14.0 and later: Int64
cpc-aa-accept | The total number of Create AA PDP Context Response messages transmitted to the SGSN with a cause code of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
cpc-aa-deny | The total number of “reject” Create AA PDP Context Response messages transmitted to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
cpc-aa-discard | The total number of Create AA PDP Context Request messages received that were discarded without transmitting a response to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
dpc-aa-rx | The total number of Delete AA PDP Context Request messages received from the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
dpc-aa-rx-accept | The total number of Delete AA PDP Context Response messages transmitted containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
dpc-aa-rx-deny | The total number of “reject” Delete AA PDP Context Response messages transmitted to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
dpc-aa-rx-discard | The total number of Delete PDP AA Context Request messages received from the SGSN(s) that were discarded Type: Counter | Int32 14.0 and later: Int64
dpc-aa-tx | The total number of Delete AA PDP Context Request messages transmitted to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
dpc-aa-tx-accept | The total number of Delete AA PDP Context Response messages received from the SGSN(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32 14.0 and later: Int64
dpc-aa-tx-deny | The total number of “reject” Delete AA PDP Context Response messages received from the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
err-ind-rx | The total number of error indication messages received from the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
err-ind-tx | The total number of error indication messages transmitted to the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
err-ind-rx-discard | The total number of error indication messages received and discarded at the SGSN(s). Type: Counter | Int32 14.0 and later: Int64
cpc-noresource | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 199 (C7H, No resources available). Type: Counter | Int32 14.0 and later: Int64
cpc-addr-occupied | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 211 (D3H, All dynamic PDP addresses are occupied). Type: Counter | Int32 14.0 and later: Int64
cpc-nomem | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 212 (D4H, No memory is available). Type: Counter | Int32 14.0 and later: Int64
cpc-missing-apn | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 219 (DBH, Missing or unknown APN). Type: Counter | Int32 14.0 and later: Int64
cpc-unknown-pdp | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 220 (DCH, Unknown PDP address or PDP type). Type: Counter | Int32 14.0 and later: Int64
cpc-no-apn-subscription | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent because there was no apn subscription. Type: Counter | Int32 14.0 and later: Int64
cpc-auth-fail | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 201. Type: Counter | Int32 14.0 and later: Int64
cpc-sys-fail | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 204 (CCH, System failure). Type: Counter | Int32 14.0 and later: Int64
cpc-sem-tft | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 215 (D7H, Semantic error in the TFT operation). Type: Counter | Int32 14.0 and later: Int64
cpc-syn-tft | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 216 (D8H, Syntactic error in the TFT operation). Type: Counter | Int32 14.0 and later: Int64
cpc-sem-pktfilter | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 217 (D9H, Semantic error in packet filter(s)). Type: Counter | Int32 14.0 and later: Int64
cpc-syn-pktfilter | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 218 (DAH, Syntactic error in packet filter(s)). Type: Counter | Int32 14.0 and later: Int64
cpc-ie-err | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 201 (C9H, Mandatory IE incorrect). Type: Counter | Int32 14.0 and later: Int64
cpc-ie-missing | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 202 (CAH, Mandatory IE missing). Type: Counter | Int32 14.0 and later: Int64
cpc-opt-ie-err | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 203 (CBH, Optional IE incorrect). Type: Counter | Int32 14.0 and later: Int64
cpc-malformed | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 193 (C1H, Invalid message format). Type: Counter | Int32 14.0 and later: Int64
cpc-version | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 198 (C6H, version not supported). Type: Counter | Int32 14.0 and later: Int64
cpc-srv-not-supp | The total number of “reject” Create PDP Context Response messages transmitted to the SGSN(s) sent with a cause code of 200 (C8H, service not Supported). Type: Counter | Int32 14.0 and later: Int64
disc-sgsn | The total number of sessions released by SGSN(s). Type: Counter | Int32 14.0 and later: Int64
disc-path-fail | The total number of session releases that occurred due to path failure. Type: Counter | Int32 14.0 and later: Int64
disc-smgr-dead | The total number of sessions released due to the termination of the session manager that was facilitating them. Type: Counter | Int32
disc-admin | The total number of sessions administratively released. Type: Counter | Int32
disc-other | The total number of sessions released due to other reasons. Type: Counter | Int32
disc-teardown | The total number of sessions disconnected normally. Type: Counter | Int32
disc-idle | The total number of sessions released due to the expiration of the idle timeout period as specified in the APN configuration. Type: Counter | Int32
disc-absolute | The total number of sessions released due to the expiration of the absolute timeout period as specified in the APN configuration. Type: Counter | Int32
disc-src-addr | The total number of sessions released due to source address violations. Type: Counter | Int32
disc-flow-add | The total number of sessions released reason due to flow addition failures. Type: Counter | Int32
disc-dhcp-renew-fail | The total number of sessions released due to failed DHCP lease renewal. Type: Counter | Int32
disc-long-durn | The total number of sessions released due to the expiration of the long duration timeout period. Type: Counter | Int32
disc-aborted | The total number of sessions released due to miscellaneous call abort conditions. Type: Counter | Int32
disc-apn-rmvd | The total number of sessions released due to the removal of an APN’s configuration. Type: Counter | Int32
pdu-notif | The total number of PDU Notification Request messages transmitted to the SGSN(s). Type: Counter | Int32
pdu-notif-accept | The total number of PDU Notification Response messages received from the SGSN(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32
pdu-notif-deny | The total number of “deny” PDU Notification Response messages received from the SGSN(s). Type: Counter | Int32
pdu-notif-rej | The total number of PDU Notification Reject Request messages received from the SGSN(s). Type: Counter | Int32
pdu-notif-rej-accept | The total number of PDU Notification Reject Response messaged transmitted to the SGSN(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32
pdu-notif-rej-deny | The total number of “deny” PDU Notification Reject Response messages transmitted to the SGSN(s). Type: Counter | Int32
pdu-notif-rej-discard | The total number of PDU Notification Reject Request messages discarded by the GGSN without any response transmitted to the SGSN(s). Type: Counter | Int32
num-dt-established | The total number of direct tunnels established between RNC and GGSN. Type: Counter | Int32
num-dt-torn-by-sgsn | The total number of established direct tunnels between SGSN and GGSN torn by SGSN. Type: Counter | Int32
num-dt-recv-err-ind | The total number of direct tunnels requests received from SGSN with error indication. Type: Counter | Int32
sri-req | The total number of Send Routing Information (SRI) for GPRS messages transmitted to the HLR(s). Type: Counter | Int32
sri-accept | The total number of Send Routing Info for GPRS Ack messages received from the HLR(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32
sri-deny | The total number of “deny” Send Routing Info for GPRS Ack messages received from the HLR(s). Type: Counter | Int32
fail-rep | The total number of Failure reports transmitted to the HLR(s). Type: Counter | Int32
fail-rep-accept | The total number of Failure reports received from the HLR(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32
fail-rep-deny | The total number of “deny” Failure reports received from the HLR(s). Type: Counter | Int32
note-ms-gprs | The total number of Note MS GPRS Present messages received from the HLR(s). Type: Counter | Int32
note-ms-gprs-accept | The total number of Note MS GPRS Present Response messages transmitted to the HLR(s) containing a cause value of 128 (80H, Request accepted). Type: Counter | Int32
note-ms-gprs-deny | The total number of “deny” Note MS GPRS Present Response messages transmitted to the HLR(s). Type: Counter | Int32
note-ms-gprs-discard | The total number of Note MS GPRS Present messages discarded with no response transmitted to the HLR(s). Type: Counter | Int32
qosconv-bytes-in | The total number of Conversational Uplink Bytes Sent Type: Counter | Int64
qosconv-pkts-in | The total number of Conversational Uplink Pkts Sent Type: Counter | Int64
qosconv-bytes-out | The total number of Conversational Downlink Bytes Rcvd Type: Counter | Int64
qosconv-pkts-out | The total number of Conversational Downlink Pkts Rcvd Type: Counter | Int64
qosstrm-bytes-in | The total number of Streaming Uplink Bytes Sent Type: Counter | Int64
qosstrm-pkts-in | The total number of Streaming Uplink Pkts Sent Type: Counter | Int64
qosstrm-bytes-out | The total number of Streaming Downlink Bytes Rcvd Type: Counter | Int64
qosstrm-pkts-out | The total number of Streaming Downlink Pkts Rcvd Type: Counter | Int64
qosint1-bytes-in | The total number of Interactive 1 Uplink Bytes Sent Type: Counter | Int64
qosint1-pkts-in | The total number of Interactive 1 Uplink Pkts Sent Type: Counter | Int64
qosint1-bytes-out | The total number of Interactive 1 Downlink Bytes Rcvd Type: Counter | Int64
qosint1-pkts-out | The total number of Interactive 1 Downlink Pkts Rcvd Type: Counter | Int64
qosint2-bytes-in | The total number of Interactive 2 Uplink Bytes Sent Type: Counter | Int64
qosint2-pkts-in | The total number of Interactive 2 Uplink Pkts Sent Type: Counter | Int64
qosint2-bytes-out | The total number of Interactive 2 Downlink Bytes Rcvd Type: Counter | Int64
qosint2-pkts-out | The total number of Interactive 2 Downlink Pkts Rcvd Type: Counter | Int64
qosint3-bytes-in | The total number of Interactive 3 Uplink Bytes Sent Type: Counter | Int64
qosint3-pkts-in | The total number of Interactive 3 Uplink Pkts Sent Type: Counter | Int64
qosint3-bytes-out | The total number of Interactive 3 Downlink Bytes Rcvd Type: Counter | Int64
qosint3-pkts-out | The total number of Interactive 3 Downlink Pkts Rcvd Type: Counter | Int64
qosint-bytes-in | The total number of Interactive 1+2=3 Uplink Bytes Sent Type: Counter | Int64
qosint-pkts-in | The total number of Interactive 1+2+3 Uplink Pkts Sent Type: Counter | Int64
qosint-bytes-out | The total number of Interactive 1+2+3 Downlink Bytes Rcvd Type: Counter | Int64
qosint-pkts-out | The total number of Interactive 1+2+3 Downlink Pkts Rcvd Type: Counter | Int64
qosback-bytes-in | The total number of Background Uplink Bytes Sent Type: Counter | Int64
qosback-pkts-in | The total number of Background Uplink Pkts Sent Type: Counter | Int64
qosback-bytes-out | The total number of Background Downlink Bytes Rcvd Type: Counter | Int64
qosback-pkts-out | The total number of Background Downlink Pkts Rcvd Type: Counter | Int64
ctrl-num-bytes-in | The total number of bytes for control packets received on the Gn and/or Gp interface. Type: Counter | Int64
ctrl-num-pkts-in | The total number of control packets received on the Gn and/or Gp interface. Type: Counter | Int64
ctrl-num-bytes-out | The total number of bytes from control packets transmitted on the Gn and/or Gp interface. Type: Counter | Int64
ctrl-num-pkts-out | The total number of control packets transmitted on the Gn and/or Gp interface. Type: Counter | Int64
num-bytes-in | The total number of bytes received on the Gn and/or Gp interface. Type: Counter | Int64
num-pkts-in | The total number of packets received on the Gn and/or Gp interface. Type: Counter | Int64
num-bytes-out | The total number of bytes transmitted on the Gn and/or Gp interface. Type: Counter | Int64
num-pkts-out | The total number of packets transmitted on the Gn and/or Gp interface. Type: Counter | Int64
current-mbms-ue | The total number of current MBMS UE sessions. Type: Gauge | Int32 14.0 and later: Int64
current-mbms-mcast | The total number of current MBMS Multicast sessions. Type: Gauge | Int32 14.0 and later: Int64
current-mbms-bcast | The total number of current MBMS Broadcast sessions. Type: Gauge | Int32 14.0 and later: Int64
setup-mbms-ue | The total number of MBMS UE Sessions setup. Type: Counter | Int32 14.0 and later: Int64
setup-mbms-mcast | The total number of MBMS Multicast Sessions setup. Type: Counter | Int32 14.0 and later: Int64
setup-mbms-bcast | The total number of MBMS Broadcast Sessions setup Type: Counter | Int32 14.0 and later: Int64
chap-auth-attempt | The total number of CHAP Auth sessions attempted. Type: Counter | Int32 14.0 and later: Int64
chap-auth-success | The total number of CHAP Auth sessions successful Type: Counter | Int32 14.0 and later: Int64
chap-auth-failure | The total number of CHAP Auth sessions failed Type: Counter | Int32 14.0 and later: Int64
pap-auth-attempt | The total number of PAP Auth sessions attempted Type: Counter | Int32 14.0 and later: Int64
pap-auth-success | The total number of PAP Auth sessions successful Type: Counter | Int32 14.0 and later: Int64
pap-auth-failure | The total number of PAP Auth sessions failed Type: Counter | Int32 14.0 and later: Int64
no-auth | The total number of No-Auth sessions. Type: Counter | Int32 14.0 and later: Int64
err-ind | Total sessions released on Error Indication Type: Counter | Int32 14.0 and later: Int64
ctxt-replace | Total sessions released due to context replacement. Type: Counter | Int32 14.0 and later: Int64
purge-audit | Total sessions purged due to audit failure Type: Counter | Int32 14.0 and later: Int64
update-handoff-rej | Total sessions released due to handoff reject in UPC Type: Counter | Int32 14.0 and later: Int64
total-handoff-fail | Total path failure due to handoff Type: Counter | Int32 14.0 and later: Int64
sgsn-restart-cpc-req | Total path failure due to SGSN restart detected via CPC Type: Counter | Int32 14.0 and later: Int64
sgsn-restart-upc-req | Total path failure due to SGSN restart detected via UPC Type: Counter | Int32 14.0 and later: Int64
sgsn-restart-echo-rsp | Total path failure due to SGSN restart detected via Echo Rsp Type: Counter | Int32 14.0 and later: Int64
gtpc-echo-timeout | Total path failure due to SGSN restart detected via GTPC echo Type: Counter | Int32 14.0 and later: Int64
gtpu-echo-timeout | Total path failure due to SGSN restart detected via GTPU echo Type: Counter | Int32 14.0 and later: Int64
ggsn-req-timeout | Total path failure due to GGSN request timeout. Type: Counter | Int32 14.0 and later: Int64
version-not-sup-rx | Version not supported received Type: Counter | Int32 14.0 and later: Int64
version-not-sup-tx | Version not supported transmitted Type: Counter | Int32 14.0 and later: Int64
sup-ext-header-rx | Extension header supported received Type: Counter | Int32 14.0 and later: Int64
sup-ext-header-tx | Extension header supported transmitted Type: Counter | Int32 14.0 and later: Int64
cmc-total | The total number of Create MBMS Context request messages received. Type: Counter | Int32 14.0 and later: Int64
cmc-initial | The total number of initial Create MBMS Context request messages received. Type: Counter | Int32 14.0 and later: Int64
cmc-retrans | The total number of retransmitted Create MBMS Context request messages received. Type: Counter | Int32 14.0 and later: Int64
cmc-accept | The total number of Create MBMS Context request messages accepted by the GGSN. Type: Counter | Int32 14.0 and later: Int64
cmc-deny | The total number of Create MBMS Context request messages denied by the GGSN. Type: Counter | Int32 14.0 and later: Int64
cmc-discard | The total number of Create MBMS Context request messages discarded by the GGSN. Type: Counter | Int32 14.0 and later: Int64
umc-rx | The total number of Update MBMS Context request messages received. Type: Counter | Int32 14.0 and later: Int64
umc-rx-accept | The total number of Update MBMS Context request messages accepted by the GGSN. Type: Counter | Int32 14.0 and later: Int64
umc-rx-deny | The total number of Update MBMS Context request messages denied by the GGSN. Type: Counter | Int32 14.0 and later: Int64
umc-rx-discard | The total number of Update MBMS Context request messages discarded by the GGSN. Type: Counter | Int32 14.0 and later: Int64
dmc-rx | The total number of Delete MBMS Context request messages received. Type: Counter | Int32 14.0 and later: Int64
dmc-rx-accept | The total number of Delete MBMS Context request messages accepted by the GGSN. Type: Counter | Int32 14.0 and later: Int64
dmc-rx-deny | The total number of Delete MBMS Context request messages denied by the GGSN. Type: Counter | Int32 14.0 and later: Int64
dmc-rx-discard | The total number of Delete MBMS Context request messages discarded by the GGSN. Type: Counter | Int32 14.0 and later: Int64
dmc-tx | The total number of Delete MBMS Context request messages transmitted. Type: Counter | Int32 14.0 and later: Int64
dmc-tx-accept | The total number of Delete MBMS Context request messages accepted by the SGSN. Type: Counter | Int32 14.0 and later: Int64
dmc-tx-deny | The total number of Delete MBMS Context request messages denied by the SGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-reg-req-total | The total number of MBMS Registration Request messages received. Type: Counter | Int32 14.0 and later: Int64
mbms-reg-req-initial | The total number of initial MBMS Registration Request messages received. Type: Counter | Int32 14.0 and later: Int64
mbms-reg-req-retrans | The total number of retransmitted MBMS Registration Request messages received. Type: Counter | Int32 14.0 and later: Int64
mbms-reg-req-accept | The total number of MBMS Registration Request messages accepted by the GGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-reg-req-deny | The total number of MBMS Registration Request messages denied by the GGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-reg-req-discard | The total number of MBMS Registration Request messages discarded by the GGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-ses-start-tx | The total number of MBMS Session Start Request messages transmitted. Type: Counter | Int32 14.0 and later: Int64
mbms-ses-start-tx-accept | The total number of MBMS Session Start Request messages accepted by the SGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-ses-start-tx-deny | The total number of MBMS Session Start Request messages denied by the SGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-ses-stop-tx | The total number of MBMS Session Stop Request messages transmitted. Type: Counter | Int32 14.0 and later: Int64
mbms-ses-stop-tx-accept | The total number of MBMS Session Stop Request messages accepted by the SGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-ses-stop-tx-deny | The total number of MBMS Session Stop Request messages denied by the SGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-dereg-rx | The total number of MBMS De-Registration Request messages received. Type: Counter | Int32 14.0 and later: Int64
mbms-dereg-rx-accept | The total number of MBMS De-Registration Request messages accepted by the GGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-dereg-rx-deny | The total number of MBMS De-Registration Request messages denied by the GGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-dereg-rx-discard | The total number of MBMS De-Registration Request messages discarded by the GGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-dereg-tx | The total number of MBMS De-Registration Request messages transmitted. Type: Counter | Int32 14.0 and later: Int64
mbms-dereg-tx-accept | The total number of MBMS De-Registration Request messages accepted by the SGSN. Type: Counter | Int32 14.0 and later: Int64
mbms-dereg-tx-deny | The total number of MBMS De-Registration Request messages denied by the SGSN. Type: Counter | Int32 14.0 and later: Int64
sess-in-preservation-mode | The total number of sessions in Preservation-Mode. This is a customer specific support only. Type: Counter | Int32 14.0 and later: Int64
transition-to-preservation-mode | The total number of sessions in transition from Non-Preservation mode (normal mode) to Preservation-Mode. This is a customer specific support only. Type: Counter | Int32 14.0 and later: Int64
transition-to-non-preservation-mode | The total number of sessions in transition from Preservation Mode to normal mode. This is a customer specific support only. Type: Counter | Int32 14.0 and later: Int64
sess-in-lorc | Indicates the number of GGSN session are in LORC state and subscriber is in out of radio coverage area. This counter is applicable when GGSN is enabled for overcharging protection for subscriber due to loss of radio coverage and SGSN notifies Update PDP Contexts for QOS change with GTP-C extension for LORC. Type: Counter | Int32 14.0 and later: Int64
transition-to-lorc | Indicates total number sessions in transitions state for overcharging protection support mode. This counter is applicable when GGSN is enabled for overcharging protection for subscriber due to loss of radio coverage and SGSN notifies Update PDP Contexts for QOS change with GTP-C extension for LORC. Type: Counter | Int32 14.0 and later: Int64
sess-in-focs | Total number of session Free of charge service. Type: Counter | Int32 14.0 and later: Int64
cnt-of-release-due-to-other | Total number of session release due to reasons other than listed in this table. Type: Counter | Int32 14.0 and later: Int64
cnt-of-release-due-to-violation | Total number of session release due to service violation. Type: Counter | Int32 14.0 and later: Int64
sess-in-odb | Indicates the total number of sessions with Operator Determined Barring enabled status. Type: Counter | Int32 14.0 and later: Int64
cnt-of-release-due-to-violation-odb | Indicates the statistics for sessions, with Operator Determined Barring enabled status, released due to violation of ODB conditions. Type: Counter | Int32 14.0 and later: Int64
cnt-of-release-due-to-other-odb | Indicates the total number of sessions, with Operator Determined Barring enabled status, released due to reasons not specified in this table. Type: Counter | Int32 14.0 and later: Int64
ipca-pdp-context-tx | Total number of PDP context activation requests sent for an Initiate PDP Context Activation. Type: Counter | Int32 14.0 and later: Int64
ipca-pdp-context-tx-accepted | Total number of PDP context activation requests sent and accepted for an Initiate PDP Context Activation. Type: Counter | Int32 14.0 and later: Int64
ipca-pdp-context-tx-denied | Total number of PDP context activation requests denied for an Initiate PDP Context Activation. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-no-resources | Total number of Initiate PDP Context Activation reject messages received due to no resource available on remote node. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-no-mem-avail | Total number of Initiate PDP Context Activation reject messages received due to no memory available on remote node. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-sys-failure | Total number of Initiate PDP Context Activation reject messages received due to system failure on remote node. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-non-existent | Total number of Initiate PDP Context Activation reject messages received due to non-existent session/subscriber on remote node. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-unsupported-service | Total number of Initiate PDP Context Activation reject messages received as service is not supported on on remote node. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-invalid-msg-format | Total number of Initiate PDP Context Activation reject messages received due to invalid message format. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-semantic-err-in-tft | Total number of Initiate PDP Context Activation reject messages received due to semantic error in Traffic Flow Template (TFT). Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-syntactic-err-in-tft | Total number of Initiate PDP Context Activation reject messages received due to syntactic error in Traffic Flow Template (TFT) Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-man-ie-incorrect | Total number of Initiate PDP Context Activation reject messages received due to incorrect information in mandatory information elements (IEs). Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-semantic-err-in-pac-filter | Total number of Initiate PDP Context Activation reject messages received due to semantic error in PAC filter. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-man-ie-missing | Total number of Initiate PDP Context Activation reject messages received as mandatory information element (IE) is missing. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-optional-ie-incorrect | Total number of Initiate PDP Context Activation reject messages received due to incorrect information in optional information elements (IEs). Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-syntactic-err-in-pac-filter | Total number of Initiate PDP Context Activation reject messages received due to syntactic error in PAC filter. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-ue-not-gprs-rsp | Total number of Initiate PDP Context Activation reject messages received as UE is not capable or subscribed to GPRS service. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-ue-refuses | Total number of Initiate PDP Context Activation reject messages received due to refusal from UE. Type: Counter | Int32 14.0 and later: Int64
ipca-reject-rx-invalid-correlation-id | Total number of Initiate PDP Context Activation reject messages received due to invalid correlation identifier. Type: Counter | Int32 14.0 and later: Int64
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.