# SS7 Routing Domain Schema Statistics

The SS7 Routing Domain schema provides operational statistics that can be used for monitoring and troubleshooting the following products: SGSN
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. SS7 Routing Domain Statistics

Variables | Description | Data Type
--- | --- | ---
ss7rd-number | Number identifying the SS7 routing domain This is a key variable. | Int32
ss7rd-asp_instance | The Application Server Process instance in the SS7 Routing domain This is a key variable. | Int32
ss7rd-sctp-init-tx | Total number of SCTP Init chunks sent per SS7 Routing Domain. | Int32
ss7rd-sctp-init-rtx | Total number of SCTP Init chunks resent per SS7 Routing Domain. | Int32
ss7rd-sctp-init-rx | Total number of SCTP Init chunks received per SS7 Routing Domain. | Int32
ss7rd-sctp-init-ack-tx | Total number of number INIT_ACKs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-init-ack-rx | Total number of number INIT_ACKs received per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-tx | Total number SHUTDOWNs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-rtx | Total number SHUTDOWNs resent per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-rx | Total Number SHUTDOWNs received per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-ack-tx | Total number of SHUTDOWN_ACKs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-ack-rtx | Total number of SHUTDOWN_ACKSs resent per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-ack-rx | Total number of SHUTDOWN_ACKs received per SS7 Routing Domain. | Int32
ss7rd-sctp-cookie-tx | Total number of COOKIEs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-cookie-rtx | Total number COOKIEs resent per SS7 Routing Domain. | Int32
ss7rd-sctp-cookie-rx | Total number of COOKIEs received per SS7 Routing Domain. | Int32
ss7rd-sctp-cookie-ack-tx | Total number of COOKIE_ACKs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-cookie-ack-rx | Total number COOKIE_ACKs received per SS7 Routing Domain. | Int32
ss7rd-sctp-data-tx | Total number of DATAs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-data-rtx | Total number of DATAs resent per SS7 Routing Domain. | Int32
ss7rd-sctp-data-rx | Total number of DATAs received per SS7 Routing Domain. | Int32
ss7rd-sctp-sack-tx | Total number of SACKs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-sack-rx | Total number of SACKs received per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-compl-tx | Total number of Shutdown completed sent per SS7 Routing Domain. | Int32
ss7rd-sctp-shutdown-compl-rx | Total number of Shutdown completed received per SS7 Routing Domain. | Int32
ss7rd-sctp-heartbeat-tx | Total number of HEARTBEATs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-heartbeat-rx | Total number of HEARTBEATs received per SS7 Routing Domain. | Int32
ss7rd-sctp-heartbeat-ack-tx | Total number of HBEAT_ACKs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-heartbeat-ack-rx | Total number of HBEAT_ACKs received per SS7 Routing Domain. | Int32
ss7rd-sctp-abort-tx | Total number of ABORTs sent per SS7 Routing Domain. | Int32
ss7rd-sctp-abort-rx | Total number of ABORTs received per SS7 Routing Domain. | Int32
ss7rd-sctp-error-tx | Total number of Errors sent per SS7 Routing Domain. | Int32
ss7rd-sctp-error-rx | Total number of Errors received per SS7 Routing Domain. | Int32
ss7rd-sctp-bytes-tx | Total number of bytes sent per SS7 Routing Domain. | Int32
ss7rd-sctp-bytes-rx | Total number of bytes received per SS7 Routing Domain. | Int32
ss7rd-m3ua-data-tx | Total number of M3UA DATA messages sent | Int32
ss7rd-m3ua-duna-tx | Total number of M3UA DUNA messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-dava-tx | Total number of M3UA DAVA messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-daud-tx | Total number of M3UA DAUD messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-scon-tx | Total number of M3UA SCON messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-dupu-tx | Total number of M3UA DUPU messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-drst-tx | Total number of M3UA DRST messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-regreq-tx | Total number of M3UA REG-REQ messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-regrsp-tx | Total number of M3UA REG-RSP messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-deregreq-tx | Total number of M3UA DEREG-REQ messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-deregrsp-tx | Total number of M3UA DEREG-RSP messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspup-tx | Total number of M3UA ASPUP messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspup-ack-tx | Total number of M3UA ASPUP ACK messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspdn-tx | Total number of M3UA ASPDN messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspdn-ack-tx | Total number of M3UA ASPDN ACK messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspac-tx | Total number of M3UA ASPAC messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspac-ack-tx | Total number of M3UA ASPAC ACK messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspia-tx | Total number of M3UA ASPIA messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspia-ack-tx | Total number of M3UA ASPIA ACK messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-hearbeat-tx | Total number of M3UA HBEAT messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-hearbeat-ack-tx | Total number of M3UA HBEAT ACK messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-error-tx | Total number of M3UA ERR messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-notify-tx | Total number of M3UA NTFY messages sent per SS7 Routing Domain. | Int32
ss7rd-m3ua-data-rx | Total number of M3UA DATA messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-duna-rx | Total number of M3UA DUNA messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-dava-rx | Total number of M3UA DAVA messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-daud-rx | Total number of M3UA DAUD messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-scon-rx | Total number of M3UA SCON messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-dupu-rx | Total number of M3UA DUPU messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-drst-rx | Total number of M3UA DRST messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-regreq-rx | Total number of M3UA REG-REQ messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-regrsp-rx | Total number of M3UA REG-RSP messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-deregreq-rx | Total number of M3UA DEREG-REQ messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-deregrsp-rx | Total number of M3UA DEREG-RSP messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspup-rx | Total number of M3UA ASPUP messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspup-ack-rx | Total number of M3UA ASPUP ACK messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspdn-rx | Total number of M3UA ASPDN messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspdn-ack-rx | Total number of M3UA ASPDN ACK messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspac-rx | Total number of M3UA ASPAC messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspac-ack-rx | Total number of M3UA ASPAC ACK messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspia-rx | Total number of M3UA ASPIA messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-aspia-ack-rx | Total number of M3UA ASPIA ACK messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-hearbeat-rx | Total number of M3UA HBEAT messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-hearbeat-ack-rx | Total number of M3UA HBEAT ACK messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-error-rx | Total number of M3UA ERR messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-notify-rx | Total number of M3UA NTFY messages received per SS7 Routing Domain. | Int32
ss7rd-m3ua-lower-intf-pdu-tx | Description: Total number of PDUs transmitted to lower interface (SCTP layer). Triggers: Availability: per SS7 routing domain Type: Counter (Proprietary) | Int32
ss7rd-m3ua-lower-intf-pdusize-tx | Size of DATA PDUs transmitted on lower interface per SS7 Routing Domain. | Int32
ss7rd-m3ua-lower-intf-pdu-rx | Number of DATA PDUs received on lower interface per SS7 Routing Domain. | Int32
ss7rd-m3ua-lower-intf-pdusize-rx | Size of DATA PDUs received on lower interface per SS7 Routing Domain. | Int32
ss7rd-m3ua-upper-intf-pdu-tx | Number of DATA PDUs transmitted on upper interface per SS7 Routing Domain. | Int32
ss7rd-m3ua-upper-intf-pdusize-tx | Size of DATA PDUs transmitted on upper interface per SS7 Routing Domain. | Int32
ss7rd-m3ua-upper-intf-pdu-rx | Number of DATA PDUs received on upper interface per SS7 Routing Domain. | Int32
ss7rd-m3ua-upper-intf-pdusize-rx | Size of DATA PDUs received on upper interface per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-no-route-found | Layer Data Error Statistics downward: no route found per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-pc-unvailable | Layer Data Error Statistics downward: point code unavailable per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-pc-congested | Layer Data Error Statistics downward: point code congested per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-no-psp-avail | Layer Data Error Statistics downward: no PSP available per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-no-nsap-avail | Layer Data Error Statistics downward: no NSAP available per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-msg-failed | Layer Data Error Statistics downward: M3UA message failed per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-loadshare-failed | Layer Data Error Statistics downward: load-sharing failed per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-data-conges-q | Layer Data Error Statistics downward: data queued in congested Q per SS7 Routing Domain. | Int32
ss7rd-m3ua-down-data-as-pend-q | Layer Data Error Statistics downward: data queued in AS pending Q per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-no-route-found | Layer Data Error Statistics upward: no route found per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-pc-unvailable | Layer Data Error Statistics upward: point code unavailable per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-pc-congested | Layer Data Error Statistics upward: point code congested per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-no-psp-avail | Layer Data Error Statistics upward: no PSP available per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-no-nsap-avail | Layer Data Error Statistics upward: no NSAP available per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-msg-failed | Layer Data Error Statistics upward: M3UA message failed per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-loadshare-failed | Layer Data Error Statistics upward: load-sharing failed per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-data-conges-q | Layer Data Error Statistics upward: data queued in congested Q per SS7 Routing Domain. | Int32
ss7rd-m3ua-up-data-as-pend-q | Layer Data Error Statistics upward: data queued in AS pending Q per SS7 Routing Domain. | Int32
ss7rd-m3ua-psp-ps-id | Peer Server Identifier This is a key variable. | Int32
ss7rd-m3ua-psp-instance | Peer Server Process Instance This is a key variable. | Int32
ss7rd-m3ua-psp-data-tx | Total number of M3UA PSP DATA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-duna-tx | Total number of M3UA PSP DUNA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-dava-tx | Total number of M3UA PSP DAVA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-daud-tx | Total number of M3UA PSP DAUD messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-scon-tx | Total number of M3UA SCON messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-dupu-tx | Total number of M3UA PSP DUPU messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-drst-tx | Total number of M3UA PSP DRST messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-regreq-tx | Total number of M3UA PSP REG-REQ messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-regrsp-tx | Total number of M3UA PSP REG-RSP messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-deregreq-tx | Total number of M3UA PSP DEREG-REQ messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-deregrsp-tx | Total number of M3UA PSP DEREG-RSP messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspup-tx | Total number of M3UA PSP ASPUP messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspup-ack-tx | Total number of M3UA PSP ASPUP ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspdn-tx | Total number of M3UA PSP ASPDN messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspdn-ack-tx | Total number of M3UA PSP ASPDN ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspac-tx | Total number of M3UA PSP ASPAC messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspac-ack-tx | Total number of M3UA PSP ASPAC ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspia-tx | Total number of M3UA PSP ASPIA messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspia-ack-tx | Total number of M3UA PSP ASPIA ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-hearbeat-tx | Total number of M3UA PSP HBEAT messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-hearbeat-ack-tx | Total number of M3UA PSP HBEAT ACK messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-error-tx | Total number of M3UA PSP ERR messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-notify-tx | Total number of M3UA PSP NTFY messages sent per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-data-rx | Total number of M3UA PSP DATA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-duna-rx | Total number of M3UA PSP DUNA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-dava-rx | Total number of M3UA PSP DAVA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-daud-rx | Total number of M3UA PSP DAUD messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-scon-rx | Total number of M3UA PSP SCON messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-dupu-rx | Total number of M3UA PSP DUPU messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-drst-rx | Total number of M3UA PSP DRST messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-regreq-rx | Total number of M3UA PSP REG-REQ messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-regrsp-rx | Total number of M3UA PSP REG-RSP messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-deregreq-rx | Total number of M3UA PSP DEREG-REQ messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-deregrsp-rx | Total number of M3UA DEREG-RSP messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspup-rx | Total number of M3UA PSP ASPUP messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspup-ack-rx | Total number of M3UA PSP ASPUP ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspdn-rx | Total number of M3UA PSP ASPDN messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspdn-ack-rx | Total number of M3UA PSP ASPDN ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspac-rx | Total number of M3UA PSP ASPAC messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspac-ack-rx | Total number of M3UA PSP ASPAC ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspia-rx | Total number of M3UA PSP ASPIA messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-aspia-ack-rx | Total number of M3UA PSP ASPIA ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-hearbeat-rx | Total number of M3UA PSP HBEAT messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-hearbeat-ack-rx | Total number of M3UA PSP HBEAT ACK messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-error-rx | Total number of M3UA PSP ERR messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-notify-rx | Total number of M3UA PSP NTFY messages received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-data-pdu-tx | Number of PSP DATA PDUs transmitted per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-data-pdusize-tx | Size of DATA PDUs transmitted per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-data-pdu-rx | Number of DATA PDUs received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-data-pdusize-rx | Size of DATA PDUs received per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-no-route-found | Layer Data Error Statistics: no route found per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-pc-unvailable | Layer Data Error Statistics: point code unavailable per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-pc-congested | Layer Data Error Statistics: point code congested per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-no-psp-avail | Layer Data Error Statistics: no PSP available per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-no-nsap-avail | Layer Data Error Statistics: no NSAP available per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-msg-failed | Layer Data Error Statistics: M3UA message failed per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-loadshare-failed | Layer Data Error Statistics: load-sharing failed per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-data-conges-q | Layer Data Error Statistics: data queued in congested Q per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-up-data-as-pend-q | Layer Data Error Statistics: data queued in AS pending Q per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-congestion-count | Congestion count per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-congestion-level1 | Congestion level 1 per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-congestion-level2 | Congestion level 2 per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-congestion-level3 | Congestion level 3 per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-congestion-queue-size | Congestion queue size per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-congestion-queue-hw | Congestion queue Hw per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-congestion-duration | Duration of Congestion per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-unvailable-count | Unavailable count per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-m3ua-psp-unvailable-duration | Unavailable duration per SS7 Routing Domain, peer server ID, and PSP instance. | Int32
ss7rd-mtp3-user-part-unavail-tx | Description: Total number of MTP3 User-part Unavailable messages that were sent. Triggers: Increments when a message is sent. Availability: per SS7 routing domain Type: Counter (ITU Q.704, ANSI T1.114) | Int32
ss7rd-mtp3-traffic-restart-allowed-tx | Description: Total number of MTP3 Traffic Restart Allowed messages that were sent. Triggers: Increments when the first signalling link of a signalling linkset is available. in the case of an ANSI variant, when a Traffic Restart Waiting message is received. Availability: per SS7 routing domain Type: Counter (ITU Q.704, ANSI T1.114) | Int32
ss7rd-mtp3-traffic-restart-waiting-tx | Description: Total number of MTP3 Traffic Restart Waiting messages that were sent. Triggers: Increments when the first signalling link of a signalling link set is available. Availability: per SS7 routing domain Type: Counter (ITU Q.704, ANSI T1.114) | Int32
ss7rd-mtp3-user-part-unavail-rx | Description: Total number of MTP3 User-part Unavailable messages that were received. Triggers: Increments when a message is received. Availability: per SS7 routing domain Type: Counter (ITU Q.704, ANSI T1.114) | Int32
ss7rd-mtp3-traffic-restart-allowed-rx | Description: Total number of MTP3 Traffic Restart Allowed messages that were received. Triggers: Increments when a message is received. Availability: per SS7 routing domain Type: Counter (ITU Q.704, ANSI T1.114) | Int32
ss7rd-mtp3-traffic-restart-waiting-rx | Description: Total number of MTP3 Traffic Restart Waiting messages that were received. Triggers: Incremenets when a message is received. Availability: per SS7 routing domain Type: Counter (ITU Q.704, ANSI T1.114) | Int32
ss7rd-mtp3-msu-dropped-routing-err | Description: Total number of M3UA messages dropped due to routing error. Triggers: Increments for anyone of the following: signalling point code restart, route restart, no route found, no NSAP found, invalid SLS, invalid link type, invalid data. Availability: per SS7 routing domain Type: Counter - Proprietary | Int32
ss7-adjacent-point-code | Adjacent Point Code This is a key variable. | Int32
ss7-adjacent-spc-not-accessible | Description: Total number of failures to access the adjacent (directly connected via SS7 link) signaling point code (SPC) element, such as the RNC, HLR, signaling gateway, etc.,. Triggers: Increments when the adjacent SPC goes to unavailable state from available state, possibly due to: - all SS7 links connected to the adjacent SPC are unavailable - the adjacent SPC is made inaccessible by management Availability: per adjacent point code Type: Counter | Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.