# ASNPC Schema Statistics

The ASNPC schema provides operational statistics that can be used for monitoring and troubleshooting the following products: ASNPC
This schema provides the following types of statistics:

- Counter: A counter records incremental data cumulatively and rolls over when the counter limit is reached. All counter statistics are cumulative and reset only by one of the following methods: roll-over when limit is reached, after a system restart, or after a clear command is performed. The limit depends upon the data type.
- Gauge: A gauge statistic indicates a single value; a snapshot representation of a single point in time within a defined time frame. The gauge changes to a new value with each snapshot though a value may repeat from one period to the next. The limit depends upon the data type.
- Information: This type of statistic provides information, often intended to differentiate sets of statistics; for example, a VPN name or IP address. The type of information provided depends upon the data type.

The data type defines the format of the data for the value provided by the statistic. The following data types are used in statistics for this schema:

- Int32/Int64: An integer, either 32-bit or 64-bit: For statistics with the Int32 data type, the roll-over to zero limit is 4,294,967,295. For statistics with the Int64 data type, the roll-over to zero limit is 18,446,744,073,709,551,615.
- Float: A numeric value that can be represented fractionally; for example, 1.345.
- String: A series of ASCII alphanumeric characters in a single grouping, usually pre-configured.

IMPORTANT:

Unless otherwise indicated, all statistics are counters and all statistics are standards-based.

Key Variables: Every schema has some variables which are typically referred to as 'key variables'. These key variables provide index markers to identify which object the statistics apply to. For example, in the card schema, the card number (variable %card%) uniquely identifies a card. For an HA service, the keys would be "%vpnname%" plus "%servname%", as the combination uniquely identifies an HA service. So, in a given measurement interval, one row of statistics will be generated per unique key. The schema keys are identified in the Description section of the table.
Table 1. Bulk Statistic Variables in the ASN-PC Schema

Variables | Description | Data Type
--- | --- | ---
vpnname | The name of the context configured on the system that is currently facilitating the ASN PC service. This is a key variable. | String
vpnid | The identification number of the context configured on the system that is currently facilitating the ASN PC service. This is an internal reference number. This is a key variable. | Int32
servname | The name of the ASN PC service for which the statistics are displayed. This is a key variable. | String
servid | The identification number of the ASN PC service for which the statistics are displayed. This is a key variable. | Int32
r6imentstachareq-totsent | The number of Idle Mode Entry State Change Requests sent to the base station on the R6 interface. | Int32
r6imentstachareq-retranssent | The total number of Idle Mode Entry State Change Requests re-transmitted on R6 the interface to the base station. | Int32
r6imentstachareq-totsendfail | The total number of failures that occurred during transaction ID generation of R6 Idle Mode Entry State Change Request messages. This counter is used to count the error while sending the R6 packets. | Int32
r6imentstachareq-totrec | The total number of Idle Mode Entry State Change Request messages received on R6 interface. | Int32
r6imentstachareq-totacc | The total number of Idle Mode Entry State Change Request messages accepted on R6 interface. | Int32
r6imentstachareq-totrelay | The total number of Idle Mode Entry State Change Requests messages relayed to the base station on the R6 interface. Triggers: Changes every time an Idle Mode Entry State Change Request message is relayed over the R6 interface. Availability: across all ASNGW services. | Int32
r6imentstachareq-totdenied | The total number of Idle Mode Entry State Change Request messages denied on R6 interface. | Int32
r6imentstachareq-totdiscard | The total number of Idle Mode Entry State Change Request messages discarded on R6 interface. | Int32
r6imentstachareq-badform | The total number of Idle Mode Entry State Change Request messages sent on the R6 interface. | Int32
r6imentstachareq-decodeerr | The total number of Idle Mode Entry State Change Request messages on R6 interface with decode error. | Int32
r6imentstachareq-unspecerr | The total number of Idle Mode Entry State Change Request messages on R6 interface with unspecified error. | Int32
r6imentstachareq-missmandtlv | The total number of Idle Mode Entry State Change Request messages on R6 interface with missing mandatory TLVs. | Int32
r6imentstachareq-tlvvalinval | The total number of Idle Mode Entry State Change Request messages on R6 interface with invalid TLV value. | Int32
r6imentstachareq-unknowntlv | The total number of Idle Mode Entry State Change Request messages on R6 interface with unknown TLVs. | Int32
r6imentstachareq-duptlvfound | The total number of Idle Mode Entry State Change Request messages on R6 interface with duplicate TLVs. | Int32
r6imentstachareq-nosessfound | The total number of Idle Mode Entry State Change Request messages on R6 interface without any session information. | Int32
r6imentstachareq-admprohibit | The total number of Idle Mode Entry State Change Request messages on R6 interface with transaction ID errors. | Int32
r6imentstachareq-noresourcedrop | The total number of Idle Mode Entry State Change Request messages discarded or denied due to admin prohibit. Triggers: Changes every time an Idle Mode Entry State Change Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6imentstachareq-transiderr | The total number of Idle Mode Entry State Change Request messages discarded or denied due to transaction ID errors | Int32
r6imentstacharsp-totsent | The total number of Idle Mode Entry State Change Responses sent to the Base Station. | Int32
r6imentstacharsp-retranssent | The total number of Idle Mode Entry State Change Responses re-transmitted on R6 the interface. | Int32
r6imentstacharsp-totsendfail | The total number of failures that occurred during transaction ID generation of R6 Idle Mode Entry State Change Response messages. This counter is used to count the error while sending the R6 packets. | Int32
r6imentstacharsp-totrec | The total number of Idle Mode Entry State Change Response messages received on R6 interface. | Int32
r6imentstacharsp-totacc | The total number of Idle Mode Entry State Change Response messages accepted on R6 interface. | Int32
r6imentstacharsp-totrelay | The total number of Idle Mode Entry State Change Response messages relayed to the base station on the R6 interface. Triggers: Changes every time an Idle Mode Entry State Change Response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6imentstacharsp-totdenied | The total number of Idle Mode Entry State Change Response messages denied on R6 interface. | Int32
r6imentstacharsp-totdiscard | The total number of Idle Mode Entry State Change Response messages discarded on R6 interface. | Int32
r6imentstacharsp-badform | The total number of Idle Mode Entry State Change Response messages sent on the R6 interface. | Int32
r6imentstacharsp-decodeerr | The total number of Idle Mode Entry State Change Response messages on R6 interface with decode error. | Int32
r6imentstacharsp-unspecerr | The total number of Idle Mode Entry State Change Response messages on R6 interface with unspecified error. | Int32
r6imentstacharsp-missmandtlv | The total number of Idle Mode Entry State Change Response messages on R6 interface with missing mandatory TLVs. | Int32
r6imentstacharsp-tlvvalinval | The total number of Idle Mode Entry State Change Response messages on R6 interface with invalid TLV value. | Int32
r6imentstacharsp-unknowntlv | The total number of Idle Mode Entry State Change Response messages on R6 interface with unknown TLVs. | Int32
r6imentstacharsp-duptlvfound | The total number of Idle Mode Entry State Change Response messages on R6 interface with duplicate TLVs | Int32
r6imentstacharsp-nosessfound | The total number of Idle Mode Entry State Change Response messages on R6 interface without any session information. | Int32
r6imentstacharsp-admprohibit | The total number of Idle Mode Entry State Change Response messages on R6 interface with transaction ID errors. | Int32
r6imentstacharsp-noresourcedrop | The total number of Idle Mode Entry State Change Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an Idle Mode Entry State Change Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6imentstacharsp-transiderr | The total number of Idle Mode Entry State Change Response messages discarded or denied due to transaction ID errors | Int32
r6imentstachaack-totsent | The total number of Idle Mode Entry State Change Acknowledgements sent to the Base Station. | Int32
r6imentstachaack-retranssent | The total number of Idle Mode Entry State Change Acknowledgement messages re-transmitted on R6 interface. | Int32
r6imentstachaack-totsendfai | The total number of R6 idle Mode Entry State Change Acknowledgement messages sent to the base station. This counter is used to count the error while sending the R6 packets. | Int32
r6imentstachaack-totrec | The total number of R6 Idle Mode Entry State Change Acknowledgement messages received on R6 interface. | Int32
r6imentstachaack-totacc | The total number of R6 Idle Mode Entry State Change Acknowledgement messages accepted on R6 interface. | Int32
r6imentstachaack-totrelay | The total number of R6 Idle Mode Entry State Change Acknowledgement messages relayed to the base station on the R6 interface. Triggers: Changes every time an R6 Idle Mode Entry State Change Acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6imentstachaack-totdenied | The total number of R6 Idle Mode Entry State Change Acknowledgement messages denied on R6 interface. | Int32
r6imentstachaack-totdiscard | The total number of R6 Idle Mode Entry State Change Acknowledgement messages discarded on R6 interface. | Int32
r6imentstachaack-badform | The total number of badly formed R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface. | Int32
r6mentstachaack-decodeerr | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface with decode error. | Int32
r6imentstachaack-unspecerr | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface with unspecified error. | Int32
r6imentstachaack-missmandtlv | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface with missing mandatory TLVs. | Int32
r6imentstachaack-tlvvalinval | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface with invalid TLV value | Int32
r6imentstachaack-unknowntlv | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface with unknown TLVs | Int32
r6imentstachaack-duptlvfound | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface with duplicate TLVs. | Int32
r6imentstachaack-nosessfound | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface without any session information. | Int32
r6imentstachaack-adminprohib | The total number of R6 Idle Mode Entry State Change Acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Idle Mode Entry State Change Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6imentstachaack-noresourcedrop | The total number of R6 Idle Mode Entry State Change Acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Idle Mode Entry State Change Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6imentstachaack-transiderr | The total number of R6 Idle Mode Entry State Change Acknowledgement messages on R6 interface with transaction ID errors. | Int32
r6imexitstachareq-totsent | The total number of Idle Mode Exit State Change Requests sent to the Base Station. | Int32
r6imexitstachareq-retranssent | The total number of R6 Idle Mode Exit State Change Request messages sent to the base station. | Int32
r6imexitstachareq-totsendfail | The total number of R6 Idle Mode Exit State Change Request messages sent to the base station. This counter is used to count the error while sending the R6 packets. | Int32
r6imexitstachareq-totrec | The total number of R6 Idle Mode Exit State Change Request messages received on R6 interface. | Int32
r6imexitstachareq-totacc | The total number of R6 Idle Mode Exit State Change Request messages accepted on R6 interface. | Int32
r6imexitstachareq-totrelay | The total number of R6 Idle Mode Exit State Change Request messages relayed to the base station on the R6 interface. Triggers: Changes every time an R6 Idle Mode Exit State Change Request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6imexitstachareq-totdenied | The total number of R6 Idle Mode Exit State Change Request messages denied on R6 interface. | Int32
r6imexitstachareq-totdiscard | The total number of R6 Idle Mode Exit State Change Request messages discarded on R6 interface. | Int32
r6imexitstachareq-badform | The total number of badly formed R6 Idle Mode Exit State Change Request messages on R6 interface. | Int32
r6imexitstachareq-decodeerr | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface with decode error. | Int32
r6imexitstachareq-unspecerr | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface with unspecified error. | Int32
r6imexitstachareq-missmandtlv | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface with missing mandatory TLVs. | Int32
r6imexitstachareq-tlvvalinval | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface with invalid TLV value | Int32
r6imexitstachareq-unknowntlv | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface with unknown TLVs | Int32
r6imexitstachareq-duptlvfound | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface with duplicate TLVs. | Int32
r6imexitstachareq-nosessfound | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface without any session information. | Int32
r6imexitstachareq-admprohibit | The total number of R6 Idle Mode Exit State Change Request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Idle Mode Exit State Change Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6imexitstachareq-noresourcedrop | The total number of R6 Idle Mode Exit State Change Request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Idle Mode Exit State Change Request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6imexitstachareq-transiderr | The total number of R6 Idle Mode Exit State Change Request messages on R6 interface with transaction ID errors. | Int32
r6imexitstacharsp-totsent | The total number of Idle Mode Exit State Change Responses sent to the Base Station. | Int32
r6imexitstacharsp-retranssent | The total number of R6 Idle Mode Exit State Change Response messages re-transmitted on R6 interface. | Int32
r6imexitstacharsp-totsendfail | The total number of failed R6 idle Mode Exit State Change Response messages sent to the base station. This counter is used to count the error while sending the R6 packets. | Int32
r6imexitstacharsp-totrec | The total number of R6 Idle Mode Exit State Change Response messages received on R6 interface. | Int32
r6imexitstacharsp-totacc | The total number of R6 Idle Mode Exit State Change Response messages accepted on R6 interface. | Int32
r6imexitstacharsp-totrelay | The total number of R6 Idle Mode Exit State Change Response messages relayed to the base station on the R6 interface. Triggers: Changes every time an R6 Idle Mode Exit State Change Response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6imexitstacharsp-totdenied | The total number of R6 Idle Mode Exit State Change Response messages denied on R6 interface. | Int32
r6imexitstacharsp-totdiscard | The total number of R6 Idle Mode Exit State Change Response messages discarded on R6 interface. | Int32
r6imexitstacharsp-badform | The total number of badly formed R6 Idle Mode Exit State Change Response messages on R6 interface. | Int32
r6imexitstacharsp-decodeerr | The total number of R6 Idle Mode Exit State Change Response messages on R6 interface with decode error. | Int32
r6imexitstacharsp-unspecerr | The total number of R6 Idle Mode Exit State Change Response messages on R6 interface with unspecified error. | Int32
r6imexitstacharsp-missmandtlv | The total number of R6 Idle Mode Exit State Change Response messages on R6 interface with missing mandatory TLVs. | Int32
r6imexitstacharsp-unknowntlv | The total number of R6 Idle Mode Exit State Change Response messages on R6 interface with an unknown TLV value. | Int32
r6imexitstacharsp-duptlvfound | The total number of R6 Idle Mode Exit State Change Response messages on R6 interface with duplicate TLVs. | Int32
r6imexitstacharsp-nosessfound | The total number of R6 Idle Mode Exit State Change Response messages on R6 interface without any session information. | Int32
r6imexitstacharsp-admprohibit | The total number of R6 Idle Mode Exit State Change Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Idle Mode Exit State Change Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6imexitstacharsp-noresourcedrop | The total number of R6 Idle Mode Exit State Change Response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Idle Mode Exit State Change Response message is discarded or denied due to resource unavailability. Availability: across all ASNGW services. | Int32
r6imexitstacharsp-transiderr | The total number of R6 Idle Mode Exit State Change Response messages with translation ID errors. | Int32
r6locupdreq-totsent | The total number of R6 Location Update Request messages sent to the base station. | Int32
r6locupdreq-retranssent | The total number of R6 Location Update Request messages re-transmitted on R6 interface. | Int32
r6locupdreq-totsendfail | The total number of failed R6 Location Update Request messages sent to the base station. This counter is used to count the error while sending the R6 packets. | Int32
r6locupdreq-totrec | The total number of R6 Location Update Request Location Update Request messages received on R6 interface. | Int32
r6locupdreq-totacc | The total number of R6 Location Update Request messages accepted on R6 interface. | Int32
r6locupdreq-totrelay | The total number of R6 Location Update Request messages relayed to the base station on the R6 interface. Triggers: Changes every time an R6 Location Update Request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6locupdreq-totdenied | The total number of R6 Location Update Request messages denied on R6 interface. | Int32
r6locupdreq-totdiscard | The total number of R6 Location Update Request messages discarded on R6 interface. | Int32
r6locupdreq-badform | The total number of badly formed R6 Location Update Request messages on R6 interface. | Int32
r6locupdreq-decodeerr | The total number of R6 Location Update Request messages on R6 interface with decode errors. | Int32
r6locupdreq-unspecerr | The total number of R6 Location Update Request messages on R6 interface with unspecified error. | Int32
r6locupdreq-missmandtlv | The total number of R6 Location Update Request messages on R6 interface with missing mandatory TLVs. | Int32
r6locupdreq-tlvvalinval | The total number of R6 Location Update Request messages on R6 interface with an unknown TLV value. | Int32
r6locupdreq-unknowntlv | The total number of R6 Location Update Request messages on R6 interface with unknown TLVs. | Int32
r6locupdreq-duptlvfound | The total number of R6 Location Update Request messages on R6 interface with duplicate TLVs. | Int32
r6locupdreq-nosessfound | The total number of R6 Location Update Request messages without any session information. | Int32
r6locupdreq-admprohibit | The total number of R6 Location Update Request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Location Update Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6locupdreq-noresourcedrop | The total number of R6 Location Update Request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Location Update Request message is discarded or denied due to resource unavailability. Availability: across all ASNGW services. | Int32
r6locupdreq-transiderr | The total number of R6 Location Update Request messages with translation ID errors. | Int32
r6locupdrsp-totsent | The total number of Location Update Responses sent to the Base Station. | Int32
r6locupdrsp-totsendfail | The total number of failed R6 Location Update Response messages sent on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int32
r6locupdrsp-totrec | The total number of R6 Location Update Response messages received on R6 interface. | Int32
r6locupdrsp-totacc | The total number of R6 Location Update Response messages accepted on R6 interface. | Int32
r6locupdrsp-totrelay | The total number of R6 Location Update Response messages relayed to the base station on the R6 interface. Triggers: Changes every time an R6 Location Update Response message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6locupdrsp-totdenied | The total number of R6 Location Update Response messages denied on R6 interface. | Int32
r6locupdrsp-totdiscard | The total number of R6 Location Update Response messages discarded on R6 interface. | Int32
r6locupdrsp-badform | The total number of badly formed R6 Location Update Response messages on R6 interface. | Int32
r6locupdrsp-decodeerr | The total number of R6 Location Update Response messages on R6 interface with decode errors. | Int32
r6locupdrsp-unspecerr | The total number of R6 Location Update Response messages on R6 interface with unspecified error. | Int32
r6locupdrsp-missmandtlv | The total number of R6 Location Update Response messages on R6 interface with missing mandatory TLVs. | Int32
r6locupdrsp-tlvvalinval | .The total number of R6 Location Update Response messages on R6 interface with an unknown TLV value. | Int32
r6locupdrsp-unknowntlv | The total number of R6 Location Update Response messages on R6 interface with unknown TLVs. | Int32
r6locupdrsp-duptlvfound | The total number of R6 Location Update Response messages on R6 interface with duplicate TLVs. | Int32
r6locupdrsp-nosessfound | The total number of R6 Location Update Response messages without any session information. | Int32
r6locupdrsp-admprohibit | The total number of R6 Location Update Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Location Update Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6locupdrsp-noresourcedrop | The total number of R6 Location Update Response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Location Update Response message is discarded or denied due to resource unavailability. Availability: across all ASNGW services. | Int32
r6locupdrsp-transiderr | The total number of R6 Location Update Response messages with translation ID errors | Int32
r6locupdcnf-totsent | Indicates the number of R6 Location Update Confirm messages sent to the Base Station. | Int32
r6locupdcnf-retranssent | The total number of Location Update Confirm messages retransmitted on the R6 interface to the base station. | Int32
r6locupdcnf-totsendfail | The total number of Location Update Confirm message failures received from the base station and relayed on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int32
r6locupdcnf-totrec | The total number of R6 Location Update Confirm messages received by the base station. | Int32
r6locupdcnf-totacc | The total number of R6 Location Update Confirm messages accepted by base station. | Int32
r6locupdcnf-totrelay | The total number of R6 Location Update Confirm messages sent to the base station and relayed on the R6 interface. Triggers: Changes every time an R6 Location Update Confirm message is relayed by the R6 interface. Availability: across all ASNGW services | Int32
r6locupdcnf-totdenied | The total number of Location Update Confirm messages denied on the R6 interface. | Int32
r6locupdcnf-totdiscard | The total number of Location Update Confirm messages discarded on the R6 interface. | Int32
r6locupdcnf-badform | The total number of badly formed R6 Location Update Confirm messages sent to the base station. | Int32
r6locupdcnf-decodeerr | The total number of R6 Location Update Confirm messages sent to the base station with decode errors. | Int32
r6locupdcnf-unspecerr | The total number of R6 Location Update Confirm messages sent to the base station with unspecified errors. | Int32
r6locupdcnf-missmandtlv | The total number of R6 Location Update Confirm messages sent to the base station with missing mandatory TLVs. | Int32
r6locupdcnf-tlvvalinval | The total number of R6 Location Update Confirm messages sent to the base station with an invalid TLV. | Int32
r6locupdcnf-unknowntlv | The total number of R6 Location Update Confirm messages sent to the base station with an unknown TLV. | Int32
r6locupdcnf-duptlvfound | The total number of R6 Location Update Confirm messages sent to the base station with duplicate TLVs. | Int32
r6locupdcnf-nosessfound | The total number of R6 Location Update Confirm messages sent to the base station without any session information. | Int32
r6locupdcnf-admprohibit | The total number of R6 Location Update Confirm messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Location Update Confirm message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6locupdcnf-noresourcedrop | The total number of R6 Location Update Confirm messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Location Update Confirm message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6locupdcnf-transiderr | The total number of R6 Location Update Confirm messages sent to the base station with a transaction ID error. | Int32
r6pagannouce-totsent | The total number of R6 Paging Announcement messages sent to the Base Station. | Int32
r6pagannouce-retranssent | The total number of Paging Announcement messages retransmitted on the R6 interface to the base station. | Int32
r6pagannouce-totsendfail | The total number of Paging Announcement message failures received from the base station and relayed on the R6 interface. This counter is used to count the error while sending the R6 packets. | Int32
r6pagannouce-totrec | The total number of R6 Paging Announcement messages received by the base station. | Int32
r6pagannouce-totacc | The total number of R6 Paging Announcement messages accepted by base station. | Int32
r6pagannouce-totrelay | The total number of R6 Paging Announcement messages sent to the base station and relayed on the R6 interface. Triggers: Changes every time an R6 Paging Announcement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6pagannouce-totdenied | The total number of Paging Announcement messages denied on the R6 interface. | Int32
r6pagannouce-totdiscard | The total number of Paging Announcement messages discarded on the R6 interface. | Int32
r6pagannouce-badform | The total number of badly formed R6 Paging Announcement messages sent to the base station. | Int32
r6pagannouce-decodeerr | The total number of R6 Paging Announcement messages sent to the base station with decode errors. | Int32
r6pagannouce-unspecerr | The total number of R6 Paging Announcement messages sent to the base station with unspecified errors. | Int32
r6pagannouce-missmandtlv | The total number of R6 Paging Announcement messages sent to the base station with missing mandatory TLVs. | Int32
r6pagannouce-tlvvalinval | The total number of R6 Paging Announcement messages sent to the base station with an invalid TLV. | Int32
r6pagannouce-unknowntlv | The total number of R6 Paging Announcement messages sent to the base station with an unknown TLV. | Int32
r6pagannouce-duptlvfound | The total number of R6 Paging Announcement messages sent to the base station with duplicate TLVs. | Int32
r6pagannouce-nosessfound | The total number of R6 Paging Announcement messages sent to the base station without any session information. | Int32
r6pagannouce-admprohibit | The total number of R6 Paging Announcement messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Paging Announcement message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6pagannouce-noresourcedrop | The total number of R6 Paging Announcement messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Paging Announcement message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6pagannouce-transiderr | The total number of R6 Paging Announcement messages sent to the base station with a transaction ID error. | Int32
r6keepalivereq-totrec | The total number of R6 Keep-alive Request messages received by the base station. | Int32
r6keepalivereq-totacc | The total number of R6 Keep-alive Request messages accepted by base station. | Int32
r6keepalivereq-totrelay | The total number of R6 Keep-alive Request messages sent to the base station and relayed on the R6 interface. Triggers: Changes every time an R6 Keep-alive Request message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6keepalivereq-totdenied | The total number of Keep-alive Request messages denied on the R6 interface. | Int32
r6keepalivereq-totdiscard | The total number of Keep-alive Request messages discarded on the R6 interface. | Int32
r6keepalivereq-badform | The total number of badly formed R6 Keep-alive Request messages sent to the base station. | Int32
r6keepalivereq-decodeerr | The total number of R6 Keep-alive Request messages sent to the base station with decode errors. | Int32
r6keepalivereq-unspecerr | The total number of R6 Keep-alive Request messages sent to the base station with unspecified errors. | Int32
r6keepalivereq-missmandtlv | The total number of R6 Keep-alive Request messages sent to the base station with missing mandatory TLVs. | Int32
r6keepalivereq-tlvvalinval | The total number of R6 Keep-alive Request messages sent to the base station with an invalid TLV. | Int32
r6keepalivereq-unknowntlv | The total number of R6 Keep-alive Request messages sent to the base station with an unknown TLV. | Int32
r6keepalivereq-duptlvfound | The total number of R6 Keep-alive Request messages sent to the base station with duplicate TLVs. | Int32
r6keepalivereq-nosessfound | The total number of R6 Keep-alive Request messages sent to the base station without any session information. | Int32
r6keepalivereq-admprohibit | The total number of R6 Keep-alive Request messages sent to the base station that were discarded or denied due to admin prohibit. Triggers: Changes every time an R6 Keep-alive Request message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r6keepalivereq-noresourcedrop | The total number of R6 Keep-alive Request messages sent to the base station that were discarded or denied due to resource unavailability. Triggers: Changes every time an R6 Keep-alive Request message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r6keepalivereq-transiderr | The total number of R6 Keep-alive Request messages sent to the base station with a transaction ID error. | Int32
r6keepaliversp-totsent | The total number of Keep-alive Response messages sent to the Base Station on the R6 interface. | Int32
r6keepaliversp-retranssent | The total number of Keep-alive Response messages retransmitted on the R6 interface. | Int32
r6keepaliversp-totsendfail | The total number of failed Keep-alive Response messages that occurred during transaction ID generation. This counter is used to count the error while sending the R6 packets. | Int32
r6unknown-totrec | The total number of Unknown messages received on R6 interface. | Int32
r6unknown-totacc | The total number of Unknown messages accepted on R6 interface. | Int32
r6unknown-totrelay | The total number of Unknown messages received from the base station and relayed on the R6 interface. Triggers: Changes every time an Unknown message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r6unknown-totdenied | The total number of Unknown messages denied on R6 interface. | Int32
r6unknown-totdiscard | The total number of Unknown messages discarded on R6 interface. | Int32
r6unknown-badform | The total number of badly formed Unknown messages on R6 interface | Int32
r6unknown-decodeerr | The total number of Unknown messages on R6 interface with decode error. | Int32
r6unknown-unspecerr | The total number of Unknown messages on R6 interface with unspecified error. | Int32
r6unknown-missmandtlv | The total number of Unknown messages on R6 interface with missing mandatory TLVs. | Int32
r6unknown-tlvvalinval | The total number of Unknown messages on R6 interface with invalid TLV value | Int32
r6unknown-unknowntlv | The total number of Unknown messages on R6 interface with unknown TLV value | Int32
r6unknown-duptlvfound | The total number of Unknown messages on R6 interface with duplicate TLVs. | Int32
r6unknown-nosessfound | The total number of Unknown messages on R6 interface without any session information. | Int32
r6unknown-admprohibit | The total number of Unknown messages discarded or denied due to admin prohibit. Triggers: Changes every time an Unknown message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r6unknown-noresourcedrop | The total number of Unknown messages discarded or denied due to resource unavailability. Triggers: Changes every time an Unknown message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r6unknown-transiderr | The total number of Unknown messages on R6 interface with transaction ID errors. | Int32
r4imentstachareq-totsent | The total number of R4 Idle Mode Entry State Change Request messages sent to the ASNGW. | Int32
r4imentstachareq-retranssent | The total number of R4 Idle Mode Entry State Change Request messages re-transmitted on R4 interface. | Int32
r4imentstachareq-totsendfail | The total number of failures occurred during transaction id generation and R4 Idle Mode Entry State Change Request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imentstachareq-totrec | The total number of R4 Idle Mode Entry State Change Request messages received on R4 interface. | Int32
r4imentstachareq-totacc | The total number of R4 Idle Mode Entry State Change Request messages accepted on R4 interface. | Int32
r4imentstachareq-totrelay | The total number of R4 Idle Mode Entry State Change Request messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Idle Mode Entry State Change Request message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4imentstachareq-totdenied | The total number of R4 Idle Mode Entry State Change Request messages denied on R4 interface. | Int32
r4imentstachareq-totdiscard | The total number of R4 Idle Mode Entry State Change Request messages discarded on R4 interface. | Int32
r4imentstachareq-badform | The total number of badly formed R4 Idle Mode Entry State Change Request messages on R4 interface. | Int32
r4imentstachareq-decodeerr | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface with decode error. | Int32
r4imentstachareq-unspecerr | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface with unspecified error. | Int32
r4imentstachareq-missmandtlv | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface with missing mandatory TLVs. | Int32
r4imentstachareq-tlvvalinval | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface with invalid TLV value | Int32
r4imentstachareq-unknowntlv | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface with unknown TLVs. | Int32
r4imentstachareq-duptlvfound | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface with duplicate TLVs. | Int32
r4imentstachareq-nosessfound | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface without any session information | Int32
r4imentstachareq-admprohibit | The total number of R4 Idle Mode Entry State Change Request messages discarded or denied due to admin prohibit. Triggers: Changes every time a R4 Idle Mode Entry State Change Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imentstachareq-noresourcedrop | The total number of R4 Idle Mode Entry State Change Request messages discarded or denied due to resource unavailability. Triggers: Changes every time a R4 idle mode entry MS state change request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imentstachareq-transiderr | The total number of R4 Idle Mode Entry State Change Request messages on R4 interface with transaction ID errors. | Int32
r4imentstacharsp-totsent | The number of Idle Mode Entry State Change Responses sent to the ASNGW. | Int32
r4imentstacharsp-retranssent | The total number of R4 Idle Mode Entry State Change Response messages re-transmitted on R4 interface. | Int32
r4imentstacharsp-totsendfail | The total number of failures occurred during transaction id generation and R4 Idle Mode Entry State Change Response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imentstacharsp-totrec | The total number of R4 Idle Mode Entry State Change Response messages received on R4 interface | Int32
r4imentstacharsp-totacc | The total number of R4 Idle Mode Entry State Change Response messages accepted on R4 interface. | Int32
r4imentstacharsp-totrelay | The total number of R4 Idle Mode Entry State Change Response messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Idle Mode Entry State Change Response message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4imentstacharsp-totdenied | The total number of R4 Idle Mode Entry State Change Response messages denied on R4 interface. | Int32
r4imentstacharsp-totdiscard | The total number of R4 Idle Mode Entry State Change Response messages discarded on R4 interface. | Int32
r4imentstacharsp-badform | The total number of badly formed R4 idle mode entry MS state change response messages on R4 interface. | Int32
r4imentstacharsp-decodeerr | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface with decode error. | Int32
r4imentstacharsp-unspecerr | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface with unspecified error. | Int32
r4imentstacharsp-missmandtlv | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface with missing mandatory TLVs. | Int32
r4imentstacharsp-tlvvalinval | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface with invalid TLV value. | Int32
r4imentstacharsp-unknowntlv | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface with unknown TLVs. | Int32
r4imentstacharsp-duptlvfound | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface with duplicate TLVs. | Int32
r4imentstacharsp-nosessfound | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface without any session information. | Int32
r4imentstacharsp-admprohibit | The total number of R4 Idle Mode Entry State Change Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Idle Mode Entry State Change Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imentstacharsp-noresourcedrop | The total number of R4 Idle Mode Entry State Change Response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Idle Mode Entry State Change Response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imentstacharsp-transiderr | The total number of R4 Idle Mode Entry State Change Response messages on R4 interface with transaction ID errors. | Int32
r4imentstachaack-totsent | The total number of Idle Mode Entry State Change Acknowledgements sent to the ASNGW. | Int32
r4imentstachaack-retranssent | The total number of R4 Idle Mode Entry State Change Acknowledgement messages re-transmitted to the ASNGW on the R4 interface. | Int32
r4imentstachaack-totsendfail | The total number of failures that occurred during transaction id generation and R4 Idle Mode Entry State Change Acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4imentstachaack-totrec | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on R4 interface | Int32
r4imentstachaack-totacc | The total number of R4 Idle Mode Entry State Change Acknowledgement messages accepted on R4 interface by the ASNGW. | Int32
r4imentstachaack-totrelay | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Idle Mode Entry State Change Acknowledgement message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4imentstachaack-totdenied | The total number of R4 Idle Mode Entry State Change Acknowledgement messages denied by the ASNGW on the R4 interface. | Int32
r4imentstachaack-totdiscard | The total number of R4 Idle Mode Entry State Change Acknowledgement messages discarded by the ASNGW on the R4 interface | Int32
r4imentstachaack-badform | The total number of badly formed R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface. | Int32
r4imentstachaack-decodeerr | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface with decode errors. | Int32
r4imentstachaack-unspecerr | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface with unspecified error. | Int32
r4imentstachaack-missmandtlv | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface with missing mandatory TLVs. | Int32
r4imentstachaack-tlvvalinval | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface with invalid TLV value. | Int32
r4imentstachaack-unknowntlv | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface with unknown TLVs. | Int32
r4imentstachaack-duptlvfound | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface with duplicate TLVs. | Int32
r4imentstachaack-nosessfound | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface without any session information. | Int32
r4imentstachaack-admprohibit | The total number of R4 Idle Mode Entry State Change Acknowledgement messages discarded or denied by the ASNGW on the R4 interface due to admin prohibit. Triggers: Changes every time an R4 Idle Mode Entry State Change Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services | Int32
r4imentstachaack-noresourcedrop | The total number of R4 Idle Mode Entry State Change Acknowledgement messages discarded or denied by the ASNGW on the R4 interface due to resource unavailability. Triggers: Changes every time an R4 Idle Mode Entry State Change Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imentstachaack-transiderr | The total number of R4 Idle Mode Entry State Change Acknowledgement messages received by the ASNGW on the R4 interface with transaction ID errors. | Int32
r4imexitstachareq-totsent | The total number of Idle Mode Exit State Change Requests sent to the ASNGW. | Int32
r4imexitstachareq-retranssent | The total number of R4R4 Idle Mode Exit State Change Request messages re-transmitted on R4 interface. | Int32
r4imexitstachareq-totsendfail | The total number of R4 idle Mode Exit State Change Request messages sent to the base station. This counter is used to count the error while sending the R4 packets. | Int32
r4imexitstachareq-totrec | The total number of R4 Idle Mode Exit State Change Request messages received on R4 interface. | Int32
r4imexitstachareq-totacc | The total number of R4 Idle Mode Exit State Change Request messages accepted on R4 interface. | Int32
r4imexitstachareq-totrelay | The total number of R4 Idle Mode Exit State Change Request messages relayed to the base station on the R4 interface. Triggers: Changes every time an R4 Idle Mode Exit State Change Request message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4imexitstachareq-totdenied | The total number of R4 Idle Mode Exit State Change Request messages denied on R4 interface. | Int32
r4imexitstachareq-totdiscard | The total number of R4 Idle Mode Exit State Change Request messages discarded on R4 interface. | Int32
r4imexitstachareq-badform | The total number of badly formed R4 Idle Mode Exit State Change Request messages on R4 interface. | Int32
r4imexitstachareq-decodeerr | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface with decode error. | Int32
r4imexitstachareq-unspecerr | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface with unspecified error. | Int32
r4imexitstachareq-missmandtlv | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface with missing mandatory TLVs. | Int32
r4imexitstachareq-tlvvalinval | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface with invalid TLV value | Int32
r4imexitstachareq-unknowntlv | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface with unknown TLVs | Int32
r4imexitstachareq-duptlvfound | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface with duplicate TLVs. | Int32
r4imexitstachareq-nosessfound | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface without any session information. | Int32
r4imexitstachareq-admprohibit | The total number of R4 Idle Mode Exit State Change Request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Idle Mode Exit State Change Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imexitstachareq-noresourcedrop | The total number of R4 Idle Mode Exit State Change Request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Idle Mode Exit State Change Request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4imexitstachareq-transiderr | The total number of R4 Idle Mode Exit State Change Request messages on R4 interface with transaction ID errors. | Int32
r4imexitstacharsp-totsent | The total number of Idle Mode Exit State Change Responses sent to the Base Station. | Int32
r4imexitstacharsp-retranssent | The total number of R4 Idle Mode Exit State Change Response messages re-transmitted on R4 interface. | Int32
r4imexitstacharsp-totsendfail | The total number of failed R4 idle Mode Exit State Change Response messages sent to the base station. This counter is used to count the error while sending the R4 packets. | Int32
r4imexitstacharsp-totrec | The total number of R4 Idle Mode Exit State Change Response messages received on R4 interface. | Int32
r4imexitstacharsp-totacc | The total number of R4 Idle Mode Exit State Change Response messages accepted on R4 interface. | Int32
r4imexitstacharsp-totrelay | The total number of R4 Idle Mode Exit State Change Response messages relayed to the base station on the R4 interface. Triggers: Changes every time an R4 Idle Mode Exit State Change Response message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4imexitstacharsp-totdenied | The total number of R4 Idle Mode Exit State Change Response messages denied on R4 interface. | Int32
r4imexitstacharsp-totdiscard | The total number of R4 Idle Mode Exit State Change Response messages discarded on R4 interface. | Int32
r4imexitstacharsp-badform | The total number of badly formed R4 Idle Mode Exit State Change Response messages on R4 interface. | Int32
r4imexitstacharsp-decodeerr | The total number of R4 Idle Mode Exit State Change Response messages on R4 interface with decode error. | Int32
r4imexitstacharsp-unspecerr | The total number of R4 Idle Mode Exit State Change Response messages on R4 interface with unspecified error. | Int32
r4imexitstacharsp-missmandtlv | The total number of R4 Idle Mode Exit State Change Response messages on R4 interface with missing mandatory TLVs. | Int32
r4imexitstacharsp-tlvvalinval | The total number of R4 Idle Mode Exit State Change Response messages on R4 interface with an invalid TLV value. | Int32
r4imexitstacharsp-unknowntlv | The total number of R4 Idle Mode Exit State Change Response messages on R4 interface with unknown TLVs. | Int32
r4imexitstacharsp-duptlvfound | The total number of R4 Idle Mode Exit State Change Response messages on R4 interface with duplicate TLVs. | Int32
r4imexitstacharsp-nosessfound | The total number of R4 Idle Mode Exit State Change Response messages with no session information. | Int32
r4imexitstacharsp-admprohibit | The total number of R4 Idle Mode Exit State Change Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Idle Mode Exit State Change Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4imexitstacharsp-noresourcedrop | The total number of R4 Idle Mode Exit State Change Response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Idle Mode Exit State Change Response message is discarded or denied due to resource unavailability. Availability: across all ASNGW services. | Int32
r4imexitstacharsp-transiderr | The total number of R4 Idle Mode Exit State Change Response messages with translation ID errors. | Int32
r4inipagreq-totsent | The total number of Initial Paging Requests sent to the ASNGW. | Int32
r4inipagreq-retranssent | The total number of R4 Initial Paging Request messages re-transmitted on R4 interface. | Int32
r4inipagreq-totsendfail | The total number of failures occurred during transaction id generation and R4 Initial Paging Request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4inipagreq-totrec | The total number of R4 Initial Paging Request messages received on R4 interface. | Int32
r4inipagreq-totacc | The total number of R4 Initial Paging Request messages accepted on R4 interface. | Int32
r4inipagreq-totrelay | The total number of R4 Initial Paging Request messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Initial Paging Request message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4inipagreq-totdenied | The total number of R4 Initial Paging Request messages denied on R4 interface. | Int32
r4inipagreq-totdiscard | The total number of R4 Initial Paging Request messages discarded on R4 interface. | Int32
r4inipagreq-badform | The total number of badly formed R4 Initial Paging Request messages on R4 interface. | Int32
r4inipagreq-decodeerr | The total number of R4 Initial Paging Request messages on R4 interface with decode error. | Int32
r4inipagreq-unspecerr | The total number of R4 Initial Paging Request messages on R4 interface with unspecified error. | Int32
r4inipagreq-missmandtlv | The total number of R4 Initial Paging Request messages on R4 interface with missing mandatory TLVs. | Int32
r4inipagreq-tlvvalinval | The total number of R4 Initial Paging Request messages on R4 interface with invalid TLV value. | Int32
r4inipagreq-unknowntlv | The total number of R4 Initial Paging Request messages on R4 interface with unknown TLVs. | Int32
r4inipagreq-duptlvfound | The total number of R4 Initial Paging Request messages on R4 interface with duplicate TLVs. | Int32
r4inipagreq-nosessfound | The total number of R4 Initial Paging Request messages on R4 interface without any session information. | Int32
r4inipagreq-admprohibit | The total number of R4 Initial Paging Request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Initial Paging Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4inipagreq-noresourcedrop | The total number of R4 Initial Paging Request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Initial Paging Request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4inipagreq-transiderr | The total number of R4 Initial Paging Request messages on R4 interface with transaction ID errors. | Int32
r4inipagrsp-totsent | The total number of Initiate Paging Responses sent to the ASNGW. | Int32
r4inipagrsp-retranssent | The total number of R4 Initial Paging Response messages re-transmitted on R4 interface. | Int32
r4inipagrsp-totsendfail | The total number of failures occurred during transaction id generation and R4 Initial Paging Response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4inipagrsp-totrec | The total number of R4 Initial Paging Response messages received on R4 interface. | Int32
r4inipagrsp-totacc | The total number of R4 Initial Paging Response messages accepted on R4 interface. | Int32
r4inipagrsp-totrelay | The total number of R4 Initial Paging Response messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Initial Paging Response message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4inipagrsp-totdenied | The total number of R4 Initial Paging Response messages denied on R4 interface | Int32
r4inipagrsp-totdiscard | The total number of R4 Initial Paging Response messages discarded on R4 interface. | Int32
r4inipagrsp-badform | The total number of badly formed R4 Initial Paging Response messages on R4 interface. | Int32
r4inipagrsp-decodeerr | The total number of R4 Initial Paging Response messages on R4 interface with decode error. | Int32
r4inipagrsp-unspecerr | The total number of R4 Initial Paging Response messages on R4 interface with unspecified error. | Int32
r4inipagrsp-missmandtlv | The total number of R4 Initial Paging Response messages on R4 interface with missing mandatory TLVs. | Int32
r4inipagrsp-tlvvalinval | The total number of R4 Initial Paging Response messages on R4 interface with invalid TLV value. | Int32
r4inipagrsp-unknowntlv | The total number of R4 Initial Paging Response messages on R4 interface with unknown TLVs. | Int32
r4inipagrsp-duptlvfound | The total number of R4 Initial Paging Response messages on R4 interface with duplicate TLVs. | Int32
r4inipagrsp-nosessfound | The total number of R4 Initial Paging Response messages on R4 interface without any session information. | Int32
r4inipagrsp-admprohibit | The total number of R4 Initial Paging Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Initial Paging Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4inipagrsp-noresourcedrop | The total number of R4 Initial Paging Response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Initial Paging Response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4inipagrsp-transiderr | The total number of R4 Initial Paging Response messages on R4 interface with transaction ID errors. | Int32
r4nwexitmsstachareq-totsent | The total number of Network Exit MS State Change Requests sent to the ASNGW. | Int32
r4nwexitmsstachareq-retranssent | The total number of Network Exit MS State Change Request messages re-transmitted on the R4 interface. | Int32
r4nwexitmsstachareq-totsendfail | The total number of failures occurred during transaction ID generation and R4 Network Exit MS State Change Request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4nwexitmsstachareq-totrec | The total number of Network Exit MS State Change Request messages received on R4 interface | Int32
r4nwexitmsstachareq-totacc | The total number of Network Exit MS State Change Request messages accepted on R4 interface | Int32
r4nwexitmsstachareq-totrelay | The total number of Network Exit MS State Change Request messages received from the base station and relayed on the R4 interface. Triggers: Changes every time a Network Exit MS State Change Request message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4nwexitmsstachareq-totdenied | The total number of Network Exit MS State Change Request messages denied on R4 interface. | Int32
r4nwexitmsstachareq-totdiscard | The total number of Network Exit MS State Change Request messages discarded on R4 interface. | Int32
r4nwexitmsstachareq-badform | The total number of badly formed Network Exit MS State Change Request messages on R4 interface. | Int32
r4nwexitmsstachareq-decodeerr | The total number of Network Exit MS State Change Request messages on R4 interface with decode error. | Int32
r4nwexitmsstachareq-unspecerr | The total number of Network Exit MS State Change Request messages on R4 interface with unspecified error. | Int32
r4nwexitmsstachareq-missmandtlv | The total number of Network Exit MS State Change Request messages on R4 interface with missing mandatory TLVs. | Int32
r4nwexitmsstachareq-tlvvalinval | The total number of Network Exit MS State Change Request messages on R4 interface with invalid TLV value. | Int32
r4nwexitmsstachareq-unknowntlv | The total number of Network Exit MS State Change Request messages on R4 interface with unknown TLVs. | Int32
r4nwexitmsstachareq-duptlvfound | The total number of Network Exit MS State Change Request messages on R4 interface with duplicate TLVs. | Int32
r4nwexitmsstachareq-nosessfound | The total number of Network Exit MS State Change Request messages on R4 interface without any session information. | Int32
r4nwexitmsstachareq-admprohibit | The total number of Network Exit MS State Change Request messages on R4 interface with transaction ID errors. | Int32
r4nwexitmsstachareq-noresourcedrop | The total number of Network Exit MS State Change Request messages discarded or denied due to admin prohibit. Triggers: Changes every time a Network Exit MS State Change Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4nwexitmsstachareq-transiderr | The total number of Network Exit MS State Change Request messages discarded or denied due to transaction ID errors. | Int32
r4nwexitmsstacharsp-totsent | The total number of Network Exit MS State Change Responses sent to the ASNGW. | Int32
r4nwexitmsstacharsp-retranssent | The total number of Network Exit MS State Change Response messages re-transmitted on R4 interface. | Int32
r4nwexitmsstacharsp-totsendfail | The total number of Network Exit MS State Change Response failures that occurred during transaction ID generation and R4 Network Exit MS State Change Response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4nwexitmsstacharsp-totrec | The total number of Network Exit MS State Change Response messages received on R4 interface. | Int32
r4nwexitmsstacharsp-totacc | The total number of Network Exit MS State Change Response messages accepted on R4 interface. | Int32
r4nwexitmsstacharsp-totrelay | The total number of Network Exit MS State Change Response messages received from the base station and relayed on the R4 interface. Triggers: Changes every time a Network Exit MS State Change Response message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4nwexitmsstacharsp-totdenied | The total number of Network Exit MS State Change Response messages denied on R4 interface. | Int32
r4nwexitmsstacharsp-totdiscard | The total number of Network Exit MS State Change Response messages discarded on R4 interface. | Int32
4nwexitmsstacharsp-badform | The total number of badly formed Network Exit MS State Change Response messages on R4 interface. | Int32
r4nwexitmsstacharsp-decodeerr | The total number of Network Exit MS State Change Response messages on R4 interface with decode error. | Int32
r4nwexitmsstacharsp-unspecerr | The total number of Network Exit MS State Change Response messages on R4 interface with unspecified error. | Int32
r4nwexitmsstacharsp-missmandtlv | The total number of Network Exit MS State Change Response messages on R4 interface with missing mandatory TLVs. | Int32
r4nwexitmsstacharsp-tlvvalinval | The total number of Network Exit MS State Change Response messages on R4 interface with invalid TLV value. | Int32
r4nwexitmsstacharsp-unknowntlv | The total number of Network Exit MS State Change Response messages on R4 interface with unknown TLVs. | Int32
r4nwexitmsstacharsp-duptlvfound | The total number of Network Exit MS State Change Response messages on R4 interface with duplicate TLVs. | Int32
r4nwexitmsstacharsp-nosessfound | The total number of Network Exit MS State Change Response messages on R4 interface without any session information. | Int32
r4nwexitmsstacharsp-admprohibit | The total number of Network Exit MS State Change Response messages discarded or denied due to admin prohibit. Triggers: Changes every time a Network Exit MS State Change Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4nwexitmsstacharsp-noresourcedrop | The total number of Network Exit MS State Change Response messages discarded or denied due to resource unavailability. Triggers: Changes every time a Network Exit MS State Change Response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service. | Int32
r4nwexitmsstacharsp-transiderr | The total number of Network Exit MS State Change Response messages on R4 interface with transaction ID errors. | Int32
r4delmsentreq-totsent | The total number of Delete MS Entry Requests sent to the ASNGW on the R4 interface. | Int32
r4delmsentreq-retranssent | The total number of R4 Delete MS Entry Request messages re-transmitted on R4 interface | Int32
r4delmsentreq-totsendfail | The total number of failures occurred during transaction id generation and R4 Delete MS Entry Request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4delmsentreq-totrec | The total number of R4 Delete MS Entry Request messages received on R4 interface. | Int32
r4delmsentreq-totacc | The total number of R4 Delete MS Entry Request messages accepted on R4 interface | Int32
r4delmsentreq-totrelay | The total number of R4 Delete MS Entry Request messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Delete MS Entry Request message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4delmsentreq-totdenied | The total number of R4 Delete MS Entry Request messages denied on R4 interface. | Int32
r4delmsentreq-totdiscard | The total number of R4 Delete MS Entry Request messages discarded on R4 interface. | Int32
r4delmsentreq-badform | The total number of badly formed R4 Delete MS Entry Request messages on R4 interface. | Int32
r4delmsentreq-decodeerr | The total number of R4 Delete MS Entry Request messages on R4 interface with decode error. | Int32
r4delmsentreq-unspecerr | The total number of R4 Delete MS Entry Request messages on R4 interface with unspecified error. | Int32
r4delmsentreq-missmandtlv | The total number of R4 Delete MS Entry Request messages on R4 interface with missing mandatory TLVs. | Int32
r4delmsentreq-tlvvalinval | The total number of R4 Delete MS Entry Request messages on R4 interface with invalid TLV value. | Int32
r4delmsentreq-unknowntlv | The total number of R4 Delete MS Entry Request messages on R4 interface with unknown TLVs. | Int32
r4delmsentreq-duptlvfound | The total number of R4 Delete MS Entry Request messages on R4 interface with duplicate TLVs. | Int32
r4delmsentreq-nosessfound | The total number of R4 Delete MS Entry Request messages on R4 interface without any session information. | Int32
r4delmsentreq-admprohibit | The total number of R4 Delete MS Entry Request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Delete MS Entry Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4delmsentreq-noresourcedrop | The total number of R4 Delete MS Entry Request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Delete MS Entry Request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4delmsentreq-transiderr | The total number of R4 Delete MS Entry Request messages on R4 interface with transaction ID errors. | Int32
r4delmsentrsp-totsent | The total number of Delete MS Entry Responses sent to the ASNGW. | Int32
r4delmsentrsp-retranssent | The total number of R4 Delete MS Entry Response messages retransmitted on the R4 interface. | Int32
r4delmsentrsp-totsendfail | The total number of failures occurred during transaction id generation and R4 Delete MS Entry Response message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4delmsentrsp-totrec | The total number of R4 Delete MS Entry Response messages received on R4 interface. | Int32
r4delmsentrsp-totacc | The total number of R4 Delete MS Entry Response messages accepted on the R4 interface. | Int32
r4delmsentrsp-totrelay | The total number of R4 Delete MS Entry Response messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Delete MS Entry Response message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4delmsentrsp-totdenied | The total number of R4 Delete MS Entry Response messages denied on R4 interface. | Int32
r4delmsentrsp-totdiscard | The total number of R4 Delete MS Entry Response messages discarded on R4 interface. | Int32
r4delmsentrsp-badform | The total number of badly formed R4 Delete MS Entry Response messages on R4 interface. | Int32
r4delmsentrsp-decodeerr | The total number of R4 Delete MS Entry Response messages on R4 interface with decode error. | Int32
r4delmsentrsp-unspecerr | The total number of R4 Delete MS Entry Response messages on R4 interface with unspecified error. | Int32
r4delmsentrsp-missmandtlv | The total number of R4 Delete MS Entry Response messages on R4 interface with missing mandatory TLVs. | Int32
r4delmsentrsp-tlvvalinval | The total number of R4 Delete MS Entry Response messages on R4 interface with invalid TLV value. | Int32
r4delmsentrsp-unknowntlv | The total number of R4 Delete MS Entry Response messages on R4 interface with unknown TLVs. | Int32
r4delmsentrsp-duptlvfound | The total number of R4 Delete MS Entry Response messages on R4 interface with duplicate TLVs. | Int32
r4delmsentrsp-nosessfound | The total number of R4 Delete MS Entry Response messages on R4 interface without any session information. | Int32
r4delmsentrsp-admprohibit | The total number of R4 Delete MS Entry Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Delete MS Entry Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4delmsentrsp-noresourcedrop | The total number of R4 Delete MS Entry Response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Delete MS Entry Response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4delmsentrsp-transiderr | The total number of R4 Delete MS Entry Response messages on R4 interface with transaction ID errors. | Int32
r4anchorpcind-totsent | The total number of Anchor Paging Controller Indicator messages sent to the ASNGW on the R4 interface. | Int32
r4anchorpcind-retranssent | The total number of R4 Anchor Paging Controller Indicator messages re-transmitted on R4 interface. | Int32
r4anchorpcind-totsendfail | The total number of failures occurred during transaction id generation and R4 Anchor Paging Controller Indicator message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4anchorpcind-totrec | The total number of R4 Anchor Paging Controller Indicator messages received on R4 interface. | Int32
r4anchorpcind-totacc | The total number of R4 Anchor Paging Controller Indicator messages accepted on R4 interface. | Int32
r4anchorpcind-totrelay | The total number of R4 Anchor Paging Controller Indicator messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Anchor Paging Controller Indicator message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4anchorpcind-totdenied | The total number of R4 Anchor Paging Controller Indicator messages denied on R4 interface. | Int32
r4anchorpcind-totdiscard | The total number of R4 Anchor Paging Controller Indicator messages discarded on R4 interface. | Int32
r4anchorpcind-badform | The total number of badly formed R4 Anchor Paging Controller Indicator messages on R4 interface. | Int32
r4anchorpcind-decodeerr | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface with decode error. | Int32
r4anchorpcind-unspecerr | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface with unspecified error. | Int32
r4anchorpcind-missmandtlv | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface with missing mandatory TLVs. | Int32
r4anchorpcind-tlvvalinval | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface with invalid TLV value. | Int32
r4anchorpcind-unknowntlv | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface with unknown TLVs. | Int32
r4anchorpcind-duptlvfound | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface with duplicate TLVs. | Int32
r4anchorpcind-nosessfound | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface without any session information. | Int32
r4anchorpcind-admprohibit | The total number of R4 Anchor Paging Controller Indicator messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Anchor Paging Controller Indicator message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4anchorpcind-noresourcedrop | The total number of R4 Anchor Paging Controller Indicator messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Anchor Paging Controller Indicator message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4anchorpcind-transiderr | The total number of R4 Anchor Paging Controller Indicator messages on R4 interface with transaction ID errors. | Int32
r4anchorpcack-totsent | The total number of Anchor Paging Controller Acknowledgements sent to the ASNGW. | Int32
r4anchorpcack-retranssent | The total number of R4 Anchor Paging Controller Acknowledgement messages re-transmitted on R4 interface. | Int32
r4anchorpcack-totsendfail | The total number of failures occurred during transaction id generation and R4 Anchor Paging Controller Acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4anchorpcack-totrec | The total number of R4 Anchor Paging Controller Acknowledgement messages received on R4 interface. | Int32
r4anchorpcack-totacc | The total number of R4 Anchor Paging Controller Acknowledgement messages accepted on R4 interface. | Int32
r4anchorpcack-totrelay | The total number of R4 Anchor Paging Controller Acknowledgement messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Anchor Paging Controller Acknowledgement message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4anchorpcack-totdenied | The total number of R4 Anchor Paging Controller Acknowledgement messages denied on R4 interface. | Int32
r4anchorpcack-totdiscard | The total number of R4 Anchor Paging Controller Acknowledgement messages discarded on R4 interface. | Int32
r4anchorpcack-badform | The total number of badly formed R4 Anchor Paging Controller Acknowledgement messages on R4 interface. | Int32
r4anchorpcack-decodeerr | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface with decode error. | Int32
r4anchorpcack-unspecerr | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface with unspecified error. | Int32
r4anchorpcack-missmandtlv | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface with missing mandatory TLVs. | Int32
r4anchorpcack-tlvvalinval | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface with invalid TLV value. | Int32
r4anchorpcack-unknowntlv | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface with unknown TLVs. | Int32
r4anchorpcack-duptlvfound | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface with duplicate TLVs. | Int32
r4anchorpcack-nosessfound | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface without any session information. | Int32
r4anchorpcack-adminprohib | The total number of R4 Anchor Paging Controller Acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Anchor Paging Controller Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4anchorpcack-noresourcedrop | The total number of R4 Anchor Paging Controller Acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Anchor Paging Controller Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4anchorpcack-transiderr | The total number of R4 Anchor Paging Controller Acknowledgement messages on R4 interface with transaction ID errors. | Int32
r4locupdreq-totsent | The total number of Location Update Requests sent to the peer ASNPC over the R4 interface. | Int32
r4locupdreq-retranssent | The total number of R4 Location Update Request messages re-transmitted on R4 interface. | Int32
r4locupdreq-totsendfail | The total number of failures occurred during transaction id generation and R4 Location Update Request messages not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4locupdreq-totrec | The total number of R4 Location Update Request messages received on R4 interface. | Int32
r4locupdreq-totacc | The total number of R4 Location Update Request messages accepted on R4 interface. | Int32
r4locupdreq-totrelay | The total number of R4 Location Update Request messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Location Update Request message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4locupdreq-totdenied | The total number of R4 Location Update Request messages denied on R4 interface. | Int32
r4locupdreq-totdiscard | The total number of R4 Location Update Request messages discarded on R4 interface. | Int32
r4locupdreq-badform | The total number of badly formed R4 Location Update Request messages on R4 interface. | Int32
r4locupdreq-decodeerr | The total number of R4 Location Update Request messages on R4 interface with decode error. | Int32
r4locupdreq-unspecerr | The total number of R4 Location Update Request messages on R4 interface with unspecified error. | Int32
r4locupdreq-missmandtlv | The total number of R4 Location Update Request messages on R4 interface with missing mandatory TLVs. | Int32
r4locupdreq-tlvvalinval | The total number of R4 Location Update Request messages on R4 interface with invalid TLV value. | Int32
r4locupdreq-unknowntlv | The total number of R4 Location Update Request messages on R4 interface with unknown TLVs. | Int32
r4locupdreq-duptlvfound | The total number of R4 Location Update Request messages on R4 interface with duplicate TLVs. | Int32
r4locupdreq-nosessfound | The total number of R4 Location Update Request messages on R4 interface without any session information. | Int32
r4locupdreq-admprohibit | The total number of R4 Location Update Request messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Location Update Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4locupdreq-noresourcedrop | The total number of R4 Location Update Request messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Location Update Request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4locupdreq-transiderr | The total number of R4 Location Update Request messages on R4 interface with transaction ID errors. | Int32
r4locupdrsp-totsent | The total number of Location Update Responses sent to the peer ASNPC. | Int32
r4locupdrsp-retranssent | The total number of R4 Location Update Response messages re-transmitted on R4 interface. | Int32
r4locupdrsp-totsendfail | The total number of failures occurred during transaction id generation and R4 Location Update Response messages not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4locupdrsp-totrec | The total number of R4 Location Update Response messages received on R4 interface. | Int32
r4locupdrsp-totacc | The total number of R4 Location Update Response messages accepted on R4 interface. | Int32
r4locupdrsp-totrelay | The total number of R4 Location Update Response messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Location Update Response message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4locupdrsp-totdenied | The total number of R4 Location Update Response messages denied on R4 interface. | Int32
r4locupdrsp-totdiscard | The total number of R4 Location Update Response messages discarded on R4 interface. | Int32
r4locupdrsp-badform | The total number of badly formed R4 Location Update Response messages on R4 interface. | Int32
r4locupdrsp-decodeerr | The total number of R4 Location Update Response messages on R4 interface with decode error. | Int32
r4locupdrsp-unspecerr | The total number of R4 Location Update Response messages on R4 interface with unspecified error. | Int32
r4locupdrsp-missmandtlv | The total number of R4 Location Update Response messages on R4 interface with missing mandatory TLVs. | Int32
r4locupdrsp-tlvvalinval | The total number of R4 Location Update Response messages on R4 interface with invalid TLV value. | Int32
r4locupdrsp-unknowntlv | The total number of R4 Location Update Response messages on R4 interface with unknown TLVs. | Int32
r4locupdrsp-duptlvfound | The total number of R4 Location Update Response messages on R4 interface with duplicate TLVs. | Int32
r4locupdrsp-nosessfound | The total number of R4 Location Update Response messages on R4 interface without any session information. | Int32
r4locupdrsp-admprohibit | The total number of R4 Location Update Response messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Location Update Response message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4locupdrsp-noresourcedrop | The total number of R4 Location Update Response messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Location Update Response message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4locupdrsp-transiderr | The total number of R4 Location Update Response messages on R4 interface with transaction ID errors. | Int32
r4locupdcnf-totsent | The total number of Location Update Confirmations sent to the peer ASNPC. | Int32
r4locupdcnf-retranssent | The total number of R4 Location Update Confirmation messages re-transmitted on R4 interface. | Int32
r4locupdcnf-totsendfail | The total number of failures occurred during transaction id generation and R4 Location Update Confirmation messages not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4locupdcnf-totrec | The total number of R4 Location Update Confirmation messages received on R4 interface. | Int32
r4locupdcnf-totacc | The total number of R4 Location Update Confirmation messages accepted on R4 interface. | Int32
r4locupdcnf-totrelay | The total number of R4 Location Update Confirmation messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Location Update Confirmation message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4locupdcnf-totdenied | The total number of R4 Location Update Confirmation messages denied on R4 interface. | Int32
r4locupdcnf-totdiscard | The total number of R4 Location Update Confirmation messages discarded on R4 interface. | Int32
r4locupdcnf-badform | The total number of badly formed R4 Location Update Confirmation messages on R4 interface. | Int32
r4locupdcnf-decodeerr | The total number of R4 Location Update Confirmation messages on R4 interface with decode error. | Int32
r4locupdcnf-unspecerr | The total number of R4 Location Update Confirmation messages on R4 interface with unspecified error. | Int32
r4locupdcnf-missmandtlv | The total number of R4 Location Update Confirmation messages on R4 interface with missing mandatory TLVs. | Int32
r4locupdcnf-tlvvalinval | The total number of R4 Location Update Confirmation messages on R4 interface with invalid TLV value. | Int32
r4locupdcnf-unknowntlv | The total number of R4 Location Update Confirmation messages on R4 interface with unknown TLVs. | Int32
r4locupdcnf-duptlvfound | The total number of R4 Location Update Confirmation messages on R4 interface with duplicate TLVs. | Int32
r4locupdcnf-nosessfound | The total number of R4 Location Update Confirmation messages on R4 interface without any session information. | Int32
r4locupdcnf-admprohibit | The total number of R4 Location Update Confirmation messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Location Update Confirmation message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4locupdcnf-noresourcedrop | The total number of R4 Location Update Confirmation messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Location Update Confirmation message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4locupdcnf-transiderr | The total number of R4 Location Update Confirmation messages on R4 interface with transaction ID errors. | Int32
r4pcrelocind-totsent | The total number of PC Relocation Indicator messages sent to the ASNGW on the R4 interface. | Int32
r4pcrelocind-retranssent | The total number of R4 PC Relocation Indicator messages re-transmitted on R4 interface. | Int32
r4pcrelocind-totsendfail | The total number of failures occurred during transaction id generation and R4 PC Relocation Indicator messages not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4pcrelocind-totrec | The total number of R4 PC Relocation Indicator messages received on R4 interface. | Int32
r4pcrelocind-totacc | The total number of R4 PC Relocation Indicator messages accepted on R4 interface. | Int32
r4pcrelocind-totrelay | The total number of R4 PC Relocation Indicator messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 PC Relocation Indicator message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4pcrelocind-totdenied | The total number of R4 PC Relocation Indicator messages denied on R4 interface. | Int32
r4pcrelocind-totdiscard | The total number of R4 PC Relocation Indicator messages discarded on R4 interface. | Int32
r4pcrelocind-badform | The total number of badly formed R4 PC Relocation Indicator messages on R4 interface. | Int32
r4pcrelocind-decodeerr | The total number of R4 PC Relocation Indicator messages on R4 interface with decode error. | Int32
r4pcrelocind-unspecerr | The total number of R4 PC Relocation Indicator messages on R4 interface with unspecified error. | Int32
r4pcrelocind-missmandtlv | The total number of R4 PC Relocation Indicator messages on R4 interface with missing mandatory TLVs. | Int32
r4pcrelocind-tlvvalinval | The total number of R4 PC Relocation Indicator messages on R4 interface with invalid TLV value. | Int32
r4pcrelocind-unknowntlv | The total number of R4 PC Relocation Indicator messages on R4 interface with unknown TLVs. | Int32
r4pcrelocind-duptlvfound | The total number of R4 PC Relocation Indicator messages on R4 interface with duplicate TLVs. | Int32
r4pcrelocind-nosessfound | The total number of R4 PC Relocation Indicator messages on R4 interface without any session information. | Int32
r4pcrelocind-admprohibit | The total number of R4 PC Relocation Indicator messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 PC Relocation Indicator message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4pcrelocind-noresourcedrop | The total number of R4 PC Relocation Indicator messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 PC Relocation Indicator message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4pcrelocind-transiderr | The total number of R4 PC Relocation Indicator messages on R4 interface with transaction ID errors. | Int32
r4pcrelocack-totsent | The total number of PC Relocation Acknowledgement messages sent to the ASNGW. | Int32
r4pcrelocack-retranssent | The total number of PC Relocation Acknowledgement messages retransmitted on the R4 interface to the ASNGW. | Int32
r4pcrelocack-totsendfail | The total number of PC Relocation Acknowledgement message failures sent to the ASNGW and relayed on the R4 interface. This counter is used to count the error while sending the R4 packets. | Int32
r4pcrelocack-totrec | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW. | Int32
r4pcrelocack-totacc | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW | Int32
r4pcrelocack-totrelay | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW and relayed on the R4 interface. Triggers: Changes every time an R4 Idle Mode Exit State Indication message is relayed by the R4 interface. Availability: across all ASNGW services | Int32
r4pcrelocack-totdenied | The total number of PC Relocation Acknowledgement messages sent to the ASNGW that were denied on the R4 interface | Int32
r4pcrelocack-totdiscard | The total number of PC Relocation Acknowledgement messages sent to the ASNGW that were discarded on the R4 interface. | Int32
r4pcrelocack-badform | The total number of badly formed R4 PC Relocation Acknowledgement messages sent to the ASNGW. | Int32
r4pcrelocack-decodeerr | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW with decode errors. | Int32
r4pcrelocack-unspecerr | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW with unspecified errors. | Int32
r4pcrelocack-missmandtlv | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW with missing mandatory TLVs. | Int32
r4pcrelocack-tlvvalinval | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW with an invalid TLV. | Int32
r4pcrelocack-unknowntlv | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW with an unknown TLV. | Int32
r4pcrelocack-duptlvfound | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW with duplicate TLVs. | Int32
r4pcrelocack-nosessfound | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW without any session information. | Int32
r4pcrelocack-admprohibit | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW that were discarded or denied due to admin prohibit. Triggers: Changes every time an R4 PC Relocation Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASN GW services. | Int32
r4pcrelocack-noresourcedrop | The total number of R4 PC Relocation Acknowledgement messages sent to the ASNGW that were discarded or denied due to resource unavailability. Triggers: Changes every time an R4 PC Relocation Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all ASN GW services. | Int32
r4pcrelocack-transiderr | The total number of R4 IPC Relocation Acknowledgement messages sent to the ASNGW with a transaction ID error. | Int32
r4contextreq-totsent | The total number of Context Request messages sent to the ASNGW. | Int32
r4contextreq-retranssent | The total number of Context Request messages re-transmitted to the ASNGW on R4 interface. | Int32
r4contextreq-totsendfail | The total number of failures that occurred during transaction ID generation and R4 Context Request message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4contextreq-totrec | The total number of Context Request messages received by the ASNGW on R4 interface. | Int32
r4contextreq-totacc | The total number of Context Request messages accepted by the ASNGW on R4 interface. | Int32
r4contextreq-totrelay | The total number of Context Request messages received on the ASNGW from the base station and relayed on the R4 interface. Triggers: Changes every time a Context Request message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4contextreq-totdenied | The total number of Context Request messages denied by the ASNGW on R4 interface. | Int32
r4contextreq-totdiscard | The total number of Context Request messages discarded by the ASNGW on R4 interface. | Int32
r4contextreq-badform | The total number of badly formed Context Request messages on R4 interface. | Int32
r4contextreq-decodeerr | The total number of Context Request messages on R4 interface with decode error. | Int32
r4contextreq-unspecerr | The total number of Context Request messages on R4 interface with unspecified error. | Int32
r4contextreq-missmandtlv | The total number of Context Request messages on R4 interface with missing mandatory TLVs. | Int32
r4contextreq-tlvvalinval | The total number of Context Request messages on R4 interface with invalid TLV value. | Int32
r4contextreq-unknowntlv | The total number of Context Request messages on R4 interface with unknown TLVs. | Int32
r4contextreq-duptlvfound | The total number of Context Request messages on R4 interface with duplicate TLV values. | Int32
r4contextreq-nosessfound | The total number of Context Request messages on R4 interface without any session information. | Int32
r4contextreq-adminprohib | The total number of Context Request messages discarded or denied due to admin prohibit. Triggers: Changes every time a Context Request message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4contextreq-noresourcedrop | The total number of Context Request messages discarded or denied due to resource unavailability. Triggers: Changes every time a Context Request message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service. | Int32
r4contextreq-transiderr | The total number of Context Request messages on R4 interface with transaction ID errors. | Int32
r4contextrpt-totsent | The total number of Context Report messages sent to the ASNGW. | Int32
r4contextrpt-retranssent | The total number of Context Report messages re-transmitted to the ASNGW on R4 interface. | Int32
r4contextrpt-totsendfail | The total number of failures that occurred during transaction ID generation and R4 Context Report message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4contextrpt-totrec | The total number of Context Report messages received by the ASNGW on R4 interface. | Int32
r4contextrpt-totacc | The total number of Context Report messages accepted by the ASNGW on R4 interface. | Int32
r4contextrpt-totrelay | The total number of Context Report messages received on the ASNGW from the base station and relayed on the R4 interface. Triggers: Changes every time a Context Report message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4contextrpt-totdenied | The total number of Context Report messages denied by the ASNGW on R4 interface. | Int32
r4contextrpt-totdiscard | The total number of Context Report messages discarded by the ASNGW on R4 interface. | Int32
r4contextrpt-badform | The total number of badly formed Context Report messages on R4 interface. | Int32
r4contextrpt-decodeerr | The total number of Context Report messages on R4 interface with decode error. | Int32
r4contextrpt-unspecerr | The total number of Context Report messages on R4 interface with unspecified error. | Int32
r4contextrpt-missmandtlv | The total number of Context Report messages on R4 interface with missing mandatory TLVs. | Int32
r4contextrpt-tlvvalinval | The total number of Context Report messages on R4 interface with invalid TLV value. | Int32
r4contextrpt-unknowntlv | The total number of Context Report messages on R4 interface with unknown TLVs. | Int32
r4contextrpt-duptlvfound | The total number of Context Report messages on R4 interface with duplicate TLV values. | Int32
r4contextrpt-nosessfound | The total number of Context Report messages on R4 interface without any session information. | Int32
r4contextrpt-adminprohib | The total number of Context Report messages discarded or denied due to admin prohibit. Triggers: Changes every time a Context Report message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4contextrpt-noresourcedrop | The total number of Context Report messages discarded or denied due to resource unavailability. Triggers: Changes every time a Context Report message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service. | Int32
r4contextrpt-transiderr | The total number of Context Report messages on R4 interface with transaction ID errors. | Int32
r4cmackeycountupd-totsent | The total number of CMAC Key Count Update messages sent to the ASNGW. | Int32
r4cmackeycountupd-retranssent | The total number of CMAC Key Count Update messages re-transmitted on R4 inter | Int32
r4cmackeycountupd-totsendfail | The total number of failures occurred during transaction ID generation and R4 CMAC Key Count Update message not sent for specific interface. This counter is used to count the error while sending the R4 packets. | Int32
r4cmackeycountupd-totrec | The total number of CMAC Key Count Update messages received on R4 interface. | Int32
r4cmackeycountupd-totacc | The total number of CMAC Key Count Update messages accepted on R4 interface. | Int32
r4cmackeycountupd-totrelay | The total number of CMAC Key Count Update messages received from the base station and relayed on the R4 interface. Triggers: Changes every time a CMAC Key Count Update message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4cmackeycountupd-totdenied | The total number of CMAC Key Count Update messages denied on R4 interface. | Int32
r4cmackeycountupd-totdiscard | The total number of CMAC Key Count Update messages discarded on R4 interface. | Int32
r4cmackeycountupd-badform | The total number of badly formed CMAC Key Count Update messages on R4 interface. | Int32
r4cmackeycountupd-decodeerr | The total number of CMAC Key Count Update messages on R4 interface with decode error. | Int32
r4cmackeycountupd-unspecerr | The total number of CMAC Key Count Update messages on R4 interface with unspecified error. | Int32
r4cmackeycountupd-missmandtlv | The total number of CMAC Key Count Update messages on R4 interface with missing mandatory TLVs. | Int32
r4cmackeycountupd-tlvvalinval | The total number of CMAC Key Count Update messages on R4 interface with invalid TLV value. | Int32
r4cmackeycountupd-unknowntlv | The total number of CMAC Key Count Update messages on R4 interface with unknown TLVs. | Int32
r4cmackeycountupd-duptlvfound | The total number of CMAC Key Count Update messages on R4 interface with duplicate TLVs. | Int32
r4cmackeycountupd-nosessfound | The total number of CMAC Key Count Update messages on R4 interface without any session information. | Int32
r4cmackeycountupd-adminprohib | The total number of CMAC Key Count Update messages discarded or denied due to admin prohibit. Triggers: Changes every time a CMAC Key Count Update message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4cmackeycountupd-noresourcedrop | The total number of CMAC Key Count Update messages discarded or denied due to resource unavailability. Triggers: Changes every time a CMAC Key Count Update message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4cmackeycountupd-transiderr | The total number of CMAC Key Count Update messages on R4 interface with transaction ID errors. | Int32
r4cmackeycountack-totsent | The total number of CMAC Key Count Acknowledgement messages sent to the ASNGW. | Int32
r4cmackeycountack-retranssent | The total number of CMAC Key Count Acknowledgement messages re-transmitted on R6 interface | Int32
r4cmackeycountack-totsendfail | The total number of failures occurred during transaction ID generation and R6 CMAC Key Count Acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets | Int32
r4cmackeycountack-totrec | The total number of failures occurred during transaction ID generation and R6 CMAC Key Count Acknowledgement message not sent for specific interface. This counter is used to count the error while sending the R6 packets | Int32
r4cmackeycountack-totacc | The total number of CMAC Key Count Acknowledgement messages accepted on R6 interface. | Int32
r4cmackeycountack-totrelay | The total number of CMAC Key Count Acknowledgement messages received from the base station and relayed on the R6 interface. Triggers: Changes every time a CMAC Key Count Acknowledgement message is relayed by the R6 interface. Availability: across all ASNGW services. | Int32
r4cmackeycountack-totdenied | The total number of CMAC Key Count Acknowledgement messages denied on R6 interface. | Int32
r4cmackeycountack-totdiscard | The total number of CMAC Key Count Acknowledgement messages discarded on R6 interface. | Int32
r4cmackeycountack-badform | The total number of badly formed CMAC Key Count Acknowledgement messages on R6 interface. | Int32
r4cmackeycountack-decodeerr | The total number of CMAC Key Count Acknowledgement messages on R6 interface with decode error. | Int32
r4cmackeycountack-unspecerr | The total number of CMAC Key Count Acknowledgement messages on R6 interface with unspecified error. | Int32
r4cmackeycountack-missmandtlv | The total number of CMAC Key Count Acknowledgement messages on R6 interface with missing mandatory TLVs. | Int32
r4cmackeycountack-tlvvalinval | The total number of CMAC Key Count Acknowledgement messages on R6 interface with invalid TLV value. | Int32
r4cmackeycountack-unknowntlv | The total number of CMAC Key Count Acknowledgement messages on R6 interface with unknown TLVs. | Int32
r4cmackeycountack-duptlvfound | The total number of CMAC Key Count Acknowledgement messages on R6 interface with duplicate TLVs. | Int32
r4cmackeycountack-nosessfound | The total number of CMAC Key Count Acknowledgement messages on R6 interface without any session information. | Int32
r4cmackeycountack-adminprohib | The total number of CMAC Key Count Acknowledgement messages discarded or denied due to admin prohibit. Triggers: Changes every time a CMAC Key Count Acknowledgement message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4cmackeycountack-noresourcedrop | The total number of CMAC Key Count Acknowledgement messages discarded or denied due to resource unavailability. Triggers: Changes every time a CMAC Key Count Acknowledgement message is discarded or denied due to resource unavailability. Availability: across all the ASNGW services. | Int32
r4cmackeycountack-transiderr | The total number of CMAC Key Count Acknowledgement messages on R6 interface with transaction ID errors. | Int32
r4unknown-totrec | The total number of Unknown messages received on the R4 interface. | Int32
r4unknown-totacc | The total number of Unknown messages accepted on R4 interface. | Int32
r4unknown-totrelay | The total number of R4 Unknown messages received from the base station and relayed on the R4 interface. Triggers: Changes every time an R4 Unknown message is relayed by the R4 interface. Availability: across all ASNGW services. | Int32
r4unknown-totdenied | The total number of Unknown messages denied on the R4 interface. | Int32
r4unknown-totdiscard | The total number of Unknown messages discarded on R4 interface. | Int32
r4unknown-badform | The total number of Unknown badly formed messages on the R4 interface. | Int32
r4unknown-decodeerr | The total number of Unknown decode errors on R4 interface. | Int32
r4unknown-unspecerr | The total number of Unknown messages with unspecified errors on R4 interface. | Int32
r4unknown-missmandtlv | The total number of Unknown messages on R4 interface with missing TLVs. | Int32
r4unknown-tlvvalinval | The total number of Unknown messages on R4 interface with invalid TLV values. | Int32
r4unknown-unknowntlv | The total number of Unknown messages on R4 interface with unknown TLVs. | Int32
r4unknown-duptlvfound | The total number of Unknown messages on R4 interface with duplicate TLV values. | Int32
r4unknown-nosessfound | The total number of Unknown messages on R4 interface with no session information. | Int32
r4unknown-admprohibit | The total number of R4 Unknown messages discarded or denied due to admin prohibit. Triggers: Changes every time an R4 Unknown message is discarded or denied due to admin prohibit. Availability: across all ASNGW services. | Int32
r4unknown-noresourcedrop | The total number of R4 Unknown messages discarded or denied due to resource unavailability. Triggers: Changes every time an R4 Unknown message is discarded or denied due to resource unavailability. Availability: across all the ASNGW service | Int32
r4unknown-transiderr | The total number of R4 Unknown messages with transaction ID errors. | Int32
total-sessions-connected | The total number of active sessions currently connected through the ASN PC. | Int32
IMPORTANT: For information on statistics that are common to all schema see the Statistics and Counters Overview chapter.