# show congestion-control

This chapter includes the show congestion-control command output tables.
show congestion-control statistics a11mgr instance
Table 1. show congestion-control statistics a11mgr instance Command Output Descriptions

Field | Description
--- | ---
Current congestion status | The current congestion control state as “Cleared” or “Applied”.
Congestion applied | Displays the number of times the system invoked a congestion control policy for the specified service type.
Congestion Control Resource Limits | Indicates the congestion control threshold that was triggered. For more information, refer to the congestion-control threshold command in the Global Configuration Mode chapter of the Command Line Interface Reference.

show congestion-control statistics asngwmgr instance
Table 2. show congestion-control statistics asngwmgr instance Command Output Descriptions

Field | Description
--- | ---
Current congestion status | The current congestion control state as “Cleared” or “Applied”.
Congestion applied | Displays the number of times the system invoked a congestion control policy for the specified service type.
Congestion Control Resource Limits | Indicates the congestion control threshold that was triggered. For more information, refer to the congestion-control threshold command in the Global Configuration Mode chapter of the Command Line Interface Reference.
system cpu use exceeded | Indicates the number of time the ASNGW Manager exceeded the system CPU usage limit.
service cpu use exceeded | Indicates the number of time the ASNGW Manager exceeded the CPU usage limit specified for this service.
system memory use exceeded | Indicates the number of time the ASNGW Manager exceeded the allocated system memory usage limit.
port rx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Rx port usage limit.
port tx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Tx port usage limit.
port specific rx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Rx port usage limit for a specific port number.
port specific tx use exceeded | Indicates the number of time the ASNGW Manager exceeded the Tx port usage limit for a specific port number.
max sess use exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum session usage limit for a service.
license use exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum license usage limit.
msg queue size use exceeded | Indicates the number of time the ASNGW Manager exceeded the message queue size usage.
msg queue wait time exceeded | Indicates the number of time the ASNGW Manager exceeded the message queue wait time.
license threshold exceeded | Indicates the number of time the ASNGW Manager exceeded the license threshold limit.
max sess threshold exceeded | Indicates the number of time the ASNGW Manager exceeded the maximum session threshold limit.
Sessions disconnected due to overload disconnect | Indicates the total number of sessions disconnected due to overload.

show congestion-control statistics mme full
Table 3. show congestion-control statistics mme full Command Output Descriptions

Field | Description
--- | ---
Critical/Major/Minor Congestion Policy Action | This section provides statistics for the Critical, Major or Minor congestion policy actions that were triggered for the MME.
Congestion Policy Applied | Displays the number of times the system invoked a congestion control policy.
PS attaches rejected/dropped | Indicates the number of packet switched Attach requests that were rejected/dropped.
Combined attaches rejected/dropped | Indicates the number of Combined Attach requests that were rejected/dropped.
S1-Setup rejected/dropped | Indicates the number of S1-Setup attempts that were rejected/dropped.
Handover rejected/dropped | Indicates the number of handover attempts that were rejected/dropped.
Addn-pdn-connect rejected/dropped | Indicates the number of additional PDN context connection attempts that were rejected/dropped.
Addn-brr-connect rejected/dropped | Indicates the number of additional bearer requests that were rejected/dropped.
Service-Request rejected/dropped | Indicates the number of service requests that were rejected/dropped.
TAU-Request rejected/dropped | Indicates the number of TAU requests that were rejected/dropped.
S1AP Overload Start Sent | Indicates the number of S1AP Overload Start messages that were sent.
S1AP Overload Stop Sent | Indicates the number of S1AP Overload Stop messages that were sent.
Excluded Emergency Events | Indicates the number of emergency events that were excluded from the Congestion Control policy based on the configuration of the exclude-emergency-events command. These events were allowed to proceed during a congestion condition.
Excluded Voice Events | Indicates the number of voice calls that were excluded from the Congestion Control policy based on the configuration of the exclude-voice-events command. These calls were allowed to proceed when a congestion condition.