# show sgw

This chapter describes the output of the show sgw command.
show sgw-service all

Displays configuration information for all S-GW services configured on the system.
Table 1. show sgw-service all Command Output Descriptions

Field | Description
--- | ---
Service name | The name of the S-GW service.
Service-ID | The system generated identification number of the service.
Context | The context name where the service is located.
Accounting context | The context where the accounting configuration and or interfaces are configured.
Accounting mode | The accounting mode to be used for the S-GW service – GTTP (default), RADIUS/Diameter or none.
Status | The status of the service.
Egress Protocol | The egress protocol, such as “gtp-pmip”
Ingress EGTP service | The ingress eGTP service configured for this S-GW service.
Egress context | The egress context configured for this service.
Egress EGTP service | The egress eGTP service configured for this S-GW service.
Egress MAG service | The egress Mobile Access Gateway (MAG) service configured for this service.
IMS auth. service | The IMS authorization (IMSA) service used by this service for IMS subscribers.
Accounting policy | The name of the operator policy associated with accounting for this service.
Newcall policy | The newcall policy configured for this service.
QCI-QOS mapping table | The QoS Class Index to QoS mapping table configured for use with this service.
GTPC Path Failure Handling
S11-Interface | local-purge: The S-GW clears the affected bearer (or PDN if the path failure is received on a default bearer) locally without informing the peers. This is the default action for all interfaces. signal-peer: The S-GW initiates control signalling towards the peer MME and P-GW.
S5-Interface
S1U-Interface
S5U-Interface
S4U-Interface
S12-Interface
GTPU Error Indication Handling
S1U-Interface | local-purge: The S-GW clears the affected bearer (or PDN if the error indication is received on the default bearer) locally without informing the peers. page-ue: The S-GW moves the complete UE state to S1-Idle and starts paging for this UE. This is the default action for GTP-U error indication messages received on the S12 and S1-U interfaces.
S5U-Interface
S12-Interface
S4U-Interface
PLMN ID List | List of Public Land Mobile Network (PLMN) identifiers associated with the operator policy for this service. A PLMN ID consists of the Mobile Country Code (MCC) + Mobile network Code (MCC).
Subscriber Map Name | Name of the subscriber map associated with the operator policy for this service.

show sgw-service statistics all verbose
Table 2. show sgw-service statistics all Command Output Descriptions

Field | Description
--- | ---
Session Level Statistics
Current
UE
Idle | The total number of UE sessions currently idle.
Idle-ISR | The total number of Idle-mode Signaling Reduction UE sessions currently idle.
Active | The total number of UE sessions currently active.
Active-ISR | The total number of Idle-mode Signaling Reduction UE sessions currently active.
PDN | The total number of current PDN sessions.
Home | The total number of current home PDN sessions.
Roaming | The total number of current roaming PDN sessions.
Visiting | The total number of current visiting PDN sessions.
Bearers | The total number of current Bearers.
Ind-Fwd-Tunnels | Indirect forward tunneling: The total number of current tunnels.
Ind-Fwd-Bearers | Indirect forward tunneling: The total number of current bearers.
Traffic Policing
uplink pkts red | The total number of uplink packets marked red by the trTCM algorithm.
uplink bytes red | The total number of uplink bytes marked red by the trTCM algorithm.
uplink pkts yellow | The total number of uplink packets marked yellow by the trTCM algorithm.
uplink bytes yellow | The total number of uplink bytes marked yellow by the trTCM algorithm.
uplink pkts green | The total number of uplink packets marked green by the trTCM algorithm.
uplink bytes green | The total number of uplink bytes marked green by the trTCM algorithm.
uplink pkts dropped | The total number of uplink packets dropped due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
uplink bytes dropped | The total number of uplink bytes dropped due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
uplink pkts low ip prec | The total number of uplink packets that were transmitted after the IP precedence was lowered due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
uplink bytes low ip prec | The total number of uplink bytes that were transmitted after the IP precedence was lowered due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
uplink pkts transmitted | The total number of uplink packets that were transmitted even after exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
uplink bytes transmitted | The total number of uplink packets that were transmitted even after exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
downlink pkts red | The total number of downlink packets marked red by the trTCM algorithm.
downlink bytes red | The total number of downlink bytes marked red by the trTCM algorithm.
downlink pkts yellow | The total number of downlink packets marked yellow by the trTCM algorithm.
downlink bytes yellow | The total number of downlink bytes marked yellow by the trTCM algorithm.
downlink pkts green | The total number of downlink packets marked green by the trTCM algorithm.
downlink bytes green | The total number of downlink bytes marked green by the trTCM algorithm.
downlink pkts dropped | The total number of downlink packets dropped due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
downlink bytes dropped | The total number of downlink bytes dropped due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
downlink pkts low ip prec | The total number of downlink packets that were transmitted after the IP precedence was lowered due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
downlink bytes low ip prec | The total number of downlink bytes that were transmitted after the IP precedence was lowered due to exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
downlink pkts transmitted | The total number of downlink packets that were transmitted even after exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
downlink bytes transmitted | The total number of downlink packets that were transmitted even after exceeding or violating the Peak Information Rate (PIR) or the Committed Information Rate (CIR).
Setup
UE | The total number of UE session set up.
PDN | The total number of PDN sessions set up.
Bearers | The total number of bearers set up.
PDNs Setup Per PDN-type
IPv4 | The total number of PDN sessions set up using IPv4.
IPv6 | The total number of PDN sessions set up using IPv6.
IPv4v6 | The total number of PDN sessions set up using IPv4 in IPv6.
PDNs Setup Per Interface
S11 | The total number of PDN sessions set up on an S11 interface.
S4 | The total number of PDN sessions set up on an S4 interface.
PDNs Setup Per S5 Proto
GTP | The total number of PDN sessions set up using GTP tunneling.
PMIP | The total number of PDN sessions set up using PMIP tunneling.
PDNs Released
IPv4 | The total number of PDN sessions released using IPv4.
IPv6 | The total number of PDN sessions released using IPv6.
IPv4v6 | The total number of PDN sessions released using IPv4 in IPv6.
PDNs Released Reason
MME Ini | The total number of PDN sessions released - initiated by the MME.
PGW Ini | The total number of PDN sessions released - initiated by the P-GW.
PCRF Ini | The total number of PDN sessions released - initiated by the PCRF.
Local | The total number of PDN sessions released - initiated locally.
S1 Error Ind | The total number of PDN sessions released due to an S1 interface error.
S5 Error Ind | The total number of PDN sessions released due to an S5 interface error.
Path Failure S11 | The total number of PDN sessions released due to an S11 path failure.
Path Failure S1-U | The total number of PDN sessions released due to an S1-U path failure.
Path Failure S5 | The total number of PDN sessions released due to an S5 path failure.
Path Failure S5-U | The total number of PDN sessions released due to an S5-U path failure.
Path Failure S4 | The total number of PDN sessions released due to an S4 path failure.
Path Failure S4-U | The total number of PDN sessions released due to an S4-U path failure.
Path Failure S12 | The total number of PDN sessions released due to an S12 path failure.
Other | The total number of PDN sessions released due to other reasons.
PDNs Rejected
IPv4 | The total number of PDN sessions rejected using IPv4.
IPv6 | The total number of PDN sessions rejected using IPv6.
IPv4v6 | The total number of PDN sessions rejected using IPv4 in IPv6.
PDNs Rejected Reason
PGW Ini | The total number of PDN sessions rejected - initiated by the P-GW.
License | The total number of PDN sessions rejected due to license reasons.
Newcall | The total number of PDN sessions rejected due to newcall reasons.
Overload | The total number of PDN sessions rejected due to overload reasons.
Congestion | The total number of PDN sessions rejected due to congestion reasons.
Other | The total number of PDN sessions rejected due to other reasons.
ISR Statistics
Total ISR Activations
MME | The total number of ISR activations by an MME.
S4-SGSN | The total number of ISR activations by an S4-SGSN.
Total ISR Deactivations
MME | The total number of ISR deactivations by an MME.
S4-SGSN | The total number of ISR deactivations by an S4-SGSN.
Call Clear | The total number of ISR deactivations by a call clear.
Bearer Level Statistics
Total EPS Bearers Setup
QCI 1 - 9 | The total number of EPS bearers set up, with a QoS Class Index.
Non-Std QCI | The total number of EPS bearers set up, with a non-standard QoS Class Index.
Total EPS Bearers Released
QCI 1 - 9 | The total number of EPS bearers released, with a QoS Class Index.
Non-Std QCI | The total number of EPS bearers released, with a non-standard QoS Class Index.
Total EPS Bearers Modified |
QCI 1 - 9 | The total number of EPS bearers modified, with a QoS Class Index.
Non-Std QCI | The total number of EPS bearers modified, with a non-standard QoS Class Index.
Dedicated Bearers Released Reason
PGW Ini | The total number of dedicated bearers released - initiated by the P-GW.
PCRF Ini | The total number of dedicated bearers released - initiated by the PCRF.
S1 Error Ind | The total number of dedicated bearers released due to an S1 interface error.
S5 Error Ind | The total number of dedicated bearers released due to an S5 interface error.
S4-U Error Ind | The total number of dedicated bearers released due to an S4-U interface error.
S12 Error Ind | The total number of dedicated bearers released due to an S12 interface error.
Local | The total number of dedicated bearers released - initiated locally.
PDN Down | The total number of dedicated bearers released due to an inaccessible PDN.
Path Failure S1-U | The total number of dedicated bearers released due to an S1-U path failure.
Path Failure S5-U | The total number of dedicated bearers released due to an S5-U path failure.
Path Failure S4-U | The total number of dedicated bearers released due to an S4-U path failure.
Path Failure S12 | The total number of dedicated bearers released due to an S12U path failure.
Other | The total number of dedicated bearers released due to other reasons.
S1U Total Data Statistics
Uplink
Pkts | The total number of uplink packets over the S1-U interface.
Bytes | The total number of uplink bytes over the S1-U interface.
Dropped Pkts | The total number of dropped uplink packets over the S1-U interface.
Dropped Bytes | The total number of dropped uplink bytes over the S1-U interface.
Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
Downlink
Pkts | The total number of downlink packets over the S1-U interface.
Bytes | The total number of downlink bytes over the S1-U interface.
Dropped Pkts | The total number of dropped downlink packets over the S1-U interface.
Dropped Bytes | The total number of dropped downlink bytes over the S1-U interface.
Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
S4U Total Data Statistics
Uplink
Pkts | The total number of uplink packets over the S4-U interface.
Bytes | The total number of uplink bytes over the S4-U interface.
Dropped Pkts | The total number of dropped uplink packets over the S4-U interface.
Dropped Bytes | The total number of dropped uplink bytes over the S4-U interface.
Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
Downlink
Pkts | The total number of downlink packets over the S4-U interface.
Bytes | The total number of downlink bytes over the S4-U interface.
Dropped Pkts | The total number of dropped downlink packets over the S4-U interface.
Dropped Bytes | The total number of dropped downlink bytes over the S4-U interface.
Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
S12 Total Data Statistics
Uplink
Pkts | The total number of uplink packets over the S12 interface.
Bytes | The total number of uplink bytes over the S12 interface.
Dropped Pkts | The total number of dropped uplink packets over the S12 interface.
Dropped Bytes | The total number of dropped uplink bytes over the S12 interface.
Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
Downlink
Pkts | The total number of downlink packets over the S12 interface.
Bytes | The total number of downlink bytes over the S12 interface.
Dropped Pkts | The total number of dropped downlink packets over the S12 interface.
Dropped Bytes | The total number of dropped downlink bytes over the S12 interface.
Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
S5 Total Data Statistics
Uplink
Pkts | The total number of uplink packets over the S5 interface.
Bytes | The total number of uplink bytes over the S5 interface.
Dropped Pkts | The total number of dropped uplink packets over the S5 interface.
Dropped Bytes | The total number of dropped uplink bytes over the S5 interface.
Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
Downlink
Pkts | The total number of downlink packets over the S5 interface.
Bytes | The total number of downlink bytes over the S5 interface.
Dropped Pkts | The total number of dropped downlink packets over the S5 interface.
Dropped Bytes | The total number of dropped downlink bytes over the S5 interface.
Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
S8 Total Data Statistics
Uplink
Pkts | The total number of uplink packets over the S8 interface.
Bytes | The total number of uplink bytes over the S8 interface.
Dropped Pkts | The total number of dropped uplink packets over the S8 interface.
Dropped Bytes | The total number of dropped uplink bytes over the S8 interface.
Pkts QCI 0 - 8 | The total number of uplink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of uplink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of uplink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of uplink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped uplink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped uplink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped uplink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped uplink bytes with a non-standard QoS Class Index.
Non-Std QCI | The total number of uplink bytes dropped with a non-standard QoS Class Index.
Downlink
Pkts | The total number of downlink packets over the S8 interface.
Bytes | The total number of downlink bytes over the S8 interface.
Dropped Pkts | The total number of dropped downlink packets over the S8 interface.
Dropped Bytes | The total number of dropped downlink bytes over the S8 interface.
Pkts QCI 0 - 8 | The total number of downlink packets with a QoS Class Index.
Pkts Non-Std QCI | The total number of downlink packets with a non-standard QoS Class Index.
Bytes QCI 0 - 8 | The total number of downlink bytes with a QoS Class Index.
Bytes Non-Std QCI | The total number of downlink bytes with a non-standard QoS Class Index.
Dropped Pkts QCI 0 - 8 | The total number of dropped downlink packets with a QoS Class Index.
Dropped Pkts Non-Std QCI | The total number of dropped downlink packets with a non-standard QoS Class Index.
Dropped Bytes QCI 0 - 8 | The total number of dropped downlink bytes with a QoS Class Index.
Dropped Bytes Non-Std QCI | The total number of dropped downlink bytes with a non-standard QoS Class Index.
Inter-SGW Handover Statistics
PDNs Incoming
X2 Based | The total number of incoming X2-based PDNs.
Idle-mode TAU | The total number of incoming PDNs Incoming - Idle-mode TAU
S1 Based | The total number of incoming S1-based PDNs.
PDNs Outgoing | The total number of outgoing PDNs.
Intra-SGW Handover Statistics
Intra-MME | Intra-MME
Inter-MME | Inter-MME
Intra-SGSN | Intra-SGSN
Inter-SGSN | Inter-SGSN
MME-to-SGSN | MME-to-SGSN
SGSN-to-MME | SGSN-to-MME
Paging Statistics
Requests | The total number of paging requests.
Success | The total number of paging successes.
Rejects | The total number of paging rejects.
Failures | The total number of paging failures.
Active-Idle Ue Transitions | The total number of Active-Idle UE transitions
Idle-Active Ue Transitions | The total number of Idle-Active UE transitions
Paging Related Data Statistics
Packets Buffered | The total number of buffered paging packets.
Bytes Buffered | The total number of buffered paging bytes.
Packets Discarded | The total number of discarded paging packets.
Bytes Discarded | The total number of discarded paging bytes.
Idle Mode ACL Statistics
Packets Discarded | The total number of discarded paging packets due to ACL idle mode.
Bytes Discarded | The total number of discarded paging bytes due to ACL idle mode.
Indirect Forwarding Statistics
Tunnels Setup | The total number of indirect forwarding tunnels setup.
Tunnels Failed | The total number of failed indirect forwarding tunnels.
Tunnels Released | The total number of indirect forwarding tunnels released.
Bearers Setup | The total number of indirect forwarding bearers setup.
Bearers Released | The total number of indirect forwarding bearers released.
DL Packets Forwarded | The total number of indirect forwarding download packets forwarded.
DL Bytes Forwarded | The total number of indirect forwarding download bytes forwarded.
Source Violations
Packets Dropped | The total number of packets dropped due to source violations.
Bytes Dropped | The total number of bytes dropped due to source violations.
PDN PLMN Statistics
Home PDNs
PDNs active | The total number of home PDNs active.
PDNs setup | The total number of home PDNs setup.
PDNs released | The total number of home PDNs released.
Roaming PDNs
PDNs active | The total number of roaming PDNs active.
PDNs setup | The total number of roaming PDNs setup.
PDNs released | The total number of roaming PDNs released.
Visiting PDNs
PDNs active | The total number of visiting PDNs active.
PDNs setup | The total number of visiting PDNs setup.
PDNs released | The total number of visiting PDNs released.
Miscellaneous
Uplink Data Before MBReq | Uplink data before MBreq
CBReq Rcvd Before CSRsp | CBReq Rcvd before CSRsp