# WEM Application MIB

The following figure illustrates the hierarchical structure of the management information base (MIB) for the Web Element Manager.
MIB Textual Conventions

This section defines the objects, traps and conformances for the WEM MIB.
starentMIB(8164).starentMIBObjects(1).starentEMSMIB(1000). starEmsMIBObjects(1)
Object

starEmsNotifInfo

Object ID

enterprises.8164.1.1000.1.5

Description

A textual description of EMS notification, which potentially contains additional information (more than just the type of alarm). If the text of the message exceeds 64 bytes, the message will be truncated to 63 bytes and a '*' character will be appended to indicate the message has been truncated.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsNotifRaisedTime

Object ID

enterprises.8164.1.1000.1.6

Description

This object indicates the time when this notification was generated.

Syntax

TimeStamp

Access

Read-only
Object

starEmsProcMonThreshold

Object ID

enterprises.8164.1.1000.1.7

Description

This object indicates the current threshold value of process monitoring.

Syntax

DisplayString (SIZE (1..10))

Access

Read-only
Object

starEmsInterfaceAddr

Object ID

enterprises.8164.1.1000.1.8

Description

The object indicates the Interface address of host machine where EMS server is running

Syntax

InetAddress

Access

Read-only
Object

starEmsInterfaceName

Object ID

enterprises.8164.1.1000.1.9

Description

This object indicates the interface name of host machine where EMS server is running.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsIMGAddr

Object ID

enterprises.8164.1.1000.1.10

Description

The object indicates the IP address of IMG.

Syntax

InetAddress

Access

Read-only
Object

starEmsFtpFileName

Object ID

enterprises.8164.1.1000.1.11

Description

This object indicates name of the file which FTP’d and then deleted from the IMG.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsIMGState

Object ID

enterprises.8164.1.1000.1.12

Description

IMG state. unreachable(0) IMG is ICMP unreachable active(1) IMG is CORBA reachable inactive(1) IMG is CORBA unreachable reachable(0) IMG is ICMP reachable

Syntax

INTEGER

Access

Read-only

Enumeration

unreachable(0)

active(1)

inactive(2)

reachable(3)
Object

starEmsBulkStatFileXferTime

Object ID

enterprises.8164.1.1000.1.13

Description

The configured value of a Bulkstat file transfer in minutes.

Syntax

INTEGER(1..999999)

Access

Read-only
Object

starEmsXMLFtpFileName

IMPORTANT:

This attribute is obsolete.

Object ID

enterprises.8164.1.1000.1.14

Description

This object indicates name of the BulkStat XML file which is to be FTPed on the NMS.

Syntax

DisplayString (SIZE (1..256))

Access

Read-only
Object

starEmsXMLFtpDestAddr

Object ID

enterprises.8164.1.1000.1.15

Description

This object indicates destination IP address (NMS) for BulkStat XML file FTP.

Syntax

InetAddress

Access

Read-only
Object

starEmsXMLFtpDestPath

Object ID

enterprises.8164.1.1000.1.16

Description

This object indicates destination path where BulkStat XML file is to be FTP’d.

Syntax

DisplayString (SIZE (1..1024))

Access

Read-only
Object

starEmsIMGPreviousState

Object ID

enterprises.8164.1.1000.1.17

Description

IMG state. unmanageable(0) IMG is not CORBA reachable manageable(1) IMG is CORBA reachable

Syntax

INTEGER

Access

Read-only

Enumeration

unmanageable(0)

manageable(1)
Object

starEmsIMGName

Object ID

enterprises.8164.1.1000.1.18

Description

The object indicates the name of IMG.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsPortMonThreshold

Object ID

enterprises.8164.1.1000.1.19

Description

This object indicates the configured threshold value of port monitoring.

Syntax

DisplayString (SIZE (1..20))

Access

Read-only
Object

starEmsPortMonCurrent

Object ID

enterprises.8164.1.1000.1.20

Description

This object indicates the current threshold value of port monitoring.

Syntax

DisplayString (SIZE (1..20))

Access

Read-only
Object

starEmsTotalPendingEvts

Object ID

enterprises.8164.1.1000.1.21

Description

This object indicates the number of pending events for monitor in server queue.

Syntax

INTEGER(1..100000)

Access

Read-only
Object

starEmsMaxLimit

Object ID

enterprises.8164.1.1000.1.22

Description

This object indicates the limit of the server queue to store pending events.

Syntax

InetAddress

Access

Read-only
Object

starEmsClientAddr

Object ID

enterprises.8164.1.1000.1.23

Description

The object indicates the IP address of EMS Client.

Syntax

DisplayString (SIZE (1..256))

Access

Read-only
Object

starEmsMonOldEvtTimeStamp

Object ID

enterprises.8164.1.1000.1.24

Description

This object indicates the timestamp for last Monitor Pending Event.

Syntax

DisplayString (SIZE (1..256))

Access

Read-only
Object

starEmsMonitorType

Object ID

enterprises.8164.1.1000.1.25

Description

This object indicates the monitor type.

Syntax

INTEGER

Access

Read-only

Enumeration

protocol(0)

subscriber(1)
Object

starEmsMonitorUserName

Object ID

enterprises.8164.1.1000.1.26

Description

This object indicates the User name.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsDevicePath

Object ID

enterprises.8164.1.1000.1.27

Description

This object indicates the Device name.

Syntax

DisplayString (SIZE (1..1024))

Access

Read-only
Object

starEmsPrevHostName

Object ID

enterprises,8164.1.1000.1.28

Description

This object indicates the name of the previous host running EMS before failover.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsCurrHostName

Object ID

enterprises,8164.1.1000.1.29

Description

This object indicates the name of the current host running EMS.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsP2PProtocolType

Object ID

enterprises,8164.1.1000.1.30

Description

This object indicates the protocol type.

Syntax

INTEGER

Access

Read-only

Enumeration

ip(1)

tcp(2)

udp(3)

http(4)

htpps(5)

ftp(6)

ftpcontrol(7)

ftpdata(8)

wtp(9)

wsp(10)

dns(11)

icmp(12)

pop3(13)

sip(14)

sdp(15)

smtp(16)

mms(17)

filetransfer(18)

rtp(19)

rtsp(20)

imap(21)

totalp2p(22)

p2punknown(23)

p2pskype(24)

p2pbittorrent(25)

p2pedonkey(26)

p2pmsn(27)

p2pyahoo(28)

p2pporb(29)

p2pfasttrack(30)

p2pslingbox(31)

p2pvcast(32)

p2pgnutella(33)
Object

starEmsP2PProtocolVal

Object ID

enterprises,8164.1.1000.1.31

Description

This object indicates the protocol value.

Syntax

INTEGER

Access

Read-only

Enumeration

uplinkbytes(0)

downlinkbytes(1)

totalbytes(2)

uplinkpkts(3)

downlinkpkts(4)

totalpkts(5)

uplinkbytespercent(6)

downlinkbytespercent(7)

totalbytespercent(8)

uplinkpktspercent(9)

downlinkpktspercent(10)

totalpktspercent(11)
Object

starEmsSyslogLoggedTime

Object ID

enterprises,8164.1.1000.1.32

Description

This object indicates the logged time for the syslog message.

Syntax

TimeStamp

Access

Read-only
Object

starEmsSyslogFacility

Object ID

enterprises,8164.1.1000.1.33

Description

This object indicates the facility of syslog message.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsSyslogPriority

Object ID

enterprises,8164.1.1000.1.34

Description

This object indicates the syslog message priority.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsSyslogHostName

Object ID

enterprises,8164.1.1000.1.35

Description

This object indicates the hostname.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsSyslogKeyword

Object ID

enterprises,8164.1.1000.1.36

Description

This object indicates the keywords detected in the syslog message.

Syntax

DisplayString (SIZE (1..64))

Access

Read-only
Object

starEmsSyslogMessage

Object ID

enterprises,8164.1.1000.1.37

Description

This object indicates the syslog message contents.

Syntax

DisplayString (SIZE (1..1024))

Access

Read-only
Object

starEmsSyslogFilePath

Object ID

enterprises,8164.1.1000.1.38

Description

This object indicates the syslog message file path.

Syntax

DisplayString (SIZE (1..1024))

Access

Read-only
Object

starEmsDBName

Object ID

enterprises,8164.1.1000.1.39

Description

This object indicates the database name.

Syntax

DisplayString (SIZE (1..1024))

Access

Read-only
Object

starEmsBulkstatCounter

Object ID

enterprises,8164.1.1000.1.40

Description

This object indicates the bulkstat counter name.

Syntax

DisplayString (SIZE (1..1024))

Access

Read-only
Object

starEmsBulkStatRecordDetails

Object ID

enterprises,8164.1.1000.1.41

Description

This object indicates the bulkstat record detail information.

Syntax

DisplayString (SIZE (1..1024))

Access

Read-only
Object

starEmsBulkStatRecordTime

Object ID

enterprises,8164.1.1000.1.42

Description

This object indicates the bulkstat record time

Syntax

TimeStamp

Access

Read-only
Object

starEmsBulkStatThreshold

IMPORTANT:

This attribute is obsolete.

Object ID

enterprises,8164.1.1000.1.43

Description

This object indicates the configured threshold value of the bulkstat counter.

Syntax

INTEGER(0..100000)

Access

Read-only
Object

starEmsbulkStatCurrent

IMPORTANT:

This attribute is obsolete.

Object ID

enterprises,8164.1.1000.1.44

Description

This object indicates the current threshold (delta) value of the bulkstat counter.

Syntax

INTEGER(0..100000)

Access

Read-only
Object

starEMSCFMcrdbsHostAddress

Object ID

enterprises,8164.1.1000.1.45

Description

MCRDBS IP address

Syntax

InetAddress

Access

Read-Only
Object

starEMSCFDbType

Object ID

enterprises,8164.1.1000.1.46

Description

Type {

sfmdb(1) Starent Format Master DataBase.

sfmdbinc(2) Starent Format Master DataBase Incremental.

optcmdb(6) Optmized Customer Master DataBase.

optcmdbinc(7) Optmized Customer Master DataBase Incremental.

optcmbldb(14) Optmized Customer Master Blacklist DataBase

sfunkdb(5) Starent format unknown URL database

}

Syntax

INTEGER {

sfmdb(1),

sfmdbinc(2),

optcmdb(6),

optcmdbinc(7),

optcmbldb(14)

sfunkdb(5)

Access

Read-Only
Object

starEmsCFSourceDbFileName

Object ID

enterprises,8164.1.1000.1.47

Description

This object indicates name of the file whose SFTP/Conversion is failed.

Syntax

Displaystring (SIZE(1..64))

Access

Read-Only
Object

starEMSCFCdpHostAddress

Object ID

enterprises,8164.1.1000.1.48

Description

CDP IP Address

Syntax

InetAddress

Access

Read-Only
Object

starEMSCFFromDbType

Object ID

enterprises,8164.1.1000.1.49

Description

Type. sfmdb(1) Starent Format Master DataBase. sfmdbinc(2) Starent Format Master DataBase Incremental . blacklist(10) Blacklist DataBase. sfmbldb(11) Starent Format Master Blacklist DataBase.

Syntax

INTEGER

sfmdb(1),

sfmdbinc(2),

blacklist(10),

sfmbldb(11)

Access

Read-Only
Object

starEMSCFToDbType

Object ID

enterprises,8164.1.1000.1.50

Description

Databases Type {

optcmdb(6) Optmized Customer Master DataBase.

optcmdbinc(7) Optmized Customer Master DataBase Incremental.

sfmbldb(11) Starent Format Master Blacklist DataBase.

optcmbldb(14) Optmized Customer Master Blacklist DataBase.

}

Syntax

INTEGER

optcmdb(6),

optcmdbinc(7),

sfmbldb(11),

optcmbldb(14)

Access

Read-Only
Object

starEMSCFDestDbName

Object ID

enterprises,8164.1.1000.1.51

Description

This object indicates the name of the destination file, used to specify the destination file created after conversion.

Syntax

DisplayString (SIZE(1..64)

Access

Read-Only
Object

starEMSCFFtpHostInfo

Object ID

enterprises,8164.1.1000.1.52

Description

FTP host IP address

Syntax

DisplayString (SIZE(1..64))

Access

Read-Only
Object

starEMSBulkstatCounterValue

Object ID

enterprises,8164.1.1000.1.53

Description

Bulkstat counter current value

Syntax

Integer (0..100000)

Access

Read-Only
Object

starEmsBulkStatFilterDetails

Object ID

enterprises,8164.1.1000.1.54.

Description

This object indicates the bulkstat Threshold related filter combinations.

Syntax

DisplayString (SIZE (1..1024))

Access

read-only
Object

starEmsBulkStatCurrentDouble

Object ID

enterprises,8164.1.1000.1.55

Description

This object indicates the current threshold (delta) value of bulkstat counter.

Syntax

DisplayString (SIZE (1..1024))

Access

read-only
Object

starEmsBulkStatThresholdDouble

Object ID

enterprises,8164.1.1000.1.56.

Description

This object indicates the configured threshold value of bulkstat counter.

Syntax

DisplayString (SIZE (1..1024))

Access

read-only
Object

starEmsConfigBackupFileName

Object ID

enterprises,8164.1.1000.1.57.

Description

This object indicates name of the IMG configuration-file created during the config-backup operation.

Syntax

DisplayString (SIZE (1..256))

Access

read-only
starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000).starEmsTraps(2)
Object

starEmsFmEmailFailed

Object ID

enterprises.8164.1.1000.2.3

Description

This notification is generated when EMS fault management module email notification failure has occurred.

Objects

starEmsNotifRaisedTime

starEmsNotifInfo
Object

starEmsFmScriptFailed

Object ID

enterprises.8164.1.1000.2.4

Description

This notification is generated when EMS fault management module script execution failure has occurred.

Objects

starEmsNotifRaisedTime

starEmsNotifInfo
Object

starEmsFmSyslogFailed

Object ID

enterprises.8164.1.1000.2.5

Description

This notification is generated when EMS fault management module syslog message logging failure has occurred.

Objects

starEmsNotifRaisedTime

starEmsNotifInfo
Object

starEmsWebServerProcStart

Object ID

enterprises.8164.1.1000.2.6

Description

This notification is generated by EMS Process Monitoring when EMS web server process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsWebServerProcStop

Object ID

enterprises.8164.1.1000.2.7

Description

This notification is generated by EMS Process Monitoring when EMS web server process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsWebServerProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.8

Description

This notification is generated by EMS Process Monitoring when EMS web server process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS web server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsWebServerProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.9

Description

This notification is generated by EMS Process Monitoring when EMS web server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS web server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsDataBaseProcStart

Object ID

enterprises.8164.1.1000.2.10

Description

This notification is generated by EMS Process Monitoring when EMS data base process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsDataBaseProcStop

Object ID

enterprises.8164.1.1000.2.11

Description

This notification is generated by EMS Process Monitoring when EMS data base process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsDataBaseProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.12

Description

This notification is generated by EMS Process Monitoring when EMS data base process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS data base process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsDataBaseProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.13

Description

This notification is generated by EMS Process Monitoring when EMS data base process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS data base process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsServerProcStart

Object ID

enterprises.8164.1.1000.2.14

Description

This notification is generated by EMS Process Monitoring when EMS server process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsServerProcStop

Object ID

enterprises.8164.1.1000.2.15

Description

This notification is generated by EMS Process Monitoring when EMS server process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsServerProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.16

Description

This notification is generated by EMS Process Monitoring when EMS server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsServerProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.17

Description

This notification is generated by EMS Process Monitoring when EMS server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsScriptServerProcStart

Object ID

enterprises.8164.1.1000.2.18

Description

This notification is generated by EMS Process Monitoring when EMS script server process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsScriptServerProcStop

Object ID

enterprises.8164.1.1000.2.19

Description

This notification is generated by EMS Process Monitoring when EMS script server process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsScriptServerProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.20

Description

This notification is generated by EMS Process Monitoring when EMS script server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS script server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsScriptServerProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.21

Description

This notification is generated by EMS Process Monitoring when EMS script server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS script server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsServerDirAccessible

Object ID

enterprises.8164.1.1000.2.22

Description

This notification is generated by EMS Process Monitoring when EMS server directory becomes accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsServerDirNonAccessible

Object ID

enterprises.8164.1.1000.2.23

Description

This notification is generated by EMS Process Monitoring when EMS server directory is not accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsServerDirUsageOverLimit

Object ID

enterprises.8164.1.1000.2.24

Description

This notification is generated by EMS Process Monitoring when EMS server directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS server directory size usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsServerDirUsageNormal

Object ID

enterprises.8164.1.1000.2.25

Description

This notification is generated by EMS Process Monitoring when EMS server directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS server directory size usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsDataBaseDirAccessible

Object ID

enterprises.8164.1.1000.2.26

Description

This notification is generated by EMS Process Monitoring when EMS data base directory becomes accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsDataBaseDirNonAccessible

Object ID

enterprises.8164.1.1000.2.27

Description

This notification is generated by EMS Process Monitoring when EMS data base directory is not accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsDataBaseDirUsageOverLimit

Object ID

enterprises.8164.1.1000.2.28

Description

This notification is generated by EMS Process Monitoring when EMS data base directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS data base directory size value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsDataBaseDirUsageNormal

Object ID

enterprises.8164.1.1000.2.29

Description

This notification is generated by EMS Process Monitoring when EMS data base directory size usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS data base directory size usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsFTPDirAccessible

Object ID

enterprises.8164.1.1000.2.30

Description

This notification is generated by EMS Process Monitoring when EMS FTP directory becomes accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsFTPDirNonAccessible

Object ID

enterprises.8164.1.1000.2.31

Description

This notification is generated by EMS Process Monitoring when EMS FTP directory is not accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsFTPDirUsageOverLimit

Object ID

enterprises.8164.1.1000.2.32

Description

This notification is generated by EMS Process Monitoring when EMS FTP directory usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS FTP directory usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsFTPDirUsageNormal

Object ID

enterprises.8164.1.1000.2.33

Description

This notification is generated by EMS Process Monitoring when EMS FTP directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS FTP directory size usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsBlkArchDirAccessible

Object ID

enterprises.8164.1.1000.2.34

Description

This notification is generated by EMS Process Monitoring when EMS bulk archive directory becomes accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsBlkArchDirNonAccessible

Object ID

enterprises.8164.1.1000.2.35

Description

This notification is generated by EMS Process Monitoring when EMS bulk archive directory is not accessible.

Objects

starEmsNotifRaisedTime
Object

starEmsBlkArchDirUsageOverLimit

Object ID

enterprises.8164.1.1000.2.36

Description

This notification is generated by EMS Process Monitoring when EMS bulk archive directory size usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS bulk archive directory size value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsBlkArchDirUsageNormal

Object ID

enterprises.8164.1.1000.2.37

Description

This notification is generated by EMS Process Monitoring when EMS bulk archive directory size usage threshold is comes to normal value. The starEmsThreshold varbind indicates current EMS bulk archive directory size usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsInterfaceStateUp

Object ID

enterprises.8164.1.1000.2.38

Description

This notification is generated by EMS Process Monitoring when EMS interface state comes up. Varbinds indicate interface IP address and name.

Objects

starEmsNotifRaisedTime

starEmsInterfaceAddr

starEmsInterfaceName
Object

starEmsInterfaceStateDown

Object ID

enterprises.8164.1.1000.2.39

Description

This notification is generated by EMS Process Monitoring when EMS interface state goes down. Varbinds indicate interface address and name

Objects

starEmsNotifRaisedTime

starEmsInterfaceAddr

starEmsInterfaceName
Object

starEmsCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.40

Description

This notification is generated by EMS Process Monitoring when EMS CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS CPU usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.41

Description

This notification is generated by Process Monitoring when EMS CPU usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS CPU usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsSwapUsageOverLimit

Object ID

enterprises.8164.1.1000.2.42

Description

This notification is generated by Process Monitoring when EMS swap usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS swap usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsSwapUsageNormal

Object ID

enterprises.8164.1.1000.2.43

Description

This notification is generated by Process Monitoring when EMS swap usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS swap usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsPCFtpFailed

Object ID

enterprises.8164.1.1000.2.44

Description

This notification is generated by Periodic Configuration Saving module when FTP fails while fetching a config file from the IMG.

Objects

starEmsNotifRaisedTime

starEmsImgAddr

starEmsFtpFileName

starEmsNotifInfo
Object

starEmsPCFileDeletionFailed

Object ID

enterprises.8164.1.1000.2.45

Description

This notification is generated by Periodic Configuration Saving module when deletion of file on the IMG fails.

Objects

starEmsNotifRaisedTime

starEmsIMGAddr

starEmsFtpFileName

starEmsNotifInfo
Object

starEmsBulkStatFtpFailed

Object ID

enterprises.8164.1.1000.2.46

Description

This notification is generated by Bulkstat module when bulkstat file transfer operation from IMG fails or gets delayed than the expected time

Objects

starEmsNotifRaisedTime

starEmsBulkStatFileXferTime

starEmsIMGState

starEmsIMGAddr
Object

starEmsBulkStatFtpClear

Object ID

enterprises.8164.1.1000.2.47

Description

This notification is generated by BulkStat module when bulkstat file transfer operation from IMG succeeds and starEmsBulkStatFtpFailed trap is already raised for the IMG.

Objects

starEmsNotifRaisedTime

starEmsIMGAddr
Object

starEmsXMLFtpFailed

Object ID

enterprises.8164.1.1000.2.48

Description

This notification is generated by EMS when FTP of Bulkstat XML file on the NMS fails.

Objects

starEmsNotifRaisedTime

starEmsXMLFtpDestAddr

starEmsXMLFtpDestPath

starEmsNotifInfo
Object

starEmsXMLFtpSuccess

Object ID

enterprises.8164.1.1000.2.49

Description

This notification is generated by EMS when FTP of Bulk stat XML file on the NMS succeed.

Objects

starEmsNotifRaisedTime

starEmsXMLFtpDestAddr

starEmsXMLFtpDestPath

starEmsNotifInfo
Object

starEmsIMGUnmanageable

Object ID

enterprises.8164.1.1000.2.50

Description

This notification is generated by EMS when IMG becomes unmanageable.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsIMGAddr

starEmsIMGPreviousState
Object

starEmsIMGManageable

Object ID

enterprises.8164.1.1000.2.51

Description

This notification is generated by EMS when IMG becomes manageable.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsIMGAddr

starEmsIMGPreviousState
Object

starEmsPortMonThresholdBelowLimit

Object ID

enterprises.8164.1.1000.2.52

Description

This notification is generated by EMS Port Monitoring when delta value for a particular port has fallen below the configured threshold value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsIMGAddr

starSlotNum

starPortNum

starEmsPortMonThreshold

starEmsPortMonCurrent
Object

starEmsPortMonThresholdNormal

Object ID

enterprises.8164.1.1000.2.53

Description

This notification is generated by EMS Port Monitoring when delta value for a particular port threshold comes to normal value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsIMGAddr

starSlotNum

starPortNum

starEmsPortMonThreshold

starEmsPortMonCurrent
Object

starEmsPortMonError

Object ID

enterprises.8164.1.1000.2.54

Description

This notification is generated by EMS Port Monitoring when any error in fetching values from a particular IMG.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsIMGAddr

starEmsNotifInfo
Object

starEmsWebServerProcDetectRestart

Object ID

enterprises.8164.1.1000.2.55

Description

This notification is generated by EMS Process Monitoring when EMS web server process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsDataBaseProcDetectRestart

Object ID

enterprises.8164.1.1000.2.56

Description

This notification is generated by EMS Process Monitoring when EMS Data Base process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsServerProcDetectRestart

Object ID

enterprises.8164.1.1000.2.57

Description

This notification is generated by EMS Process Monitoring when EMS server process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsScriptServerProcDetectRestart

Object ID

enterprises.8164.1.1000.2.58

Description

This notification is generated by EMS Process Monitoring when EMS Script server process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsBulkStatServerProcStart

Object ID

enterprises.8164.1.1000.2.59

Description

This notification is generated by EMS Process Monitoring when Ems Bulkstat server process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsBulkStatServerProcStop

Object ID

enterprises.8164.1.1000.2.60

Description

This notification is generated by EMS Process Monitoring when Ems Bulkstat server process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsBulkStatServerProcDetectRestart

Object ID

enterprises.8164.1.1000.2.61

Description

This notification is generated by EMS Process Monitoring when Ems Bulkstat server process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsBulkStatServerProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.62

Description

This notification is generated by EMS Process Monitoring when EMS Bulkstat server process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS Bulkstat server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsBulkStatServerProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.63

Description

This notification is generated by EMS Process Monitoring when EMS Bulkstat server process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS Bulkstat server process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsBulkStatParserProcStart

Object ID

enterprises.8164.1.1000.2.64

Description

his notification is generated by EMS Process Monitoring when Ems Bulkstat parser process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsBulkStatParserProcStop

Object ID

enterprises.8164.1.1000.2.65

Description

This notification is generated by EMS Process Monitoring when Ems Bulkstat parser process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsBulkStatParserProcDetectRestart

Object ID

enterprises.8164.1.1000.2.66

Description

This notification is generated by EMS Process Monitoring when Ems Bulkstat parser process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsBulkStatParserProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.67

Description

This notification is generated by EMS Process Monitoring when EMS Bulkstat parser process cpu usage threshold is exceeded. The starEmsThreshold varbind indicates current EMS Bulkstat parser process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsBulkStatParserProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.68

Description

This notification is generated by EMS Process Monitoring when EMS Bulkstat parser process cpu usage threshold comes to normal value. The starEmsThreshold varbind indicates current EMS Bulkstat parser process cpu usage value in percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsIMGRateControlStart

Object ID

enterprises.8164.1.1000.2.69

Description

This notification is generated by EMS when IMG Rate-Control is stated. IMG's CORBA server resource utilization is over limit.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsIMGAddr
Object

starEmsIMGRateControlStop

Object ID

enterprises.8164.1.1000.2.70

Description

This notification is generated by EMS when IMG Rate-Control is stopped. IMG's CORBA server resource utilization is over limit.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsIMGAddr
Object

starEmsMonitorQueueFull

Object ID

enterprises.8164.1.1000.2.71

Description

This notification is generated by EMS when monitor event queue is full.

Objects

starEmsNotifRaisedTime

starEmsTotalPendingEvts

starEmsMaxLimit

starEmsClientAddr

starEmsMonOldEvtTimeStamp

starEmsMonitorType

starEmsMonitorUserName
Object

starEmsMonitorQueueInLimit

Object ID

enterprises.8164.1.1000.2.72

Description

This notification is generated by EMS when the monitor event queue is partially full.

Objects

starEmsNotifRaisedTime

starEmsTotalPendingEvts

starEmsMaxLimit

starEmsClientAddr

starEmsMonitorType

starEmsMonitorUserName
Object

starClusterFailoverHappened

Object ID

enterprises.8164.1.1000.2.73

Description

This notification is generated by EMS when cluster failover happens.

Objects

starEmsNotifRaisedTime

starEmsPrevHostName

starEmsCurrHostName
Object

starEmsDBBackupNoDiscSpace

Object ID

enterprises.8164.1.1000.2.74

Description

This notification is generated by EMS when disc space gets full. No disc space is available.

Objects

starEmsNotifRaisedTime

starEmsDevicePath
Object

starEMSP2PProtocolUsageHigh

Object ID

enterprises.8164.1.1000.2.75

Description

This notification is generated by EMS when protocol values are beyond the threshold value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsP2PProtocolType

starEmsP2PProtocolVal
Object

starEmsP2PProtocolUsageLimit

Object ID

enterprises.8164.1.1000.2.76

Description

This notification is generated by EMS when protocol values are within limit.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsP2PProtocolType

starEmsP2PProtocolVal
Object

starEmsKeywordDetectedInSyslog

Object ID

enterprises.8164.1.1000.2.77

Description

This notification is generated by EMS when a configured keyword is detected in the syslog message.

Objects

starEmsNotifRaisedTime

starEmsSyslogLoggedTime

starEmsSyslogFacility

starEmsSyslogPriority

starEmsSyslogHostname

starEmsSyslogKeyword

starEmsSyslogMessage

starEmsSyslogFilePath
Object

starEmsDBMigration

Object ID

enterprises.8164.1.1000.2.78

Description

This notification is generated by EMS when the database migration is done for a particular database.

Objects

starEmsNotifRaisedTime

starEmsDBName
Object

starEmsNBServerProcStart

Object ID

enterprises.8164.1.1000.2.79

Description

This notification is generated by EMS process monitoring when the EMS NB server process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsNBServerProcStop

Object ID

enterprises.8164.1.1000.2.80

Description

This notification is generated by EMS process monitoring when the EMS NB server process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsNBServerProcDetectRestart

Object ID

enterprises.8164.1.1000.2.81

Description

This notification is generated by EMS process monitoring when the EMS NB server process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsNBServerProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.82

Description

This notification is generated by EMS process monitoring when the NB server process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current NB server process CPU value as a percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsNBServerProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.83

Description

This notification is generated by EMS process monitoring when the NB server process CPU usage threshold comes to a normal value. The starEmsThreshold varbind indicates current NB server process cpu value as a percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsNotifyServiceProcStart

Object ID

enterprises.8164.1.1000.2.84

Description

This notification is generated by EMS process monitoring when the EMS notification service process comes up.

Objects

starEmsNotifRaisedTime
Object

starEmsNotifyServiceProcStop

Object ID

enterprises.8164.1.1000.2.85

Description

This notification is generated by EMS process monitoring when the EMS notification service process goes down.

Objects

starEmsNotifRaisedTime
Object

starEmsNotifyServiceProcDetectRestart

Object ID

enterprises.8164.1.1000.2.86

Description

This notification is generated by EMS process monitoring when the EMS notification service process restart is detected.

Objects

starEmsNotifRaisedTime
Object

starEmsNotifyServiceProcCPUUsageOverLimit

Object ID

enterprises.8164.1.1000.2.87

Description

This notification is generated by EMS process monitoring when the Ems Notification Service process CPU usage threshold is exceeded. The starEmsThreshold varbind indicates current Ems Notification Service process cpu usage value as a percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsNotifyServiceProcCPUUsageNormal

Object ID

enterprises.8164.1.1000.2.88

Description

This notification is generated by EMS process monitoring when the Ems Notification Service process CPU usage threshold comes to normal. The starEmsThreshold varbind indicates current Ems Notification Service process cpu usage value as a percentage.

Objects

starEmsNotifRaisedTime

starEmsProcMonThreshold
Object

starEmsBulkStatCounterThresholdAboveLimit

IMPORTANT:

This Trap is obsolete.

Object ID

enterprises.8164.1.1000.2.89

Description

This notification is generated by the EMS bulkstat parser when the delta value for a particular bulkstat counter has exceeded its configured threshold value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsBulkstatCounter

starEmsBulkStatRecordDetails

starEmsBulkStatRecordTime

starEmsBulkStatThreshold

starEmsBulkStatCurrent
Object

starEmsBulkStatCounterThresholdNormal

IMPORTANT:

This Trap is obsolete.

Object ID

enterprises.8164.1.1000.2.90

Description

This notification is generated by the EMS bulkstat parser when the delta value for a particular bulkstat counter comes to the normal value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsBulkstatCounter

starEmsBulkStatRecordDetails

starEmsBulkStatRecordTime

starEmsBulkStatThreshold

starEmsBulkStatCurrent
Object

starEmsCFDBDirAccessible

Object ID

enterprises.8164.1.1000.2.91

Description

This notification is generated by EMS Process Monitoring when EMS content filtering directory is accessible.

Objects

starEMSNotifRaisedTime
Object

starEmsCFDBDirNonAccessible

Object ID

enterprises.8164.1.1000.2.92

Description

This notification is generated by EMS Process Monitoring when EMS content filtering directory is not accessible. A starEmsCFDBDirAccessible message is generated when the database comes back online.

Objects

starEMSNotifRaisedTime
Object

starEmsCFDBDirUsageOverLimit

Object ID

enterprises.8164.1.1000.2.93

Description

EMS content filtering directory usage threshold is exceeded.

Possible Cause: This is a user-configurable parameter.

Action Clear: A starEMSCFDBDirUsageNormal notification is issued when usage drops below the threshold.

Objects

starEMSNotifRaisedTime

starEMSProcMonThreshold
Object

starEmsCFDBDirUsageNormal

Object ID

enterprises.8164.1.1000.2.94

Description

EMS content filtering directory usage has come to normal value.

Objects

starEMSNotifRaisedTime

starEMSProcMonThreshold
Object

starEmsCFDbImportFailed

Object ID

enterprises.8164.1.1000.2.95

Description

This notification is generated by CFEMS when failed to Import database file.

Possible Cause: None given

Action Clear: A starEmsCFDbImportSucceeded message is generated when the database file is successfully imported.

Objects

starEmsNotifRaisedTime,

starEmsCFMcrdbsHostAddress,

starEmsCFDbType,

starEmsCFSourceDbFileName
Object

starEmsCFDbImportSucceeded

Object ID

enterprises.8164.1.1000.2.96

Description

This notification is generated by CFEMS Database file is imported.

Objects

starEmsNotifRaisedTime,

starEmsCFMcrdbsHostAddress,

starEmsCFDbType,

starEmsCFSourceDbFileName
Object

starEmsCFDbExportFailed

Object ID

enterprises.8164.1.1000.2.97

Description

This notification is generated by CFEMS when database has failed to export.

Possible Cause: None given

Action Clear: A starEmsCFDbExportSucceeded message is generated.

Objects

starEmsNotifRaisedTime,

starEmsCFCdpHostAddress,

starEmsCFDbType,

starEmsCFSourceDbFileName
Object

starEmsCFDbExportSucceeded

Object ID

enterprises.8164.1.1000.2.98

Description

This notification is generated by CFEMS on successful export of a database file.

Objects

starEmsNotifRaisedTime,

starEmsCFCdpHostAddress,

starEmsCFDbType,

starEmsCFSourceDbFileName
Object

starEmsCFDbConversionFailed

Object ID

enterprises.8164.1.1000.2.99

Description

CF database conversion/manipulation operation failed.

Possible Cause: None given

Action Clear: A starEmsCFDbConversionSucceeded message is generated.

Objects

starEmsNotifRaisedTime,

starEmsCFFromDbType,

starEmsCFToDbType,

starEmsCFSourceDbFileName,

starEmsCFDestDbFileName
Object

starEmsCFDbConversionSucceeded

Object ID

enterprises.8164.1.1000.2.100

Description

This notification is generated by CFEMS when Database conversion done successfully.

Objects

starEmsNotifRaisedTime,

starEmsCFFromDbType,

starEmsCFToDbType,

starEmsCFSourceDbFileName,

starEmsCFDestDbFileName
Object

starEmsCFFtpConnetionFailed

Object ID

enterprises.8164.1.1000.2.101

Description

SFTP Connection failed.

Objects

starEmsNotifRaisedTime,

starEmsCFFtpHostInfo
Object

starEmsBulkStatCounterUsageOverLimit

IMPORTANT:

This Trap is obsolete.

Object ID

enterprises.8164.1.1000.2.102

Description

This notification is generated by EMS bulkstat parser when counter value for a particular bulkstat counter has reached or exceeded the configured threshold value.

Possible Cause: This is a user-configurable parameter.

Action Clear: A starEmsBulkStatCounterUsageNormal message is generated when usage drops below the threshold.

Objects

starEmsNotifRaisedTime,

starEmsIMGName,

starEmsBulkStatCounter,

starEmsBulkStatRecordDetails,

starEmsBulkStatRecordTime,

starEmsBulkStatThreshold,

starEmsBulkStatCounterValue
Object

starEmsBulkStatCounterUsageNormal

IMPORTANT:

This Trap is obsolete.

Object ID

enterprises.8164.1.1000.2.103

Description

This message is generated when usage drops below the threshold.

Objects

starEmsNotifRaisedTime,

starEmsIMGName,

starEmsBulkStatCounter,

starEmsBulkStatRecordDetails,

starEmsBulkStatRecordTime,

starEmsBulkStatThreshold,

starEmsBulkStatCounterValue
Object

starEmsConfigBackupFtpFailed

Object ID

enterprises.8164.1.1000.2.104

Description

This notification is generated by EMS when FTP of Config Backup file from STxx to EMS fails.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsNotifInfo
Object

starEmsConfigBackupFtpSuccess

Object ID

enterprises.8164.1.1000.2.105

Description

This notification is generated by EMS when FTP of Config Backup file from STxx to EMS succeed.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsNotifInfo
Object

starEmsBulkStatIncrementalCounterThresholdAboveLimit

Object ID

enterprises.8164.1.1000.2.106

Description

This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter has exceeded the configured threshold value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsBulkStatCounter

starEmsBulkStatRecordDetails

starEmsBulkStatRecordTime

starEmsBulkStatThresholdDouble

starEmsBulkStatCurrentDouble

starEmsBulkStatFilterDetails
Object

starEmsBulkStatIncrementalCounterThresholdNormal

Object ID

enterprises.8164.1.1000.2.107

Description

This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter comes to normal value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsBulkStatCounter

starEmsBulkStatRecordDetails

starEmsBulkStatRecordTime

starEmsBulkStatThresholdDouble

starEmsBulkStatCurrentDouble

starEmsBulkStatFilterDetails
Object

starEmsBulkStatGaugeCounterUsageOverLimit

Object ID

enterprises.8164.1.1000.2.108

Description

This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter has exceeded the configured threshold value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsBulkStatCounter

starEmsBulkStatRecordDetails

starEmsBulkStatRecordTime

starEmsBulkStatThresholdDouble

starEmsBulkStatCurrentDouble

starEmsBulkStatFilterDetails
Object

starEmsBulkStatGaugeCounterUsageNormal

Object ID

enterprises.8164.1.1000.2.109

Description

This notification is generated by EMS bulkstat parser when delta value for a particular bulkstat counter comes to normal value.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsBulkStatCounter

starEmsBulkStatRecordDetails

starEmsBulkStatRecordTime

starEmsBulkStatThresholdDouble

starEmsBulkStatCurrentDouble

starEmsBulkStatFilterDetails
Object

starEmsConfigBackupFileDiff

Object ID

enterprises.8164.1.1000.2.110

Description

This notification is generated by WEM during periodic config-backup operation. It is generated to indicate that the recently downloaded configuration file is different from the configuration file downloaded in the last config-backup operation. The third varbind indicates the name of the latest downloaded config-file. The fourth varbind indicates the name of the config file that was downloaded during the last config-backup opeartions.

Objects

starEmsNotifRaisedTime

starEmsIMGName

starEmsConfigBackupFileName

starEmsConfigBackupFileName
starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000).starEmsMIBConformances(3).starEmsMIBGroups(1).starEmsNotifMgmtGroup(1)
Object Group:

starEmsNotifMgmtGroup

Description

This is a collection of objects related with notification management on EMS.

Objects

starEmsNotifInfo

starEmsNotifRaisedTime

starEmsProcMonThreshold

starEmsInterfaceAddr

starEmsInterfaceName

starEmsIMGAddr

starEmsFtpFileName

starEmsIMGState

starEmsBulkStatFileXferTime

starEmsXMLFtpFileName

starEmsXMLFtpDestAddr

starEmsXMLFtpDestPath

starEmsIMGPreviousState

starEmsIMGName

starEmsPortMonThreshold

starEmsPortMonCurrent

starEmsDevicePath

starEmsPrevHostName

starEmsCurrHostName

starEmsP2PProtocolType

starEmsP2PProtocolValue

starEmsSyslogLoggedTime

starEmsSyslogFacility

starEmsSyslogPriority

starEmsSyslogHostname

starEmsSyslogKeyword

starEmsSyslogMessage

starEmsSyslogFilePath

starEmsDBName

starEmsBulkStatCounter

starEmsBulkStatRecordDetails

starEmsBulkStatRecordTime

starEmsBulkStatThreshold

starEmsBulkStatCurrent

starEmsCFMcrdbsHostAddress,

starEmsCFDbType,

starEmsCFSourceDbFileName,

starEmsCFCdpHostAddress,

starEmsCFFromDbType,

starEmsCFToDbType,

starEmsCFDestDbFileName,

starEmsBulkStatCounterValue

starEmsBulkStatFilterDetails

starEmsBulkStatCounterDouble

starEmsBulkStatThresholdDouble

starEmsConfigBackupFileName

starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000).starEmsMIBConformances(3).starEmsMIBGroups(1).starEmsNotifGroup(2)

Object Group:

starEmsNotifGroup

Description

A collection of EMS notifications.
Object Group:

starEmsFmEmailFailed

starEmsFmScriptFailed

starEmsFmSyslogFailed

starEmsWebServerProcStart

starEmsWebServerProcStop

starEmsWebServerProcCPUUsageOverLimit

starEmsWebServerProcCPUUsageNormal

starEmsDataBaseProcStart

starEmsDataBaseProcStop

starEmsDataBaseProcCPUUsageOverLimit

starEmsDataBaseProcCPUUsageNormal

starEmsServerProcStart

starEmsServerProcStop

starEmsServerProcCPUUsageOverLimit

starEmsServerProcCPUUsageNormal

starEmsScriptServerProcStart

starEmsScriptServerProcStop

starEmsScriptServerProcCPUUsageOverLimit

starEmsScriptServerProcCPUUsageNormal

starEmsServerDirAccessible

starEmsServerDirNonAccessible

starEmsServerDirUsageOverLimit

starEmsServerDirUsageNormal

starEmsDataBaseDirAccessible

starEmsDataBaseDirNonAccessible

starEmsDataBaseDirUsageOverLimit

starEmsDataBaseDirUsageNormal

starEmsFTPDirAccessible

starEmsFTPDirNonAccessible

starEmsFTPDirUsageOverLimit

starEmsFTPDirUsageNormal

starEmsBlkArchDirAccessible

starEmsBlkArchDirNonAccessible

starEmsBlkArchDirUsageOverLimit

starEmsBlkArchDirUsageNormal

starEmsInterfaceStateUp

starEmsInterfaceStateDown

starEmsCPUUsageOverLimit

starEmsCPUUsageNormal

starEmsSwapUsageOverLimit

starEmsSwapUsageNormal

starEmsPCFtpFailed

starEmsPCFileDeletionFailed

starEmsBulkStatFtpFailed

starEmsBulkStatFtpClear

starEmsXMLFtpFailed

starEmsXMLFtpSuccess

starEmsIMGUnmanageable

starEmsIMGManageable

starEmsPortMonThresholdBelowLimit

starEmsPortMonThresholdNormal

starEmsPortMonError

starEmsWebServerProcDetectRestart

starEmsDataBaseProcDetectRestart

starEmsServerProcDetectRestart

starEmsScriptServerProcDetectRestart

starEmsBulkStatServerProcStart

starEmsBulkStatServerProcStop

starEmsBulkStatServerProcDetectRestart

starEmsBulkStatServerProcCPUUsageOverLimit

starEmsBulkStatServerProcCPUUsageNormal

starEmsBulkStatParserProcStart

starEmsBulkStatParserProcStop

starEmsBulkStatParserProcDetectRestart

starEmsBulkStatParserProcCPUUsageOverLimit

starEmsBulkStatParserProcCPUUsageNormal

starEmsIMGRateControlStart

starEmsIMGRateControlStop

starEmsMonitorQueueFull

starEmsMonitorQueueInLimit

starEmsNotifRaisedTime

starClusterFailoverHappened

starEmsDBBackupNoDiscSpace

starEmsP2PProtocolUsageHigh

starEmsP2PProtocolUsageLimit

starEmsNBServerProcStart

starEmsNBServerProcStop

starEmsNBServerProcDetectRestart

starEmsNBServerProcCPUUsageOverLimit

starEmsNBServerProcCPUUsageNormal

starEmsNotifyServiceProcStart

starEmsNotifyServiceProcStop

starEmsNotifyServiceProcDetectRestart

starEmsNotifyServiceProcCPUUsageOverLimit

starEmsNotifyServiceProcCPUUsageNormal

starEmsKeywordDetectedInSyslog

starEmsDBMigration

starEmsBulkStatCounterThresholdAboveLimit

starEmsBulkStatCounterThresholdNormal

starEmsCFDBDirAccessible

starEmsCFDBDirNonAccessible,

starEmsCFDBDirUsageOverLimit,

starEmsCFDBDirUsageNormal,

starEmsCFDbImportFailed,

starEmsCFDbImportSucceeded,

starEmsCFDbExportFailed,

starEmsCFDbExportSucceeded,

starEmsCFDbConversionFailed,

starEmsCFDbConversionSucceeded,

starEmsCFFtpConnetionFailed,

starEmsBulkStatCounterUsageOverLimit,

starEmsBulkStatCounterUsageNormal

starEmsConfigBackupFtpFailed

starEmsConfigBackupFtpSuccess

starEmsBulkStatIncrementalCounterThresholdAboveLimit

starEmsBulkStatIncrementalCounterThresholdNormal

starEmsBulkStatGaugeCounterUsageOverLimit

starEmsBulkStatGaugeCounterUsageNormal

starEmsConfigBackupFileDiff
starentMIB(8164).starentMIBObjects(1).starentEmsMIB(1000).starEmsMIBConformances(3).starEmsMIBCompliances(2)
Object

starEmsMIBCompliance

Description

The compliance statements for entities which implement the STARENT EMS MIB.

Required Groups

starEmsNotifMgmtGroup

starEmsNotifGroup